{"text_format":"1","workbook":"xlsx","n_sheets":76,"sheets":["10A61 Liquid 1.5\"","10A61 Liquid 3\"","10A61 Liquid 3\" ViscosityLINEST","10A61 3\" Density LINEST","10A61 3\" Results Interpol.","Sheet2","5\" Theoretical Test","10A61 3\" Gas+liquid Curves","10A61 3\" Gas+liquid Calcs","10A61 Water","10A61 5\" Curves","10A61 3\" Gas+liquid Results","10A61 3","10A61 5\" + 6\" Results","10A61 10\"+6\" Curves","10A61 10\"+6\" Calcs","10A61 10\" Results","10A4 Capacity Tables","10A22 Curves","Sheet1","10A61 5","10A61 10","BasicFluid","Start","Basic","BasicStructure","BasicMeter10A61 3 inch","BasicMeter10A61 5 inch","BasicMeter10A4 Standard","BasicMeter10A4 Low Pressure Dro","BasicMeter10A4 Alarm","BasicResults","VA Sizing","Calculating","Bulk Sizing","Graphics","Sheet3","Log","10A61 5\" Calcs","10A32 Capacity","Basic10A32","10A32 Tables","IX Preview","Temp-Press Limits","SizingSummary","Steam","MixedGas","10A4 Standard Floats Results","10A22 Standard Results","10A61 Naming","10A45 Naming Standard","10A22 Naming","10A45 Naming Low PSI","10A45 Naming Alarm","10A45 Naming TA","10A45 Naming PTFE","10A45 Naming PVC","10A4 Low PSI Drop Floats Result","Photos","10A4 Alarm Floats Results","10A4 TA Floats Results","10A4 PTFE Floats Results","10A4 PVC Floats Results","10A22 Alarm Results","Modified Inputs","10A22 Capacity Table","BasicMeter10A22 Standard Liquid","BasicMeter Consolidation","BasicPartNumber","BulkPartNumber","BasicMeter10A22 Alarm Liquid","BasicMeter10A22 Standard Gas","BasicMeter10A22 Alarm Gas","Assistant","Descriptions","Viscosity Limits"],"not_rendered":{"charts":93,"images":21,"macros":1,"external_links":0,"defined_names":13,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"10A61 Liquid 1.5\"","index":0,"n_rows":234,"n_cols":6,"rows_kept":234,"cut":false,"hidden":true,"merged":[[1,1,1,5]]}
[]
[null,"10A61 1-1/2\""]
[null,"Tube","Float","SG","Max Flow (mL/min)","Min Flow (mL/min)"]
[null,"1/8-21","SA",0.4,94.87,10]
[null,null,null,0.41,93.7,10]
[null,null,null,0.42,92.58,10]
[null,null,null,0.43,91.5,10]
[null,null,null,0.44,90.45,10]
[null,null,null,0.45,89.44,10]
[null,null,null,0.46,88.47,10]
[null,null,null,0.47,87.52,10]
[null,null,null,0.48,86.6,10]
[null,null,null,0.49,85.71,10]
[null,null,null,0.5,84.85,10]
[null,null,null,0.50999999999999901,84.02,10]
[null,null,null,0.51999999999999902,83.21,10]
[null,null,null,0.52999999999999903,82.42,10]
[null,null,null,0.53999999999999904,81.650000000000006,10]
[null,null,null,0.54999999999999905,80.900000000000006,10]
[null,null,null,0.55999999999999905,80.180000000000007,10]
[null,null,null,0.56999999999999895,79.47,10]
[null,null,null,0.57999999999999896,78.78,10]
[null,null,null,0.58999999999999897,78.11,10]
[null,null,null,0.59999999999999898,77.459999999999994,10]
[null,null,null,0.60999999999999899,76.819999999999993,10]
[null,null,null,0.619999999999999,76.2,10]
[null,null,null,0.62999999999999901,75.59,10]
[null,null,null,0.63999999999999901,75,10]
[null,null,null,0.64999999999999902,74.42,10]
[null,null,null,0.65999999999999903,73.849999999999994,10]
[null,null,null,0.66999999999999904,73.3,10]
[null,null,null,0.67999999999999905,72.760000000000005,10]
[null,null,null,0.68999999999999895,72.23,10]
[null,null,null,0.69999999999999896,71.709999999999994,10]
[null,null,null,0.70999999999999897,71.209999999999994,10]
[null,null,null,0.71999999999999897,70.709999999999994,10]
[null,null,null,0.72999999999999798,70.22,10]
[null,null,null,0.73999999999999799,69.75,10]
[null,null,null,0.749999999999998,69.28,10]
[null,null,null,0.75999999999999801,68.819999999999993,10]
[null,null,null,0.76999999999999802,68.38,10]
[null,null,null,0.77999999999999803,67.94,10]
[null,null,null,0.78999999999999804,67.510000000000005,10]
[null,null,null,0.79999999999999805,67.08,10]
[null,null,null,0.80999999999999805,66.67,10]
[null,null,null,0.81999999999999795,66.260000000000005,10]
[null,null,null,0.82999999999999796,65.86,10]
[null,null,null,0.83999999999999797,65.47,10]
[null,null,null,0.84999999999999798,65.08,10]
[null,null,null,0.85999999999999799,64.7,10]
[null,null,null,0.869999999999998,64.33,10]
[null,null,null,0.87999999999999801,63.96,10]
[null,null,null,0.88999999999999801,63.6,10]
[null,null,null,0.89999999999999802,63.25,10]
[null,null,null,0.90999999999999803,62.9,10]
[null,null,null,0.91999999999999804,62.55,10]
[null,null,null,0.92999999999999805,62.22,8]
[null,null,null,0.93999999999999695,61.89,8]
[null,null,null,0.94999999999999696,61.56,8]
[null,null,null,0.95999999999999697,61.24,8]
[null,null,null,0.96999999999999698,60.92,8]
[null,null,null,0.97999999999999698,60.61,8]
[null,null,null,0.98999999999999699,60.3,8]
[null,null,null,0.999999999999997,60,8]
[null,null,null,1.01,59.7,8]
[null,null,null,1.02,59.41,8]
[null,null,null,1.03,59.12,8]
[null,null,null,1.04,58.83,8]
[null,null,null,1.05,58.55,8]
[null,null,null,1.06,58.28,8]
[null,null,null,1.07,58,8]
[null,null,null,1.08,57.74,8]
[null,null,null,1.0900000000000001,57.47,8]
[null,null,null,1.1000000000000001,57.21,8]
[null,null,null,1.1100000000000001,56.95,8]
[null,null,null,1.1200000000000001,56.69,8]
[null,null,null,1.1299999999999999,56.44,8]
[null,null,null,1.1399999999999999,56.2,8]
[null,null,null,1.1499999999999999,55.95,8]
[null,null,null,1.1599999999999999,55.71,8]
[null,null,null,1.17,55.47,8]
[null,null,null,1.18,55.23,8]
[null,null,null,1.19,55,8]
[null,null,null,1.2,54.77,8]
[null,null,null,1.21,54.55,8]
[null,null,null,1.22,54.32,8]
[null,null,null,1.23,54.1,8]
[null,null,null,1.24,53.88,8]
[null,null,null,1.25,53.67,8]
[null,null,null,1.26,53.45,8]
[null,null,null,1.27,53.24,8]
[null,null,null,1.28,53.03,8]
[null,null,null,1.29,52.83,8]
[null,null,null,1.3,52.62,8]
[null,null,null,1.31,52.42,8]
[null,null,null,1.32,52.22,8]
[null,null,null,1.33,52.03,8]
[null,null,null,1.34,51.83,8]
[null,null,null,1.35,51.64,8]
[null,null,null,1.36,51.45,8]
[null,null,null,1.37,51.26,8]
[null,null,null,1.38,51.08,8]
[null,null,null,1.39,50.89,6]
[null,null,null,1.4,50.71,6]
[null,null,null,1.41,50.53,6]
[null,null,null,1.42,50.35,6]
[null,null,null,1.43,50.17,6]
[null,null,null,1.44,50,6]
[null,null,null,1.45,49.83,6]
[null,null,null,1.46,49.66,6]
[null,null,null,1.46999999999999,49.49,6]
[null,null,null,1.47999999999999,49.32,6]
[null,null,null,1.48999999999999,49.15,6]
[null,null,null,1.49999999999999,48.99,6]
[]
[]
[]
[]
[]
[]
[null,"10A61 1-1/2\""]
[null,"SG","1/16-08","BG"]
[null,null,"Max Flow (mL/min)","Min Flow (mL/min)"]
[null,0.4,1.2649999999999999,0.15]
[null,0.41,1.2490000000000001]
[null,0.42,1.234]
[null,0.43,1.22]
[null,0.44,1.206]
[null,0.45,1.1930000000000001]
[null,0.46,1.18]
[null,0.47,1.167]
[null,0.48,1.155]
[null,0.49,1.143]
[null,0.5,1.131]
[null,0.50999999999999901,1.1200000000000001]
[null,0.51999999999999902,1.109]
[null,0.52999999999999903,1.099]
[null,0.53999999999999904,1.089]
[null,0.54999999999999905,1.079]
[null,0.55999999999999905,1.069]
[null,0.56999999999999895,1.06]
[null,0.57999999999999896,1.05]
[null,0.58999999999999897,1.05]
[null,0.59999999999999898,1.05]
[null,0.60999999999999899,1.024,0.1]
[null,0.619999999999999,1.016]
[null,0.62999999999999901,1.008]
[null,0.63999999999999901,1]
[null,0.64999999999999902,0.99229999999999996]
[null,0.65999999999999903,0.98470000000000002]
[null,0.66999999999999904,0.97740000000000005]
[null,0.67999999999999905,0.97009999999999996]
[null,0.68999999999999895,0.96309999999999996]
[null,0.69999999999999896,0.95620000000000005]
[null,0.70999999999999897,0.94940000000000002]
[null,0.71999999999999897,0.94279999999999997]
[null,0.72999999999999798,0.93630000000000002]
[null,0.73999999999999799,0.93]
[null,0.749999999999998,0.92379999999999995]
[null,0.75999999999999801,0.91769999999999996]
[null,0.76999999999999802,0.91169999999999995]
[null,0.77999999999999803,0.90580000000000005]
[null,0.78999999999999804,0.90010000000000001]
[null,0.79999999999999805,0.89439999999999997]
[null,0.80999999999999805,0.88890000000000002]
[null,0.81999999999999795,0.88349999999999995]
[null,0.82999999999999796,0.87809999999999999]
[null,0.83999999999999797,0.87290000000000001]
[null,0.84999999999999798,0.86770000000000003]
[null,0.85999999999999799,0.86270000000000002]
[null,0.869999999999998,0.85770000000000002]
[null,0.87999999999999801,0.8528]
[null,0.88999999999999801,0.84799999999999998]
[null,0.89999999999999802,0.84330000000000005]
[null,0.90999999999999803,0.83860000000000001]
[null,0.91999999999999804,0.83409999999999995]
[null,0.92999999999999805,0.8296]
[null,0.93999999999999695,0.82509999999999994]
[null,0.94999999999999696,0.82079999999999997]
[null,0.95999999999999697,0.8165]
[null,0.96999999999999698,0.81230000000000002]
[null,0.97999999999999698,0.80810000000000004]
[null,0.98999999999999699,0.80400000000000005]
[null,0.999999999999997,0.8]
[null,1.01]
[null,1.02]
[null,1.03]
[null,1.04]
[null,1.05]
[null,1.06]
[null,1.07]
[null,1.08]
[null,1.0900000000000001]
[null,1.1000000000000001]
[null,1.1100000000000001]
[null,1.1200000000000001]
[null,1.1299999999999999]
[null,1.1399999999999999]
[null,1.1499999999999999]
[null,1.1599999999999999]
[null,1.17]
[null,1.18]
[null,1.19]
[null,1.2]
[null,1.21]
[null,1.22]
[null,1.23]
[null,1.24]
[null,1.25]
[null,1.26]
[null,1.27]
[null,1.28]
[null,1.29]
[null,1.3]
[null,1.31]
[null,1.32]
[null,1.33]
[null,1.34]
[null,1.35]
[null,1.36]
[null,1.37]
[null,1.38]
[null,1.39]
[null,1.4]
[null,1.41]
[null,1.42]
[null,1.43]
[null,1.44]
[null,1.45]
[null,1.46]
[null,1.46999999999999]
[null,1.47999999999999]
[null,1.48999999999999]
[null,1.49999999999999]

{"sheet":"10A61 Liquid 3\"","index":1,"n_rows":121,"n_cols":61,"rows_kept":121,"cut":false,"hidden":true,"merged":[[1,4,1,5],[2,4,2,5],[3,4,3,6],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[3,15,3,16],[3,17,3,18],[3,19,3,20],[3,31,3,32],[3,33,3,34],[3,37,3,38],[3,35,3,36],[3,21,3,22],[3,23,3,24],[3,25,3,26],[3,27,3,28],[3,29,3,30],[3,39,3,40],[3,41,3,42],[3,45,3,46],[3,43,3,44],[3,47,3,48],[3,59,3,60],[3,49,3,50],[3,53,3,54],[3,51,3,52],[3,55,3,56],[3,57,3,58]]}
[]
[null,null,"10A61 3\"",null,"Tube/Float"]
["sg","viscosity",null,null,"Real Data",null,"Interpolated Data"]
[0.42,{"$f":"'10A61 3\" Density LINEST'!D19","v":0},"SG","Viscosity","1/8-08-BG",null,null,"1/8-08-SA",null,"1/8-08-SS",null,"1/8-08-CA",null,"1/8-08-TA",null,"1/8-20-BG",null,"1/8-20-SA",null,"1/8-20-SS",null,"1/8-20-CA",null,"1/8-20-TA",null,"1/4-15-CD",null,"1/4-15-SA",null,"1/4-20-CD",null,"1/4-20-SA",null,"1/4-15-SS",null,"1/4-15-CA",null,"1/4-20-SS",null,"1/4-15-TA",null,"1/4-41-G-SA",null,"1/4-20-CA",null,"1/4-20-TA",null,"1/4-41-P-SA",null,"1/4-41-G-SS",null,"1/4-41-P-SS",null,"1/4-41-G-CA",null,"1/4-41-G-TA",null,"1/4-41-P-CA",null,"1/4-41-P-TA"]
[null,null,null,null,"Max Flow (mL/min)","Min Flow (mL/min)","Max Flow Formula","Viscosity","Max Flow"]
[null,null,0.4,0.5,11.97,1.5,null,0.5,19.18,0.5,37.25,0.5,61.81,0.5,67.03,0.5,67.62,0.5,97.36,0.5,157.1,0.5,230.5,0.5,245.6,0.5,292.8,0.5,431.6,0.5,456.8,0.5,649.20000000000005,0.5,667.8,0.5,949.7,0.5,980.8,0.5,1006,0.5,1352,0.5,1382,0.5,1462,0.5,1744,0.5,2056,0.5,2595,0.5,2933,0.5,3111,0.5,6329,0.5,3837]
[null,null,0.4,0.6,10.1,1,null,0.6,16.48,0.6,32.61,0.6,56.32,0.6,61.08,0.6,61.14,0.6,90.24,0.6,151.19999999999999,0.6,223.2,0.6,237.7,0.6,275,0.6,416.3,0.6,441.1,0.6,639,0.6,651,0.6,937.3,0.6,964,0.6,992.9,0.6,1326,0.6,1370,0.6,1449,0.6,1714,0.6,2014,0.6,2578,0.6,2884,0.6,3058,0.6,3605,0.6,3811]
[null,null,0.4,1,6.202,0.8,null,0.7,14.43,0.7,28.96,0.7,50.99,0.7,55.96,0.7,55.72,0.7,84.12,0.7,144.5,0.7,216.5,0.7,231,0.7,257.10000000000002,0.7,401.9,0.7,426.8,0.7,628.4,0.7,634.79999999999995,0.7,921.1,0.7,950.5,0.7,979.3,0.7,1302,0.7,1354,0.7,1436,0.7,1688,0.7,1981,0.7,2555,0.7,2838,0.7,3012,0.7,3584,0.7,3790]
[null,null,0.4,1.3,4.8520000000000003,0.6,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J7","v":{"$error":"#NUM!"}},0.8,12.69,0.8,25.92,0.8,46.26,0.8,50.76,0.8,49.62,0.8,77.67,0.8,136.69999999999999,0.8,210.5,0.8,224.6,0.8,238.6,0.8,383.8,0.8,413.1,0.8,612.5,0.8,618.29999999999995,0.8,904,0.8,939.5,0.8,961.1,0.8,1270,0.8,1337,0.8,1417,0.8,1667,0.8,1953,0.8,2522,0.8,2795,0.8,2967,0.8,3567,0.8,3771]
[null,null,0.4,1.5,4.1900000000000004,0.4,null,0.9,11.32,0.9,23.5,0.9,42.45,0.9,46.59,0.9,44.8,0.9,72.400000000000006,0.9,130.19999999999999,0.9,205.3,0.9,219.1,0.9,223.4,0.9,368.6,0.9,401.3,0.9,598.9,0.9,604.1,0.9,889.2,0.9,930,0.9,945.4,0.9,1243,0.9,1322,0.9,1402,0.9,1649,0.9,1930,0.9,2493,0.9,2758,0.9,2928,0.9,3552,0.9,3756]
[null,null,0.4,2,3.1030000000000002,0.4,null,1,10.25,1,21.49,1,38.93,1,42.96,1,40.89,1,66.12,1,124.3,1,197,1,212.5,1,210.1,1,347.8,1,390.2,1,593.70000000000005,1,590.70000000000005,1,871.5,1,920.4,1,929.4,1,1219,1,1310,1,1388,1,1625,1,1907,1,2468,1,2727,1,2894,1,3519,1,3732]
[null,null,0.4,2.5,2.5169999999999999,0.2,null,1.5,6.9809999999999999,1.5,14.56,1.5,27.44,1.5,30.49,1.5,28.17,1.5,46.24,1.5,94.19,1.5,163.5,1.5,178.2,1.5,154.9,1.5,273.10000000000002,1.5,326.39999999999998,1.5,521.29999999999995,1.5,499.6,1.5,793.4,1.5,845.9,1.5,852.8,1.5,1119,1.5,1252,1.5,1335,1.5,1526,1.5,1769,1.5,2362,1.5,2595,1.5,2766,1.5,3384,1.5,3589]
[null,null,0.4,3,2.12,0.2,null,2,5.2380000000000004,2,11.08,2,20.82,2,23.12,2,21.79,2,35.409999999999997,2,73.319999999999993,2,134.30000000000001,2,148.4,2,123.2,2,219.9,2,271.10000000000002,2,458.9,2,424.8,2,704.3,2,787.2,2,765.7,2,1030,2,1179,2,1261,2,1442,2,1675,2,2268,2,2461,2,2622,2,3280,2,3487]
[null,null,0.4,3.4,1.88,0.2,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J8","v":{"$error":"#NUM!"}},2.5,4.1470000000000002,2.5,8.9969999999999999,2.5,16.84,2.5,18.7,2.5,17.440000000000001,2.5,29.01,2.5,59.67,2.5,110.6,2.5,122.3,2.5,100.7,2.5,183.8,2.5,226.8,2.5,400.6,2.5,362.6,2.5,621.79999999999995,2.5,722.8,2.5,676.1,2.5,961.7,2.5,1116,2.5,1194,2.5,1376,2.5,1572,2.5,2165,2.5,2360,2.5,2516,2.5,3180,2.5,3381]
[null,null,null,null,null,null,null,3,3.4910000000000001,3,7.4080000000000004,3,14.18,3,15.73,3,14.52,3,24.38,3,50.34,3,93.92,3,104.1,3,85.18,3,157.6,3,192.6,3,349.8,3,313.5,3,553.79999999999995,3,659.3,3,607,3,899.8,3,1054,3,1135,3,1302,3,1490,3,2093,3,2261,3,2422,3,3081,3,3287]
[null,null,null,null,null,null,null,3.5,3.024,3.5,6.2949999999999999,3.5,12.28,3.5,13.63,3.5,12.54,3.5,20.77,3.5,43.82,3.5,81.459999999999994,3.5,90.33,3.5,73.680000000000007,3.5,137.1,3.5,166.2,3.5,309.2,3.5,276.8,3.5,496.4,3.5,601,3.5,544.1,3.5,846.2,3.5,993.8,3.5,1070,3.5,1233,3.5,1422,3.5,2029,3.5,2164,3.5,2318,3.5,2984,3.5,3184]
[null,null,null,null,null,null,null,4,2.6629999999999998,4,5.54,4,10.66,4,11.94,4,10.97,4,18.25,4,39.049999999999997,4,71.930000000000007,4,79.81,4,64.8,4,121.1,4,145.5,4,274.3,4,249.4,4,446.3,4,548.4,4,492.5,4,801.2,4,929.2,4,1010,4,1161,4,1361,4,1960,4,2081,4,2231,4,2911,4,3101]
[null,null,null,null,null,null,null,4.5,2.379,4.5,4.9630000000000001,4.5,9.3390000000000004,4.5,10.47,4.5,9.7539999999999996,4.5,16.309999999999999,4.5,34.56,4.5,64.430000000000007,4.5,71.489999999999995,4.5,57.86,4.5,108.8,4.5,129.4,4.5,245.9,4.5,224.2,4.5,404.5,4.5,499.1,4.5,446.4,4.5,763.3,4.5,870.5,4.5,946.3,4.5,1097,4.5,1298,4.5,1881,4.5,2010,4.5,2155,4.5,2851,4.5,3037]
[null,null,null,null,null,null,null,null,null,5,4.4000000000000004,5,8.4250000000000007,5,9.36,5,8.7789999999999999,5,14.69,5,30.97,5,58.88,5,65.010000000000005,5,52.27,5,98.3,5,116.5,5,221.5,5,203.9,5,372.8,5,458.8,5,409.9,5,717.3,5,811.9,5,888.3,5,1037,5,1245,5,1812,5,1944,5,2087,5,2780,5,2973]
[]
[]
[]
[null,null,0.59999999999999898,0.5,10.57,1.5,null,0.5,17.46,0.5,33.659999999999997,0.5,54.81,0.5,59.16,0.5,56.04,0.5,81.84,0.5,131.19999999999999,0.5,191.8,0.5,203.5,0.5,233.3,0.5,352.9,0.5,357.7,0.5,523.20000000000005,0.5,548.4,0.5,776.9,0.5,800.6,0.5,821.3,0.5,1093,0.5,1134,0.5,1202,0.5,1401,0.5,1689,0.5,2106,0.5,2408,0.5,2547,0.5,2953,0.5,3118]
[null,null,null,0.6,9.0860000000000003,1,null,0.6,15.11,0.6,30.17,0.6,50.47,0.6,54.8,0.6,51.95,0.6,76.98,0.6,126.7,0.6,187.4,0.6,199.8,0.6,223.2,0.6,341.9,0.6,350.2,0.6,514.6,0.6,538.6,0.6,770.8,0.6,790.8,0.6,817.1,0.6,1071,0.6,1121,0.6,1187,0.6,1383,0.6,1658,0.6,2092,0.6,2382,0.6,2527,0.6,2944,0.6,3115]
[null,null,null,0.9,6.1680000000000001,0.8,null,0.7,13.29,0.7,26.96,0.7,46.65,0.7,50.65,0.7,47.52,0.7,72.19,0.7,122.7,0.7,182.3,0.7,194.4,0.7,211.7,0.7,331.6,0.7,340,0.7,507.8,0.7,527.1,0.7,762.3,0.7,779.3,0.7,808.1,0.7,1054,0.7,1113,0.7,1178,0.7,1362,0.7,1630,0.7,2080,0.7,2348,0.7,2492,0.7,2927,0.7,3097]
[null,null,null,1.1000000000000001,5.0970000000000004,0.6,null,0.8,11.89,0.8,24.45,0.8,43.27,0.8,47.31,0.8,43.88,0.8,68.28,0.8,119.2,0.8,177.8,0.8,189.8,0.8,199.9,0.8,323,0.8,330.4,0.8,502,0.8,517.20000000000005,0.8,753.4,0.8,769.5,0.8,800.4,0.8,1040,0.8,1104,0.8,1171,0.8,1345,0.8,1605,0.8,2069,0.8,2317,0.8,2461,0.8,2913,0.8,3082]
[null,null,null,1.4,4.0629999999999997,0.4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J9","v":{"$error":"#NUM!"}},0.9,10.63,0.9,22.17,0.9,39.71,0.9,43.63,0.9,39.799999999999997,0.9,63.73,0.9,113.5,0.9,173.5,0.9,185.3,0.9,187.1,0.9,310.5,0.9,321.10000000000002,0.9,491.2,0.9,505.3,0.9,741.1,0.9,761.7,0.9,788.5,0.9,1018,0.9,1092,0.9,1159,0.9,1330,0.9,1586,0.9,2046,0.9,2286,0.9,2429,0.9,2901,0.9,3069]
[null,null,null,1.9,2.9689999999999999,0.2,null,1,9.6010000000000009,1,20.309999999999999,1,36.770000000000003,1,40.4,1,36.32,1,59.84,1,108.6,1,169.7,1,181.3,1,176.5,1,299.39999999999998,1,312.89999999999998,1,481.4,1,494.4,1,730.2,1,754.8,1,777,1,998.5,1,1081,1,1147,1,1317,1,1568,1,2025,1,2259,1,2400,1,2890,1,3057]
[null,null,null,2.5,2.258,0.2,null,1.5,6.5229999999999997,1.5,14.06,1.5,26.52,1.5,29.3,1.5,25.26,1.5,42.91,1.5,88.03,1.5,146.4,1.5,158.1,1.5,135,1.5,242.5,1.5,272.8,1.5,437.7,1.5,441.7,1.5,678,1.5,711.6,1.5,723.7,1.5,926,1.5,1043,1.5,1106,1.5,1249,1.5,1476,1.5,1949,1.5,2164,1.5,2298,1.5,2796,1.5,2968]
[null,null,null,3,1.905,0.2,null,2,4.9820000000000002,2,10.69,2,20.36,2,22.66,2,19.32,2,33.03,2,69.680000000000007,2,125.5,2,136.9,2,106.7,2,199.9,2,231.5,2,396,2,381.1,2,623.29999999999995,2,665.4,2,670.6,2,859.5,2,997.5,2,1064,2,1182,2,1399,2,1877,2,2069,2,2207,2,2721,2,2888]
[null,null,null,3.8,1.522,0.15,null,2.5,3.9329999999999998,2.5,8.65,2.5,16.45,2.5,18.29,2.5,15.9,2.5,26.83,2.5,57.26,2.5,106.3,2.5,117.7,2.5,88.74,2.5,137.5,2.5,196.8,2.5,354.3,2.5,334.2,2.5,562.4,2.5,626.1,2.5,612.20000000000005,2.5,805.3,2.5,949.7,2.5,1016,2.5,1134,2.5,1336,2.5,1814,2.5,1985,2.5,2117,2.5,2650,2.5,2819]
[null,null,null,4,1.45,0.15,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J10","v":{"$error":"#NUM!"}},3,3.2639999999999998,3,7.298,3,13.83,3,15.38,3,13.16,3,22.85,3,48.39,3,90.85,3,100.5,3,75.27,3,144.9,3,170.1,3,316,3,293.60000000000002,3,508,3,584,3,553,3,760.9,3,908.3,3,972,3,1090,3,1269,3,1747,3,1919,3,2047,3,2584,3,2749]
[null,null,null,null,null,null,null,3.5,2.8220000000000001,3.5,6.21,3.5,11.95,3.5,13.28,3.5,11.28,3.5,19.739999999999998,3.5,41.92,3.5,79.150000000000006,3.5,87.87,3.5,65.290000000000006,3.5,127.3,3.5,147.6,3.5,281.89999999999998,3.5,260.10000000000002,3.5,462.5,3.5,541.70000000000005,3.5,507.4,3.5,719.6,3.5,868.5,3.5,936,3.5,1040,3.5,1213,3.5,1697,3.5,1855,3.5,1989,3.5,2520,3.5,2690]
[null,null,null,null,null,null,null,4,2.4910000000000001,4,5.351,4,10.56,4,11.73,4,9.9390000000000001,4,17.190000000000001,4,37.020000000000003,4,69.97,4,77.69,4,57.59,4,112.8,4,129.9,4,253.4,4,232.8,4,420.7,4,502.8,4,461.7,4,682.3,4,825.2,4,889.7,4,992.3,4,1166,4,1657,4,1796,4,1915,4,2451,4,2617]
[null,null,null,null,null,null,null,4.5,2.23,4.5,4.7789999999999999,4.5,9.43,4.5,10.51,4.5,8.8420000000000005,4.5,15.27,4.5,33.51,4.5,62.74,4.5,69.680000000000007,4.5,51.42,4.5,101.4,4.5,115.6,4.5,229.3,4.5,212.6,4.5,386.2,4.5,464.4,4.5,424.7,4.5,650.6,4.5,786.8,4.5,850.5,4.5,946.5,4.5,1123,4.5,1610,4.5,1727,4.5,1852,4.5,2393,4.5,2554]
[null,null,null,null,null,null,null,5,2.016,5,4.3250000000000002,5,8.3800000000000008,5,9.4049999999999994,5,7.9580000000000002,5,13.82,5,30.38,5,56.86,5,63.17,5,46.47,5,91.94,5,104.1,5,207.9,5,194.9,5,353.7,5,430.1,5,390.9,5,622.9,5,742.2,5,807.7,5,899.7,5,1082,5,1561,5,1674,5,1796,5,2349,5,2504]
[]
[]
[]
[]
[null,null,0.79999999999999805,0.5,9.343,1,null,0.5,15.93,0.5,30.73,0.5,49.67,0.5,53.05,0.5,47.71,0.5,70.400000000000006,0.5,114.8,0.5,166.9,0.5,177.3,0.5,192.7,0.5,301.2,0.5,292.8,0.5,444.2,0.5,472.9,0.5,670.5,0.5,688.3,0.5,711.1,0.5,929.8,0.5,984.1,0.5,1040,0.5,1182,0.5,1461,0.5,1807,0.5,2081,0.5,2205,0.5,2540,0.5,2684]
[null,null,null,0.6,8.0280000000000005,1,null,0.6,13.95,0.6,28,0.6,46.27,0.6,50,0.6,44.22,0.6,67.760000000000005,0.6,111.1,0.6,164.3,0.6,174.4,0.6,185.8,0.6,293.60000000000002,0.6,288.2,0.6,436.6,0.6,466.8,0.6,667.5,0.6,682.2,0.6,706.2,0.6,910.8,0.6,972.2,0.6,1031,0.6,1174,0.6,1436,0.6,1795,0.6,2067,0.6,2189,0.6,2540,0.6,2684]
[null,null,null,0.8,6.17,0.8,null,0.7,12.27,0.7,25.33,0.7,43.02,0.7,46.76,0.7,41.12,0.7,63.58,0.7,107.7,0.7,160.69999999999999,0.7,171.4,0.7,176.9,0.7,284.89999999999998,0.7,280.60000000000002,0.7,430.8,0.7,458.6,0.7,662,0.7,674,0.7,702.3,0.7,896.3,0.7,963.6,0.7,1021,0.7,1157,0.7,1413,0.7,1785,0.7,2045,0.7,2127,0.7,2530,0.7,2679]
[null,null,null,1,4.9829999999999997,0.6,null,0.8,10.98,0.8,22.98,0.8,40.19,0.8,43.68,0.8,37.97,0.8,60.13,0.8,104.8,0.8,156.9,0.8,167.4,0.8,169,0.8,277.39999999999998,0.8,273.60000000000002,0.8,425.8,0.8,450.1,0.8,655.7,0.8,665.5,0.8,695.7,0.8,883.9,0.8,957.3,0.8,1014,0.8,1142,0.8,1392,0.8,1777,0.8,2020,0.8,2145,0.8,2518,0.8,2666]
[null,null,null,1.2,4.1900000000000004,0.4,null,0.9,9.9559999999999995,0.9,21.09,0.9,37.74,0.9,41.13,0.9,35.28,0.9,57.25,0.9,102.2,0.9,153.6,0.9,163.9,0.9,159.1,0.9,271.10000000000002,0.9,266.2,0.9,421.5,0.9,442.7,0.9,649.70000000000005,0.9,658.1,0.9,689.8,0.9,873.1,0.9,951.2,0.9,1008,0.9,1129,0.9,1373,0.9,1769,0.9,1997,0.9,2122,0.9,2507,0.9,2654]
[null,null,null,1.7,3.0219999999999998,0.2,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J11","v":{"$error":"#NUM!"}},1,8.9969999999999999,1,19.329999999999998,1,34.950000000000003,1,38.44,1,32.200000000000003,1,53.79,1,97.96,1,150.19999999999999,1,160.6,1,150,1,261.5,1,259.39999999999998,1,413.2,1,433.8,1,640.1,1,652.1,1,681.7,1,856.5,1,941.7,1,1000,1,1118,1,1358,1,1752,1,1973,1,2098,1,2497,1,2644]
[null,null,null,2,2.5409999999999999,0.2,null,1.5,6.1029999999999998,1.5,13.62,1.5,25.56,1.5,28.27,1.5,22.5,1.5,39.78,1.5,81.28,1.5,133.30000000000001,1.5,144.1,1.5,116.1,1.5,217,1.5,228.7,1.5,378,1.5,394.7,1.5,599,1.5,623.20000000000005,1.5,639.9,1.5,794.5,1.5,907.4,1.5,963.5,1.5,1066,1.5,1292,1.5,1685,1.5,1888,1.5,2006,1.5,2437,1.5,2588]
[null,null,null,2.5,2.0169999999999999,0.2,null,2,4.6509999999999998,2,10.33,2,19.98,2,22.25,2,17.23,2,30.81,2,66.66,2,117.2,2,127.8,2,92.72,2,182,2,198,2,347.4,2,350.1,2,561.9,2,586.79999999999995,2,604.6,2,745.6,2,880.6,2,939.8,2,1017,2,1225,2,1633,2,1825,2,1947,2,2370,2,2517]
[null,null,null,3,1.698,0.2,null,2.5,3.7509999999999999,2.5,8.3559999999999999,2.5,16.11,2.5,17.96,2.5,14.13,2.5,25.06,2.5,54.91,2.5,102.5,2.5,112,2.5,77.569999999999993,2.5,154.6,2.5,170.6,2.5,316.89999999999998,2.5,309.10000000000002,2.5,520.29999999999995,2.5,555.6,2.5,560.29999999999995,2.5,699.5,2.5,843.8,2.5,901.1,2.5,971.8,2.5,1175,2.5,1583,2.5,1751,2.5,1869,2.5,2321,2.5,2465]
[null,null,null,3.4,1.5109999999999999,0.15,null,3,3.0579999999999998,3,7.0389999999999997,3,13.55,3,15.08,3,11.84,3,21.13,3,46.62,3,87.89,3,97.43,3,65.8,3,132.80000000000001,3,147.5,3,286.5,3,275.10000000000002,3,471.5,3,524.29999999999995,3,513.9,3,662.8,3,807.7,3,865.1,3,941.1,3,1125,3,1533,3,1693,3,1807,3,2264,3,2411]
[null,null,null,4,1.2949999999999999,0.15,null,3.5,2.637,3.5,6.0960000000000001,3.5,11.7,3.5,13.03,3.5,10.09,3.5,18.54,3.5,40.43,3.5,76.88,3.5,85.52,3.5,57.17,3.5,117.9,3.5,129.30000000000001,3.5,258.3,3.5,246.6,3.5,432.7,3.5,494.3,3.5,471.5,3.5,630.9,3.5,777.8,3.5,833.1,3.5,906.2,3.5,1077,3.5,1485,3.5,1645,3.5,1756,3.5,2216,3.5,2360]
[null,null,null,4.4000000000000004,1.1819999999999999,0.15,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J12","v":{"$error":"#NUM!"}},4,2.3260000000000001,4,5.2850000000000001,4,10.31,4,11.47,4,8.8740000000000006,4,16.239999999999998,4,35.700000000000003,4,68.27,4,75.89,4,50.53,4,105,4,114.2,4,233,4,221.6,4,398.7,4,461.9,4,437.7,4,599.6,4,747.8,4,806.3,4,867.5,4,1035,4,1449,4,1597,4,1713,4,2168,4,2317]
[null,null,null,null,null,null,null,4.5,2.0840000000000001,4.5,4.6319999999999997,4.5,9.24,4.5,10.28,4.5,7.931,4.5,14.37,4.5,31.98,4.5,61.24,4.5,68.09,4.5,45.16,4.5,94.4,4.5,101.8,4.5,212.1,4.5,200.9,4.5,366.7,4.5,403,4.5,432.7,4.5,572.1,4.5,714.9,4.5,771.5,4.5,832.3,4.5,1000,4.5,1419,4.5,1544,4.5,1658,4.5,2116,4.5,2262]
[null,null,null,null,null,null,null,5,1.887,5,4.181,5,8.375,5,9.3170000000000002,5,7.1379999999999999,5,12.92,5,29.23,5,55.56,5,61.78,5,40.81,5,85.77,5,91.66,5,194,5,185.2,5,340.3,5,403.4,5,373.9,5,548.29999999999995,5,686.6,5,741,5,798.1,5,967,5,1384,5,1499,5,1609,5,2070,5,2213]
[]
[]
[null,null,0.999999999999997,0.5,8.1989999999999998,1,null,0.5,14.61,0.5,28.48,0.5,45.02,0.5,48.13,0.5,41,0.5,61.98,0.5,103,0.5,149.80000000000001,0.5,159.19999999999999,0.5,161.5,0.5,263.7,0.5,244.4,0.5,387.5,0.5,420,0.5,599.6,0.5,610,0.5,636.4,0.5,812.3,0.5,874,0.5,924.2,0.5,1026,0.5,1300,0.5,1600,0.5,1858,0.5,1971,0.5,2255,0.5,2385]
[null,null,null,0.7,6.1980000000000004,0.8,null,0.6,12.79,0.6,25.95,0.6,42.87,0.6,46.38,0.6,38,0.6,59.65,0.6,99.69,0.6,147.19999999999999,0.6,156.4,0.6,155.80000000000001,0.6,257.10000000000002,0.6,240.6,0.6,380.9,0.6,414.6,0.6,594.4,0.6,604.6,0.6,629,0.6,795.7,0.6,870,0.6,923.8,0.6,1019,0.6,1278,0.6,1589,0.6,1843,0.6,1952,0.6,2255,0.6,2385]
[null,null,null,0.9,4.8650000000000002,0.6,null,0.7,11.35,0.7,23.99,0.7,40.28,0.7,43.57,0.7,35.64,0.7,56.89,0.7,96.98,0.7,145.30000000000001,0.7,154.4,0.7,149.19999999999999,0.7,250.5,0.7,235.2,0.7,375.6,0.7,410,0.7,592.1,0.7,600,0.7,626.9,0.7,782.4,0.7,860.3,0.7,913.5,0.7,1009,0.7,1260,0.7,1580,0.7,1833,0.7,1942,0.7,2255,0.7,2385]
[null,null,null,1.1000000000000001,4.0179999999999998,0.4,null,0.8,10.15,0.8,21.76,0.8,37.65,0.8,40.96,0.8,32.93,0.8,53.81,0.8,94.3,0.8,141.9,0.8,151.6,0.8,142.5,0.8,244,0.8,229.3,0.8,371.2,0.8,402.4,0.8,586.70000000000005,0.8,592.4,0.8,622.9,0.8,771.6,0.8,854.5,0.8,906.2,0.8,996.4,0.8,1241,0.8,1572,0.8,1811,0.8,1925,0.8,2245,0.8,2379]
[null,null,null,1.5,2.996,0.2,null,0.9,9.2070000000000007,0.9,19.97,0.9,35.450000000000003,0.9,38.57,0.9,30.69,0.9,51.24,0.9,92,0.9,139,0.9,148.5,0.9,135.30000000000001,0.9,238.4,0.9,223.5,0.9,367.5,0.9,395.8,0.9,581.79999999999995,0.9,585.79999999999995,0.9,617.70000000000005,0.9,762.2,0.9,849.6,0.9,900.9,0.9,985.1,0.9,1224,0.9,1566,0.9,1791,0.9,1904,0.9,2235,0.9,2368]
[null,null,null,2,2.2629999999999999,0.2,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J13","v":{"$error":"#NUM!"}},1,8.4079999999999995,1,18.489999999999998,1,33.49,1,36.549999999999997,1,28.31,1,48.83,1,89.98,1,136.30000000000001,1,145.69999999999999,1,127.6,1,232.7,1,217.9,1,363.3,1,390,1,576.9,1,580,1,613.1,1,752.5,1,844.7,1,896.3,1,975.2,1,1210,1,1560,1,1773,1,1886,1,2226,1,2359]
[null,null,null,2.5,1.7809999999999999,0.2,null,1.5,5.6970000000000001,1.5,13.2,1.5,24.76,1.5,27.43,1.5,19.84,1.5,36.89,1.5,75.98,1.5,123.6,1.5,133.6,1.5,99.33,1.5,196.4,1.5,193.1,1.5,333.6,1.5,360,1.5,543.1,1.5,560,1.5,580.70000000000005,1.5,698.1,1.5,813.2,1.5,684.1,1.5,932.8,1.5,1160,1.5,1500,1.5,1695,1.5,1803,1.5,2186,1.5,2324]
[null,null,null,2.9,1.546,0.15,null,2,4.3360000000000003,2,9.9979999999999993,2,19.489999999999998,2,21.59,2,15.2,2,28.7,2,63.99,2,109.6,2,118.7,2,79.42,2,166.7,2,168.3,2,310,2,326,2,513.1,2,530,2,548.6,2,660.2,2,793.2,2,842.9,2,894.8,2,1100,2,1460,2,1645,2,1749,2,2126,2,2260]
[null,null,null,3,1.498,0.15,null,2.5,3.5209999999999999,2.5,8.0860000000000003,2.5,15.83,2.5,17.670000000000002,2.5,12.41,2.5,23.35,2.5,52.71,2.5,96.92,2.5,106,2.5,66.62,2.5,142.30000000000001,2.5,146,2.5,284.7,2.5,287.8,2.5,479,2.5,501.9,2.5,516.4,2.5,619.70000000000005,2.5,764.5,2.5,817.1,2.5,854.3,2.5,1055,2.5,1415,2.5,1585,2.5,1694,2.5,2081,2.5,2213]
[null,null,null,3.5,1.298,0.15,null,3,2.8929999999999998,3,6.7990000000000004,3,13.29,3,14.82,3,10.5,3,19.7,3,44.99,3,85.47,3,94.88,3,56.7,3,122.8,3,126.6,3,259.10000000000002,3,260,3,443.9,3,480,3,484.3,3,587.5,3,735.8,3,788.8,3,826.3,3,1020,3,1380,3,1533,3,1638,3,2040,3,2175]
[null,null,null,4,1.1439999999999999,0.15,null,3.5,2.4630000000000001,3.5,5.8890000000000002,3.5,11.47,3.5,12.8,3.5,8.9480000000000004,3.5,17.170000000000002,3.5,39.020000000000003,3.5,74.760000000000005,3.5,82.99,3.5,49.31,3.5,108.5,3.5,111.6,3.5,235.9,3.5,233.1,3.5,407.3,3.5,452.5,3.5,444.4,3.5,560.29999999999995,3.5,708.6,3.5,759.7,3.5,800.1,3.5,976.3,3.5,1336,3.5,1489,3.5,1591,3.5,1997,3.5,2128]
[null,null,null,4.5,1.022,0.1,null,4,2.1680000000000001,4,5.1989999999999998,4,10.11,4,11.27,4,7.8339999999999996,4,15.27,4,34.5,4,66.569999999999993,4,73.900000000000006,4,43.58,4,97.64,4,98.54,4,214.9,4,212,4,378.1,4,427.7,4,412.5,4,535.79999999999995,4,685.9,4,735.3,4,772.3,4,940,4,1300,4,1453,4,1552,4,1960,4,2089]
[null,null,null,4.5999999999999996,1.0009999999999999,0.1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J14","v":{"$error":"#NUM!"}},4.5,1.9430000000000001,4.5,4.5570000000000004,4.5,9.0449999999999999,4.5,10.08,4.5,7.0049999999999999,4.5,13.51,4.5,30.9,4.5,59.89,4.5,66.69,4.5,39.01,4.5,87.79,4.5,88.02,4.5,195.6,4.5,192.2,4.5,350.7,4.5,402.8,4.5,385.9,4.5,511.2,4.5,660.7,4.5,713.8,4.5,741,4.5,907.8,4.5,1273,4.5,1413,4.5,1518,4.5,1920,4.5,2054]
[null,null,null,null,null,null,null,5,1.7609999999999999,5,4.05,5,8.1989999999999998,5,9.1340000000000003,5,6.3170000000000002,5,12.11,5,28,5,54.34,5,60.51,5,35.25,5,79.819999999999993,5,79.27,5,179.8,5,176,5,325.5,5,380,5,358.1,5,490.2,5,634.6,5,685.6,5,714,5,880,5,1250,5,1371,5,1473,5,1879,5,2010]
[]
[]
[null,null,1.2,0.5,7.109,1,null,0.5,13.42,0.5,26.44,0.5,41.47,0.5,44.38,0.5,35.229999999999997,0.5,55.3,0.5,93.28,0.5,136.80000000000001,0.5,145.6,0.5,135.6,0.5,234.4,0.5,205.1,0.5,343.5,0.5,378.5,0.5,546.4,0.5,551.9,0.5,580.4,0.5,720.8,0.5,792.1,0.5,838.3,0.5,906.5,0.5,1173,0.5,1440,0.5,1692,0.5,1796,0.5,2044,0.5,2163]
[null,null,null,0.6,6.1079999999999997,0.8,null,0.6,11.75,0.6,24.29,0.6,40.020000000000003,0.6,42.83,0.6,32.65,0.6,53.22,0.6,90.93,0.6,134.4,0.6,143.1,0.6,130.80000000000001,0.6,228.4,0.6,201.9,0.6,337.6,0.6,375.1,0.6,539.9,0.6,546,0.6,573.5,0.6,706.1,0.6,792.1,0.6,838.3,0.6,900.6,0.6,1158,0.6,1434,0.6,1675,0.6,1778,0.6,2044,0.6,2163]
[null,null,null,0.8,4.7389999999999999,0.6,null,0.7,10.49,0.7,22.45,0.7,37.770000000000003,0.7,40.9,0.7,30.62,0.7,51.36,0.7,88.47,0.7,132.6,0.7,141,0.7,125.4,0.7,223.4,0.7,197.5,0.7,332.7,0.7,370.9,0.7,537.6,0.7,541.9,0.7,569.70000000000005,0.7,693.9,0.7,784.5,0.7,833.6,0.7,894.8,0.7,1142,0.7,1426,0.7,1666,0.7,1767,0.7,2044,0.7,2163]
[null,null,null,0.9,4.2300000000000004,0.4,null,0.8,9.3840000000000003,0.8,20.71,0.8,35.61,0.8,38.74,0.8,28.4,0.8,48.58,0.8,86.23,0.8,130.6,0.8,139.4,0.8,119.7,0.8,217.6,0.8,192.5,0.8,328.9,0.8,366,0.8,534.9,0.8,537,0.8,568,0.8,684.4,0.8,777.7,0.8,825.6,0.8,883.3,0.8,1126,0.8,1419,0.8,1654,0.8,1759,0.8,2041,0.8,2163]
[null,null,null,1.3,2.98,0.2,null,0.9,8.5079999999999991,0.9,19,0.9,33.54,0.9,36.53,0.9,26.47,0.9,46.25,0.9,84.13,0.9,127.9,0.9,136.69999999999999,0.9,113.8,0.9,212.6,0.9,187.7,0.9,325.60000000000002,0.9,360,0.9,530.5,0.9,531,0.9,563.70000000000005,0.9,676,0.9,773.2,0.9,820.5,0.9,873.3,0.9,1111,0.9,1413,0.9,1636,0.9,1741,0.9,2032,0.9,2155]
[null,null,null,2,1.974,0.2,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J15","v":{"$error":"#NUM!"}},1,7.7939999999999996,1,17.600000000000001,1,31.78,1,34.619999999999997,1,24.56,1,44.26,1,82.29,1,125.5,1,134.19999999999999,1,107.3,1,208.2,1,183,1,322.60000000000002,1,354.7,1,526.5,1,525.70000000000005,1,559.4,1,668.7,1,769.2,1,816.3,1,864.4,1,1098,1,1407,1,1620,1,1724,1,2024,1,2146]
[null,null,null,2.5,1.5489999999999999,0.15,null,1.5,5.3,1.5,12.66,1.5,24.01,1.5,26.48,1.5,17.23,1.5,34.159999999999997,1.5,70.16,1.5,115.5,1.5,123.7,1.5,83.67,1.5,178.7,1.5,162.30000000000001,1.5,298.3,1.5,328.9,1.5,499.8,1.5,507.2,1.5,533.1,1.5,622,1.5,742.5,1.5,790.1,1.5,828.9,1.5,1052,1.5,1360,1.5,1550,1.5,1651,1.5,1995,1.5,2115]
[null,null,null,3,1.302,0.15,null,2,4.032,2,9.6869999999999994,2,18.940000000000001,2,21.01,2,13.2,2,26.61,2,60.28,2,102.9,2,111.5,2,66.95,2,152.19999999999999,2,141.69999999999999,2,278,2,301.2,2,472.8,2,483.9,2,506,2,589.6,2,724.1,2,770.1,2,796.4,2,1004,2,1323,2,1504,2,1601,2,1942,2,2067]
[null,null,null,3.5,1.127,0.15,null,2.5,3.2719999999999998,2.5,7.8259999999999996,2.5,15.56,2.5,17.39,2.5,10.76,2.5,21.69,2.5,50.7,2.5,92.36,2.5,101.1,2.5,56.14,2.5,130.6,2.5,122.9,2.5,256.5,2.5,270.3,2.5,446.9,2.5,460.1,2.5,482.3,2.5,555.20000000000005,2.5,704.1,2.5,753.3,2.5,762.1,2.5,963.1,2.5,1287,2.5,1459,2.5,1561,2.5,1901,2.5,2023]
[null,null,null,3.9,1.0189999999999999,0.1,null,3,2.7170000000000001,3,6.58,3,13.05,3,14.58,3,9.1449999999999996,3,18.309999999999999,3,43.27,3,82.83,3,90.68,3,47.87,3,113.5,3,106.7,3,235.7,3,244.2,3,419.6,3,440.1,3,452.9,3,526.70000000000005,3,679.9,3,727.4,3,735.8,3,930.9,3,1255,3,1411,3,1509,3,1869,3,1989]
[null,null,null,4.5,0.88829999999999998,0.1,null,3.5,2.2919999999999998,3.5,5.6909999999999998,3.5,11.26,3.5,12.58,3.5,7.7919999999999998,3.5,15.88,3.5,37.69,3.5,72.88,3.5,81.02,3.5,41.59,3.5,99.92,3.5,94.09,3.5,216.1,3.5,221.4,3.5,386.9,3.5,419.3,3.5,422.6,3.5,503,3.5,655.6,3.5,703.4,3.5,715.3,3.5,897.8,3.5,1222,3.5,1371,3.5,1466,3.5,1831,3.5,1953]
[null,null,null,4.7,0.85209999999999997,0.1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J16","v":{"$error":"#NUM!"}},4,2.0169999999999999,4,5.0250000000000004,4,9.92,4,11.08,4,6.81,4,14.18,4,33.32,4,64.900000000000006,4,72.150000000000006,4,36.76,4,90.18,4,83.11,4,197.4,4,201.4,4,359.1,4,398.4,4,392.2,4,481.9,4,634.5,4,680.9,4,692.2,4,864.4,4,1188,4,1337,4,1430,4,1798,4,1917]
[null,null,null,null,null,null,null,4.5,1.8049999999999999,4.5,4.468,4.5,8.8689999999999998,4.5,9.9060000000000006,4.5,6.0890000000000004,4.5,12.63,4.5,29.87,4.5,58.59,4.5,65.13,4.5,32.909999999999997,4.5,81.45,4.5,74.28,4.5,180.4,4.5,184.3,4.5,336.2,4.5,378.2,4.5,367.3,4.5,461,4.5,616.6,4.5,661.5,4.5,666.4,4.5,835.6,4.5,1161,4.5,1308,4.5,1399,4.5,1768,4.5,1886]
[null,null,null,null,null,null,null,5,1.6359999999999999,5,3.9710000000000001,5,8.0359999999999996,5,8.9659999999999993,5,5.4969999999999999,5,11.32,5,27.07,5,53.22,5,59.35,5,29.74,5,74.06,5,66.89,5,165.9,5,168.8,5,313.10000000000002,5,356.8,5,344.9,5,442,5,593.9,5,642.29999999999995,5,642.20000000000005,5,809.9,5,1140,5,1273,5,1369,5,1733,5,1855]
[]
[]
[]
[]
[]
[null,null,1.4,0.5,6.0510000000000002,0.8,null,0.5,12.32,0.5,24.74,0.5,38.64,0.5,41.23,0.5,30.04,0.5,49.73,0.5,85.54,0.5,126.6,0.5,134.6,0.5,112.8,0.5,210.1,0.5,171,0.5,307.5,0.5,345.7,0.5,504.4,0.5,505.7,0.5,535,0.5,645.79999999999995,0.5,728,0.5,771,0.5,809.6,0.5,1072,0.5,1313,0.5,1560,0.5,1657,0.5,1879,0.5,1990]
[null,null,null,0.7,4.5739999999999998,0.6,null,0.6,10.79,0.6,22.87,0.6,37.29,0.6,39.94,0.6,27.84,0.6,47.87,0.6,83.87,0.6,124.4,0.6,132.5,0.6,108.8,0.6,204.9,0.6,168.3,0.6,302.3,0.6,343.6,0.6,498.5,0.6,499.6,0.6,529.9,0.6,632.6,0.6,728,0.6,771,0.6,804.4,0.6,1063,0.6,1311,0.6,1546,0.6,1642,0.6,1879,0.6,1990]
[null,null,null,0.8,4.032,0.4,null,0.7,9.6440000000000001,0.7,21.14,0.7,35.71,0.7,38.71,0.7,26.11,0.7,46.34,0.7,81.599999999999994,0.7,122.6,0.7,130.5,0.7,103.9,0.7,200.5,0.7,164.3,0.7,297.89999999999998,0.7,339.9,0.7,494.8,0.7,495.8,0.7,524.79999999999995,0.7,621.6,0.7,724.6,0.7,770.7,0.7,800,0.7,1047,0.7,1303,0.7,1535,0.7,1629,0.7,1879,0.7,1990]
[null,null,null,1.1000000000000001,2.972,0.2,null,0.8,8.6509999999999998,0.8,19.739999999999998,0.8,33.82,0.8,36.67,0.8,24.2,0.8,44.05,0.8,79.680000000000007,0.8,121.2,0.8,129,0.8,99.19,0.8,195.6,0.8,160.1,0.8,294.39999999999998,0.8,336.6,0.8,493.4,0.8,492.6,0.8,523.29999999999995,0.8,612.9,0.8,717.6,0.8,763.3,0.8,790.8,0.8,1035,0.8,1297,0.8,1528,0.8,1621,0.8,1879,0.8,1990]
[null,null,null,1.5,2.2149999999999999,0.2,null,0.9,7.843,0.9,18.14,0.9,31.94,0.9,34.840000000000003,0.9,22.56,0.9,41.94,0.9,77.739999999999995,0.9,119,0.9,127.3,0.9,93.82,0.9,191.1,0.9,156,0.9,291.39999999999998,0.9,331.2,0.9,490,0.9,487.2,0.9,521.1,0.9,605.5,0.9,713,0.9,757.4,0.9,781.9,0.9,1021,0.9,1292,0.9,1514,0.9,1612,0.9,1872,0.9,1987]
[null,null,null,2,1.679,0.2,null,1,7.1849999999999996,1,16.8,1,30.27,1,33.01,1,20.91,1,40.14,1,76.040000000000006,1,116.8,1,125,1,88.46,1,187.1,1,152,1,288.7,1,326.39999999999998,1,486.3,1,482.3,1,517.20000000000005,1,598.9,1,709.4,1,753.4,1,774,1,1009,1,1287,1,1499,1,1596,1,1865,1,1979]
[null,null,null,2.2000000000000002,1.5089999999999999,0.15,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J17","v":{"$error":"#NUM!"}},1.5,4.9089999999999998,1.5,12.16,1.5,23.22,1.5,25.64,1.5,14.66,1.5,31.54,1.5,66.08,1.5,107.7,1.5,115.5,1.5,68.69,1.5,162.9,1.5,134.30000000000001,1.5,268.60000000000002,1.5,303.7,1.5,463.9,1.5,465.2,1.5,495.3,1.5,558.9,1.5,687,1.5,731.6,1.5,743.4,1.5,965.9,1.5,1248,1.5,1436,1.5,1530,1.5,1838,1.5,1950]
[null,null,null,2.5,1.3180000000000001,0.15,null,2,3.734,2,9.3819999999999997,2,18.45,2,20.49,2,11.24,2,24.56,2,57.06,2,97.37,2,105.6,2,54.79,2,138.80000000000001,2,116.8,2,250.4,2,270.7,2,440.5,2,446.7,2,471.9,2,529.79999999999995,2,669.6,2,712.7,2,714.3,2,926.2,2,1214,2,1392,2,1483,2,1797,2,1914]
[null,null,null,3,1.1080000000000001,0.15,null,2.5,3.0289999999999999,2.5,7.5739999999999998,2.5,15.29,2.5,17.02,2.5,9.1590000000000007,2.5,20.07,2.5,48.81,2.5,88.5,2.5,96.24,2.5,46.02,2.5,119.8,2.5,101,2.5,232.2,2.5,255.3,2.5,420.7,2.5,426.1,2.5,451.6,2.5,500.8,2.5,655.8,2.5,699.1,2.5,685.4,2.5,888.7,2.5,1184,2.5,1359,2.5,1449,2.5,1759,2.5,1873]
[null,null,null,3.3,1.0129999999999999,0.1,null,3,2.5339999999999998,3,6.3680000000000003,3,12.82,3,14.36,3,7.7789999999999999,3,16.95,3,41.66,3,79.37,3,86.99,3,39.07,3,104.7,3,87.38,3,214.9,3,230.6,3,395.1,3,407.5,3,426.8,3,475.3,3,633.29999999999995,3,678.2,3,660.9,3,859,3,1155,3,1314,3,1406,3,1729,3,1841]
[null,null,null,4,0.84609999999999996,0.1,null,3.5,2.1320000000000001,3.5,5.5010000000000003,3.5,11.06,3.5,12.37,3.5,6.6280000000000001,3.5,14.68,3.5,36.409999999999997,3.5,71.16,3.5,79.23,3.5,33.96,3.5,92.03,3.5,76.819999999999993,3.5,197.3,3.5,211.1,3.5,369.7,3.5,391.7,3.5,404.3,3.5,454.1,3.5,612.9,3.5,658.3,3.5,643.20000000000005,3.5,833.5,3.5,1129,3.5,1277,3.5,1367,3.5,1699,3.5,1814]
[null,null,null,4.5,0.75590000000000002,0.1,null,4,1.869,4,4.8570000000000002,4,9.7430000000000003,4,10.9,4,5.7939999999999996,4,13.08,4,32.19,4,63.37,4,70.55,4,30.01,4,82.93,4,67.86,4,180.9,4,192,4,343.1,4,372.2,4,375.2,4,435.4,4,593.20000000000005,4,637.1,4,623.4,4,802.5,4,1098,4,1245,4,1333,4,1668,4,1781]
[null,null,null,4.7,0.72509999999999997,0.1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J18","v":{"$error":"#NUM!"}},4.5,1.671,4.5,4.3520000000000003,4.5,8.7100000000000009,4.5,9.7439999999999998,4.5,5.181,4.5,11.74,4.5,28.87,4.5,57.21,4.5,63.69,4.5,26.85,4.5,75.3,4.5,60.54,4.5,166.1,4.5,176.6,4.5,321.3,4.5,355.8,4.5,351.4,4.5,417.7,4.5,576.4,4.5,619.1,4.5,602.70000000000005,4.5,776.1,4.5,1072,4.5,1218,4.5,1304,4.5,1641,4.5,1752]
[null,null,null,null,null,null,null,5,1.5149999999999999,5,3.883,5,7.8819999999999997,5,8.8140000000000001,5,4.6760000000000002,5,10.52,5,26.17,5,52.17,5,58.12,5,24.26,5,68.47,5,54.52,5,152.69999999999999,5,162.19999999999999,5,302.3,5,336.8,5,331.3,5,400.6,5,560.6,5,603.29999999999995,5,580.79999999999995,5,752.5,5,1051,5,1193,5,1279,5,1616,5,1727]
[]
[]
[null,null,1.49999999999999,0.5,5.5309999999999997,0.8,null,0.5,11.75,0.5,23.98,0.5,37.36,0.5,39.840000000000003,0.5,27.59,0.5,47.22,0.5,82.21,0.5,122.1,0.5,129.80000000000001,0.5,102.1,0.5,199.2,0.5,155.19999999999999,0.5,291.5,0.5,331.7,0.5,486.1,0.5,485.8,0.5,515.4,0.5,612.5,0.5,700.7,0.5,742.4,0.5,767.3,0.5,1029,0.5,1259,0.5,1504,0.5,1597,0.5,1808,0.5,1916]
[null,null,null,0.6,4.7530000000000001,0.6,null,0.6,10.33,0.6,22.23,0.6,36.11,0.6,38.69,0.6,25.57,0.6,45.48,0.6,80.8,0.6,120.1,0.6,128,0.6,98.45,0.6,194.5,0.6,152.80000000000001,0.6,286.7,0.6,330.1,0.6,480.4,0.6,479.6,0.6,511.3,0.6,600.20000000000005,0.6,700.7,0.6,742.4,0.6,762.3,0.6,1021,0.6,1258,0.6,1490,0.6,1584,0.6,1808,0.6,1916]
[null,null,null,0.7,4.181,0.4,null,0.7,9.2330000000000005,0.7,20.55,0.7,34.799999999999997,0.7,37.549999999999997,0.7,23.98,0.7,44.03,0.7,78.61,0.7,118.3,0.7,126,0.7,93.64,0.7,190.3,0.7,148.69999999999999,0.7,282.5,0.7,326.5,0.7,476.6,0.7,476,0.7,506.2,0.7,589.79999999999995,0.7,699.1,0.7,742.4,0.7,758.1,0.7,1007,0.7,1251,0.7,1479,0.7,1571,0.7,1808,0.7,1916]
[null,null,null,1,2.9,0.2,null,0.8,8.2949999999999999,0.8,19.190000000000001,0.8,32.97,0.8,35.76,0.8,22.18,0.8,41.98,0.8,76.760000000000005,0.8,117,0.8,124.6,0.8,89.43,0.8,185.8,0.8,144.9,0.8,279.2,0.8,323.39999999999998,0.8,475.3,0.8,472.9,0.8,504.2,0.8,581.4,0.8,692.3,0.8,736.6,0.8,750.1,0.8,994.4,0.8,1245,0.8,1472,0.8,1563,0.8,1808,0.8,1916]
[null,null,null,1.5,2.0219999999999998,0.2,null,0.9,7.5209999999999999,0.9,17.739999999999998,0.9,31.23,0.9,34.08,0.9,20.67,0.9,39.97,0.9,74.959999999999994,0.9,115.2,0.9,123.3,0.9,84.12,0.9,181.5,0.9,141,0.9,276.39999999999998,0.9,318.8,0.9,472.6,0.9,468.3,0.9,502.9,0.9,574.4,0.9,687.4,0.9,730.4,0.9,741.7,0.9,981.8,0.9,1239,0.9,1461,0.9,1556,0.9,1804,0.9,1916]
[null,null,null,2,1.5289999999999999,0.15,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J19","v":{"$error":"#NUM!"}},1,6.89,1,16.420000000000002,1,29.59,1,32.299999999999997,1,19.100000000000001,1,38.25,1,73.319999999999993,1,113,1,121,1,79.319999999999993,1,177.8,1,137.4,1,273.8,1,314.10000000000002,1,469.1,1,463.6,1,499.1,1,568.1,1,683.8,1,726.6,1,734.1,1,970.2,1,1235,1,1447,1,1541,1,1797,1,1908]
[null,null,null,2.5,1.2030000000000001,0.15,null,1.5,4.7160000000000002,1.5,11.92,1.5,22.86,1.5,25.26,1.5,13.39,1.5,30.26,1.5,64.069999999999993,1.5,104.4,1.5,111.9,1.5,61.35,1.5,155.6,1.5,121,1.5,255.3,1.5,292.7,1.5,448.4,1.5,447,1.5,479,1.5,530.79999999999995,1.5,663.2,1.5,706.5,1.5,705.6,1.5,928.6,1.5,1199,1.5,1387,1.5,1479,1.5,1771,1.5,1880]
[null,null,null,3,1.0109999999999999,0.1,null,2,3.5870000000000002,2,9.2319999999999993,2,18.22,2,20.25,2,10.26,2,23.57,2,55.59,2,94.93,2,103,2,48.78,2,132.5,2,104.7,2,238,2,271.60000000000002,2,426.6,2,430.5,2,457.2,2,503.2,2,646.20000000000005,2,688.1,2,677.9,2,892.4,2,1167,2,1344,2,1433,2,1735,2,1849]
[null,null,null,3.5,0.87590000000000001,0.1,null,2.5,2.9089999999999998,2.5,7.45,2.5,15.13,2.5,16.82,2.5,8.3710000000000004,2.5,19.27,2.5,47.9,2.5,86.5,2.5,90.06,2.5,40.93,2.5,114.6,2.5,90.07,2.5,221.2,2.5,248.4,2.5,408.2,2.5,411.2,2.5,437.5,2.5,476.3,2.5,633.79999999999995,2.5,674.9,2.5,651.20000000000005,2.5,856.3,2.5,1140,2.5,1313,2.5,1400,2.5,1698,2.5,1809]
[null,null,null,4,0.7722,0.1,null,3,2.44,3,6.2640000000000002,3,12.72,3,14.25,3,7.0940000000000003,3,16.28,3,40.89,3,77.81,3,85.34,3,34.72,3,100.4,3,77.86,3,205.3,3,224.4,3,384.3,3,393.3,3,415.4,3,452.2,3,613.20000000000005,3,656.9,3,627.6,3,827.8,3,1111,3,1272,3,1362,3,1669,3,1778]
[null,null,null,4.5,0.68989999999999996,0.1,null,3.5,2.0529999999999999,3.5,5.41,3.5,10.96,3.5,12.28,3.5,6.0439999999999996,3.5,14.09,3.5,35.76,3.5,70.349999999999994,3.5,77.84,3.5,30.16,3.5,88.25,3.5,68.23,3.5,188.5,3.5,205.9,3.5,362,3.5,378.8,3.5,393.9,3.5,432,3.5,594.29999999999995,3.5,637.79999999999995,3.5,610.79999999999995,3.5,804.3,3.5,1088,3.5,1236,3.5,1324,3.5,1643,3.5,1753]
[null,null,null,4.7,0.66180000000000005,0.1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!J20","v":{"$error":"#NUM!"}},4,1.7949999999999999,4,4.7750000000000004,4,9.6560000000000006,4,10.81,4,5.2889999999999997,4,12.54,4,31.64,4,62.65,4,69.8,4,26.66,4,79.44,4,60.27,4,173,4,187.6,4,336,4,360.5,4,367.7,4,414.3,4,575.29999999999995,4,618.20000000000005,4,592.6,4,775.3,4,1059,4,1205,4,1291,4,1613,4,1722]
[null,null,null,null,null,null,null,4.5,1.605,4.5,4.2789999999999999,4.5,8.6329999999999991,4.5,9.6649999999999991,4.5,4.7290000000000001,4.5,11.29,4.5,28.38,4.5,56.56,4.5,63.01,4.5,23.82,4.5,72.28,4.5,53.68,4.5,159.19999999999999,4.5,172.6,4.5,314.60000000000002,4.5,344.6,4.5,344.3,4.5,398,4.5,558.9,4.5,600.70000000000005,4.5,573.9,4.5,749.8,4.5,1033,4.5,1179,4.5,1263,4.5,1586,4.5,1694]
[null,null,null,null,null,null,null,5,1.45,5,3.8370000000000002,5,7.81,5,8.7430000000000003,5,4.266,5,10.119999999999999,5,25.73,5,51.61,5,57.5,5,21.53,5,65.72,5,48.34,5,146.4,5,159,5,296.60000000000002,5,327.8,5,324.60000000000002,5,381.6,5,544.70000000000005,5,585.4,5,553,5,727.2,5,1013,5,1156,5,1239,5,1563,5,1670]

{"sheet":"10A61 Liquid 3\" ViscosityLINEST","index":2,"n_rows":452,"n_cols":10,"rows_kept":452,"cut":false,"hidden":true,"merged":[[0,1,0,2],[1,1,1,7],[3,1,3,7]]}
[]
[]
[]
["SG","LINEST",null,null,null,null,null,null,"ORDER","MAX FLOW"]
[]
["1/8-08-BG"]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!E6:E10,'10A61 Liquid 3\"'!D6:D10^{1,2,3,4})","v":7.3404761904759601},-37.979047619046582,75.571166666664908,-72.192809523808251,33.462214285713998,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B7:H7)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B7*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I7+'10A61 Liquid 3\" ViscosityLINEST'!C7*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I7-1)+'10A61 Liquid 3\" ViscosityLINEST'!D7*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I7-2)+'10A61 Liquid 3\" ViscosityLINEST'!E7*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I7-3)+'10A61 Liquid 3\" ViscosityLINEST'!F7*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I7-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E10:E14,'10A61 Liquid 3\"'!D10:D14^{1,2,3,4})","v":0.15787802840434179},-1.8369022556390788,8.1948713450292026,-17.318285714285722,17.129255639097789,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B8:H8)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B8*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I8+'10A61 Liquid 3\" ViscosityLINEST'!C8*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I8-1)+'10A61 Liquid 3\" ViscosityLINEST'!D8*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I8-2)+'10A61 Liquid 3\" ViscosityLINEST'!E8*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I8-3)+'10A61 Liquid 3\" ViscosityLINEST'!F8*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I8-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!E23:E28,'10A61 Liquid 3\"'!D23:D28^{1,2,3,4})","v":2.3857402257892892},-15.135437235303087,36.946890381537138,-43.404275008143259,24.781472587349548,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B9:H9)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B9*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I9+'10A61 Liquid 3\" ViscosityLINEST'!C9*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I9-1)+'10A61 Liquid 3\" ViscosityLINEST'!D9*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I9-2)+'10A61 Liquid 3\" ViscosityLINEST'!E9*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I9-3)+'10A61 Liquid 3\" ViscosityLINEST'!F9*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I9-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E28:E32,'10A61 Liquid 3\"'!D28:D32^{1,2,3,4})","v":4.7528933055248031E-2},-0.66950660450657928,3.6402633930395218,-9.482662669201634,11.817452214451762,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B10*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I10+'10A61 Liquid 3\" ViscosityLINEST'!C10*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I10-1)+'10A61 Liquid 3\" ViscosityLINEST'!D10*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I10-2)+'10A61 Liquid 3\" ViscosityLINEST'!E10*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I10-3)+'10A61 Liquid 3\" ViscosityLINEST'!F10*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I10-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!E41:E47,'10A61 Liquid 3\"'!D41:D47^{1,2,3,4})","v":1.8627805217714601},-12.184154489985387,30.541113205881512,-36.7075042371671,21.461014956228365,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B11:H11)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B11*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I11+'10A61 Liquid 3\" ViscosityLINEST'!C11*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I11-1)+'10A61 Liquid 3\" ViscosityLINEST'!D11*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I11-2)+'10A61 Liquid 3\" ViscosityLINEST'!E11*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I11-3)+'10A61 Liquid 3\" ViscosityLINEST'!F11*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I11-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E47:E52,'10A61 Liquid 3\"'!D47:D52^{1,2,3,4})","v":3.4241786480434092E-2},-0.51487447212889426,2.9719372339678838,-8.1474256100966862,10.519080542258941,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B12*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I12+'10A61 Liquid 3\" ViscosityLINEST'!C12*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I12-1)+'10A61 Liquid 3\" ViscosityLINEST'!D12*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I12-2)+'10A61 Liquid 3\" ViscosityLINEST'!E12*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I12-3)+'10A61 Liquid 3\" ViscosityLINEST'!F12*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I12-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!E57:E62,'10A61 Liquid 3\"'!D57:D62^{1,2,3,4})","v":1.4194453789938961},-9.4071041858310007,24.149744759184969,-30.02696143339514,18.263551709968993,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B13*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I13+'10A61 Liquid 3\" ViscosityLINEST'!C13*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I13-1)+'10A61 Liquid 3\" ViscosityLINEST'!D13*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I13-2)+'10A61 Liquid 3\" ViscosityLINEST'!E13*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I13-3)+'10A61 Liquid 3\" ViscosityLINEST'!F13*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I13-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E62:E69,'10A61 Liquid 3\"'!D62:D69^{1,2,3,4})","v":3.2180070420798276E-2},-0.48874746765629223,2.8354515818404105,-7.7489290447954922,9.8136974912677069,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B14*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I14+'10A61 Liquid 3\" ViscosityLINEST'!C14*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I14-1)+'10A61 Liquid 3\" ViscosityLINEST'!D14*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I14-2)+'10A61 Liquid 3\" ViscosityLINEST'!E14*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I14-3)+'10A61 Liquid 3\" ViscosityLINEST'!F14*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I14-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!E73:E78,'10A61 Liquid 3\"'!D73:D78^{1,2,3,4})","v":2.5050068251118729},-14.082139311524559,30.467164075572693,-32.273440031228404,17.229254129272498,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B15:H15)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B15*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I15+'10A61 Liquid 3\" ViscosityLINEST'!C15*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I15-1)+'10A61 Liquid 3\" ViscosityLINEST'!D15*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I15-2)+'10A61 Liquid 3\" ViscosityLINEST'!E15*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I15-3)+'10A61 Liquid 3\" ViscosityLINEST'!F15*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I15-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E78:E84,'10A61 Liquid 3\"'!D78:D84^{1,2,3,4})","v":2.4764226746506184E-2},-0.38616187497527216,2.2994442475878043,-6.4450343782526245,8.358831358901174,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B16*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I16+'10A61 Liquid 3\" ViscosityLINEST'!C16*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I16-1)+'10A61 Liquid 3\" ViscosityLINEST'!D16*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I16-2)+'10A61 Liquid 3\" ViscosityLINEST'!E16*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I16-3)+'10A61 Liquid 3\" ViscosityLINEST'!F16*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I16-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!E92:E98,'10A61 Liquid 3\"'!D92:D98^{1,2,3,4})","v":0.79543048681950312},-5.7371933744741819,15.809320511304788,-20.771670649396096,13.148824897907279,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B17:H17)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B17*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I17+'10A61 Liquid 3\" ViscosityLINEST'!C17*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I17-1)+'10A61 Liquid 3\" ViscosityLINEST'!D17*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I17-2)+'10A61 Liquid 3\" ViscosityLINEST'!E17*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I17-3)+'10A61 Liquid 3\" ViscosityLINEST'!F17*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I17-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E98:E104,'10A61 Liquid 3\"'!D98:D104^{1,2,3,4})","v":1.9248042539319801E-2},-0.30180537587628065,1.8107598873488149,-5.1354846321305621,6.8050500135867686,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B18*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I18+'10A61 Liquid 3\" ViscosityLINEST'!C18*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I18-1)+'10A61 Liquid 3\" ViscosityLINEST'!D18*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I18-2)+'10A61 Liquid 3\" ViscosityLINEST'!E18*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I18-3)+'10A61 Liquid 3\" ViscosityLINEST'!F18*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I18-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!E108:E113,'10A61 Liquid 3\"'!D108:D113^{1,2,3,4})","v":0.33160512828898009},-3.4502126673886879,11.748098728480389,-17.442110340578935,11.716940017823802,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B19*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I19+'10A61 Liquid 3\" ViscosityLINEST'!C19*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I19-1)+'10A61 Liquid 3\" ViscosityLINEST'!D19*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I19-2)+'10A61 Liquid 3\" ViscosityLINEST'!E19*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I19-3)+'10A61 Liquid 3\" ViscosityLINEST'!F19*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I19-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!E113:E119,'10A61 Liquid 3\"'!D113:D119^{1,2,3,4})","v":1.8607985650509855E-2},-0.29051618702762849,1.7333412275460356,-4.8763786808830618,6.374463220120921,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B20*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I20+'10A61 Liquid 3\" ViscosityLINEST'!C20*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I20-1)+'10A61 Liquid 3\" ViscosityLINEST'!D20*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I20-2)+'10A61 Liquid 3\" ViscosityLINEST'!E20*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I20-3)+'10A61 Liquid 3\" ViscosityLINEST'!F20*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I20-4)","v":{"$error":"#NUM!"}}]
[]
["1/8-08-SA"]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!I6:I11,'10A61 Liquid 3\"'!H6:H11^{1,2,3,4})","v":56.249999999987338},-183.2870370370006,238.14583333329489,-159.78677248675484,58.930079365076388,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B23*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I23+'10A61 Liquid 3\" ViscosityLINEST'!C23*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I23-1)+'10A61 Liquid 3\" ViscosityLINEST'!D23*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I23-2)+'10A61 Liquid 3\" ViscosityLINEST'!E23*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I23-3)+'10A61 Liquid 3\" ViscosityLINEST'!F23*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I23-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I11:I18,'10A61 Liquid 3\"'!H11:H18^{1,2,3,4})","v":0.10586363636364292},-1.4885606060606815,7.9737007575760614,-20.140419372294872,23.786434523809806,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B24*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I24+'10A61 Liquid 3\" ViscosityLINEST'!C24*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I24-1)+'10A61 Liquid 3\" ViscosityLINEST'!D24*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I24-2)+'10A61 Liquid 3\" ViscosityLINEST'!E24*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I24-3)+'10A61 Liquid 3\" ViscosityLINEST'!F24*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I24-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!I23:I28,'10A61 Liquid 3\"'!H23:H28^{1,2,3,4})","v":41.87499999999995},-147.24537037037177,202.9270833333367,-140.95343915344165,52.995579365079941,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B25*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I25+'10A61 Liquid 3\" ViscosityLINEST'!C25*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I25-1)+'10A61 Liquid 3\" ViscosityLINEST'!D25*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I25-2)+'10A61 Liquid 3\" ViscosityLINEST'!E25*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I25-3)+'10A61 Liquid 3\" ViscosityLINEST'!F25*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I25-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I28:I36,'10A61 Liquid 3\"'!H28:H36^{1,2,3,4})","v":7.5379953379950515E-2},-1.1318793058792689,6.4416398601396896,-17.203272597772276,21.384222222222029,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B26*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I26+'10A61 Liquid 3\" ViscosityLINEST'!C26*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I26-1)+'10A61 Liquid 3\" ViscosityLINEST'!D26*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I26-2)+'10A61 Liquid 3\" ViscosityLINEST'!E26*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I26-3)+'10A61 Liquid 3\" ViscosityLINEST'!F26*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I26-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!I41:I46,'10A61 Liquid 3\"'!H41:H46^{1,2,3,4})","v":-60.624999999990379},167.55092592589767,-154.4645833333029,38.286455026440763,18.248658730161171,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B27*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I27+'10A61 Liquid 3\" ViscosityLINEST'!C27*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I27-1)+'10A61 Liquid 3\" ViscosityLINEST'!D27*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I27-2)+'10A61 Liquid 3\" ViscosityLINEST'!E27*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I27-3)+'10A61 Liquid 3\" ViscosityLINEST'!F27*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I27-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I46:I54,'10A61 Liquid 3\"'!H46:H54^{1,2,3,4})","v":7.5701631701628691E-2},-1.1182242942242546,6.2560745920744099,-16.443277259776917,20.190388888888673,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B28*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I28+'10A61 Liquid 3\" ViscosityLINEST'!C28*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I28-1)+'10A61 Liquid 3\" ViscosityLINEST'!D28*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I28-2)+'10A61 Liquid 3\" ViscosityLINEST'!E28*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I28-3)+'10A61 Liquid 3\" ViscosityLINEST'!F28*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I28-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!I57:I62,'10A61 Liquid 3\"'!H57:H62^{1,2,3,4})","v":5.6249999999954632},-27.328703703690636,54.789583333319541,-57.305462962956639,32.62872222222115,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B29*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I29+'10A61 Liquid 3\" ViscosityLINEST'!C29*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I29-1)+'10A61 Liquid 3\" ViscosityLINEST'!D29*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I29-2)+'10A61 Liquid 3\" ViscosityLINEST'!E29*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I29-3)+'10A61 Liquid 3\" ViscosityLINEST'!F29*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I29-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I62:I70,'10A61 Liquid 3\"'!H62:H70^{1,2,3,4})","v":7.6046620046617303E-2},-1.1083439523439158,6.1042610722609041,-15.777217042216726,19.079888888888689,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B30*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I30+'10A61 Liquid 3\" ViscosityLINEST'!C30*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I30-1)+'10A61 Liquid 3\" ViscosityLINEST'!D30*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I30-2)+'10A61 Liquid 3\" ViscosityLINEST'!E30*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I30-3)+'10A61 Liquid 3\" ViscosityLINEST'!F30*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I30-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!I73:I78,'10A61 Liquid 3\"'!H73:H78^{1,2,3,4})","v":39.166666666657036},-126.87037037034253,161.89166666663715,-105.49629629628269,39.104222222219917,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B31*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I31+'10A61 Liquid 3\" ViscosityLINEST'!C31*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I31-1)+'10A61 Liquid 3\" ViscosityLINEST'!D31*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I31-2)+'10A61 Liquid 3\" ViscosityLINEST'!E31*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I31-3)+'10A61 Liquid 3\" ViscosityLINEST'!F31*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I31-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I78:I86,'10A61 Liquid 3\"'!H78:H86^{1,2,3,4})","v":7.1132867132864541E-2},-1.03360787360784,5.673277389277235,-14.621128334628045,17.675944444444266,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B32*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I32+'10A61 Liquid 3\" ViscosityLINEST'!C32*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I32-1)+'10A61 Liquid 3\" ViscosityLINEST'!D32*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I32-2)+'10A61 Liquid 3\" ViscosityLINEST'!E32*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I32-3)+'10A61 Liquid 3\" ViscosityLINEST'!F32*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I32-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!I92:I97,'10A61 Liquid 3\"'!H92:H97^{1,2,3,4})","v":40.833333333325648},-132.44444444442257,167.61666666664388,-106.47448412697381,37.655238095236371,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B33*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I33+'10A61 Liquid 3\" ViscosityLINEST'!C33*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I33-1)+'10A61 Liquid 3\" ViscosityLINEST'!D33*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I33-2)+'10A61 Liquid 3\" ViscosityLINEST'!E33*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I33-3)+'10A61 Liquid 3\" ViscosityLINEST'!F33*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I33-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I97:I105,'10A61 Liquid 3\"'!H97:H105^{1,2,3,4})","v":6.5491841491838995E-2},-0.95018492618489381,5.2068088578087091,-13.408378010877732,16.247833333333169,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B34*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I34+'10A61 Liquid 3\" ViscosityLINEST'!C34*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I34-1)+'10A61 Liquid 3\" ViscosityLINEST'!D34*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I34-2)+'10A61 Liquid 3\" ViscosityLINEST'!E34*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I34-3)+'10A61 Liquid 3\" ViscosityLINEST'!F34*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I34-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!I108:I113,'10A61 Liquid 3\"'!H108:H113^{1,2,3,4})","v":29.791666666661627},-97.569444444430204,126.31458333331867,-84.301626984120446,32.655595238094172,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B35*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I35+'10A61 Liquid 3\" ViscosityLINEST'!C35*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I35-1)+'10A61 Liquid 3\" ViscosityLINEST'!D35*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I35-2)+'10A61 Liquid 3\" ViscosityLINEST'!E35*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I35-3)+'10A61 Liquid 3\" ViscosityLINEST'!F35*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I35-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!I113:I121,'10A61 Liquid 3\"'!H113:H121^{1,2,3,4})","v":6.2447552447550167E-2},-0.90683190883187881,4.9724790209788825,-12.814670810670549,15.555055555555393,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B36*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I36+'10A61 Liquid 3\" ViscosityLINEST'!C36*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I36-1)+'10A61 Liquid 3\" ViscosityLINEST'!D36*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I36-2)+'10A61 Liquid 3\" ViscosityLINEST'!E36*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I36-3)+'10A61 Liquid 3\" ViscosityLINEST'!F36*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I36-4)","v":{"$error":"#NUM!"}}]
[]
["1/8-08-SS"]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!K6:K11,'10A61 Liquid 3\"'!J6:J11^{1,2,3,4})","v":35.416666666657811},-132.82407407404926,209.18749999997465,-179.25568783067661,88.968015873014053,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B39*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I39+'10A61 Liquid 3\" ViscosityLINEST'!C39*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I39-1)+'10A61 Liquid 3\" ViscosityLINEST'!D39*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I39-2)+'10A61 Liquid 3\" ViscosityLINEST'!E39*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I39-3)+'10A61 Liquid 3\" ViscosityLINEST'!F39*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I39-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K11:K19,'10A61 Liquid 3\"'!J11:J19^{1,2,3,4})","v":0.18941258741257988},-2.783004921004824,15.42825291375247,-40.078051800050964,48.646277777777264,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B40*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I40+'10A61 Liquid 3\" ViscosityLINEST'!C40*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I40-1)+'10A61 Liquid 3\" ViscosityLINEST'!D40*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I40-2)+'10A61 Liquid 3\" ViscosityLINEST'!E40*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I40-3)+'10A61 Liquid 3\" ViscosityLINEST'!F40*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I40-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!K23:K28,'10A61 Liquid 3\"'!J23:J28^{1,2,3,4})","v":-47.916666666647693},137.17592592586962,-122.47916666660531,6.7800264549973992,46.74373015873519,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B41*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I41+'10A61 Liquid 3\" ViscosityLINEST'!C41*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I41-1)+'10A61 Liquid 3\" ViscosityLINEST'!D41*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I41-2)+'10A61 Liquid 3\" ViscosityLINEST'!E41*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I41-3)+'10A61 Liquid 3\" ViscosityLINEST'!F41*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I41-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K28:K36,'10A61 Liquid 3\"'!J28:J36^{1,2,3,4})","v":0.17680186480185761},-2.5758715358714439,14.185344988344573,-36.814804843304074,45.293055555555085,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B42*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I42+'10A61 Liquid 3\" ViscosityLINEST'!C42*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I42-1)+'10A61 Liquid 3\" ViscosityLINEST'!D42*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I42-2)+'10A61 Liquid 3\" ViscosityLINEST'!E42*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I42-3)+'10A61 Liquid 3\" ViscosityLINEST'!F42*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I42-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!K41:K46,'10A61 Liquid 3\"'!J41:J46^{1,2,3,4})","v":-122.91666666665486},375.87962962959642,-408.31249999996578,162.35370370368841,12.327222222224719,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B43*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I43+'10A61 Liquid 3\" ViscosityLINEST'!C43*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I43-1)+'10A61 Liquid 3\" ViscosityLINEST'!D43*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I43-2)+'10A61 Liquid 3\" ViscosityLINEST'!E43*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I43-3)+'10A61 Liquid 3\" ViscosityLINEST'!F43*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I43-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K46:K54,'10A61 Liquid 3\"'!J46:J54^{1,2,3,4})","v":0.14390209790209174},-2.1527174307173516,12.201842657342295,-32.703063066562386,41.818777777777385,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B44*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I44+'10A61 Liquid 3\" ViscosityLINEST'!C44*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I44-1)+'10A61 Liquid 3\" ViscosityLINEST'!D44*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I44-2)+'10A61 Liquid 3\" ViscosityLINEST'!E44*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I44-3)+'10A61 Liquid 3\" ViscosityLINEST'!F44*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I44-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!K57:K62,'10A61 Liquid 3\"'!J57:J62^{1,2,3,4})","v":147.91666666662456},-436.06481481469143,482.47916666653401,-257.89113756607554,82.059603174592553,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B45*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I45+'10A61 Liquid 3\" ViscosityLINEST'!C45*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I45-1)+'10A61 Liquid 3\" ViscosityLINEST'!D45*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I45-2)+'10A61 Liquid 3\" ViscosityLINEST'!E45*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I45-3)+'10A61 Liquid 3\" ViscosityLINEST'!F45*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I45-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K62:K70,'10A61 Liquid 3\"'!J62:J70^{1,2,3,4})","v":0.11027039627039074},-1.7239114219113509,10.234493006992682,-28.771385780885172,38.626333333332965,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B46*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I46+'10A61 Liquid 3\" ViscosityLINEST'!C46*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I46-1)+'10A61 Liquid 3\" ViscosityLINEST'!D46*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I46-2)+'10A61 Liquid 3\" ViscosityLINEST'!E46*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I46-3)+'10A61 Liquid 3\" ViscosityLINEST'!F46*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I46-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!K73:K78,'10A61 Liquid 3\"'!J73:J78^{1,2,3,4})","v":102.08333333332415},-308.19444444441922,349.60416666664156,-194.15555555554479,68.261666666664993,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B47*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I47+'10A61 Liquid 3\" ViscosityLINEST'!C47*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I47-1)+'10A61 Liquid 3\" ViscosityLINEST'!D47*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I47-2)+'10A61 Liquid 3\" ViscosityLINEST'!E47*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I47-3)+'10A61 Liquid 3\" ViscosityLINEST'!F47*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I47-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K78:K86,'10A61 Liquid 3\"'!J78:J86^{1,2,3,4})","v":9.5883449883445618E-2},-1.5118202538201981,9.0946048951046379,-26.056666148665666,35.957388888888595,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B48*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I48+'10A61 Liquid 3\" ViscosityLINEST'!C48*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I48-1)+'10A61 Liquid 3\" ViscosityLINEST'!D48*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I48-2)+'10A61 Liquid 3\" ViscosityLINEST'!E48*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I48-3)+'10A61 Liquid 3\" ViscosityLINEST'!F48*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I48-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!K92:K97,'10A61 Liquid 3\"'!J92:J97^{1,2,3,4})","v":56.250000000009749},-177.91666666669738,212.31250000003547,-128.49047619049395,54.637857142860383,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B49*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I49+'10A61 Liquid 3\" ViscosityLINEST'!C49*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I49-1)+'10A61 Liquid 3\" ViscosityLINEST'!D49*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I49-2)+'10A61 Liquid 3\" ViscosityLINEST'!E49*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I49-3)+'10A61 Liquid 3\" ViscosityLINEST'!F49*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I49-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K97:K105,'10A61 Liquid 3\"'!J97:J105^{1,2,3,4})","v":8.615384615384214E-2},-1.3617922817922286,8.2506736596734118,-23.946657990157522,33.747388888888608,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B50*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I50+'10A61 Liquid 3\" ViscosityLINEST'!C50*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I50-1)+'10A61 Liquid 3\" ViscosityLINEST'!D50*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I50-2)+'10A61 Liquid 3\" ViscosityLINEST'!E50*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I50-3)+'10A61 Liquid 3\" ViscosityLINEST'!F50*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I50-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!K108:K113,'10A61 Liquid 3\"'!J108:J113^{1,2,3,4})","v":-6.2499999999834888},10.138888888839141,4.1875000000551017,-27.446031746058296,35.784523809528501,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B51*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I51+'10A61 Liquid 3\" ViscosityLINEST'!C51*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I51-1)+'10A61 Liquid 3\" ViscosityLINEST'!D51*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I51-2)+'10A61 Liquid 3\" ViscosityLINEST'!E51*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I51-3)+'10A61 Liquid 3\" ViscosityLINEST'!F51*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I51-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!K113:K121,'10A61 Liquid 3\"'!J113:J121^{1,2,3,4})","v":8.3142191142187419E-2},-1.3099891219890734,7.9311841491839221,-23.082487567987133,32.773499999999736,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B52*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I52+'10A61 Liquid 3\" ViscosityLINEST'!C52*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I52-1)+'10A61 Liquid 3\" ViscosityLINEST'!D52*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I52-2)+'10A61 Liquid 3\" ViscosityLINEST'!E52*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I52-3)+'10A61 Liquid 3\" ViscosityLINEST'!F52*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I52-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B53*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I53+'10A61 Liquid 3\" ViscosityLINEST'!C53*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I53-1)+'10A61 Liquid 3\" ViscosityLINEST'!D53*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I53-2)+'10A61 Liquid 3\" ViscosityLINEST'!E53*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I53-3)+'10A61 Liquid 3\" ViscosityLINEST'!F53*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I53-4)","v":{"$error":"#NUM!"}}]
["1/8-08-CA",null,null,null,null,null,null,null,null,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B54*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I54+'10A61 Liquid 3\" ViscosityLINEST'!C54*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I54-1)+'10A61 Liquid 3\" ViscosityLINEST'!D54*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I54-2)+'10A61 Liquid 3\" ViscosityLINEST'!E54*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I54-3)+'10A61 Liquid 3\" ViscosityLINEST'!F54*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I54-4)","v":{"$error":"#NUM!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!M6:M11,'10A61 Liquid 3\"'!L6:L11^{1,2,3,4})","v":-222.91666666665003},683.65740740736157,-742.3124999999543,289.29021164019207,31.214841269844314,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B55*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I55+'10A61 Liquid 3\" ViscosityLINEST'!C55*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I55-1)+'10A61 Liquid 3\" ViscosityLINEST'!D55*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I55-2)+'10A61 Liquid 3\" ViscosityLINEST'!E55*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I55-3)+'10A61 Liquid 3\" ViscosityLINEST'!F55*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I55-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M11:M19,'10A61 Liquid 3\"'!L11:L19^{1,2,3,4})","v":0.28741724941723618},-4.305862211862042,24.445327505826736,-65.633792022790601,84.093055555554685,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B56*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I56+'10A61 Liquid 3\" ViscosityLINEST'!C56*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I56-1)+'10A61 Liquid 3\" ViscosityLINEST'!D56*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I56-2)+'10A61 Liquid 3\" ViscosityLINEST'!E56*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I56-3)+'10A61 Liquid 3\" ViscosityLINEST'!F56*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I56-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!M23:M28,'10A61 Liquid 3\"'!L23:L28^{1,2,3,4})","v":183.33333333333496},-562.59259259260227,649.00000000001614,-368.82407407408448,135.84555555555784,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B57*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I57+'10A61 Liquid 3\" ViscosityLINEST'!C57*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I57-1)+'10A61 Liquid 3\" ViscosityLINEST'!D57*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I57-2)+'10A61 Liquid 3\" ViscosityLINEST'!E57*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I57-3)+'10A61 Liquid 3\" ViscosityLINEST'!F57*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I57-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M28:M36,'10A61 Liquid 3\"'!L28:L36^{1,2,3,4})","v":0.19379953379952541},-3.0658637658636563,18.535489510489004,-53.478837088836137,74.537222222221644,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B58*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I58+'10A61 Liquid 3\" ViscosityLINEST'!C58*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I58-1)+'10A61 Liquid 3\" ViscosityLINEST'!D58*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I58-2)+'10A61 Liquid 3\" ViscosityLINEST'!E58*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I58-3)+'10A61 Liquid 3\" ViscosityLINEST'!F58*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I58-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!M41:M46,'10A61 Liquid 3\"'!L41:L46^{1,2,3,4})","v":-206.24999999998195},594.9537037036531,-617.39583333328164,242.20939153436862,21.434206349210072,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B59*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I59+'10A61 Liquid 3\" ViscosityLINEST'!C59*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I59-1)+'10A61 Liquid 3\" ViscosityLINEST'!D59*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I59-2)+'10A61 Liquid 3\" ViscosityLINEST'!E59*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I59-3)+'10A61 Liquid 3\" ViscosityLINEST'!F59*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I59-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M46:M54,'10A61 Liquid 3\"'!L46:L54^{1,2,3,4})","v":0.17132867132866389},-2.6782336182335209,16.185955710955263,-47.438168868168027,68.652222222221738,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B60*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I60+'10A61 Liquid 3\" ViscosityLINEST'!C60*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I60-1)+'10A61 Liquid 3\" ViscosityLINEST'!D60*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I60-2)+'10A61 Liquid 3\" ViscosityLINEST'!E60*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I60-3)+'10A61 Liquid 3\" ViscosityLINEST'!F60*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I60-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!M57:M62,'10A61 Liquid 3\"'!L57:L62^{1,2,3,4})","v":-122.9166666666567},413.2870370370099,-502.2291666666398,237.511772486761,7.8399206349223718,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B61*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I61+'10A61 Liquid 3\" ViscosityLINEST'!C61*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I61-1)+'10A61 Liquid 3\" ViscosityLINEST'!D61*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I61-2)+'10A61 Liquid 3\" ViscosityLINEST'!E61*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I61-3)+'10A61 Liquid 3\" ViscosityLINEST'!F61*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I61-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M62:M70,'10A61 Liquid 3\"'!L62:L70^{1,2,3,4})","v":0.15413053613052946},-2.4077415177414307,14.606346153845752,-43.342837347836593,64.425611111110669,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B62*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I62+'10A61 Liquid 3\" ViscosityLINEST'!C62*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I62-1)+'10A61 Liquid 3\" ViscosityLINEST'!D62*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I62-2)+'10A61 Liquid 3\" ViscosityLINEST'!E62*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I62-3)+'10A61 Liquid 3\" ViscosityLINEST'!F62*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I62-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!M73:M78,'10A61 Liquid 3\"'!L73:L78^{1,2,3,4})","v":-139.58333333330322},470.13888888880257,-578.72916666657602,287.67182539678413,-7.7226190476121985,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B63*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I63+'10A61 Liquid 3\" ViscosityLINEST'!C63*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I63-1)+'10A61 Liquid 3\" ViscosityLINEST'!D63*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I63-2)+'10A61 Liquid 3\" ViscosityLINEST'!E63*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I63-3)+'10A61 Liquid 3\" ViscosityLINEST'!F63*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I63-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M78:M86,'10A61 Liquid 3\"'!L78:L86^{1,2,3,4})","v":0.12020979020978395},-1.9170562030561231,11.987856643356281,-37.174023828023159,58.734944444444046,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B64*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I64+'10A61 Liquid 3\" ViscosityLINEST'!C64*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I64-1)+'10A61 Liquid 3\" ViscosityLINEST'!D64*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I64-2)+'10A61 Liquid 3\" ViscosityLINEST'!E64*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I64-3)+'10A61 Liquid 3\" ViscosityLINEST'!F64*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I64-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!M92:M97,'10A61 Liquid 3\"'!L92:L97^{1,2,3,4})","v":58.333333333322223},-145.74074074070836,122.08333333329868,-54.185449735433586,49.781587301584537,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B65*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I65+'10A61 Liquid 3\" ViscosityLINEST'!C65*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I65-1)+'10A61 Liquid 3\" ViscosityLINEST'!D65*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I65-2)+'10A61 Liquid 3\" ViscosityLINEST'!E65*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I65-3)+'10A61 Liquid 3\" ViscosityLINEST'!F65*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I65-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M97:M105,'10A61 Liquid 3\"'!L97:L105^{1,2,3,4})","v":9.9696969696964233E-2},-1.6044511784511073,10.213499999999673,-32.68176599326538,54.221555555555184,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B66*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I66+'10A61 Liquid 3\" ViscosityLINEST'!C66*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I66-1)+'10A61 Liquid 3\" ViscosityLINEST'!D66*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I66-2)+'10A61 Liquid 3\" ViscosityLINEST'!E66*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I66-3)+'10A61 Liquid 3\" ViscosityLINEST'!F66*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I66-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!M108:M113,'10A61 Liquid 3\"'!L108:L113^{1,2,3,4})","v":97.916666666636615},-269.39814814805965,262.4791666665709,-121.37923280418771,59.978174603166806,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B67*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I67+'10A61 Liquid 3\" ViscosityLINEST'!C67*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I67-1)+'10A61 Liquid 3\" ViscosityLINEST'!D67*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I67-2)+'10A61 Liquid 3\" ViscosityLINEST'!E67*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I67-3)+'10A61 Liquid 3\" ViscosityLINEST'!F67*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I67-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!M113:M121,'10A61 Liquid 3\"'!L113:L121^{1,2,3,4})","v":9.0354312354307825E-2},-1.4645143745143148,9.4313205128202338,-30.719159285158753,52.235833333333019,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B68*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I68+'10A61 Liquid 3\" ViscosityLINEST'!C68*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I68-1)+'10A61 Liquid 3\" ViscosityLINEST'!D68*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I68-2)+'10A61 Liquid 3\" ViscosityLINEST'!E68*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I68-3)+'10A61 Liquid 3\" ViscosityLINEST'!F68*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I68-4)","v":{"$error":"#NUM!"}}]
[]
["1/8-08-TA"]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!O6:O11,'10A61 Liquid 3\"'!N6:N11^{1,2,3,4})","v":87.499999999952294},-245.0925925924513,277.70833333317967,-199.79550264542993,122.65412698411437,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B71:H71)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B71*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I71+'10A61 Liquid 3\" ViscosityLINEST'!C71*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I71-1)+'10A61 Liquid 3\" ViscosityLINEST'!D71*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I71-2)+'10A61 Liquid 3\" ViscosityLINEST'!E71*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I71-3)+'10A61 Liquid 3\" ViscosityLINEST'!F71*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I71-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O11:O19,'10A61 Liquid 3\"'!N11:N19^{1,2,3,4})","v":0.28331002331001037},-4.3377000776999104,25.204627039626274,-69.336635586634159,91.104999999999166,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B72*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I72+'10A61 Liquid 3\" ViscosityLINEST'!C72*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I72-1)+'10A61 Liquid 3\" ViscosityLINEST'!D72*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I72-2)+'10A61 Liquid 3\" ViscosityLINEST'!E72*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I72-3)+'10A61 Liquid 3\" ViscosityLINEST'!F72*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I72-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!O23:O28,'10A61 Liquid 3\"'!N23:N28^{1,2,3,4})","v":39.583333333365346},-139.58333333343148,191.2291666667773,-154.37023809529231,103.52642857143829,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B73*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I73+'10A61 Liquid 3\" ViscosityLINEST'!C73*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I73-1)+'10A61 Liquid 3\" ViscosityLINEST'!D73*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I73-2)+'10A61 Liquid 3\" ViscosityLINEST'!E73*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I73-3)+'10A61 Liquid 3\" ViscosityLINEST'!F73*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I73-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O28:O36,'10A61 Liquid 3\"'!N28:N36^{1,2,3,4})","v":0.20484848484847473},-3.2340740740739431,19.600909090908491,-57.027542087540965,80.796111111110434,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B74*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I74+'10A61 Liquid 3\" ViscosityLINEST'!C74*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I74-1)+'10A61 Liquid 3\" ViscosityLINEST'!D74*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I74-2)+'10A61 Liquid 3\" ViscosityLINEST'!E74*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I74-3)+'10A61 Liquid 3\" ViscosityLINEST'!F74*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I74-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!O41:O46,'10A61 Liquid 3\"'!N41:N46^{1,2,3,4})","v":-212.49999999998886},650.09259259256339,-722.95833333330586,316.00978835977736,7.8001587301602484,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B75*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I75+'10A61 Liquid 3\" ViscosityLINEST'!C75*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I75-1)+'10A61 Liquid 3\" ViscosityLINEST'!D75*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I75-2)+'10A61 Liquid 3\" ViscosityLINEST'!E75*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I75-3)+'10A61 Liquid 3\" ViscosityLINEST'!F75*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I75-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O46:O54,'10A61 Liquid 3\"'!N46:N54^{1,2,3,4})","v":0.17938461538460704},-2.8077130277129179,17.048729603729093,-50.490192955191986,74.439888888888277,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B76*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I76+'10A61 Liquid 3\" ViscosityLINEST'!C76*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I76-1)+'10A61 Liquid 3\" ViscosityLINEST'!D76*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I76-2)+'10A61 Liquid 3\" ViscosityLINEST'!E76*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I76-3)+'10A61 Liquid 3\" ViscosityLINEST'!F76*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I76-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!O57:O62,'10A61 Liquid 3\"'!N57:N62^{1,2,3,4})","v":-231.24999999995796},760.50925925913873,-914.39583333320672,451.11455026449255,-29.43341269840306,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B77*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I77+'10A61 Liquid 3\" ViscosityLINEST'!C77*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I77-1)+'10A61 Liquid 3\" ViscosityLINEST'!D77*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I77-2)+'10A61 Liquid 3\" ViscosityLINEST'!E77*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I77-3)+'10A61 Liquid 3\" ViscosityLINEST'!F77*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I77-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O62:O70,'10A61 Liquid 3\"'!N62:N70^{1,2,3,4})","v":0.14636829836829157},-2.3246620046619153,14.427529137528721,-44.171561771560974,68.435333333332878,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B78*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I78+'10A61 Liquid 3\" ViscosityLINEST'!C78*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I78-1)+'10A61 Liquid 3\" ViscosityLINEST'!D78*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I78-2)+'10A61 Liquid 3\" ViscosityLINEST'!E78*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I78-3)+'10A61 Liquid 3\" ViscosityLINEST'!F78*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I78-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!O73:O78,'10A61 Liquid 3\"'!N73:N78^{1,2,3,4})","v":41.666666666664796},-88.518518518513773,50.499999999995694,-18.489814814813176,49.46111111111091,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B79*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I79+'10A61 Liquid 3\" ViscosityLINEST'!C79*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I79-1)+'10A61 Liquid 3\" ViscosityLINEST'!D79*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I79-2)+'10A61 Liquid 3\" ViscosityLINEST'!E79*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I79-3)+'10A61 Liquid 3\" ViscosityLINEST'!F79*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I79-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O78:O86,'10A61 Liquid 3\"'!N78:N86^{1,2,3,4})","v":0.11784615384614723},-1.8906386946386082,11.974538461538062,-38.022006993006237,62.414666666666186,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B80*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I80+'10A61 Liquid 3\" ViscosityLINEST'!C80*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I80-1)+'10A61 Liquid 3\" ViscosityLINEST'!D80*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I80-2)+'10A61 Liquid 3\" ViscosityLINEST'!E80*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I80-3)+'10A61 Liquid 3\" ViscosityLINEST'!F80*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I80-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!O92:O97,'10A61 Liquid 3\"'!N92:N97^{1,2,3,4})","v":137.49999999995094},-386.94444444429968,388.12499999984306,-179.23769841262435,73.579523809510988,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B81*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I81+'10A61 Liquid 3\" ViscosityLINEST'!C81*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I81-1)+'10A61 Liquid 3\" ViscosityLINEST'!D81*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I81-2)+'10A61 Liquid 3\" ViscosityLINEST'!E81*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I81-3)+'10A61 Liquid 3\" ViscosityLINEST'!F81*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I81-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O97:O105,'10A61 Liquid 3\"'!N97:N105^{1,2,3,4})","v":9.4041958041952534E-2},-1.5389546749546039,10.034610722610401,-33.211655270654674,57.61922222222185,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B82*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I82+'10A61 Liquid 3\" ViscosityLINEST'!C82*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I82-1)+'10A61 Liquid 3\" ViscosityLINEST'!D82*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I82-2)+'10A61 Liquid 3\" ViscosityLINEST'!E82*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I82-3)+'10A61 Liquid 3\" ViscosityLINEST'!F82*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I82-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!O108:O113,'10A61 Liquid 3\"'!N108:N113^{1,2,3,4})","v":93.749999999964913},-265.23148148137801,264.52083333322128,-123.44947089941812,62.719603174594042,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B83*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I83+'10A61 Liquid 3\" ViscosityLINEST'!C83*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I83-1)+'10A61 Liquid 3\" ViscosityLINEST'!D83*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I83-2)+'10A61 Liquid 3\" ViscosityLINEST'!E83*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I83-3)+'10A61 Liquid 3\" ViscosityLINEST'!F83*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I83-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!O113:O121,'10A61 Liquid 3\"'!N113:N121^{1,2,3,4})","v":8.3529137529132685E-2},-1.3865449365448739,9.207511655011368,-31.177227402226865,55.5676111111108,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B84*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I84+'10A61 Liquid 3\" ViscosityLINEST'!C84*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I84-1)+'10A61 Liquid 3\" ViscosityLINEST'!D84*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I84-2)+'10A61 Liquid 3\" ViscosityLINEST'!E84*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I84-3)+'10A61 Liquid 3\" ViscosityLINEST'!F84*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I84-4)","v":{"$error":"#NUM!"}}]
[]
["1/8-20-BG"]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!Q6:Q11,'10A61 Liquid 3\"'!P6:P11^{1,2,3,4})","v":285.41666666657238},-808.74999999972204,864.27083333303244,-469.6142857141441,169.59071428568996,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B87*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I87+'10A61 Liquid 3\" ViscosityLINEST'!C87*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I87-1)+'10A61 Liquid 3\" ViscosityLINEST'!D87*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I87-2)+'10A61 Liquid 3\" ViscosityLINEST'!E87*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I87-3)+'10A61 Liquid 3\" ViscosityLINEST'!F87*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I87-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q11:Q19,'10A61 Liquid 3\"'!P11:P19^{1,2,3,4})","v":0.32532400932399702},-4.8189184149182553,27.03830536130463,-71.562421911420529,89.760333333332454,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B88*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I88+'10A61 Liquid 3\" ViscosityLINEST'!C88*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I88-1)+'10A61 Liquid 3\" ViscosityLINEST'!D88*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I88-2)+'10A61 Liquid 3\" ViscosityLINEST'!E88*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I88-3)+'10A61 Liquid 3\" ViscosityLINEST'!F88*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I88-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!Q23:Q28,'10A61 Liquid 3\"'!P23:P28^{1,2,3,4})","v":-18.749999999947686},65.601851851695301,-75.10416666649455,-6.5042328043150937,71.05817460318903,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B89*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I89+'10A61 Liquid 3\" ViscosityLINEST'!C89*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I89-1)+'10A61 Liquid 3\" ViscosityLINEST'!D89*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I89-2)+'10A61 Liquid 3\" ViscosityLINEST'!E89*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I89-3)+'10A61 Liquid 3\" ViscosityLINEST'!F89*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I89-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q28:Q36,'10A61 Liquid 3\"'!P28:P36^{1,2,3,4})","v":0.29557575757574572},-4.3456228956227436,24.183015151514464,-63.535048821547548,79.614555555554773,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B90*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I90+'10A61 Liquid 3\" ViscosityLINEST'!C90*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I90-1)+'10A61 Liquid 3\" ViscosityLINEST'!D90*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I90-2)+'10A61 Liquid 3\" ViscosityLINEST'!E90*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I90-3)+'10A61 Liquid 3\" ViscosityLINEST'!F90*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I90-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!Q41:Q46,'10A61 Liquid 3\"'!P41:P46^{1,2,3,4})","v":-85.416666666681976},234.30555555560281,-226.52083333338672,58.919444444470614,50.921666666661949,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B91*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I91+'10A61 Liquid 3\" ViscosityLINEST'!C91*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I91-1)+'10A61 Liquid 3\" ViscosityLINEST'!D91*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I91-2)+'10A61 Liquid 3\" ViscosityLINEST'!E91*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I91-3)+'10A61 Liquid 3\" ViscosityLINEST'!F91*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I91-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q46:Q54,'10A61 Liquid 3\"'!P46:P54^{1,2,3,4})","v":0.25937995337994313},-3.8122025382024032,21.216821678321057,-55.810782698781537,70.262055555554838,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B92*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I92+'10A61 Liquid 3\" ViscosityLINEST'!C92*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I92-1)+'10A61 Liquid 3\" ViscosityLINEST'!D92*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I92-2)+'10A61 Liquid 3\" ViscosityLINEST'!E92*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I92-3)+'10A61 Liquid 3\" ViscosityLINEST'!F92*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I92-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!Q57:Q62,'10A61 Liquid 3\"'!P57:P62^{1,2,3,4})","v":79.166666666622191},-250.83333333320155,298.20833333319001,-182.12023809517027,83.901428571416773,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B93*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I93+'10A61 Liquid 3\" ViscosityLINEST'!C93*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I93-1)+'10A61 Liquid 3\" ViscosityLINEST'!D93*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I93-2)+'10A61 Liquid 3\" ViscosityLINEST'!E93*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I93-3)+'10A61 Liquid 3\" ViscosityLINEST'!F93*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I93-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q62:Q70,'10A61 Liquid 3\"'!P62:P70^{1,2,3,4})","v":0.22788344988344045},-3.3483455063453862,18.625544289043745,-48.971171199170186,61.712388888888306,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B94*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I94+'10A61 Liquid 3\" ViscosityLINEST'!C94*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I94-1)+'10A61 Liquid 3\" ViscosityLINEST'!D94*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I94-2)+'10A61 Liquid 3\" ViscosityLINEST'!E94*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I94-3)+'10A61 Liquid 3\" ViscosityLINEST'!F94*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I94-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!Q73:Q78,'10A61 Liquid 3\"'!P73:P78^{1,2,3,4})","v":97.916666666634498},-304.95370370360911,355.72916666656454,-204.82724867720066,80.702936507928186,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B95*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I95+'10A61 Liquid 3\" ViscosityLINEST'!C95*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I95-1)+'10A61 Liquid 3\" ViscosityLINEST'!D95*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I95-2)+'10A61 Liquid 3\" ViscosityLINEST'!E95*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I95-3)+'10A61 Liquid 3\" ViscosityLINEST'!F95*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I95-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q78:Q86,'10A61 Liquid 3\"'!P78:P86^{1,2,3,4})","v":0.198447552447544},-2.9141181041179949,16.195691142190643,-42.534455322454392,53.563499999999436,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B96*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I96+'10A61 Liquid 3\" ViscosityLINEST'!C96*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I96-1)+'10A61 Liquid 3\" ViscosityLINEST'!D96*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I96-2)+'10A61 Liquid 3\" ViscosityLINEST'!E96*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I96-3)+'10A61 Liquid 3\" ViscosityLINEST'!F96*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I96-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!Q92:Q97,'10A61 Liquid 3\"'!P92:P97^{1,2,3,4})","v":77.083333333304722},-240.97222222213799,282.35416666657562,-164.59206349202071,67.044047619040242,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B97*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I97+'10A61 Liquid 3\" ViscosityLINEST'!C97*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I97-1)+'10A61 Liquid 3\" ViscosityLINEST'!D97*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I97-2)+'10A61 Liquid 3\" ViscosityLINEST'!E97*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I97-3)+'10A61 Liquid 3\" ViscosityLINEST'!F97*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I97-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q97:Q105,'10A61 Liquid 3\"'!P97:P105^{1,2,3,4})","v":0.16910955710955047},-2.4828231028230174,13.796268065267675,-36.227233618232887,45.609444444444023,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B98*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I98+'10A61 Liquid 3\" ViscosityLINEST'!C98*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I98-1)+'10A61 Liquid 3\" ViscosityLINEST'!D98*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I98-2)+'10A61 Liquid 3\" ViscosityLINEST'!E98*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I98-3)+'10A61 Liquid 3\" ViscosityLINEST'!F98*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I98-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!Q108:Q113,'10A61 Liquid 3\"'!P108:P113^{1,2,3,4})","v":60.416666666637553},-190.04629629621036,224.18749999990683,-133.92989417985024,58.479920634913057,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B99*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I99+'10A61 Liquid 3\" ViscosityLINEST'!C99*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I99-1)+'10A61 Liquid 3\" ViscosityLINEST'!D99*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I99-2)+'10A61 Liquid 3\" ViscosityLINEST'!E99*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I99-3)+'10A61 Liquid 3\" ViscosityLINEST'!F99*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I99-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Q113:Q121,'10A61 Liquid 3\"'!P113:P121^{1,2,3,4})","v":0.1539067599067539},-2.2609080549079774,12.572856643356287,-33.046106319605656,41.638222222221856,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B100*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I100+'10A61 Liquid 3\" ViscosityLINEST'!C100*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I100-1)+'10A61 Liquid 3\" ViscosityLINEST'!D100*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I100-2)+'10A61 Liquid 3\" ViscosityLINEST'!E100*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I100-3)+'10A61 Liquid 3\" ViscosityLINEST'!F100*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I100-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B101*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I101+'10A61 Liquid 3\" ViscosityLINEST'!C101*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I101-1)+'10A61 Liquid 3\" ViscosityLINEST'!D101*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I101-2)+'10A61 Liquid 3\" ViscosityLINEST'!E101*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I101-3)+'10A61 Liquid 3\" ViscosityLINEST'!F101*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I101-4)","v":{"$error":"#DIV/0!"}}]
["1/8-20-SA",null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B102*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I102+'10A61 Liquid 3\" ViscosityLINEST'!C102*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I102-1)+'10A61 Liquid 3\" ViscosityLINEST'!D102*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I102-2)+'10A61 Liquid 3\" ViscosityLINEST'!E102*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I102-3)+'10A61 Liquid 3\" ViscosityLINEST'!F102*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I102-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!S6:S11,'10A61 Liquid 3\"'!R6:R11^{1,2,3,4})","v":-179.16666666671512},486.38888888903716,-463.95833333349998,118.31825396833538,104.56380952379496,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B103*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I103+'10A61 Liquid 3\" ViscosityLINEST'!C103*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I103-1)+'10A61 Liquid 3\" ViscosityLINEST'!D103*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I103-2)+'10A61 Liquid 3\" ViscosityLINEST'!E103*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I103-3)+'10A61 Liquid 3\" ViscosityLINEST'!F103*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I103-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S11:S19,'10A61 Liquid 3\"'!R11:R19^{1,2,3,4})","v":0.53328671328669208},-7.8356021756019016,43.590617715616474,-114.60973581973353,144.27499999999861,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B104*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I104+'10A61 Liquid 3\" ViscosityLINEST'!C104*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I104-1)+'10A61 Liquid 3\" ViscosityLINEST'!D104*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I104-2)+'10A61 Liquid 3\" ViscosityLINEST'!E104*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I104-3)+'10A61 Liquid 3\" ViscosityLINEST'!F104*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I104-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!S23:S28,'10A61 Liquid 3\"'!R23:R28^{1,2,3,4})","v":102.08333333337329},-321.15740740752994,381.52083333347161,-245.74378306885095,143.11658730159951,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B105*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I105+'10A61 Liquid 3\" ViscosityLINEST'!C105*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I105-1)+'10A61 Liquid 3\" ViscosityLINEST'!D105*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I105-2)+'10A61 Liquid 3\" ViscosityLINEST'!E105*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I105-3)+'10A61 Liquid 3\" ViscosityLINEST'!F105*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I105-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S28:S36,'10A61 Liquid 3\"'!R28:R36^{1,2,3,4})","v":0.40778554778553139},-6.1127531727529574,34.866235431234436,-94.789235949234069,125.40277777777663,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B106*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I106+'10A61 Liquid 3\" ViscosityLINEST'!C106*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I106-1)+'10A61 Liquid 3\" ViscosityLINEST'!D106*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I106-2)+'10A61 Liquid 3\" ViscosityLINEST'!E106*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I106-3)+'10A61 Liquid 3\" ViscosityLINEST'!F106*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I106-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!S41:S46,'10A61 Liquid 3\"'!R41:R46^{1,2,3,4})","v":-712.49999999990064},2177.4999999997167,-2444.374999999704,1158.6321428570086,-125.47285714283493,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B107*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I107+'10A61 Liquid 3\" ViscosityLINEST'!C107*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I107-1)+'10A61 Liquid 3\" ViscosityLINEST'!D107*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I107-2)+'10A61 Liquid 3\" ViscosityLINEST'!E107*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I107-3)+'10A61 Liquid 3\" ViscosityLINEST'!F107*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I107-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S46:S54,'10A61 Liquid 3\"'!R46:R54^{1,2,3,4})","v":0.24233100233098942},-3.8926184926183285,24.011841491840748,-71.41639083138945,104.83166666666591,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B108*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I108+'10A61 Liquid 3\" ViscosityLINEST'!C108*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I108-1)+'10A61 Liquid 3\" ViscosityLINEST'!D108*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I108-2)+'10A61 Liquid 3\" ViscosityLINEST'!E108*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I108-3)+'10A61 Liquid 3\" ViscosityLINEST'!F108*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I108-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!S57:S62,'10A61 Liquid 3\"'!R57:R62^{1,2,3,4})","v":-95.833333333340121},337.87037037039323,-429.62500000002814,206.5820105820255,29.843492063489222,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B109*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I109+'10A61 Liquid 3\" ViscosityLINEST'!C109*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I109-1)+'10A61 Liquid 3\" ViscosityLINEST'!D109*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I109-2)+'10A61 Liquid 3\" ViscosityLINEST'!E109*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I109-3)+'10A61 Liquid 3\" ViscosityLINEST'!F109*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I109-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S62:S70,'10A61 Liquid 3\"'!R62:R70^{1,2,3,4})","v":0.14158508158507249},-2.5085159285158114,17.053088578088044,-55.827113442112442,89.979999999999393,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B110*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I110+'10A61 Liquid 3\" ViscosityLINEST'!C110*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I110-1)+'10A61 Liquid 3\" ViscosityLINEST'!D110*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I110-2)+'10A61 Liquid 3\" ViscosityLINEST'!E110*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I110-3)+'10A61 Liquid 3\" ViscosityLINEST'!F110*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I110-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!S73:S78,'10A61 Liquid 3\"'!R73:R78^{1,2,3,4})","v":214.58333333326655},-600.13888888869212,608.97916666645347,-287.58611111101055,108.43833333331592,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B111*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I111+'10A61 Liquid 3\" ViscosityLINEST'!C111*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I111-1)+'10A61 Liquid 3\" ViscosityLINEST'!D111*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I111-2)+'10A61 Liquid 3\" ViscosityLINEST'!E111*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I111-3)+'10A61 Liquid 3\" ViscosityLINEST'!F111*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I111-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S78:S86,'10A61 Liquid 3\"'!R78:R86^{1,2,3,4})","v":6.7832167832161921E-2},-1.4642890442889658,11.629102564102201,-43.213624708624025,77.279999999999561,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B112*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I112+'10A61 Liquid 3\" ViscosityLINEST'!C112*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I112-1)+'10A61 Liquid 3\" ViscosityLINEST'!D112*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I112-2)+'10A61 Liquid 3\" ViscosityLINEST'!E112*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I112-3)+'10A61 Liquid 3\" ViscosityLINEST'!F112*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I112-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!S92:S97,'10A61 Liquid 3\"'!R92:R97^{1,2,3,4})","v":254.16666666661013},-737.31481481464937,780.29166666648894,-375.83399470891158,118.84174603173176,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B113*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I113+'10A61 Liquid 3\" ViscosityLINEST'!C113*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I113-1)+'10A61 Liquid 3\" ViscosityLINEST'!D113*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I113-2)+'10A61 Liquid 3\" ViscosityLINEST'!E113*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I113-3)+'10A61 Liquid 3\" ViscosityLINEST'!F113*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I113-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S97:S105,'10A61 Liquid 3\"'!R97:R105^{1,2,3,4})","v":1.9440559440554128E-2},-0.76076146076139084,7.8408974358971131,-33.922688422687813,67.028333333332952,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B114*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I114+'10A61 Liquid 3\" ViscosityLINEST'!C114*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I114-1)+'10A61 Liquid 3\" ViscosityLINEST'!D114*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I114-2)+'10A61 Liquid 3\" ViscosityLINEST'!E114*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I114-3)+'10A61 Liquid 3\" ViscosityLINEST'!F114*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I114-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!S108:S113,'10A61 Liquid 3\"'!R108:R113^{1,2,3,4})","v":237.49999999995353},-694.722222222087,741.62499999985562,-359.89563492056794,113.75047619046477,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B115*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I115+'10A61 Liquid 3\" ViscosityLINEST'!C115*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I115-1)+'10A61 Liquid 3\" ViscosityLINEST'!D115*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I115-2)+'10A61 Liquid 3\" ViscosityLINEST'!E115*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I115-3)+'10A61 Liquid 3\" ViscosityLINEST'!F115*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I115-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!S113:S121,'10A61 Liquid 3\"'!R113:R121^{1,2,3,4})","v":3.2634032633986959E-3},-0.51740999740993721,6.4740326340323557,-30.371405076404553,62.733888888888579,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B116*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I116+'10A61 Liquid 3\" ViscosityLINEST'!C116*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I116-1)+'10A61 Liquid 3\" ViscosityLINEST'!D116*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I116-2)+'10A61 Liquid 3\" ViscosityLINEST'!E116*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I116-3)+'10A61 Liquid 3\" ViscosityLINEST'!F116*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I116-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B117*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I117+'10A61 Liquid 3\" ViscosityLINEST'!C117*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I117-1)+'10A61 Liquid 3\" ViscosityLINEST'!D117*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I117-2)+'10A61 Liquid 3\" ViscosityLINEST'!E117*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I117-3)+'10A61 Liquid 3\" ViscosityLINEST'!F117*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I117-4)","v":{"$error":"#DIV/0!"}}]
["1/8-20-SS",null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B118*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I118+'10A61 Liquid 3\" ViscosityLINEST'!C118*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I118-1)+'10A61 Liquid 3\" ViscosityLINEST'!D118*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I118-2)+'10A61 Liquid 3\" ViscosityLINEST'!E118*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I118-3)+'10A61 Liquid 3\" ViscosityLINEST'!F118*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I118-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!U6:U11,'10A61 Liquid 3\"'!T6:T11^{1,2,3,4})","v":-83.333333333371328},381.48148148160027,-570.0000000001362,278.14947089953864,118.0253968253845,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B119*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I119+'10A61 Liquid 3\" ViscosityLINEST'!C119*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I119-1)+'10A61 Liquid 3\" ViscosityLINEST'!D119*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I119-2)+'10A61 Liquid 3\" ViscosityLINEST'!E119*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I119-3)+'10A61 Liquid 3\" ViscosityLINEST'!F119*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I119-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U11:U19,'10A61 Liquid 3\"'!T11:T19^{1,2,3,4})","v":0.33328671328668902},-6.0267132867129742,41.73001165501023,-138.89332167831901,227.1866666666651,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B120*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I120+'10A61 Liquid 3\" ViscosityLINEST'!C120*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I120-1)+'10A61 Liquid 3\" ViscosityLINEST'!D120*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I120-2)+'10A61 Liquid 3\" ViscosityLINEST'!E120*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I120-3)+'10A61 Liquid 3\" ViscosityLINEST'!F120*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I120-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!U23:U28,'10A61 Liquid 3\"'!T23:T28^{1,2,3,4})","v":625.00000000000807},-1936.1111111111502,2188.7500000000591,-1112.1388888889246,343.06666666667422,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B121*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I121+'10A61 Liquid 3\" ViscosityLINEST'!C121*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I121-1)+'10A61 Liquid 3\" ViscosityLINEST'!D121*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I121-2)+'10A61 Liquid 3\" ViscosityLINEST'!E121*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I121-3)+'10A61 Liquid 3\" ViscosityLINEST'!F121*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I121-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U28:U36,'10A61 Liquid 3\"'!T28:T36^{1,2,3,4})","v":-7.7762237762248179E-2},-8.2341362341225854E-2,10.60489510489448,-68.582141932140772,166.96444444444379,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B122*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I122+'10A61 Liquid 3\" ViscosityLINEST'!C122*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I122-1)+'10A61 Liquid 3\" ViscosityLINEST'!D122*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I122-2)+'10A61 Liquid 3\" ViscosityLINEST'!E122*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I122-3)+'10A61 Liquid 3\" ViscosityLINEST'!F122*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I122-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!U41:U46,'10A61 Liquid 3\"'!T41:T46^{1,2,3,4})","v":-445.83333333329847},1242.129629629532,-1258.9583333332334,516.98941798937381,43.63793650794355,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B123*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I123+'10A61 Liquid 3\" ViscosityLINEST'!C123*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I123-1)+'10A61 Liquid 3\" ViscosityLINEST'!D123*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I123-2)+'10A61 Liquid 3\" ViscosityLINEST'!E123*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I123-3)+'10A61 Liquid 3\" ViscosityLINEST'!F123*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I123-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U46:U54,'10A61 Liquid 3\"'!T46:T54^{1,2,3,4})","v":-0.12372960372960781},0.91694379694385175,3.1885081585079029,-45.491357161356682,139.58111111111083,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B124*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I124+'10A61 Liquid 3\" ViscosityLINEST'!C124*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I124-1)+'10A61 Liquid 3\" ViscosityLINEST'!D124*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I124-2)+'10A61 Liquid 3\" ViscosityLINEST'!E124*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I124-3)+'10A61 Liquid 3\" ViscosityLINEST'!F124*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I124-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!U57:U62,'10A61 Liquid 3\"'!T57:T62^{1,2,3,4})","v":97.916666666642868},-298.84259259252309,349.72916666659228,-211.2312169311823,152.41341269840677,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B125*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I125+'10A61 Liquid 3\" ViscosityLINEST'!C125*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I125-1)+'10A61 Liquid 3\" ViscosityLINEST'!D125*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I125-2)+'10A61 Liquid 3\" ViscosityLINEST'!E125*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I125-3)+'10A61 Liquid 3\" ViscosityLINEST'!F125*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I125-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U62:U70,'10A61 Liquid 3\"'!T62:T70^{1,2,3,4})","v":-0.19002331002330922},1.9733436933436885,-3.2358275058275061,-27.631669256669223,119.07722222222216,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B126*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I126+'10A61 Liquid 3\" ViscosityLINEST'!C126*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I126-1)+'10A61 Liquid 3\" ViscosityLINEST'!D126*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I126-2)+'10A61 Liquid 3\" ViscosityLINEST'!E126*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I126-3)+'10A61 Liquid 3\" ViscosityLINEST'!F126*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I126-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!U73:U78,'10A61 Liquid 3\"'!T73:T78^{1,2,3,4})","v":-43.749999999986251},146.15740740736788,-171.10416666662496,60.922354497335363,90.061984126987369,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B127*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I127+'10A61 Liquid 3\" ViscosityLINEST'!C127*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I127-1)+'10A61 Liquid 3\" ViscosityLINEST'!D127*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I127-2)+'10A61 Liquid 3\" ViscosityLINEST'!E127*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I127-3)+'10A61 Liquid 3\" ViscosityLINEST'!F127*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I127-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U78:U86,'10A61 Liquid 3\"'!T78:T86^{1,2,3,4})","v":-0.11571095571095459},1.2304169904169786,-1.5559207459207025,-24.545180005180075,107.20444444444449,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B128*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I128+'10A61 Liquid 3\" ViscosityLINEST'!C128*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I128-1)+'10A61 Liquid 3\" ViscosityLINEST'!D128*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I128-2)+'10A61 Liquid 3\" ViscosityLINEST'!E128*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I128-3)+'10A61 Liquid 3\" ViscosityLINEST'!F128*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I128-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!U92:U97,'10A61 Liquid 3\"'!T92:T97^{1,2,3,4})","v":-143.74999999995805},459.86111111098842,-537.68749999986824,252.2746031745416,45.334047619058168,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B129*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I129+'10A61 Liquid 3\" ViscosityLINEST'!C129*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I129-1)+'10A61 Liquid 3\" ViscosityLINEST'!D129*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I129-2)+'10A61 Liquid 3\" ViscosityLINEST'!E129*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I129-3)+'10A61 Liquid 3\" ViscosityLINEST'!F129*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I129-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U97:U105,'10A61 Liquid 3\"'!T97:T105^{1,2,3,4})","v":-0.13006993006992873},1.5419839419839285,-4.0229370629370154,-15.834435379435449,94.45388888888894,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B130*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I130+'10A61 Liquid 3\" ViscosityLINEST'!C130*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I130-1)+'10A61 Liquid 3\" ViscosityLINEST'!D130*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I130-2)+'10A61 Liquid 3\" ViscosityLINEST'!E130*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I130-3)+'10A61 Liquid 3\" ViscosityLINEST'!F130*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I130-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!U108:U113,'10A61 Liquid 3\"'!T108:T113^{1,2,3,4})","v":-210.41666666661635},666.71296296281662,-774.93749999984402,372.38108465601249,19.572936507948725,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B131*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I131+'10A61 Liquid 3\" ViscosityLINEST'!C131*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I131-1)+'10A61 Liquid 3\" ViscosityLINEST'!D131*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I131-2)+'10A61 Liquid 3\" ViscosityLINEST'!E131*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I131-3)+'10A61 Liquid 3\" ViscosityLINEST'!F131*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I131-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!U113:U121,'10A61 Liquid 3\"'!T113:T121^{1,2,3,4})","v":-0.11804195804195634},1.4446516446516251,-4.0532167832167048,-13.936465941466066,89.94277777777782,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B132*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I132+'10A61 Liquid 3\" ViscosityLINEST'!C132*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I132-1)+'10A61 Liquid 3\" ViscosityLINEST'!D132*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I132-2)+'10A61 Liquid 3\" ViscosityLINEST'!E132*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I132-3)+'10A61 Liquid 3\" ViscosityLINEST'!F132*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I132-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B133*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I133+'10A61 Liquid 3\" ViscosityLINEST'!C133*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I133-1)+'10A61 Liquid 3\" ViscosityLINEST'!D133*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I133-2)+'10A61 Liquid 3\" ViscosityLINEST'!E133*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I133-3)+'10A61 Liquid 3\" ViscosityLINEST'!F133*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I133-4)","v":{"$error":"#DIV/0!"}}]
["1/8-20-CA",null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B134*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I134+'10A61 Liquid 3\" ViscosityLINEST'!C134*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I134-1)+'10A61 Liquid 3\" ViscosityLINEST'!D134*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I134-2)+'10A61 Liquid 3\" ViscosityLINEST'!E134*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I134-3)+'10A61 Liquid 3\" ViscosityLINEST'!F134*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I134-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!W6:W11,'10A61 Liquid 3\"'!V6:V11^{1,2,3,4})","v":-833.33333333328108},2331.4814814813367,-2374.999999999854,977.97089947083566,95.896825396835879,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"COUNT(B135:H135)-1","v":4},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B135*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I135+'10A61 Liquid 3\" ViscosityLINEST'!C135*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I135-1)+'10A61 Liquid 3\" ViscosityLINEST'!D135*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I135-2)+'10A61 Liquid 3\" ViscosityLINEST'!E135*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I135-3)+'10A61 Liquid 3\" ViscosityLINEST'!F135*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I135-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W11:W19,'10A61 Liquid 3\"'!V11:V19^{1,2,3,4})","v":-0.25006993006993922},1.8754519554520741,6.1664568764563406,-90.760832685831716,280.17611111111057,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B136*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I136+'10A61 Liquid 3\" ViscosityLINEST'!C136*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I136-1)+'10A61 Liquid 3\" ViscosityLINEST'!D136*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I136-2)+'10A61 Liquid 3\" ViscosityLINEST'!E136*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I136-3)+'10A61 Liquid 3\" ViscosityLINEST'!F136*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I136-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!W23:W28,'10A61 Liquid 3\"'!V23:V28^{1,2,3,4})","v":-208.33333333327604},669.44444444427643,-777.91666666648587,341.7341269840424,144.76190476191925,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B137*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I137+'10A61 Liquid 3\" ViscosityLINEST'!C137*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I137-1)+'10A61 Liquid 3\" ViscosityLINEST'!D137*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I137-2)+'10A61 Liquid 3\" ViscosityLINEST'!E137*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I137-3)+'10A61 Liquid 3\" ViscosityLINEST'!F137*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I137-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W28:W36,'10A61 Liquid 3\"'!V28:V36^{1,2,3,4})","v":-0.30731934731934785},3.4999533799533946,-8.1258974358975333,-40.016958041957814,214.6216666666665,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B138*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I138+'10A61 Liquid 3\" ViscosityLINEST'!C138*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I138-1)+'10A61 Liquid 3\" ViscosityLINEST'!D138*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I138-2)+'10A61 Liquid 3\" ViscosityLINEST'!E138*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I138-3)+'10A61 Liquid 3\" ViscosityLINEST'!F138*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I138-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!W41:W46,'10A61 Liquid 3\"'!V41:V46^{1,2,3,4})","v":-291.66666666664935},936.11111111106595,-1107.0833333332907,535.92460317458597,76.91904761905019,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B139*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I139+'10A61 Liquid 3\" ViscosityLINEST'!C139*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I139-1)+'10A61 Liquid 3\" ViscosityLINEST'!D139*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I139-2)+'10A61 Liquid 3\" ViscosityLINEST'!E139*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I139-3)+'10A61 Liquid 3\" ViscosityLINEST'!F139*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I139-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W46:W54,'10A61 Liquid 3\"'!V46:V54^{1,2,3,4})","v":-0.22578088578088495},3.0200103600103532,-10.458706293706275,-19.260760165760193,177.00222222222223,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B140*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I140+'10A61 Liquid 3\" ViscosityLINEST'!C140*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I140-1)+'10A61 Liquid 3\" ViscosityLINEST'!D140*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I140-2)+'10A61 Liquid 3\" ViscosityLINEST'!E140*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I140-3)+'10A61 Liquid 3\" ViscosityLINEST'!F140*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I140-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!W57:W62,'10A61 Liquid 3\"'!V57:V62^{1,2,3,4})","v":395.83333333323873},-1155.0925925923164,1228.124999999704,-589.85978835965034,257.31984126981774,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B141*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I141+'10A61 Liquid 3\" ViscosityLINEST'!C141*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I141-1)+'10A61 Liquid 3\" ViscosityLINEST'!D141*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I141-2)+'10A61 Liquid 3\" ViscosityLINEST'!E141*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I141-3)+'10A61 Liquid 3\" ViscosityLINEST'!F141*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I141-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W62:W70,'10A61 Liquid 3\"'!V62:V70^{1,2,3,4})","v":-0.18004662004661307},2.546822066821981,-9.9268065268061516,-11.804129759130442,155.72166666666709,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B142*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I142+'10A61 Liquid 3\" ViscosityLINEST'!C142*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I142-1)+'10A61 Liquid 3\" ViscosityLINEST'!D142*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I142-2)+'10A61 Liquid 3\" ViscosityLINEST'!E142*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I142-3)+'10A61 Liquid 3\" ViscosityLINEST'!F142*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I142-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!W73:W78,'10A61 Liquid 3\"'!V73:V78^{1,2,3,4})","v":374.99999999995748},-1152.7777777776589,1296.249999999879,-652.7579365078833,259.78095238094375,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B143*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I143+'10A61 Liquid 3\" ViscosityLINEST'!C143*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I143-1)+'10A61 Liquid 3\" ViscosityLINEST'!D143*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I143-2)+'10A61 Liquid 3\" ViscosityLINEST'!E143*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I143-3)+'10A61 Liquid 3\" ViscosityLINEST'!F143*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I143-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W78:W86,'10A61 Liquid 3\"'!V78:V86^{1,2,3,4})","v":-0.10027972027972339},1.5789121989122368,-6.5879603729605325,-11.891546231545968,142.68166666666653,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B144*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I144+'10A61 Liquid 3\" ViscosityLINEST'!C144*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I144-1)+'10A61 Liquid 3\" ViscosityLINEST'!D144*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I144-2)+'10A61 Liquid 3\" ViscosityLINEST'!E144*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I144-3)+'10A61 Liquid 3\" ViscosityLINEST'!F144*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I144-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!W92:W97,'10A61 Liquid 3\"'!V92:V97^{1,2,3,4})","v":166.6666666666712},-551.85185185187004,665.00000000002512,-363.91005291006735,200.88253968254264,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B145*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I145+'10A61 Liquid 3\" ViscosityLINEST'!C145*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I145-1)+'10A61 Liquid 3\" ViscosityLINEST'!D145*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I145-2)+'10A61 Liquid 3\" ViscosityLINEST'!E145*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I145-3)+'10A61 Liquid 3\" ViscosityLINEST'!F145*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I145-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W97:W105,'10A61 Liquid 3\"'!V97:V105^{1,2,3,4})","v":-3.2634032634150313E-4},0.31819217819219503,-1.5547668997669799,-16.66545713545699,134.7905555555555,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B146*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I146+'10A61 Liquid 3\" ViscosityLINEST'!C146*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I146-1)+'10A61 Liquid 3\" ViscosityLINEST'!D146*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I146-2)+'10A61 Liquid 3\" ViscosityLINEST'!E146*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I146-3)+'10A61 Liquid 3\" ViscosityLINEST'!F146*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I146-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!W108:W113,'10A61 Liquid 3\"'!V108:V113^{1,2,3,4})","v":-41.666666666639841},69.444444444363171,-14.583333333242811,-39.765873015916853,139.56190476191253,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B147*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I147+'10A61 Liquid 3\" ViscosityLINEST'!C147*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I147-1)+'10A61 Liquid 3\" ViscosityLINEST'!D147*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I147-2)+'10A61 Liquid 3\" ViscosityLINEST'!E147*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I147-3)+'10A61 Liquid 3\" ViscosityLINEST'!F147*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I147-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!W113:W121,'10A61 Liquid 3\"'!V113:V121^{1,2,3,4})","v":1.5058275058272706E-2},9.1421911421942781E-2,-0.6046736596738026,-16.929067599067348,130.50499999999985,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B148*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I148+'10A61 Liquid 3\" ViscosityLINEST'!C148*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I148-1)+'10A61 Liquid 3\" ViscosityLINEST'!D148*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I148-2)+'10A61 Liquid 3\" ViscosityLINEST'!E148*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I148-3)+'10A61 Liquid 3\" ViscosityLINEST'!F148*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I148-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B149*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I149+'10A61 Liquid 3\" ViscosityLINEST'!C149*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I149-1)+'10A61 Liquid 3\" ViscosityLINEST'!D149*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I149-2)+'10A61 Liquid 3\" ViscosityLINEST'!E149*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I149-3)+'10A61 Liquid 3\" ViscosityLINEST'!F149*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I149-4)","v":{"$error":"#DIV/0!"}}]
["1/8-20-TA",null,null,null,null,null,null,null,-1,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B150*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I150+'10A61 Liquid 3\" ViscosityLINEST'!C150*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I150-1)+'10A61 Liquid 3\" ViscosityLINEST'!D150*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I150-2)+'10A61 Liquid 3\" ViscosityLINEST'!E150*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I150-3)+'10A61 Liquid 3\" ViscosityLINEST'!F150*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I150-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!Y6:Y11,'10A61 Liquid 3\"'!X6:X11^{1,2,3,4})","v":-229.16666666668013},597.68518518522842,-535.62500000005082,121.04100529103108,258.58174603174126,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B151*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I151+'10A61 Liquid 3\" ViscosityLINEST'!C151*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I151-1)+'10A61 Liquid 3\" ViscosityLINEST'!D151*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I151-2)+'10A61 Liquid 3\" ViscosityLINEST'!E151*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I151-3)+'10A61 Liquid 3\" ViscosityLINEST'!F151*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I151-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y11:Y19,'10A61 Liquid 3\"'!X11:X19^{1,2,3,4})","v":-0.37850815850815872},3.6095053095053213,-1.8520396270397146,-78.689042994042794,289.93555555555542,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B152*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I152+'10A61 Liquid 3\" ViscosityLINEST'!C152*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I152-1)+'10A61 Liquid 3\" ViscosityLINEST'!D152*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I152-2)+'10A61 Liquid 3\" ViscosityLINEST'!E152*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I152-3)+'10A61 Liquid 3\" ViscosityLINEST'!F152*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I152-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!Y23:Y28,'10A61 Liquid 3\"'!X23:X28^{1,2,3,4})","v":-437.49999999990433},1394.90740740713,-1628.5416666663718,777.56878306864701,74.848412698435766,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B153*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I153+'10A61 Liquid 3\" ViscosityLINEST'!C153*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I153-1)+'10A61 Liquid 3\" ViscosityLINEST'!D153*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I153-2)+'10A61 Liquid 3\" ViscosityLINEST'!E153*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I153-3)+'10A61 Liquid 3\" ViscosityLINEST'!F153*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I153-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y28:Y36,'10A61 Liquid 3\"'!X28:X36^{1,2,3,4})","v":-0.28979020979020442},3.4998394198393599,-9.3860372960370579,-36.482384097384504,223.87388888888913,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B154*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I154+'10A61 Liquid 3\" ViscosityLINEST'!C154*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I154-1)+'10A61 Liquid 3\" ViscosityLINEST'!D154*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I154-2)+'10A61 Liquid 3\" ViscosityLINEST'!E154*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I154-3)+'10A61 Liquid 3\" ViscosityLINEST'!F154*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I154-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!Y41:Y46,'10A61 Liquid 3\"'!X41:X46^{1,2,3,4})","v":124.99999999994189},-319.44444444427216,281.24999999981236,-130.55555555546661,204.36666666665118,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B155*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I155+'10A61 Liquid 3\" ViscosityLINEST'!C155*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I155-1)+'10A61 Liquid 3\" ViscosityLINEST'!D155*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I155-2)+'10A61 Liquid 3\" ViscosityLINEST'!E155*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I155-3)+'10A61 Liquid 3\" ViscosityLINEST'!F155*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I155-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y46:Y54,'10A61 Liquid 3\"'!X46:X54^{1,2,3,4})","v":-0.24167832167831332},3.3158974358973383,-12.440489510489103,-15.131853146853848,185.03166666666706,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B156*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I156+'10A61 Liquid 3\" ViscosityLINEST'!C156*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I156-1)+'10A61 Liquid 3\" ViscosityLINEST'!D156*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I156-2)+'10A61 Liquid 3\" ViscosityLINEST'!E156*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I156-3)+'10A61 Liquid 3\" ViscosityLINEST'!F156*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I156-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!Y57:Y62,'10A61 Liquid 3\"'!X57:X62^{1,2,3,4})","v":458.3333333332489},-1384.2592592590145,1528.7499999997394,-757.01455026442954,299.89841269839224,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B157*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I157+'10A61 Liquid 3\" ViscosityLINEST'!C157*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I157-1)+'10A61 Liquid 3\" ViscosityLINEST'!D157*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I157-2)+'10A61 Liquid 3\" ViscosityLINEST'!E157*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I157-3)+'10A61 Liquid 3\" ViscosityLINEST'!F157*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I157-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y62:Y70,'10A61 Liquid 3\"'!X62:X70^{1,2,3,4})","v":-0.13519813519813714},2.0614348614348845,-8.4255944055944969,-13.602328412328282,165.99111111111105,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B158*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I158+'10A61 Liquid 3\" ViscosityLINEST'!C158*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I158-1)+'10A61 Liquid 3\" ViscosityLINEST'!D158*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I158-2)+'10A61 Liquid 3\" ViscosityLINEST'!E158*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I158-3)+'10A61 Liquid 3\" ViscosityLINEST'!F158*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I158-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!Y73:Y78,'10A61 Liquid 3\"'!X73:X78^{1,2,3,4})","v":250.00000000002564},-803.70370370378691,943.33333333343239,-500.14153439158525,244.69365079366025,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B159*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I159+'10A61 Liquid 3\" ViscosityLINEST'!C159*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I159-1)+'10A61 Liquid 3\" ViscosityLINEST'!D159*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I159-2)+'10A61 Liquid 3\" ViscosityLINEST'!E159*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I159-3)+'10A61 Liquid 3\" ViscosityLINEST'!F159*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I159-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y78:Y86,'10A61 Liquid 3\"'!X78:X86^{1,2,3,4})","v":-2.1258741258742338E-2},0.62116550116551716,-2.7865034965035735,-17.966048951048815,154.47499999999991,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B160*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I160+'10A61 Liquid 3\" ViscosityLINEST'!C160*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I160-1)+'10A61 Liquid 3\" ViscosityLINEST'!D160*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I160-2)+'10A61 Liquid 3\" ViscosityLINEST'!E160*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I160-3)+'10A61 Liquid 3\" ViscosityLINEST'!F160*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I160-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!Y92:Y97,'10A61 Liquid 3\"'!X92:X97^{1,2,3,4})","v":-166.66666666663343},448.14814814805095,-434.16666666656249,160.26851851847002,117.41111111111945,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B161*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I161+'10A61 Liquid 3\" ViscosityLINEST'!C161*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I161-1)+'10A61 Liquid 3\" ViscosityLINEST'!D161*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I161-2)+'10A61 Liquid 3\" ViscosityLINEST'!E161*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I161-3)+'10A61 Liquid 3\" ViscosityLINEST'!F161*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I161-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y97:Y105,'10A61 Liquid 3\"'!X97:X105^{1,2,3,4})","v":3.7715617715615025E-2},-0.21629111629108239,0.83602564102549193,-20.948654493654235,145.36888888888876,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B162*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I162+'10A61 Liquid 3\" ViscosityLINEST'!C162*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I162-1)+'10A61 Liquid 3\" ViscosityLINEST'!D162*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I162-2)+'10A61 Liquid 3\" ViscosityLINEST'!E162*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I162-3)+'10A61 Liquid 3\" ViscosityLINEST'!F162*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I162-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!Y108:Y113,'10A61 Liquid 3\"'!X108:X113^{1,2,3,4})","v":-395.83333333327874},1136.5740740739175,-1193.9583333331682,526.5092592591833,47.705555555568395,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B163*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I163+'10A61 Liquid 3\" ViscosityLINEST'!C163*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I163-1)+'10A61 Liquid 3\" ViscosityLINEST'!D163*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I163-2)+'10A61 Liquid 3\" ViscosityLINEST'!E163*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I163-3)+'10A61 Liquid 3\" ViscosityLINEST'!F163*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I163-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!Y113:Y121,'10A61 Liquid 3\"'!X113:X121^{1,2,3,4})","v":-0.12909090909091062},1.5141414141414382,-4.9189393939395174,-13.299595959595718,138.0883333333332,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B164*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I164+'10A61 Liquid 3\" ViscosityLINEST'!C164*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I164-1)+'10A61 Liquid 3\" ViscosityLINEST'!D164*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I164-2)+'10A61 Liquid 3\" ViscosityLINEST'!E164*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I164-3)+'10A61 Liquid 3\" ViscosityLINEST'!F164*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I164-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B165*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I165+'10A61 Liquid 3\" ViscosityLINEST'!C165*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I165-1)+'10A61 Liquid 3\" ViscosityLINEST'!D165*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I165-2)+'10A61 Liquid 3\" ViscosityLINEST'!E165*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I165-3)+'10A61 Liquid 3\" ViscosityLINEST'!F165*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I165-4)","v":{"$error":"#NUM!"}}]
["1/4-15-CD",null,null,null,null,null,null,null,{"$f":"COUNT(B166:H166)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B166*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I166+'10A61 Liquid 3\" ViscosityLINEST'!C166*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I166-1)+'10A61 Liquid 3\" ViscosityLINEST'!D166*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I166-2)+'10A61 Liquid 3\" ViscosityLINEST'!E166*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I166-3)+'10A61 Liquid 3\" ViscosityLINEST'!F166*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I166-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AA6:AA11,'10A61 Liquid 3\"'!Z6:Z11^{1,2,3,4})","v":-187.50000000006352},763.425925926123,-1012.708333333558,369.38359788370929,277.53730158728126,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B167*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I167+'10A61 Liquid 3\" ViscosityLINEST'!C167*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I167-1)+'10A61 Liquid 3\" ViscosityLINEST'!D167*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I167-2)+'10A61 Liquid 3\" ViscosityLINEST'!E167*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I167-3)+'10A61 Liquid 3\" ViscosityLINEST'!F167*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I167-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA11:AA19,'10A61 Liquid 3\"'!Z11:Z19^{1,2,3,4})","v":1.1183216783216328},-16.97514633514573,99.324662004659203,-283.45166796166268,409.63777777777466,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B168*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I168+'10A61 Liquid 3\" ViscosityLINEST'!C168*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I168-1)+'10A61 Liquid 3\" ViscosityLINEST'!D168*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I168-2)+'10A61 Liquid 3\" ViscosityLINEST'!E168*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I168-3)+'10A61 Liquid 3\" ViscosityLINEST'!F168*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I168-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AA23:AA28,'10A61 Liquid 3\"'!Z23:Z28^{1,2,3,4})","v":437.50000000002137},-1165.2777777778501,1101.8750000000896,-547.57936507941281,349.95952380953304,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B169*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I169+'10A61 Liquid 3\" ViscosityLINEST'!C169*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I169-1)+'10A61 Liquid 3\" ViscosityLINEST'!D169*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I169-2)+'10A61 Liquid 3\" ViscosityLINEST'!E169*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I169-3)+'10A61 Liquid 3\" ViscosityLINEST'!F169*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I169-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA28:AA36,'10A61 Liquid 3\"'!Z28:Z36^{1,2,3,4})","v":0.65594405594402116},-10.469847189846742,65.247226107224066,-201.72481092980709,322.76611111110873,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B170*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I170+'10A61 Liquid 3\" ViscosityLINEST'!C170*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I170-1)+'10A61 Liquid 3\" ViscosityLINEST'!D170*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I170-2)+'10A61 Liquid 3\" ViscosityLINEST'!E170*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I170-3)+'10A61 Liquid 3\" ViscosityLINEST'!F170*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I170-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AA41:AA46,'10A61 Liquid 3\"'!Z41:Z46^{1,2,3,4})","v":-41.666666666538546},171.29629629591375,-268.74999999958061,95.894179893980066,193.17936507939996,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B171*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I171+'10A61 Liquid 3\" ViscosityLINEST'!C171*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I171-1)+'10A61 Liquid 3\" ViscosityLINEST'!D171*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I171-2)+'10A61 Liquid 3\" ViscosityLINEST'!E171*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I171-3)+'10A61 Liquid 3\" ViscosityLINEST'!F171*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I171-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA46:AA54,'10A61 Liquid 3\"'!Z46:Z54^{1,2,3,4})","v":0.49505827505825123},-7.9609686609683461,50.323508158506705,-159.64672753172479,266.74555555555389,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B172*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I172+'10A61 Liquid 3\" ViscosityLINEST'!C172*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I172-1)+'10A61 Liquid 3\" ViscosityLINEST'!D172*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I172-2)+'10A61 Liquid 3\" ViscosityLINEST'!E172*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I172-3)+'10A61 Liquid 3\" ViscosityLINEST'!F172*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I172-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AA57:AA62,'10A61 Liquid 3\"'!Z57:Z62^{1,2,3,4})","v":-166.66666666664889},507.40740740735606,-589.99999999994566,241.71164021161516,135.1412698412741,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B173*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I173+'10A61 Liquid 3\" ViscosityLINEST'!C173*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I173-1)+'10A61 Liquid 3\" ViscosityLINEST'!D173*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I173-2)+'10A61 Liquid 3\" ViscosityLINEST'!E173*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I173-3)+'10A61 Liquid 3\" ViscosityLINEST'!F173*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I173-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA62:AA70,'10A61 Liquid 3\"'!Z62:Z70^{1,2,3,4})","v":0.39967365967363838},-6.4725148925146128,41.259778554777256,-132.3317197617173,224.74055555555398,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B174*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I174+'10A61 Liquid 3\" ViscosityLINEST'!C174*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I174-1)+'10A61 Liquid 3\" ViscosityLINEST'!D174*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I174-2)+'10A61 Liquid 3\" ViscosityLINEST'!E174*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I174-3)+'10A61 Liquid 3\" ViscosityLINEST'!F174*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I174-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AA73:AA78,'10A61 Liquid 3\"'!Z73:Z78^{1,2,3,4})","v":-145.83333333332408},440.27777777775424,-507.2916666666456,207.29365079364305,112.85476190476288,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B175*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I175+'10A61 Liquid 3\" ViscosityLINEST'!C175*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I175-1)+'10A61 Liquid 3\" ViscosityLINEST'!D175*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I175-2)+'10A61 Liquid 3\" ViscosityLINEST'!E175*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I175-3)+'10A61 Liquid 3\" ViscosityLINEST'!F175*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I175-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA78:AA86,'10A61 Liquid 3\"'!Z78:Z86^{1,2,3,4})","v":0.33006993006991203},-5.3554519554517208,34.234755244754169,-110.25977337477136,188.35388888888767,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B176*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I176+'10A61 Liquid 3\" ViscosityLINEST'!C176*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I176-1)+'10A61 Liquid 3\" ViscosityLINEST'!D176*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I176-2)+'10A61 Liquid 3\" ViscosityLINEST'!E176*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I176-3)+'10A61 Liquid 3\" ViscosityLINEST'!F176*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I176-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AA92:AA97,'10A61 Liquid 3\"'!Z92:Z97^{1,2,3,4})","v":-87.499999999948571},281.01851851836631,-346.54166666650133,143.35767195759388,98.111746031759566,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B177*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I177+'10A61 Liquid 3\" ViscosityLINEST'!C177*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I177-1)+'10A61 Liquid 3\" ViscosityLINEST'!D177*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I177-2)+'10A61 Liquid 3\" ViscosityLINEST'!E177*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I177-3)+'10A61 Liquid 3\" ViscosityLINEST'!F177*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I177-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA97:AA105,'10A61 Liquid 3\"'!Z97:Z105^{1,2,3,4})","v":0.28913752913751395},-4.6497176897174883,29.399230769229824,-93.396661486659681,156.81222222222112,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B178*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I178+'10A61 Liquid 3\" ViscosityLINEST'!C178*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I178-1)+'10A61 Liquid 3\" ViscosityLINEST'!D178*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I178-2)+'10A61 Liquid 3\" ViscosityLINEST'!E178*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I178-3)+'10A61 Liquid 3\" ViscosityLINEST'!F178*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I178-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AA108:AA113,'10A61 Liquid 3\"'!Z108:Z113^{1,2,3,4})","v":-31.249999999929525},123.84259259238108,-184.89583333310026,73.545502645391011,98.05087301589262,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B179*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I179+'10A61 Liquid 3\" ViscosityLINEST'!C179*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I179-1)+'10A61 Liquid 3\" ViscosityLINEST'!D179*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I179-2)+'10A61 Liquid 3\" ViscosityLINEST'!E179*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I179-3)+'10A61 Liquid 3\" ViscosityLINEST'!F179*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I179-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AA113:AA121,'10A61 Liquid 3\"'!Z113:Z121^{1,2,3,4})","v":0.27160839160837685},-4.3492670292668398,27.315734265733411,-85.874501424499854,141.95222222222131,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B180*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I180+'10A61 Liquid 3\" ViscosityLINEST'!C180*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I180-1)+'10A61 Liquid 3\" ViscosityLINEST'!D180*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I180-2)+'10A61 Liquid 3\" ViscosityLINEST'!E180*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I180-3)+'10A61 Liquid 3\" ViscosityLINEST'!F180*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I180-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B181*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I181+'10A61 Liquid 3\" ViscosityLINEST'!C181*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I181-1)+'10A61 Liquid 3\" ViscosityLINEST'!D181*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I181-2)+'10A61 Liquid 3\" ViscosityLINEST'!E181*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I181-3)+'10A61 Liquid 3\" ViscosityLINEST'!F181*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I181-4)","v":{"$error":"#NUM!"}}]
["1/4-15-SA",null,null,null,null,null,null,null,{"$f":"COUNT(B182:H182)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B182*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I182+'10A61 Liquid 3\" ViscosityLINEST'!C182*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I182-1)+'10A61 Liquid 3\" ViscosityLINEST'!D182*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I182-2)+'10A61 Liquid 3\" ViscosityLINEST'!E182*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I182-3)+'10A61 Liquid 3\" ViscosityLINEST'!F182*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I182-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AC6:AC11,'10A61 Liquid 3\"'!AB6:AB11^{1,2,3,4})","v":-812.5000000002085},2319.9074074080477,-2477.2916666673887,1012.3544973548509,305.43412698406394,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B183*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I183+'10A61 Liquid 3\" ViscosityLINEST'!C183*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I183-1)+'10A61 Liquid 3\" ViscosityLINEST'!D183*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I183-2)+'10A61 Liquid 3\" ViscosityLINEST'!E183*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I183-3)+'10A61 Liquid 3\" ViscosityLINEST'!F183*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I183-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC11:AC19,'10A61 Liquid 3\"'!AB11:AB19^{1,2,3,4})","v":0.9296037296036731},-15.452887852887123,101.63426573426243,-338.13677803677194,598.85555555555197,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B184*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I184+'10A61 Liquid 3\" ViscosityLINEST'!C184*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I184-1)+'10A61 Liquid 3\" ViscosityLINEST'!D184*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I184-2)+'10A61 Liquid 3\" ViscosityLINEST'!E184*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I184-3)+'10A61 Liquid 3\" ViscosityLINEST'!F184*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I184-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AC23:AC28,'10A61 Liquid 3\"'!AB23:AB28^{1,2,3,4})","v":895.83333333341841},-2810.6481481484257,3223.1250000003311,-1703.0185185186888,694.03888888892038,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B185*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I185+'10A61 Liquid 3\" ViscosityLINEST'!C185*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I185-1)+'10A61 Liquid 3\" ViscosityLINEST'!D185*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I185-2)+'10A61 Liquid 3\" ViscosityLINEST'!E185*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I185-3)+'10A61 Liquid 3\" ViscosityLINEST'!F185*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I185-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC28:AC36,'10A61 Liquid 3\"'!AB28:AB36^{1,2,3,4})","v":-0.8924941724942046},6.045687645688063,12.443123543121652,-175.66142191141844,459.3033333333313,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B186*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I186+'10A61 Liquid 3\" ViscosityLINEST'!C186*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I186-1)+'10A61 Liquid 3\" ViscosityLINEST'!D186*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I186-2)+'10A61 Liquid 3\" ViscosityLINEST'!E186*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I186-3)+'10A61 Liquid 3\" ViscosityLINEST'!F186*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I186-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AC41:AC46,'10A61 Liquid 3\"'!AB41:AB46^{1,2,3,4})","v":-1416.6666666665756},4148.1481481479013,-4456.666666666425,2002.6256613755597,-15.931746031730768,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B187*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I187+'10A61 Liquid 3\" ViscosityLINEST'!C187*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I187-1)+'10A61 Liquid 3\" ViscosityLINEST'!D187*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I187-2)+'10A61 Liquid 3\" ViscosityLINEST'!E187*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I187-3)+'10A61 Liquid 3\" ViscosityLINEST'!F187*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I187-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC46:AC54,'10A61 Liquid 3\"'!AB46:AB54^{1,2,3,4})","v":3.860139860138441E-2},-2.2862470862468984,28.371561771560899,-149.33904428904265,384.72666666666566,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B188*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I188+'10A61 Liquid 3\" ViscosityLINEST'!C188*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I188-1)+'10A61 Liquid 3\" ViscosityLINEST'!D188*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I188-2)+'10A61 Liquid 3\" ViscosityLINEST'!E188*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I188-3)+'10A61 Liquid 3\" ViscosityLINEST'!F188*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I188-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AC57:AC62,'10A61 Liquid 3\"'!AB57:AB62^{1,2,3,4})","v":-229.16666666668837},705.09259259266344,-782.29166666675167,307.25264550268969,231.82301587300748,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B189*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I189+'10A61 Liquid 3\" ViscosityLINEST'!C189*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I189-1)+'10A61 Liquid 3\" ViscosityLINEST'!D189*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I189-2)+'10A61 Liquid 3\" ViscosityLINEST'!E189*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I189-3)+'10A61 Liquid 3\" ViscosityLINEST'!F189*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I189-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC62:AC70,'10A61 Liquid 3\"'!AB62:AB70^{1,2,3,4})","v":-0.15314685314686219},0.63863765863778599,11.400407925407302,-102.54405335405212,323.3294444444436,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B190*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I190+'10A61 Liquid 3\" ViscosityLINEST'!C190*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I190-1)+'10A61 Liquid 3\" ViscosityLINEST'!D190*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I190-2)+'10A61 Liquid 3\" ViscosityLINEST'!E190*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I190-3)+'10A61 Liquid 3\" ViscosityLINEST'!F190*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I190-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AC73:AC78,'10A61 Liquid 3\"'!AB73:AB78^{1,2,3,4})","v":333.33333333323884},-974.07407407379606,1058.3333333330331,-560.1878306876896,350.81587301584858,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B191*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I191+'10A61 Liquid 3\" ViscosityLINEST'!C191*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I191-1)+'10A61 Liquid 3\" ViscosityLINEST'!D191*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I191-2)+'10A61 Liquid 3\" ViscosityLINEST'!E191*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I191-3)+'10A61 Liquid 3\" ViscosityLINEST'!F191*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I191-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC78:AC86,'10A61 Liquid 3\"'!AB78:AB86^{1,2,3,4})","v":-0.279766899766903},2.5839368039368509,-8.7937062937291213E-2,-69.510378140377696,275.58277777777749,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B192*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I192+'10A61 Liquid 3\" ViscosityLINEST'!C192*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I192-1)+'10A61 Liquid 3\" ViscosityLINEST'!D192*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I192-2)+'10A61 Liquid 3\" ViscosityLINEST'!E192*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I192-3)+'10A61 Liquid 3\" ViscosityLINEST'!F192*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I192-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AC92:AC97,'10A61 Liquid 3\"'!AB92:AB97^{1,2,3,4})","v":291.66666666659467},-863.88888888867746,949.58333333310532,-505.39682539671838,315.1476190476007,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B193*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I193+'10A61 Liquid 3\" ViscosityLINEST'!C193*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I193-1)+'10A61 Liquid 3\" ViscosityLINEST'!D193*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I193-2)+'10A61 Liquid 3\" ViscosityLINEST'!E193*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I193-3)+'10A61 Liquid 3\" ViscosityLINEST'!F193*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I193-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC97:AC105,'10A61 Liquid 3\"'!AB97:AB105^{1,2,3,4})","v":-0.33650349650349981},3.5573685573686031,-6.5998135198137424,-47.91737244237202,238.60722222222199,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B194*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I194+'10A61 Liquid 3\" ViscosityLINEST'!C194*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I194-1)+'10A61 Liquid 3\" ViscosityLINEST'!D194*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I194-2)+'10A61 Liquid 3\" ViscosityLINEST'!E194*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I194-3)+'10A61 Liquid 3\" ViscosityLINEST'!F194*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I194-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AC108:AC113,'10A61 Liquid 3\"'!AB108:AB113^{1,2,3,4})","v":249.99999999996376},-731.4814814813767,793.33333333322184,-421.43518518513343,287.3888888888801,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B195*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I195+'10A61 Liquid 3\" ViscosityLINEST'!C195*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I195-1)+'10A61 Liquid 3\" ViscosityLINEST'!D195*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I195-2)+'10A61 Liquid 3\" ViscosityLINEST'!E195*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I195-3)+'10A61 Liquid 3\" ViscosityLINEST'!F195*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I195-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AC113:AC121,'10A61 Liquid 3\"'!AB113:AB121^{1,2,3,4})","v":-0.34820512820512789},3.7814918414918419,-8.3381002331002545,-40.986130536130467,223.9516666666666,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B196*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I196+'10A61 Liquid 3\" ViscosityLINEST'!C196*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I196-1)+'10A61 Liquid 3\" ViscosityLINEST'!D196*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I196-2)+'10A61 Liquid 3\" ViscosityLINEST'!E196*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I196-3)+'10A61 Liquid 3\" ViscosityLINEST'!F196*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I196-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B197*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I197+'10A61 Liquid 3\" ViscosityLINEST'!C197*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I197-1)+'10A61 Liquid 3\" ViscosityLINEST'!D197*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I197-2)+'10A61 Liquid 3\" ViscosityLINEST'!E197*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I197-3)+'10A61 Liquid 3\" ViscosityLINEST'!F197*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I197-4)","v":{"$error":"#NUM!"}}]
["1/4-20-CD",null,null,null,null,null,null,null,{"$f":"COUNT(B198:H198)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B198*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I198+'10A61 Liquid 3\" ViscosityLINEST'!C198*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I198-1)+'10A61 Liquid 3\" ViscosityLINEST'!D198*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I198-2)+'10A61 Liquid 3\" ViscosityLINEST'!E198*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I198-3)+'10A61 Liquid 3\" ViscosityLINEST'!F198*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I198-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AE6:AE11,'10A61 Liquid 3\"'!AD6:AD11^{1,2,3,4})","v":-83.333333333378278},253.70370370383881,-225.00000000014956,-83.358465608393459,528.20634920633643,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B199*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I199+'10A61 Liquid 3\" ViscosityLINEST'!C199*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I199-1)+'10A61 Liquid 3\" ViscosityLINEST'!D199*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I199-2)+'10A61 Liquid 3\" ViscosityLINEST'!E199*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I199-3)+'10A61 Liquid 3\" ViscosityLINEST'!F199*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I199-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE11:AE19,'10A61 Liquid 3\"'!AD11:AD19^{1,2,3,4})","v":-0.26480186480188889},1.3284641284644458,18.635897435895966,-180.21696451696175,550.95555555555381,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B200*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I200+'10A61 Liquid 3\" ViscosityLINEST'!C200*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I200-1)+'10A61 Liquid 3\" ViscosityLINEST'!D200*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I200-2)+'10A61 Liquid 3\" ViscosityLINEST'!E200*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I200-3)+'10A61 Liquid 3\" ViscosityLINEST'!F200*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I200-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AE23:AE28,'10A61 Liquid 3\"'!AD23:AD28^{1,2,3,4})","v":-520.83333333323446},1730.0925925923059,-2099.3749999996949,1008.2883597882187,194.70873015875392,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B201*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I201+'10A61 Liquid 3\" ViscosityLINEST'!C201*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I201-1)+'10A61 Liquid 3\" ViscosityLINEST'!D201*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I201-2)+'10A61 Liquid 3\" ViscosityLINEST'!E201*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I201-3)+'10A61 Liquid 3\" ViscosityLINEST'!F201*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I201-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE28:AE36,'10A61 Liquid 3\"'!AD28:AD36^{1,2,3,4})","v":-0.61724941724942062},7.008339808339862,-17.482051282051561,-68.467236467235921,392.92222222222193,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B202*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I202+'10A61 Liquid 3\" ViscosityLINEST'!C202*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I202-1)+'10A61 Liquid 3\" ViscosityLINEST'!D202*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I202-2)+'10A61 Liquid 3\" ViscosityLINEST'!E202*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I202-3)+'10A61 Liquid 3\" ViscosityLINEST'!F202*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I202-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AE41:AE46,'10A61 Liquid 3\"'!AD41:AD46^{1,2,3,4})","v":-541.66666666649485},1763.8888888883839,-2122.0833333327887,1045.0396825394271,114.19523809528206,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B203*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I203+'10A61 Liquid 3\" ViscosityLINEST'!C203*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I203-1)+'10A61 Liquid 3\" ViscosityLINEST'!D203*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I203-2)+'10A61 Liquid 3\" ViscosityLINEST'!E203*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I203-3)+'10A61 Liquid 3\" ViscosityLINEST'!F203*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I203-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE46:AE54,'10A61 Liquid 3\"'!AD46:AD54^{1,2,3,4})","v":-0.49305361305360706},5.923646723646657,-17.748251748251484,-42.238487438487866,314.10222222222245,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B204*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I204+'10A61 Liquid 3\" ViscosityLINEST'!C204*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I204-1)+'10A61 Liquid 3\" ViscosityLINEST'!D204*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I204-2)+'10A61 Liquid 3\" ViscosityLINEST'!E204*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I204-3)+'10A61 Liquid 3\" ViscosityLINEST'!F204*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I204-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AE57:AE62,'10A61 Liquid 3\"'!AD57:AD62^{1,2,3,4})","v":-208.33333333330083},724.99999999990712,-932.91666666656931,468.24999999995555,165.90000000000748,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B205*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I205+'10A61 Liquid 3\" ViscosityLINEST'!C205*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I205-1)+'10A61 Liquid 3\" ViscosityLINEST'!D205*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I205-2)+'10A61 Liquid 3\" ViscosityLINEST'!E205*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I205-3)+'10A61 Liquid 3\" ViscosityLINEST'!F205*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I205-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE62:AE70,'10A61 Liquid 3\"'!AD62:AD70^{1,2,3,4})","v":-0.37846153846153346},4.6170940170939545,-14.182960372960094,-33.702152292152824,261.64333333333366,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B206*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I206+'10A61 Liquid 3\" ViscosityLINEST'!C206*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I206-1)+'10A61 Liquid 3\" ViscosityLINEST'!D206*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I206-2)+'10A61 Liquid 3\" ViscosityLINEST'!E206*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I206-3)+'10A61 Liquid 3\" ViscosityLINEST'!F206*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I206-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AE73:AE78,'10A61 Liquid 3\"'!AD73:AD78^{1,2,3,4})","v":-145.83333333332291},519.90740740738181,-683.95833333331177,345.35449735449021,147.53412698412774,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B207*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I207+'10A61 Liquid 3\" ViscosityLINEST'!C207*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I207-1)+'10A61 Liquid 3\" ViscosityLINEST'!D207*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I207-2)+'10A61 Liquid 3\" ViscosityLINEST'!E207*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I207-3)+'10A61 Liquid 3\" ViscosityLINEST'!F207*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I207-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE78:AE86,'10A61 Liquid 3\"'!AD78:AD86^{1,2,3,4})","v":-0.32223776223775819},3.9446982646982192,-12.311864801864624,-27.213295778296068,218.97277777777794,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B208*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I208+'10A61 Liquid 3\" ViscosityLINEST'!C208*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I208-1)+'10A61 Liquid 3\" ViscosityLINEST'!D208*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I208-2)+'10A61 Liquid 3\" ViscosityLINEST'!E208*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I208-3)+'10A61 Liquid 3\" ViscosityLINEST'!F208*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I208-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AE92:AE97,'10A61 Liquid 3\"'!AD92:AD97^{1,2,3,4})","v":-229.16666666663608},760.648148148063,-934.7916666665808,462.73280423276691,92.575396825402834,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B209*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I209+'10A61 Liquid 3\" ViscosityLINEST'!C209*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I209-1)+'10A61 Liquid 3\" ViscosityLINEST'!D209*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I209-2)+'10A61 Liquid 3\" ViscosityLINEST'!E209*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I209-3)+'10A61 Liquid 3\" ViscosityLINEST'!F209*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I209-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE97:AE105,'10A61 Liquid 3\"'!AD97:AD105^{1,2,3,4})","v":-0.27226107226106877},3.303765863765824,-10.02344988344972,-24.206850556850849,183.2544444444446,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B210*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I210+'10A61 Liquid 3\" ViscosityLINEST'!C210*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I210-1)+'10A61 Liquid 3\" ViscosityLINEST'!D210*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I210-2)+'10A61 Liquid 3\" ViscosityLINEST'!E210*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I210-3)+'10A61 Liquid 3\" ViscosityLINEST'!F210*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I210-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AE108:AE113,'10A61 Liquid 3\"'!AD108:AD113^{1,2,3,4})","v":-333.33333333326829},1081.4814814812946,-1294.999999999804,639.25661375652464,44.98253968255446,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B211*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I211+'10A61 Liquid 3\" ViscosityLINEST'!C211*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I211-1)+'10A61 Liquid 3\" ViscosityLINEST'!D211*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I211-2)+'10A61 Liquid 3\" ViscosityLINEST'!E211*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I211-3)+'10A61 Liquid 3\" ViscosityLINEST'!F211*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I211-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AE113:AE121,'10A61 Liquid 3\"'!AD113:AD121^{1,2,3,4})","v":-0.2629836829836818},3.1460398860398779,-9.3300116550116421,-22.828631183631185,166.7522222222222,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B212*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I212+'10A61 Liquid 3\" ViscosityLINEST'!C212*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I212-1)+'10A61 Liquid 3\" ViscosityLINEST'!D212*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I212-2)+'10A61 Liquid 3\" ViscosityLINEST'!E212*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I212-3)+'10A61 Liquid 3\" ViscosityLINEST'!F212*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I212-4)","v":{"$error":"#NUM!"}}]
[null,null,null,null,null,null,null,null,null,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B213*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I213+'10A61 Liquid 3\" ViscosityLINEST'!C213*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I213-1)+'10A61 Liquid 3\" ViscosityLINEST'!D213*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I213-2)+'10A61 Liquid 3\" ViscosityLINEST'!E213*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I213-3)+'10A61 Liquid 3\" ViscosityLINEST'!F213*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I213-4)","v":{"$error":"#NUM!"}}]
["1/4-20-SA",null,null,null,null,null,null,null,{"$f":"COUNT(B214:H214)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B214*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I214+'10A61 Liquid 3\" ViscosityLINEST'!C214*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I214-1)+'10A61 Liquid 3\" ViscosityLINEST'!D214*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I214-2)+'10A61 Liquid 3\" ViscosityLINEST'!E214*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I214-3)+'10A61 Liquid 3\" ViscosityLINEST'!F214*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I214-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AG6:AG11,'10A61 Liquid 3\"'!AF6:AF11^{1,2,3,4})","v":2291.6666666662904},-6256.4814814803849,6210.4166666654965,-2774.4351851846427,1122.5888888887966,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B215*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I215+'10A61 Liquid 3\" ViscosityLINEST'!C215*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I215-1)+'10A61 Liquid 3\" ViscosityLINEST'!D215*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I215-2)+'10A61 Liquid 3\" ViscosityLINEST'!E215*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I215-3)+'10A61 Liquid 3\" ViscosityLINEST'!F215*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I215-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG11:AG19,'10A61 Liquid 3\"'!AF11:AF19^{1,2,3,4})","v":-0.36829836829835494},4.0114996114994588,-0.55641025640963993,-156.51196581196686,746.80000000000064,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B216*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I216+'10A61 Liquid 3\" ViscosityLINEST'!C216*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I216-1)+'10A61 Liquid 3\" ViscosityLINEST'!D216*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I216-2)+'10A61 Liquid 3\" ViscosityLINEST'!E216*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I216-3)+'10A61 Liquid 3\" ViscosityLINEST'!F216*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I216-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AG23:AG28,'10A61 Liquid 3\"'!AF23:AF28^{1,2,3,4})","v":1416.6666666666708},-4453.7037037037517,5104.1666666667588,-2602.3915343915974,1016.5936507936653,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B217*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I217+'10A61 Liquid 3\" ViscosityLINEST'!C217*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I217-1)+'10A61 Liquid 3\" ViscosityLINEST'!D217*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I217-2)+'10A61 Liquid 3\" ViscosityLINEST'!E217*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I217-3)+'10A61 Liquid 3\" ViscosityLINEST'!F217*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I217-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG28:AG36,'10A61 Liquid 3\"'!AF28:AF36^{1,2,3,4})","v":-0.40279720279719955},5.7440041440041165,-21.196270396270332,-56.320849520849549,553.32222222222219,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B218*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I218+'10A61 Liquid 3\" ViscosityLINEST'!C218*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I218-1)+'10A61 Liquid 3\" ViscosityLINEST'!D218*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I218-2)+'10A61 Liquid 3\" ViscosityLINEST'!E218*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I218-3)+'10A61 Liquid 3\" ViscosityLINEST'!F218*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I218-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AG41:AG46,'10A61 Liquid 3\"'!AF41:AF46^{1,2,3,4})","v":-770.83333333331939},2041.2037037036753,-1934.3749999999834,712.85582010581913,364.37063492063362,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B219*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I219+'10A61 Liquid 3\" ViscosityLINEST'!C219*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I219-1)+'10A61 Liquid 3\" ViscosityLINEST'!D219*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I219-2)+'10A61 Liquid 3\" ViscosityLINEST'!E219*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I219-3)+'10A61 Liquid 3\" ViscosityLINEST'!F219*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I219-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG46:AG54,'10A61 Liquid 3\"'!AF46:AF54^{1,2,3,4})","v":0.2708624708624594},-2.5291375291373832,11.268648018647358,-86.102564102562894,489.94999999999942,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B220*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I220+'10A61 Liquid 3\" ViscosityLINEST'!C220*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I220-1)+'10A61 Liquid 3\" ViscosityLINEST'!D220*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I220-2)+'10A61 Liquid 3\" ViscosityLINEST'!E220*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I220-3)+'10A61 Liquid 3\" ViscosityLINEST'!F220*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I220-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AG57:AG62,'10A61 Liquid 3\"'!AF57:AF62^{1,2,3,4})","v":-166.66666666664079},411.11111111103514,-318.33333333325129,22.174603174564616,415.01904761905428,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B221*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I221+'10A61 Liquid 3\" ViscosityLINEST'!C221*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I221-1)+'10A61 Liquid 3\" ViscosityLINEST'!D221*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I221-2)+'10A61 Liquid 3\" ViscosityLINEST'!E221*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I221-3)+'10A61 Liquid 3\" ViscosityLINEST'!F221*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I221-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG62:AG70,'10A61 Liquid 3\"'!AF62:AF70^{1,2,3,4})","v":0.30536130536130462},-3.1761201761201572,13.784265734265611,-77.602939652939384,429.55555555555549,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B222*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I222+'10A61 Liquid 3\" ViscosityLINEST'!C222*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I222-1)+'10A61 Liquid 3\" ViscosityLINEST'!D222*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I222-2)+'10A61 Liquid 3\" ViscosityLINEST'!E222*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I222-3)+'10A61 Liquid 3\" ViscosityLINEST'!F222*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I222-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AG73:AG78,'10A61 Liquid 3\"'!AF73:AF78^{1,2,3,4})","v":-62.500000000018979},138.42592592598393,-58.958333333398059,-78.437830687799448,384.06587301586745,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B223*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I223+'10A61 Liquid 3\" ViscosityLINEST'!C223*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I223-1)+'10A61 Liquid 3\" ViscosityLINEST'!D223*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I223-2)+'10A61 Liquid 3\" ViscosityLINEST'!E223*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I223-3)+'10A61 Liquid 3\" ViscosityLINEST'!F223*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I223-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG78:AG86,'10A61 Liquid 3\"'!AF78:AF86^{1,2,3,4})","v":0.24662004662003784},-2.6705516705515566,11.771678321677813,-65.415695415694529,378.44999999999953,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B224*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I224+'10A61 Liquid 3\" ViscosityLINEST'!C224*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I224-1)+'10A61 Liquid 3\" ViscosityLINEST'!D224*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I224-2)+'10A61 Liquid 3\" ViscosityLINEST'!E224*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I224-3)+'10A61 Liquid 3\" ViscosityLINEST'!F224*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I224-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AG92:AG97,'10A61 Liquid 3\"'!AF92:AF97^{1,2,3,4})","v":-62.499999999999282},153.24074074074036,-97.291666666667979,-42.657407407406133,337.90555555555528,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B225*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I225+'10A61 Liquid 3\" ViscosityLINEST'!C225*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I225-1)+'10A61 Liquid 3\" ViscosityLINEST'!D225*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I225-2)+'10A61 Liquid 3\" ViscosityLINEST'!E225*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I225-3)+'10A61 Liquid 3\" ViscosityLINEST'!F225*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I225-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG97:AG105,'10A61 Liquid 3\"'!AF97:AF105^{1,2,3,4})","v":0.1878787878787796},-2.0451178451177405,9.0136363636358965,-53.952356902356065,335.42222222222176,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B226*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I226+'10A61 Liquid 3\" ViscosityLINEST'!C226*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I226-1)+'10A61 Liquid 3\" ViscosityLINEST'!D226*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I226-2)+'10A61 Liquid 3\" ViscosityLINEST'!E226*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I226-3)+'10A61 Liquid 3\" ViscosityLINEST'!F226*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I226-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AG108:AG113,'10A61 Liquid 3\"'!AF108:AF113^{1,2,3,4})","v":-124.99999999995822},345.37037037024811,-317.08333333320178,70.189153439091783,300.32063492064549,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B227*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I227+'10A61 Liquid 3\" ViscosityLINEST'!C227*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I227-1)+'10A61 Liquid 3\" ViscosityLINEST'!D227*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I227-2)+'10A61 Liquid 3\" ViscosityLINEST'!E227*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I227-3)+'10A61 Liquid 3\" ViscosityLINEST'!F227*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I227-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AG113:AG121,'10A61 Liquid 3\"'!AF113:AF121^{1,2,3,4})","v":0.18648018648018111},-2.0465164465163763,8.9170163170159906,-50.970189070188461,317.68888888888858,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B228*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I228+'10A61 Liquid 3\" ViscosityLINEST'!C228*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I228-1)+'10A61 Liquid 3\" ViscosityLINEST'!D228*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I228-2)+'10A61 Liquid 3\" ViscosityLINEST'!E228*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I228-3)+'10A61 Liquid 3\" ViscosityLINEST'!F228*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I228-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-15-SS",null,null,null,null,null,null,null,{"$f":"COUNT(B230:H230)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B230*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I230+'10A61 Liquid 3\" ViscosityLINEST'!C230*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I230-1)+'10A61 Liquid 3\" ViscosityLINEST'!D230*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I230-2)+'10A61 Liquid 3\" ViscosityLINEST'!E230*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I230-3)+'10A61 Liquid 3\" ViscosityLINEST'!F230*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I230-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AI6:AI11,'10A61 Liquid 3\"'!AH6:AH11^{1,2,3,4})","v":-125.00000000011275},456.48148148182554,-552.08333333371866,109.57804232822983,701.75396825393477,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B231*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I231+'10A61 Liquid 3\" ViscosityLINEST'!C231*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I231-1)+'10A61 Liquid 3\" ViscosityLINEST'!D231*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I231-2)+'10A61 Liquid 3\" ViscosityLINEST'!E231*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I231-3)+'10A61 Liquid 3\" ViscosityLINEST'!F231*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I231-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI11:AI19,'10A61 Liquid 3\"'!AH11:AH19^{1,2,3,4})","v":-0.43822843822845037},2.329448329448506,25.200466200465321,-251.79448329448155,815.33333333333212,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B232*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I232+'10A61 Liquid 3\" ViscosityLINEST'!C232*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I232-1)+'10A61 Liquid 3\" ViscosityLINEST'!D232*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I232-2)+'10A61 Liquid 3\" ViscosityLINEST'!E232*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I232-3)+'10A61 Liquid 3\" ViscosityLINEST'!F232*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I232-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AI23:AI28,'10A61 Liquid 3\"'!AH23:AH28^{1,2,3,4})","v":-62.499999999851838},212.4999999995554,-275.62499999951064,50.535714285480495,569.43571428575513,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B233*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I233+'10A61 Liquid 3\" ViscosityLINEST'!C233*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I233-1)+'10A61 Liquid 3\" ViscosityLINEST'!D233*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I233-2)+'10A61 Liquid 3\" ViscosityLINEST'!E233*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I233-3)+'10A61 Liquid 3\" ViscosityLINEST'!F233*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I233-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI28:AI36,'10A61 Liquid 3\"'!AH28:AH36^{1,2,3,4})","v":-0.9766899766899706},11.757316757316696,-36.101282051281835,-70.666601916602247,591.24444444444453,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B234*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I234+'10A61 Liquid 3\" ViscosityLINEST'!C234*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I234-1)+'10A61 Liquid 3\" ViscosityLINEST'!D234*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I234-2)+'10A61 Liquid 3\" ViscosityLINEST'!E234*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I234-3)+'10A61 Liquid 3\" ViscosityLINEST'!F234*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I234-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AI41:AI46,'10A61 Liquid 3\"'!AH41:AH46^{1,2,3,4})","v":-916.66666666657659},2816.6666666664191,-3200.8333333330866,1512.6904761903706,221.95714285715923,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B235*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I235+'10A61 Liquid 3\" ViscosityLINEST'!C235*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I235-1)+'10A61 Liquid 3\" ViscosityLINEST'!D235*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I235-2)+'10A61 Liquid 3\" ViscosityLINEST'!E235*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I235-3)+'10A61 Liquid 3\" ViscosityLINEST'!F235*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I235-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI46:AI54,'10A61 Liquid 3\"'!AH46:AH54^{1,2,3,4})","v":-0.82610722610721232},10.64864024864008,-39.269230769230042,-28.024281274282544,491.81666666666729,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B236*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I236+'10A61 Liquid 3\" ViscosityLINEST'!C236*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I236-1)+'10A61 Liquid 3\" ViscosityLINEST'!D236*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I236-2)+'10A61 Liquid 3\" ViscosityLINEST'!E236*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I236-3)+'10A61 Liquid 3\" ViscosityLINEST'!F236*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I236-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AI57:AI62,'10A61 Liquid 3\"'!AH57:AH62^{1,2,3,4})","v":749.99999999975876},-2138.8888888881756,2212.4999999992256,-1041.7539682536024,608.19047619041271,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B237*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I237+'10A61 Liquid 3\" ViscosityLINEST'!C237*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I237-1)+'10A61 Liquid 3\" ViscosityLINEST'!D237*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I237-2)+'10A61 Liquid 3\" ViscosityLINEST'!E237*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I237-3)+'10A61 Liquid 3\" ViscosityLINEST'!F237*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I237-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI62:AI70,'10A61 Liquid 3\"'!AH62:AH70^{1,2,3,4})","v":-1.0354312354312052},13.454804454804087,-55.065384615383003,21.165086765083796,411.70555555555734,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B238*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I238+'10A61 Liquid 3\" ViscosityLINEST'!C238*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I238-1)+'10A61 Liquid 3\" ViscosityLINEST'!D238*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I238-2)+'10A61 Liquid 3\" ViscosityLINEST'!E238*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I238-3)+'10A61 Liquid 3\" ViscosityLINEST'!F238*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I238-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AI73:AI78,'10A61 Liquid 3\"'!AH73:AH78^{1,2,3,4})","v":354.16666666662832},-1004.1666666665585,1010.2083333332214,-469.72619047614018,464.2071428571345,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B239*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I239+'10A61 Liquid 3\" ViscosityLINEST'!C239*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I239-1)+'10A61 Liquid 3\" ViscosityLINEST'!D239*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I239-2)+'10A61 Liquid 3\" ViscosityLINEST'!E239*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I239-3)+'10A61 Liquid 3\" ViscosityLINEST'!F239*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I239-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI78:AI86,'10A61 Liquid 3\"'!AH78:AH86^{1,2,3,4})","v":-0.72680652680650704},9.7122507122504658,-40.906177156176049,11.249210049207973,375.32777777777915,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B240*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I240+'10A61 Liquid 3\" ViscosityLINEST'!C240*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I240-1)+'10A61 Liquid 3\" ViscosityLINEST'!D240*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I240-2)+'10A61 Liquid 3\" ViscosityLINEST'!E240*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I240-3)+'10A61 Liquid 3\" ViscosityLINEST'!F240*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I240-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AI92:AI97,'10A61 Liquid 3\"'!AH92:AH97^{1,2,3,4})","v":145.83333333340187},-405.09259259280151,373.12500000023357,-162.96693121704456,375.46269841271845,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B241*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I241+'10A61 Liquid 3\" ViscosityLINEST'!C241*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I241-1)+'10A61 Liquid 3\" ViscosityLINEST'!D241*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I241-2)+'10A61 Liquid 3\" ViscosityLINEST'!E241*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I241-3)+'10A61 Liquid 3\" ViscosityLINEST'!F241*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I241-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI97:AI105,'10A61 Liquid 3\"'!AH97:AH105^{1,2,3,4})","v":5.9673659673642306E-2},-0.63662263662241925,5.727505827504876,-65.178723128721444,387.19444444444338,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B242*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I242+'10A61 Liquid 3\" ViscosityLINEST'!C242*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I242-1)+'10A61 Liquid 3\" ViscosityLINEST'!D242*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I242-2)+'10A61 Liquid 3\" ViscosityLINEST'!E242*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I242-3)+'10A61 Liquid 3\" ViscosityLINEST'!F242*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I242-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AI108:AI113,'10A61 Liquid 3\"'!AH108:AH113^{1,2,3,4})","v":-229.16666666658458},719.90740740716876,-865.62499999974534,432.96164021152202,255.99126984128992,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B243*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I243+'10A61 Liquid 3\" ViscosityLINEST'!C243*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I243-1)+'10A61 Liquid 3\" ViscosityLINEST'!D243*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I243-2)+'10A61 Liquid 3\" ViscosityLINEST'!E243*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I243-3)+'10A61 Liquid 3\" ViscosityLINEST'!F243*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I243-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AI113:AI121,'10A61 Liquid 3\"'!AH113:AH121^{1,2,3,4})","v":-0.3319347319347154},4.951566951566746,-22.5958041958033,-4.8318311318327289,336.64444444444536,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B244*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I244+'10A61 Liquid 3\" ViscosityLINEST'!C244*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I244-1)+'10A61 Liquid 3\" ViscosityLINEST'!D244*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I244-2)+'10A61 Liquid 3\" ViscosityLINEST'!E244*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I244-3)+'10A61 Liquid 3\" ViscosityLINEST'!F244*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I244-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-15-CA",null,null,null,null,null,null,null,{"$f":"COUNT(B246:H246)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B246*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I246+'10A61 Liquid 3\" ViscosityLINEST'!C246*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I246-1)+'10A61 Liquid 3\" ViscosityLINEST'!D246*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I246-2)+'10A61 Liquid 3\" ViscosityLINEST'!E246*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I246-3)+'10A61 Liquid 3\" ViscosityLINEST'!F246*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I246-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AK6:AK11,'10A61 Liquid 3\"'!AJ6:AJ11^{1,2,3,4})","v":-1687.4999999998631},5193.0555555551746,-5911.8749999996126,2787.7658730157023,490.08809523812238,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B247*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I247+'10A61 Liquid 3\" ViscosityLINEST'!C247*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I247-1)+'10A61 Liquid 3\" ViscosityLINEST'!D247*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I247-2)+'10A61 Liquid 3\" ViscosityLINEST'!E247*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I247-3)+'10A61 Liquid 3\" ViscosityLINEST'!F247*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I247-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK11:AK19,'10A61 Liquid 3\"'!AJ11:AJ19^{1,2,3,4})","v":-1.6787878787878587},21.647811447811197,-80.243939393938248,-52.913468013470279,985.77222222222395,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B248*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I248+'10A61 Liquid 3\" ViscosityLINEST'!C248*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I248-1)+'10A61 Liquid 3\" ViscosityLINEST'!D248*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I248-2)+'10A61 Liquid 3\" ViscosityLINEST'!E248*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I248-3)+'10A61 Liquid 3\" ViscosityLINEST'!F248*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I248-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AK23:AK28,'10A61 Liquid 3\"'!AJ23:AJ28^{1,2,3,4})","v":583.33333333339226},-1657.4074074075991,1650.8333333335615,-763.14021164032931,916.53015873018091,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B249*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I249+'10A61 Liquid 3\" ViscosityLINEST'!C249*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I249-1)+'10A61 Liquid 3\" ViscosityLINEST'!D249*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I249-2)+'10A61 Liquid 3\" ViscosityLINEST'!E249*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I249-3)+'10A61 Liquid 3\" ViscosityLINEST'!F249*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I249-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK28:AK36,'10A61 Liquid 3\"'!AJ28:AJ36^{1,2,3,4})","v":-1.3496503496503041},18.246309246308666,-77.726223776221175,17.203574203569367,773.55000000000314,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B250*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I250+'10A61 Liquid 3\" ViscosityLINEST'!C250*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I250-1)+'10A61 Liquid 3\" ViscosityLINEST'!D250*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I250-2)+'10A61 Liquid 3\" ViscosityLINEST'!E250*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I250-3)+'10A61 Liquid 3\" ViscosityLINEST'!F250*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I250-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AK41:AK46,'10A61 Liquid 3\"'!AJ41:AJ46^{1,2,3,4})","v":-1166.6666666665781},3479.6296296293854,-3874.9999999997535,1849.9179894178819,352.23650793652473,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B251*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I251+'10A61 Liquid 3\" ViscosityLINEST'!C251*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I251-1)+'10A61 Liquid 3\" ViscosityLINEST'!D251*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I251-2)+'10A61 Liquid 3\" ViscosityLINEST'!E251*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I251-3)+'10A61 Liquid 3\" ViscosityLINEST'!F251*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I251-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK46:AK54,'10A61 Liquid 3\"'!AJ46:AJ54^{1,2,3,4})","v":-0.26433566433564215},5.4541828541825872,-29.852097902096755,-23.337788137790223,687.10555555555686,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B252*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I252+'10A61 Liquid 3\" ViscosityLINEST'!C252*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I252-1)+'10A61 Liquid 3\" ViscosityLINEST'!D252*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I252-2)+'10A61 Liquid 3\" ViscosityLINEST'!E252*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I252-3)+'10A61 Liquid 3\" ViscosityLINEST'!F252*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I252-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AK57:AK62,'10A61 Liquid 3\"'!AJ57:AJ62^{1,2,3,4})","v":1145.8333333331227},-3471.7592592586516,3850.6249999993565,-1893.9788359785396,946.23412698407662,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B253*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I253+'10A61 Liquid 3\" ViscosityLINEST'!C253*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I253-1)+'10A61 Liquid 3\" ViscosityLINEST'!D253*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I253-2)+'10A61 Liquid 3\" ViscosityLINEST'!E253*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I253-3)+'10A61 Liquid 3\" ViscosityLINEST'!F253*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I253-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK62:AK70,'10A61 Liquid 3\"'!AJ62:AJ70^{1,2,3,4})","v":0.12820512820512245},-6.4750064749243387E-3,-5.447202797203202,-49.657472157471368,631.194444444444,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B254*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I254+'10A61 Liquid 3\" ViscosityLINEST'!C254*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I254-1)+'10A61 Liquid 3\" ViscosityLINEST'!D254*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I254-2)+'10A61 Liquid 3\" ViscosityLINEST'!E254*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I254-3)+'10A61 Liquid 3\" ViscosityLINEST'!F254*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I254-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AK73:AK78,'10A61 Liquid 3\"'!AJ73:AJ78^{1,2,3,4})","v":1395.8333333331702},-4399.537037036579,5100.6249999995298,-2608.7367724865626,1038.3150793650443,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B255*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I255+'10A61 Liquid 3\" ViscosityLINEST'!C255*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I255-1)+'10A61 Liquid 3\" ViscosityLINEST'!D255*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I255-2)+'10A61 Liquid 3\" ViscosityLINEST'!E255*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I255-3)+'10A61 Liquid 3\" ViscosityLINEST'!F255*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I255-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK78:AK86,'10A61 Liquid 3\"'!AJ78:AJ86^{1,2,3,4})","v":0.48717948717947607},-4.6629888629887173,14.260023310022641,-70.158495208493974,586.38888888888812,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B256*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I256+'10A61 Liquid 3\" ViscosityLINEST'!C256*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I256-1)+'10A61 Liquid 3\" ViscosityLINEST'!D256*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I256-2)+'10A61 Liquid 3\" ViscosityLINEST'!E256*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I256-3)+'10A61 Liquid 3\" ViscosityLINEST'!F256*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I256-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AK92:AK97,'10A61 Liquid 3\"'!AJ92:AJ97^{1,2,3,4})","v":333.33333333338686},-1235.1851851853548,1653.3333333335313,-979.79100529110553,714.56825396827253,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B257*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I257+'10A61 Liquid 3\" ViscosityLINEST'!C257*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I257-1)+'10A61 Liquid 3\" ViscosityLINEST'!D257*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I257-2)+'10A61 Liquid 3\" ViscosityLINEST'!E257*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I257-3)+'10A61 Liquid 3\" ViscosityLINEST'!F257*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I257-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK97:AK105,'10A61 Liquid 3\"'!AJ97:AJ105^{1,2,3,4})","v":0.73193473193471492},-7.7906241906239835,27.453379953379059,-83.337192437190851,549.27777777777681,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B258*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I258+'10A61 Liquid 3\" ViscosityLINEST'!C258*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I258-1)+'10A61 Liquid 3\" ViscosityLINEST'!D258*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I258-2)+'10A61 Liquid 3\" ViscosityLINEST'!E258*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I258-3)+'10A61 Liquid 3\" ViscosityLINEST'!F258*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I258-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AK108:AK113,'10A61 Liquid 3\"'!AJ108:AJ113^{1,2,3,4})","v":1.0957781531802337E-10},-233.33333333367011,552.50000000038062,-454.55952380971092,604.45714285717668,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B259*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I259+'10A61 Liquid 3\" ViscosityLINEST'!C259*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I259-1)+'10A61 Liquid 3\" ViscosityLINEST'!D259*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I259-2)+'10A61 Liquid 3\" ViscosityLINEST'!E259*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I259-3)+'10A61 Liquid 3\" ViscosityLINEST'!F259*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I259-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AK113:AK121,'10A61 Liquid 3\"'!AJ113:AJ121^{1,2,3,4})","v":0.73379953379951712},-8.0298368298366203,29.198368298367367,-83.883449883448193,531.23333333333221,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B260*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I260+'10A61 Liquid 3\" ViscosityLINEST'!C260*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I260-1)+'10A61 Liquid 3\" ViscosityLINEST'!D260*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I260-2)+'10A61 Liquid 3\" ViscosityLINEST'!E260*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I260-3)+'10A61 Liquid 3\" ViscosityLINEST'!F260*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I260-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-20-SS",null,null,null,null,null,null,null,{"$f":"COUNT(B262:H262)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B262*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I262+'10A61 Liquid 3\" ViscosityLINEST'!C262*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I262-1)+'10A61 Liquid 3\" ViscosityLINEST'!D262*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I262-2)+'10A61 Liquid 3\" ViscosityLINEST'!E262*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I262-3)+'10A61 Liquid 3\" ViscosityLINEST'!F262*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I262-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AM6:AM11,'10A61 Liquid 3\"'!AL6:AL11^{1,2,3,4})","v":-166.66666666667484},314.81481481483922,-41.666666666693942,-296.71957671956312,1110.6396825396801,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B263*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I263+'10A61 Liquid 3\" ViscosityLINEST'!C263*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I263-1)+'10A61 Liquid 3\" ViscosityLINEST'!D263*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I263-2)+'10A61 Liquid 3\" ViscosityLINEST'!E263*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I263-3)+'10A61 Liquid 3\" ViscosityLINEST'!F263*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I263-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM11:AM19,'10A61 Liquid 3\"'!AL11:AL19^{1,2,3,4})","v":0.71701631701628898},-7.4876974876971172,32.89953379953208,-192.16746956746636,1085.3555555555536,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B264*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I264+'10A61 Liquid 3\" ViscosityLINEST'!C264*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I264-1)+'10A61 Liquid 3\" ViscosityLINEST'!D264*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I264-2)+'10A61 Liquid 3\" ViscosityLINEST'!E264*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I264-3)+'10A61 Liquid 3\" ViscosityLINEST'!F264*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I264-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AM23:AM28,'10A61 Liquid 3\"'!AL23:AL28^{1,2,3,4})","v":-937.49999999988745},2941.2037037033738,-3337.7083333329788,1525.6415343913686,563.15634920637763,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B265*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I265+'10A61 Liquid 3\" ViscosityLINEST'!C265*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I265-1)+'10A61 Liquid 3\" ViscosityLINEST'!D265*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I265-2)+'10A61 Liquid 3\" ViscosityLINEST'!E265*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I265-3)+'10A61 Liquid 3\" ViscosityLINEST'!F265*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I265-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM28:AM36,'10A61 Liquid 3\"'!AL28:AL36^{1,2,3,4})","v":0.30116550116548801},-3.2234136234134501,13.809557109556305,-111.16990416990268,855.37777777777706,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B266*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I266+'10A61 Liquid 3\" ViscosityLINEST'!C266*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I266-1)+'10A61 Liquid 3\" ViscosityLINEST'!D266*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I266-2)+'10A61 Liquid 3\" ViscosityLINEST'!E266*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I266-3)+'10A61 Liquid 3\" ViscosityLINEST'!F266*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I266-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AM41:AM46,'10A61 Liquid 3\"'!AL41:AL46^{1,2,3,4})","v":-312.50000000001052},1138.4259259259718,-1478.9583333334001,739.74074074078067,565.39444444443598,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B267*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I267+'10A61 Liquid 3\" ViscosityLINEST'!C267*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I267-1)+'10A61 Liquid 3\" ViscosityLINEST'!D267*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I267-2)+'10A61 Liquid 3\" ViscosityLINEST'!E267*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I267-3)+'10A61 Liquid 3\" ViscosityLINEST'!F267*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I267-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM46:AM54,'10A61 Liquid 3\"'!AL46:AL54^{1,2,3,4})","v":2.692773892773809},-30.730795130794078,120.16620046619585,-252.30366485365664,814.86111111110654,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B268*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I268+'10A61 Liquid 3\" ViscosityLINEST'!C268*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I268-1)+'10A61 Liquid 3\" ViscosityLINEST'!D268*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I268-2)+'10A61 Liquid 3\" ViscosityLINEST'!E268*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I268-3)+'10A61 Liquid 3\" ViscosityLINEST'!F268*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I268-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AM57:AM62,'10A61 Liquid 3\"'!AL57:AL62^{1,2,3,4})","v":749.99999999979241},-2138.8888888882725,2212.4999999993279,-1041.7539682536494,798.19047619042067,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B269*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I269+'10A61 Liquid 3\" ViscosityLINEST'!C269*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I269-1)+'10A61 Liquid 3\" ViscosityLINEST'!D269*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I269-2)+'10A61 Liquid 3\" ViscosityLINEST'!E269*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I269-3)+'10A61 Liquid 3\" ViscosityLINEST'!F269*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I269-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM62:AM70,'10A61 Liquid 3\"'!AL62:AL70^{1,2,3,4})","v":-0.39114219114219312},5.1980833980834156,-23.477972027972058,-9.5783087283088069,609.08888888888896,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B270*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I270+'10A61 Liquid 3\" ViscosityLINEST'!C270*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I270-1)+'10A61 Liquid 3\" ViscosityLINEST'!D270*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I270-2)+'10A61 Liquid 3\" ViscosityLINEST'!E270*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I270-3)+'10A61 Liquid 3\" ViscosityLINEST'!F270*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I270-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AM73:AM78,'10A61 Liquid 3\"'!AL73:AL78^{1,2,3,4})","v":916.66666666654874},-2809.2592592589226,3156.6666666663155,-1589.9431216929627,851.56984126981502,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B271*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I271+'10A61 Liquid 3\" ViscosityLINEST'!C271*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I271-1)+'10A61 Liquid 3\" ViscosityLINEST'!D271*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I271-2)+'10A61 Liquid 3\" ViscosityLINEST'!E271*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I271-3)+'10A61 Liquid 3\" ViscosityLINEST'!F271*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I271-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM78:AM86,'10A61 Liquid 3\"'!AL78:AL86^{1,2,3,4})","v":-0.50023310023308531},6.117948717948539,-25.571911421910659,-0.54766899767036425,546.53333333333421,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B272*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I272+'10A61 Liquid 3\" ViscosityLINEST'!C272*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I272-1)+'10A61 Liquid 3\" ViscosityLINEST'!D272*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I272-2)+'10A61 Liquid 3\" ViscosityLINEST'!E272*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I272-3)+'10A61 Liquid 3\" ViscosityLINEST'!F272*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I272-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AM92:AM97,'10A61 Liquid 3\"'!AL92:AL97^{1,2,3,4})","v":916.66666666662707},-2911.1111111110117,3393.3333333332453,-1761.2103174602851,844.59523809523375,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B273*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I273+'10A61 Liquid 3\" ViscosityLINEST'!C273*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I273-1)+'10A61 Liquid 3\" ViscosityLINEST'!D273*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I273-2)+'10A61 Liquid 3\" ViscosityLINEST'!E273*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I273-3)+'10A61 Liquid 3\" ViscosityLINEST'!F273*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I273-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM97:AM105,'10A61 Liquid 3\"'!AL97:AL105^{1,2,3,4})","v":-0.40233100233099134},4.8744366744365406,-20.153962703962122,-3.824669774670828,501.86666666666736,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B274*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I274+'10A61 Liquid 3\" ViscosityLINEST'!C274*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I274-1)+'10A61 Liquid 3\" ViscosityLINEST'!D274*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I274-2)+'10A61 Liquid 3\" ViscosityLINEST'!E274*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I274-3)+'10A61 Liquid 3\" ViscosityLINEST'!F274*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I274-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AM108:AM113,'10A61 Liquid 3\"'!AL108:AL113^{1,2,3,4})","v":729.16666666658352},-2368.0555555553228,2823.9583333330957,-1503.4801587300537,781.99761904760248,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B275*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I275+'10A61 Liquid 3\" ViscosityLINEST'!C275*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I275-1)+'10A61 Liquid 3\" ViscosityLINEST'!D275*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I275-2)+'10A61 Liquid 3\" ViscosityLINEST'!E275*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I275-3)+'10A61 Liquid 3\" ViscosityLINEST'!F275*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I275-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AM113:AM121,'10A61 Liquid 3\"'!AL113:AL121^{1,2,3,4})","v":-0.25920745920744903},3.2263144263142993,-13.644289044288481,-11.685366485367522,485.94444444444514,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B276*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I276+'10A61 Liquid 3\" ViscosityLINEST'!C276*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I276-1)+'10A61 Liquid 3\" ViscosityLINEST'!D276*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I276-2)+'10A61 Liquid 3\" ViscosityLINEST'!E276*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I276-3)+'10A61 Liquid 3\" ViscosityLINEST'!F276*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I276-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-15-TA",null,null,null,null,null,null,null,{"$f":"COUNT(B278:H278)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B278*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I278+'10A61 Liquid 3\" ViscosityLINEST'!C278*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I278-1)+'10A61 Liquid 3\" ViscosityLINEST'!D278*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I278-2)+'10A61 Liquid 3\" ViscosityLINEST'!E278*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I278-3)+'10A61 Liquid 3\" ViscosityLINEST'!F278*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I278-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AO6:AO11,'10A61 Liquid 3\"'!AN6:AN11^{1,2,3,4})","v":270.83333333310003},-606.01851851782237,390.20833333256985,-185.45767195730755,1059.9182539681899,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B279*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I279+'10A61 Liquid 3\" ViscosityLINEST'!C279*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I279-1)+'10A61 Liquid 3\" ViscosityLINEST'!D279*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I279-2)+'10A61 Liquid 3\" ViscosityLINEST'!E279*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I279-3)+'10A61 Liquid 3\" ViscosityLINEST'!F279*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I279-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO11:AO19,'10A61 Liquid 3\"'!AN11:AN19^{1,2,3,4})","v":-2.1696969696969224},28.133333333332757,-111.34242424242173,4.0757575757530731,1011.5000000000024,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B280*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I280+'10A61 Liquid 3\" ViscosityLINEST'!C280*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I280-1)+'10A61 Liquid 3\" ViscosityLINEST'!D280*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I280-2)+'10A61 Liquid 3\" ViscosityLINEST'!E280*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I280-3)+'10A61 Liquid 3\" ViscosityLINEST'!F280*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I280-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AO23:AO28,'10A61 Liquid 3\"'!AN23:AN28^{1,2,3,4})","v":-312.49999999975734},1025.4629629622457,-1317.2916666658889,678.37037037000403,702.87222222228525,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B281*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I281+'10A61 Liquid 3\" ViscosityLINEST'!C281*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I281-1)+'10A61 Liquid 3\" ViscosityLINEST'!D281*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I281-2)+'10A61 Liquid 3\" ViscosityLINEST'!E281*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I281-3)+'10A61 Liquid 3\" ViscosityLINEST'!F281*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I281-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO28:AO36,'10A61 Liquid 3\"'!AN28:AN36^{1,2,3,4})","v":-0.8890442890442728},13.001864801864617,-58.480769230768502,-9.832284382285593,832.63333333333389,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B282*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I282+'10A61 Liquid 3\" ViscosityLINEST'!C282*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I282-1)+'10A61 Liquid 3\" ViscosityLINEST'!D282*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I282-2)+'10A61 Liquid 3\" ViscosityLINEST'!E282*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I282-3)+'10A61 Liquid 3\" ViscosityLINEST'!F282*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I282-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AO41:AO46,'10A61 Liquid 3\"'!AN41:AN46^{1,2,3,4})","v":166.66666666651747},-553.7037037032552,629.16666666617186,-345.85582010558295,785.47936507932343,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B283*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I283+'10A61 Liquid 3\" ViscosityLINEST'!C283*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I283-1)+'10A61 Liquid 3\" ViscosityLINEST'!D283*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I283-2)+'10A61 Liquid 3\" ViscosityLINEST'!E283*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I283-3)+'10A61 Liquid 3\" ViscosityLINEST'!F283*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I283-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO46:AO54,'10A61 Liquid 3\"'!AN46:AN54^{1,2,3,4})","v":-3.1473193473192453},38.50924630924505,-159.77074592074038,180.75147630146628,622.26666666667234,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B284*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I284+'10A61 Liquid 3\" ViscosityLINEST'!C284*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I284-1)+'10A61 Liquid 3\" ViscosityLINEST'!D284*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I284-2)+'10A61 Liquid 3\" ViscosityLINEST'!E284*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I284-3)+'10A61 Liquid 3\" ViscosityLINEST'!F284*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I284-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AO57:AO62,'10A61 Liquid 3\"'!AN57:AN62^{1,2,3,4})","v":1874.9999999996494},-5823.1481481471365,6649.5833333322653,-3345.9828042323147,1257.6746031745211,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B285*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I285+'10A61 Liquid 3\" ViscosityLINEST'!C285*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I285-1)+'10A61 Liquid 3\" ViscosityLINEST'!D285*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I285-2)+'10A61 Liquid 3\" ViscosityLINEST'!E285*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I285-3)+'10A61 Liquid 3\" ViscosityLINEST'!F285*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I285-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO62:AO70,'10A61 Liquid 3\"'!AN62:AN70^{1,2,3,4})","v":0.42284382284380795},-3.6539238539236609,9.4033799533790763,-72.574397824396257,679.16666666666595,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B286*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I286+'10A61 Liquid 3\" ViscosityLINEST'!C286*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I286-1)+'10A61 Liquid 3\" ViscosityLINEST'!D286*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I286-2)+'10A61 Liquid 3\" ViscosityLINEST'!E286*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I286-3)+'10A61 Liquid 3\" ViscosityLINEST'!F286*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I286-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AO73:AO78,'10A61 Liquid 3\"'!AN73:AN78^{1,2,3,4})","v":749.99999999999557},-2524.074074074083,3116.6666666667011,-1706.2949735450015,923.05873015873726,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B287*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I287+'10A61 Liquid 3\" ViscosityLINEST'!C287*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I287-1)+'10A61 Liquid 3\" ViscosityLINEST'!D287*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I287-2)+'10A61 Liquid 3\" ViscosityLINEST'!E287*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I287-3)+'10A61 Liquid 3\" ViscosityLINEST'!F287*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I287-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO78:AO86,'10A61 Liquid 3\"'!AN78:AN86^{1,2,3,4})","v":0.78275058275055354},-8.2192696192692498,28.474009324007682,-91.680031080028101,630.01666666666495,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B288*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I288+'10A61 Liquid 3\" ViscosityLINEST'!C288*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I288-1)+'10A61 Liquid 3\" ViscosityLINEST'!D288*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I288-2)+'10A61 Liquid 3\" ViscosityLINEST'!E288*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I288-3)+'10A61 Liquid 3\" ViscosityLINEST'!F288*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I288-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AO92:AO97,'10A61 Liquid 3\"'!AN92:AN97^{1,2,3,4})","v":-958.33333333313556},2676.8518518512724,-2692.0833333327087,1114.7314814811878,375.98888888893981,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B289*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I289+'10A61 Liquid 3\" ViscosityLINEST'!C289*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I289-1)+'10A61 Liquid 3\" ViscosityLINEST'!D289*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I289-2)+'10A61 Liquid 3\" ViscosityLINEST'!E289*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I289-3)+'10A61 Liquid 3\" ViscosityLINEST'!F289*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I289-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO97:AO105,'10A61 Liquid 3\"'!AN97:AN105^{1,2,3,4})","v":0.7724941724941583},-8.6807044807042928,32.467482517481656,-92.793460243458668,585.75555555555479,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B290*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I290+'10A61 Liquid 3\" ViscosityLINEST'!C290*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I290-1)+'10A61 Liquid 3\" ViscosityLINEST'!D290*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I290-2)+'10A61 Liquid 3\" ViscosityLINEST'!E290*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I290-3)+'10A61 Liquid 3\" ViscosityLINEST'!F290*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I290-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AO108:AO113,'10A61 Liquid 3\"'!AN108:AN113^{1,2,3,4})","v":-1520.8333333330997},4426.3888888882175,-4693.5416666659612,2113.0039682536462,174.05952380957797,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B291*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I291+'10A61 Liquid 3\" ViscosityLINEST'!C291*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I291-1)+'10A61 Liquid 3\" ViscosityLINEST'!D291*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I291-2)+'10A61 Liquid 3\" ViscosityLINEST'!E291*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I291-3)+'10A61 Liquid 3\" ViscosityLINEST'!F291*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I291-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AO113:AO121,'10A61 Liquid 3\"'!AN113:AN121^{1,2,3,4})","v":0.59860139860137895},-6.8074592074589582,25.556410256409166,-79.451165501163587,559.54999999999893,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B292*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I292+'10A61 Liquid 3\" ViscosityLINEST'!C292*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I292-1)+'10A61 Liquid 3\" ViscosityLINEST'!D292*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I292-2)+'10A61 Liquid 3\" ViscosityLINEST'!E292*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I292-3)+'10A61 Liquid 3\" ViscosityLINEST'!F292*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I292-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-G-SA",null,null,null,null,null,null,null,{"$f":"COUNT(B294:H294)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B294*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I294+'10A61 Liquid 3\" ViscosityLINEST'!C294*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I294-1)+'10A61 Liquid 3\" ViscosityLINEST'!D294*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I294-2)+'10A61 Liquid 3\" ViscosityLINEST'!E294*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I294-3)+'10A61 Liquid 3\" ViscosityLINEST'!F294*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I294-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AQ6:AQ11,'10A61 Liquid 3\"'!AP6:AP11^{1,2,3,4})","v":1666.6666666660758},-4592.592592590845,4591.666666664767,-2240.8597883588895,1794.2698412696845,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B295*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I295+'10A61 Liquid 3\" ViscosityLINEST'!C295*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I295-1)+'10A61 Liquid 3\" ViscosityLINEST'!D295*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I295-2)+'10A61 Liquid 3\" ViscosityLINEST'!E295*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I295-3)+'10A61 Liquid 3\" ViscosityLINEST'!F295*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I295-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ11:AQ19,'10A61 Liquid 3\"'!AP11:AP19^{1,2,3,4})","v":-0.44662004662006816},1.8577570577573492,26.602564102562727,-272.77656047655785,1463.7222222222204,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B296*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I296+'10A61 Liquid 3\" ViscosityLINEST'!C296*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I296-1)+'10A61 Liquid 3\" ViscosityLINEST'!D296*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I296-2)+'10A61 Liquid 3\" ViscosityLINEST'!E296*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I296-3)+'10A61 Liquid 3\" ViscosityLINEST'!F296*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I296-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AQ23:AQ28,'10A61 Liquid 3\"'!AP23:AP28^{1,2,3,4})","v":2604.166666666662},-8233.7962962963484,9546.8750000001291,-4983.4656084657026,2064.5992063492286,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B297*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I297+'10A61 Liquid 3\" ViscosityLINEST'!C297*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I297-1)+'10A61 Liquid 3\" ViscosityLINEST'!D297*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I297-2)+'10A61 Liquid 3\" ViscosityLINEST'!E297*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I297-3)+'10A61 Liquid 3\" ViscosityLINEST'!F297*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I297-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ28:AQ36,'10A61 Liquid 3\"'!AP28:AP36^{1,2,3,4})","v":0.24009324009319202},-4.6030044030037898,40.288461538458805,-230.59015799015305,1193.7388888888859,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B298*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I298+'10A61 Liquid 3\" ViscosityLINEST'!C298*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I298-1)+'10A61 Liquid 3\" ViscosityLINEST'!D298*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I298-2)+'10A61 Liquid 3\" ViscosityLINEST'!E298*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I298-3)+'10A61 Liquid 3\" ViscosityLINEST'!F298*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I298-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AQ41:AQ46,'10A61 Liquid 3\"'!AP41:AP46^{1,2,3,4})","v":-1041.6666666666786},2634.2592592593051,-2292.9166666667265,636.08597883601158,920.77301587300929,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B299*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I299+'10A61 Liquid 3\" ViscosityLINEST'!C299*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I299-1)+'10A61 Liquid 3\" ViscosityLINEST'!D299*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I299-2)+'10A61 Liquid 3\" ViscosityLINEST'!E299*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I299-3)+'10A61 Liquid 3\" ViscosityLINEST'!F299*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I299-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ46:AQ54,'10A61 Liquid 3\"'!AP46:AP54^{1,2,3,4})","v":0.35151515151512081},-5.8518518518514613,42.051515151513414,-202.80673400673089,1022.6777777777759,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B300*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I300+'10A61 Liquid 3\" ViscosityLINEST'!C300*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I300-1)+'10A61 Liquid 3\" ViscosityLINEST'!D300*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I300-2)+'10A61 Liquid 3\" ViscosityLINEST'!E300*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I300-3)+'10A61 Liquid 3\" ViscosityLINEST'!F300*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I300-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AQ57:AQ62,'10A61 Liquid 3\"'!AP57:AP62^{1,2,3,4})","v":-187.50000000005403},365.27777777793966,-86.875000000178474,-276.95634920626327,938.55476190474656,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B301*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I301+'10A61 Liquid 3\" ViscosityLINEST'!C301*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I301-1)+'10A61 Liquid 3\" ViscosityLINEST'!D301*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I301-2)+'10A61 Liquid 3\" ViscosityLINEST'!E301*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I301-3)+'10A61 Liquid 3\" ViscosityLINEST'!F301*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I301-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ62:AQ70,'10A61 Liquid 3\"'!AP62:AP70^{1,2,3,4})","v":0.19347319347318084},-3.7499611499609542,30.657692307691278,-163.31554001553789,888.1166666666652,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B302*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I302+'10A61 Liquid 3\" ViscosityLINEST'!C302*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I302-1)+'10A61 Liquid 3\" ViscosityLINEST'!D302*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I302-2)+'10A61 Liquid 3\" ViscosityLINEST'!E302*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I302-3)+'10A61 Liquid 3\" ViscosityLINEST'!F302*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I302-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AQ73:AQ78,'10A61 Liquid 3\"'!AP73:AP78^{1,2,3,4})","v":-41.666666666662159},15.740740740730304,201.25000000000838,-355.55026455026712,848.91269841269877,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B303*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I303+'10A61 Liquid 3\" ViscosityLINEST'!C303*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I303-1)+'10A61 Liquid 3\" ViscosityLINEST'!D303*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I303-2)+'10A61 Liquid 3\" ViscosityLINEST'!E303*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I303-3)+'10A61 Liquid 3\" ViscosityLINEST'!F303*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I303-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ78:AQ86,'10A61 Liquid 3\"'!AP78:AP86^{1,2,3,4})","v":0.1151515151515187},-2.5730639730639915,23.328787878787836,-134.66885521885493,781.87777777777774,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B304*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I304+'10A61 Liquid 3\" ViscosityLINEST'!C304*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I304-1)+'10A61 Liquid 3\" ViscosityLINEST'!D304*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I304-2)+'10A61 Liquid 3\" ViscosityLINEST'!E304*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I304-3)+'10A61 Liquid 3\" ViscosityLINEST'!F304*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I304-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AQ92:AQ97,'10A61 Liquid 3\"'!AP92:AP97^{1,2,3,4})","v":-124.99999999999581},282.40740740739784,-120.41666666666008,-173.03835978836074,734.94126984126967,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B305*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I305+'10A61 Liquid 3\" ViscosityLINEST'!C305*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I305-1)+'10A61 Liquid 3\" ViscosityLINEST'!D305*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I305-2)+'10A61 Liquid 3\" ViscosityLINEST'!E305*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I305-3)+'10A61 Liquid 3\" ViscosityLINEST'!F305*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I305-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ97:AQ105,'10A61 Liquid 3\"'!AP97:AP105^{1,2,3,4})","v":7.7855477855482053E-2},-1.8790468790469075,18.280536130536138,-112.98023828023805,694.89444444444416,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B306*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I306+'10A61 Liquid 3\" ViscosityLINEST'!C306*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I306-1)+'10A61 Liquid 3\" ViscosityLINEST'!D306*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I306-2)+'10A61 Liquid 3\" ViscosityLINEST'!E306*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I306-3)+'10A61 Liquid 3\" ViscosityLINEST'!F306*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I306-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AQ108:AQ113,'10A61 Liquid 3\"'!AP108:AP113^{1,2,3,4})","v":-166.66666666667726},427.77777777781495,-310.83333333337953,-58.670634920610695,676.49047619047167,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B307*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I307+'10A61 Liquid 3\" ViscosityLINEST'!C307*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I307-1)+'10A61 Liquid 3\" ViscosityLINEST'!D307*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I307-2)+'10A61 Liquid 3\" ViscosityLINEST'!E307*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I307-3)+'10A61 Liquid 3\" ViscosityLINEST'!F307*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I307-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AQ113:AQ121,'10A61 Liquid 3\"'!AP113:AP121^{1,2,3,4})","v":5.9673659673660923E-2},-1.5713027713027778,16.163869463869446,-104.02990157990146,657.00555555555559,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B308*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I308+'10A61 Liquid 3\" ViscosityLINEST'!C308*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I308-1)+'10A61 Liquid 3\" ViscosityLINEST'!D308*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I308-2)+'10A61 Liquid 3\" ViscosityLINEST'!E308*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I308-3)+'10A61 Liquid 3\" ViscosityLINEST'!F308*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I308-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-20-CA",null,null,null,null,null,null,null,{"$f":"COUNT(B310:H310)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B310*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I310+'10A61 Liquid 3\" ViscosityLINEST'!C310*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I310-1)+'10A61 Liquid 3\" ViscosityLINEST'!D310*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I310-2)+'10A61 Liquid 3\" ViscosityLINEST'!E310*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I310-3)+'10A61 Liquid 3\" ViscosityLINEST'!F310*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I310-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AS6:AS11,'10A61 Liquid 3\"'!AR6:AR11^{1,2,3,4})","v":-416.66666666662354},1657.4074074072932,-2287.4999999998913,1168.0687830687393,1188.6984126984187,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B311*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I311+'10A61 Liquid 3\" ViscosityLINEST'!C311*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I311-1)+'10A61 Liquid 3\" ViscosityLINEST'!D311*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I311-2)+'10A61 Liquid 3\" ViscosityLINEST'!E311*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I311-3)+'10A61 Liquid 3\" ViscosityLINEST'!F311*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I311-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS11:AS19,'10A61 Liquid 3\"'!AR11:AR19^{1,2,3,4})","v":-0.44708624708624456},5.6633514633514341,-23.006410256410099,-92.756746956747321,1421.8388888888892,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B312*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I312+'10A61 Liquid 3\" ViscosityLINEST'!C312*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I312-1)+'10A61 Liquid 3\" ViscosityLINEST'!D312*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I312-2)+'10A61 Liquid 3\" ViscosityLINEST'!E312*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I312-3)+'10A61 Liquid 3\" ViscosityLINEST'!F312*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I312-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AS23:AS28,'10A61 Liquid 3\"'!AR23:AR28^{1,2,3,4})","v":2083.3333333330938},-6490.7407407400715,7420.8333333326491,-3784.7354497351466,1852.301587301539,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B313*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I313+'10A61 Liquid 3\" ViscosityLINEST'!C313*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I313-1)+'10A61 Liquid 3\" ViscosityLINEST'!D313*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I313-2)+'10A61 Liquid 3\" ViscosityLINEST'!E313*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I313-3)+'10A61 Liquid 3\" ViscosityLINEST'!F313*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I313-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS28:AS36,'10A61 Liquid 3\"'!AR28:AR36^{1,2,3,4})","v":-1.1072261072260807},13.427454027453711,-55.638344988343633,5.4673789173764682,1119.2555555555571,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B314*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I314+'10A61 Liquid 3\" ViscosityLINEST'!C314*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I314-1)+'10A61 Liquid 3\" ViscosityLINEST'!D314*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I314-2)+'10A61 Liquid 3\" ViscosityLINEST'!E314*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I314-3)+'10A61 Liquid 3\" ViscosityLINEST'!F314*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I314-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AS41:AS46,'10A61 Liquid 3\"'!AR41:AR46^{1,2,3,4})","v":-541.66666666667163},1256.4814814815038,-922.91666666669892,116.36375661377528,1033.4396825396786,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B315*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I315+'10A61 Liquid 3\" ViscosityLINEST'!C315*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I315-1)+'10A61 Liquid 3\" ViscosityLINEST'!D315*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I315-2)+'10A61 Liquid 3\" ViscosityLINEST'!E315*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I315-3)+'10A61 Liquid 3\" ViscosityLINEST'!F315*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I315-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS46:AS54,'10A61 Liquid 3\"'!AR46:AR54^{1,2,3,4})","v":-0.24009324009320604},3.5309505309501201,-16.961188811187071,-33.872131572134599,988.50555555555729,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B316*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I316+'10A61 Liquid 3\" ViscosityLINEST'!C316*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I316-1)+'10A61 Liquid 3\" ViscosityLINEST'!D316*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I316-2)+'10A61 Liquid 3\" ViscosityLINEST'!E316*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I316-3)+'10A61 Liquid 3\" ViscosityLINEST'!F316*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I316-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AS57:AS62,'10A61 Liquid 3\"'!AR57:AR62^{1,2,3,4})","v":-2187.4999999996035},6743.0555555544088,-7614.374999998784,3663.9444444438845,239.51666666676101,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B317*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I317+'10A61 Liquid 3\" ViscosityLINEST'!C317*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I317-1)+'10A61 Liquid 3\" ViscosityLINEST'!D317*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I317-2)+'10A61 Liquid 3\" ViscosityLINEST'!E317*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I317-3)+'10A61 Liquid 3\" ViscosityLINEST'!F317*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I317-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS62:AS70,'10A61 Liquid 3\"'!AR62:AR70^{1,2,3,4})","v":-4.4289044289038251E-2},0.69375809375803144,-3.0374125874123554,-48.48253043253083,894.41111111111138,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B318*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I318+'10A61 Liquid 3\" ViscosityLINEST'!C318*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I318-1)+'10A61 Liquid 3\" ViscosityLINEST'!D318*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I318-2)+'10A61 Liquid 3\" ViscosityLINEST'!E318*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I318-3)+'10A61 Liquid 3\" ViscosityLINEST'!F318*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I318-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AS73:AS78,'10A61 Liquid 3\"'!AR73:AR78^{1,2,3,4})","v":-2124.9999999997017},6791.6666666658193,-7978.7499999991196,4021.2261904757938,60.042857142922799,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B319*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I319+'10A61 Liquid 3\" ViscosityLINEST'!C319*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I319-1)+'10A61 Liquid 3\" ViscosityLINEST'!D319*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I319-2)+'10A61 Liquid 3\" ViscosityLINEST'!E319*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I319-3)+'10A61 Liquid 3\" ViscosityLINEST'!F319*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I319-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS78:AS86,'10A61 Liquid 3\"'!AR78:AR86^{1,2,3,4})","v":0.34125874125873867},-3.9038591038590678,15.732867132866962,-69.966459466459156,826.05555555555554,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B320*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I320+'10A61 Liquid 3\" ViscosityLINEST'!C320*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I320-1)+'10A61 Liquid 3\" ViscosityLINEST'!D320*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I320-2)+'10A61 Liquid 3\" ViscosityLINEST'!E320*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I320-3)+'10A61 Liquid 3\" ViscosityLINEST'!F320*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I320-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AS92:AS97,'10A61 Liquid 3\"'!AR92:AR97^{1,2,3,4})","v":-250.00000000008421},1120.3703703706342,-1700.8333333336379,1022.3677248678779,517.54920634917812,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B321*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I321+'10A61 Liquid 3\" ViscosityLINEST'!C321*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I321-1)+'10A61 Liquid 3\" ViscosityLINEST'!D321*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I321-2)+'10A61 Liquid 3\" ViscosityLINEST'!E321*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I321-3)+'10A61 Liquid 3\" ViscosityLINEST'!F321*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I321-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS97:AS105,'10A61 Liquid 3\"'!AR97:AR105^{1,2,3,4})","v":0.81818181818179303},-9.3447811447808249,36.853030303028888,-95.992592592590057,776.56111111110977,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B322*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I322+'10A61 Liquid 3\" ViscosityLINEST'!C322*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I322-1)+'10A61 Liquid 3\" ViscosityLINEST'!D322*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I322-2)+'10A61 Liquid 3\" ViscosityLINEST'!E322*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I322-3)+'10A61 Liquid 3\" ViscosityLINEST'!F322*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I322-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AS108:AS113,'10A61 Liquid 3\"'!AR108:AR113^{1,2,3,4})","v":624.99999999972079},-1543.5185185176833,1265.4166666657482,-402.35052910008955,739.32539682531979,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B323*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I323+'10A61 Liquid 3\" ViscosityLINEST'!C323*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I323-1)+'10A61 Liquid 3\" ViscosityLINEST'!D323*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I323-2)+'10A61 Liquid 3\" ViscosityLINEST'!E323*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I323-3)+'10A61 Liquid 3\" ViscosityLINEST'!F323*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I323-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AS113:AS121,'10A61 Liquid 3\"'!AR113:AR121^{1,2,3,4})","v":0.880652680652659},-10.164465164464868,40.476806526805113,-99.740701890699185,752.05555555555384,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B324*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I324+'10A61 Liquid 3\" ViscosityLINEST'!C324*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I324-1)+'10A61 Liquid 3\" ViscosityLINEST'!D324*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I324-2)+'10A61 Liquid 3\" ViscosityLINEST'!E324*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I324-3)+'10A61 Liquid 3\" ViscosityLINEST'!F324*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I324-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-20-TA",null,null,null,null,null,null,null,{"$f":"COUNT(B326:H326)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B326*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I326+'10A61 Liquid 3\" ViscosityLINEST'!C326*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I326-1)+'10A61 Liquid 3\" ViscosityLINEST'!D326*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I326-2)+'10A61 Liquid 3\" ViscosityLINEST'!E326*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I326-3)+'10A61 Liquid 3\" ViscosityLINEST'!F326*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I326-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AU6:AU11,'10A61 Liquid 3\"'!AT6:AT11^{1,2,3,4})","v":624.99999999963177},-1550.9259259248265,1314.5833333321268,-577.16931216873581,1576.6269841268831,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B327*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I327+'10A61 Liquid 3\" ViscosityLINEST'!C327*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I327-1)+'10A61 Liquid 3\" ViscosityLINEST'!D327*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I327-2)+'10A61 Liquid 3\" ViscosityLINEST'!E327*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I327-3)+'10A61 Liquid 3\" ViscosityLINEST'!F327*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I327-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU11:AU19,'10A61 Liquid 3\"'!AT11:AT19^{1,2,3,4})","v":-0.99813519813519691},12.678632478632458,-54.595920745920623,-35.380264180264504,1467.9833333333336,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B328*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I328+'10A61 Liquid 3\" ViscosityLINEST'!C328*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I328-1)+'10A61 Liquid 3\" ViscosityLINEST'!D328*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I328-2)+'10A61 Liquid 3\" ViscosityLINEST'!E328*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I328-3)+'10A61 Liquid 3\" ViscosityLINEST'!F328*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I328-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AU23:AU28,'10A61 Liquid 3\"'!AT23:AT28^{1,2,3,4})","v":1874.9999999999154},-6097.2222222220153,7268.7499999998263,-3858.8492063491485,1959.2619047618987,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B329*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I329+'10A61 Liquid 3\" ViscosityLINEST'!C329*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I329-1)+'10A61 Liquid 3\" ViscosityLINEST'!D329*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I329-2)+'10A61 Liquid 3\" ViscosityLINEST'!E329*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I329-3)+'10A61 Liquid 3\" ViscosityLINEST'!F329*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I329-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU28:AU36,'10A61 Liquid 3\"'!AT28:AT36^{1,2,3,4})","v":-0.68717948717947042},8.409116809116604,-35.000932400931511,-28.382582232583815,1202.7388888888895,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B330*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I330+'10A61 Liquid 3\" ViscosityLINEST'!C330*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I330-1)+'10A61 Liquid 3\" ViscosityLINEST'!D330*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I330-2)+'10A61 Liquid 3\" ViscosityLINEST'!E330*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I330-3)+'10A61 Liquid 3\" ViscosityLINEST'!F330*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I330-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AU41:AU46,'10A61 Liquid 3\"'!AT41:AT46^{1,2,3,4})","v":-1458.3333333331143},4273.1481481475166,-4556.2499999993333,2010.66137566107,730.75396825401947,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B331*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I331+'10A61 Liquid 3\" ViscosityLINEST'!C331*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I331-1)+'10A61 Liquid 3\" ViscosityLINEST'!D331*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I331-2)+'10A61 Liquid 3\" ViscosityLINEST'!E331*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I331-3)+'10A61 Liquid 3\" ViscosityLINEST'!F331*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I331-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU46:AU54,'10A61 Liquid 3\"'!AT46:AT54^{1,2,3,4})","v":-0.4125874125873743},5.392126392125939,-23.945337995336114,-23.55712250712569,1041.2444444444461,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B332*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I332+'10A61 Liquid 3\" ViscosityLINEST'!C332*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I332-1)+'10A61 Liquid 3\" ViscosityLINEST'!D332*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I332-2)+'10A61 Liquid 3\" ViscosityLINEST'!E332*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I332-3)+'10A61 Liquid 3\" ViscosityLINEST'!F332*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I332-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AU57:AU62,'10A61 Liquid 3\"'!AT57:AT62^{1,2,3,4})","v":-2958.3333333327569},9337.9629629612919,-10827.083333331557,5390.0489417981207,-46.349206349067572,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B333*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I333+'10A61 Liquid 3\" ViscosityLINEST'!C333*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I333-1)+'10A61 Liquid 3\" ViscosityLINEST'!D333*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I333-2)+'10A61 Liquid 3\" ViscosityLINEST'!E333*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I333-3)+'10A61 Liquid 3\" ViscosityLINEST'!F333*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I333-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU62:AU70,'10A61 Liquid 3\"'!AT62:AT70^{1,2,3,4})","v":17.809324009323809},-222.07754467754191,958.96282051280684,-1690.6215229214954,1806.5166666666496,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B334*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I334+'10A61 Liquid 3\" ViscosityLINEST'!C334*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I334-1)+'10A61 Liquid 3\" ViscosityLINEST'!D334*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I334-2)+'10A61 Liquid 3\" ViscosityLINEST'!E334*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I334-3)+'10A61 Liquid 3\" ViscosityLINEST'!F334*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I334-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AU73:AU78,'10A61 Liquid 3\"'!AT73:AT78^{1,2,3,4})","v":-708.33333333333928},2556.4814814815195,-3353.7500000000655,1841.1137566138,480.83968253967259,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B335*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I335+'10A61 Liquid 3\" ViscosityLINEST'!C335*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I335-1)+'10A61 Liquid 3\" ViscosityLINEST'!D335*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I335-2)+'10A61 Liquid 3\" ViscosityLINEST'!E335*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I335-3)+'10A61 Liquid 3\" ViscosityLINEST'!F335*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I335-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU78:AU86,'10A61 Liquid 3\"'!AT78:AT86^{1,2,3,4})","v":0.83589743589740439},-9.5398601398597478,37.642540792539059,-103.67412587412275,890.38333333333173,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B336*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I336+'10A61 Liquid 3\" ViscosityLINEST'!C336*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I336-1)+'10A61 Liquid 3\" ViscosityLINEST'!D336*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I336-2)+'10A61 Liquid 3\" ViscosityLINEST'!E336*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I336-3)+'10A61 Liquid 3\" ViscosityLINEST'!F336*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I336-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AU92:AU97,'10A61 Liquid 3\"'!AT92:AT97^{1,2,3,4})","v":1499.9999999995946},-4159.2592592580622,4118.3333333320343,-1746.1216931210795,1040.5412698411633,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B337*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I337+'10A61 Liquid 3\" ViscosityLINEST'!C337*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I337-1)+'10A61 Liquid 3\" ViscosityLINEST'!D337*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I337-2)+'10A61 Liquid 3\" ViscosityLINEST'!E337*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I337-3)+'10A61 Liquid 3\" ViscosityLINEST'!F337*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I337-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU97:AU105,'10A61 Liquid 3\"'!AT97:AT105^{1,2,3,4})","v":0.95804195804192005},-11.253405853405377,45.630186480184356,-111.78816368815981,829.72777777777571,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B338*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I338+'10A61 Liquid 3\" ViscosityLINEST'!C338*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I338-1)+'10A61 Liquid 3\" ViscosityLINEST'!D338*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I338-2)+'10A61 Liquid 3\" ViscosityLINEST'!E338*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I338-3)+'10A61 Liquid 3\" ViscosityLINEST'!F338*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I338-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AU108:AU113,'10A61 Liquid 3\"'!AT108:AT113^{1,2,3,4})","v":1791.6666666663464},-5113.8888888879574,5259.583333332339,-2330.8253968249346,1120.1190476189686,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B339*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I339+'10A61 Liquid 3\" ViscosityLINEST'!C339*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I339-1)+'10A61 Liquid 3\" ViscosityLINEST'!D339*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I339-2)+'10A61 Liquid 3\" ViscosityLINEST'!E339*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I339-3)+'10A61 Liquid 3\" ViscosityLINEST'!F339*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I339-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AU113:AU121,'10A61 Liquid 3\"'!AT113:AT121^{1,2,3,4})","v":0.867132867132829},-10.362496762496288,42.798368298366256,-106.0836182336147,799.42777777777576,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B340*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I340+'10A61 Liquid 3\" ViscosityLINEST'!C340*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I340-1)+'10A61 Liquid 3\" ViscosityLINEST'!D340*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I340-2)+'10A61 Liquid 3\" ViscosityLINEST'!E340*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I340-3)+'10A61 Liquid 3\" ViscosityLINEST'!F340*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I340-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-P-SA",null,null,null,null,null,null,null,{"$f":"COUNT(B342:H342)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B342*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I342+'10A61 Liquid 3\" ViscosityLINEST'!C342*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I342-1)+'10A61 Liquid 3\" ViscosityLINEST'!D342*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I342-2)+'10A61 Liquid 3\" ViscosityLINEST'!E342*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I342-3)+'10A61 Liquid 3\" ViscosityLINEST'!F342*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I342-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AW6:AW11,'10A61 Liquid 3\"'!AV6:AV11^{1,2,3,4})","v":-2083.3333333331466},5731.4814814809524,-5612.4999999994525,2056.9708994706539,1532.3968253968656,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B343*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I343+'10A61 Liquid 3\" ViscosityLINEST'!C343*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I343-1)+'10A61 Liquid 3\" ViscosityLINEST'!D343*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I343-2)+'10A61 Liquid 3\" ViscosityLINEST'!E343*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I343-3)+'10A61 Liquid 3\" ViscosityLINEST'!F343*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I343-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW11:AW19,'10A61 Liquid 3\"'!AV11:AV19^{1,2,3,4})","v":2.186480186480114},-28.183890183889261,133.87762237761822,-417.49948199947431,1934.5555555555507,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B344*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I344+'10A61 Liquid 3\" ViscosityLINEST'!C344*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I344-1)+'10A61 Liquid 3\" ViscosityLINEST'!D344*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I344-2)+'10A61 Liquid 3\" ViscosityLINEST'!E344*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I344-3)+'10A61 Liquid 3\" ViscosityLINEST'!F344*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I344-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AW23:AW28,'10A61 Liquid 3\"'!AV23:AV28^{1,2,3,4})","v":-1458.3333333330311},4550.9259259250493,-5131.2499999990669,2298.9550264545946,1056.6587301588031,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B345*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I345+'10A61 Liquid 3\" ViscosityLINEST'!C345*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I345-1)+'10A61 Liquid 3\" ViscosityLINEST'!D345*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I345-2)+'10A61 Liquid 3\" ViscosityLINEST'!E345*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I345-3)+'10A61 Liquid 3\" ViscosityLINEST'!F345*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I345-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW28:AW36,'10A61 Liquid 3\"'!AV28:AV36^{1,2,3,4})","v":0.91841491841486778},-13.799430199429541,76.385547785544773,-278.39105154104595,1532.9055555555522,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B346*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I346+'10A61 Liquid 3\" ViscosityLINEST'!C346*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I346-1)+'10A61 Liquid 3\" ViscosityLINEST'!D346*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I346-2)+'10A61 Liquid 3\" ViscosityLINEST'!E346*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I346-3)+'10A61 Liquid 3\" ViscosityLINEST'!F346*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I346-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AW41:AW46,'10A61 Liquid 3\"'!AV41:AV46^{1,2,3,4})","v":-2291.6666666662622},7384.2592592581013,-8722.916666665451,4330.6216931211384,417.65873015882289,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B347*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I347+'10A61 Liquid 3\" ViscosityLINEST'!C347*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I347-1)+'10A61 Liquid 3\" ViscosityLINEST'!D347*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I347-2)+'10A61 Liquid 3\" ViscosityLINEST'!E347*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I347-3)+'10A61 Liquid 3\" ViscosityLINEST'!F347*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I347-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW46:AW54,'10A61 Liquid 3\"'!AV46:AV54^{1,2,3,4})","v":0.34219114219111518},-6.1857549857546319,40.614452214450573,-185.67022792022485,1269.8388888888869,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B348*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I348+'10A61 Liquid 3\" ViscosityLINEST'!C348*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I348-1)+'10A61 Liquid 3\" ViscosityLINEST'!D348*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I348-2)+'10A61 Liquid 3\" ViscosityLINEST'!E348*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I348-3)+'10A61 Liquid 3\" ViscosityLINEST'!F348*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I348-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AW57:AW62,'10A61 Liquid 3\"'!AV57:AV62^{1,2,3,4})","v":-62.500000000072234},499.53703703726177,-943.95833333359008,557.45105820118545,924.69920634918321,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B349*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I349+'10A61 Liquid 3\" ViscosityLINEST'!C349*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I349-1)+'10A61 Liquid 3\" ViscosityLINEST'!D349*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I349-2)+'10A61 Liquid 3\" ViscosityLINEST'!E349*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I349-3)+'10A61 Liquid 3\" ViscosityLINEST'!F349*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I349-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW62:AW70,'10A61 Liquid 3\"'!AV62:AV70^{1,2,3,4})","v":-0.35477855477855219},2.6822584822584581,0.91899766899775515,-98.952382802382942,1071.3444444444447,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B350*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I350+'10A61 Liquid 3\" ViscosityLINEST'!C350*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I350-1)+'10A61 Liquid 3\" ViscosityLINEST'!D350*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I350-2)+'10A61 Liquid 3\" ViscosityLINEST'!E350*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I350-3)+'10A61 Liquid 3\" ViscosityLINEST'!F350*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I350-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AW73:AW78,'10A61 Liquid 3\"'!AV73:AV78^{1,2,3,4})","v":1124.9999999996317},-3128.7037037026116,3109.5833333321443,-1382.3915343909716,1140.9936507935531,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B351*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I351+'10A61 Liquid 3\" ViscosityLINEST'!C351*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I351-1)+'10A61 Liquid 3\" ViscosityLINEST'!D351*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I351-2)+'10A61 Liquid 3\" ViscosityLINEST'!E351*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I351-3)+'10A61 Liquid 3\" ViscosityLINEST'!F351*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I351-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW78:AW86,'10A61 Liquid 3\"'!AV78:AV86^{1,2,3,4})","v":-0.66433566433566094},6.6420616420616181,-17.230885780885739,-54.66203056203058,930.53888888888878,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B352*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I352+'10A61 Liquid 3\" ViscosityLINEST'!C352*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I352-1)+'10A61 Liquid 3\" ViscosityLINEST'!D352*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I352-2)+'10A61 Liquid 3\" ViscosityLINEST'!E352*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I352-3)+'10A61 Liquid 3\" ViscosityLINEST'!F352*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I352-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AW92:AW97,'10A61 Liquid 3\"'!AV92:AV97^{1,2,3,4})","v":1312.499999999703},-3786.5740740732049,3944.7916666657334,-1822.5806878302524,1125.923015872942,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B353*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I353+'10A61 Liquid 3\" ViscosityLINEST'!C353*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I353-1)+'10A61 Liquid 3\" ViscosityLINEST'!D353*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I353-2)+'10A61 Liquid 3\" ViscosityLINEST'!E353*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I353-3)+'10A61 Liquid 3\" ViscosityLINEST'!F353*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I353-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW97:AW105,'10A61 Liquid 3\"'!AV97:AV105^{1,2,3,4})","v":-0.75524475524474644},7.9962703962702815,-24.396037296036756,-32.106643356644391,823.35000000000059,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B354*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I354+'10A61 Liquid 3\" ViscosityLINEST'!C354*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I354-1)+'10A61 Liquid 3\" ViscosityLINEST'!D354*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I354-2)+'10A61 Liquid 3\" ViscosityLINEST'!E354*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I354-3)+'10A61 Liquid 3\" ViscosityLINEST'!F354*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I354-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AW108:AW113,'10A61 Liquid 3\"'!AV108:AV113^{1,2,3,4})","v":1208.3333333330947},-3530.5555555548644,3730.4166666659312,-1749.0158730155322,1074.9619047618471,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B355*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I355+'10A61 Liquid 3\" ViscosityLINEST'!C355*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I355-1)+'10A61 Liquid 3\" ViscosityLINEST'!D355*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I355-2)+'10A61 Liquid 3\" ViscosityLINEST'!E355*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I355-3)+'10A61 Liquid 3\" ViscosityLINEST'!F355*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I355-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AW113:AW121,'10A61 Liquid 3\"'!AV113:AV121^{1,2,3,4})","v":-0.79627039627037788},8.6057498057495891,-27.61002331002241,-22.246891996893556,776.18333333333408,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B356*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I356+'10A61 Liquid 3\" ViscosityLINEST'!C356*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I356-1)+'10A61 Liquid 3\" ViscosityLINEST'!D356*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I356-2)+'10A61 Liquid 3\" ViscosityLINEST'!E356*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I356-3)+'10A61 Liquid 3\" ViscosityLINEST'!F356*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I356-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-G-SS",null,null,null,null,null,null,null,{"$f":"COUNT(B358:H358)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B358*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I358+'10A61 Liquid 3\" ViscosityLINEST'!C358*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I358-1)+'10A61 Liquid 3\" ViscosityLINEST'!D358*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I358-2)+'10A61 Liquid 3\" ViscosityLINEST'!E358*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I358-3)+'10A61 Liquid 3\" ViscosityLINEST'!F358*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I358-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!AY6:AY11,'10A61 Liquid 3\"'!AX6:AX11^{1,2,3,4})","v":-208.33333333341307},208.33333333356569,489.58333333308525,-1006.1904761903611,2423.6428571428373,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B359*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I359+'10A61 Liquid 3\" ViscosityLINEST'!C359*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I359-1)+'10A61 Liquid 3\" ViscosityLINEST'!D359*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I359-2)+'10A61 Liquid 3\" ViscosityLINEST'!E359*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I359-3)+'10A61 Liquid 3\" ViscosityLINEST'!F359*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I359-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY11:AY19,'10A61 Liquid 3\"'!AX11:AX19^{1,2,3,4})","v":0.42424242424240804},-8.720538720538455,74.348484848483395,-407.04713804713498,2246.277777777776,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B360*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I360+'10A61 Liquid 3\" ViscosityLINEST'!C360*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I360-1)+'10A61 Liquid 3\" ViscosityLINEST'!D360*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I360-2)+'10A61 Liquid 3\" ViscosityLINEST'!E360*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I360-3)+'10A61 Liquid 3\" ViscosityLINEST'!F360*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I360-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!AY23:AY28,'10A61 Liquid 3\"'!AX23:AX28^{1,2,3,4})","v":-1041.6666666666524},3115.740740740715,-3243.7499999999914,1124.3783068783123,1613.3412698412671,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B361*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I361+'10A61 Liquid 3\" ViscosityLINEST'!C361*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I361-1)+'10A61 Liquid 3\" ViscosityLINEST'!D361*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I361-2)+'10A61 Liquid 3\" ViscosityLINEST'!E361*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I361-3)+'10A61 Liquid 3\" ViscosityLINEST'!F361*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I361-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY28:AY36,'10A61 Liquid 3\"'!AX28:AX36^{1,2,3,4})","v":0.41491841491839698},-6.3056203056200486,46.320512820511553,-268.30238280238029,1795.1111111111095,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B362*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I362+'10A61 Liquid 3\" ViscosityLINEST'!C362*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I362-1)+'10A61 Liquid 3\" ViscosityLINEST'!D362*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I362-2)+'10A61 Liquid 3\" ViscosityLINEST'!E362*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I362-3)+'10A61 Liquid 3\" ViscosityLINEST'!F362*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I362-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!AY41:AY46,'10A61 Liquid 3\"'!AX41:AX46^{1,2,3,4})","v":416.66666666663934},-1157.4074074073344,1287.4999999999293,-893.06878306875365,1704.3015873015827,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B363*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I363+'10A61 Liquid 3\" ViscosityLINEST'!C363*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I363-1)+'10A61 Liquid 3\" ViscosityLINEST'!D363*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I363-2)+'10A61 Liquid 3\" ViscosityLINEST'!E363*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I363-3)+'10A61 Liquid 3\" ViscosityLINEST'!F363*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I363-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY46:AY54,'10A61 Liquid 3\"'!AX46:AX54^{1,2,3,4})","v":0.35431235431232616},-4.7770007770004188,32.275058275056665,-198.65423465423171,1529.3333333333317,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B364*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I364+'10A61 Liquid 3\" ViscosityLINEST'!C364*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I364-1)+'10A61 Liquid 3\" ViscosityLINEST'!D364*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I364-2)+'10A61 Liquid 3\" ViscosityLINEST'!E364*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I364-3)+'10A61 Liquid 3\" ViscosityLINEST'!F364*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I364-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!AY57:AY62,'10A61 Liquid 3\"'!AX57:AX62^{1,2,3,4})","v":1249.9999999997476},-3712.9629629622309,4129.1666666658884,-2219.656084655725,1763.4920634920027,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B365*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I365+'10A61 Liquid 3\" ViscosityLINEST'!C365*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I365-1)+'10A61 Liquid 3\" ViscosityLINEST'!D365*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I365-2)+'10A61 Liquid 3\" ViscosityLINEST'!E365*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I365-3)+'10A61 Liquid 3\" ViscosityLINEST'!F365*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I365-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY62:AY70,'10A61 Liquid 3\"'!AX62:AX70^{1,2,3,4})","v":0.17668997668994726},-2.5667443667439849,20.377039627037895,-153.23558663558347,1346.7499999999984,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B366*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I366+'10A61 Liquid 3\" ViscosityLINEST'!C366*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I366-1)+'10A61 Liquid 3\" ViscosityLINEST'!D366*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I366-2)+'10A61 Liquid 3\" ViscosityLINEST'!E366*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I366-3)+'10A61 Liquid 3\" ViscosityLINEST'!F366*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I366-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!AY73:AY78,'10A61 Liquid 3\"'!AX73:AX78^{1,2,3,4})","v":9.457072377053763E-12},166.66666666663914,-349.99999999997061,83.333333333319729,1198.0000000000025,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B367*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I367+'10A61 Liquid 3\" ViscosityLINEST'!C367*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I367-1)+'10A61 Liquid 3\" ViscosityLINEST'!D367*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I367-2)+'10A61 Liquid 3\" ViscosityLINEST'!E367*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I367-3)+'10A61 Liquid 3\" ViscosityLINEST'!F367*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I367-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY78:AY86,'10A61 Liquid 3\"'!AX78:AX86^{1,2,3,4})","v":0.10675990675987104},-2.0629370629366095,18.570279720277711,-136.482750582747,1218.7499999999982,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B368*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I368+'10A61 Liquid 3\" ViscosityLINEST'!C368*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I368-1)+'10A61 Liquid 3\" ViscosityLINEST'!D368*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I368-2)+'10A61 Liquid 3\" ViscosityLINEST'!E368*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I368-3)+'10A61 Liquid 3\" ViscosityLINEST'!F368*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I368-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!AY92:AY97,'10A61 Liquid 3\"'!AX92:AX97^{1,2,3,4})","v":-1458.3333333328676},4624.9999999986321,-5397.9166666651918,2611.0714285707359,629.07142857154895,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B369*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I369+'10A61 Liquid 3\" ViscosityLINEST'!C369*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I369-1)+'10A61 Liquid 3\" ViscosityLINEST'!D369*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I369-2)+'10A61 Liquid 3\" ViscosityLINEST'!E369*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I369-3)+'10A61 Liquid 3\" ViscosityLINEST'!F369*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I369-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY97:AY105,'10A61 Liquid 3\"'!AX97:AX105^{1,2,3,4})","v":0.11701631701629854},-2.4648018648016223,20.704079254078131,-130.45046620046409,1121.5999999999985,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B370*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I370+'10A61 Liquid 3\" ViscosityLINEST'!C370*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I370-1)+'10A61 Liquid 3\" ViscosityLINEST'!D370*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I370-2)+'10A61 Liquid 3\" ViscosityLINEST'!E370*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I370-3)+'10A61 Liquid 3\" ViscosityLINEST'!F370*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I370-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!AY108:AY113,'10A61 Liquid 3\"'!AX108:AX113^{1,2,3,4})","v":-1333.3333333330229},4285.1851851842912,-5073.333333332389,2493.1481481477144,598.4888888889617,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B371*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I371+'10A61 Liquid 3\" ViscosityLINEST'!C371*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I371-1)+'10A61 Liquid 3\" ViscosityLINEST'!D371*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I371-2)+'10A61 Liquid 3\" ViscosityLINEST'!E371*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I371-3)+'10A61 Liquid 3\" ViscosityLINEST'!F371*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I371-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!AY113:AY121,'10A61 Liquid 3\"'!AX113:AX121^{1,2,3,4})","v":8.5314685314678854E-2},-2.1018907018905999,18.930186480185967,-122.68361823361728,1076.2777777777771,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B372*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I372+'10A61 Liquid 3\" ViscosityLINEST'!C372*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I372-1)+'10A61 Liquid 3\" ViscosityLINEST'!D372*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I372-2)+'10A61 Liquid 3\" ViscosityLINEST'!E372*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I372-3)+'10A61 Liquid 3\" ViscosityLINEST'!F372*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I372-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-P-SS",null,null,null,null,null,null,null,{"$f":"COUNT(B374:H374)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B374*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I374+'10A61 Liquid 3\" ViscosityLINEST'!C374*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I374-1)+'10A61 Liquid 3\" ViscosityLINEST'!D374*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I374-2)+'10A61 Liquid 3\" ViscosityLINEST'!E374*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I374-3)+'10A61 Liquid 3\" ViscosityLINEST'!F374*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I374-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!BA6:BA11,'10A61 Liquid 3\"'!AZ6:AZ11^{1,2,3,4})","v":833.33333333291876},-1648.1481481469036,724.99999999862598,-19.232804232143824,2577.1746031744865,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B375*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I375+'10A61 Liquid 3\" ViscosityLINEST'!C375*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I375-1)+'10A61 Liquid 3\" ViscosityLINEST'!D375*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I375-2)+'10A61 Liquid 3\" ViscosityLINEST'!E375*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I375-3)+'10A61 Liquid 3\" ViscosityLINEST'!F375*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I375-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA11:BA19,'10A61 Liquid 3\"'!AZ11:AZ19^{1,2,3,4})","v":-1.2634032634032635},11.194509194509232,-16.259906759907068,-217.17741517741442,2692.3888888888887,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B376*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I376+'10A61 Liquid 3\" ViscosityLINEST'!C376*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I376-1)+'10A61 Liquid 3\" ViscosityLINEST'!D376*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I376-2)+'10A61 Liquid 3\" ViscosityLINEST'!E376*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I376-3)+'10A61 Liquid 3\" ViscosityLINEST'!F376*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I376-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!BA23:BA28,'10A61 Liquid 3\"'!AZ23:AZ28^{1,2,3,4})","v":3125.0000000000159},-9736.111111111235,11006.250000000218,-5493.1746031747452,3122.8809523809841,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B377*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I377+'10A61 Liquid 3\" ViscosityLINEST'!C377*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I377-1)+'10A61 Liquid 3\" ViscosityLINEST'!D377*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I377-2)+'10A61 Liquid 3\" ViscosityLINEST'!E377*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I377-3)+'10A61 Liquid 3\" ViscosityLINEST'!F377*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I377-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA28:BA36,'10A61 Liquid 3\"'!AZ28:AZ36^{1,2,3,4})","v":-1.6969696969696515},18.949494949494404,-61.454545454543123,-69.797979797983899,2138.3333333333358,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B378*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I378+'10A61 Liquid 3\" ViscosityLINEST'!C378*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I378-1)+'10A61 Liquid 3\" ViscosityLINEST'!D378*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I378-2)+'10A61 Liquid 3\" ViscosityLINEST'!E378*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I378-3)+'10A61 Liquid 3\" ViscosityLINEST'!F378*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I378-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!BA41:BA46,'10A61 Liquid 3\"'!AZ41:AZ46^{1,2,3,4})","v":-1874.9999999998538},5060.185185184775,-4960.4166666662459,1991.005291005104,1536.246031746062,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B379*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I379+'10A61 Liquid 3\" ViscosityLINEST'!C379*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I379-1)+'10A61 Liquid 3\" ViscosityLINEST'!D379*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I379-2)+'10A61 Liquid 3\" ViscosityLINEST'!E379*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I379-3)+'10A61 Liquid 3\" ViscosityLINEST'!F379*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I379-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA46:BA54,'10A61 Liquid 3\"'!AZ46:AZ54^{1,2,3,4})","v":0.11188811188811734},-1.4504014504015015,15.487179487179642,-156.72830872830889,1893.2222222222219,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B380*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I380+'10A61 Liquid 3\" ViscosityLINEST'!C380*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I380-1)+'10A61 Liquid 3\" ViscosityLINEST'!D380*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I380-2)+'10A61 Liquid 3\" ViscosityLINEST'!E380*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I380-3)+'10A61 Liquid 3\" ViscosityLINEST'!F380*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I380-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!BA57:BA62,'10A61 Liquid 3\"'!AZ57:AZ62^{1,2,3,4})","v":-208.33333333336148},560.18518518527242,-477.08333333343234,46.005291005339735,1639.2460317460227,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B381*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I381+'10A61 Liquid 3\" ViscosityLINEST'!C381*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I381-1)+'10A61 Liquid 3\" ViscosityLINEST'!D381*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I381-2)+'10A61 Liquid 3\" ViscosityLINEST'!E381*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I381-3)+'10A61 Liquid 3\" ViscosityLINEST'!F381*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I381-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA62:BA70,'10A61 Liquid 3\"'!AZ62:AZ70^{1,2,3,4})","v":1.6130536130535684},-19.087283087282508,85.172494172491511,-248.01605801605308,1739.4444444444416,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B382*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I382+'10A61 Liquid 3\" ViscosityLINEST'!C382*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I382-1)+'10A61 Liquid 3\" ViscosityLINEST'!D382*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I382-2)+'10A61 Liquid 3\" ViscosityLINEST'!E382*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I382-3)+'10A61 Liquid 3\" ViscosityLINEST'!F382*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I382-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!BA73:BA78,'10A61 Liquid 3\"'!AZ73:AZ78^{1,2,3,4})","v":-833.33333333320832},2592.5925925922343,-2949.9999999996244,1384.431216931046,1213.3015873016161,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B383*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I383+'10A61 Liquid 3\" ViscosityLINEST'!C383*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I383-1)+'10A61 Liquid 3\" ViscosityLINEST'!D383*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I383-2)+'10A61 Liquid 3\" ViscosityLINEST'!E383*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I383-3)+'10A61 Liquid 3\" ViscosityLINEST'!F383*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I383-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA78:BA86,'10A61 Liquid 3\"'!AZ78:AZ86^{1,2,3,4})","v":1.2447552447552075},-14.970732970732495,67.264568764566619,-200.37852887852492,1553.7777777777753,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B384*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I384+'10A61 Liquid 3\" ViscosityLINEST'!C384*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I384-1)+'10A61 Liquid 3\" ViscosityLINEST'!D384*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I384-2)+'10A61 Liquid 3\" ViscosityLINEST'!E384*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I384-3)+'10A61 Liquid 3\" ViscosityLINEST'!F384*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I384-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!BA92:BA97,'10A61 Liquid 3\"'!AZ92:AZ97^{1,2,3,4})","v":-1874.9999999996749},5874.9999999990659,-6768.7499999990168,3335.3571428566934,720.35714285721838,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B385*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I385+'10A61 Liquid 3\" ViscosityLINEST'!C385*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I385-1)+'10A61 Liquid 3\" ViscosityLINEST'!D385*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I385-2)+'10A61 Liquid 3\" ViscosityLINEST'!E385*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I385-3)+'10A61 Liquid 3\" ViscosityLINEST'!F385*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I385-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA97:BA105,'10A61 Liquid 3\"'!AZ97:AZ105^{1,2,3,4})","v":0.87179487179483484},-10.926184926184453,51.08508158507945,-162.91996891996502,1409.1666666666642,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B386*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I386+'10A61 Liquid 3\" ViscosityLINEST'!C386*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I386-1)+'10A61 Liquid 3\" ViscosityLINEST'!D386*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I386-2)+'10A61 Liquid 3\" ViscosityLINEST'!E386*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I386-3)+'10A61 Liquid 3\" ViscosityLINEST'!F386*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I386-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!BA108:BA113,'10A61 Liquid 3\"'!AZ108:AZ113^{1,2,3,4})","v":-1041.6666666664134},3467.59259259186,-4235.4166666658884,2189.7883597880004,854.65873015879106,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B387*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I387+'10A61 Liquid 3\" ViscosityLINEST'!C387*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I387-1)+'10A61 Liquid 3\" ViscosityLINEST'!D387*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I387-2)+'10A61 Liquid 3\" ViscosityLINEST'!E387*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I387-3)+'10A61 Liquid 3\" ViscosityLINEST'!F387*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I387-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BA113:BA121,'10A61 Liquid 3\"'!AZ113:AZ121^{1,2,3,4})","v":0.76456876456872924},-9.673141673141231,45.50582750582555,-148.09686609686256,1346.7777777777756,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B388*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I388+'10A61 Liquid 3\" ViscosityLINEST'!C388*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I388-1)+'10A61 Liquid 3\" ViscosityLINEST'!D388*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I388-2)+'10A61 Liquid 3\" ViscosityLINEST'!E388*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I388-3)+'10A61 Liquid 3\" ViscosityLINEST'!F388*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I388-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-G-CA",null,null,null,null,null,null,null,{"$f":"COUNT(B390:H390)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B390*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I390+'10A61 Liquid 3\" ViscosityLINEST'!C390*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I390-1)+'10A61 Liquid 3\" ViscosityLINEST'!D390*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I390-2)+'10A61 Liquid 3\" ViscosityLINEST'!E390*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I390-3)+'10A61 Liquid 3\" ViscosityLINEST'!F390*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I390-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!BC6:BC11,'10A61 Liquid 3\"'!BB6:BB11^{1,2,3,4})","v":-4.1069696612967943E-11},222.22222222234376,-275.00000000013188,-388.29365079358854,3168.0952380952272,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B391*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I391+'10A61 Liquid 3\" ViscosityLINEST'!C391*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I391-1)+'10A61 Liquid 3\" ViscosityLINEST'!D391*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I391-2)+'10A61 Liquid 3\" ViscosityLINEST'!E391*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I391-3)+'10A61 Liquid 3\" ViscosityLINEST'!F391*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I391-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC11:BC19,'10A61 Liquid 3\"'!BB11:BB19^{1,2,3,4})","v":0.6573426573425819},-8.9857549857540295,62.411421911417641,-394.37477337476565,3068.3888888888846,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B392*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I392+'10A61 Liquid 3\" ViscosityLINEST'!C392*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I392-1)+'10A61 Liquid 3\" ViscosityLINEST'!D392*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I392-2)+'10A61 Liquid 3\" ViscosityLINEST'!E392*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I392-3)+'10A61 Liquid 3\" ViscosityLINEST'!F392*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I392-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!BC23:BC28,'10A61 Liquid 3\"'!BB23:BB28^{1,2,3,4})","v":-1458.333333332934},4847.2222222210594,-5872.9166666654237,2762.7777777772003,1980.1666666667652,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B393*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I393+'10A61 Liquid 3\" ViscosityLINEST'!C393*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I393-1)+'10A61 Liquid 3\" ViscosityLINEST'!D393*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I393-2)+'10A61 Liquid 3\" ViscosityLINEST'!E393*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I393-3)+'10A61 Liquid 3\" ViscosityLINEST'!F393*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I393-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC28:BC36,'10A61 Liquid 3\"'!BB28:BB36^{1,2,3,4})","v":-0.28904428904431945},0.69412069412109867,22.587412587410721,-259.09777259776916,2496.7222222222204,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B394*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I394+'10A61 Liquid 3\" ViscosityLINEST'!C394*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I394-1)+'10A61 Liquid 3\" ViscosityLINEST'!D394*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I394-2)+'10A61 Liquid 3\" ViscosityLINEST'!E394*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I394-3)+'10A61 Liquid 3\" ViscosityLINEST'!F394*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I394-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!BC41:BC46,'10A61 Liquid 3\"'!BB41:BB46^{1,2,3,4})","v":-1666.6666666665449},5462.9629629626415,-6649.9999999996944,3323.9417989416752,1502.7936507936688,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B395*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I395+'10A61 Liquid 3\" ViscosityLINEST'!C395*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I395-1)+'10A61 Liquid 3\" ViscosityLINEST'!D395*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I395-2)+'10A61 Liquid 3\" ViscosityLINEST'!E395*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I395-3)+'10A61 Liquid 3\" ViscosityLINEST'!F395*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I395-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC46:BC54,'10A61 Liquid 3\"'!BB46:BB54^{1,2,3,4})","v":-0.3170163170163216},1.716653716653793,12.80652680652638,-199.12613312613217,2157.2222222222217,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B396*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I396+'10A61 Liquid 3\" ViscosityLINEST'!C396*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I396-1)+'10A61 Liquid 3\" ViscosityLINEST'!D396*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I396-2)+'10A61 Liquid 3\" ViscosityLINEST'!E396*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I396-3)+'10A61 Liquid 3\" ViscosityLINEST'!F396*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I396-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!BC57:BC62,'10A61 Liquid 3\"'!BB57:BB62^{1,2,3,4})","v":3541.6666666657729},-10374.999999997379,11052.083333330513,-5231.785714284395,2786.2142857140598,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B397*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I397+'10A61 Liquid 3\" ViscosityLINEST'!C397*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I397-1)+'10A61 Liquid 3\" ViscosityLINEST'!D397*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I397-2)+'10A61 Liquid 3\" ViscosityLINEST'!E397*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I397-3)+'10A61 Liquid 3\" ViscosityLINEST'!F397*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I397-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC62:BC70,'10A61 Liquid 3\"'!BB62:BB70^{1,2,3,4})","v":-0.32634032634030624},1.9362859362857185,10.566433566434373,-172.39316239316358,1931.3333333333337,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B398*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I398+'10A61 Liquid 3\" ViscosityLINEST'!C398*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I398-1)+'10A61 Liquid 3\" ViscosityLINEST'!D398*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I398-2)+'10A61 Liquid 3\" ViscosityLINEST'!E398*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I398-3)+'10A61 Liquid 3\" ViscosityLINEST'!F398*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I398-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!BC73:BC78,'10A61 Liquid 3\"'!BB73:BB78^{1,2,3,4})","v":3958.3333333328787},-12236.111111109838,13847.916666665362,-6924.6031746025947,2974.4523809522875,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B399*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I399+'10A61 Liquid 3\" ViscosityLINEST'!C399*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I399-1)+'10A61 Liquid 3\" ViscosityLINEST'!D399*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I399-2)+'10A61 Liquid 3\" ViscosityLINEST'!E399*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I399-3)+'10A61 Liquid 3\" ViscosityLINEST'!F399*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I399-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC78:BC86,'10A61 Liquid 3\"'!BB78:BB86^{1,2,3,4})","v":0.47086247086246102},-7.0038850038848501,44.124708624707807,-207.03690753690583,1787.6666666666658,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B400*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I400+'10A61 Liquid 3\" ViscosityLINEST'!C400*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I400-1)+'10A61 Liquid 3\" ViscosityLINEST'!D400*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I400-2)+'10A61 Liquid 3\" ViscosityLINEST'!E400*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I400-3)+'10A61 Liquid 3\" ViscosityLINEST'!F400*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I400-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!BC92:BC97,'10A61 Liquid 3\"'!BB92:BB97^{1,2,3,4})","v":1041.6666666668252},-3615.7407407412502,4518.7500000005994,-2526.1640211643266,2080.3730158730723,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B401*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I401+'10A61 Liquid 3\" ViscosityLINEST'!C401*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I401-1)+'10A61 Liquid 3\" ViscosityLINEST'!D401*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I401-2)+'10A61 Liquid 3\" ViscosityLINEST'!E401*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I401-3)+'10A61 Liquid 3\" ViscosityLINEST'!F401*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I401-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC97:BC105,'10A61 Liquid 3\"'!BB97:BB105^{1,2,3,4})","v":1.5058275058274639},-18.80393680393626,89.381118881116379,-264.17780367779898,1689.888888888886,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B402*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I402+'10A61 Liquid 3\" ViscosityLINEST'!C402*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I402-1)+'10A61 Liquid 3\" ViscosityLINEST'!D402*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I402-2)+'10A61 Liquid 3\" ViscosityLINEST'!E402*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I402-3)+'10A61 Liquid 3\" ViscosityLINEST'!F402*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I402-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!BC108:BC113,'10A61 Liquid 3\"'!BB108:BB113^{1,2,3,4})","v":1.6697699071764136E-10},-500.00000000051153,1125.0000000005764,-926.78571428599673,1748.7142857143365,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B403*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I403+'10A61 Liquid 3\" ViscosityLINEST'!C403*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I403-1)+'10A61 Liquid 3\" ViscosityLINEST'!D403*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I403-2)+'10A61 Liquid 3\" ViscosityLINEST'!E403*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I403-3)+'10A61 Liquid 3\" ViscosityLINEST'!F403*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I403-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BC113:BC121,'10A61 Liquid 3\"'!BB113:BB121^{1,2,3,4})","v":1.6503496503496096},-20.598808598808066,96.769230769228315,-271.77454027453564,1640.0555555555527,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B404*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I404+'10A61 Liquid 3\" ViscosityLINEST'!C404*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I404-1)+'10A61 Liquid 3\" ViscosityLINEST'!D404*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I404-2)+'10A61 Liquid 3\" ViscosityLINEST'!E404*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I404-3)+'10A61 Liquid 3\" ViscosityLINEST'!F404*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I404-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-G-TA",null,null,null,null,null,null,null,{"$f":"COUNT(B406:H406)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B406*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I406+'10A61 Liquid 3\" ViscosityLINEST'!C406*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I406-1)+'10A61 Liquid 3\" ViscosityLINEST'!D406*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I406-2)+'10A61 Liquid 3\" ViscosityLINEST'!E406*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I406-3)+'10A61 Liquid 3\" ViscosityLINEST'!F406*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I406-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!BE6:BE11,'10A61 Liquid 3\"'!BD6:BD11^{1,2,3,4})","v":1041.6666666663914},-3078.7037037029027,3560.4166666658111,-2339.7486772482798,3710.4365079364406,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B407*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I407+'10A61 Liquid 3\" ViscosityLINEST'!C407*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I407-1)+'10A61 Liquid 3\" ViscosityLINEST'!D407*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I407-2)+'10A61 Liquid 3\" ViscosityLINEST'!E407*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I407-3)+'10A61 Liquid 3\" ViscosityLINEST'!F407*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I407-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE11:BE19,'10A61 Liquid 3\"'!BD11:BD19^{1,2,3,4})","v":0.52214452214444618},-7.3162393162383417,54.869463869459501,-386.33760683759897,3234.8333333333289,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B408*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I408+'10A61 Liquid 3\" ViscosityLINEST'!C408*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I408-1)+'10A61 Liquid 3\" ViscosityLINEST'!D408*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I408-2)+'10A61 Liquid 3\" ViscosityLINEST'!E408*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I408-3)+'10A61 Liquid 3\" ViscosityLINEST'!F408*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I408-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!BE23:BE28,'10A61 Liquid 3\"'!BD23:BD28^{1,2,3,4})","v":-3124.9999999992665},10069.444444442315,-11956.249999997732,5877.6984126973621,1533.9761904763689,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B409*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I409+'10A61 Liquid 3\" ViscosityLINEST'!C409*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I409-1)+'10A61 Liquid 3\" ViscosityLINEST'!D409*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I409-2)+'10A61 Liquid 3\" ViscosityLINEST'!E409*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I409-3)+'10A61 Liquid 3\" ViscosityLINEST'!F409*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I409-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE28:BE36,'10A61 Liquid 3\"'!BD28:BD36^{1,2,3,4})","v":0.24242424242419716},-5.5084175084169216,47.696969696967052,-304.83501683501203,2663.4444444444416,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B410*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I410+'10A61 Liquid 3\" ViscosityLINEST'!C410*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I410-1)+'10A61 Liquid 3\" ViscosityLINEST'!D410*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I410-2)+'10A61 Liquid 3\" ViscosityLINEST'!E410*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I410-3)+'10A61 Liquid 3\" ViscosityLINEST'!F410*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I410-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!BE41:BE46,'10A61 Liquid 3\"'!BD41:BD46^{1,2,3,4})","v":-17916.666666660312},52472.222222203469,-56170.833333312985,25803.134920625311,-2091.4761904745246,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B411*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I411+'10A61 Liquid 3\" ViscosityLINEST'!C411*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I411-1)+'10A61 Liquid 3\" ViscosityLINEST'!D411*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I411-2)+'10A61 Liquid 3\" ViscosityLINEST'!E411*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I411-3)+'10A61 Liquid 3\" ViscosityLINEST'!F411*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I411-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE46:BE54,'10A61 Liquid 3\"'!BD46:BD54^{1,2,3,4})","v":-0.72261072261069081},6.3076923076919487,-4.3951048951034988,-178.28904428904647,2273.1666666666679,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B412*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I412+'10A61 Liquid 3\" ViscosityLINEST'!C412*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I412-1)+'10A61 Liquid 3\" ViscosityLINEST'!D412*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I412-2)+'10A61 Liquid 3\" ViscosityLINEST'!E412*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I412-3)+'10A61 Liquid 3\" ViscosityLINEST'!F412*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I412-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!BE57:BE62,'10A61 Liquid 3\"'!BD57:BD62^{1,2,3,4})","v":4791.6666666659257},-14569.444444442322,16214.583333331107,-7979.4841269831122,3428.7380952379253,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B413*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I413+'10A61 Liquid 3\" ViscosityLINEST'!C413*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I413-1)+'10A61 Liquid 3\" ViscosityLINEST'!D413*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I413-2)+'10A61 Liquid 3\" ViscosityLINEST'!E413*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I413-3)+'10A61 Liquid 3\" ViscosityLINEST'!F413*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I413-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE62:BE70,'10A61 Liquid 3\"'!BD62:BD70^{1,2,3,4})","v":0.10722610722610519},-3.3001813001812512,33.367132867132533,-216.87192437192354,2070.4444444444434,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B414*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I414+'10A61 Liquid 3\" ViscosityLINEST'!C414*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I414-1)+'10A61 Liquid 3\" ViscosityLINEST'!D414*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I414-2)+'10A61 Liquid 3\" ViscosityLINEST'!E414*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I414-3)+'10A61 Liquid 3\" ViscosityLINEST'!F414*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I414-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!BE73:BE78,'10A61 Liquid 3\"'!BD73:BD78^{1,2,3,4})","v":3124.9999999999504},-10013.88888888882,11731.250000000013,-6076.4682539683026,2957.9761904762063,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B415*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I415+'10A61 Liquid 3\" ViscosityLINEST'!C415*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I415-1)+'10A61 Liquid 3\" ViscosityLINEST'!D415*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I415-2)+'10A61 Liquid 3\" ViscosityLINEST'!E415*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I415-3)+'10A61 Liquid 3\" ViscosityLINEST'!F415*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I415-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE78:BE86,'10A61 Liquid 3\"'!BD78:BD86^{1,2,3,4})","v":1.4731934731934406},-18.540274540274101,90.207459207457092,-284.3194768194727,1933.6111111111086,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B416*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I416+'10A61 Liquid 3\" ViscosityLINEST'!C416*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I416-1)+'10A61 Liquid 3\" ViscosityLINEST'!D416*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I416-2)+'10A61 Liquid 3\" ViscosityLINEST'!E416*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I416-3)+'10A61 Liquid 3\" ViscosityLINEST'!F416*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I416-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!BE92:BE97,'10A61 Liquid 3\"'!BD92:BD97^{1,2,3,4})","v":-1874.9999999997046},5041.6666666658075,-4868.7499999990814,1873.6904761900491,1424.3571428572163,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B417*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I417+'10A61 Liquid 3\" ViscosityLINEST'!C417*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I417-1)+'10A61 Liquid 3\" ViscosityLINEST'!D417*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I417-2)+'10A61 Liquid 3\" ViscosityLINEST'!E417*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I417-3)+'10A61 Liquid 3\" ViscosityLINEST'!F417*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I417-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE97:BE105,'10A61 Liquid 3\"'!BD97:BD105^{1,2,3,4})","v":1.9207459207458655},-24.180264180263464,113.88344988344662,-312.13675213674605,1815.6666666666631,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B418*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I418+'10A61 Liquid 3\" ViscosityLINEST'!C418*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I418-1)+'10A61 Liquid 3\" ViscosityLINEST'!D418*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I418-2)+'10A61 Liquid 3\" ViscosityLINEST'!E418*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I418-3)+'10A61 Liquid 3\" ViscosityLINEST'!F418*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I418-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!BE108:BE113,'10A61 Liquid 3\"'!BD108:BD113^{1,2,3,4})","v":-2916.6666666663004},8268.5185185174687,-8537.4999999988977,3693.0291005285976,1033.6031746032593,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B419*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I419+'10A61 Liquid 3\" ViscosityLINEST'!C419*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I419-1)+'10A61 Liquid 3\" ViscosityLINEST'!D419*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I419-2)+'10A61 Liquid 3\" ViscosityLINEST'!E419*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I419-3)+'10A61 Liquid 3\" ViscosityLINEST'!F419*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I419-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BE113:BE121,'10A61 Liquid 3\"'!BD113:BD121^{1,2,3,4})","v":1.8927738927738345},-23.96581196581122,113.04195804195467,-305.76612276611655,1755.3333333333301,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B420*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I420+'10A61 Liquid 3\" ViscosityLINEST'!C420*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I420-1)+'10A61 Liquid 3\" ViscosityLINEST'!D420*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I420-2)+'10A61 Liquid 3\" ViscosityLINEST'!E420*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I420-3)+'10A61 Liquid 3\" ViscosityLINEST'!F420*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I420-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-P-CA",null,null,null,null,null,null,null,{"$f":"COUNT(B422:H422)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B422*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I422+'10A61 Liquid 3\" ViscosityLINEST'!C422*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I422-1)+'10A61 Liquid 3\" ViscosityLINEST'!D422*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I422-2)+'10A61 Liquid 3\" ViscosityLINEST'!E422*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I422-3)+'10A61 Liquid 3\" ViscosityLINEST'!F422*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I422-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!BG6:BG11,'10A61 Liquid 3\"'!BF6:BF11^{1,2,3,4})","v":558124.99999990035},-1800402.7777774923,2153431.2499997006,-1131503.2936506574,223879.59523807251,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B423*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I423+'10A61 Liquid 3\" ViscosityLINEST'!C423*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I423-1)+'10A61 Liquid 3\" ViscosityLINEST'!D423*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I423-2)+'10A61 Liquid 3\" ViscosityLINEST'!E423*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I423-3)+'10A61 Liquid 3\" ViscosityLINEST'!F423*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I423-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG11:BG19,'10A61 Liquid 3\"'!BF11:BF19^{1,2,3,4})","v":0.39160839160838357},-5.0629370629369372,40.477855477854781,-330.35547785547629,3810.8333333333321,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B424*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I424+'10A61 Liquid 3\" ViscosityLINEST'!C424*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I424-1)+'10A61 Liquid 3\" ViscosityLINEST'!D424*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I424-2)+'10A61 Liquid 3\" ViscosityLINEST'!E424*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I424-3)+'10A61 Liquid 3\" ViscosityLINEST'!F424*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I424-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!BG23:BG28,'10A61 Liquid 3\"'!BF23:BF28^{1,2,3,4})","v":-2499.9999999995575},7888.888888887619,-9124.999999998663,4443.2539682533561,2182.8095238096275,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B425*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I425+'10A61 Liquid 3\" ViscosityLINEST'!C425*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I425-1)+'10A61 Liquid 3\" ViscosityLINEST'!D425*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I425-2)+'10A61 Liquid 3\" ViscosityLINEST'!E425*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I425-3)+'10A61 Liquid 3\" ViscosityLINEST'!F425*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I425-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG28:BG36,'10A61 Liquid 3\"'!BF28:BF36^{1,2,3,4})","v":2.4568764568763761},-29.974099974098948,135.96153846153385,-405.12768712767866,3186.7222222222172,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B426*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I426+'10A61 Liquid 3\" ViscosityLINEST'!C426*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I426-1)+'10A61 Liquid 3\" ViscosityLINEST'!D426*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I426-2)+'10A61 Liquid 3\" ViscosityLINEST'!E426*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I426-3)+'10A61 Liquid 3\" ViscosityLINEST'!F426*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I426-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!BG41:BG46,'10A61 Liquid 3\"'!BF41:BF46^{1,2,3,4})","v":-1666.6666666664244},5592.5925925919082,-6941.6666666659612,3664.4312169309019,1848.3015873016393,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B427*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I427+'10A61 Liquid 3\" ViscosityLINEST'!C427*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I427-1)+'10A61 Liquid 3\" ViscosityLINEST'!D427*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I427-2)+'10A61 Liquid 3\" ViscosityLINEST'!E427*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I427-3)+'10A61 Liquid 3\" ViscosityLINEST'!F427*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I427-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG46:BG54,'10A61 Liquid 3\"'!BF46:BF54^{1,2,3,4})","v":-3.7296037296061652E-2},-0.62988862988830951,12.312354312352841,-155.66070966070694,2641.8888888888873,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B428*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I428+'10A61 Liquid 3\" ViscosityLINEST'!C428*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I428-1)+'10A61 Liquid 3\" ViscosityLINEST'!D428*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I428-2)+'10A61 Liquid 3\" ViscosityLINEST'!E428*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I428-3)+'10A61 Liquid 3\" ViscosityLINEST'!F428*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I428-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!BG57:BG62,'10A61 Liquid 3\"'!BF57:BF62^{1,2,3,4})","v":2291.666666666099},-6550.9259259242617,6697.9166666648744,-2937.1693121684721,2724.6269841268395,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B429*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I429+'10A61 Liquid 3\" ViscosityLINEST'!C429*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I429-1)+'10A61 Liquid 3\" ViscosityLINEST'!D429*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I429-2)+'10A61 Liquid 3\" ViscosityLINEST'!E429*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I429-3)+'10A61 Liquid 3\" ViscosityLINEST'!F429*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I429-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG62:BG70,'10A61 Liquid 3\"'!BF62:BF70^{1,2,3,4})","v":-1.3053613053612978},15.112147112147023,-56.400932400931993,-13.747733747734596,2283.8888888888891,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B430*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I430+'10A61 Liquid 3\" ViscosityLINEST'!C430*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I430-1)+'10A61 Liquid 3\" ViscosityLINEST'!D430*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I430-2)+'10A61 Liquid 3\" ViscosityLINEST'!E430*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I430-3)+'10A61 Liquid 3\" ViscosityLINEST'!F430*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I430-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!BG73:BG78,'10A61 Liquid 3\"'!BF73:BF78^{1,2,3,4})","v":2083.3333333331816},-6287.0370370366254,6837.4999999995935,-3200.3439153437421,2590.5079365079096,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B431*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I431+'10A61 Liquid 3\" ViscosityLINEST'!C431*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I431-1)+'10A61 Liquid 3\" ViscosityLINEST'!D431*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I431-2)+'10A61 Liquid 3\" ViscosityLINEST'!E431*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I431-3)+'10A61 Liquid 3\" ViscosityLINEST'!F431*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I431-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG78:BG86,'10A61 Liquid 3\"'!BF78:BF86^{1,2,3,4})","v":-1.5617715617715469},18.855736855736666,-75.518648018647141,38.907277907276153,2045.0555555555563,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B432*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I432+'10A61 Liquid 3\" ViscosityLINEST'!C432*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I432-1)+'10A61 Liquid 3\" ViscosityLINEST'!D432*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I432-2)+'10A61 Liquid 3\" ViscosityLINEST'!E432*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I432-3)+'10A61 Liquid 3\" ViscosityLINEST'!F432*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I432-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!BG92:BG97,'10A61 Liquid 3\"'!BF92:BF97^{1,2,3,4})","v":1458.3333333333687},-4569.4444444445853,5147.9166666668607,-2488.0555555556675,2316.1666666666897,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B433*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I433+'10A61 Liquid 3\" ViscosityLINEST'!C433*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I433-1)+'10A61 Liquid 3\" ViscosityLINEST'!D433*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I433-2)+'10A61 Liquid 3\" ViscosityLINEST'!E433*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I433-3)+'10A61 Liquid 3\" ViscosityLINEST'!F433*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I433-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG97:BG105,'10A61 Liquid 3\"'!BF97:BF105^{1,2,3,4})","v":-0.91375291375290701},11.705775705775622,-49.074592074591685,11.391737891737085,1893.0555555555563,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B434*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I434+'10A61 Liquid 3\" ViscosityLINEST'!C434*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I434-1)+'10A61 Liquid 3\" ViscosityLINEST'!D434*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I434-2)+'10A61 Liquid 3\" ViscosityLINEST'!E434*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I434-3)+'10A61 Liquid 3\" ViscosityLINEST'!F434*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I434-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!BG108:BG113,'10A61 Liquid 3\"'!BF108:BF113^{1,2,3,4})","v":208.33333333339036},-875.00000000018008,1160.4166666668752,-622.14285714296182,1925.357142857162,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B435*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I435+'10A61 Liquid 3\" ViscosityLINEST'!C435*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I435-1)+'10A61 Liquid 3\" ViscosityLINEST'!D435*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I435-2)+'10A61 Liquid 3\" ViscosityLINEST'!E435*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I435-3)+'10A61 Liquid 3\" ViscosityLINEST'!F435*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I435-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BG113:BG121,'10A61 Liquid 3\"'!BF113:BF121^{1,2,3,4})","v":-0.81118881118880426},10.407666407666323,-43.857808857808465,8.0950530950522861,1824.111111111112,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B436*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I436+'10A61 Liquid 3\" ViscosityLINEST'!C436*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I436-1)+'10A61 Liquid 3\" ViscosityLINEST'!D436*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I436-2)+'10A61 Liquid 3\" ViscosityLINEST'!E436*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I436-3)+'10A61 Liquid 3\" ViscosityLINEST'!F436*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I436-4)","v":{"$error":"#NUM!"}}]
[]
["1/4-41-P-TA",null,null,null,null,null,null,null,{"$f":"COUNT(B438:H438)-1","v":-1},{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B438*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I438+'10A61 Liquid 3\" ViscosityLINEST'!C438*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I438-1)+'10A61 Liquid 3\" ViscosityLINEST'!D438*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I438-2)+'10A61 Liquid 3\" ViscosityLINEST'!E438*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I438-3)+'10A61 Liquid 3\" ViscosityLINEST'!F438*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I438-4)","v":{"$error":"#DIV/0!"}}]
[0.4,{"$f":"LINEST('10A61 Liquid 3\"'!BI6:BI11,'10A61 Liquid 3\"'!BH6:BH11^{1,2,3,4})","v":-2083.3333333333208},5657.4074074074015,-5495.833333333363,2039.8544973545283,3613.9841269841195,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B439*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I439+'10A61 Liquid 3\" ViscosityLINEST'!C439*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I439-1)+'10A61 Liquid 3\" ViscosityLINEST'!D439*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I439-2)+'10A61 Liquid 3\" ViscosityLINEST'!E439*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I439-3)+'10A61 Liquid 3\" ViscosityLINEST'!F439*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I439-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI11:BI19,'10A61 Liquid 3\"'!BH11:BH19^{1,2,3,4})","v":2.3636363636362958},-28.168350168349296,133.8030303030263,-486.8215488215414,4108.3888888888841,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B440*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I440+'10A61 Liquid 3\" ViscosityLINEST'!C440*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I440-1)+'10A61 Liquid 3\" ViscosityLINEST'!D440*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I440-2)+'10A61 Liquid 3\" ViscosityLINEST'!E440*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I440-3)+'10A61 Liquid 3\" ViscosityLINEST'!F440*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I440-4)","v":{"$error":"#NUM!"}}]
[0.6,{"$f":"LINEST('10A61 Liquid 3\"'!BI23:BI28,'10A61 Liquid 3\"'!BH23:BH28^{1,2,3,4})","v":-3958.3333333326268},12587.962962960935,-14739.583333331198,7380.0132275122514,1786.8650793652432,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B441*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I441+'10A61 Liquid 3\" ViscosityLINEST'!C441*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I441-1)+'10A61 Liquid 3\" ViscosityLINEST'!D441*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I441-2)+'10A61 Liquid 3\" ViscosityLINEST'!E441*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I441-3)+'10A61 Liquid 3\" ViscosityLINEST'!F441*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I441-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI28:BI36,'10A61 Liquid 3\"'!BH28:BH36^{1,2,3,4})","v":1.8648018648017852},-23.45506345506244,110.04895104894651,-362.72714322713495,3332.0555555555507,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B442*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I442+'10A61 Liquid 3\" ViscosityLINEST'!C442*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I442-1)+'10A61 Liquid 3\" ViscosityLINEST'!D442*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I442-2)+'10A61 Liquid 3\" ViscosityLINEST'!E442*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I442-3)+'10A61 Liquid 3\" ViscosityLINEST'!F442*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I442-4)","v":{"$error":"#NUM!"}}]
[0.8,{"$f":"LINEST('10A61 Liquid 3\"'!BI41:BI46,'10A61 Liquid 3\"'!BH41:BH46^{1,2,3,4})","v":833.33333333303676},-1925.9259259250393,1324.9999999990264,-259.312169311704,2670.9841269840454,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B443*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I443+'10A61 Liquid 3\" ViscosityLINEST'!C443*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I443-1)+'10A61 Liquid 3\" ViscosityLINEST'!D443*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I443-2)+'10A61 Liquid 3\" ViscosityLINEST'!E443*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I443-3)+'10A61 Liquid 3\" ViscosityLINEST'!F443*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I443-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI46:BI54,'10A61 Liquid 3\"'!BH46:BH54^{1,2,3,4})","v":-0.94638694638694332},9.962703962703932,-30.217948717948595,-88.26340326340349,2754.8333333333335,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B444*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I444+'10A61 Liquid 3\" ViscosityLINEST'!C444*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I444-1)+'10A61 Liquid 3\" ViscosityLINEST'!D444*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I444-2)+'10A61 Liquid 3\" ViscosityLINEST'!E444*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I444-3)+'10A61 Liquid 3\" ViscosityLINEST'!F444*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I444-4)","v":{"$error":"#NUM!"}}]
[1,{"$f":"LINEST('10A61 Liquid 3\"'!BI57:BI62,'10A61 Liquid 3\"'!BH57:BH62^{1,2,3,4})","v":2708.3333333329979},-8004.6296296286764,8527.0833333323408,-3912.6322751318271,3040.8492063491326,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B445*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I445+'10A61 Liquid 3\" ViscosityLINEST'!C445*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I445-1)+'10A61 Liquid 3\" ViscosityLINEST'!D445*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I445-2)+'10A61 Liquid 3\" ViscosityLINEST'!E445*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I445-3)+'10A61 Liquid 3\" ViscosityLINEST'!F445*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I445-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI62:BI70,'10A61 Liquid 3\"'!BH62:BH70^{1,2,3,4})","v":-1.8275058275058109},21.876197876197669,-86.846153846152873,40.182465682463693,2387.6111111111122,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B446*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I446+'10A61 Liquid 3\" ViscosityLINEST'!C446*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I446-1)+'10A61 Liquid 3\" ViscosityLINEST'!D446*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I446-2)+'10A61 Liquid 3\" ViscosityLINEST'!E446*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I446-3)+'10A61 Liquid 3\" ViscosityLINEST'!F446*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I446-4)","v":{"$error":"#NUM!"}}]
[1.2,{"$f":"LINEST('10A61 Liquid 3\"'!BI73:BI78,'10A61 Liquid 3\"'!BH73:BH78^{1,2,3,4})","v":1458.3333333333853},-4643.5185185187083,5289.5833333335831,-2576.9576719578113,2618.4682539682817,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B447*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I447+'10A61 Liquid 3\" ViscosityLINEST'!C447*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I447-1)+'10A61 Liquid 3\" ViscosityLINEST'!D447*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I447-2)+'10A61 Liquid 3\" ViscosityLINEST'!E447*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I447-3)+'10A61 Liquid 3\" ViscosityLINEST'!F447*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I447-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI78:BI86,'10A61 Liquid 3\"'!BH78:BH86^{1,2,3,4})","v":-1.1421911421911335},14.44030044030033,-60.168997668997136,18.283864283863153,2175.9444444444453,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B448*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I448+'10A61 Liquid 3\" ViscosityLINEST'!C448*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I448-1)+'10A61 Liquid 3\" ViscosityLINEST'!D448*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I448-2)+'10A61 Liquid 3\" ViscosityLINEST'!E448*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I448-3)+'10A61 Liquid 3\" ViscosityLINEST'!F448*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I448-4)","v":{"$error":"#NUM!"}}]
[1.4,{"$f":"LINEST('10A61 Liquid 3\"'!BI92:BI97,'10A61 Liquid 3\"'!BH92:BH97^{1,2,3,4})","v":-416.66666666658972},935.18518518495739,-762.49999999975239,266.36243386231661,1956.6031746031947,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B449*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I449+'10A61 Liquid 3\" ViscosityLINEST'!C449*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I449-1)+'10A61 Liquid 3\" ViscosityLINEST'!D449*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I449-2)+'10A61 Liquid 3\" ViscosityLINEST'!E449*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I449-3)+'10A61 Liquid 3\" ViscosityLINEST'!F449*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I449-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI97:BI105,'10A61 Liquid 3\"'!BH97:BH105^{1,2,3,4})","v":-0.84848484848483618},10.976430976430825,-46.7878787878781,9.4225589225576218,2006.9444444444455,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B450*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I450+'10A61 Liquid 3\" ViscosityLINEST'!C450*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I450-1)+'10A61 Liquid 3\" ViscosityLINEST'!D450*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I450-2)+'10A61 Liquid 3\" ViscosityLINEST'!E450*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I450-3)+'10A61 Liquid 3\" ViscosityLINEST'!F450*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I450-4)","v":{"$error":"#NUM!"}}]
[1.5,{"$f":"LINEST('10A61 Liquid 3\"'!BI108:BI113,'10A61 Liquid 3\"'!BH108:BH113^{1,2,3,4})","v":-1666.6666666665683},4629.6296296293622,-4749.9999999997372,2132.2751322750214,1562.7936507936674,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B451*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I451+'10A61 Liquid 3\" ViscosityLINEST'!C451*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I451-1)+'10A61 Liquid 3\" ViscosityLINEST'!D451*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I451-2)+'10A61 Liquid 3\" ViscosityLINEST'!E451*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I451-3)+'10A61 Liquid 3\" ViscosityLINEST'!F451*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I451-4)","v":{"$error":"#NUM!"}}]
[null,{"$f":"LINEST('10A61 Liquid 3\"'!BI113:BI121,'10A61 Liquid 3\"'!BH113:BH121^{1,2,3,4})","v":-0.84382284382282735},10.967624967624761,-47.425407925407008,16.409608909607226,1929.2222222222233,{"$error":"#N/A"},{"$error":"#N/A"},4,{"$f":"'10A61 Liquid 3\" ViscosityLINEST'!B452*'10A61 Liquid 3\"'!$B$4^'10A61 Liquid 3\" ViscosityLINEST'!I452+'10A61 Liquid 3\" ViscosityLINEST'!C452*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I452-1)+'10A61 Liquid 3\" ViscosityLINEST'!D452*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I452-2)+'10A61 Liquid 3\" ViscosityLINEST'!E452*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I452-3)+'10A61 Liquid 3\" ViscosityLINEST'!F452*'10A61 Liquid 3\"'!$B$4^('10A61 Liquid 3\" ViscosityLINEST'!I452-4)","v":{"$error":"#NUM!"}}]

{"sheet":"10A61 3\" Density LINEST","index":3,"n_rows":451,"n_cols":12,"rows_kept":451,"cut":false,"hidden":true,"merged":[[17,6,17,8],[33,6,33,8],[49,6,49,8],[65,6,65,8],[81,6,81,8],[97,6,97,8],[113,6,113,8],[129,6,129,8],[145,6,145,8],[161,6,161,8],[177,6,177,8],[193,6,193,8],[209,6,209,8],[225,6,225,8],[241,6,241,8],[257,6,257,8],[273,6,273,8],[289,6,289,8],[305,6,305,8],[321,6,321,8],[417,6,417,8],[433,6,433,8],[449,6,449,8],[337,6,337,8],[353,6,353,8],[369,6,369,8],[385,6,385,8],[401,6,401,8]]}
[]
[null,"Density","Viscosity"]
[null,{"$f":"'Modified Inputs'!M2","v":0},{"$f":"'Modified Inputs'!G2","v":0}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-08-BG"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D14,\"\",\nIF(D19>1.5001,'10A61 Liquid 3\" ViscosityLINEST'!J8,'10A61 Liquid 3\" ViscosityLINEST'!J7))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 1.5","TOP"]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D32,\"\",\nIF(D19>1.9001,'10A61 Liquid 3\" ViscosityLINEST'!J10,'10A61 Liquid 3\" ViscosityLINEST'!J9))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 1.9","TOP"]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D52,\"\",\nIF(D19>2.001,'10A61 Liquid 3\" ViscosityLINEST'!J12,'10A61 Liquid 3\" ViscosityLINEST'!J11))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 2","BOTTOM"]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D69,\"\",\nIF(D19>2.001,'10A61 Liquid 3\" ViscosityLINEST'!J14,'10A61 Liquid 3\" ViscosityLINEST'!J13))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 2","BOTTOM"]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D84,\"\",\nIF(D19>2.001,'10A61 Liquid 3\" ViscosityLINEST'!J16,'10A61 Liquid 3\" ViscosityLINEST'!J15))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 2","BOTTOM"]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D104,\"\",\nIF(D19>2.2001,'10A61 Liquid 3\" ViscosityLINEST'!J18,'10A61 Liquid 3\" ViscosityLINEST'!J17))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 2.2","BOTTOM"]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D19>'10A61 Liquid 3\"'!D119,\"\",\nIF(D19>2.001,'10A61 Liquid 3\" ViscosityLINEST'!J20,'10A61 Liquid 3\" ViscosityLINEST'!J19))","v":{"$error":"#NUM!"}},null,null,"OVERLAP AT 2","BOTTOM"]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G19*C19^2+H19*C19+I19","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E10=\"\")),LINEST(E10:E16,C10:C16^{1,2}),\nIF(AND(E10=\"\",NOT(E11=\"\"),NOT(E12=\"\"),NOT(E13=\"\"),NOT(E14=\"\"),NOT(E15=\"\"),NOT(E16=\"\")),LINEST(E11:E16,C11:C16^{1,2}),\nIF(AND(E11=\"\",NOT(E12=\"\"),NOT(E13=\"\"),NOT(E14=\"\"),NOT(E15=\"\"),NOT(E16=\"\")),LINEST(E12:E16,C12:C16^{1,2}),\nIF(AND(E12=\"\",NOT(E13=\"\"),NOT(E14=\"\"),NOT(E15=\"\"),NOT(E16=\"\")),LINEST(E13:E16,C13:C16^{1,2}),\nIF(AND(E13=\"\",NOT(E14=\"\"),NOT(E15=\"\"),NOT(E16=\"\")),LINEST(E14:E16,C14:C16^{1,2}),\nIF(AND(E14=\"\",NOT(E15=\"\"),NOT(E16=\"\")),LINEST(E15:E16,C15:C16^{1,2}),\nIF(AND(E15=\"\",NOT(E16=\"\")),LINEST(E16,C16^{1,2}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-08-SA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H18,\"\",\nIF(D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J24,'10A61 Liquid 3\" ViscosityLINEST'!J23))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H36,\"\",\nIF('10A61 3\" Density LINEST'!D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J26,'10A61 Liquid 3\" ViscosityLINEST'!J25))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H54,\"\",\nIF('10A61 3\" Density LINEST'!D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J28,'10A61 Liquid 3\" ViscosityLINEST'!J27))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H70,\"\",\nIF('10A61 3\" Density LINEST'!D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J30,'10A61 Liquid 3\" ViscosityLINEST'!J29))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H86,\"\",\nIF('10A61 3\" Density LINEST'!D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J32,'10A61 Liquid 3\" ViscosityLINEST'!J31))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H105,\"\",\nIF('10A61 3\" Density LINEST'!D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J34,'10A61 Liquid 3\" ViscosityLINEST'!J33))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D35>'10A61 Liquid 3\"'!H121,\"\",\nIF('10A61 3\" Density LINEST'!D35>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J36,'10A61 Liquid 3\" ViscosityLINEST'!J35))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G35*C35^2+H35*C35+I35","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E26=\"\")),LINEST(E26:E32,C26:C32^{1,2}),\nIF(AND(E26=\"\",NOT(E27=\"\"),NOT(E28=\"\"),NOT(E29=\"\"),NOT(E30=\"\"),NOT(E31=\"\"),NOT(E32=\"\")),LINEST(E27:E32,C27:C32^{1,2}),\nIF(AND(E27=\"\",NOT(E28=\"\"),NOT(E29=\"\"),NOT(E30=\"\"),NOT(E31=\"\"),NOT(E32=\"\")),LINEST(E28:E32,C28:C32^{1,2}),\nIF(AND(E28=\"\",NOT(E29=\"\"),NOT(E30=\"\"),NOT(E31=\"\"),NOT(E32=\"\")),LINEST(E29:E32,C29:C32^{1,2}),\nIF(AND(E29=\"\",NOT(E30=\"\"),NOT(E31=\"\"),NOT(E32=\"\")),LINEST(E30:E32,C30:C32^{1,2}),\nIF(AND(E30=\"\",NOT(E31=\"\"),NOT(E32=\"\")),LINEST(E31:E32,C31:C32^{1,2}),\nIF(AND(E31=\"\",NOT(E32=\"\")),LINEST(E32,C32^{1,2}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-08-SS"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J40,'10A61 Liquid 3\" ViscosityLINEST'!J39))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J42,'10A61 Liquid 3\" ViscosityLINEST'!J41))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J44,'10A61 Liquid 3\" ViscosityLINEST'!J43))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J46,'10A61 Liquid 3\" ViscosityLINEST'!J45))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J48,'10A61 Liquid 3\" ViscosityLINEST'!J47))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J50,'10A61 Liquid 3\" ViscosityLINEST'!J49))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D51>5,\"\",\nIF(D51>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J52,'10A61 Liquid 3\" ViscosityLINEST'!J51))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G51*C51^4+H51*C51^3+I51*C51^2+J51*C51+K51","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E42=\"\")),LINEST(E42:E48,C42:C48^{1,2,3,4}),\nIF(AND(E42=\"\",NOT(E43=\"\"),NOT(E44=\"\"),NOT(E45=\"\"),NOT(E46=\"\"),NOT(E47=\"\"),NOT(E48=\"\")),LINEST(E43:E48,C43:C48^{1,2,3,4}),\nIF(AND(E43=\"\",NOT(E44=\"\"),NOT(E45=\"\"),NOT(E46=\"\"),NOT(E47=\"\"),NOT(E48=\"\")),LINEST(E44:E48,C44:C48^{1,2,3,4}),\nIF(AND(E44=\"\",NOT(E45=\"\"),NOT(E46=\"\"),NOT(E47=\"\"),NOT(E48=\"\")),LINEST(E45:E48,C45:C48^{1,2,3,4}),\nIF(AND(E45=\"\",NOT(E46=\"\"),NOT(E47=\"\"),NOT(E48=\"\")),LINEST(E46:E48,C46:C48^{1,2,3,4}),\nIF(AND(E46=\"\",NOT(E47=\"\"),NOT(E48=\"\")),LINEST(E47:E48,C47:C48^{1,2,3,4}),\nIF(AND(E47=\"\",NOT(E48=\"\")),LINEST(E48,C48^{1,2,3,4}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-08-CA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J56,'10A61 Liquid 3\" ViscosityLINEST'!J55))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J58,'10A61 Liquid 3\" ViscosityLINEST'!J57))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J60,'10A61 Liquid 3\" ViscosityLINEST'!J59))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J62,'10A61 Liquid 3\" ViscosityLINEST'!J61))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J64,'10A61 Liquid 3\" ViscosityLINEST'!J63))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J66,'10A61 Liquid 3\" ViscosityLINEST'!J65))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D67>5,\"\",\nIF(D67>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J68,'10A61 Liquid 3\" ViscosityLINEST'!J67))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G67*C67^3+H67*C67^2+I67*C67+J67","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E58=\"\")),LINEST(E58:E64,C58:C64^{1,2,3}),\nIF(AND(E58=\"\",NOT(E59=\"\"),NOT(E60=\"\"),NOT(E61=\"\"),NOT(E62=\"\"),NOT(E63=\"\"),NOT(E64=\"\")),LINEST(E59:E64,C59:C64^{1,2,3}),\nIF(AND(E59=\"\",NOT(E60=\"\"),NOT(E61=\"\"),NOT(E62=\"\"),NOT(E63=\"\"),NOT(E64=\"\")),LINEST(E60:E64,C60:C64^{1,2,3}),\nIF(AND(E60=\"\",NOT(E61=\"\"),NOT(E62=\"\"),NOT(E63=\"\"),NOT(E64=\"\")),LINEST(E61:E64,C61:C64^{1,2,3}),\nIF(AND(E61=\"\",NOT(E62=\"\"),NOT(E63=\"\"),NOT(E64=\"\")),LINEST(E62:E64,C62:C64^{1,2,3}),\nIF(AND(E62=\"\",NOT(E63=\"\"),NOT(E64=\"\")),LINEST(E63:E64,C63:C64^{1,2,3}),\nIF(AND(E63=\"\",NOT(E64=\"\")),LINEST(E64,C64^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-08-TA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J72,'10A61 Liquid 3\" ViscosityLINEST'!J71))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J74,'10A61 Liquid 3\" ViscosityLINEST'!J73))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J76,'10A61 Liquid 3\" ViscosityLINEST'!J75))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J78,'10A61 Liquid 3\" ViscosityLINEST'!J77))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J80,'10A61 Liquid 3\" ViscosityLINEST'!J79))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J82,'10A61 Liquid 3\" ViscosityLINEST'!J81))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D83>5,\"\",\nIF(D83>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J84,'10A61 Liquid 3\" ViscosityLINEST'!J83))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G83*C83^2+H83*C83+I83","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E74=\"\")),LINEST(E74:E80,C74:C80^{1,2}),\nIF(AND(E74=\"\",NOT(E75=\"\"),NOT(E76=\"\"),NOT(E77=\"\"),NOT(E78=\"\"),NOT(E79=\"\"),NOT(E80=\"\")),LINEST(E75:E80,C75:C80^{1,2}),\nIF(AND(E75=\"\",NOT(E76=\"\"),NOT(E77=\"\"),NOT(E78=\"\"),NOT(E79=\"\"),NOT(E80=\"\")),LINEST(E76:E80,C76:C80^{1,2}),\nIF(AND(E76=\"\",NOT(E77=\"\"),NOT(E78=\"\"),NOT(E79=\"\"),NOT(E80=\"\")),LINEST(E77:E80,C77:C80^{1,2}),\nIF(AND(E77=\"\",NOT(E78=\"\"),NOT(E79=\"\"),NOT(E80=\"\")),LINEST(E78:E80,C78:C80^{1,2}),\nIF(AND(E78=\"\",NOT(E79=\"\"),NOT(E80=\"\")),LINEST(E79:E80,C79:C80^{1,2}),\nIF(AND(E79=\"\",NOT(E80=\"\")),LINEST(E80,C80^{1,2}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-20-BG"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J88,'10A61 Liquid 3\" ViscosityLINEST'!J87))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J90,'10A61 Liquid 3\" ViscosityLINEST'!J89))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J92,'10A61 Liquid 3\" ViscosityLINEST'!J91))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J94,'10A61 Liquid 3\" ViscosityLINEST'!J93))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J96,'10A61 Liquid 3\" ViscosityLINEST'!J95))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J98,'10A61 Liquid 3\" ViscosityLINEST'!J97))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D99>5,\"\",\nIF(D99>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J100,'10A61 Liquid 3\" ViscosityLINEST'!J99))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G99*C99^2+H99*C99+I99","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E90=\"\")),LINEST(E90:E96,C90:C96^{1,2}),\nIF(AND(E90=\"\",NOT(E91=\"\"),NOT(E92=\"\"),NOT(E93=\"\"),NOT(E94=\"\"),NOT(E95=\"\"),NOT(E96=\"\")),LINEST(E91:E96,C91:C96^{1,2}),\nIF(AND(E91=\"\",NOT(E92=\"\"),NOT(E93=\"\"),NOT(E94=\"\"),NOT(E95=\"\"),NOT(E96=\"\")),LINEST(E92:E96,C92:C96^{1,2}),\nIF(AND(E92=\"\",NOT(E93=\"\"),NOT(E94=\"\"),NOT(E95=\"\"),NOT(E96=\"\")),LINEST(E93:E96,C93:C96^{1,2}),\nIF(AND(E93=\"\",NOT(E94=\"\"),NOT(E95=\"\"),NOT(E96=\"\")),LINEST(E94:E96,C94:C96^{1,2}),\nIF(AND(E94=\"\",NOT(E95=\"\"),NOT(E96=\"\")),LINEST(E95:E96,C95:C96^{1,2}),\nIF(AND(E95=\"\",NOT(E96=\"\")),LINEST(E96,C96^{1,2}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-20-SA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J104,'10A61 Liquid 3\" ViscosityLINEST'!J103))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J106,'10A61 Liquid 3\" ViscosityLINEST'!J105))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J108,'10A61 Liquid 3\" ViscosityLINEST'!J107))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J110,'10A61 Liquid 3\" ViscosityLINEST'!J109))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J112,'10A61 Liquid 3\" ViscosityLINEST'!J111))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J114,'10A61 Liquid 3\" ViscosityLINEST'!J113))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D115>5,\"\",\nIF(D115>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J116,'10A61 Liquid 3\" ViscosityLINEST'!J115))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G115*C115^3+H115*C115^2+I115*C115+J115","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E106=\"\")),LINEST(E106:E112,C106:C112^{1,2,3}),\nIF(AND(E106=\"\",NOT(E107=\"\"),NOT(E108=\"\"),NOT(E109=\"\"),NOT(E110=\"\"),NOT(E111=\"\"),NOT(E112=\"\")),LINEST(E107:E112,C107:C112^{1,2,3}),\nIF(AND(E107=\"\",NOT(E108=\"\"),NOT(E109=\"\"),NOT(E110=\"\"),NOT(E111=\"\"),NOT(E112=\"\")),LINEST(E108:E112,C108:C112^{1,2,3}),\nIF(AND(E108=\"\",NOT(E109=\"\"),NOT(E110=\"\"),NOT(E111=\"\"),NOT(E112=\"\")),LINEST(E109:E112,C109:C112^{1,2,3}),\nIF(AND(E109=\"\",NOT(E110=\"\"),NOT(E111=\"\"),NOT(E112=\"\")),LINEST(E110:E112,C110:C112^{1,2,3}),\nIF(AND(E110=\"\",NOT(E111=\"\"),NOT(E112=\"\")),LINEST(E111:E112,C111:C112^{1,2,3}),\nIF(AND(E111=\"\",NOT(E112=\"\")),LINEST(E112,C112^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-20-SS"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J120,'10A61 Liquid 3\" ViscosityLINEST'!J119))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J122,'10A61 Liquid 3\" ViscosityLINEST'!J121))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J124,'10A61 Liquid 3\" ViscosityLINEST'!J123))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J126,'10A61 Liquid 3\" ViscosityLINEST'!J125))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J128,'10A61 Liquid 3\" ViscosityLINEST'!J127))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J130,'10A61 Liquid 3\" ViscosityLINEST'!J129))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D131>5,\"\",\nIF(D131>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J132,'10A61 Liquid 3\" ViscosityLINEST'!J131))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G131*C131^3+H131*C131^2+I131*C131+J131","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E122=\"\")),LINEST(E122:E128,C122:C128^{1,2,3}),\nIF(AND(E122=\"\",NOT(E123=\"\"),NOT(E124=\"\"),NOT(E125=\"\"),NOT(E126=\"\"),NOT(E127=\"\"),NOT(E128=\"\")),LINEST(E123:E128,C123:C128^{1,2,3}),\nIF(AND(E123=\"\",NOT(E124=\"\"),NOT(E125=\"\"),NOT(E126=\"\"),NOT(E127=\"\"),NOT(E128=\"\")),LINEST(E124:E128,C124:C128^{1,2,3}),\nIF(AND(E124=\"\",NOT(E125=\"\"),NOT(E126=\"\"),NOT(E127=\"\"),NOT(E128=\"\")),LINEST(E125:E128,C125:C128^{1,2,3}),\nIF(AND(E125=\"\",NOT(E126=\"\"),NOT(E127=\"\"),NOT(E128=\"\")),LINEST(E126:E128,C126:C128^{1,2,3}),\nIF(AND(E126=\"\",NOT(E127=\"\"),NOT(E128=\"\")),LINEST(E127:E128,C127:C128^{1,2,3}),\nIF(AND(E127=\"\",NOT(E128=\"\")),LINEST(E128,C128^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-20-CA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J136,'10A61 Liquid 3\" ViscosityLINEST'!J135))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J138,'10A61 Liquid 3\" ViscosityLINEST'!J137))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J140,'10A61 Liquid 3\" ViscosityLINEST'!J139))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J142,'10A61 Liquid 3\" ViscosityLINEST'!J141))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J144,'10A61 Liquid 3\" ViscosityLINEST'!J143))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J146,'10A61 Liquid 3\" ViscosityLINEST'!J145))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D147>5,\"\",\nIF(D147>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J148,'10A61 Liquid 3\" ViscosityLINEST'!J147))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G147*C147^3+H147*C147^2+I147*C147+J147","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E138=\"\")),LINEST(E138:E144,C138:C144^{1,2,3}),\nIF(AND(E138=\"\",NOT(E139=\"\"),NOT(E140=\"\"),NOT(E141=\"\"),NOT(E142=\"\"),NOT(E143=\"\"),NOT(E144=\"\")),LINEST(E139:E144,C139:C144^{1,2,3}),\nIF(AND(E139=\"\",NOT(E140=\"\"),NOT(E141=\"\"),NOT(E142=\"\"),NOT(E143=\"\"),NOT(E144=\"\")),LINEST(E140:E144,C140:C144^{1,2,3}),\nIF(AND(E140=\"\",NOT(E141=\"\"),NOT(E142=\"\"),NOT(E143=\"\"),NOT(E144=\"\")),LINEST(E141:E144,C141:C144^{1,2,3}),\nIF(AND(E141=\"\",NOT(E142=\"\"),NOT(E143=\"\"),NOT(E144=\"\")),LINEST(E142:E144,C142:C144^{1,2,3}),\nIF(AND(E142=\"\",NOT(E143=\"\"),NOT(E144=\"\")),LINEST(E143:E144,C143:C144^{1,2,3}),\nIF(AND(E143=\"\",NOT(E144=\"\")),LINEST(E144,C144^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/8-20-TA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J152,'10A61 Liquid 3\" ViscosityLINEST'!J151))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J154,'10A61 Liquid 3\" ViscosityLINEST'!J153))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J156,'10A61 Liquid 3\" ViscosityLINEST'!J155))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J158,'10A61 Liquid 3\" ViscosityLINEST'!J157))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J160,'10A61 Liquid 3\" ViscosityLINEST'!J159))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J162,'10A61 Liquid 3\" ViscosityLINEST'!J161))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D163>5,\"\",\nIF(D163>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J164,'10A61 Liquid 3\" ViscosityLINEST'!J163))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G163*C163^3+H163*C163^2+I163*C163+J163","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E154=\"\")),LINEST(E154:E160,C154:C160^{1,2,3}),\nIF(AND(E154=\"\",NOT(E155=\"\"),NOT(E156=\"\"),NOT(E157=\"\"),NOT(E158=\"\"),NOT(E159=\"\"),NOT(E160=\"\")),LINEST(E155:E160,C155:C160^{1,2,3}),\nIF(AND(E155=\"\",NOT(E156=\"\"),NOT(E157=\"\"),NOT(E158=\"\"),NOT(E159=\"\"),NOT(E160=\"\")),LINEST(E156:E160,C156:C160^{1,2,3}),\nIF(AND(E156=\"\",NOT(E157=\"\"),NOT(E158=\"\"),NOT(E159=\"\"),NOT(E160=\"\")),LINEST(E157:E160,C157:C160^{1,2,3}),\nIF(AND(E157=\"\",NOT(E158=\"\"),NOT(E159=\"\"),NOT(E160=\"\")),LINEST(E158:E160,C158:C160^{1,2,3}),\nIF(AND(E158=\"\",NOT(E159=\"\"),NOT(E160=\"\")),LINEST(E159:E160,C159:C160^{1,2,3}),\nIF(AND(E159=\"\",NOT(E160=\"\")),LINEST(E160,C160^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-15-CD"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J168,'10A61 Liquid 3\" ViscosityLINEST'!J167))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J170,'10A61 Liquid 3\" ViscosityLINEST'!J169))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J172,'10A61 Liquid 3\" ViscosityLINEST'!J171))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J174,'10A61 Liquid 3\" ViscosityLINEST'!J173))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J176,'10A61 Liquid 3\" ViscosityLINEST'!J175))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J178,'10A61 Liquid 3\" ViscosityLINEST'!J177))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D179>5,\"\",\nIF(D179>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J180,'10A61 Liquid 3\" ViscosityLINEST'!J179))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G179*C179^3+H179*C179^2+I179*C179+J179","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E170=\"\")),LINEST(E170:E176,C170:C176^{1,2,3}),\nIF(AND(E170=\"\",NOT(E171=\"\"),NOT(E172=\"\"),NOT(E173=\"\"),NOT(E174=\"\"),NOT(E175=\"\"),NOT(E176=\"\")),LINEST(E171:E176,C171:C176^{1,2,3}),\nIF(AND(E171=\"\",NOT(E172=\"\"),NOT(E173=\"\"),NOT(E174=\"\"),NOT(E175=\"\"),NOT(E176=\"\")),LINEST(E172:E176,C172:C176^{1,2,3}),\nIF(AND(E172=\"\",NOT(E173=\"\"),NOT(E174=\"\"),NOT(E175=\"\"),NOT(E176=\"\")),LINEST(E173:E176,C173:C176^{1,2,3}),\nIF(AND(E173=\"\",NOT(E174=\"\"),NOT(E175=\"\"),NOT(E176=\"\")),LINEST(E174:E176,C174:C176^{1,2,3}),\nIF(AND(E174=\"\",NOT(E175=\"\"),NOT(E176=\"\")),LINEST(E175:E176,C175:C176^{1,2,3}),\nIF(AND(E175=\"\",NOT(E176=\"\")),LINEST(E176,C176^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-15-SA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J184,'10A61 Liquid 3\" ViscosityLINEST'!J183))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J186,'10A61 Liquid 3\" ViscosityLINEST'!J185))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J188,'10A61 Liquid 3\" ViscosityLINEST'!J187))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J190,'10A61 Liquid 3\" ViscosityLINEST'!J189))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J192,'10A61 Liquid 3\" ViscosityLINEST'!J191))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J194,'10A61 Liquid 3\" ViscosityLINEST'!J193))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D195>5,\"\",\nIF(D195>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J196,'10A61 Liquid 3\" ViscosityLINEST'!J195))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G195*C195^3+H195*C195^2+I195*C195+J195","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E186=\"\")),LINEST(E186:E192,C186:C192^{1,2,3}),\nIF(AND(E186=\"\",NOT(E187=\"\"),NOT(E188=\"\"),NOT(E189=\"\"),NOT(E190=\"\"),NOT(E191=\"\"),NOT(E192=\"\")),LINEST(E187:E192,C187:C192^{1,2,3}),\nIF(AND(E187=\"\",NOT(E188=\"\"),NOT(E189=\"\"),NOT(E190=\"\"),NOT(E191=\"\"),NOT(E192=\"\")),LINEST(E188:E192,C188:C192^{1,2,3}),\nIF(AND(E188=\"\",NOT(E189=\"\"),NOT(E190=\"\"),NOT(E191=\"\"),NOT(E192=\"\")),LINEST(E189:E192,C189:C192^{1,2,3}),\nIF(AND(E189=\"\",NOT(E190=\"\"),NOT(E191=\"\"),NOT(E192=\"\")),LINEST(E190:E192,C190:C192^{1,2,3}),\nIF(AND(E190=\"\",NOT(E191=\"\"),NOT(E192=\"\")),LINEST(E191:E192,C191:C192^{1,2,3}),\nIF(AND(E191=\"\",NOT(E192=\"\")),LINEST(E192,C192^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-20-CD"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J200,'10A61 Liquid 3\" ViscosityLINEST'!J199))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J202,'10A61 Liquid 3\" ViscosityLINEST'!J201))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J204,'10A61 Liquid 3\" ViscosityLINEST'!J203))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J206,'10A61 Liquid 3\" ViscosityLINEST'!J205))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J208,'10A61 Liquid 3\" ViscosityLINEST'!J207))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J210,'10A61 Liquid 3\" ViscosityLINEST'!J209))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D211>5,\"\",\nIF(D211>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J212,'10A61 Liquid 3\" ViscosityLINEST'!J211))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G211*C211^3+H211*C211^2+I211*C211+J211","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E202=\"\")),LINEST(E202:E208,C202:C208^{1,2,3}),\nIF(AND(E202=\"\",NOT(E203=\"\"),NOT(E204=\"\"),NOT(E205=\"\"),NOT(E206=\"\"),NOT(E207=\"\"),NOT(E208=\"\")),LINEST(E203:E208,C203:C208^{1,2,3}),\nIF(AND(E203=\"\",NOT(E204=\"\"),NOT(E205=\"\"),NOT(E206=\"\"),NOT(E207=\"\"),NOT(E208=\"\")),LINEST(E204:E208,C204:C208^{1,2,3}),\nIF(AND(E204=\"\",NOT(E205=\"\"),NOT(E206=\"\"),NOT(E207=\"\"),NOT(E208=\"\")),LINEST(E205:E208,C205:C208^{1,2,3}),\nIF(AND(E205=\"\",NOT(E206=\"\"),NOT(E207=\"\"),NOT(E208=\"\")),LINEST(E206:E208,C206:C208^{1,2,3}),\nIF(AND(E206=\"\",NOT(E207=\"\"),NOT(E208=\"\")),LINEST(E207:E208,C207:C208^{1,2,3}),\nIF(AND(E207=\"\",NOT(E208=\"\")),LINEST(E208,C208^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-20-SA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J216,'10A61 Liquid 3\" ViscosityLINEST'!J215))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J218,'10A61 Liquid 3\" ViscosityLINEST'!J217))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J220,'10A61 Liquid 3\" ViscosityLINEST'!J219))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J222,'10A61 Liquid 3\" ViscosityLINEST'!J221))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J224,'10A61 Liquid 3\" ViscosityLINEST'!J223))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J226,'10A61 Liquid 3\" ViscosityLINEST'!J225))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D227>5,\"\",\nIF(D227>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J228,'10A61 Liquid 3\" ViscosityLINEST'!J227))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G227*C227^3+H227*C227^2+I227*C227+J227","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E218=\"\")),LINEST(E218:E224,C218:C224^{1,2,3}),\nIF(AND(E218=\"\",NOT(E219=\"\"),NOT(E220=\"\"),NOT(E221=\"\"),NOT(E222=\"\"),NOT(E223=\"\"),NOT(E224=\"\")),LINEST(E219:E224,C219:C224^{1,2,3}),\nIF(AND(E219=\"\",NOT(E220=\"\"),NOT(E221=\"\"),NOT(E222=\"\"),NOT(E223=\"\"),NOT(E224=\"\")),LINEST(E220:E224,C220:C224^{1,2,3}),\nIF(AND(E220=\"\",NOT(E221=\"\"),NOT(E222=\"\"),NOT(E223=\"\"),NOT(E224=\"\")),LINEST(E221:E224,C221:C224^{1,2,3}),\nIF(AND(E221=\"\",NOT(E222=\"\"),NOT(E223=\"\"),NOT(E224=\"\")),LINEST(E222:E224,C222:C224^{1,2,3}),\nIF(AND(E222=\"\",NOT(E223=\"\"),NOT(E224=\"\")),LINEST(E223:E224,C223:C224^{1,2,3}),\nIF(AND(E223=\"\",NOT(E224=\"\")),LINEST(E224,C224^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-15-SS"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J232,'10A61 Liquid 3\" ViscosityLINEST'!J231))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J234,'10A61 Liquid 3\" ViscosityLINEST'!J233))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J236,'10A61 Liquid 3\" ViscosityLINEST'!J235))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J238,'10A61 Liquid 3\" ViscosityLINEST'!J237))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J240,'10A61 Liquid 3\" ViscosityLINEST'!J239))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J242,'10A61 Liquid 3\" ViscosityLINEST'!J241))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D243>5,\"\",\nIF(D243>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J244,'10A61 Liquid 3\" ViscosityLINEST'!J243))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G243*C243^3+H243*C243^2+I243*C243+J243","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E234=\"\")),LINEST(E234:E240,C234:C240^{1,2,3}),\nIF(AND(E234=\"\",NOT(E235=\"\"),NOT(E236=\"\"),NOT(E237=\"\"),NOT(E238=\"\"),NOT(E239=\"\"),NOT(E240=\"\")),LINEST(E235:E240,C235:C240^{1,2,3}),\nIF(AND(E235=\"\",NOT(E236=\"\"),NOT(E237=\"\"),NOT(E238=\"\"),NOT(E239=\"\"),NOT(E240=\"\")),LINEST(E236:E240,C236:C240^{1,2,3}),\nIF(AND(E236=\"\",NOT(E237=\"\"),NOT(E238=\"\"),NOT(E239=\"\"),NOT(E240=\"\")),LINEST(E237:E240,C237:C240^{1,2,3}),\nIF(AND(E237=\"\",NOT(E238=\"\"),NOT(E239=\"\"),NOT(E240=\"\")),LINEST(E238:E240,C238:C240^{1,2,3}),\nIF(AND(E238=\"\",NOT(E239=\"\"),NOT(E240=\"\")),LINEST(E239:E240,C239:C240^{1,2,3}),\nIF(AND(E239=\"\",NOT(E240=\"\")),LINEST(E240,C240^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-15-CA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J248,'10A61 Liquid 3\" ViscosityLINEST'!J247))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J250,'10A61 Liquid 3\" ViscosityLINEST'!J249))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J252,'10A61 Liquid 3\" ViscosityLINEST'!J251))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J254,'10A61 Liquid 3\" ViscosityLINEST'!J253))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J256,'10A61 Liquid 3\" ViscosityLINEST'!J255))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J258,'10A61 Liquid 3\" ViscosityLINEST'!J257))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D259>5,\"\",\nIF(D259>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J260,'10A61 Liquid 3\" ViscosityLINEST'!J259))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G259*C259^3+H259*C259^2+I259*C259+J259","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E250=\"\")),LINEST(E250:E256,C250:C256^{1,2,3}),\nIF(AND(E250=\"\",NOT(E251=\"\"),NOT(E252=\"\"),NOT(E253=\"\"),NOT(E254=\"\"),NOT(E255=\"\"),NOT(E256=\"\")),LINEST(E251:E256,C251:C256^{1,2,3}),\nIF(AND(E251=\"\",NOT(E252=\"\"),NOT(E253=\"\"),NOT(E254=\"\"),NOT(E255=\"\"),NOT(E256=\"\")),LINEST(E252:E256,C252:C256^{1,2,3}),\nIF(AND(E252=\"\",NOT(E253=\"\"),NOT(E254=\"\"),NOT(E255=\"\"),NOT(E256=\"\")),LINEST(E253:E256,C253:C256^{1,2,3}),\nIF(AND(E253=\"\",NOT(E254=\"\"),NOT(E255=\"\"),NOT(E256=\"\")),LINEST(E254:E256,C254:C256^{1,2,3}),\nIF(AND(E254=\"\",NOT(E255=\"\"),NOT(E256=\"\")),LINEST(E255:E256,C255:C256^{1,2,3}),\nIF(AND(E255=\"\",NOT(E256=\"\")),LINEST(E256,C256^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-20-SS"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J264,'10A61 Liquid 3\" ViscosityLINEST'!J263))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J266,'10A61 Liquid 3\" ViscosityLINEST'!J265))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J268,'10A61 Liquid 3\" ViscosityLINEST'!J267))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J270,'10A61 Liquid 3\" ViscosityLINEST'!J269))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J272,'10A61 Liquid 3\" ViscosityLINEST'!J271))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J274,'10A61 Liquid 3\" ViscosityLINEST'!J273))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D275>5,\"\",\nIF(D275>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J276,'10A61 Liquid 3\" ViscosityLINEST'!J275))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G275*C275^3+H275*C275^2+I275*C275+J275","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E266=\"\")),LINEST(E266:E272,C266:C272^{1,2,3}),\nIF(AND(E266=\"\",NOT(E267=\"\"),NOT(E268=\"\"),NOT(E269=\"\"),NOT(E270=\"\"),NOT(E271=\"\"),NOT(E272=\"\")),LINEST(E267:E272,C267:C272^{1,2,3}),\nIF(AND(E267=\"\",NOT(E268=\"\"),NOT(E269=\"\"),NOT(E270=\"\"),NOT(E271=\"\"),NOT(E272=\"\")),LINEST(E268:E272,C268:C272^{1,2,3}),\nIF(AND(E268=\"\",NOT(E269=\"\"),NOT(E270=\"\"),NOT(E271=\"\"),NOT(E272=\"\")),LINEST(E269:E272,C269:C272^{1,2,3}),\nIF(AND(E269=\"\",NOT(E270=\"\"),NOT(E271=\"\"),NOT(E272=\"\")),LINEST(E270:E272,C270:C272^{1,2,3}),\nIF(AND(E270=\"\",NOT(E271=\"\"),NOT(E272=\"\")),LINEST(E271:E272,C271:C272^{1,2,3}),\nIF(AND(E271=\"\",NOT(E272=\"\")),LINEST(E272,C272^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-15-TA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J280,'10A61 Liquid 3\" ViscosityLINEST'!J279))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J282,'10A61 Liquid 3\" ViscosityLINEST'!J281))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J284,'10A61 Liquid 3\" ViscosityLINEST'!J283))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J286,'10A61 Liquid 3\" ViscosityLINEST'!J285))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J288,'10A61 Liquid 3\" ViscosityLINEST'!J287))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J290,'10A61 Liquid 3\" ViscosityLINEST'!J289))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D291>5,\"\",\nIF(D291>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J292,'10A61 Liquid 3\" ViscosityLINEST'!J291))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G291*C291^3+H291*C291^2+I291*C291+J291","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E282=\"\")),LINEST(E282:E288,C282:C288^{1,2,3}),\nIF(AND(E282=\"\",NOT(E283=\"\"),NOT(E284=\"\"),NOT(E285=\"\"),NOT(E286=\"\"),NOT(E287=\"\"),NOT(E288=\"\")),LINEST(E283:E288,C283:C288^{1,2,3}),\nIF(AND(E283=\"\",NOT(E284=\"\"),NOT(E285=\"\"),NOT(E286=\"\"),NOT(E287=\"\"),NOT(E288=\"\")),LINEST(E284:E288,C284:C288^{1,2,3}),\nIF(AND(E284=\"\",NOT(E285=\"\"),NOT(E286=\"\"),NOT(E287=\"\"),NOT(E288=\"\")),LINEST(E285:E288,C285:C288^{1,2,3}),\nIF(AND(E285=\"\",NOT(E286=\"\"),NOT(E287=\"\"),NOT(E288=\"\")),LINEST(E286:E288,C286:C288^{1,2,3}),\nIF(AND(E286=\"\",NOT(E287=\"\"),NOT(E288=\"\")),LINEST(E287:E288,C287:C288^{1,2,3}),\nIF(AND(E287=\"\",NOT(E288=\"\")),LINEST(E288,C288^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-G-SA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J296,'10A61 Liquid 3\" ViscosityLINEST'!J295))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J298,'10A61 Liquid 3\" ViscosityLINEST'!J297))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J300,'10A61 Liquid 3\" ViscosityLINEST'!J299))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J302,'10A61 Liquid 3\" ViscosityLINEST'!J301))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J304,'10A61 Liquid 3\" ViscosityLINEST'!J303))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J306,'10A61 Liquid 3\" ViscosityLINEST'!J305))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D307>5,\"\",\nIF(D307>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J308,'10A61 Liquid 3\" ViscosityLINEST'!J307))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G307*C307^3+H307*C307^2+I307*C307+J307","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E298=\"\")),LINEST(E298:E304,C298:C304^{1,2,3}),\nIF(AND(E298=\"\",NOT(E299=\"\"),NOT(E300=\"\"),NOT(E301=\"\"),NOT(E302=\"\"),NOT(E303=\"\"),NOT(E304=\"\")),LINEST(E299:E304,C299:C304^{1,2,3}),\nIF(AND(E299=\"\",NOT(E300=\"\"),NOT(E301=\"\"),NOT(E302=\"\"),NOT(E303=\"\"),NOT(E304=\"\")),LINEST(E300:E304,C300:C304^{1,2,3}),\nIF(AND(E300=\"\",NOT(E301=\"\"),NOT(E302=\"\"),NOT(E303=\"\"),NOT(E304=\"\")),LINEST(E301:E304,C301:C304^{1,2,3}),\nIF(AND(E301=\"\",NOT(E302=\"\"),NOT(E303=\"\"),NOT(E304=\"\")),LINEST(E302:E304,C302:C304^{1,2,3}),\nIF(AND(E302=\"\",NOT(E303=\"\"),NOT(E304=\"\")),LINEST(E303:E304,C303:C304^{1,2,3}),\nIF(AND(E303=\"\",NOT(E304=\"\")),LINEST(E304,C304^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-20-CA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J312,'10A61 Liquid 3\" ViscosityLINEST'!J311))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J314,'10A61 Liquid 3\" ViscosityLINEST'!J313))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J316,'10A61 Liquid 3\" ViscosityLINEST'!J315))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J318,'10A61 Liquid 3\" ViscosityLINEST'!J317))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J320,'10A61 Liquid 3\" ViscosityLINEST'!J319))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J322,'10A61 Liquid 3\" ViscosityLINEST'!J321))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D323>5,\"\",\nIF(D323>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J324,'10A61 Liquid 3\" ViscosityLINEST'!J323))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G323*C323^3+H323*C323^2+I323*C323+J323","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E314=\"\")),LINEST(E314:E320,C314:C320^{1,2,3}),\nIF(AND(E314=\"\",NOT(E315=\"\"),NOT(E316=\"\"),NOT(E317=\"\"),NOT(E318=\"\"),NOT(E319=\"\"),NOT(E320=\"\")),LINEST(E315:E320,C315:C320^{1,2,3}),\nIF(AND(E315=\"\",NOT(E316=\"\"),NOT(E317=\"\"),NOT(E318=\"\"),NOT(E319=\"\"),NOT(E320=\"\")),LINEST(E316:E320,C316:C320^{1,2,3}),\nIF(AND(E316=\"\",NOT(E317=\"\"),NOT(E318=\"\"),NOT(E319=\"\"),NOT(E320=\"\")),LINEST(E317:E320,C317:C320^{1,2,3}),\nIF(AND(E317=\"\",NOT(E318=\"\"),NOT(E319=\"\"),NOT(E320=\"\")),LINEST(E318:E320,C318:C320^{1,2,3}),\nIF(AND(E318=\"\",NOT(E319=\"\"),NOT(E320=\"\")),LINEST(E319:E320,C319:C320^{1,2,3}),\nIF(AND(E319=\"\",NOT(E320=\"\")),LINEST(E320,C320^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-20-TA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J328,'10A61 Liquid 3\" ViscosityLINEST'!J327))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J330,'10A61 Liquid 3\" ViscosityLINEST'!J329))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J332,'10A61 Liquid 3\" ViscosityLINEST'!J331))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J334,'10A61 Liquid 3\" ViscosityLINEST'!J333))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J336,'10A61 Liquid 3\" ViscosityLINEST'!J335))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J338,'10A61 Liquid 3\" ViscosityLINEST'!J337))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D339>5,\"\",\nIF(D339>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J340,'10A61 Liquid 3\" ViscosityLINEST'!J339))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G339*C339^3+H339*C339^2+I339*C339+J339","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E330=\"\")),LINEST(E330:E336,C330:C336^{1,2,3}),\nIF(AND(E330=\"\",NOT(E331=\"\"),NOT(E332=\"\"),NOT(E333=\"\"),NOT(E334=\"\"),NOT(E335=\"\"),NOT(E336=\"\")),LINEST(E331:E336,C331:C336^{1,2,3}),\nIF(AND(E331=\"\",NOT(E332=\"\"),NOT(E333=\"\"),NOT(E334=\"\"),NOT(E335=\"\"),NOT(E336=\"\")),LINEST(E332:E336,C332:C336^{1,2,3}),\nIF(AND(E332=\"\",NOT(E333=\"\"),NOT(E334=\"\"),NOT(E335=\"\"),NOT(E336=\"\")),LINEST(E333:E336,C333:C336^{1,2,3}),\nIF(AND(E333=\"\",NOT(E334=\"\"),NOT(E335=\"\"),NOT(E336=\"\")),LINEST(E334:E336,C334:C336^{1,2,3}),\nIF(AND(E334=\"\",NOT(E335=\"\"),NOT(E336=\"\")),LINEST(E335:E336,C335:C336^{1,2,3}),\nIF(AND(E335=\"\",NOT(E336=\"\")),LINEST(E336,C336^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-P-SA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J344,'10A61 Liquid 3\" ViscosityLINEST'!J343))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J346,'10A61 Liquid 3\" ViscosityLINEST'!J345))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J348,'10A61 Liquid 3\" ViscosityLINEST'!J347))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J350,'10A61 Liquid 3\" ViscosityLINEST'!J349))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J352,'10A61 Liquid 3\" ViscosityLINEST'!J351))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J354,'10A61 Liquid 3\" ViscosityLINEST'!J353))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D355>5,\"\",\nIF(D355>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J356,'10A61 Liquid 3\" ViscosityLINEST'!J355))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G355*C355^3+H355*C355^2+I355*C355+J355","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E346=\"\")),LINEST(E346:E352,C346:C352^{1,2,3}),\nIF(AND(E346=\"\",NOT(E347=\"\"),NOT(E348=\"\"),NOT(E349=\"\"),NOT(E350=\"\"),NOT(E351=\"\"),NOT(E352=\"\")),LINEST(E347:E352,C347:C352^{1,2,3}),\nIF(AND(E347=\"\",NOT(E348=\"\"),NOT(E349=\"\"),NOT(E350=\"\"),NOT(E351=\"\"),NOT(E352=\"\")),LINEST(E348:E352,C348:C352^{1,2,3}),\nIF(AND(E348=\"\",NOT(E349=\"\"),NOT(E350=\"\"),NOT(E351=\"\"),NOT(E352=\"\")),LINEST(E349:E352,C349:C352^{1,2,3}),\nIF(AND(E349=\"\",NOT(E350=\"\"),NOT(E351=\"\"),NOT(E352=\"\")),LINEST(E350:E352,C350:C352^{1,2,3}),\nIF(AND(E350=\"\",NOT(E351=\"\"),NOT(E352=\"\")),LINEST(E351:E352,C351:C352^{1,2,3}),\nIF(AND(E351=\"\",NOT(E352=\"\")),LINEST(E352,C352^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-G-SS"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J360,'10A61 Liquid 3\" ViscosityLINEST'!J359))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J362,'10A61 Liquid 3\" ViscosityLINEST'!J361))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J364,'10A61 Liquid 3\" ViscosityLINEST'!J363))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J366,'10A61 Liquid 3\" ViscosityLINEST'!J365))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J368,'10A61 Liquid 3\" ViscosityLINEST'!J367))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J370,'10A61 Liquid 3\" ViscosityLINEST'!J369))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D371>5,\"\",\nIF(D371>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J372,'10A61 Liquid 3\" ViscosityLINEST'!J371))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G371*C371^3+H371*C371^2+I371*C371+J371","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E362=\"\")),LINEST(E362:E368,C362:C368^{1,2,3}),\nIF(AND(E362=\"\",NOT(E363=\"\"),NOT(E364=\"\"),NOT(E365=\"\"),NOT(E366=\"\"),NOT(E367=\"\"),NOT(E368=\"\")),LINEST(E363:E368,C363:C368^{1,2,3}),\nIF(AND(E363=\"\",NOT(E364=\"\"),NOT(E365=\"\"),NOT(E366=\"\"),NOT(E367=\"\"),NOT(E368=\"\")),LINEST(E364:E368,C364:C368^{1,2,3}),\nIF(AND(E364=\"\",NOT(E365=\"\"),NOT(E366=\"\"),NOT(E367=\"\"),NOT(E368=\"\")),LINEST(E365:E368,C365:C368^{1,2,3}),\nIF(AND(E365=\"\",NOT(E366=\"\"),NOT(E367=\"\"),NOT(E368=\"\")),LINEST(E366:E368,C366:C368^{1,2,3}),\nIF(AND(E366=\"\",NOT(E367=\"\"),NOT(E368=\"\")),LINEST(E367:E368,C367:C368^{1,2,3}),\nIF(AND(E367=\"\",NOT(E368=\"\")),LINEST(E368,C368^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-P-SS"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J376,'10A61 Liquid 3\" ViscosityLINEST'!J375))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J378,'10A61 Liquid 3\" ViscosityLINEST'!J377))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J380,'10A61 Liquid 3\" ViscosityLINEST'!J379))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J382,'10A61 Liquid 3\" ViscosityLINEST'!J381))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J384,'10A61 Liquid 3\" ViscosityLINEST'!J383))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J386,'10A61 Liquid 3\" ViscosityLINEST'!J385))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D387>5,\"\",\nIF(D387>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J388,'10A61 Liquid 3\" ViscosityLINEST'!J387))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G387*C387^3+H387*C387^2+I387*C387+J387","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E378=\"\")),LINEST(E378:E384,C378:C384^{1,2,3}),\nIF(AND(E378=\"\",NOT(E379=\"\"),NOT(E380=\"\"),NOT(E381=\"\"),NOT(E382=\"\"),NOT(E383=\"\"),NOT(E384=\"\")),LINEST(E379:E384,C379:C384^{1,2,3}),\nIF(AND(E379=\"\",NOT(E380=\"\"),NOT(E381=\"\"),NOT(E382=\"\"),NOT(E383=\"\"),NOT(E384=\"\")),LINEST(E380:E384,C380:C384^{1,2,3}),\nIF(AND(E380=\"\",NOT(E381=\"\"),NOT(E382=\"\"),NOT(E383=\"\"),NOT(E384=\"\")),LINEST(E381:E384,C381:C384^{1,2,3}),\nIF(AND(E381=\"\",NOT(E382=\"\"),NOT(E383=\"\"),NOT(E384=\"\")),LINEST(E382:E384,C382:C384^{1,2,3}),\nIF(AND(E382=\"\",NOT(E383=\"\"),NOT(E384=\"\")),LINEST(E383:E384,C383:C384^{1,2,3}),\nIF(AND(E383=\"\",NOT(E384=\"\")),LINEST(E384,C384^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-G-CA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J392,'10A61 Liquid 3\" ViscosityLINEST'!J391))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J394,'10A61 Liquid 3\" ViscosityLINEST'!J393))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J396,'10A61 Liquid 3\" ViscosityLINEST'!J395))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J398,'10A61 Liquid 3\" ViscosityLINEST'!J397))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J400,'10A61 Liquid 3\" ViscosityLINEST'!J399))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J402,'10A61 Liquid 3\" ViscosityLINEST'!J401))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D403>5,\"\",\nIF(D403>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J404,'10A61 Liquid 3\" ViscosityLINEST'!J403))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G403*C403^3+H403*C403^2+I403*C403+J403","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E394=\"\")),LINEST(E394:E400,C394:C400^{1,2,3}),\nIF(AND(E394=\"\",NOT(E395=\"\"),NOT(E396=\"\"),NOT(E397=\"\"),NOT(E398=\"\"),NOT(E399=\"\"),NOT(E400=\"\")),LINEST(E395:E400,C395:C400^{1,2,3}),\nIF(AND(E395=\"\",NOT(E396=\"\"),NOT(E397=\"\"),NOT(E398=\"\"),NOT(E399=\"\"),NOT(E400=\"\")),LINEST(E396:E400,C396:C400^{1,2,3}),\nIF(AND(E396=\"\",NOT(E397=\"\"),NOT(E398=\"\"),NOT(E399=\"\"),NOT(E400=\"\")),LINEST(E397:E400,C397:C400^{1,2,3}),\nIF(AND(E397=\"\",NOT(E398=\"\"),NOT(E399=\"\"),NOT(E400=\"\")),LINEST(E398:E400,C398:C400^{1,2,3}),\nIF(AND(E398=\"\",NOT(E399=\"\"),NOT(E400=\"\")),LINEST(E399:E400,C399:C400^{1,2,3}),\nIF(AND(E399=\"\",NOT(E400=\"\")),LINEST(E400,C400^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-G-TA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J408,'10A61 Liquid 3\" ViscosityLINEST'!J407))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J410,'10A61 Liquid 3\" ViscosityLINEST'!J409))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J412,'10A61 Liquid 3\" ViscosityLINEST'!J411))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J414,'10A61 Liquid 3\" ViscosityLINEST'!J413))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J416,'10A61 Liquid 3\" ViscosityLINEST'!J415))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J418,'10A61 Liquid 3\" ViscosityLINEST'!J417))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D419>5,\"\",\nIF(D419>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J420,'10A61 Liquid 3\" ViscosityLINEST'!J419))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G419*C419^3+H419*C419^2+I419*C419+J419","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E410=\"\")),LINEST(E410:E416,C410:C416^{1,2,3}),\nIF(AND(E410=\"\",NOT(E411=\"\"),NOT(E412=\"\"),NOT(E413=\"\"),NOT(E414=\"\"),NOT(E415=\"\"),NOT(E416=\"\")),LINEST(E411:E416,C411:C416^{1,2,3}),\nIF(AND(E411=\"\",NOT(E412=\"\"),NOT(E413=\"\"),NOT(E414=\"\"),NOT(E415=\"\"),NOT(E416=\"\")),LINEST(E412:E416,C412:C416^{1,2,3}),\nIF(AND(E412=\"\",NOT(E413=\"\"),NOT(E414=\"\"),NOT(E415=\"\"),NOT(E416=\"\")),LINEST(E413:E416,C413:C416^{1,2,3}),\nIF(AND(E413=\"\",NOT(E414=\"\"),NOT(E415=\"\"),NOT(E416=\"\")),LINEST(E414:E416,C414:C416^{1,2,3}),\nIF(AND(E414=\"\",NOT(E415=\"\"),NOT(E416=\"\")),LINEST(E415:E416,C415:C416^{1,2,3}),\nIF(AND(E415=\"\",NOT(E416=\"\")),LINEST(E416,C416^{1,2,3}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-P-CA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J424,'10A61 Liquid 3\" ViscosityLINEST'!J423))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J426,'10A61 Liquid 3\" ViscosityLINEST'!J425))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J428,'10A61 Liquid 3\" ViscosityLINEST'!J427))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J430,'10A61 Liquid 3\" ViscosityLINEST'!J429))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J432,'10A61 Liquid 3\" ViscosityLINEST'!J431))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J434,'10A61 Liquid 3\" ViscosityLINEST'!J433))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D435>5,\"\",\nIF(D435>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J436,'10A61 Liquid 3\" ViscosityLINEST'!J435))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G435*C435^5+H435*C435^4+I435*C435^3+J435*C435^2+K435*C435+L435","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E426=\"\")),LINEST(E426:E432,C426:C432^{1,2,3,4,5}),\nIF(AND(E426=\"\",NOT(E427=\"\"),NOT(E428=\"\"),NOT(E429=\"\"),NOT(E430=\"\"),NOT(E431=\"\"),NOT(E432=\"\")),LINEST(E427:E432,C427:C432^{1,2,3,4,5}),\nIF(AND(E427=\"\",NOT(E428=\"\"),NOT(E429=\"\"),NOT(E430=\"\"),NOT(E431=\"\"),NOT(E432=\"\")),LINEST(E428:E432,C428:C432^{1,2,3,4,5}),\nIF(AND(E428=\"\",NOT(E429=\"\"),NOT(E430=\"\"),NOT(E431=\"\"),NOT(E432=\"\")),LINEST(E429:E432,C429:C432^{1,2,3,4,5}),\nIF(AND(E429=\"\",NOT(E430=\"\"),NOT(E431=\"\"),NOT(E432=\"\")),LINEST(E430:E432,C430:C432^{1,2,3,4,5}),\nIF(AND(E430=\"\",NOT(E431=\"\"),NOT(E432=\"\")),LINEST(E431:E432,C431:C432^{1,2,3,4,5}),\nIF(AND(E431=\"\",NOT(E432=\"\")),LINEST(E432,C432^{1,2,3,4,5}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]
[]
[]
[]
[null,null,null,null,null,null,"1/4-41-P-TA"]
[]
[null,null,"Density","viscosity","Max Flow"]
[null,null,0.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.011,'10A61 Liquid 3\" ViscosityLINEST'!J440,'10A61 Liquid 3\" ViscosityLINEST'!J439))","v":{"$error":"#NUM!"}}]
[null,null,0.6,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J442,'10A61 Liquid 3\" ViscosityLINEST'!J441))","v":{"$error":"#NUM!"}}]
[null,null,0.8,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J444,'10A61 Liquid 3\" ViscosityLINEST'!J443))","v":{"$error":"#NUM!"}}]
[null,null,1,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J446,'10A61 Liquid 3\" ViscosityLINEST'!J445))","v":{"$error":"#NUM!"}}]
[null,null,1.2,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J448,'10A61 Liquid 3\" ViscosityLINEST'!J447))","v":{"$error":"#NUM!"}}]
[null,null,1.4,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J450,'10A61 Liquid 3\" ViscosityLINEST'!J449))","v":{"$error":"#NUM!"}}]
[null,null,1.5,{"$f":"'10A61 Liquid 3\"'!$B$4","v":0},{"$f":"IF(D451>5,\"\",\nIF(D451>1.001,'10A61 Liquid 3\" ViscosityLINEST'!J452,'10A61 Liquid 3\" ViscosityLINEST'!J451))","v":{"$error":"#NUM!"}}]
[]
[null,null,"DENSITY","VISCOSITY","MAX FLOW",null,"LINEST"]
[null,null,{"$f":"$B$3","v":0},{"$f":"$C$3","v":0},{"$f":"G451*C451^5+H451*C451^4+I451*C451^3+J451*C451^2+K451*C451+L451","v":{"$error":"#NUM!"}},null,{"$f":"IF(AND(NOT(E442=\"\")),LINEST(E442:E448,C442:C448^{1,2,3,4,5}),\nIF(AND(E442=\"\",NOT(E443=\"\"),NOT(E444=\"\"),NOT(E445=\"\"),NOT(E446=\"\"),NOT(E447=\"\"),NOT(E448=\"\")),LINEST(E443:E448,C443:C448^{1,2,3,4,5}),\nIF(AND(E443=\"\",NOT(E444=\"\"),NOT(E445=\"\"),NOT(E446=\"\"),NOT(E447=\"\"),NOT(E448=\"\")),LINEST(E444:E448,C444:C448^{1,2,3,4,5}),\nIF(AND(E444=\"\",NOT(E445=\"\"),NOT(E446=\"\"),NOT(E447=\"\"),NOT(E448=\"\")),LINEST(E445:E448,C445:C448^{1,2,3,4,5}),\nIF(AND(E445=\"\",NOT(E446=\"\"),NOT(E447=\"\"),NOT(E448=\"\")),LINEST(E446:E448,C446:C448^{1,2,3,4,5}),\nIF(AND(E446=\"\",NOT(E447=\"\"),NOT(E448=\"\")),LINEST(E447:E448,C447:C448^{1,2,3,4,5}),\nIF(AND(E447=\"\",NOT(E448=\"\")),LINEST(E448,C448^{1,2,3,4,5}),\"NOT APPLICABLE\")))))))","v":{"$error":"#NUM!"}},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"}]

{"sheet":"10A61 3\" Results Interpol.","index":4,"n_rows":30,"n_cols":4,"rows_kept":30,"cut":false,"hidden":true,"merged":[]}
[]
[null,"Tube/Float","Max Flow mL/min","Min Flow mL/min"]
[null,"1/8-08-BG",{"$f":"'10A61 3\" Density LINEST'!E19","v":{"$error":"#NUM!"}},{"$f":"C3/10","v":{"$error":"#NUM!"}}]
[null,"1/8-08-SA",{"$f":"'10A61 3\" Density LINEST'!E35","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-08-SS",{"$f":"'10A61 3\" Density LINEST'!E51","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-08-CA",{"$f":"'10A61 3\" Density LINEST'!E67","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-08-TA",{"$f":"'10A61 3\" Density LINEST'!E83","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-20-BG",{"$f":"'10A61 3\" Density LINEST'!E99","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-20-SA",{"$f":"'10A61 3\" Density LINEST'!E115","v":{"$error":"#NUM!"}},{"$f":"C9/10","v":{"$error":"#NUM!"}}]
[null,"1/8-20-SS",{"$f":"'10A61 3\" Density LINEST'!E131","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-20-CA",{"$f":"'10A61 3\" Density LINEST'!E147","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/8-20-TA",{"$f":"'10A61 3\" Density LINEST'!E163","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-15-CD",{"$f":"'10A61 3\" Density LINEST'!E179","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-15-SA",{"$f":"'10A61 3\" Density LINEST'!E195","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-20-CD",{"$f":"'10A61 3\" Density LINEST'!E211","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-20-SA",{"$f":"'10A61 3\" Density LINEST'!E227","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-15-SS",{"$f":"'10A61 3\" Density LINEST'!E243","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-15-CA",{"$f":"'10A61 3\" Density LINEST'!E259","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-20-SS",{"$f":"'10A61 3\" Density LINEST'!E275","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-15-TA",{"$f":"'10A61 3\" Density LINEST'!E291","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-G-SA",{"$f":"'10A61 3\" Density LINEST'!E307","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-20-CA",{"$f":"'10A61 3\" Density LINEST'!E323","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-20-TA",{"$f":"'10A61 3\" Density LINEST'!E339","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-P-SA",{"$f":"'10A61 3\" Density LINEST'!E355","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-G-SS",{"$f":"'10A61 3\" Density LINEST'!E371","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-P-SS",{"$f":"'10A61 3\" Density LINEST'!E387","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-G-CA",{"$f":"'10A61 3\" Density LINEST'!E403","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-G-TA",{"$f":"'10A61 3\" Density LINEST'!E419","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-P-CA",{"$f":"'10A61 3\" Density LINEST'!E435","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]
[null,"1/4-41-P-TA",{"$f":"'10A61 3\" Density LINEST'!E451","v":{"$error":"#NUM!"}},{"$error":"#NUM!"}]

{"sheet":"Sheet2","index":5,"n_rows":67,"n_cols":24,"rows_kept":67,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[null,null,"1/8-08-SS"]
[null,null,1.2,1.4,1.6,{"$f":"INDIRECT(\"RC[-1]\",0)","v":1.6},null,null,null,null,"1/4-15-ss"]
[null,0.5,26.45,567,null,null,null,null,null,null,378.5]
[null,0.6,24.3,null,null,null,null,null,null,null,375.1]
[null,0.7,22.46,null,null,null,null,null,null,null,370.9]
[null,0.8,20.72,null,null,null,null,null,null,null,366]
[null,0.9,19.010000000000002,null,null,null,null,null,null,null,360]
[null,1,17.600000000000001,null,null,null,null,{"$f":"INDEX(B8:C29,1,1)","v":0.5},null,null,354.7]
[null,1.25,14.74,null,null,null,null,null,null,null,340.9]
[null,1.5,12.66,null,null,null,null,null,null,null,328.9]
[1.2,1.75,11.02,null,null,null,null,null,null,null,315.39999999999998]
[null,2,9.6890000000000001,567,null,null,null,null,null,null,301.2]
[null,2.25,8.6530000000000005,null,null,null,null,null,null,null,286.7]
[null,2.5,7.8280000000000003,null,null,null,null,null,null,null,270.3]
[null,2.75,7.149,null,567567,null,null,null,null,null,256.3]
[null,3,6.5819999999999999,null,null,null,null,null,null,null,244.2]
[null,3.25,6.0990000000000002,null,null,null,null,null,null,null,233.4]
[null,3.5,5.6920000000000002,null,null,null,null,null,null,null,221.4]
[null,3.75,5.3380000000000001,null,null,null,null,null,null,null,210.9]
[null,4,5.0259999999999998,null,null,null,null,null,null,null,201.4]
[null,4.25,4.75,null,null,null,null,null,null,null,192.9]
[null,4.5,4.468,null,null,null,null,null,null,null,184.3]
[null,4.75,4.2060000000000004,null,null,null,null,null,null,null,176.2]
[null,5,3.9710000000000001,null,null,null,null,null,null,null,168.8]
[]
[]
[]
[]
[]
[null,null,null,null,{"$f":"LINEST(C$8:C$29,$B$8:$B$29^{1,2,3,4,5})","v":-3.9218989460610157E-2},0.69416844568190095,-4.9707321028605698,18.469696697786905,-37.8198637221114,41.346360554077307]
[null,null,null,null,{"$f":"LINEST(C$8:C$29,$B$8:$B$29^{1,2,3,4,5})","v":-3.9218989460610157E-2},0.69416844568190095,-4.9707321028605698,18.469696697786905,-37.8198637221114,41.346360554077307]
[null,null,null,null,null,null,{"$f":"LINEST(E$8:E$29,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,{"$f":"LINEST(P14:P35,O14:O35^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,{"$f":"LINEST(F$8:F$29,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"$f":"LINEST(X14:X35,O14:O35^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,{"$f":"LINEST(G$8:G$29,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRANSPOSE(E35:J35)","v":-3.9218989460610157E-2},{"$f":"TRANSPOSE(F35:K35)","v":0.69416844568190095},{"$f":"TRANSPOSE(K23:K29)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,{"$f":"LINEST(C$8:C$29,$B$8:$B$29^{1,2,3,4,5})","v":-3.9218989460610157E-2},0.69416844568190095,-4.9707321028605698,18.469696697786905,-37.8198637221114,41.346360554077307,null,null,null,null,{"$f":"INDEX(E35:J35,ROWS(O42:O47)*2-1)","v":{"$error":"#REF!"}},null,0.69416844568190095,-4.9707321028605698]
[null,null,null,null,{"$f":"LINEST(C8:C29,$B$8:$B$29^{1,2,3,4,5})","v":-3.9218989460610157E-2},0.69416844568190095,-4.9707321028605698,18.469696697786905,-37.8198637221114,41.346360554077307,null,null,null,null,{"$error":"#REF!"},null,-4.9707321028605698,18.469696697786905]
[null,null,null,null,{"$f":"LINEST(C9:C30,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,{"$error":"#REF!"},null,18.469696697786905,-37.8198637221114]
[null,null,null,null,{"$f":"LINEST(C10:C31,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,{"$error":"#REF!"},null,-37.8198637221114,41.346360554077307]
[null,null,null,null,{"$f":"LINEST(C8:C29,$B$8:$B$29^{1,2,3,4,5})","v":-3.9218989460610157E-2},0.69416844568190095,-4.9707321028605698,18.469696697786905,-37.8198637221114,41.346360554077307,null,null,null,null,{"$error":"#REF!"},null,41.346360554077307,0]
[null,null,null,null,{"$f":"LINEST(C12:C33,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,{"$error":"#REF!"},null,{"$f":"TRANSPOSE(E41:J41)","v":0}]
[null,null,null,null,{"$f":"LINEST(C13:C34,$B$8:$B$29^{1,2,3,4,5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,null,null,null,{"$error":"#REF!"},null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[null,null,null,null,null,null,null,null,null,null,1.2]
[null,null,0.5,0.6,0.7,0.8,0.9,1,1.25,1.5,1.75,2,2.25,2.5,2.75,3,3.25,3.5,3.75,4,4.25,4.5,4.75,5]
["1/8-08-SS",1.2,26.45,24.3,22.46,20.72,19.010000000000002,17.600000000000001,14.74,12.66,11.02,9.6890000000000001,8.6530000000000005,7.8280000000000003,7.149,6.5819999999999999,6.0990000000000002,5.6920000000000002,5.3380000000000001,5.0259999999999998,4.75,4.468,4.2060000000000004,3.9710000000000001]
[null,1.4,567,null,null,null,null,null,null,null,null,567]
[null,1.6,null,null,null,null,null,null,null,null,null,null,null,null,567567]
[]
[]
[null,null,{"$f":"LINEST(C53:X53,$C$52:$X$52^{1;2;3;4;5})","v":-3.9218989460610157E-2},0.69416844568190095,-4.9707321028605698,18.469696697786905,-37.8198637221114,41.346360554077307]
[null,null,{"$f":"LINEST(C54:X54,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C55:X55,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C56:X56,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C57:X57,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C58:X58,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C59:X59,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C60:X60,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C61:X61,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,{"$f":"LINEST(C62:X62,$C$52:$X$52^{1;2;3;4;5})","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]

{"sheet":"5\" Theoretical Test","index":6,"n_rows":33,"n_cols":19,"rows_kept":33,"cut":false,"hidden":true,"merged":[[18,0,18,1]]}
["x","y"]
["N","C"]
[30,0.08,null,{"$f":"LINEST(B3:B9,LN(A3:A9))","v":0.13693027110752118},-0.39603758830901137]
[45,0.12,null,30,700,null,null,null,null,null,null,null,null,null,"N","C","W","actual","% error"]
[70,0.18,null,null,null,null,null,null,null,null,null,null,null,"SS",{"$f":"1142*SQRT(7.02)","v":3025.7612728039203},{"$f":"$D$17*LN(O5)+$E$17","v":0.61774362837822128},{"$f":"P5*434*SQRT(7.02)","v":710.34047312994596},716.4,{"$f":"100*(R5-Q5)/R5","v":0.84583010469765696}]
[100,0.23,null,null,null,null,null,null,null,null,null,null,null,"CA",{"$f":"1142*SQRT(14)","v":4272.972735695841},{"$f":"$D$17*LN(O6)+$E$17","v":0.64340692652263498},{"$f":"P6*434*SQRT(14)","v":1044.8151932270221},1042,{"$f":"100*(R6-Q6)/R6","v":-0.27017209472380654}]
[200,0.33,null,null,null,null,null,null,null,null,null,null,null,"TA",{"$f":"1142*SQRT(15.6)","v":4510.5385931172341},{"$f":"$D$17*LN(O7)+$E$17","v":0.64743001963515112},{"$f":"P7*434*SQRT(15.6)","v":1109.8003599121164},1108,-0.16248735668920503]
[400,0.43]
[700,0.5]
[1000,0.54]
[2000,0.59299999999999997]
[5000,0.66,null,null,null,null,null,null,null,null,null,null,null,"R","Pstp","Popt"]
[10000,0.7,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(30/14.7)*(530/560)","v":1.9314868804664722},1.1999999999999999E-3,{"$f":"O13*N13","v":2.3177842565597663E-3}]
[20000,0.72050000000000003,null,null,null,null,null,null,null,null,null,null,null,"Ustp","temp coef","t-70","Uopt"]
[40000,0.75,null,null,null,null,null,null,null,null,null,null,null,1.8120000000000001E-2,2.5999999999999998E-5,30,{"$f":"N15+O15*P15","v":1.89E-2}]
[100000,0.78]
[200000,0.8,null,{"$f":"LINEST(B9:B13,LN(A9:A13))","v":7.4354677851053805E-2},2.1796982542503951E-2,null,null,null,null,null,null,null,null,null,"N","C","W","actual","%error"]
[null,null,null,700,10000,null,null,null,null,null,null,null,null,"SS",{"$f":"(1142/$Q$15)*SQRT((8.02-$P$13)*$P$13)","v":8236.9271212727472},{"$f":"D17*LN(O18)+E17","v":0.69220720846536632},{"$f":"P18*434*SQRT((8.02-$P$13)*$P$13)","v":40.953098961677782},40.450000000000003,{"$f":"100*(R18-Q18)/R18","v":-1.2437551586595272}]
["1/4-25",null,null,null,null,null,null,null,null,null,null,null,null,"CA",{"$f":"(1142/$Q$15)*SQRT((15-$P$13)*$P$13)","v":11265.56240368002},{"$f":"D32*LN(O19)+E32","v":0.70380957305091951},{"$f":"P19*434*SQRT((15-$P$13)*$P$13)","v":56.949967044599859},56.59,{"$f":"100*(R19-Q19)/R19","v":-0.63609656228990186}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"TA",{"$f":"(1142/$Q$15)*SQRT((16.6-$P$13)*$P$13)","v":11851.260016462829},{"$f":"D32*LN(O20)+E32","v":0.70553929395998438},{"$f":"P20*434*SQRT((16.6-$P$13)*$P$13)","v":60.058041066852127},59.82,-0.3979288981145544]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"LINEST(B13:B17,LN(A13:A17))","v":3.4127758675246346E-2},0.38541445135148822]
[null,null,null,10000,200000]

{"sheet":"10A61 3\" Gas+liquid Curves","index":7,"n_rows":128,"n_cols":21,"rows_kept":128,"cut":false,"hidden":true,"merged":[]}
[]
[]
["1/8-08","X",21,15,13,4.5999999999999996,4,2.5,2,1.8,1.5,1.25,0.94,0.78,0.64,0.36,0.25,0.13]
[null,"Y",1,1.4,1.6,4.4000000000000004,5,8,10,11,13,15.1,19,22,25,32,34,35]
[]
[]
[]
[null,null,{"$f":"LINEST(LN(C4:K4),LN(C3:K3))","v":-0.97387384072301764},2.9681733559373455,null,null,null,null,null,null,{"$f":"LINEST(K4:R4,K3:R3^{1;2;3;4})","v":-19.098143812200441},71.813858472749217,-84.521345409750552,15.433358760513263,34.315359228047079,null,{"$f":"K8*(0.5^4)+L8*0.5^3+M8*0.5^2+N8*0.5+O8","v":28.684800576697196}]
[null,null,null,{"$f":"EXP(D8)","v":19.456347295687859}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/8-20","X",90,80,44,26,12,8.4,7,4.5999999999999996,3.2,1.8,1.5,1.2,1,0.6,0.12]
[null,"Y",1.6,1.8,3.3,5.6,12,17,20,30,42,68,76,84,90,100,110]
[]
[null,null,{"$f":"LINEST(LN(C28:J28),LN(C27:J27))","v":-0.98807102107474298},4.9265438410321547]
[null,null,null,{"$f":"EXP(D30)","v":137.90207627014709},null,null,null,null,null,{"$f":"LINEST(J28:Q28,J27:Q27^{1;2;3;4})","v":-0.47262646109200579},4.9333024826654661,-13.810759116791797,-12.610865069447886,111.67497350218625]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-15","X",70,58,38,35,19,15,13,12,10,6.6,4,3.4,3,2.5,1.7,1,0.88,0.5,0.13]
[null,"Y",14,17,26,28,51,66,76,75,97,150,210,230,260,290,350,390,400,420,437]
[]
[]
[null,null,{"$f":"LINEST(LN(C51:I51),LN(C50:I50))","v":-1.0009407190145534},6.893772807903952,null,null,null,null,null,{"$f":"LINEST(I51:U51,I50:U50^{1;2;3;4})","v":-9.6145417061474746E-3},4.7592060839260077E-2,4.8720518779824369,-80.087044961569219,459.07257891595384]
[null,null,null,{"$f":"EXP(D54)","v":986.11482964111372}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-20","X",86,58,36,30,27,24,18,12,7.6,4.5999999999999996,3.4,1.9,1.5,0.7,0.13]
[null,"Y",25,34,60,72,80,90,120,180,280,400,460,540,560,600,620]
[]
[]
[null,null,{"$f":"LINEST(LN(C77:K77),LN(C76:K76))","v":-1.01337793516429},7.7092385285920919,null,null,null,null,null,null,{"$f":"LINEST(K77:Q77,K76:Q76^{1;2;3;4})","v":-0.10886394698005425},2.0155820126125392,-11.048599635382233,-29.999107414230895,624.55164261782738]
[null,null,null,{"$f":"EXP(D80)","v":2228.8444105451795}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-41-G","X",98,58,46,39,32,27,24,20,15,12,8.1999999999999993,6.2,4.4000000000000004,2,1.2,0.44,0.11]
[null,"Y",90,150,190,220,270,320,360,430,540,620,740,820,920,1100,1200,1300,1370]
[]
[]
[null,null,{"$f":"LINEST(LN(C101:I101),LN(C100:I100))","v":-0.98471286020147009},9.011791040675309,null,null,null,null,null,null,null,{"$f":"LINEST(I101:S101,I100:S100^{1;2;3;4})","v":9.7181331831853717E-3},-0.58315127430627278,12.8713364351882,-149.27494739622105,1368.572077312846]
[null,null,null,{"$f":"EXP(D104)","v":8199.1932205595149}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-41-P","X",90,70,58,46,34,27,22,18,12,8,6,4.2,2.7,1.6,0.5,0.11]
[null,"Y",150,190,230,290,390,480,580,680,900,1100,1200,1300,1400,1500,1600,1630]
[]
[]
[null,null,{"$f":"LINEST(LN(C124:I124),LN(C123:I123))","v":-0.96591145157053193},9.3591624714358996,null,null,null,null,null,null,null,{"$f":"LINEST(I124:R124,I123:R123^{1;2;3;4})","v":5.6543339749193233E-3},-0.28433599684739286,5.9205898453107562,-101.16140921122313,1643.9548772023693]
[null,null,null,{"$f":"EXP(D127)","v":11604.66523222963}]

{"sheet":"10A61 3\" Gas+liquid Calcs","index":8,"n_rows":42,"n_cols":18,"rows_kept":42,"cut":false,"hidden":true,"merged":[[5,9,5,10],[5,13,5,14],[5,16,5,17]]}
[]
[null,"Operating Temp Deg F","Operating Pressure psia","Standard Density","R Standard","R Normal/Actual","Operating Density","Standard Viscosity","temp coeff","t-32","t-70","Operating Viscosity"]
[null,{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),G3/E3,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),G3/F3,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},{"$f":"(C3/14.7)*(530/(460+B3))","v":0},{"$f":"(C3/14.7)*(492/(460+B3))","v":0},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M46*'10A61 5\" Calcs'!L46,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N46*'10A61 5\" Calcs'!L46,\"\"))))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"B3-32","v":-32},{"$f":"B3-70","v":-70},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P46+'10A61 5\" Calcs'!Q46*'10A61 5\" Calcs'!S46,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P46+'10A61 5\" Calcs'!Q46*'10A61 5\" Calcs'!R46,\"\")))","v":""}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Gas",null,null,null,"Liquid",null,null,"RESULTS"]
["Tube",null,null,null,null,null,"Float","X gas","Y gas","W grams/min","mL/min","X liquid","Y liquid","W grams/min","mL/min",null,"(mL/min)","Tube/Float"]
["1/8-08",-0.97387384072301764,2.9681733559373455,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H8<$B$11+0.001,$B$10*(H8^4)+$C$10*(H8^3)+$D$10*(H8^2)+$E$10*H8+$F$10,$C$9*(H8^$B$8))","v":{"$error":"#VALUE!"}},{"$f":"I8/(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J8/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J8/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J8/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J8/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J8/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L8<$B$11+0.001,$B$10*(L8^4)+$C$10*(L8^3)+$D$10*(L8^2)+$E$10*L8+$F$10,$C$9*(L8^$B$8))","v":{"$error":"#DIV/0!"}},{"$f":"M8/(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N8/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K8,\nIF('VA Sizing'!$C$3=\"Liquid\",O8,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G8)","v":"1/8-08-BG"}]
[null,null,19.456347295687859,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H9<$B$11+0.001,$B$10*(H9^4)+$C$10*(H9^3)+$D$10*(H9^2)+$E$10*H9+$F$10,$C$9*(H9^$B$8))","v":{"$error":"#VALUE!"}},{"$f":"I9/(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J9/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J9/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J9/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J9/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J9/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L9<$B$11+0.001,$B$10*(L9^4)+$C$10*(L9^3)+$D$10*(L9^2)+$E$10*L9+$F$10,$C$9*(L9^$B$8))","v":{"$error":"#DIV/0!"}},{"$f":"M9/(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N9/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K9,\nIF('VA Sizing'!$C$3=\"Liquid\",O9,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G9)","v":"1/8-08-SA"}]
[null,-19.098143812200441,71.813858472749217,-84.521345409750552,15.433358760513263,34.315359228047079,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I10/(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J10/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J10/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J10/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J10/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J10/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M10/(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N10/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K10,\nIF('VA Sizing'!$C$3=\"Liquid\",O10,\"\"))","v":""},"1/8-08-SS"]
[null,1.5,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I11/(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J11/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J11/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J11/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J11/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J11/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M11/(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N11/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K11,\nIF('VA Sizing'!$C$3=\"Liquid\",O11,\"\"))","v":""},"1/8-08-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I12/(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J12/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J12/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J12/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J12/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J12/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M12/(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N12/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K12,\nIF('VA Sizing'!$C$3=\"Liquid\",O12,\"\"))","v":""},"1/8-08-TA"]
[]
["1/8-20",-0.98807102107474298,4.9265438410321547,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H14<$B$17+0.001,$B$16*(H14^4)+$C$16*(H14^3)+$D$16*(H14^2)+$E$16*H14+$F$16,$C$15*(H14^$B$14))","v":{"$error":"#VALUE!"}},{"$f":"I14/(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J14/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J14/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J14/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J14/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J14/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L14<$B$17+0.001,$B$16*(L14^4)+$C$16*(L14^3)+$D$16*(L14^2)+$E$16*L14+$F$16,$C$15*(L14^$B$14))","v":{"$error":"#DIV/0!"}},{"$f":"M14/(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N14/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K14,\nIF('VA Sizing'!$C$3=\"Liquid\",O14,\"\"))","v":""},{"$f":"CONCATENATE($A$14,\"-\",G14)","v":"1/8-20-BG"}]
[null,null,137.90207627014709,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H15<$B$17+0.001,$B$16*(H15^4)+$C$16*(H15^3)+$D$16*(H15^2)+$E$16*H15+$F$16,$C$15*(H15^$B$14))","v":{"$error":"#VALUE!"}},{"$f":"I15/(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J15/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J15/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J15/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J15/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J15/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L15<$B$17+0.001,$B$16*(L15^4)+$C$16*(L15^3)+$D$16*(L15^2)+$E$16*L15+$F$16,$C$15*(L15^$B$14))","v":{"$error":"#DIV/0!"}},{"$f":"M15/(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N15/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K15,\nIF('VA Sizing'!$C$3=\"Liquid\",O15,\"\"))","v":""},{"$f":"CONCATENATE($A$14,\"-\",G15)","v":"1/8-20-SA"}]
[null,-0.47262646109200579,4.9333024826654661,-13.810759116791797,-12.610865069447886,111.67497350218625,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I16/(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J16/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J16/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J16/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J16/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J16/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M16/(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N16/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K16,\nIF('VA Sizing'!$C$3=\"Liquid\",O16,\"\"))","v":""},"1/8-20-SS"]
[null,4.5999999999999996,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I17/(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J17/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J17/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J17/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J17/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J17/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M17/(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N17/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K17,\nIF('VA Sizing'!$C$3=\"Liquid\",O17,\"\"))","v":""},"1/8-20-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I18/(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J18/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J18/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J18/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J18/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J18/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M18/(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N18/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K18,\nIF('VA Sizing'!$C$3=\"Liquid\",O18,\"\"))","v":""},"1/8-20-TA"]
[]
["1/4-15",-1.0009407190145534,6.893772807903952,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H20<$B$23+0.001,$B$22*(H20^4)+$C$22*(H20^3)+$D$22*(H20^2)+$E$22*H20+$F$22,$C$21*(H20^$B$20))","v":{"$error":"#VALUE!"}},{"$f":"I20/(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J20/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J20/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J20/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J20/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J20/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L20<$B$23+0.001,$B$22*(L20^4)+$C$22*(L20^3)+$D$22*(L20^2)+$E$22*L20+$F$22,$C$21*(L20^$B$20))","v":{"$error":"#DIV/0!"}},{"$f":"M20/(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N20/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K20,\nIF('VA Sizing'!$C$3=\"Liquid\",O20,\"\"))","v":""},{"$f":"CONCATENATE($A$20,\"-\",G20)","v":"1/4-15-BG"}]
[null,null,986.11482964111372,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H21<$B$23+0.001,$B$22*(H21^4)+$C$22*(H21^3)+$D$22*(H21^2)+$E$22*H21+$F$22,$C$21*(H21^$B$20))","v":{"$error":"#VALUE!"}},{"$f":"I21/(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J21/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J21/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J21/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J21/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J21/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L21<$B$23+0.001,$B$22*(L21^4)+$C$22*(L21^3)+$D$22*(L21^2)+$E$22*L21+$F$22,$C$21*(L21^$B$20))","v":{"$error":"#DIV/0!"}},{"$f":"M21/(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N21/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K21,\nIF('VA Sizing'!$C$3=\"Liquid\",O21,\"\"))","v":""},{"$f":"CONCATENATE($A$20,\"-\",G21)","v":"1/4-15-SA"}]
[null,-9.6145417061474746E-3,4.7592060839260077E-2,4.8720518779824369,-80.087044961569219,459.07257891595384,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I22/(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J22/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J22/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J22/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J22/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J22/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M22/(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N22/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K22,\nIF('VA Sizing'!$C$3=\"Liquid\",O22,\"\"))","v":""},"1/4-15-SS"]
[null,13,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I23/(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J23/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J23/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J23/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J23/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J23/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M23/(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N23/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K23,\nIF('VA Sizing'!$C$3=\"Liquid\",O23,\"\"))","v":""},"1/4-15-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I24/(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J24/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J24/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J24/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J24/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J24/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M24/(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N24/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K24,\nIF('VA Sizing'!$C$3=\"Liquid\",O24,\"\"))","v":""},"1/4-15-TA"]
[]
["1/4-20",-1.01337793516429,7.7092385285920919,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H26<$B$29+0.001,$B$28*(H26^4)+$C$28*(H26^3)+$D$28*(H26^2)+$E$28*H26+$F$28,$C$27*(H26^$B$26))","v":{"$error":"#VALUE!"}},{"$f":"I26/(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J26/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J26/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J26/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J26/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J26/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L26<$B$29+0.001,$B$28*(L26^4)+$C$28*(L26^3)+$D$28*(L26^2)+$E$28*L26+$F$28,$C$27*(L26^$B$26))","v":{"$error":"#DIV/0!"}},{"$f":"M26/(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N26/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K26,\nIF('VA Sizing'!$C$3=\"Liquid\",O26,\"\"))","v":""},{"$f":"CONCATENATE($A$26,\"-\",G26)","v":"1/4-20-BG"}]
[null,null,2228.8444105451795,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H27<$B$29+0.001,$B$28*(H27^4)+$C$28*(H27^3)+$D$28*(H27^2)+$E$28*H27+$F$28,$C$27*(H27^$B$26))","v":{"$error":"#VALUE!"}},{"$f":"I27/(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J27/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J27/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J27/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J27/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J27/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L27<$B$29+0.001,$B$28*(L27^4)+$C$28*(L27^3)+$D$28*(L27^2)+$E$28*L27+$F$28,$C$27*(L27^$B$26))","v":{"$error":"#DIV/0!"}},{"$f":"M27/(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N27/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K27,\nIF('VA Sizing'!$C$3=\"Liquid\",O27,\"\"))","v":""},{"$f":"CONCATENATE($A$26,\"-\",G27)","v":"1/4-20-SA"}]
[null,-0.10886394698005425,2.0155820126125392,-11.048599635382233,-29.999107414230895,624.55164261782738,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I28/(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J28/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J28/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J28/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J28/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J28/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M28/(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N28/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K28,\nIF('VA Sizing'!$C$3=\"Liquid\",O28,\"\"))","v":""},"1/4-20-SS"]
[null,7.6,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I29/(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J29/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J29/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J29/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J29/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J29/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M29/(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N29/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K29,\nIF('VA Sizing'!$C$3=\"Liquid\",O29,\"\"))","v":""},"1/4-20-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I30/(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J30/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J30/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J30/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J30/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J30/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M30/(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N30/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K30,\nIF('VA Sizing'!$C$3=\"Liquid\",O30,\"\"))","v":""},"1/4-20-TA"]
[]
["1/4-41-G",-0.98471286020147009,9.011791040675309,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H32<$B$35+0.001,$B$34*(H32^4)+$C$34*(H32^3)+$D$34*(H32^2)+$E$34*H32+$F$34,$C$33*(H32^$B$32))","v":{"$error":"#VALUE!"}},{"$f":"I32/(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J32/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J32/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J32/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J32/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J32/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L32<$B$35+0.001,$B$34*(L32^4)+$C$34*(L32^3)+$D$34*(L32^2)+$E$34*L32+$F$34,$C$33*(L32^$B$32))","v":{"$error":"#DIV/0!"}},{"$f":"M32/(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N32/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K32,\nIF('VA Sizing'!$C$3=\"Liquid\",O32,\"\"))","v":""},{"$f":"CONCATENATE($A$32,\"-\",G32)","v":"1/4-41-G-BG"}]
[null,null,8199.1932205595149,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H33<$B$35+0.001,$B$34*(H33^4)+$C$34*(H33^3)+$D$34*(H33^2)+$E$34*H33+$F$34,$C$33*(H33^$B$32))","v":{"$error":"#VALUE!"}},{"$f":"I33/(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J33/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J33/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J33/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J33/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J33/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L33<$B$35+0.001,$B$34*(L33^4)+$C$34*(L33^3)+$D$34*(L33^2)+$E$34*L33+$F$34,$C$33*(L33^$B$32))","v":{"$error":"#DIV/0!"}},{"$f":"M33/(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N33/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K33,\nIF('VA Sizing'!$C$3=\"Liquid\",O33,\"\"))","v":""},{"$f":"CONCATENATE($A$32,\"-\",G33)","v":"1/4-41-G-SA"}]
[null,9.7181331831853717E-3,-0.58315127430627278,12.8713364351882,-149.27494739622105,1368.572077312846,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I34/(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J34/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J34/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J34/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J34/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J34/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M34/(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N34/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K34,\nIF('VA Sizing'!$C$3=\"Liquid\",O34,\"\"))","v":""},"1/4-41-G-SS"]
[null,24,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I35/(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J35/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J35/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J35/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J35/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J35/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M35/(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N35/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K35,\nIF('VA Sizing'!$C$3=\"Liquid\",O35,\"\"))","v":""},"1/4-41-G-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I36/(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J36/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J36/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J36/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J36/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J36/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M36/(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N36/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K36,\nIF('VA Sizing'!$C$3=\"Liquid\",O36,\"\"))","v":""},"1/4-41-G-TA"]
[]
["1/4-41-P",-0.96591145157053193,9.3591624714358996,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H38<$B$41+0.001,$B$40*(H38^4)+$C$40*(H38^3)+$D$40*(H38^2)+$E$40*H38+$F$40,$C$39*(H38^$B$38))","v":{"$error":"#VALUE!"}},{"$f":"I38/(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J38/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J38/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J38/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J38/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J38/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L38<$B$41+0.001,$B$40*(L38^4)+$C$40*(L38^3)+$D$40*(L38^2)+$E$40*L38+$F$40,$C$39*(L38^$B$38))","v":{"$error":"#DIV/0!"}},{"$f":"M38/(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N38/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K38,\nIF('VA Sizing'!$C$3=\"Liquid\",O38,\"\"))","v":""},{"$f":"CONCATENATE($A$38,\"-\",G38)","v":"1/4-41-P-BG"}]
[null,null,11604.66523222963,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H39<$B$41+0.001,$B$40*(H39^4)+$C$40*(H39^3)+$D$40*(H39^2)+$E$40*H39+$F$40,$C$39*(H39^$B$38))","v":{"$error":"#VALUE!"}},{"$f":"I39/(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J39/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J39/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J39/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J39/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J39/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L39<$B$41+0.001,$B$40*(L39^4)+$C$40*(L39^3)+$D$40*(L39^2)+$E$40*L39+$F$40,$C$39*(L39^$B$38))","v":{"$error":"#DIV/0!"}},{"$f":"M39/(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N39/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K39,\nIF('VA Sizing'!$C$3=\"Liquid\",O39,\"\"))","v":""},{"$f":"CONCATENATE($A$38,\"-\",G39)","v":"1/4-41-P-SA"}]
[null,5.6543339749193233E-3,-0.28433599684739286,5.9205898453107562,-101.16140921122313,1643.9548772023693,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I40/(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J40/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J40/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J40/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J40/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J40/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M40/(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N40/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K40,\nIF('VA Sizing'!$C$3=\"Liquid\",O40,\"\"))","v":""},"1/4-41-P-SS"]
[null,22,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I41/(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J41/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J41/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J41/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J41/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J41/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M41/(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N41/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K41,\nIF('VA Sizing'!$C$3=\"Liquid\",O41,\"\"))","v":""},"1/4-41-P-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I42/(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 3\" Gas+liquid Calcs'!$G$3)*'10A61 3\" Gas+liquid Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J42/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J42/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J42/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J42/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J42/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M42/(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N42/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K42,\nIF('VA Sizing'!$C$3=\"Liquid\",O42,\"\"))","v":""},"1/4-41-P-TA"]

{"sheet":"10A61 Water","index":9,"n_rows":32,"n_cols":14,"rows_kept":32,"cut":false,"hidden":true,"merged":[[2,4,2,7]]}
[]
["Water"]
[null,null,null,null,"10A61 1.5\" Scale"]
["Density",1,"g/ml",null,"Tube","Float","Range Low (mL/min)","Range High (mL/min)"]
["Viscosity",1,"cP",null,"1/16-08","BG",0.1,0.8,"1/16-08"]
[null,null,null,null,"1/16-08","SA",0.1,1,"1/16-08"]
[null,null,null,null,"1/16-08","SS",0.4,4,"1/16-08"]
[null,null,null,null,"1/16-30","BG",1,7,"1/16-30"]
[null,null,null,null,"1/16-30","SA",1.5,13,"1/16-30"]
[null,null,null,null,"1/16-30","SS",2,22,"1/16-30"]
[null,null,null,null,"1/8-21","BG",4,38,"1/8-21"]
[null,null,null,null,"1/8-21","SA",8,60,"1/8-21",null,null,null,{"$f":"VLOOKUP(N12,$H$5:$I$18,2,TRUE)","v":"1/16-30"},{"$f":"MAX(IF(H5:H18<$K$17,H5:H18))","v":7}]
["Units","Factor (multiplied by)",null,null,"1/8-21","SS",15,120,"1/8-21",null,null,null,{"$f":"VLOOKUP(N13,$H$5:$I$18,2,TRUE)","v":"1/16-30"},{"$f":"MIN(IF(H5:H18>$K$17,H5:H18))","v":13}]
[null,null,null,null,"1/8-21","CA",20,180,"1/8-21","above",{"$f":"MIN(IF(H5:H18>$K$17,H5:H18))","v":13},null,{"$f":"VLOOKUP(N14,$H$5:$I$18,2,TRUE)","v":"1/16-30"},{"$f":"MIN(IF(H5:H18>$N$13,H5:H18))","v":22}]
["mL/min",1,null,null,"1/4-28","SA",80,580,"1/4-28","below",{"$f":"MAX(IF(H5:H18<$K$17,H5:H18))","v":7},null,"1/8-21",{"$f":"MIN(IF(H5:H18>$N$14,H5:H18))","v":38}]
["mL/h",60,null,null,"1/4-28","SS",100,850,"1/4-28"]
["mL/s",{"$f":"1/60","v":1.6666666666666666E-2},null,null,"1/4-41","SS",200,1600,"1/4-41","input",10]
["l/h",0.06,null,null,"1/4-41","CA",200,2200,"1/4-41"]
["l/min",{"$f":"1/1000","v":1E-3}]
["l/s",{"$f":"1/60000","v":1.6666666666666667E-5},null,null,null,null,null,null,null,null,"control + shift  + enter"]
["m3/h",{"$f":"60/(1000*1000)","v":6.0000000000000002E-5}]
["m3/min",{"$f":"1/(1000^2)","v":9.9999999999999995E-7}]
["ft3/h"]
["ft3/min"]
["ft3/s"]
["I GPH"]
["I GPM"]
["US GPH"]
["US GPM"]
["in3/h"]
["in3/min"]
["in3/s"]

{"sheet":"10A61 5\" Curves","index":10,"n_rows":60,"n_cols":18,"rows_kept":60,"cut":false,"hidden":true,"merged":[]}
[]
[]
["1/4-25","N",{"$f":"TRANSPOSE('5\" Theoretical Test'!$A$3:$A$17)","v":30},45,70,100,200,400,700,1000,2000,5000,10000,20000,40000,100000,200000]
[null,"C",{"$f":"TRANSPOSE('5\" Theoretical Test'!B3:B17)","v":0.08},0.12,0.18,0.23,0.33,0.43,0.5,0.54,0.59299999999999997,0.66,0.7,0.72050000000000003,0.75,0.78,0.8]
[]
[]
[]
[]
[]
["1/4-20","N",30,40,80,95,180,280,300,600,800,2200,3400,8500,14000,28000,50000,140000]
[null,"C",4.3999999999999997E-2,0.06,0.123,0.14000000000000001,0.22,0.27,0.28000000000000003,0.35,0.38,0.46,0.49,0.54,0.56000000000000005,0.57999999999999996,0.59,0.6]
[]
[]
[]
[]
[]
["1/4-16","N",30,38,90,120,160,300,600,850,2400,3400,8000,14000,20000,50000,75000]
[null,"C",2.5000000000000001E-2,3.1E-2,7.3999999999999996E-2,0.1,0.13,0.19,0.25,0.28000000000000003,0.35,0.37,0.41,0.43,0.44,0.46,0.47]
[]
[]
[]
[]
[]
["1/4-10","N",30,40,90,260,400,650,900,1600,3000,4000,7000,10000,26000,50000,120000]
[null,"C",7.0000000000000001E-3,9.1999999999999998E-3,2.1000000000000001E-2,0.06,8.7999999999999995E-2,0.12,0.14000000000000001,0.17,0.2,0.21,0.23,0.24,0.26,0.27,0.28000000000000003]
[]
[]
[]
[]
[]
["1/8-12","N",36,100,160,200,400,1000,1400,2000,3000,6000,8000,16000,36000,60000,120000]
[null,"C",1.4E-2,0.04,6.4000000000000001E-2,0.08,0.13,0.19,0.21,0.23,0.25,0.28000000000000003,0.28999999999999998,0.31,0.33,0.34,0.35]
[]
[]
[]
[]
[]
["1/8-08","N",32,70,85,180,220,450,1000,1600,2000,4500,6500,9000,14000,45000,120000]
[null,"C",4.1000000000000003E-3,8.9999999999999993E-3,1.0999999999999999E-2,2.1999999999999999E-2,2.8000000000000001E-2,5.8000000000000003E-2,9.8000000000000004E-2,0.12,0.13,0.16,0.17,0.18,0.19,0.21,0.22]
[]
[]
[]
[]
[]
["1/16-12","N",32,55,100,200,260,320,400,600,800,1800,2600,3200,5500,7000,8500]
[null,"C",0.01,1.7000000000000001E-2,3.1E-2,6.4000000000000001E-2,8.2000000000000003E-2,0.1,0.12,0.16,0.19,0.24,0.26,0.27,0.3,0.31,0.32]
[]
[]
[]
[]
[]
["1/16-16","N",45,60,80,100,180,300,400,600,700,1000,2000,2400,2800,4000,6000]
[null,"C",2.4E-2,3.2000000000000001E-2,4.4999999999999998E-2,5.3999999999999999E-2,9.8000000000000004E-2,0.16,0.2,0.26,0.28000000000000003,0.32,0.37,0.38,0.39,0.41,0.43]
[]
[]
[]
[]
[]
["1/16-20","N",36,45,75,100,180,240,280,360,400,450,500,850,2200,3600,5000]
[null,"C",0.03,3.6999999999999998E-2,0.06,8.2000000000000003E-2,0.15,0.2,0.23,0.28000000000000003,0.3,0.32,0.34,0.41,0.49,0.52,0.54]

{"sheet":"10A61 3\" Gas+liquid Results","index":11,"n_rows":69,"n_cols":19,"rows_kept":69,"cut":false,"hidden":true,"merged":[[1,1,1,3],[13,7,13,8]]}
[]
[null,"RESULTS"]
[null,"Tube/Float","Max Flow mL/min","Min Flow mL/min","Tube/Float","Max Flow Specified Units","Max Rounded"]
[null,"1/8-08-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q8","v":""},{"$f":"C4/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B4,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L8>10),CONCATENATE(\" \",B4),B4))","v":{"$error":"#DIV/0!"}},{"$f":"C4*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F4<0.99999,ROUND(F4,2),\nIF(F4<9.999,ROUND(F4,2),\nIF(F4<99.99,ROUND(F4,1),\nIF(F4<999.99,ROUND(F4,0),\nIF(F4<9999.99,ROUND(F4,-1),\nIF(F4<99999,ROUND(F4,-2),ROUND(F4,2)))))))","v":{"$error":"#VALUE!"}}]
[null,"1/8-08-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q9","v":""},{"$f":"C5/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B5,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L9>10),CONCATENATE(\" \",B5),B5))","v":{"$error":"#DIV/0!"}},{"$f":"C5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#VALUE!"}}]
[null,"1/8-08-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q10","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B6,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L10>10),CONCATENATE(\" \",B6),B6))","v":{"$error":"#DIV/0!"}},{"$f":"C6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Max Flow Raw (mL/min)","Min Flow Raw (mL/min)","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated","ED3 Data"]
[null,"1/8-08-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q11","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B7,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L11>10),CONCATENATE(\" \",B7),B7))","v":{"$error":"#DIV/0!"}},{"$f":"C7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I7,$C$4:$E$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($C$4:$C$33<'Modified Inputs'!$O$2,C4:C33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I7,$C$4:$D$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"R22","v":{"$error":"#N/A"}},{"$f":"ROUND(L7,2)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N7,\" \",\"-\",\" \",M7)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",S22,\"\"),\"\")","v":""}]
[null,"1/8-08-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q12","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B8,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L12>10),CONCATENATE(\" \",B8),B8))","v":{"$error":"#DIV/0!"}},{"$f":"C8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I8,$C$4:$E$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$4:$C$33>'Modified Inputs'!$O$2,$C$4:$C$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I8,$C$4:$D$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"R23","v":{"$error":"#N/A"}},{"$f":"ROUND(L8,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N8,\" \",\"-\",\" \",M8)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",S23,\"\"),\"\")","v":""}]
[null,"1/8-20-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q14","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B9,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L14>60),CONCATENATE(\" \",B9),B9))","v":{"$error":"#DIV/0!"}},{"$f":"C9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$f":"MIN(IF($C$4:$C$33>I8,$C$4:$C$33))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"I9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"ROUND(L9,1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",S24,\"\"),\"\")","v":""}]
[null,"1/8-20-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q15","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B10,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L15>60),CONCATENATE(\" \",B10),B10))","v":{"$error":"#DIV/0!"}},{"$f":"C10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$f":"MIN(IF($C$4:$C$33>I9,$C$4:$C$33))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"I10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",S25,\"\"),\"\")","v":""}]
[null,"1/8-20-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q16","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B11,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L16>60),CONCATENATE(\" \",B11),B11))","v":{"$error":"#DIV/0!"}},{"$f":"C11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q17","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B12,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L17>60),CONCATENATE(\" \",B12),B12))","v":{"$error":"#DIV/0!"}},{"$f":"C12*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q18","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B13,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L18>60),CONCATENATE(\" \",B13),B13))","v":{"$error":"#DIV/0!"}},{"$f":"C13*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-15-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q20","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B14,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L20>60),CONCATENATE(\" \",B14),B14))","v":{"$error":"#DIV/0!"}},{"$f":"C14*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Output"]
[null,"1/4-15-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q21","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B15,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L21>60),CONCATENATE(\" \",B15),B15))","v":{"$error":"#DIV/0!"}},{"$f":"C15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Range"]
[null,"1/4-15-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q22","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B16,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L22>60),CONCATENATE(\" \",B16),B16))","v":{"$error":"#DIV/0!"}},{"$f":"C16*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(H7,\"\")","v":""},{"$f":"IF(H16=\"\",\"\",O7)","v":""}]
[null,"1/4-15-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q23","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B17,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L23>60),CONCATENATE(\" \",B17),B17))","v":{"$error":"#DIV/0!"}},{"$f":"C17*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(H8,\"\")","v":""},{"$f":"IF(H17=\"\",\"\",O8)","v":""}]
[null,"1/4-15-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q24","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B18,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L24>60),CONCATENATE(\" \",B18),B18))","v":{"$error":"#DIV/0!"}},{"$f":"C18*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(H17=\"\",\"\",H9),\"\")","v":""},""]
[null,"1/4-20-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q26","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B19,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L26>60),CONCATENATE(\" \",B19),B19))","v":{"$error":"#DIV/0!"}},{"$f":"C19*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(OR(H17=\"\",H18=\"\"),\"\",H10),\"\")","v":""},""]
[null,"1/4-20-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q27","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B20,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L27>60),CONCATENATE(\" \",B20),B20))","v":{"$error":"#DIV/0!"}},{"$f":"C20*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-20-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q28","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B21,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L28>60),CONCATENATE(\" \",B21),B21))","v":{"$error":"#DIV/0!"}},{"$f":"C21*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,"Range","Name",null,"Requested","Modified 1","Modified 2","Output Range","Final Range","Output Name"]
[null,"1/4-20-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q29","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B22,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L29>60),CONCATENATE(\" \",B22),B22))","v":{"$error":"#DIV/0!"}},{"$f":"C22*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,100,"ED-3-100",{"$f":"R22","v":{"$error":"#N/A"}},{"$f":"K7","v":{"$error":"#N/A"}},{"$f":"N22+0.00000000001","v":{"$error":"#N/A"}},{"$f":"IF(AND(O22>0.000975,O22<0.00974999),O22*10^5,\nIF(AND(O22>0.00975,O22<0.0974999),O22*10^4,\nIF(AND(O22>0.0975,O22<0.974999),O22*10^3,\nIF(AND(O22>0.975,O22<9.74999),O22*10^2,\nIF(AND(O22>9.75,O22<97.4999),O22*10^1,\nIF(AND(O22>97.5,O22<974.999),O22*10^0,\nIF(AND(O22>975,O22<9749.99),O22*10^-1,\nIF(AND(O22>9750,O22<97499.9),O22*10^-2,\nIF(AND(O22>97500,O22<974999),O22*10^-3,\"error\")))))))))","v":{"$error":"#N/A"}},{"$f":"INDEX($K$22:$K$69,MATCH(MIN(ABS($K$22:$K$69-P22)),ABS($K$22:$K$69-P22),0))","v":{"$error":"#N/A"}},{"$f":"IF(AND(O22>0.000975,O22<0.00974999),Q22*10^-5,\nIF(AND(O22>0.00975,O22<0.0974999),Q22*10^-4,\nIF(AND(O22>0.0975,O22<0.974999),Q22*10^-3,\nIF(AND(O22>0.975,O22<9.74999),Q22*10^-2,\nIF(AND(O22>9.75,O22<97.4999),Q22*10^-1,\nIF(AND(O22>97.5,O22<974.999),Q22*10^0,\nIF(AND(O22>975,O22<9749.99),Q22*10^1,\nIF(AND(O22>9750,O22<97499.9),Q22*10^2,\nIF(AND(O22>97500,O22<974999),Q22*10^3,\"error\")))))))))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Q22,$K$22:$L$69,2,FALSE)","v":{"$error":"#N/A"}}]
[null,"1/4-20-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q30","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B23,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L30>60),CONCATENATE(\" \",B23),B23))","v":{"$error":"#DIV/0!"}},{"$f":"C23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,105,"ED-3-105",{"$f":"R23","v":{"$error":"#N/A"}},{"$f":"K8","v":{"$error":"#N/A"}},{"$f":"N23+0.00000000001","v":{"$error":"#N/A"}},{"$f":"IF(AND(O23>0.000975,O23<0.00974999),O23*10^5,\nIF(AND(O23>0.00975,O23<0.0974999),O23*10^4,\nIF(AND(O23>0.0975,O23<0.974999),O23*10^3,\nIF(AND(O23>0.975,O23<9.74999),O23*10^2,\nIF(AND(O23>9.75,O23<97.4999),O23*10^1,\nIF(AND(O23>97.5,O23<974.999),O23*10^0,\nIF(AND(O23>975,O23<9749.99),O23*10^-1,\nIF(AND(O23>9750,O23<97499.9),O23*10^-2,\nIF(AND(O23>97500,O23<974999),O23*10^-3,\"error\")))))))))","v":{"$error":"#N/A"}},{"$f":"INDEX($K$22:$K$69,MATCH(MIN(ABS($K$22:$K$69-P23)),ABS($K$22:$K$69-P23),0))","v":{"$error":"#N/A"}},{"$f":"IF(AND(O23>0.000975,O23<0.00974999),Q23*10^-5,\nIF(AND(O23>0.00975,O23<0.0974999),Q23*10^-4,\nIF(AND(O23>0.0975,O23<0.974999),Q23*10^-3,\nIF(AND(O23>0.975,O23<9.74999),Q23*10^-2,\nIF(AND(O23>9.75,O23<97.4999),Q23*10^-1,\nIF(AND(O23>97.5,O23<974.999),Q23*10^0,\nIF(AND(O23>975,O23<9749.99),Q23*10^1,\nIF(AND(O23>9750,O23<97499.9),Q23*10^2,\nIF(AND(O23>97500,O23<974999),Q23*10^3,\"error\")))))))))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Q23,$K$22:$L$69,2,FALSE)","v":{"$error":"#N/A"}}]
[null,"1/4-41-G-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q32","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L32>60),CONCATENATE(\" \",B24),B24))","v":{"$error":"#DIV/0!"}},{"$f":"C24*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,110,"ED-3-110",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"INDEX($K$22:$K$69,MATCH(MIN(ABS($K$22:$K$69-P24)),ABS($K$22:$K$69-P24),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"1/4-41-G-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q33","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L33>60),CONCATENATE(\" \",B25),B25))","v":{"$error":"#DIV/0!"}},{"$f":"C25*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,115,"ED-3-115",{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"INDEX($K$22:$K$69,MATCH(MIN(ABS($K$22:$K$69-P25)),ABS($K$22:$K$69-P25),0))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"1/4-41-G-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q34","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L34>60),CONCATENATE(\" \",B26),B26))","v":{"$error":"#DIV/0!"}},{"$f":"C26*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,120,"ED-3-120"]
[null,"1/4-41-G-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q35","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L35>60),CONCATENATE(\" \",B27),B27))","v":{"$error":"#DIV/0!"}},{"$f":"C27*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,125,"ED-3-125"]
[null,"1/4-41-G-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q36","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L36>60),CONCATENATE(\" \",B28),B28))","v":{"$error":"#DIV/0!"}},{"$f":"C28*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,130,"ED-3-130"]
[null,"1/4-41-P-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L38>60),CONCATENATE(\" \",B29),B29))","v":{"$error":"#DIV/0!"}},{"$f":"C29*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,135,"ED-3-135"]
[null,"1/4-41-P-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L39>60),CONCATENATE(\" \",B30),B30))","v":{"$error":"#DIV/0!"}},{"$f":"C30*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,140,"ED-3-140"]
[null,"1/4-41-P-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L40>60),CONCATENATE(\" \",B31),B31))","v":{"$error":"#DIV/0!"}},{"$f":"C31*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,145,"ED-3-145"]
[null,"1/4-41-P-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L41>60),CONCATENATE(\" \",B32),B32))","v":{"$error":"#DIV/0!"}},{"$f":"C32*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,150,"ED-3-150"]
[null,"1/4-41-P-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L42>60),CONCATENATE(\" \",B33),B33))","v":{"$error":"#DIV/0!"}},{"$f":"C33*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,160,"ED-3-160"]
[null,null,null,null,null,null,null,null,null,null,170,"ED-3-170"]
[null,null,null,null,null,null,null,null,null,null,180,"ED-3-180"]
[null,null,null,null,null,null,null,null,null,null,190,"ED-3-190"]
[null,null,null,null,null,null,null,null,null,null,200,"ED-3-200"]
[null,null,null,null,null,null,null,null,null,null,210,"ED-3-210"]
[null,null,null,null,null,null,null,null,null,null,220,"ED-3-220"]
[null,null,null,null,null,null,null,null,null,null,230,"ED-3-230"]
[null,null,null,null,null,null,null,null,null,null,240,"ED-3-240"]
[null,null,null,null,null,null,null,null,null,null,250,"ED-3-250"]
[null,null,null,null,null,null,null,null,null,null,260,"ED-3-260"]
[null,null,null,null,null,null,null,null,null,null,270,"ED-3-270"]
[null,null,null,null,null,null,null,null,null,null,280,"ED-3-280"]
[null,null,null,null,null,null,null,null,null,null,290,"ED-3-290"]
[null,null,null,null,null,null,null,null,null,null,300,"ED-3-300"]
[null,null,null,null,null,null,null,null,null,null,320,"ED-3-320"]
[null,null,null,null,null,null,null,null,null,null,240,"ED-3-340"]
[null,null,null,null,null,null,null,null,null,null,360,"ED-3-360"]
[null,null,null,null,null,null,null,null,null,null,380,"ED-3-380"]
[null,null,null,null,null,null,null,null,null,null,400,"ED-3-400"]
[null,null,null,null,null,null,null,null,null,null,420,"ED-3-420"]
[null,null,null,null,null,null,null,null,null,null,440,"ED-3-440"]
[null,null,null,null,null,null,null,null,null,null,460,"ED-3-460"]
[null,null,null,null,null,null,null,null,null,null,480,"ED-3-480"]
[null,null,null,null,null,null,null,null,null,null,500,"ED-3-500"]
[null,null,null,null,null,null,null,null,null,null,520,"ED-3-520"]
[null,null,null,null,null,null,null,null,null,null,540,"ED-3-540"]
[null,null,null,null,null,null,null,null,null,null,560,"ED-3-560"]
[null,null,null,null,null,null,null,null,null,null,580,"ED-3-580"]
[null,null,null,null,null,null,null,null,null,null,600,"ED-3-600"]
[null,null,null,null,null,null,null,null,null,null,650,"ED-3-650"]
[null,null,null,null,null,null,null,null,null,null,700,"ED-3-700"]
[null,null,null,null,null,null,null,null,null,null,750,"ED-3-750"]
[null,null,null,null,null,null,null,null,null,null,800,"ED-3-800"]
[null,null,null,null,null,null,null,null,null,null,850,"ED-3-850"]
[null,null,null,null,null,null,null,null,null,null,900,"ED-3-900"]
[null,null,null,null,null,null,null,null,null,null,950,"ED-3-950"]

{"sheet":"10A61 3","index":12,"n_rows":33,"n_cols":17,"rows_kept":33,"cut":false,"hidden":true,"merged":[[1,1,1,3],[13,7,13,8]]}
[]
[null,"RESULTS"]
[null,"Tube/Float","Max Flow mL/min","Min Flow mL/min","Tube/Float","Max Flow Specified Units","Max Rounded"]
[null,"1/8-08-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q8","v":""},{"$f":"C4/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B4,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L8>10),CONCATENATE(\" \",B4),B4))","v":{"$error":"#DIV/0!"}},{"$f":"C4*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F4<0.99999,ROUND(F4,2),\nIF(F4<9.999,ROUND(F4,2),\nIF(F4<99.99,ROUND(F4,1),\nIF(F4<999.99,ROUND(F4,0),\nIF(F4<9999.99,ROUND(F4,-1),\nIF(F4<99999,ROUND(F4,-2),ROUND(F4,2)))))))","v":{"$error":"#VALUE!"}}]
[null,"1/8-08-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q9","v":""},{"$f":"C5/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B5,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L9>10),CONCATENATE(\" \",B5),B5))","v":{"$error":"#DIV/0!"}},{"$f":"C5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#VALUE!"}}]
[null,"1/8-08-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q10","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B6,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L10>10),CONCATENATE(\" \",B6),B6))","v":{"$error":"#DIV/0!"}},{"$f":"C6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Max Flow Raw (mL/min)","Min Flow Raw (mL/min)","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated","ED3 Data"]
[null,"1/8-08-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q11","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B7,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L11>10),CONCATENATE(\" \",B7),B7))","v":{"$error":"#DIV/0!"}},{"$f":"C7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I7,$C$4:$E$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($C$4:$C$33<'Modified Inputs'!$O$2,C4:C33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I7,$C$4:$D$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(K7<0.99999,ROUND(K7,2),\nIF(K7<9.999,ROUND(K7,2),\nIF(K7<99.99,ROUND(K7,1),\nIF(K7<999.99,ROUND(K7,0),\nIF(K7<9999.99,ROUND(K7,-1),\nIF(K7<99999,ROUND(K7,-2),ROUND(K7,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(L7,2)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N7,\" \",\"-\",\" \",M7)","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!P7","v":""}]
[null,"1/8-08-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q12","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B8,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L12>10),CONCATENATE(\" \",B8),B8))","v":{"$error":"#DIV/0!"}},{"$f":"C8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I8,$C$4:$E$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$4:$C$33>'Modified Inputs'!$O$2,$C$4:$C$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I8,$C$4:$D$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(K8<0.99999,ROUND(K8,2),\nIF(K8<9.999,ROUND(K8,2),\nIF(K8<99.99,ROUND(K8,1),\nIF(K8<999.99,ROUND(K8,0),\nIF(K8<9999.99,ROUND(K8,-1),\nIF(K8<99999,ROUND(K8,-2),ROUND(K8,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(L8,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N8,\" \",\"-\",\" \",M8)","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!P8","v":""}]
[null,"1/8-20-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q14","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B9,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L14>60),CONCATENATE(\" \",B9),B9))","v":{"$error":"#DIV/0!"}},{"$f":"C9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$f":"MIN(IF($C$4:$C$33>I8,$C$4:$C$33))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"I9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"ROUND(L9,1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"'10A61 3\" Gas+liquid Results'!P9","v":""}]
[null,"1/8-20-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q15","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B10,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L15>60),CONCATENATE(\" \",B10),B10))","v":{"$error":"#DIV/0!"}},{"$f":"C10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#N/A"},{"$f":"MIN(IF($C$4:$C$33>I9,$C$4:$C$33))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"I10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"'10A61 3\" Gas+liquid Results'!P10","v":""}]
[null,"1/8-20-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q16","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B11,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L16>60),CONCATENATE(\" \",B11),B11))","v":{"$error":"#DIV/0!"}},{"$f":"C11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q17","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B12,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L17>60),CONCATENATE(\" \",B12),B12))","v":{"$error":"#DIV/0!"}},{"$f":"C12*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q18","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B13,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L18>60),CONCATENATE(\" \",B13),B13))","v":{"$error":"#DIV/0!"}},{"$f":"C13*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-15-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q20","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B14,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L20>60),CONCATENATE(\" \",B14),B14))","v":{"$error":"#DIV/0!"}},{"$f":"C14*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Output"]
[null,"1/4-15-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q21","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B15,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L21>60),CONCATENATE(\" \",B15),B15))","v":{"$error":"#DIV/0!"}},{"$f":"C15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Range"]
[null,"1/4-15-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q22","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B16,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L22>60),CONCATENATE(\" \",B16),B16))","v":{"$error":"#DIV/0!"}},{"$f":"C16*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(H7,\"\")","v":""},{"$f":"IF(H16=\"\",\"\",O7)","v":""}]
[null,"1/4-15-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q23","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B17,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L23>60),CONCATENATE(\" \",B17),B17))","v":{"$error":"#DIV/0!"}},{"$f":"C17*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(H8,\"\")","v":""},{"$f":"IF(H17=\"\",\"\",O8)","v":""}]
[null,"1/4-15-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q24","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B18,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L24>60),CONCATENATE(\" \",B18),B18))","v":{"$error":"#DIV/0!"}},{"$f":"C18*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(H17=\"\",\"\",H9),\"\")","v":""},""]
[null,"1/4-20-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q26","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B19,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L26>60),CONCATENATE(\" \",B19),B19))","v":{"$error":"#DIV/0!"}},{"$f":"C19*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(OR(H17=\"\",H18=\"\"),\"\",H10),\"\")","v":""},""]
[null,"1/4-20-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q27","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B20,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L27>60),CONCATENATE(\" \",B20),B20))","v":{"$error":"#DIV/0!"}},{"$f":"C20*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-20-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q28","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B21,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L28>60),CONCATENATE(\" \",B21),B21))","v":{"$error":"#DIV/0!"}},{"$f":"C21*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!N21","v":"Requested"},{"$f":"'10A61 3\" Gas+liquid Results'!O21","v":"Modified 1"},{"$f":"'10A61 3\" Gas+liquid Results'!P21","v":"Modified 2"},{"$f":"'10A61 3\" Gas+liquid Results'!Q21","v":"Output Range"},{"$f":"'10A61 3\" Gas+liquid Results'!R21","v":"Final Range"},{"$f":"'10A61 3\" Gas+liquid Results'!S21","v":"Output Name"}]
[null,"1/4-20-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q29","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B22,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L29>60),CONCATENATE(\" \",B22),B22))","v":{"$error":"#DIV/0!"}},{"$f":"C22*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!M22","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!N22","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!O22","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!P22","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!Q22","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!R22","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!S22","v":{"$error":"#N/A"}}]
[null,"1/4-20-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q30","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B23,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L30>60),CONCATENATE(\" \",B23),B23))","v":{"$error":"#DIV/0!"}},{"$f":"C23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!M23","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!N23","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!O23","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!P23","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!Q23","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!R23","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!S23","v":{"$error":"#N/A"}}]
[null,"1/4-41-G-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q32","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L32>60),CONCATENATE(\" \",B24),B24))","v":{"$error":"#DIV/0!"}},{"$f":"C24*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!M24","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!N24","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!O24","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!P24","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!Q24","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!R24","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!S24","v":{"$error":"#N/A"}}]
[null,"1/4-41-G-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q33","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L33>60),CONCATENATE(\" \",B25),B25))","v":{"$error":"#DIV/0!"}},{"$f":"C25*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!M25","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!N25","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!O25","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!P25","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!Q25","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!R25","v":{"$error":"#N/A"}},{"$f":"'10A61 3\" Gas+liquid Results'!S25","v":{"$error":"#N/A"}}]
[null,"1/4-41-G-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q34","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L34>60),CONCATENATE(\" \",B26),B26))","v":{"$error":"#DIV/0!"}},{"$f":"C26*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-G-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q35","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L35>60),CONCATENATE(\" \",B27),B27))","v":{"$error":"#DIV/0!"}},{"$f":"C27*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-G-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q36","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L36>60),CONCATENATE(\" \",B28),B28))","v":{"$error":"#DIV/0!"}},{"$f":"C28*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-P-BG",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L38>60),CONCATENATE(\" \",B29),B29))","v":{"$error":"#DIV/0!"}},{"$f":"C29*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-P-SA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L39>60),CONCATENATE(\" \",B30),B30))","v":{"$error":"#DIV/0!"}},{"$f":"C30*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-P-SS",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L40>60),CONCATENATE(\" \",B31),B31))","v":{"$error":"#DIV/0!"}},{"$f":"C31*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-P-CA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L41>60),CONCATENATE(\" \",B32),B32))","v":{"$error":"#DIV/0!"}},{"$f":"C32*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-41-P-TA",{"$f":"'10A61 3\" Gas+liquid Calcs'!Q42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",B33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 3\" Gas+liquid Calcs'!L42>60),CONCATENATE(\" \",B33),B33))","v":{"$error":"#DIV/0!"}},{"$f":"C33*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]

{"sheet":"10A61 5\" + 6\" Results","index":13,"n_rows":71,"n_cols":15,"rows_kept":71,"cut":false,"hidden":true,"merged":[[10,7,10,8]]}
[]
[null,"Tube/Float","Max Flow (mL/min)","Min Flow (mL/min)","Tube/Float"]
[null,"1/4-25-CD",{"$f":"'10A61 5\" Calcs'!AD46","v":""},{"$f":"C3/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B3,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y46<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B3),'10A61 5\" + 6\" Results'!B3))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-25-SA",{"$f":"'10A61 5\" Calcs'!AD47","v":""},{"$f":"C4/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B4,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y47<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B4),'10A61 5\" + 6\" Results'!B4))","v":{"$error":"#DIV/0!"}},null,null,"Tube/Float","Max Flow Raw (mL/min)","Min Flow Raw (mL/min)","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,"1/4-25-SS",{"$f":"'10A61 5\" Calcs'!AD48","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B5,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y48<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B5),'10A61 5\" + 6\" Results'!B5))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"VLOOKUP(I5,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($C$3:$C$71<'Modified Inputs'!$O$2,C3:C71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I5,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(K5<0.99999,ROUND(K5,2),\nIF(K5<9.999,ROUND(K5,2),\nIF(K5<99.99,ROUND(K5,1),\nIF(K5<999.99,ROUND(K5,0),\nIF(K5<9999.99,ROUND(K5,-1),\nIF(K5<99999,ROUND(K5,-2),ROUND(K5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(L5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N5,\" \",\"-\",\" \",M5)","v":{"$error":"#N/A"}}]
[null,"1/4-25-CA",{"$f":"'10A61 5\" Calcs'!AD49","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B6,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y49<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B6),'10A61 5\" + 6\" Results'!B6))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"VLOOKUP(I6,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$3:$C$71>'Modified Inputs'!$O$2,$C$3:$C$71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I6,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(K6<0.99999,ROUND(K6,2),\nIF(K6<9.999,ROUND(K6,2),\nIF(K6<99.99,ROUND(K6,1),\nIF(K6<999.99,ROUND(K6,0),\nIF(K6<9999.99,ROUND(K6,-1),\nIF(K6<99999,ROUND(K6,-2),ROUND(K6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(L6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N6,\" \",\"-\",\" \",M6)","v":{"$error":"#N/A"}}]
[null,"1/4-25-TA",{"$f":"'10A61 5\" Calcs'!AD50","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B7,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y50<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B7),'10A61 5\" + 6\" Results'!B7))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"VLOOKUP(I7,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$3:$C$71>I6,$C$3:$C$71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I7,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(N7,\" \",\"-\",\" \",M7)","v":{"$error":"#N/A"}}]
[null,"1/4-25-BG",{"$f":"'10A61 5\" Calcs'!AD51","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B8,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y51<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B8),'10A61 5\" + 6\" Results'!B8))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"VLOOKUP(I8,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$3:$C$71>I7,$C$3:$C$71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I8,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(N8,\" \",\"-\",\" \",M8)","v":{"$error":"#N/A"}}]
[null,"1/4-20-CD",{"$f":"'10A61 5\" Calcs'!AD53","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B9,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y53<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B9),'10A61 5\" + 6\" Results'!B9))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-20-SA",{"$f":"'10A61 5\" Calcs'!AD54","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B10,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y54<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B10),'10A61 5\" + 6\" Results'!B10))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-20-SS",{"$f":"'10A61 5\" Calcs'!AD55","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B11,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y55<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B11),'10A61 5\" + 6\" Results'!B11))","v":{"$error":"#DIV/0!"}},null,null,"Output"]
[null,"1/4-20-CA",{"$f":"'10A61 5\" Calcs'!AD56","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B12,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y56<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B12),'10A61 5\" + 6\" Results'!B12))","v":{"$error":"#DIV/0!"}},null,null,"Tube/Float","Range"]
[null,"1/4-20-TA",{"$f":"'10A61 5\" Calcs'!AD57","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B13,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y57<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B13),'10A61 5\" + 6\" Results'!B13))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(H5,\"\")","v":""},{"$f":"IF(H13=\"\",\"\",O5)","v":""}]
[null,"1/4-20-BG",{"$f":"'10A61 5\" Calcs'!AD58","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B14,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y58<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B14),'10A61 5\" + 6\" Results'!B14))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(H6,\"\")","v":""},{"$f":"IF(H14=\"\",\"\",O6)","v":""}]
[null,"1/4-16-CD",{"$f":"'10A61 5\" Calcs'!AD60","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B15,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y60<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B15),'10A61 5\" + 6\" Results'!B15))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(IF(H14=\"\",\"\",H7),\"\")","v":""},{"$f":"IF(H15=\"\",\"\",O7)","v":""}]
[null,"1/4-16-SA",{"$f":"'10A61 5\" Calcs'!AD61","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B16,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y61<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B16),'10A61 5\" + 6\" Results'!B16))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"IFERROR(IF(OR(H14=\"\",H15=\"\"),\"\",H8),\"\")","v":""},{"$f":"IF(H16=\"\",\"\",O8)","v":""}]
[null,"1/4-16-SS",{"$f":"'10A61 5\" Calcs'!AD62","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B17,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y62<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B17),'10A61 5\" + 6\" Results'!B17))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-16-CA",{"$f":"'10A61 5\" Calcs'!AD63","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B18,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y63<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B18),'10A61 5\" + 6\" Results'!B18))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-16-TA",{"$f":"'10A61 5\" Calcs'!AD64","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B19,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y64<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B19),'10A61 5\" + 6\" Results'!B19))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-16-BG",{"$f":"'10A61 5\" Calcs'!AD65","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B20,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y65<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B20),'10A61 5\" + 6\" Results'!B20))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-10-CD",{"$f":"'10A61 5\" Calcs'!AD67","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B21,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y67<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B21),'10A61 5\" + 6\" Results'!B21))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-10-SA",{"$f":"'10A61 5\" Calcs'!AD68","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B22,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y68<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B22),'10A61 5\" + 6\" Results'!B22))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-10-SS",{"$f":"'10A61 5\" Calcs'!AD69","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B23,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y69<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B23),'10A61 5\" + 6\" Results'!B23))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-10-CA",{"$f":"'10A61 5\" Calcs'!AD70","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y70<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B24),'10A61 5\" + 6\" Results'!B24))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-10-TA",{"$f":"'10A61 5\" Calcs'!AD71","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y71<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B25),'10A61 5\" + 6\" Results'!B25))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-10-BG",{"$f":"'10A61 5\" Calcs'!AD72","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y72<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B26),'10A61 5\" + 6\" Results'!B26))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-12-SA",{"$f":"'10A61 5\" Calcs'!AD75","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y75<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B27),'10A61 5\" + 6\" Results'!B27))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-12-SS",{"$f":"'10A61 5\" Calcs'!AD76","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y76<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B28),'10A61 5\" + 6\" Results'!B28))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-12-CA",{"$f":"'10A61 5\" Calcs'!AD77","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y77<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B29),'10A61 5\" + 6\" Results'!B29))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-12-TA",{"$f":"'10A61 5\" Calcs'!AD78","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y78<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B30),'10A61 5\" + 6\" Results'!B30))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-12-BG",{"$f":"'10A61 5\" Calcs'!AD79","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y79<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B31),'10A61 5\" + 6\" Results'!B31))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-08-SA",{"$f":"'10A61 5\" Calcs'!AD82","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y82<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B32),'10A61 5\" + 6\" Results'!B32))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-08-SS",{"$f":"'10A61 5\" Calcs'!AD83","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y83<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B33),'10A61 5\" + 6\" Results'!B33))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-08-CA",{"$f":"'10A61 5\" Calcs'!AD84","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y84<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B34),'10A61 5\" + 6\" Results'!B34))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-08-TA",{"$f":"'10A61 5\" Calcs'!AD85","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y85<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B35),'10A61 5\" + 6\" Results'!B35))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-08-BG",{"$f":"'10A61 5\" Calcs'!AD86","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y86<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B36),'10A61 5\" + 6\" Results'!B36))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-12-SA",{"$f":"'10A61 5\" Calcs'!AD89","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y89<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B37),'10A61 5\" + 6\" Results'!B37))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-12-SS",{"$f":"'10A61 5\" Calcs'!AD90","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y90<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B38),'10A61 5\" + 6\" Results'!B38))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-12-CA",{"$f":"'10A61 5\" Calcs'!AD91","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y91<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B39),'10A61 5\" + 6\" Results'!B39))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-12-TA",{"$f":"'10A61 5\" Calcs'!AD92","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y92<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B40),'10A61 5\" + 6\" Results'!B40))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-12-BG",{"$f":"'10A61 5\" Calcs'!AD93","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y93<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B41),'10A61 5\" + 6\" Results'!B41))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-16-SA",{"$f":"'10A61 5\" Calcs'!AD96","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y96<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B42),'10A61 5\" + 6\" Results'!B42))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-16-SS",{"$f":"'10A61 5\" Calcs'!AD97","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y97<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B43),'10A61 5\" + 6\" Results'!B43))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-16-CA",{"$f":"'10A61 5\" Calcs'!AD98","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y98<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B44),'10A61 5\" + 6\" Results'!B44))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-16-TA",{"$f":"'10A61 5\" Calcs'!AD99","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y99<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B45),'10A61 5\" + 6\" Results'!B45))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-16-BG",{"$f":"'10A61 5\" Calcs'!AD100","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y100<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B46),'10A61 5\" + 6\" Results'!B46))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-20-SA",{"$f":"'10A61 5\" Calcs'!AD103","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y103<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B47),'10A61 5\" + 6\" Results'!B47))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-20-SS",{"$f":"'10A61 5\" Calcs'!AD104","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y104<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B48),'10A61 5\" + 6\" Results'!B48))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-20-CA",{"$f":"'10A61 5\" Calcs'!AD105","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y105<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B49),'10A61 5\" + 6\" Results'!B49))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-20-TA",{"$f":"'10A61 5\" Calcs'!AD106","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y106<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B50),'10A61 5\" + 6\" Results'!B50))","v":{"$error":"#DIV/0!"}}]
[null,"1/16-20-BG",{"$f":"'10A61 5\" Calcs'!AD107","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B51,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y107<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B51),'10A61 5\" + 6\" Results'!B51))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-25-SA",{"$f":"'10A61 5\" Calcs'!AP47","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B52,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK47<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B52),'10A61 5\" + 6\" Results'!B52))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-25-SS",{"$f":"'10A61 5\" Calcs'!AP48","v":""},{"$f":"C53/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B53,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK48<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B53),'10A61 5\" + 6\" Results'!B53))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-25-CA",{"$f":"'10A61 5\" Calcs'!AP49","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B54,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK49<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B54),'10A61 5\" + 6\" Results'!B54))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-25-TA",{"$f":"'10A61 5\" Calcs'!AP50","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B55,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK50<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B55),'10A61 5\" + 6\" Results'!B55))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-25-BG",{"$f":"'10A61 5\" Calcs'!AP51","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B56,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK51<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B56),'10A61 5\" + 6\" Results'!B56))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-20-SA",{"$f":"'10A61 5\" Calcs'!AP54","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B57,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK54<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B57),'10A61 5\" + 6\" Results'!B57))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-20-SS",{"$f":"'10A61 5\" Calcs'!AP55","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B58,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK55<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B58),'10A61 5\" + 6\" Results'!B58))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-20-CA",{"$f":"'10A61 5\" Calcs'!AP56","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B59,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK56<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B59),'10A61 5\" + 6\" Results'!B59))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-20-TA",{"$f":"'10A61 5\" Calcs'!AP57","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B60,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK57<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B60),'10A61 5\" + 6\" Results'!B60))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-20-BG",{"$f":"'10A61 5\" Calcs'!AP58","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B61,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK58<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B61),'10A61 5\" + 6\" Results'!B61))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-16-SA",{"$f":"'10A61 5\" Calcs'!AP61","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B62,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK61<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B62),'10A61 5\" + 6\" Results'!B62))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-16-SS",{"$f":"'10A61 5\" Calcs'!AP62","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B63,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK62<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B63),'10A61 5\" + 6\" Results'!B63))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-16-CA",{"$f":"'10A61 5\" Calcs'!AP63","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B64,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK63<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B64),'10A61 5\" + 6\" Results'!B64))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-16-TA",{"$f":"'10A61 5\" Calcs'!AP64","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B65,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK64<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B65),'10A61 5\" + 6\" Results'!B65))","v":{"$error":"#DIV/0!"}}]
[null,"1/8-16-BG",{"$f":"'10A61 5\" Calcs'!AP65","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B66,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK65<30),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B66),'10A61 5\" + 6\" Results'!B66))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-40-G-6-BG",{"$f":"'10A61 10\"+6\" Calcs'!T38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B67,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B67),'10A61 5\" + 6\" Results'!B67))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-40-G-6-SA",{"$f":"'10A61 10\"+6\" Calcs'!T39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B68,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B68),'10A61 5\" + 6\" Results'!B68))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-40-G-6-SS",{"$f":"'10A61 10\"+6\" Calcs'!T40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B69,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B69),'10A61 5\" + 6\" Results'!B69))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-40-G-6-CA",{"$f":"'10A61 10\"+6\" Calcs'!T41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B70,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B70),'10A61 5\" + 6\" Results'!B70))","v":{"$error":"#DIV/0!"}}]
[null,"1/4-40-G-6-TA",{"$f":"'10A61 10\"+6\" Calcs'!T42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" + 6\" Results'!B71,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5\" + 6\" Results'!B71),'10A61 5\" + 6\" Results'!B71))","v":{"$error":"#DIV/0!"}}]

{"sheet":"10A61 10\"+6\" Curves","index":14,"n_rows":138,"n_cols":26,"rows_kept":138,"cut":false,"hidden":true,"merged":[]}
["1/8-077-G"]
[null,"X",28,26,19,16,13,9.4,6.8,5,4,3,1.9,1.2,1,0.6,0.37,0.2,0.15,0.11]
[null,"Y",1,1.1000000000000001,1.5,1.8,2.2000000000000002,3.1,4.2,5.6,7,9,13,18,20,25,29,33,35,36]
[]
[]
[null,null,{"$f":"LINEST(LN(C3:K3),LN(C2:K2))","v":-0.99522564718323192},3.3369630210724299]
[null,null,null,{"$f":"EXP(D6)","v":28.13355581651312},null,null,null,null,null,null,{"$f":"LINEST(K3:T3,K2:T2^{1;2;3;4})","v":0.36615392147128045},-3.7930708761556633,15.040874901139189,-30.898133717856396,38.978566107375613]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/8-13.3-G"]
[null,"X",90,84,62,56,42,32,22,16,13,11,9,7,5.6,5,4.2,3,2.2000000000000002,1.3,0.9,0.64,0.44,0.28000000000000003,0.15,0.11]
[null,"Y",1.3,1.4,1.9,2.1,2.8,3.7,5.4,7.4,9,10.6,12.7,16,19,21,24,30,35,44,50,54,58,62,66,68]
[]
[]
[null,null,{"$f":"LINEST(LN(C28:K28),LN(C27:K27))","v":-1.0026579886860623},4.7786376067749714,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(K28:Z28,K27:Z27^{1;2;3;4})","v":1.0879156784224131E-2},-0.35112730055377034,4.126765430230579,-22.743810491851104,68.335782309462374]
[null,null,null,{"$f":"EXP(D31)","v":118.94219357076393}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/8-32-G"]
[null,"X",100,90,80,62,50,44,38,30,24,22,20,16,13,10,7.4,5.8,4.5999999999999996,3.5,2.5,1.6,0.9,0.3,0.1]
[null,"Y",8,9,10,13,16,18,21,26,32,34,37,44,52,62,74,84,92,100,110,120,130,150,160]
[]
[]
[null,null,null,{"$f":"LINEST(LN(C56:K56),LN(C55:K55))","v":-0.97168967369697867},6.5663244942920382,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(K56:Y56,K55:Y55^{1;2;3;4})","v":1.6367296666517745E-3},-9.5076277697651229E-2,2.0320922839349831,-21.688067994504209,154.85911490071709]
[null,null,null,null,{"$f":"EXP(E59)","v":710.75266088306114}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-10-G"]
[null,"X",92,78,56,38,34,24,21,17,14,12,11,8.6,5.6,3.7,2.4,1.5,0.8,0.4,0.2,0.1]
[null,"Y",10,12,17,25,28,39,44,54,64,74,80,90,130,160,190,220,250,280,300,320]
[]
[]
[]
[null,null,{"$f":"LINEST(LN(C82:K82),LN(C81:K81))","v":-0.9855450197853951},6.7856575755914932,null,null,null,null,null,null,null,null,{"$f":"LINEST(K82:V82,K81:V81^{1;2;3;4})","v":2.7760136668528338E-2},-0.96500710273022983,12.31473006042196,-77.207495050386669,314.76278879456891]
[null,null,null,{"$f":"EXP(D86)","v":885.06189073045607}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-19-G"]
[null,"X",80,66,50,31,25,22,18,13,11,8.1999999999999993,6,4,2.8,1.3,0.6,0.3,0.2,0.1]
[null,"Y",64,76,100,150,180,200,230,280,300,340,380,420,460,520,560,600,620,660]
[]
[]
[null,null,null,{"$f":"LINEST(LN(C109:G109),LN(C108:G108))","v":-0.88985122785688997},8.0654153525387571,null,null,null,null,null,null,null,{"$f":"LINEST(G109:T109,G108:T108^{1;2;3;4})","v":6.0302239920945163E-3},-0.36054223071254216,7.6624439382943921,-78.274475467196837,629.99822294518913]
[null,null,null,null,{"$f":"EXP(E112)","v":3182.4777929336292}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["1/4-40-G","N",88,70,60,40,29,24.5,18,11.5,9,7,4.7,3,2.35,1.1499999999999999,0.35,0.15,0.1]
[null,"K",2,2.4,2.7,3.7,4.8,5.4,6.4,7.6,8.1999999999999993,8.8000000000000007,9.6,10.5,11,12,13,13.5,13.7]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(G134:S134,G133:S133^{1;2;3;4})","v":6.2412961452429293E-5},-4.3314681918760834E-3,0.10614317719263495,-1.2575928005198056,13.55252243907665]
[null,null,{"$f":"LINEST(LN(C134:G134),LN(C133:G133))","v":-0.78593610175687545},4.2120717920323996]
[null,null,null,{"$f":"EXP(D137)","v":67.496233210494708}]

{"sheet":"10A61 10\"+6\" Calcs","index":15,"n_rows":50,"n_cols":23,"rows_kept":50,"cut":false,"hidden":true,"merged":[[5,9,5,10],[5,13,5,14],[5,16,5,17],[43,15,43,16],[43,21,43,22]]}
[]
[null,"Operating Temp Deg F","Operating Pressure psia","Standard Density","R Standard","R Normal/Actual","Operating Density","Standard Viscosity","temp coeff","t-32","t-70","Operating Viscosity"]
[null,{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),G3/E3,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),G3/F3,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},{"$f":"(C3/14.7)*(530/(460+B3))","v":0},{"$f":"(C3/14.7)*(492/(460+B3))","v":0},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M46*'10A61 5\" Calcs'!L46,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N46*'10A61 5\" Calcs'!L46,\"\"))))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"B3-32","v":-32},{"$f":"B3-70","v":-70},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P46+'10A61 5\" Calcs'!Q46*'10A61 5\" Calcs'!S46,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P46+'10A61 5\" Calcs'!Q46*'10A61 5\" Calcs'!R46,\"\")))","v":""}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Gas",null,null,null,"Liquid",null,null,"RESULTS"]
["Tube",null,null,null,null,null,"Float","X gas","Y gas","W grams/min","mL/min","X liquid","Y liquid","W grams/min","mL/min",null,"(mL/min)","Tube/Float"]
["1/8-077-G-10",-0.99522564718323192,3.3369630210724299,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H8<$B$11+0.001,$B$10*(H8^4)+$C$10*(H8^3)+$D$10*(H8^2)+$E$10*H8+$F$10,$C$9*(H8^$B$8))","v":{"$error":"#VALUE!"}},{"$f":"I8/(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J8/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J8/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J8/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J8/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J8/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L8<$B$11+0.001,$B$10*(L8^4)+$C$10*(L8^3)+$D$10*(L8^2)+$E$10*L8+$F$10,$C$9*(L8^$B$8))","v":{"$error":"#DIV/0!"}},{"$f":"M8/(SQRT((7.02/((VLOOKUP(G8,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N8/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K8,\nIF('VA Sizing'!$C$3=\"Liquid\",O8,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G8)","v":"1/8-077-G-10-BG"}]
[null,null,28.13355581651312,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H9<$B$11+0.001,$B$10*(H9^4)+$C$10*(H9^3)+$D$10*(H9^2)+$E$10*H9+$F$10,$C$9*(H9^$B$8))","v":{"$error":"#VALUE!"}},{"$f":"I9/(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J9/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J9/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J9/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J9/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J9/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L9<$B$11+0.001,$B$10*(L9^4)+$C$10*(L9^3)+$D$10*(L9^2)+$E$10*L9+$F$10,$C$9*(L9^$B$8))","v":{"$error":"#DIV/0!"}},{"$f":"M9/(SQRT((7.02/((VLOOKUP(G9,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N9/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K9,\nIF('VA Sizing'!$C$3=\"Liquid\",O9,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G9)","v":"1/8-077-G-10-SA"}]
[null,0.36615392147128045,-3.7930708761556633,15.040874901139189,-30.898133717856396,38.978566107375613,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I10/(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J10/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J10/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J10/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J10/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J10/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M10/(SQRT((7.02/((VLOOKUP(G10,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N10/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K10,\nIF('VA Sizing'!$C$3=\"Liquid\",O10,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G10)","v":"1/8-077-G-10-SS"}]
[null,4,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I11/(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J11/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J11/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J11/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J11/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J11/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M11/(SQRT((7.02/((VLOOKUP(G11,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N11/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K11,\nIF('VA Sizing'!$C$3=\"Liquid\",O11,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G11)","v":"1/8-077-G-10-CA"}]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I12/(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J12/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J12/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J12/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J12/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J12/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M12/(SQRT((7.02/((VLOOKUP(G12,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N12/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K12,\nIF('VA Sizing'!$C$3=\"Liquid\",O12,\"\"))","v":""},{"$f":"CONCATENATE($A$8,\"-\",G12)","v":"1/8-077-G-10-TA"}]
[]
["1/8-13.3-G-10",-1.0026579886860623,4.7786376067749714,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H14<$B$17+0.001,$B$16*(H14^4)+$C$16*(H14^3)+$D$16*(H14^2)+$E$16*H14+$F$16,$C$15*(H14^$B$14))","v":{"$error":"#VALUE!"}},{"$f":"I14/(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J14/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J14/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J14/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J14/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J14/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L14<$B$17+0.001,$B$16*(L14^4)+$C$16*(L14^3)+$D$16*(L14^2)+$E$16*L14+$F$16,$C$15*(L14^$B$14))","v":{"$error":"#DIV/0!"}},{"$f":"M14/(SQRT((7.02/((VLOOKUP(G14,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N14/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K14,\nIF('VA Sizing'!$C$3=\"Liquid\",O14,\"\"))","v":""},{"$f":"CONCATENATE($A$14,\"-\",G14)","v":"1/8-13.3-G-10-BG"}]
[null,null,118.94219357076393,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H15<$B$17+0.001,$B$16*(H15^4)+$C$16*(H15^3)+$D$16*(H15^2)+$E$16*H15+$F$16,$C$15*(H15^$B$14))","v":{"$error":"#VALUE!"}},{"$f":"I15/(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J15/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J15/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J15/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J15/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J15/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L15<$B$17+0.001,$B$16*(L15^4)+$C$16*(L15^3)+$D$16*(L15^2)+$E$16*L15+$F$16,$C$15*(L15^$B$14))","v":{"$error":"#DIV/0!"}},{"$f":"M15/(SQRT((7.02/((VLOOKUP(G15,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N15/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K15,\nIF('VA Sizing'!$C$3=\"Liquid\",O15,\"\"))","v":""},{"$f":"CONCATENATE($A$14,\"-\",G15)","v":"1/8-13.3-G-10-SA"}]
[null,1.0879156784224131E-2,-0.35112730055377034,4.126765430230579,-22.743810491851104,68.335782309462374,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I16/(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J16/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J16/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J16/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J16/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J16/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M16/(SQRT((7.02/((VLOOKUP(G16,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N16/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K16,\nIF('VA Sizing'!$C$3=\"Liquid\",O16,\"\"))","v":""},"1/8-13.3-G-10-SS"]
[null,13,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I17/(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J17/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J17/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J17/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J17/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J17/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M17/(SQRT((7.02/((VLOOKUP(G17,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N17/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K17,\nIF('VA Sizing'!$C$3=\"Liquid\",O17,\"\"))","v":""},"1/8-13.3-G-10-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I18/(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J18/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J18/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J18/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J18/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J18/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M18/(SQRT((7.02/((VLOOKUP(G18,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N18/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K18,\nIF('VA Sizing'!$C$3=\"Liquid\",O18,\"\"))","v":""},"1/8-13.3-G-10-TA"]
[]
["1/8-32-G-10",-0.97168967369697867,6.5663244942920382,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H20<$B$23+0.001,$B$22*(H20^4)+$C$22*(H20^3)+$D$22*(H20^2)+$E$22*H20+$F$22,$C$21*(H20^$B$20))","v":{"$error":"#VALUE!"}},{"$f":"I20/(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J20/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J20/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J20/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J20/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J20/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L20<$B$23+0.001,$B$22*(L20^4)+$C$22*(L20^3)+$D$22*(L20^2)+$E$22*L20+$F$22,$C$21*(L20^$B$20))","v":{"$error":"#DIV/0!"}},{"$f":"M20/(SQRT((7.02/((VLOOKUP(G20,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N20/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K20,\nIF('VA Sizing'!$C$3=\"Liquid\",O20,\"\"))","v":""},{"$f":"CONCATENATE($A$20,\"-\",G20)","v":"1/8-32-G-10-BG"}]
[null,null,710.75266088306114,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H21<$B$23+0.001,$B$22*(H21^4)+$C$22*(H21^3)+$D$22*(H21^2)+$E$22*H21+$F$22,$C$21*(H21^$B$20))","v":{"$error":"#VALUE!"}},{"$f":"I21/(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J21/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J21/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J21/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J21/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J21/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L21<$B$23+0.001,$B$22*(L21^4)+$C$22*(L21^3)+$D$22*(L21^2)+$E$22*L21+$F$22,$C$21*(L21^$B$20))","v":{"$error":"#DIV/0!"}},{"$f":"M21/(SQRT((7.02/((VLOOKUP(G21,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N21/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K21,\nIF('VA Sizing'!$C$3=\"Liquid\",O21,\"\"))","v":""},{"$f":"CONCATENATE($A$20,\"-\",G21)","v":"1/8-32-G-10-SA"}]
[null,1.6367296666517745E-3,-9.5076277697651229E-2,2.0320922839349831,-21.688067994504209,154.85911490071709,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I22/(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J22/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J22/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J22/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J22/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J22/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M22/(SQRT((7.02/((VLOOKUP(G22,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N22/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K22,\nIF('VA Sizing'!$C$3=\"Liquid\",O22,\"\"))","v":""},"1/8-32-G-10-SS"]
[null,24,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I23/(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J23/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J23/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J23/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J23/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J23/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M23/(SQRT((7.02/((VLOOKUP(G23,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N23/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K23,\nIF('VA Sizing'!$C$3=\"Liquid\",O23,\"\"))","v":""},"1/8-32-G-10-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I24/(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J24/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J24/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J24/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J24/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J24/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M24/(SQRT((7.02/((VLOOKUP(G24,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N24/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K24,\nIF('VA Sizing'!$C$3=\"Liquid\",O24,\"\"))","v":""},"1/8-32-G-10-TA"]
[]
["1/4-10-G-10",-0.9855450197853951,6.7856575755914932,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H26<$B$29+0.001,$B$28*(H26^4)+$C$28*(H26^3)+$D$28*(H26^2)+$E$28*H26+$F$28,$C$27*(H26^$B$26))","v":{"$error":"#VALUE!"}},{"$f":"I26/(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J26/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J26/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J26/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J26/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J26/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L26<$B$29+0.001,$B$28*(L26^4)+$C$28*(L26^3)+$D$28*(L26^2)+$E$28*L26+$F$28,$C$27*(L26^$B$26))","v":{"$error":"#DIV/0!"}},{"$f":"M26/(SQRT((7.02/((VLOOKUP(G26,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N26/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K26,\nIF('VA Sizing'!$C$3=\"Liquid\",O26,\"\"))","v":""},{"$f":"CONCATENATE($A$26,\"-\",G26)","v":"1/4-10-G-10-BG"}]
[null,null,885.06189073045607,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H27<$B$29+0.001,$B$28*(H27^4)+$C$28*(H27^3)+$D$28*(H27^2)+$E$28*H27+$F$28,$C$27*(H27^$B$26))","v":{"$error":"#VALUE!"}},{"$f":"I27/(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J27/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J27/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J27/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J27/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J27/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L27<$B$29+0.001,$B$28*(L27^4)+$C$28*(L27^3)+$D$28*(L27^2)+$E$28*L27+$F$28,$C$27*(L27^$B$26))","v":{"$error":"#DIV/0!"}},{"$f":"M27/(SQRT((7.02/((VLOOKUP(G27,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N27/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K27,\nIF('VA Sizing'!$C$3=\"Liquid\",O27,\"\"))","v":""},{"$f":"CONCATENATE($A$26,\"-\",G27)","v":"1/4-10-G-10-SA"}]
[null,2.7760136668528338E-2,-0.96500710273022983,12.31473006042196,-77.207495050386669,314.76278879456891,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I28/(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J28/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J28/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J28/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J28/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J28/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M28/(SQRT((7.02/((VLOOKUP(G28,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N28/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K28,\nIF('VA Sizing'!$C$3=\"Liquid\",O28,\"\"))","v":""},"1/4-10-G-10-SS"]
[null,14,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I29/(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J29/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J29/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J29/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J29/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J29/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M29/(SQRT((7.02/((VLOOKUP(G29,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N29/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K29,\nIF('VA Sizing'!$C$3=\"Liquid\",O29,\"\"))","v":""},"1/4-10-G-10-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I30/(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J30/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J30/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J30/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J30/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J30/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M30/(SQRT((7.02/((VLOOKUP(G30,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N30/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K30,\nIF('VA Sizing'!$C$3=\"Liquid\",O30,\"\"))","v":""},"1/4-10-G-10-TA"]
[]
["1/4-19-G-10",-0.88985122785688997,8.0654153525387571,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H32<$B$35+0.001,$B$34*(H32^4)+$C$34*(H32^3)+$D$34*(H32^2)+$E$34*H32+$F$34,$C$33*(H32^$B$32))","v":{"$error":"#VALUE!"}},{"$f":"I32/(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J32/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J32/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J32/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J32/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J32/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L32<$B$35+0.001,$B$34*(L32^4)+$C$34*(L32^3)+$D$34*(L32^2)+$E$34*L32+$F$34,$C$33*(L32^$B$32))","v":{"$error":"#DIV/0!"}},{"$f":"M32/(SQRT((7.02/((VLOOKUP(G32,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N32/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K32,\nIF('VA Sizing'!$C$3=\"Liquid\",O32,\"\"))","v":""},{"$f":"CONCATENATE($A$32,\"-\",G32)","v":"1/4-19-G-10-BG"}]
[null,null,3182.4777929336292,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(H33<$B$35+0.001,$B$34*(H33^4)+$C$34*(H33^3)+$D$34*(H33^2)+$E$34*H33+$F$34,$C$33*(H33^$B$32))","v":{"$error":"#VALUE!"}},{"$f":"I33/(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J33/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J33/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J33/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J33/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J33/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L33<$B$35+0.001,$B$34*(L33^4)+$C$34*(L33^3)+$D$34*(L33^2)+$E$34*L33+$F$34,$C$33*(L33^$B$32))","v":{"$error":"#DIV/0!"}},{"$f":"M33/(SQRT((7.02/((VLOOKUP(G33,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N33/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K33,\nIF('VA Sizing'!$C$3=\"Liquid\",O33,\"\"))","v":""},{"$f":"CONCATENATE($A$32,\"-\",G33)","v":"1/4-19-G-10-SA"}]
[null,6.0302239920945163E-3,-0.36054223071254216,7.6624439382943921,-78.274475467196837,629.99822294518913,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I34/(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J34/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J34/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J34/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J34/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J34/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M34/(SQRT((7.02/((VLOOKUP(G34,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N34/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K34,\nIF('VA Sizing'!$C$3=\"Liquid\",O34,\"\"))","v":""},"1/4-19-G-10-SS"]
[null,25,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I35/(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J35/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J35/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J35/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J35/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J35/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M35/(SQRT((7.02/((VLOOKUP(G35,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N35/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K35,\nIF('VA Sizing'!$C$3=\"Liquid\",O35,\"\"))","v":""},"1/4-19-G-10-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I36/(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J36/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J36/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J36/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J36/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J36/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M36/(SQRT((7.02/((VLOOKUP(G36,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N36/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",K36,\nIF('VA Sizing'!$C$3=\"Liquid\",O36,\"\"))","v":""},"1/4-19-G-10-TA"]
[]
["1/4-40-G-10",-0.78593610175687545,4.2120717920323996,null,null,null,"BG",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(M46<$B$41+0.001,$B$40*(M46^4)+$C$40*(M46^3)+$D$40*(M46^2)+$E$40*M46+$F$40,$C$39*(M46^$B$38))","v":{"$error":"#VALUE!"}},{"$f":"I38/(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J38/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J38/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J38/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J38/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J38/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L38<$B$41+0.001,$B$40*(L38^4)+$C$40*(L38^3)+$D$40*(L38^2)+$E$40*L38+$F$40,$C$39*(L38^$B$38))","v":{"$error":"#DIV/0!"}},{"$f":"M38/(SQRT((7.02/((VLOOKUP(G38,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N38/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q46,\nIF('VA Sizing'!$C$3=\"Liquid\",W46,\"\"))","v":""},{"$f":"CONCATENATE($A$38,\"-\",G38)","v":"1/4-40-G-10-BG"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q46,\nIF('VA Sizing'!$C$3=\"Liquid\",W46,\"\"))","v":""},"1/4-40-G-6-BG"]
[null,null,67.496233210494708,null,null,null,"SA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(M47<$B$41+0.001,$B$40*(M47^4)+$C$40*(M47^3)+$D$40*(M47^2)+$E$40*M47+$F$40,$C$39*(M47^$B$38))","v":{"$error":"#VALUE!"}},{"$f":"I39/(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J39/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J39/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J39/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J39/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J39/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"IF(L39<$B$41+0.001,$B$40*(L39^4)+$C$40*(L39^3)+$D$40*(L39^2)+$E$40*L39+$F$40,$C$39*(L39^$B$38))","v":{"$error":"#DIV/0!"}},{"$f":"M39/(SQRT((7.02/((VLOOKUP(G39,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N39/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q47,\nIF('VA Sizing'!$C$3=\"Liquid\",W47,\"\"))","v":""},{"$f":"CONCATENATE($A$38,\"-\",G39)","v":"1/4-40-G-10-SA"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q47,\nIF('VA Sizing'!$C$3=\"Liquid\",W47,\"\"))","v":""},"1/4-40-G-6-SA"]
[null,6.2412961452429293E-5,-4.3314681918760834E-3,0.10614317719263495,-1.2575928005198056,13.55252243907665,"SS",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I40/(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J40/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J40/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J40/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J40/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J40/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M40/(SQRT((7.02/((VLOOKUP(G40,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N40/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q48,\nIF('VA Sizing'!$C$3=\"Liquid\",W48,\"\"))","v":""},"1/4-40-G-10-SS",null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q48,\nIF('VA Sizing'!$C$3=\"Liquid\",W48,\"\"))","v":""},"1/4-40-G-6-SS"]
[null,29,null,null,null,null,"CA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I41/(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J41/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J41/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J41/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J41/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J41/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M41/(SQRT((7.02/((VLOOKUP(G41,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N41/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q49,\nIF('VA Sizing'!$C$3=\"Liquid\",W49,\"\"))","v":""},"1/4-40-G-10-CA",null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q49,\nIF('VA Sizing'!$C$3=\"Liquid\",W49,\"\"))","v":""},"1/4-40-G-6-CA"]
[null,null,null,null,null,null,"TA",{"$f":"$L$3*(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"I42/(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'10A61 10\"+6\" Calcs'!$G$3)*'10A61 10\"+6\" Calcs'!$G$3))))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),J42/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),J42/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",J42/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",J42/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",J42/$G$3,\"\")))))","v":""},{"$f":"'Modified Inputs'!$G$2*(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"M42/(SQRT((7.02/((VLOOKUP(G42,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))))","v":{"$error":"#DIV/0!"}},{"$f":"N42/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q50,\nIF('VA Sizing'!$C$3=\"Liquid\",W50,\"\"))","v":""},"1/4-40-G-10-TA",null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",Q50,\nIF('VA Sizing'!$C$3=\"Liquid\",W50,\"\"))","v":""},"1/4-40-G-6-TA"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gas",null,null,null,null,null,"Liquid"]
[null,null,null,null,null,null,"Float","Weight grams","Diameter inches","Density g/mL",null,"F gas","N gas","K","W lbs/min","W g/min","W mL/min","F liquid","N liquid","K","W lbs/min","W g/min","W mL/min"]
[null,null,null,null,null,null,"BG",{"$f":"VLOOKUP(G46,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)*(2.54)^3*(0.125^3)*3.14159*(4/3)","v":0.34052825113299579},0.25,{"$f":"VLOOKUP(G46,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)","v":2.54},null,{"$f":"H46*((J46-$G$3)/J46)","v":{"$error":"#VALUE!"}},{"$f":"$L$3/(SQRT(L46*$G$3))","v":{"$error":"#VALUE!"}},{"$f":"I38","v":{"$error":"#VALUE!"}},{"$f":"N46*I46*SQRT(L46*$G$3)","v":{"$error":"#VALUE!"}},{"$f":"O46*453.592","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),P46/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),P46/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",P46/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",P46/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",P46/$G$3,\"\")))))","v":""},{"$f":"H46*((J46-'Modified Inputs'!$M$2)/J46)","v":0.34052825113299579},{"$f":"'Modified Inputs'!$G$2/(SQRT(R46*'Modified Inputs'!$M$2))","v":{"$error":"#DIV/0!"}},{"$f":"IF(S46<$B$41+0.001,$B$40*(S46^4)+$C$40*(S46^3)+$D$40*(S46^2)+$E$40*S46+$F$40,$C$39*(S46^$B$38))","v":{"$error":"#DIV/0!"}},{"$f":"T46*I46*SQRT(R46*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"U46*453.592","v":{"$error":"#DIV/0!"}},{"$f":"V46/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"SA",{"$f":"VLOOKUP(G47,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)*(2.54)^3*(0.125^3)*3.14159*(4/3)","v":0.53358363760209571},0.25,{"$f":"VLOOKUP(G47,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)","v":3.98},null,{"$f":"H47*((J47-$G$3)/J47)","v":{"$error":"#VALUE!"}},{"$f":"$L$3/(SQRT(L47*$G$3))","v":{"$error":"#VALUE!"}},{"$f":"I39","v":{"$error":"#VALUE!"}},{"$f":"N47*I47*SQRT(L47*$G$3)","v":{"$error":"#VALUE!"}},{"$f":"O47*453.592","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),P47/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),P47/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",P47/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",P47/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",P47/$G$3,\"\")))))","v":""},{"$f":"H47*((J47-'Modified Inputs'!$M$2)/J47)","v":0.53358363760209571},{"$f":"'Modified Inputs'!$G$2/(SQRT(R47*'Modified Inputs'!$M$2))","v":{"$error":"#DIV/0!"}},{"$f":"IF(S47<$B$41+0.001,$B$40*(S47^4)+$C$40*(S47^3)+$D$40*(S47^2)+$E$40*S47+$F$40,$C$39*(S47^$B$38))","v":{"$error":"#DIV/0!"}},{"$f":"T47*I47*SQRT(R47*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"U47*453.592","v":{"$error":"#DIV/0!"}},{"$f":"V47/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"SS",{"$f":"VLOOKUP(G48,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)*(2.54)^3*(0.125^3)*3.14159*(4/3)","v":1.0752112496404038},0.25,{"$f":"VLOOKUP(G48,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)","v":8.02},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),P48/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),P48/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",P48/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",P48/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",P48/$G$3,\"\")))))","v":""},{"$f":"H48*((J48-'Modified Inputs'!$M$2)/J48)","v":1.0752112496404038},{"$f":"'Modified Inputs'!$G$2/(SQRT(R48*'Modified Inputs'!$M$2))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"T48*I48*SQRT(R48*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"V48/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"CA",{"$f":"VLOOKUP(G49,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)*(2.54)^3*(0.125^3)*3.14159*(4/3)","v":2.0109936090531244},0.25,{"$f":"VLOOKUP(G49,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)","v":15},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),P49/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),P49/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",P49/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",P49/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",P49/$G$3,\"\")))))","v":""},{"$f":"H49*((J49-'Modified Inputs'!$M$2)/J49)","v":2.0109936090531244},{"$f":"'Modified Inputs'!$G$2/(SQRT(R49*'Modified Inputs'!$M$2))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"T49*I49*SQRT(R49*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"V49/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"TA",{"$f":"VLOOKUP(G50,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)*(2.54)^3*(0.125^3)*3.14159*(4/3)","v":2.2254995940187912},0.25,{"$f":"VLOOKUP(G50,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)","v":16.600000000000001},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),P50/$D$3,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),P50/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",P50/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",P50/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",P50/$G$3,\"\")))))","v":""},{"$f":"H50*((J50-'Modified Inputs'!$M$2)/J50)","v":2.2254995940187912},{"$f":"'Modified Inputs'!$G$2/(SQRT(R50*'Modified Inputs'!$M$2))","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"T50*I50*SQRT(R50*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"V50/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}}]

{"sheet":"10A61 10\" Results","index":16,"n_rows":38,"n_cols":16,"rows_kept":38,"cut":false,"hidden":true,"merged":[[13,8,13,9]]}
[]
[]
[null,null,"Tube/Float","Max Flow (mL/min)","Min Flow","Tube/Float","Max Flow Specified Units","Max Round"]
[null,null,"1/8-077-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q8","v":""},{"$f":"D4/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C4,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>10),CONCATENATE(\" \",'10A61 10\" Results'!C4),'10A61 10\" Results'!C4))","v":{"$error":"#DIV/0!"}},{"$f":"D4*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(G4<0.99999,ROUND(G4,2),\nIF(G4<9.999,ROUND(G4,2),\nIF(G4<99.99,ROUND(G4,1),\nIF(G4<999.99,ROUND(G4,0),\nIF(G4<9999.99,ROUND(G4,-1),\nIF(G4<99999,ROUND(G4,-2),ROUND(G4,2)))))))","v":{"$error":"#VALUE!"}}]
[null,null,"1/8-077-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q9","v":""},{"$f":"D5/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C5,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>10),CONCATENATE(\" \",'10A61 10\" Results'!C5),'10A61 10\" Results'!C5))","v":{"$error":"#DIV/0!"}},{"$f":"D5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(G5<0.99999,ROUND(G5,2),\nIF(G5<9.999,ROUND(G5,2),\nIF(G5<99.99,ROUND(G5,1),\nIF(G5<999.99,ROUND(G5,0),\nIF(G5<9999.99,ROUND(G5,-1),\nIF(G5<99999,ROUND(G5,-2),ROUND(G5,2)))))))","v":{"$error":"#VALUE!"}}]
[null,null,"1/8-077-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q10","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C6,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>10),CONCATENATE(\" \",'10A61 10\" Results'!C6),'10A61 10\" Results'!C6))","v":{"$error":"#DIV/0!"}},{"$f":"D6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/8-077-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q11","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C7,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>10),CONCATENATE(\" \",'10A61 10\" Results'!C7),'10A61 10\" Results'!C7))","v":{"$error":"#DIV/0!"}},{"$f":"D7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Max Flow Raw (mL/min)","Min Flow Raw (mL/min)","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,null,"1/8-077-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q12","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C8,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>10),CONCATENATE(\" \",'10A61 10\" Results'!C8),'10A61 10\" Results'!C8))","v":{"$error":"#DIV/0!"}},{"$f":"D8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J8,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($D$9:$D$33<'Modified Inputs'!$O$2,D9:D33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J8,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(L8<0.99999,ROUND(L8,2),\nIF(L8<9.999,ROUND(L8,2),\nIF(L8<99.99,ROUND(L8,1),\nIF(L8<999.99,ROUND(L8,0),\nIF(L8<9999.99,ROUND(L8,-1),\nIF(L8<99999,ROUND(L8,-2),ROUND(L8,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(M8,2)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(O8,\" \",\"-\",\" \",N8)","v":{"$error":"#N/A"}}]
[null,null,"1/8-13.3-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q14","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C9,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10\" Results'!C9),'10A61 10\" Results'!C9))","v":{"$error":"#DIV/0!"}},{"$f":"D9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J9,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($D$9:$D$33>'Modified Inputs'!$O$2,$D$9:$D$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J9,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(L9<0.99999,ROUND(L9,2),\nIF(L9<9.999,ROUND(L9,2),\nIF(L9<99.99,ROUND(L9,1),\nIF(L9<999.99,ROUND(L9,0),\nIF(L9<9999.99,ROUND(L9,-1),\nIF(L9<99999,ROUND(L9,-2),ROUND(L9,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(M9,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(O9,\" \",\"-\",\" \",N9)","v":{"$error":"#N/A"}}]
[null,null,"1/8-13.3-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q15","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C10,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10\" Results'!C10),'10A61 10\" Results'!C10))","v":{"$error":"#DIV/0!"}},{"$f":"D10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J10,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($D$9:$D$33>J9,$D$9:$D$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J10,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"ROUND(M10,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(O10,\" \",\"-\",\" \",N10)","v":{"$error":"#N/A"}}]
[null,null,"1/8-13.3-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q16","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C11,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10\" Results'!C11),'10A61 10\" Results'!C11))","v":{"$error":"#DIV/0!"}},{"$f":"D11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J11,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($D$9:$D$33>J10,$D$9:$D$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J11,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,"1/8-13.3-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q17","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C12,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10\" Results'!C12),'10A61 10\" Results'!C12))","v":{"$error":"#DIV/0!"}},{"$f":"D12*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/8-13.3-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q18","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C13,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10\" Results'!C13),'10A61 10\" Results'!C13))","v":{"$error":"#DIV/0!"}},{"$f":"D13*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/8-32-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q20","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C14,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10\" Results'!C14),'10A61 10\" Results'!C14))","v":{"$error":"#DIV/0!"}},{"$f":"D14*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Output"]
[null,null,"1/8-32-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q21","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C15,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10\" Results'!C15),'10A61 10\" Results'!C15))","v":{"$error":"#DIV/0!"}},{"$f":"D15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Range"]
[null,null,"1/8-32-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q22","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C16,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10\" Results'!C16),'10A61 10\" Results'!C16))","v":{"$error":"#DIV/0!"}},{"$f":"D16*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(I8,\"\")","v":""},{"$f":"IF(I16=\"\",\"\",P8)","v":""}]
[null,null,"1/8-32-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q23","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C17,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10\" Results'!C17),'10A61 10\" Results'!C17))","v":{"$error":"#DIV/0!"}},{"$f":"D17*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(I9,\"\")","v":""},{"$f":"IF(I17=\"\",\"\",P9)","v":""}]
[null,null,"1/8-32-G-10-TA",null,0,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C18,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10\" Results'!C18),'10A61 10\" Results'!C18))","v":{"$error":"#DIV/0!"}},{"$f":"D18*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IFERROR(IF(I17=\"\",\"\",I10),\"\")","v":""},{"$f":"IF(I18=\"\",\"\",P10)","v":""}]
[null,null,"1/4-10-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q26","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C19,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10\" Results'!C19),'10A61 10\" Results'!C19))","v":{"$error":"#DIV/0!"}},{"$f":"D19*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(OR(I17=\"\",I18=\"\"),\"\",I11),\"\")","v":""},{"$f":"IF(I19=\"\",\"\",P11)","v":""}]
[null,null,"1/4-10-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q27","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C20,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10\" Results'!C20),'10A61 10\" Results'!C20))","v":{"$error":"#DIV/0!"}},{"$f":"D20*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-10-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q28","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C21,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10\" Results'!C21),'10A61 10\" Results'!C21))","v":{"$error":"#DIV/0!"}},{"$f":"D21*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-10-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q29","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C22,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10\" Results'!C22),'10A61 10\" Results'!C22))","v":{"$error":"#DIV/0!"}},{"$f":"D22*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-10-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q30","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C23,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10\" Results'!C23),'10A61 10\" Results'!C23))","v":{"$error":"#DIV/0!"}},{"$f":"D23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q32","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10\" Results'!C24),'10A61 10\" Results'!C24))","v":{"$error":"#DIV/0!"}},{"$f":"D24*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q33","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10\" Results'!C25),'10A61 10\" Results'!C25))","v":{"$error":"#DIV/0!"}},{"$f":"D25*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q34","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10\" Results'!C26),'10A61 10\" Results'!C26))","v":{"$error":"#DIV/0!"}},{"$f":"D26*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q35","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10\" Results'!C27),'10A61 10\" Results'!C27))","v":{"$error":"#DIV/0!"}},{"$f":"D27*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q36","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10\" Results'!C28),'10A61 10\" Results'!C28))","v":{"$error":"#DIV/0!"}},{"$f":"D28*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10\" Results'!C29),'10A61 10\" Results'!C29))","v":{"$error":"#DIV/0!"}},{"$f":"D29*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10\" Results'!C30),'10A61 10\" Results'!C30))","v":{"$error":"#DIV/0!"}},{"$f":"D30*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10\" Results'!C31),'10A61 10\" Results'!C31))","v":{"$error":"#DIV/0!"}},{"$f":"D31*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10\" Results'!C32),'10A61 10\" Results'!C32))","v":{"$error":"#DIV/0!"}},{"$f":"D32*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10\" Results'!C33),'10A61 10\" Results'!C33))","v":{"$error":"#DIV/0!"}},{"$f":"D33*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-BG",{"$f":"'10A61 10\"+6\" Calcs'!T38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10\" Results'!C34),'10A61 10\" Results'!C34))","v":{"$error":"#DIV/0!"}},{"$f":"D34*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-SA",{"$f":"'10A61 10\"+6\" Calcs'!T39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10\" Results'!C35),'10A61 10\" Results'!C35))","v":{"$error":"#DIV/0!"}},{"$f":"D35*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-SS",{"$f":"'10A61 10\"+6\" Calcs'!T40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10\" Results'!C36),'10A61 10\" Results'!C36))","v":{"$error":"#DIV/0!"}},{"$f":"D36*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-CA",{"$f":"'10A61 10\"+6\" Calcs'!T41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10\" Results'!C37),'10A61 10\" Results'!C37))","v":{"$error":"#DIV/0!"}},{"$f":"D37*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-TA",{"$f":"'10A61 10\"+6\" Calcs'!T42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10\" Results'!C38),'10A61 10\" Results'!C38))","v":{"$error":"#DIV/0!"}},{"$f":"D38*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]

{"sheet":"10A4 Capacity Tables","index":17,"n_rows":187,"n_cols":17,"rows_kept":187,"cut":false,"hidden":true,"merged":[[173,2,173,8],[2,2,2,8],[23,2,23,8],[85,2,85,8],[140,2,140,8],[159,2,159,8]]}
[]
[]
[null,null,"Low Pressure Drop"]
[null,null,"Water GPM","Air SCFM","Tube","Float (SST)","VIC","psia Critical","Pressure Drop (in. H2O)","Max Flow Specified Units (Liquid)","Max Rounded (Liquid)"]
[null,null,0.19800000000000001,0.8,"FP-1/2-17-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,0.53,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D5/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J5<0.99999,ROUND(J5,2),\nIF(J5<9.999,ROUND(J5,2),\nIF(J5<99.99,ROUND(J5,1),\nIF(J5<999.99,ROUND(J5,0),\nIF(J5<9999.99,ROUND(J5,-1),\nIF(J5<99999,ROUND(J5,-2),ROUND(J5,2)))))))","v":0}]
[null,null,0.23799999999999999,0.98199999999999998,"FP-1/2-21-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,0.53,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D6/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J6<0.99999,ROUND(J6,2),\nIF(J6<9.999,ROUND(J6,2),\nIF(J6<99.99,ROUND(J6,1),\nIF(J6<999.99,ROUND(J6,0),\nIF(J6<9999.99,ROUND(J6,-1),\nIF(J6<99999,ROUND(J6,-2),ROUND(J6,2)))))))","v":0}]
[null,null,0.32400000000000001,1.339,"FP-1/2-27-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,0.57999999999999996,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D7/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.436,1.796,"FP-1/2-35-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,1,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D8/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.82499999999999996,3.4,"FP-1/2-50-G-9","1/2-GUSVT-410",2.2000000000000002,3.6,2,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D9/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.63300000000000001,2.62,"FP-3/4-21-G-10","3/4-GUSVT-510",3.3,3.1,0.6,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D10/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.86,3.54,"FP-3/4-27-G-10","3/4-GUSVT-510",3.3,1.5,0.71,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D11/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.2050000000000001,4.9800000000000004,"FP-1-27-G-10","1-GUSVT-611",4,1,1.28,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D12/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.67,6.9,"FP-1-35-G-10","1-GUSVT-611",4,0.75,1.83,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D13/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.58,10.7,"FP-1-27-G-10","1-GUSVT-610",8.6,4.5,5.47,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D14/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.6,14.84,"FP-1-35-G-10","1-GUSVT-610",8.6,3.4,7.97,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C15/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D15/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.4500000000000002,10.3,"FP-1-1/2-21-G-10","1-1/2-GUSVT-867",6.5,1,0.92,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C16/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D16/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.33,13.8,"FP-1-1/2-27-G-10","1-1/2-GUSVT-867",6.5,1,1.24,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C17/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D17/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6.5,27,"FP-1-1/2-21-G-10","1-1/2-GUSVGT-814",16.2,6.8,5.75,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C18/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D18/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,8.6999999999999993,36,"FP-1-1/2-27-G-10","1-1/2-GUSVGT-814",16.2,6.8,7.2,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C19/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D19/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.54,22.9,"FP-2-27-G-10","2-GUSVT-913",8.9,1,1.65,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C20/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D20/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,13.75,56.7,"FP-2-27-G-10","2-GUSVGT-914",22,6.2,9,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C21/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D21/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0,null,null,null,0,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C22/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D22/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[]
[null,null,"Standard Floats"]
[null,null,"Water GPM","Air SCFM","Tube","Float (SST)","VIC","psia Critical","Pressure Drop (in. H2O)","Max Flow Specified Units","Max Rounded"]
[null,null,0.26700000000000002,1.1000000000000001,"FP-1/2-17-G-10","1/2-GUSVT-40A",2.9,5.5,1.2,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C26/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D26/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J26<0.99999,ROUND(J26,2),\nIF(J26<9.999,ROUND(J26,2),\nIF(J26<99.99,ROUND(J26,1),\nIF(J26<999.99,ROUND(J26,0),\nIF(J26<9999.99,ROUND(J26,-1),\nIF(J26<99999,ROUND(J26,-2),ROUND(J26,2)))))))","v":0}]
[null,null,0.32800000000000001,1.35,"FP-1/2-21-G-10","1/2-GUSVT-40A",2.9,3.5,1.4,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C27/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D27/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J27<0.99999,ROUND(J27,2),\nIF(J27<9.999,ROUND(J27,2),\nIF(J27<99.99,ROUND(J27,1),\nIF(J27<999.99,ROUND(J27,0),\nIF(J27<9999.99,ROUND(J27,-1),\nIF(J27<99999,ROUND(J27,-2),ROUND(J27,2)))))))","v":0}]
[null,null,0.442,1.82,"FP-1/2-27-G-10","1/2-GUSVT-40A",2.9,2.7,2,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C28/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D28/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.48,1.92,"FP-1/2-17-G-10","1/2-GSVT-45A",5.0999999999999996,17.899999999999999,3.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C29/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D29/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.6,2.4700000000000002,"FP-1/2-21-G-10","1/2-GSVT-45A",5.0999999999999996,11.5,4.5999999999999996,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C30/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D30/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.61899999999999999,2.5499999999999998,"FP-1/2-35-G-10","1/2-GUSVT-40A",2.9,2,3.1,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C31/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D31/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.67,2.76,"FP-1/2-17-G-10","1/2-GSVT-44A",7.1,33.4,6.4,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C32/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D32/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.69,2.85,"FP-1/2-17-G-10","1/2-GSVT-48A",7.6,39,7.3,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C33/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D33/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.81,3.35,"FP-1/2-27-G-10","1/2-GSVT-45A",4.0999999999999996,8.4,6.8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C34/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D34/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.83,3.42,"FP-1/2-21-G-10","1/2-GSVT-44A",7.1,33.799999999999997,7.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C35/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D35/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.88,3.62,"FP-1/2-21-G-10","1/2-GSVT-48A",7.6,24.6,8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C36/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D36/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.88500000000000001,3.65,"FP-1/2-17-G-10","1/2-GNSVT-48A",1.1000000000000001,19.8,8.1999999999999993,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C37/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D37/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.1000000000000001,4.5199999999999996,"FP-1/2-21-G-10","1/2-GNSVT-48A",1.1000000000000001,20,9.9,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C38/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D38/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.1200000000000001,4.5999999999999996,"FP-1/2-27-G-10","1/2-GSVT-44A",7.1,16.2,12.3,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C39/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D39/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.1499999999999999,4.74,"FP-1/2-35-G-10","1/2-GSVT-45A",5.0999999999999996,8.5,8.1999999999999993,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C40/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D40/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.19,4.9000000000000004,"FP-1/2-27-G-10","1/2-GSVT-48A",7.6,18.600000000000001,13.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C41/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D41/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.44,5.93,"FP-1/2-27-G-10","1/2-GNSVT-48A",1.1000000000000001,16.5,15.8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C42/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D42/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.56,6.43,"FP-1/2-35-G-10","1/2-GSVT-44A",7.1,16.5,14.8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C43/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D43/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.66,6.85,"FP-1/2-35-G-10","1/2-GSVT-48A",7.6,18.8,17.2,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C44/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D44/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2,8.24,"FP-1/2-50-G-9","1/2-GSVT-45A",5.0999999999999996,4,12,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C45/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D45/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.76,11.4,"FP-1/2-50-G-9","1/2-GSVT-44A",7.1,7.7,31,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C46/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D46/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.9,12,"FP-1/2-50-G-9","1/2-GSVT-48A",7.6,8.9,35.200000000000003,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C47/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D47/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.52,14.5,"FP-1/2-50-G-9","1/2-GNSVT-48A",1.1000000000000001,8.8000000000000007,52,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C48/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D48/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.96,8.1,"FP-3/4-21-G-10","3/4-GSVGT-54A",10.4,13.9,5.3,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C49/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D49/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.4900000000000002,10.199999999999999,"FP-3/4-21-G-10","3/4-GNSVGT-54A",1.6,13.9,6.8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C50/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D50/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.66,11,"FP-3/4-21-G-10","3/4-GSVGT-59A",14.1,28.7,7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C51/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D51/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.7,11.1,"FP-3/4-27-G-10","3/4-GSVGT-54A",10.4,9.6,7.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C52/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D52/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.37,13.9,"FP-3/4-21-G-10","3/4-GNSVGT-59A",2.1,25.3,11.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C53/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D53/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.55,14.6,"FP-3/4-27-G-10","3/4-GNSVGT-54A",1.6,9.6,11.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C54/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D54/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.67,15.1,"FP-3/4-27-G-10","3/4-GSVGT-59A",14,19.8,13.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C55/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D55/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.8,19.8,"FP-3/4-27-G-10","3/4-GNSVGT-59A",2.1,19.8,20.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C56/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D56/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.25,17.5,"FP-1-27-G-10","1-GSVGT-64A",14.8,11.5,12.9,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C57/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D57/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.82,19.899999999999999,"FP-1-27-G-10","1-GSVGT-68A",16.899999999999999,15.6,18.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C58/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D58/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.63,23.2,"FP-1-27-G-10","1-GNSVGT-64A",2.2000000000000002,11.3,20.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C59/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D59/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D59/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D59/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6,24.7,"FP-1-35-G-10","1-GSVGT-64A",14.8,6.8,24.6,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C60/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D60/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D60/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D60/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6.46,26.6,"FP-1-27-G-10","1-GNSVGT-68A",2.5,15.6,32.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C61/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D61/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D61/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D61/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6.8,28,"FP-1-35-G-10","1-GSVGT-68A",16.899999999999999,8.9,37,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C62/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D62/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D62/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D62/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,7.62,31.4,"FP-1-27-G-10","1-GNSVGT-69A",1.5,22.2,75,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C63/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D63/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D63/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D63/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,7.84,32.4,"FP-1-35-G-10","1-GNSVGT-64A",2.2000000000000002,6.8,37.700000000000003,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C64/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D64/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D64/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D64/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,9,37,"FP-1-35-G-10","1-GNSVGT-68A",2.5,8.9,62.8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C65/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D65/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D65/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D65/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,9.5,39.200000000000003,"FP-1-35-G-10","1-GSVGT-69A",8.5,13.4,65.3,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C66/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D66/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D66/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D66/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,11,45.3,"FP-1-35-G-10","1-GNSVGT-69A",1.5,13.4,112,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C67/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D67/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D67/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D67/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,13.2,54.4,"FP-1-1/2-27-G-10","1-1/2-GSVGT-87A",27.6,15.4,9.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C68/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D68/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D68/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D68/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,14.6,60,"FP-1-1/2-27-G-10","1-1/2-GSVGT-86A",31,22,13.5,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C69/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D69/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D69/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D69/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,17.600000000000001,72,"FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A",4.2,15.4,12.8,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C70/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D70/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D70/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D70/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,18.600000000000001,76.5,"FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A",4.8,22,15.2,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C71/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D71/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D71/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D71/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,24,99,"FP-2-27-G-10","2-GSVGT-97A",26.5,16.399999999999999,24,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C72/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D72/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D72/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D72/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,30,123.8,"FP-2-27-G-10","2-GSVGT-98A",18.5,21.2,34,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C73/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D73/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D73/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D73/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,32,132,"FP-2-27-G-10","2-GNSVGT-97A",3,16.399999999999999,32,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C74/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D74/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D74/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D74/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,36.1,149,"FP-2-27-G-10","2-GNSVGT-98A",3.3,21.2,45,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C75/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D75/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D75/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D75/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,48,null,"FP-2-27-G-10","BL-954",2,null,70,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C76/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",0,\"\"))","v":""},{"$f":"IFERROR(IF(J76<0.99999,ROUND(J76,2),\nIF(J76<9.999,ROUND(J76,2),\nIF(J76<99.99,ROUND(J76,1),\nIF(J76<999.99,ROUND(J76,0),\nIF(J76<9999.99,ROUND(J76,-1),\nIF(J76<99999,ROUND(J76,-2),ROUND(J76,2))))))),\"\")","v":""}]
[null,null,60,null,"FP-2-27-G-10","BL-953",2,null,95,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C77/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",0,\"\"))","v":""},{"$f":"IFERROR(IF(J77<0.99999,ROUND(J77,2),\nIF(J77<9.999,ROUND(J77,2),\nIF(J77<99.99,ROUND(J77,1),\nIF(J77<999.99,ROUND(J77,0),\nIF(J77<9999.99,ROUND(J77,-1),\nIF(J77<99999,ROUND(J77,-2),ROUND(J77,2))))))),\"\")","v":""}]
[null,null,68,null,"FP-2-27-G-10","BL-950",2,null,110,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C78/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",0,\"\"))","v":""},""]
[null,null,90,null,"FP-2-27-G-10","BL-951",1,null,192.7,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C79/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",0,\"\"))","v":""},""]
[null,null,0,null,null,null,0,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C80/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\"\",\"\"))","v":""},""]
[]
[]
[]
[]
[]
[null,null,"Alarm Floats"]
[null,null,"Water GPM","Air SCFM","Tube","Float (SST)","VIC","psia Critical","Pressure Drop (in. H2O)","Max Flow Specified Units (Liquid)","Max Rounded (Liquid)"]
[null,null,0.67,2.76,"FP-1/2-17-G-10","1/2-GSVTA-44",7.1,33.4,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C88/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D88/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D88/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D88/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J88<0.99999,ROUND(J88,2),\nIF(J88<9.999,ROUND(J88,2),\nIF(J88<99.99,ROUND(J88,1),\nIF(J88<999.99,ROUND(J88,0),\nIF(J88<9999.99,ROUND(J88,-1),\nIF(J88<99999,ROUND(J88,-2),ROUND(J88,2)))))))","v":0}]
[null,null,0.69,2.85,"FP-1/2-17-G-10","1/2-GSVTA-48",7.6,39,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C89/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D89/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D89/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D89/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J89<0.99999,ROUND(J89,2),\nIF(J89<9.999,ROUND(J89,2),\nIF(J89<99.99,ROUND(J89,1),\nIF(J89<999.99,ROUND(J89,0),\nIF(J89<9999.99,ROUND(J89,-1),\nIF(J89<99999,ROUND(J89,-2),ROUND(J89,2)))))))","v":0}]
[null,null,0.83,3.42,"FP-1/2-21-G-10","1/2-GSVTA-44",7.1,33.799999999999997,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C90/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D90/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D90/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D90/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.88,3.62,"FP-1/2-21-G-10","1/2-GSVTA-48",7.6,24.6,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C91/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D91/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D91/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D91/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0.88500000000000001,3.65,"FP-1/2-17-G-10","1/2-GNSVTA-48",1.1000000000000001,19.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C92/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D92/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D92/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D92/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.03,4.24,"FP-1/2-21-G-10","1/2-GNSVTA-44",1.1000000000000001,33.4,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C93/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D93/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D93/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D93/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.1000000000000001,4.5199999999999996,"FP-1/2-21-G-10","1/2-GNSVTA-48",1.1000000000000001,20,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C94/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D94/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D94/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D94/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.1200000000000001,4.5999999999999996,"FP-1/2-27-G-10","1/2-GSVTA-44",7.1,16.2,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C95/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D95/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D95/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D95/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.19,4.9000000000000004,"FP-1/2-27-G-10","1/2-GSVTA-48",7.6,18.600000000000001,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C96/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D96/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D96/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D96/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.44,5.93,"FP-1/2-27-G-10","1/2-GNSVTA-48",1.1000000000000001,16.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C97/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D97/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D97/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D97/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.56,6.43,"FP-1/2-35-G-10","1/2-GSVTA-44",7.1,16.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C98/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D98/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D98/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D98/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.66,6.85,"FP-1/2-35-G-10","1/2-GSVTA-48",7.3,18.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C99/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D99/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D99/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D99/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.84,7.6,"FP-1/2-27-G-10","1/2-GNSVTA-43",1.3,27.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C100/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D100/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D100/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D100/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2,8.24,"FP-1/2-35-G-10","1/2-GNSVTA-48",1.1000000000000001,8.8000000000000007,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C101/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D101/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D101/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D101/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.4300000000000002,10,"FP-1/2-35-G-10","1/2-GNSVTA-43",1.3,22.7,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C102/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D102/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D102/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D102/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.76,11.4,"FP-1/2-50-G-9","1/2-GSVTA-44",7,7.7,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C103/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D103/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D103/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D103/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.9,12,"FP-1/2-50-G-9","1/2-GSVTA-48",7.6,8.9,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C104/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D104/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D104/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D104/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.52,14.5,"FP-1/2-50-G-9","1/2-GNSVTA-48",1.1000000000000001,8.8000000000000007,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C105/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D105/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D105/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D105/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4,16,"FP-1/2-50-G-9","1/2-GNSVTA-43",1.3,12.3,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C106/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D106/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D106/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D106/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.96,8.1,"FP-3/4-21-G-10","3/4-GSVTA-54",10.4,13.9,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C107/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D107/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D107/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D107/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.4900000000000002,10.199999999999999,"FP-3/4-21-G-10","3/4-GNSVTA-54",1.6,13.9,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C108/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D108/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D108/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D108/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.7,11.1,"FP-3/4-27-G-10","3/4-GSVTA-54",10.4,9.6,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C109/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D109/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D109/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D109/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.15,13,"FP-3/4-21-G-10","3/4-GSVTA-53",16.600000000000001,36,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C110/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D110/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D110/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D110/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.55,14.6,"FP-3/4-27-G-10","3/4-GNSVTA-54",1.6,9.6,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C111/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D111/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D111/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D111/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.85,15.8,"FP-3/4-27-G-10","3/4-GSVTA-56",14.9,19.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C112/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D112/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D112/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D112/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.3499999999999996,18,"FP-3/4-27-G-10","3/4-GSVTA-53",16.8,25,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C113/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D113/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D113/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D113/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.05,20.8,"FP-3/4-27-G-10","3/4-GNSVTA-56",2.2000000000000002,19.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C114/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D114/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D114/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D114/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.7,23.6,"FP-3/4-27-G-10","3/4-GNSVTA-53",2.5,25,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C115/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D115/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D115/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D115/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.25,17.5,"FP-1-27-G-10","1-GSVTA-64",14.8,11.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C116/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D116/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D116/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D116/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.82,19.8,"FP-1-27-G-10","1-GSVTA-65",16.899999999999999,14.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C117/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D117/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D117/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D117/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.63,23.2,"FP-1-27-G-10","1-GNSVTA-64",2.2000000000000002,11.3,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C118/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D118/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D118/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D118/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6,24.7,"FP-1-35-G-10","1-GSVTA-64",14.8,6.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C119/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D119/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D119/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D119/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6.75,27.9,"FP-1-35-G-10","1-GSVTA-65",16.899999999999999,8.9,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C120/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D120/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D120/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D120/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,7.84,32.4,"FP-1-35-G-10","1-GNSVTA-64",2.2000000000000002,6.8,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C121/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D121/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D121/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D121/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,8.4600000000000009,35.1,"FP-1-35-G-10","1-GSVTA-63",20.8,13.9,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C122/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D122/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D122/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D122/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,9,36.9,"FP-1-35-G-10","1-GNSVTA-65",2.5,8.9,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C123/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D123/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D123/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D123/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,9.9,10.6,"FP-1-35-G-10","1-GSVTA-66",8.5,13.4,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C124/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D124/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D124/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D124/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C125/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D125/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D125/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D125/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0,10.8,44.5,"FP-1-35-G-10","1-GNSVTA-66",1.5,14.5]
[null,null,11.1,45.7,"FP-1-35-G-10","1-GNSVTA-63",2.9,13.1,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C126/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D126/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D126/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D126/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,13.4,55,"FP-1-1/2-27-G-10","1-1/2-GSVTA-84",27.6,15.4,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C127/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D127/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D127/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D127/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,15.4,63.5,"FP-1-1/2-27-G-10","1-1/2-GSVTA-85",32,20.3,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C128/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D128/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D128/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D128/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,16,66,"FP-1-1/2-27-G-10","1-1/2-GSVTA-83",33,22,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C129/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D129/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D129/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D129/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,17.600000000000001,72,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-84",4.2,15.4,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C130/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D130/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D130/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D130/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,20.399999999999999,84,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-85",5,20.3,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C131/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D131/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D131/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D131/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,21.2,87,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-83",4.9000000000000004,22,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C132/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D132/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D132/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D132/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,23.9,99,"FP-2-27-G-10","2-GSVTA-94",40.5,16.399999999999999,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C133/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D133/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D133/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D133/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,27.9,115.2,"FP-2-27-G-10","2-GSVTA-93",49,24,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C134/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D134/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D134/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D134/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,31.5,129.80000000000001,"FP-2-27-G-10","2-GNSVTA-94",6.1,17.399999999999999,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C135/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D135/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D135/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D135/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,36.9,152.1,"FP-2-27-G-10","2-GNSVTA-96",7.6,21.2,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C136/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D136/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D136/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D136/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,38.200000000000003,156.6,"FP-2-27-G-10","2-GNSVTA-93",7.3,24,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C137/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D137/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D137/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D137/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,0,null,null,null,0,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C138/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D138/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D138/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D138/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[]
[]
[null,null,"Tantalum Floats"]
[null,null,"Water GPM","Air SCFM","Tube","Float (TA)","VIC","psia Critical","Pressure Drop (in. H2O)","Max Flow Specified Units (Liquid)","Max Rounded (Liquid)"]
[null,null,0.8,null,"FP-1/2-17-G-10","BS-41",8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C143/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D143/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D143/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D143/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J143<0.99999,ROUND(J143,2),\nIF(J143<9.999,ROUND(J143,2),\nIF(J143<99.99,ROUND(J143,1),\nIF(J143<999.99,ROUND(J143,0),\nIF(J143<9999.99,ROUND(J143,-1),\nIF(J143<99999,ROUND(J143,-2),ROUND(J143,2)))))))","v":0}]
[null,null,1,null,"FP-1/2-21-G-10","BS-41",8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C144/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D144/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D144/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D144/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J144<0.99999,ROUND(J144,2),\nIF(J144<9.999,ROUND(J144,2),\nIF(J144<99.99,ROUND(J144,1),\nIF(J144<999.99,ROUND(J144,0),\nIF(J144<9999.99,ROUND(J144,-1),\nIF(J144<99999,ROUND(J144,-2),ROUND(J144,2)))))))","v":0}]
[null,null,1.3,null,"FP-1/2-27-G-10","BS-41",8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C145/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D145/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D145/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D145/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.9,null,"FP-1/2-35-G-10","BS-41",6,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C146/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D146/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D146/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D146/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,3.32,null,"FP-1/2-50-G-9","BS-41",5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C147/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D147/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D147/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D147/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.9000001,null,"FP-3/4-21-G-10","BS-50",10,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C148/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D148/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D148/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D148/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.5,null,"FP-3/4-27-G-10","BS-50",10,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C149/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D149/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D149/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D149/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.4000000000000004,null,"FP-1-27-G-10","BS-62",16,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C150/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D150/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D150/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D150/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.8,null,"FP-1-27-G-10","BS-60",20,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C151/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D151/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D151/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D151/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,6.3,null,"FP-1-35-G-10","BS-62",16,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C152/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D152/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D152/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D152/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,8.1,null,"FP-1-35-G-10","BS-60",20,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C153/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D153/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D153/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D153/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,8.3000000000000007,null,"FP-1-1/2-21-G-10","BS-80",24,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C154/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D154/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D154/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D154/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,11,null,"FP-1-1/2-27-G-10","BS-80",24,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C155/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D155/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D155/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D155/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,14.4,null,"FP-2-27-G-10","BS-90",26,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C156/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D156/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D156/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D156/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,20.7,null,"FP-2-27-G-10","BS-91",37,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C157/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D157/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D157/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D157/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[]
[]
[null,null,"PTFE Floats"]
[null,null,"Water GPM","Air SCFM","Tube","Float (PTFE or PVC)","VIC","Float Density",null,"Max Flow Specified Units (Liquid)","Max Rounded (Liquid)"]
[null,null,0.55000000000000004,null,"FP-1/2-17-G-10","1/2-GL-471",1.8,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C162/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D162/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D162/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D162/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J162<0.99999,ROUND(J162,2),\nIF(J162<9.999,ROUND(J162,2),\nIF(J162<99.99,ROUND(J162,1),\nIF(J162<999.99,ROUND(J162,0),\nIF(J162<9999.99,ROUND(J162,-1),\nIF(J162<99999,ROUND(J162,-2),ROUND(J162,2)))))))","v":0}]
[null,null,0.66,null,"FP-1/2-21-G-10","1/2-GL-471",1.8,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C163/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D163/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D163/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D163/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J163<0.99999,ROUND(J163,2),\nIF(J163<9.999,ROUND(J163,2),\nIF(J163<99.99,ROUND(J163,1),\nIF(J163<999.99,ROUND(J163,0),\nIF(J163<9999.99,ROUND(J163,-1),\nIF(J163<99999,ROUND(J163,-2),ROUND(J163,2)))))))","v":0}]
[null,null,0.96,null,"FP-1/2-27-G-10","1/2-GL-471",1.8,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C164/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D164/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D164/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D164/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.42,null,"FP-1/2-35-G-10","1/2-GL-471",1.8,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C165/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D165/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D165/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D165/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.13,null,"FP-1/2-50-G-9","1/2-GL-471",1.8,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C166/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D166/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D166/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D166/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,1.95,null,"FP-3/4-21-G-10","3/4-GL-571",2.2000000000000002,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C167/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D167/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D167/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D167/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.55,null,"FP-1-27-G-10","1-GL-671",3,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C168/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D168/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D168/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D168/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,9.3800000000000008,null,"FP-1-1/2-21-G-10","1-1/2-GL-871",3.98,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C169/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D169/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D169/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D169/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,13.3,null,"FP-1-1/2-27-G-10","1-1/2-GL-871",3.98,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C170/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D170/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D170/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D170/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,21.8,null,"FP-2-27-G-10","2-GL-971",5.95,2.31,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C171/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D171/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D171/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D171/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[]
[]
[null,null,"PVC Floats"]
[null,null,"Water GPM","Air SCFM","Tube","Float (PTFE or PVC)","VIC","Float Density",null,"Max Flow Specified Units (Liquid)","Max Rounded (Liquid)"]
[null,null,1.02,null,"FP-1/2-17-G-10","1/2-GL-410",2.4500000000000002,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C176/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D176/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D176/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D176/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J176<0.99999,ROUND(J176,2),\nIF(J176<9.999,ROUND(J176,2),\nIF(J176<99.99,ROUND(J176,1),\nIF(J176<999.99,ROUND(J176,0),\nIF(J176<9999.99,ROUND(J176,-1),\nIF(J176<99999,ROUND(J176,-2),ROUND(J176,2)))))))","v":0}]
[null,null,1.33,null,"FP-1/2-21-G-10","1/2-GL-410",2.4500000000000002,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C177/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D177/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D177/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D177/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},{"$f":"IF(J177<0.99999,ROUND(J177,2),\nIF(J177<9.999,ROUND(J177,2),\nIF(J177<99.99,ROUND(J177,1),\nIF(J177<999.99,ROUND(J177,0),\nIF(J177<9999.99,ROUND(J177,-1),\nIF(J177<99999,ROUND(J177,-2),ROUND(J177,2)))))))","v":0}]
[null,null,1.92,null,"FP-1/2-27-G-10","1/2-GL-410",2.4500000000000002,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C178/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D178/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D178/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D178/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,2.85,null,"FP-1/2-35-G-10","1/2-GL-410",2.4500000000000002,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C179/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D179/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D179/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D179/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.9000000000000004,null,"FP-1/2-50-G-9","1/2-GL-410",2.4500000000000002,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C180/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D180/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D180/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D180/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,4.2,null,"FP-3/4-21-G-10","3/4-GL-510",2.97,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C181/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D181/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D181/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D181/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,5.87,null,"FP-3/4-27-G-10","3/4-GL-510",2.97,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C182/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D182/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D182/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D182/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,9.7200000000000006,null,"FP-1-27-G-10","1-GL-610",3.89,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C183/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D183/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D183/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D183/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,14.7,null,"FP-1-35-G-10","1-GL-610",3.89,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C184/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D184/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D184/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D184/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,23.5,null,"FP-1-1/2-21-G-10","1-1/2-GL-810",6.4,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C185/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D185/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D185/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D185/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,32.6,null,"FP-1-1/2-27-G-10","1-1/2-GL-810",6.4,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C186/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D186/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D186/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D186/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]
[null,null,56.7,null,"FP-2-27-G-10","2-GL-910",9.6999999999999993,5.5,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",(C187/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$3=\"Gas\",\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D187/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D187/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(D187/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":false},0]

{"sheet":"10A22 Curves","index":18,"n_rows":219,"n_cols":19,"rows_kept":219,"cut":false,"hidden":true,"merged":[]}
[]
[null,"Curve"]
[null,0.36,"cP",null,1,1.5,2.5,4,5,7,10,15,20,{"$f":"LINEST(E4:M4,LN(E3:M3))","v":-9.0671110845037595E-2},0.36776172436962118]
[null,null,"GPM",null,0.36,0.34,0.28999999999999998,0.24,0.22,0.189,0.155,0.122,0.1]
[]
[]
[null,null,null,null,null,{"$f":"LINEST(E4:M4,E3:M3^{1;2;3;4;5})","v":-4.8935978962246658E-7},3.1087875660266861E-5,-7.8300899064807721E-4,1.0164237050588385E-2,-7.7014021139189634E-2,0.43056391860657994]
[]
[]
[]
[]
[]
[]
[]
[]
[null,0.6,"cP",null,1,3,5,7,9,15,20,30,40,50]
[null,null,"GPM",null,0.6,0.46,0.38,0.32,0.28000000000000003,0.21,0.18,0.14000000000000001,0.11600000000000001,0.1]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,{"$f":"LINEST(E17:K17,LN(E16:K16))","v":-0.14441675283103528},0.60616394630257053]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(K17:N17,LN(K16:N16))","v":-8.7750902136795053E-2},0.44108059900735908]
[]
[]
[]
[]
[null,1,"cP",1,2.5,4,6,9,15,20,25,30,35,40,100]
[null,null,"GPM",1,0.85,0.75,0.64,0.52,0.39,0.32,0.28000000000000003,0.25,0.22500000000000001,0.20499999999999999,0.108]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"LINEST(D35:N35,D34:N34^{1;2;3;4})","v":1.2449379445687849E-6},-1.3358016289070139E-4,5.3317414011228009E-3,-0.10109881951109238,1.0833868585031605,null,null,null,null,null,{"$f":"LINEST(LN(G35:O35),LN(G34:O34))","v":-0.63206397221236332},0.73975499972041581]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(O44)","v":2.0954220726065942}]
[null,null,null,null,null,null,{"$f":"D44*(cP^4)+E44*(cP^3)+F44*(cP^2)+G44*cP+H44","v":1.0833868585031605}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"O45*('Modified Inputs'!G2^'10A22 Curves'!N44)","v":{"$error":"#DIV/0!"}}]
[]
[]
[null,1.3,"cP",1,2,4,10,15,20,30,40,60,80,100,150]
[null,null,"GPM",1.3,1.137,1.012,0.66600000000000004,0.52170000000000005,0.43859999999999999,0.3332,0.27410000000000001,0.20469999999999999,0.16400000000000001,0.1381,0.1012]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"LINEST(D51:K51,D50:K50^{1;2;3;4})","v":1.3862185674054601E-6},-1.4863551939310016E-4,6.0131989613041283E-3,-0.119316111537143,1.3898249385070673,{"$f":"B61*(cP^4)+C61*(cP^3)+D61*(cP^2)+E61*cP+F61","v":1.3898249385070673}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(LN(K51:O51),LN(K50:O50))","v":-0.75589142622189587},1.5010637859420248,null,{"$f":"M63*('Modified Inputs'!G2^L62)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(M62)","v":4.486459164897548}]
[]
[null,2,"cP",1,2,5,9,15,20,25,30,38,45,50,90,200,275]
[null,null,"GPM",2,1.8,1.4,1.1000000000000001,0.82820000000000005,0.7,0.6,0.53410000000000002,0.45629999999999998,0.40760000000000002,0.38,0.24,0.13,0.1]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"LINEST(D66:N66,D65:N65^{1;2;3;4;5;6})","v":1.8895227177836788E-9},-3.3416149445220684E-7,2.366837328719152E-5,-8.6808359499241858E-4,1.8106061666299477E-2,-0.23213895429661285,2.2073198215122067,{"$f":"A77*(cP^6)+B77*(cP^5)+C77*(cP^4)+D77*(cP^3)+E77*(cP^2)+F77*cP+G77","v":2.2073198215122067},null,null,null,{"$f":"LINEST(LN(N66:Q66),LN(N65:Q65))","v":-0.77986635160652007},2.0837272934488085,null,{"$f":"M78*('Modified Inputs'!G2^'10A22 Curves'!L77)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(M77)","v":8.0343595898962565}]
[null,3,"cP",1,1.5,4,6,10,25,80,100,200,300,500]
[null,null,"GPM",3,2.9,2.4,2.1,1.7,1,0.44,0.38,0.22,0.16,0.106]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,{"$f":"LINEST(D80:H80,D79:H79^{1;2})","v":9.153597982111867E-3},-0.24558740774114859,3.2409241174905947,{"$f":"E92*(cP^2)+F92*cP+G92","v":3.2409241174905947},null,null,null,null,{"$f":"LINEST(LN(H80:N80),LN(H79:N79))","v":-0.71333851708873763},2.2545662283474845,null,{"$f":"N93*(cP^M92)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(N92)","v":9.531158067150832}]
[null,4,"cP",1,2.5,7,10,20,25,50,60,70,80,150,300,500,900]
[null,null,"GPM",4,3.6,2.8,2.4,1.7,1.5,0.94,0.85,0.77500000000000002,0.7,0.43,0.255,0.17,0.1]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"LINEST(D95:M95,D94:M94^{1;2;3;4;5})","v":-1.1662574208023447E-8},2.8045155089456245E-6,-2.578645512705751E-4,1.1553472935940168E-2,-0.27652745483678148,4.2465286709495524]
[null,null,null,null,null,{"$f":"D105*(cP^5)+E105*(cP^4)+F105*(cP^3)+G105*(cP^2)+H105*cP+I105","v":4.2465286709495524},null,null,null,null,null,null,null,{"$f":"LINEST(LN(M95:Q95),LN(M94:Q94))","v":-0.79644178964518642},3.1498091139973878,null,{"$f":"O107*(cP^N106)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(O106)","v":23.331610477984636}]
[]
[null,6,"cP",1,3,8,15,20,40,60,80,85,90,100,200,250,400,600,1000]
[null,null,"GPM",6,5.8,5.2,4.7,4.4000000000000004,3.6,3.05,2.65,2.5209999999999999,2.44,2.2999999999999998,1.4,1.2,0.8,0.56000000000000005,0.34200000000000003]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(LN(N110:S110),LN(N109:S109))","v":-0.82911604637703373},4.7106026312417768,null,{"$f":"O120*(cP^N119)","v":{"$error":"#DIV/0!"}}]
[null,null,null,{"$f":"LINEST(D110:N110,D109:N109^{1;2;3})","v":-5.4010574216279727E-6},1.1775223397536849E-3,-0.10176751933305865,6.0402307220420814,null,null,null,null,null,null,null,{"$f":"EXP(O119)","v":111.11910357587273}]
[null,null,null,null,{"$f":"D120*(cP^3)+E120*(cP^2)+F120*cP+G120","v":6.0402307220420814}]
[]
[]
[]
[null,8,"cP",1,5,8,15,30,50,70,150,200,300,600,700,800,900,1000]
[null,null,"GPM",8,7.5,7,6.4,5.4,4.5,3.8,2.4,1.95,1.44,0.8,0.7,0.62,0.56000000000000005,0.52]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(J126:R126,J125:R125^{1;2;3;4;5;6})","v":9.2336874412014188E-17},-3.4903490482679924E-13,5.3212169909993303E-10,-4.1956347587664849E-7,1.8318237265365739E-4,-4.4682665623323646E-2,6.1606278882276015,null,{"$f":"K137*(cP^6)+L137*(cP^5)+M137*(cP^4)+N137*(cP^3)+O137*(cP^2)+P137*cP+Q137","v":6.1606278882276015}]
[null,null,null,{"$f":"LINEST(D126:J126,D125:J125^{1;2;3})","v":-1.331440924137923E-5},2.0947463199077871E-3,-0.14319065648641396,8.1184216091186983]
[null,null,null,null,{"$f":"D138*(cP^3)+E138*(cP^2)+F138*cP+G138","v":8.1184216091186983}]
[]
[]
[null,11,"cP",1,9,30,50,60,90,125,150,250,700,1000]
[null,null,"GPM",11,9.5,7.5,6.5,6,4.9000000000000004,4.1390000000000002,3.6,2.5,1.1000000000000001,0.8]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"LINEST(D143:K143,D142:K142^{1;2;3;4;5})","v":-1.0223995330044516E-9},4.2538731197692557E-7,-6.6268115420712765E-5,4.9792978303622136E-3,-0.2246358453835377,11.200648188033762,null,{"$f":"B155*(cP^5)+C155*(cP^4)+D155*(cP^3)+E155*(cP^2)+F155*cP+G155","v":11.200648188033762},null,null,{"$f":"LINEST(LN(K143:N143),LN(K142:N142))","v":-0.79259774057458965},5.271137391345075,null,{"$f":"M156*(cP^L155)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(M155)","v":194.63721528010012}]
[null,15,"cP",1,4,15,40,60,100,250,400,1000]
[null,null,"GPM",15,14,12,9.5,8.3000000000000007,6.5,3.6,2.5,1.1499999999999999]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(LN(I158:L158),LN(I157:L157))","v":-0.75316007549716768},5.3877350803483637,null,{"$f":"N169*(cP^M168)","v":{"$error":"#DIV/0!"}}]
[null,null,{"$f":"LINEST(D158:I158,D157:I157^{1;2;3;4})","v":3.0627593360716876E-7},-7.2020729629589038E-5,6.2245447985198625E-3,-0.29560463055801073,15.208550566244075,null,{"$f":"C169*(cP^4)+D169*(cP^3)+E169*(cP^2)+F169*cP+G169","v":15.208550566244075},null,null,null,null,{"$f":"EXP(N168)","v":218.70746931552358}]
[]
[]
[null,20,"cP",1,6,15,20,50,80,150,200,250,275,300,700,1000]
[null,null,"GPM",20,18,16,15,12,10,7,5.8,4.9000000000000004,4.5579999999999998,4.4000000000000004,2.2000000000000002,1.6]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,{"$f":"LINEST(D173:N173,D172:N172^{1;2;3;4})","v":8.5690676627480391E-9},-6.3111353445729796E-6,1.7033492613217566E-3,-0.22409333521128733,19.453630832316449,null,{"$f":"D183*(cP^4)+E183*(cP^3)+F183*(cP^2)+G183*cP+H183","v":19.453630832316449},null,null,{"$f":"LINEST(LN(N173:P173),LN(N172:P172))","v":-0.83620617178589374},6.2546550146219673,null,{"$f":"N184*(cP^M183)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(N183)","v":520.42980311204826}]
[]
[null,24,"cP",1,5,10,30,50,80,100,120,200,300,600,1000]
[null,null,"GPM",24,23,21,16.600000000000001,14,12.61,12,10.37,6.899,4.9109999999999996,2.899,2.2010000000000001]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"LINEST(D187:K187,D186:K186^{1;2;3})","v":-1.7776797331672905E-5},4.3270104877662034E-3,-0.38101040761425586,24.531259079376575,null,null,null,null,{"$f":"LINEST(LN(K187:O187),LN(K186:O186))","v":-0.74149052301425566},5.8576358095072809,null,{"$f":"L199*(cP^K198)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,{"$f":"C198*(cP^3)+D198*(cP^2)+E198*cP+F198","v":24.531259079376575},null,null,null,null,{"$f":"EXP(L198)","v":349.89594472926018}]
[]
[]
[null,35,"cP",1,1.2,1.4,1.6,1.8,1.9]
[null,null,"GPM",35,34.17,33.5,32.93,32.43,32.21]
[]
[]
[null,null,null,null,null,null,{"$f":"LINEST(LN(D203:I203),LN(D202:I202))","v":-0.12932837484315235},3.5551489207219635]
[null,null,null,null,null,null,null,{"$f":"EXP(H206)","v":34.993030767091469},null,{"$f":"H207*(cP^G206)","v":{"$error":"#DIV/0!"}}]
[]
[]
[]
[]
[]
[]
[null,50,"cP",1,1.2,1.4,1.6,1.8,1.9]
[null,null,"GPM",50,48.9,48,47.24,46.58,46.27]
[]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"LINEST(LN(D215:I215),LN(D214:I214))","v":-0.1205310291323429},3.9118830139269543]
[null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(K218)","v":49.993000914858058},null,{"$f":"K219*(cP^J218)","v":{"$error":"#DIV/0!"}}]

{"sheet":"Sheet1","index":19,"n_rows":1472,"n_cols":8,"rows_kept":1472,"cut":false,"hidden":true,"merged":[]}
[null,"Trivelli, Peter,  N."]
[]
["Database","Number","vlookup","Count Database","Count Name","Count Company","Name","Company"]
["Trivelli, Peter,  N.",1,{"$f":"IFERROR(VLOOKUP($B$1,$A$4:$B$500,2,FALSE),2)","v":1},{"$f":"\"$\"&\"A\"&\"$\"&4+COUNTA(A4:A500)","v":"$A$5"},{"$f":"\"$\"&\"G\"&\"$\"&4+COUNTA(A4:A500)","v":"$G$5"},{"$f":"\"$\"&\"H\"&\"$\"&4+COUNTA(A4:A500)","v":"$H$5"}]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]
[null,1]

{"sheet":"10A61 5","index":20,"n_rows":71,"n_cols":15,"rows_kept":71,"cut":false,"hidden":true,"merged":[[10,7,10,8]]}
[]
[null,"Tube/Float","Max Flow (mL/min)","Min Flow (mL/min)","Tube/Float","Max Flowrate Specified Units","Max Rounded"]
[null,"1/4-25-CD",{"$f":"'10A61 5\" Calcs'!AD46","v":""},{"$f":"C3/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B3,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y46<30),CONCATENATE(\" \",'10A61 5'!B3),'10A61 5'!B3))","v":{"$error":"#DIV/0!"}},{"$f":"C3*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F3<0.99999,ROUND(F3,2),\nIF(F3<9.999,ROUND(F3,2),\nIF(F3<99.99,ROUND(F3,1),\nIF(F3<999.99,ROUND(F3,0),\nIF(F3<9999.99,ROUND(F3,-1),\nIF(F3<99999,ROUND(F3,-2),ROUND(F3,2)))))))","v":{"$error":"#VALUE!"}}]
[null,"1/4-25-SA",{"$f":"'10A61 5\" Calcs'!AD47","v":""},{"$f":"C4/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B4,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y47<30),CONCATENATE(\" \",'10A61 5'!B4),'10A61 5'!B4))","v":{"$error":"#DIV/0!"}},{"$f":"C4*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F4<0.99999,ROUND(F4,2),\nIF(F4<9.999,ROUND(F4,2),\nIF(F4<99.99,ROUND(F4,1),\nIF(F4<999.99,ROUND(F4,0),\nIF(F4<9999.99,ROUND(F4,-1),\nIF(F4<99999,ROUND(F4,-2),ROUND(F4,2)))))))","v":{"$error":"#VALUE!"}},"Tube/Float","Max Flow Raw (mL/min)","Min Flow Raw (mL/min)","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,"1/4-25-SS",{"$f":"'10A61 5\" Calcs'!AD48","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B5,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y48<30),CONCATENATE(\" \",'10A61 5'!B5),'10A61 5'!B5))","v":{"$error":"#DIV/0!"}},{"$f":"C5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I5,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($C$3:$C$71<'Modified Inputs'!$O$2,C3:C71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I5,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(K5<0.99999,ROUND(K5,2),\nIF(K5<9.999,ROUND(K5,2),\nIF(K5<99.99,ROUND(K5,1),\nIF(K5<999.99,ROUND(K5,0),\nIF(K5<9999.99,ROUND(K5,-1),\nIF(K5<99999,ROUND(K5,-2),ROUND(K5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(L5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N5,\" \",\"-\",\" \",M5)","v":{"$error":"#N/A"}}]
[null,"1/4-25-CA",{"$f":"'10A61 5\" Calcs'!AD49","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B6,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y49<30),CONCATENATE(\" \",'10A61 5'!B6),'10A61 5'!B6))","v":{"$error":"#DIV/0!"}},{"$f":"C6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I6,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$3:$C$71>'Modified Inputs'!$O$2,$C$3:$C$71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I6,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(K6<0.99999,ROUND(K6,2),\nIF(K6<9.999,ROUND(K6,2),\nIF(K6<99.99,ROUND(K6,1),\nIF(K6<999.99,ROUND(K6,0),\nIF(K6<9999.99,ROUND(K6,-1),\nIF(K6<99999,ROUND(K6,-2),ROUND(K6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(L6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(N6,\" \",\"-\",\" \",M6)","v":{"$error":"#N/A"}}]
[null,"1/4-25-TA",{"$f":"'10A61 5\" Calcs'!AD50","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B7,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y50<30),CONCATENATE(\" \",'10A61 5'!B7),'10A61 5'!B7))","v":{"$error":"#DIV/0!"}},{"$f":"C7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I7,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$3:$C$71>I6,$C$3:$C$71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I7,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(N7,\" \",\"-\",\" \",M7)","v":{"$error":"#N/A"}}]
[null,"1/4-25-BG",{"$f":"'10A61 5\" Calcs'!AD51","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B8,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y51<30),CONCATENATE(\" \",'10A61 5'!B8),'10A61 5'!B8))","v":{"$error":"#DIV/0!"}},{"$f":"C8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(I8,$C$3:$E$71,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($C$3:$C$71>I7,$C$3:$C$71))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(I8,$C$3:$E$71,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(N8,\" \",\"-\",\" \",M8)","v":{"$error":"#N/A"}}]
[null,"1/4-20-CD",{"$f":"'10A61 5\" Calcs'!AD53","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B9,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y53<30),CONCATENATE(\" \",'10A61 5'!B9),'10A61 5'!B9))","v":{"$error":"#DIV/0!"}},{"$f":"C9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-20-SA",{"$f":"'10A61 5\" Calcs'!AD54","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B10,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y54<30),CONCATENATE(\" \",'10A61 5'!B10),'10A61 5'!B10))","v":{"$error":"#DIV/0!"}},{"$f":"C10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-20-SS",{"$f":"'10A61 5\" Calcs'!AD55","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B11,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y55<30),CONCATENATE(\" \",'10A61 5'!B11),'10A61 5'!B11))","v":{"$error":"#DIV/0!"}},{"$f":"C11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Output"]
[null,"1/4-20-CA",{"$f":"'10A61 5\" Calcs'!AD56","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B12,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y56<30),CONCATENATE(\" \",'10A61 5'!B12),'10A61 5'!B12))","v":{"$error":"#DIV/0!"}},{"$f":"C12*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Range"]
[null,"1/4-20-TA",{"$f":"'10A61 5\" Calcs'!AD57","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B13,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y57<30),CONCATENATE(\" \",'10A61 5'!B13),'10A61 5'!B13))","v":{"$error":"#DIV/0!"}},{"$f":"C13*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(H5,\"\")","v":""},{"$f":"IF(H13=\"\",\"\",O5)","v":""},null,{"$f":"M5","v":{"$error":"#N/A"}},{"$f":"K5","v":{"$error":"#N/A"}}]
[null,"1/4-20-BG",{"$f":"'10A61 5\" Calcs'!AD58","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B14,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y58<30),CONCATENATE(\" \",'10A61 5'!B14),'10A61 5'!B14))","v":{"$error":"#DIV/0!"}},{"$f":"C14*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(H6,\"\")","v":""},{"$f":"IF(H14=\"\",\"\",O6)","v":""},null,{"$f":"M6","v":{"$error":"#N/A"}},{"$f":"K6","v":{"$error":"#N/A"}}]
[null,"1/4-16-CD",{"$f":"'10A61 5\" Calcs'!AD60","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B15,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y60<30),CONCATENATE(\" \",'10A61 5'!B15),'10A61 5'!B15))","v":{"$error":"#DIV/0!"}},{"$f":"C15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(H14=\"\",\"\",H7),\"\")","v":""},{"$f":"IF(H15=\"\",\"\",O7)","v":""},null,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"1/4-16-SA",{"$f":"'10A61 5\" Calcs'!AD61","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B16,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y61<30),CONCATENATE(\" \",'10A61 5'!B16),'10A61 5'!B16))","v":{"$error":"#DIV/0!"}},{"$f":"C16*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(OR(H14=\"\",H15=\"\"),\"\",H8),\"\")","v":""},{"$f":"IF(H16=\"\",\"\",O8)","v":""},null,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,"1/4-16-SS",{"$f":"'10A61 5\" Calcs'!AD62","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B17,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y62<30),CONCATENATE(\" \",'10A61 5'!B17),'10A61 5'!B17))","v":{"$error":"#DIV/0!"}},{"$f":"C17*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-16-CA",{"$f":"'10A61 5\" Calcs'!AD63","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B18,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y63<30),CONCATENATE(\" \",'10A61 5'!B18),'10A61 5'!B18))","v":{"$error":"#DIV/0!"}},{"$f":"C18*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-16-TA",{"$f":"'10A61 5\" Calcs'!AD64","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B19,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y64<30),CONCATENATE(\" \",'10A61 5'!B19),'10A61 5'!B19))","v":{"$error":"#DIV/0!"}},{"$f":"C19*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-16-BG",{"$f":"'10A61 5\" Calcs'!AD65","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B20,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y65<30),CONCATENATE(\" \",'10A61 5'!B20),'10A61 5'!B20))","v":{"$error":"#DIV/0!"}},{"$f":"C20*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-10-CD",{"$f":"'10A61 5\" Calcs'!AD67","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B21,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y67<30),CONCATENATE(\" \",'10A61 5'!B21),'10A61 5'!B21))","v":{"$error":"#DIV/0!"}},{"$f":"C21*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-10-SA",{"$f":"'10A61 5\" Calcs'!AD68","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B22,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y68<30),CONCATENATE(\" \",'10A61 5'!B22),'10A61 5'!B22))","v":{"$error":"#DIV/0!"}},{"$f":"C22*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-10-SS",{"$f":"'10A61 5\" Calcs'!AD69","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B23,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y69<30),CONCATENATE(\" \",'10A61 5'!B23),'10A61 5'!B23))","v":{"$error":"#DIV/0!"}},{"$f":"C23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-10-CA",{"$f":"'10A61 5\" Calcs'!AD70","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y70<30),CONCATENATE(\" \",'10A61 5'!B24),'10A61 5'!B24))","v":{"$error":"#DIV/0!"}},{"$f":"C24*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-10-TA",{"$f":"'10A61 5\" Calcs'!AD71","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y71<30),CONCATENATE(\" \",'10A61 5'!B25),'10A61 5'!B25))","v":{"$error":"#DIV/0!"}},{"$f":"C25*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-10-BG",{"$f":"'10A61 5\" Calcs'!AD72","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y72<30),CONCATENATE(\" \",'10A61 5'!B26),'10A61 5'!B26))","v":{"$error":"#DIV/0!"}},{"$f":"C26*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-12-SA",{"$f":"'10A61 5\" Calcs'!AD75","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y75<30),CONCATENATE(\" \",'10A61 5'!B27),'10A61 5'!B27))","v":{"$error":"#DIV/0!"}},{"$f":"C27*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-12-SS",{"$f":"'10A61 5\" Calcs'!AD76","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y76<30),CONCATENATE(\" \",'10A61 5'!B28),'10A61 5'!B28))","v":{"$error":"#DIV/0!"}},{"$f":"C28*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-12-CA",{"$f":"'10A61 5\" Calcs'!AD77","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y77<30),CONCATENATE(\" \",'10A61 5'!B29),'10A61 5'!B29))","v":{"$error":"#DIV/0!"}},{"$f":"C29*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-12-TA",{"$f":"'10A61 5\" Calcs'!AD78","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y78<30),CONCATENATE(\" \",'10A61 5'!B30),'10A61 5'!B30))","v":{"$error":"#DIV/0!"}},{"$f":"C30*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-12-BG",{"$f":"'10A61 5\" Calcs'!AD79","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y79<30),CONCATENATE(\" \",'10A61 5'!B31),'10A61 5'!B31))","v":{"$error":"#DIV/0!"}},{"$f":"C31*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-08-SA",{"$f":"'10A61 5\" Calcs'!AD82","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y82<30),CONCATENATE(\" \",'10A61 5'!B32),'10A61 5'!B32))","v":{"$error":"#DIV/0!"}},{"$f":"C32*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-08-SS",{"$f":"'10A61 5\" Calcs'!AD83","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y83<30),CONCATENATE(\" \",'10A61 5'!B33),'10A61 5'!B33))","v":{"$error":"#DIV/0!"}},{"$f":"C33*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-08-CA",{"$f":"'10A61 5\" Calcs'!AD84","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y84<30),CONCATENATE(\" \",'10A61 5'!B34),'10A61 5'!B34))","v":{"$error":"#DIV/0!"}},{"$f":"C34*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-08-TA",{"$f":"'10A61 5\" Calcs'!AD85","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y85<30),CONCATENATE(\" \",'10A61 5'!B35),'10A61 5'!B35))","v":{"$error":"#DIV/0!"}},{"$f":"C35*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-08-BG",{"$f":"'10A61 5\" Calcs'!AD86","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y86<30),CONCATENATE(\" \",'10A61 5'!B36),'10A61 5'!B36))","v":{"$error":"#DIV/0!"}},{"$f":"C36*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-12-SA",{"$f":"'10A61 5\" Calcs'!AD89","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y89<30),CONCATENATE(\" \",'10A61 5'!B37),'10A61 5'!B37))","v":{"$error":"#DIV/0!"}},{"$f":"C37*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-12-SS",{"$f":"'10A61 5\" Calcs'!AD90","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y90<30),CONCATENATE(\" \",'10A61 5'!B38),'10A61 5'!B38))","v":{"$error":"#DIV/0!"}},{"$f":"C38*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-12-CA",{"$f":"'10A61 5\" Calcs'!AD91","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y91<30),CONCATENATE(\" \",'10A61 5'!B39),'10A61 5'!B39))","v":{"$error":"#DIV/0!"}},{"$f":"C39*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-12-TA",{"$f":"'10A61 5\" Calcs'!AD92","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y92<30),CONCATENATE(\" \",'10A61 5'!B40),'10A61 5'!B40))","v":{"$error":"#DIV/0!"}},{"$f":"C40*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-12-BG",{"$f":"'10A61 5\" Calcs'!AD93","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y93<30),CONCATENATE(\" \",'10A61 5'!B41),'10A61 5'!B41))","v":{"$error":"#DIV/0!"}},{"$f":"C41*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-16-SA",{"$f":"'10A61 5\" Calcs'!AD96","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y96<30),CONCATENATE(\" \",'10A61 5'!B42),'10A61 5'!B42))","v":{"$error":"#DIV/0!"}},{"$f":"C42*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-16-SS",{"$f":"'10A61 5\" Calcs'!AD97","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y97<30),CONCATENATE(\" \",'10A61 5'!B43),'10A61 5'!B43))","v":{"$error":"#DIV/0!"}},{"$f":"C43*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-16-CA",{"$f":"'10A61 5\" Calcs'!AD98","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y98<30),CONCATENATE(\" \",'10A61 5'!B44),'10A61 5'!B44))","v":{"$error":"#DIV/0!"}},{"$f":"C44*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-16-TA",{"$f":"'10A61 5\" Calcs'!AD99","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y99<30),CONCATENATE(\" \",'10A61 5'!B45),'10A61 5'!B45))","v":{"$error":"#DIV/0!"}},{"$f":"C45*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-16-BG",{"$f":"'10A61 5\" Calcs'!AD100","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y100<30),CONCATENATE(\" \",'10A61 5'!B46),'10A61 5'!B46))","v":{"$error":"#DIV/0!"}},{"$f":"C46*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-20-SA",{"$f":"'10A61 5\" Calcs'!AD103","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y103<30),CONCATENATE(\" \",'10A61 5'!B47),'10A61 5'!B47))","v":{"$error":"#DIV/0!"}},{"$f":"C47*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-20-SS",{"$f":"'10A61 5\" Calcs'!AD104","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y104<30),CONCATENATE(\" \",'10A61 5'!B48),'10A61 5'!B48))","v":{"$error":"#DIV/0!"}},{"$f":"C48*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-20-CA",{"$f":"'10A61 5\" Calcs'!AD105","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y105<30),CONCATENATE(\" \",'10A61 5'!B49),'10A61 5'!B49))","v":{"$error":"#DIV/0!"}},{"$f":"C49*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-20-TA",{"$f":"'10A61 5\" Calcs'!AD106","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y106<30),CONCATENATE(\" \",'10A61 5'!B50),'10A61 5'!B50))","v":{"$error":"#DIV/0!"}},{"$f":"C50*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/16-20-BG",{"$f":"'10A61 5\" Calcs'!AD107","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B51,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!Y107<30),CONCATENATE(\" \",'10A61 5'!B51),'10A61 5'!B51))","v":{"$error":"#DIV/0!"}},{"$f":"C51*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-25-SA",{"$f":"'10A61 5\" Calcs'!AP47","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B52,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK47<30),CONCATENATE(\" \",'10A61 5'!B52),'10A61 5'!B52))","v":{"$error":"#DIV/0!"}},{"$f":"C52*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-25-SS",{"$f":"'10A61 5\" Calcs'!AP48","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B53,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK48<30),CONCATENATE(\" \",'10A61 5'!B53),'10A61 5'!B53))","v":{"$error":"#DIV/0!"}},{"$f":"C53*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-25-CA",{"$f":"'10A61 5\" Calcs'!AP49","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B54,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK49<30),CONCATENATE(\" \",'10A61 5'!B54),'10A61 5'!B54))","v":{"$error":"#DIV/0!"}},{"$f":"C54*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-25-TA",{"$f":"'10A61 5\" Calcs'!AP50","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B55,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK50<30),CONCATENATE(\" \",'10A61 5'!B55),'10A61 5'!B55))","v":{"$error":"#DIV/0!"}},{"$f":"C55*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-25-BG",{"$f":"'10A61 5\" Calcs'!AP51","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B56,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK51<30),CONCATENATE(\" \",'10A61 5'!B56),'10A61 5'!B56))","v":{"$error":"#DIV/0!"}},{"$f":"C56*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-SA",{"$f":"'10A61 5\" Calcs'!AP54","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B57,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK54<30),CONCATENATE(\" \",'10A61 5'!B57),'10A61 5'!B57))","v":{"$error":"#DIV/0!"}},{"$f":"C57*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-SS",{"$f":"'10A61 5\" Calcs'!AP55","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B58,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK55<30),CONCATENATE(\" \",'10A61 5'!B58),'10A61 5'!B58))","v":{"$error":"#DIV/0!"}},{"$f":"C58*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-CA",{"$f":"'10A61 5\" Calcs'!AP56","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B59,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK56<30),CONCATENATE(\" \",'10A61 5'!B59),'10A61 5'!B59))","v":{"$error":"#DIV/0!"}},{"$f":"C59*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-TA",{"$f":"'10A61 5\" Calcs'!AP57","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B60,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK57<30),CONCATENATE(\" \",'10A61 5'!B60),'10A61 5'!B60))","v":{"$error":"#DIV/0!"}},{"$f":"C60*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-20-BG",{"$f":"'10A61 5\" Calcs'!AP58","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B61,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK58<30),CONCATENATE(\" \",'10A61 5'!B61),'10A61 5'!B61))","v":{"$error":"#DIV/0!"}},{"$f":"C61*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-16-SA",{"$f":"'10A61 5\" Calcs'!AP61","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B62,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK61<30),CONCATENATE(\" \",'10A61 5'!B62),'10A61 5'!B62))","v":{"$error":"#DIV/0!"}},{"$f":"C62*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-16-SS",{"$f":"'10A61 5\" Calcs'!AP62","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B63,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK62<30),CONCATENATE(\" \",'10A61 5'!B63),'10A61 5'!B63))","v":{"$error":"#DIV/0!"}},{"$f":"C63*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-16-CA",{"$f":"'10A61 5\" Calcs'!AP63","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B64,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK63<30),CONCATENATE(\" \",'10A61 5'!B64),'10A61 5'!B64))","v":{"$error":"#DIV/0!"}},{"$f":"C64*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-16-TA",{"$f":"'10A61 5\" Calcs'!AP64","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B65,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK64<30),CONCATENATE(\" \",'10A61 5'!B65),'10A61 5'!B65))","v":{"$error":"#DIV/0!"}},{"$f":"C65*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/8-16-BG",{"$f":"'10A61 5\" Calcs'!AP65","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B66,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AK65<30),CONCATENATE(\" \",'10A61 5'!B66),'10A61 5'!B66))","v":{"$error":"#DIV/0!"}},{"$f":"C66*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-40-G-6-BG",{"$f":"'10A61 10\"+6\" Calcs'!T38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B67,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5'!B67),'10A61 5'!B67))","v":{"$error":"#DIV/0!"}},{"$f":"C67*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-40-G-6-SA",{"$f":"'10A61 10\"+6\" Calcs'!T39","v":""},{"$f":"C68/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B68,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5'!B68),'10A61 5'!B68))","v":{"$error":"#DIV/0!"}},{"$f":"C68*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(F68<0.99999,ROUND(F68,2),\nIF(F68<9.999,ROUND(F68,2),\nIF(F68<99.99,ROUND(F68,1),\nIF(F68<999.99,ROUND(F68,0),\nIF(F68<9999.99,ROUND(F68,-1),\nIF(F68<99999,ROUND(F68,-2),ROUND(F68,2)))))))","v":{"$error":"#VALUE!"}}]
[null,"1/4-40-G-6-SS",{"$f":"'10A61 10\"+6\" Calcs'!T40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B69,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5'!B69),'10A61 5'!B69))","v":{"$error":"#DIV/0!"}},{"$f":"C69*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-40-G-6-CA",{"$f":"'10A61 10\"+6\" Calcs'!T41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B70,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5'!B70),'10A61 5'!B70))","v":{"$error":"#DIV/0!"}},{"$f":"C70*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,"1/4-40-G-6-TA",{"$f":"'10A61 10\"+6\" Calcs'!T42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5'!B71,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!$L$8>60),CONCATENATE(\" \",'10A61 5'!B71),'10A61 5'!B71))","v":{"$error":"#DIV/0!"}},{"$f":"C71*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]

{"sheet":"10A61 10","index":21,"n_rows":38,"n_cols":16,"rows_kept":38,"cut":false,"hidden":true,"merged":[[13,8,13,9]]}
[]
[]
[null,null,"Tube/Float","Max Flow (mL/min)","Min Flow","Tube/Float","Max Flow Specified Units","Max Round"]
[null,null,"1/8-077-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q8","v":""},{"$f":"D4/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C4,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>10),CONCATENATE(\" \",'10A61 10'!C4),'10A61 10'!C4))","v":{"$error":"#DIV/0!"}},{"$f":"D4*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(G4<0.99999,ROUND(G4,2),\nIF(G4<9.999,ROUND(G4,2),\nIF(G4<99.99,ROUND(G4,1),\nIF(G4<999.99,ROUND(G4,0),\nIF(G4<9999.99,ROUND(G4,-1),\nIF(G4<99999,ROUND(G4,-2),ROUND(G4,2)))))))","v":{"$error":"#VALUE!"}}]
[null,null,"1/8-077-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q9","v":""},{"$f":"D5/10","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C5,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>10),CONCATENATE(\" \",'10A61 10'!C5),'10A61 10'!C5))","v":{"$error":"#DIV/0!"}},{"$f":"D5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(G5<0.99999,ROUND(G5,2),\nIF(G5<9.999,ROUND(G5,2),\nIF(G5<99.99,ROUND(G5,1),\nIF(G5<999.99,ROUND(G5,0),\nIF(G5<9999.99,ROUND(G5,-1),\nIF(G5<99999,ROUND(G5,-2),ROUND(G5,2)))))))","v":{"$error":"#VALUE!"}}]
[null,null,"1/8-077-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q10","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C6,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>10),CONCATENATE(\" \",'10A61 10'!C6),'10A61 10'!C6))","v":{"$error":"#DIV/0!"}},{"$f":"D6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/8-077-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q11","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C7,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>10),CONCATENATE(\" \",'10A61 10'!C7),'10A61 10'!C7))","v":{"$error":"#DIV/0!"}},{"$f":"D7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Max Flow Raw (mL/min)","Min Flow Raw (mL/min)","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,null,"1/8-077-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q12","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C8,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>10),CONCATENATE(\" \",'10A61 10'!C8),'10A61 10'!C8))","v":{"$error":"#DIV/0!"}},{"$f":"D8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J8,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($D$9:$D$33<'Modified Inputs'!$O$2,D9:D33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J8,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(L8<0.99999,ROUND(L8,2),\nIF(L8<9.999,ROUND(L8,2),\nIF(L8<99.99,ROUND(L8,1),\nIF(L8<999.99,ROUND(L8,0),\nIF(L8<9999.99,ROUND(L8,-1),\nIF(L8<99999,ROUND(L8,-2),ROUND(L8,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(M8,2)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(O8,\" \",\"-\",\" \",N8)","v":{"$error":"#N/A"}}]
[null,null,"1/8-13.3-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q14","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C9,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10'!C9),'10A61 10'!C9))","v":{"$error":"#DIV/0!"}},{"$f":"D9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J9,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($D$9:$D$33>'Modified Inputs'!$O$2,$D$9:$D$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J9,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(L9<0.99999,ROUND(L9,2),\nIF(L9<9.999,ROUND(L9,2),\nIF(L9<99.99,ROUND(L9,1),\nIF(L9<999.99,ROUND(L9,0),\nIF(L9<9999.99,ROUND(L9,-1),\nIF(L9<99999,ROUND(L9,-2),ROUND(L9,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(M9,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(O9,\" \",\"-\",\" \",N9)","v":{"$error":"#N/A"}}]
[null,null,"1/8-13.3-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q15","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C10,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10'!C10),'10A61 10'!C10))","v":{"$error":"#DIV/0!"}},{"$f":"D10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J10,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($D$9:$D$33>J9,$D$9:$D$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J10,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"ROUND(M10,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(O10,\" \",\"-\",\" \",N10)","v":{"$error":"#N/A"}}]
[null,null,"1/8-13.3-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q16","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C11,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10'!C11),'10A61 10'!C11))","v":{"$error":"#DIV/0!"}},{"$f":"D11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"VLOOKUP(J11,$D$9:$F$33,3,FALSE)","v":{"$error":"#N/A"}},{"$f":"MIN(IF($D$9:$D$33>J10,$D$9:$D$33))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(J11,$D$9:$E$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"J11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"K11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,"1/8-13.3-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q17","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C12,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10'!C12),'10A61 10'!C12))","v":{"$error":"#DIV/0!"}},{"$f":"D12*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/8-13.3-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q18","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C13,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10'!C13),'10A61 10'!C13))","v":{"$error":"#DIV/0!"}},{"$f":"D13*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/8-32-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q20","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C14,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10'!C14),'10A61 10'!C14))","v":{"$error":"#DIV/0!"}},{"$f":"D14*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Output"]
[null,null,"1/8-32-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q21","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C15,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10'!C15),'10A61 10'!C15))","v":{"$error":"#DIV/0!"}},{"$f":"D15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"Tube/Float","Range"]
[null,null,"1/8-32-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q22","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C16,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10'!C16),'10A61 10'!C16))","v":{"$error":"#DIV/0!"}},{"$f":"D16*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(I8,\"\")","v":""},{"$f":"IF(I16=\"\",\"\",P8)","v":""}]
[null,null,"1/8-32-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q23","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C17,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10'!C17),'10A61 10'!C17))","v":{"$error":"#DIV/0!"}},{"$f":"D17*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(I9,\"\")","v":""},{"$f":"IF(I17=\"\",\"\",P9)","v":""}]
[null,null,"1/8-32-G-10-TA",null,0,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C18,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10'!C18),'10A61 10'!C18))","v":{"$error":"#DIV/0!"}},{"$f":"D18*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IFERROR(IF(I17=\"\",\"\",I10),\"\")","v":""},{"$f":"IF(I18=\"\",\"\",P10)","v":""}]
[null,null,"1/4-10-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q26","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C19,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10'!C19),'10A61 10'!C19))","v":{"$error":"#DIV/0!"}},{"$f":"D19*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IFERROR(IF(OR(I17=\"\",I18=\"\"),\"\",I11),\"\")","v":""},{"$f":"IF(I19=\"\",\"\",P11)","v":""}]
[null,null,"1/4-10-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q27","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C20,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10'!C20),'10A61 10'!C20))","v":{"$error":"#DIV/0!"}},{"$f":"D20*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-10-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q28","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C21,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10'!C21),'10A61 10'!C21))","v":{"$error":"#DIV/0!"}},{"$f":"D21*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-10-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q29","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C22,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10'!C22),'10A61 10'!C22))","v":{"$error":"#DIV/0!"}},{"$f":"D22*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-10-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q30","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C23,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10'!C23),'10A61 10'!C23))","v":{"$error":"#DIV/0!"}},{"$f":"D23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q32","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10'!C24),'10A61 10'!C24))","v":{"$error":"#DIV/0!"}},{"$f":"D24*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q33","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10'!C25),'10A61 10'!C25))","v":{"$error":"#DIV/0!"}},{"$f":"D25*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q34","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10'!C26),'10A61 10'!C26))","v":{"$error":"#DIV/0!"}},{"$f":"D26*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q35","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10'!C27),'10A61 10'!C27))","v":{"$error":"#DIV/0!"}},{"$f":"D27*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-19-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q36","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10'!C28),'10A61 10'!C28))","v":{"$error":"#DIV/0!"}},{"$f":"D28*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-BG",{"$f":"'10A61 10\"+6\" Calcs'!Q38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10'!C29),'10A61 10'!C29))","v":{"$error":"#DIV/0!"}},{"$f":"D29*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-SA",{"$f":"'10A61 10\"+6\" Calcs'!Q39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10'!C30),'10A61 10'!C30))","v":{"$error":"#DIV/0!"}},{"$f":"D30*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-SS",{"$f":"'10A61 10\"+6\" Calcs'!Q40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10'!C31),'10A61 10'!C31))","v":{"$error":"#DIV/0!"}},{"$f":"D31*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-CA",{"$f":"'10A61 10\"+6\" Calcs'!Q41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10'!C32),'10A61 10'!C32))","v":{"$error":"#DIV/0!"}},{"$f":"D32*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-10-TA",{"$f":"'10A61 10\"+6\" Calcs'!Q42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10'!C33),'10A61 10'!C33))","v":{"$error":"#DIV/0!"}},{"$f":"D33*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-BG",{"$f":"'10A61 10\"+6\" Calcs'!T38","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L8>60),CONCATENATE(\" \",'10A61 10'!C34),'10A61 10'!C34))","v":{"$error":"#DIV/0!"}},{"$f":"D34*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-SA",{"$f":"'10A61 10\"+6\" Calcs'!T39","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L9>60),CONCATENATE(\" \",'10A61 10'!C35),'10A61 10'!C35))","v":{"$error":"#DIV/0!"}},{"$f":"D35*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-SS",{"$f":"'10A61 10\"+6\" Calcs'!T40","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L10>60),CONCATENATE(\" \",'10A61 10'!C36),'10A61 10'!C36))","v":{"$error":"#DIV/0!"}},{"$f":"D36*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-CA",{"$f":"'10A61 10\"+6\" Calcs'!T41","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L11>60),CONCATENATE(\" \",'10A61 10'!C37),'10A61 10'!C37))","v":{"$error":"#DIV/0!"}},{"$f":"D37*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,"1/4-40-G-6-TA",{"$f":"'10A61 10\"+6\" Calcs'!T42","v":""},{"$error":"#VALUE!"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",C38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",'10A61 10\"+6\" Calcs'!L12>60),CONCATENATE(\" \",'10A61 10'!C38),'10A61 10'!C38))","v":{"$error":"#DIV/0!"}},{"$f":"D38*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]

{"sheet":"BasicFluid","index":22,"n_rows":79,"n_cols":37,"rows_kept":79,"cut":false,"hidden":true,"merged":[[2,10,2,36]]}
[]
[null,"Current Tab","Current Step",null,null,"Value","Units"]
[null,"Fluid",{"$f":"Step","v":1},null,"Fluid Type",null,null,null,"Description","Step","Dropdown Selections"]
[null,null,null,null,"Fluid Name",null,null,null,"Fluid Type",1,"Liquid","Gas",{"$f":"\"\"","v":""}]
[null,null,null,null,"Reference Condition",{"$f":"IF(OR(D5=\"\",G12=\"\"),\"\",\nIF(D5=\"Actual\",\"Actual\",\nIF(AND(D5=\"Reference\",OR(G12=\"m3/h\",G12=\"m3/min\")),\"Normal\",\nIF(D5=\"Reference\",\"Standard\",\"Error\"))))","v":""},null,null,"Fluid Name",2,{"$f":"IF($F$3=\"Liquid\",\"\",\nIF($F$3=\"Gas\",\"Air\",\"\"))","v":""},{"$f":"IF($F$3=\"Liquid\",\"Potable Water\",\nIF($F$3=\"Gas\",\"Argon (Ar)\",\"\"))","v":""},{"$f":"IF($F$3=\"Liquid\",\"Other Water\",\nIF($F$3=\"Gas\",\"Butane (C4H10)\",\"\"))","v":""},{"$f":"IF($F$3=\"Liquid\",\"Other Liquid\",\nIF($F$3=\"Gas\",\"Acetylene (C2H2)\",\"\"))","v":""},{"$f":"IF($F$3=\"Gas\",\"Ammonia (NH3)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Carbon Monoxide (CO)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Carbon Dioxide (CO2)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Chlorine (Cl2)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Ethane (C2H6)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Ethylene (C2H4)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Helium (He)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Hydrochloric Acid (HCl)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Hydrogen (H2)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Hydrogen Sulfide (H2S)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Krypton (Kr)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Methane (CH4)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Methyl Chloride (CH3Cl)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Natural Gas\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Neon (Ne)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Nitric Oxide (NO)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Nitrogen (N2)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Nitrous Oxide (N2O)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Oxygen (O2)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Propane (C3H8)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Propylene (C3H6)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Sulfur Dioxide (SO2)\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\" Other\",\"\")","v":""}]
[null,null,null,null,"Type of Density",null,null,null,"Ref Cond.",3,{"$f":"IF($F$3=\"Gas\",\"Actual\",\"\")","v":""},{"$f":"IF($F$3=\"Gas\",\"Reference\",\"\")","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,"Density at Reference Conditions",null,null,null,"Type Density",4,"at Reference/Base Conditions","at Operating Conditions",{"$f":"\"\"","v":""}]
[null,null,null,null,"Viscosity at Operating Conditions"]
[null,null,null,null,"Operating Pressure"]
[null,null,null,null,"Operating Temperature"]
[null,null,null,null,"Density at Operating Conditions"]
[null,null,null,null,"Maximum Flowrate"]
[]
[]
[null,null,null,null,"Consolidated Dropdown",null,"Flowrate Units",null,"Pressure Units visible","Pressure Units original","Temperature Units","Viscosity Units","Density Units"]
[null,null,null,null,{"$f":"IF($C$3=1,\"\",\nIF($C$3=2,$K$5,\nIF($C$3=3,\"\",\nIF($C$3=4,\"\",\"\"))))","v":""},null,null,null,"psi","psi(g)","°F","cP",{"$f":"IF($F$3=\"Liquid\",\"S.G.\",\"\")","v":""}]
[null,null,null,null,{"$f":"IF($C$3=1,\"\",\nIF($C$3=2,$L$5,\nIF($C$3=3,\"\",\nIF($C$3=4,\"\",\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"sccm\",\"cc/min\")","v":"cc/min"},"s","psi(a)","psi(a)","°C","cSt","kg/m3"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$M$5,\nIF($C$3=3,$M$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"mL/min","s","bar","bar(g)",null,null,"kg/L"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$N$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"mL/h","s","bar(a)","bar(a)",null,null,"g/mL"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$O$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"mL/s","s","atm","atm(g)",null,null,"g/cm3"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$P$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"l/h","s","atm(a)","atm(a)",null,null,"lb/ft3"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$Q$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"l/min","s","kpa","kpa(g)",null,null,"lb/USgal"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$R$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"l/s","s","kpa(a)","kpa(a)"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$S$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"m3/h","n","inH2O","inH2O(g)"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$T$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"m3/min","n","inH2O(a)","inH2O(a)"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$U$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"scfh\",\"ft3/h\")","v":"ft3/h"},"s","kg/cm2","kg/cm2(g)"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$V$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"scfm\",\"ft3/min\")","v":"ft3/min"},"s","kg/cm2(a)","kg/cm2(a)",null,"Units","Language"]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$W$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"scfs\",\"ft3/s\")","v":"ft3/s"},"s",null,null,null,"cc/min","\"Centimeters Cubed per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$X$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"US GPH","s","Input pressure","original pressure",null,"sccm","\"Standard Centimeters Cubed per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$Y$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,"US GPM","s",null,{"$f":"IFERROR(VLOOKUP(I30,I16:J27,2,FALSE),\"\")","v":""},null,"mL/min","\"Milliliters per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$Z$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"\",\"g/min\")","v":"g/min"},"g/min",null,null,null,"mL/h","\"Milliliters per Hour\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AA$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"\",\"g/h\")","v":"g/h"},"g/h",null,null,null,"mL/s","\"Milliliters per Second\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AB$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"\",\"kg/min\")","v":"kg/min"},null,null,null,null,"l/h","\"Liters per Hour\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AC$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"\",\"kg/h\")","v":"kg/h"},null,null,null,null,"l/min","\"Liters per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AD$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"\",\"lb/min\")","v":"lb/min"},null,null,null,null,"l/s","\"Liters per Second\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AE$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,{"$f":"IF(AND($F$3=\"Gas\",$D$5=\"Reference\"),\"\",\"lb/h\")","v":"lb/h"},null,null,null,null,"m3/h","\"Meters Cubed per Hour\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AF$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,null,null,null,null,null,"m3/min","\"Meters Cubed per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AG$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,null,null,null,null,null,"ft3/h","\"Feet Cubed per Hour\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AH$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,null,null,null,null,null,"scfh","\"Standard Feet Cubed per Hour\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AI$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,null,null,null,null,null,"ft3/min","\"Feet Cubed per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AJ$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,null,null,null,null,null,"scfm","\"Standard Feet Cubed per Minute\""]
[null,null,null,null,{"$f":"IF($C$3=1,$M$4,\nIF($C$3=2,$AK$5,\nIF($C$3=3,$N$6,\nIF($C$3=4,$M$7,\"\"))))","v":""},null,null,null,null,null,null,"ft3/s","\"Feet Cubed per Second\""]
[null,null,null,null,null,null,null,null,null,null,null,"scfs","\"Standard Feet Cubed per Second\""]
[null,null,null,null,null,null,null,null,null,null,null,"US GPH","\"Gallons per Hour\""]
[null,null,null,null,null,null,null,null,null,null,null,"US GPM","\"Gallons per Minute\""]
[null,null,null,null,null,null,null,null,null,null,null,"grams/min","\"Grams per Minute\""]
[null,null,null,null,null,null,null,null,null,null,null,"g/min","\"Grams per Minute\""]
[null,null,null,null,null,null,null,null,null,null,null,"grams/h","\"Grams per Hour\""]
[null,null,null,null,null,null,null,null,null,null,null,"g/h","\"Grams per Hour\""]
[null,null,null,null,null,null,null,null,null,null,null,"kg/min","\"Kilograms per Minute\""]
[null,null,null,null,null,null,null,null,null,null,null,"kg/h","\"Kilograms per Hour\""]
[null,null,null,null,null,null,null,null,null,null,null,"lb/min","\"Pounds per Minute\""]
[null,null,null,null,null,null,null,null,null,null,null,"lb/h","\"Pounds per Hour\""]
[null,null,null,null,null,null,null,null,null,null,null,"S.G.","\"Specific Gravity\""]
[null,null,null,null,null,null,null,null,null,null,null,"kg/m3","\"Kilograms per Meter Cubed\""]
[null,null,null,null,null,null,null,null,null,null,null,"kg/L","\"Kilograms per Liter\""]
[null,null,null,null,null,null,null,null,null,null,null,"g/mL","\"Grams per Milliliter\""]
[null,null,null,null,null,null,null,null,null,null,null,"g/cm3","\"Grams per Centimeter Cubed\""]
[null,null,null,null,null,null,null,null,null,null,null,"lb/ft3","\"Pounds per Foot Cubed\""]
[null,null,null,null,null,null,null,null,null,null,null,"lb/USgal","\"Pounds per Gallon\""]
[null,null,null,null,null,null,null,null,null,null,null,"°F","\"Degrees Fahrenheit\""]
[null,null,null,null,null,null,null,null,null,null,null,"°C","\"Degrees Celsius\""]
[null,null,null,null,null,null,null,null,null,null,null,"cP","\"Centipoise\""]
[null,null,null,null,null,null,null,null,null,null,null,"cSt","\"Centistokes\""]
[null,null,null,null,null,null,null,null,null,null,null,"psi","\"Pounds per Inches Squared (Gauge)\""]
[null,null,null,null,null,null,null,null,null,null,null,"psi(a)","\"Pounds per Inches Squared (Absolute)\""]
[null,null,null,null,null,null,null,null,null,null,null,"bar","\"bar (Gauge)\""]
[null,null,null,null,null,null,null,null,null,null,null,"bar(a)","\"bar (Absolute)\""]
[null,null,null,null,null,null,null,null,null,null,null,"atm","\"Atmospheres (Gauge)\""]
[null,null,null,null,null,null,null,null,null,null,null,"atm(a)","\"Atmospheres (Absolute)\""]
[null,null,null,null,null,null,null,null,null,null,null,"kpa","\"Kilopascals (Gauge)\""]
[null,null,null,null,null,null,null,null,null,null,null,"kpa(a)","\"Kilopascals (Absolute)\""]
[null,null,null,null,null,null,null,null,null,null,null,"inH2O","\"inches Water (Gauge)\""]
[null,null,null,null,null,null,null,null,null,null,null,"inH2O(a)","\"inches Water (Absolute)\""]
[null,null,null,null,null,null,null,null,null,null,null,"kg/cm2","\"Kilograms per Centimeter Squared (Gauge)\""]
[null,null,null,null,null,null,null,null,null,null,null,"kg/cm2(a)","\"Kilograms per Centimeter Squared (Absolute)\""]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,"Select Units",{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"\"\"","v":""}]

{"sheet":"Start","index":23,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":true,"merged":[[9,4,13,6],[16,4,20,6],[8,1,9,3]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Select your interface"]
[null,"VA Sizing Tool"]
[null,null,null,null,"Basic",null,null,null,"Simplified Interface"]
[null," Version 3.0",null,null,null,null,null,null,"Automatic Sizing Selection"]
[null,null,null,null,null,null,null,null,"Ideal for New Applications"]
[null,null,null,null,null,null,null,null,"Unavailable Meter Explanation"]
[null,null,null,null,null,null,null,null,"Model Code Generator"]
[]
[]
[null,null,null,null,"Advanced",null,null,null,"Flexible Input Fields"]
[null,null,null,null,null,null,null,null,"Detailed Sizing Record"]
[null,null,null,null,null,null,null,null,"Ideal for Non-Standard Applications"]
[null,null,null,null,null,null,null,null,"Float Height Visual Indication"]
[null,null,null,null,null,null,null,null,"Complete List of Sizing Options"]
[]
[]
[]
[null,null,null,null,"Note:    You may switch between these interfaces during sizing"]

{"sheet":"Basic","index":24,"n_rows":27,"n_cols":18,"rows_kept":27,"cut":false,"hidden":true,"merged":[[15,9,22,13],[14,2,15,4],[9,1,10,3],[11,14,11,15]]}
[]
[null,"STEP"]
[null,{"$f":"BasicStructure!$C$3","v":1}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(Step,BasicStructure!$E$6:$F$15,2,FALSE),\"\")","v":"Is the fluid a liquid or a gas?"}]
[]
[null,"VA Sizing Tool",null,null,null,null,null,null,null,null,{"$f":"BasicStructure!$H$17","v":"Liquid"},null,{"$f":"BasicStructure!$H$18","v":"Gas"}]
[]
[null," Version 3.0",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR($L$8=\"What is the operating temperature in the line?\",$L$8=\"What is the operating temperature in the line? (Optional)\"),\"Use Ambient Temperature\",\nIF(OR($L$8=\"What is the operating pressure in the line?\",$L$8=\"What is the operating pressure in the line? (Optional)\"),\"Use Ambient Pressure\",\"\"))","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"BasicStructure!$H$19","v":""},null,{"$f":"VLOOKUP($M$12,BasicFluid!$L$28:$M$79,2,FALSE)","v":""}]
[null,null,"Fluid Characteristics"]
[null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L8,BasicStructure!M18:N32,2,FALSE)","v":"Common liquids are Water and Oil\n\n\nCommon gases are Air, Nitrogen (N2), Oxygen (O2), Methane (CH4), and Carbon Dioxide (CO2)"}]
[null,null,"Fluid Type",{"$f":"IF(BasicFluid!F3=\"\",\"\",BasicFluid!F3)","v":""}]
[null,null,"Fluid Name",{"$f":"IF(BasicFluid!F4=\"\",\"\",BasicFluid!F4)","v":""}]
[null,null,{"$f":"IF(BasicFluid!F3=\"Liquid\",\"Viscosity\",\nIF(BasicFluid!F3=\"Gas\",\"Measuring Condition\",\"\"))","v":""},{"$f":"IF(BasicFluid!F4=\"Potable Water\",1,\nIF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!F8=\"\")),BasicFluid!F8,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!D5=\"\")),BasicFluid!D5,\"\")))","v":""},{"$f":"IF(BasicFluid!F4=\"Potable Water\",\"cP\",\nIF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!G8=\"\")),BasicFluid!G8,\nIF(BasicFluid!F3=\"Gas\",\"\",\"\")))","v":""}]
[null,null,{"$f":"IF(BasicFluid!F3=\"Liquid\",\"Density\",\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\")),\"Pressure\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\"),\"Operating Density\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\", NOT(BasicFluid!F4=\"Natural Gas\")),\"Base Density\",\"\"))))","v":""},{"$f":"IF(BasicFluid!F4=\"Potable Water\",1,\nIF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!F11=\"\")),BasicFluid!F11,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\"),NOT(BasicFluid!F9=\"\")),BasicFluid!F9,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!F11=\"\")),BasicFluid!F11,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!F7=\"\")),BasicFluid!F7,\"\")))))","v":""},{"$f":"IF(BasicFluid!F4=\"Potable Water\",\"g/mL\",\nIF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!G11=\"\")),BasicFluid!G11,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"),NOT(BasicFluid!F4=\"Natural Gas\"),NOT(BasicFluid!G9=\"\")),BasicFluid!G9,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!G11=\"\")),BasicFluid!G11,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!G7=\"\")),BasicFluid!G7,\"\")))))","v":""}]
[null,null,{"$f":"IF(BasicFluid!F3=\"Liquid\",\"Pressure\",\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\")),\"Temperature\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\"),\"Pressure\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\"),\"Pressure\",\"\"))))","v":""},{"$f":"IF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!F9=\"\")),BasicFluid!F9,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\"),NOT(BasicFluid!F10=\"\")),BasicFluid!F10,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!F9=\"\")),BasicFluid!F9,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!F9=\"\")),BasicFluid!F9,\"\"))))","v":""},{"$f":"IF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!G9=\"\")),BasicFluid!G9,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\"),NOT(BasicFluid!G10=\"\")),BasicFluid!G10,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!G9=\"\")),BasicFluid!G9,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!G9=\"\")),BasicFluid!G9,\"\"))))","v":""}]
[null,null,{"$f":"IF(BasicFluid!F3=\"Liquid\",\"Temperature\",\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\")),\"Flowrate\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\"),\"Temperature\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\"),\"Temperature\",\"\"))))","v":""},{"$f":"IF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!F10=\"\")),BasicFluid!F10,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\"),NOT(BasicFluid!F12=\"\")),BasicFluid!F12,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!F10=\"\")),BasicFluid!F10,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!F10=\"\")),BasicFluid!F10,\"\"))))","v":""},{"$f":"IF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!G10=\"\")),BasicFluid!G10,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\"),NOT(BasicFluid!G12=\"\")),BasicFluid!G12,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!G10=\"\")),BasicFluid!G10,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!G10=\"\")),BasicFluid!G10,\"\"))))","v":""}]
[null,null,{"$f":"IF(BasicFluid!F3=\"Liquid\",\"Flowrate\",\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\")),\"\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\"),\"Flowrate\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\"),\"Flowrate\",\"\"))))","v":""},{"$f":"IF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!F12=\"\")),BasicFluid!F12,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\")),\"\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!F12=\"\")),BasicFluid!F12,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!F12=\"\")),BasicFluid!F12,\"\"))))","v":""},{"$f":"IF(AND(BasicFluid!F3=\"Liquid\",NOT(BasicFluid!G12=\"\")),BasicFluid!G12,\nIF(AND(BasicFluid!F3=\"Gas\",NOT(BasicFluid!F4=\" Other\"), NOT(BasicFluid!F4=\"Natural Gas\")),\"\",\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Operating Conditions\",NOT(BasicFluid!G12=\"\")),BasicFluid!G12,\nIF(AND(BasicFluid!F3=\"Gas\",BasicFluid!F6=\"at Reference Conditions\",NOT(BasicFluid!G12=\"\")),BasicFluid!G12,\"\"))))","v":""}]
[]
[null,null,"QUICK NAVIGATION"]
[null,null,"Click to Jump to any Previous Step"]
[null,null,null,null,null,{"$f":"IF(Step=1,\"\",\"BACK\")","v":""},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Step=1,\"\",\nIF(AND(Step=3,BasicFluid!$F$3=\"Liquid\",$L$8=\"What is the operating pressure in the line? (Optional)\",OR(L12=\"\",M12=\"\",L12=\"Enter Number\",M12=\"Select Units\") ),\"SKIP\",\nIF(AND(Step=4,BasicFluid!$F$3=\"Liquid\",$L$8=\"What is the operating temperature in the line? (Optional)\",OR(L12=\"\",M12=\"\",L12=\"Enter Number\",M12=\"Select Units\")  ),\"SKIP\",\nIF(AND(Step=5,BasicFluid!$F$3=\"Liquid\",$L$8=\"What is the operating pressure in the line? (Optional)\",OR(L12=\"\",M12=\"\",L12=\"Enter Number\",M12=\"Select Units\")  ),\"SKIP\",\nIF(AND(Step=6,BasicFluid!$F$3=\"Liquid\",$L$8=\"What is the operating temperature in the line? (Optional)\",OR(L12=\"\",M12=\"\",L12=\"Enter Number\",M12=\"Select Units\")  ),\"SKIP\",\nIF(AND(Step=2,NOT($L$10=\"\"),NOT($L$10=\"Select Name\")),\"NEXT\",\nIF(AND(Step=3,BasicFluid!$F$3=\"Liquid\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\nIF(AND(Step=4,NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\"),OR($L$8=\"What is the operating temperature in the line? (Optional)\",$L$8=\"What is the operating temperature in the line?\",$L$8=\"What is the density of this fluid?\",$L$8=\"What is the operating pressure in the line? (Optional)\",$L$8=\"What is the operating pressure in the line?\")),\"NEXT\",\nIF(AND(Step=5,BasicFluid!$F$3=\"Liquid\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\nIF(AND(Step=5,BasicFluid!$F$3=\"Gas\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\nIF(AND(Step=6,BasicFluid!$F$3=\"Liquid\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\")),\"NEXT\",\nIF(AND(Step=7,BasicFluid!$F$3=\"Liquid\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\nIF(AND(Step=6,BasicFluid!$F$3=\"Gas\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\nIF(AND(Step=7,BasicFluid!$F$3=\"Gas\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\nIF(AND(Step=8,BasicFluid!$F$3=\"Gas\",NOT(Basic!$L$12=\"\"),NOT(Basic!$M$12=\"\"),NOT(Basic!$L$12=\"Enter Number\"),NOT(Basic!$M$12=\"Select Units\")),\"NEXT\",\n\"\")))))))))))))))","v":""}]

{"sheet":"BasicStructure","index":25,"n_rows":43,"n_cols":19,"rows_kept":43,"cut":false,"hidden":true,"merged":[[5,3,12,3]]}
[]
[null,"Current Tab","Current Step"]
[null,"Fluid",1]
[]
[null,null,null,null,"Step","Prompt","Dropdown Field","Dropdown Units","Free Text Field","Free Text Units","Main Notes","Assume Notes","Option 1","Option 2","Option 3","Option 4","Option 5","Option 6","Additional Notes"]
[null,null,null,"Fluid",1,"Is the fluid a liquid or a gas?"]
[null,null,null,null,2,"What is the name of the fluid?"]
[null,null,null,null,3,{"$f":"IF(BasicFluid!$F$3=\"Gas\",\"Is this gas being measured at actual or reference conditions?\",\nIF(BasicFluid!$F$4=\"Potable Water\",\"What is the operating pressure in the line? (Optional)\",\n\"What is the viscosity of this fluid?\"))","v":"What is the viscosity of this fluid?"}]
[null,null,null,null,4,{"$f":"IF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\"),\"What density is provided by the customer?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\"Natural Gas\"),\"What density should be used for the sizing?\",\nIF(BasicFluid!$F$3=\"Gas\",\"What is the operating pressure in the line?\",\nIF(AND(BasicFluid!$F$3=\"Liquid\",BasicFluid!$F$4=\"Potable Water\"),\"What is the operating temperature in the line? (Optional)\",\nIF(BasicFluid!$F$3=\"Liquid\",\"What is the density of this fluid?\",\"\")))))","v":""}]
[null,null,null,null,5,{"$f":"IF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Reference Conditions\",NOT(BasicFluid!$F$4=\"Natural Gas\")),\"What is the density at reference/base conditions?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Reference Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the operating pressure in the line?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Operating Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the density at operating conditions?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Operating Conditions\"),\"What is the density at operating conditions?\",\nIF(BasicFluid!$F$3=\"Gas\",\"What is the operating temperature in the line?\",\nIF(AND(BasicFluid!$F$3=\"Liquid\",BasicFluid!$F$4=\"Potable Water\"),\"What is the flowrate this meter should be sized to?\",\nIF(BasicFluid!$F$3=\"Liquid\",\"What is the operating pressure in the line? (Optional)\",\"\")))))))","v":""}]
[null,null,null,null,6,{"$f":"IF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Reference Conditions\",NOT(BasicFluid!$F$4=\"Natural Gas\")),\"What is the operating pressure in the line?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Operating Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the operating pressure in the line?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Reference Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the operating temperature in the line?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Operating Conditions\"),\"What is the operating pressure in the line?\",\nIF(BasicFluid!$F$3=\"Gas\",\"What is the flowrate this meter should be sized to?\",\nIF(AND(BasicFluid!$F$3=\"Liquid\",BasicFluid!$F$4=\"Potable Water\"),\"\",\nIF(BasicFluid!$F$3=\"Liquid\",\"What is the operating temperature in the line? (Optional)\",\"\")))))))","v":""}]
[null,null,null,null,7,{"$f":"IF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Reference Conditions\",NOT(BasicFluid!$F$4=\"Natural Gas\")),\"What is the operating temperature in the line?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Operating Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the operating temperature in the line?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Reference Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the flowrate this meter should be sized to?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Operating Conditions\"),\"What is the operating temperature in the line?\",\nIF(BasicFluid!$F$3=\"Gas\",\"\",\nIF(AND(BasicFluid!$F$3=\"Liquid\",BasicFluid!$F$4=\"Potable Water\"),\"\",\nIF(BasicFluid!$F$3=\"Liquid\",\"What is the flowrate this meter should be sized to?\",\"\")))))))","v":""}]
[null,null,null,null,8,{"$f":"IF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Reference Conditions\"),\"What is the flowrate this meter should be sized to?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$6=\"at Operating Conditions\",BasicFluid!$F$4=\"Natural Gas\"),\"What is the flowrate this meter should be sized to?\",\nIF(AND(BasicFluid!$F$3=\"Gas\",BasicFluid!$F$4=\" Other\",BasicFluid!$F$6=\"at Operating Conditions\"),\"What is the flowrate this meter should be sized to?\",\nIF(BasicFluid!$F$3=\"Gas\",\"\",\nIF(AND(BasicFluid!$F$3=\"Liquid\",BasicFluid!$F$4=\"Potable Water\"),\"\",\nIF(BasicFluid!$F$3=\"Liquid\",\"\",\"\"))))))","v":""}]
[]
[null,null,null,null,null,null,null,null,"Units Dropdown",null,"Master Next Button"]
[null,null,null,null,"Master Dropdown",null,"Option","text",{"$f":"\"\"","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E16,\"\")","v":""},null,1,{"$f":"IF(Basic!$L$8=\"Is the fluid a liquid or a gas?\",\"Liquid\",\nIF(Basic!$L$8=\"Is this gas being measured at actual or reference conditions?\",\"Actual\",\nIF(Basic!$L$8=\"What density is provided by the customer?\",\"Operating Density\",\nIF(Basic!$L$8=\"What density should be used for the sizing?\",\"Operating Density\",\n\"\"))))","v":"Liquid"},{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I16,\nIF(Basic!$L$8=\"What is the viscosity of this fluid?\",BasicFluid!L16,\nIF(OR(Basic!$L$8=\"What is the operating temperature in the line?\",Basic!$L$8=\"What is the operating temperature in the line? (Optional)\"),BasicFluid!K16,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M16,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G17,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M16,\n\"\"))))))","v":""},null,null,null,"Prompt","Hints"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E17,\"\")","v":""},null,2,{"$f":"IF(Basic!$L$8=\"Is the fluid a liquid or a gas?\",\"Gas\",\nIF(Basic!$L$8=\"Is this gas being measured at actual or reference conditions?\",\"Reference\",\nIF(Basic!$L$8=\"What density is provided by the customer?\",\"Base/Reference Density\",\nIF(Basic!$L$8=\"What density should be used for the sizing?\",\"Base/Reference Density\",\n\"\"))))","v":"Gas"},{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I17,\nIF(Basic!$L$8=\"What is the viscosity of this fluid?\",BasicFluid!L17,\nIF(OR(Basic!$L$8=\"What is the operating temperature in the line?\",Basic!$L$8=\"What is the operating temperature in the line? (Optional)\"),BasicFluid!K17,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M17,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G18,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M17,\n\"\"))))))","v":""},null,null,null,"Is the fluid a liquid or a gas?","Common liquids are Water and Oil\n\n\nCommon gases are Air, Nitrogen (N2), Oxygen (O2), Methane (CH4), and Carbon Dioxide (CO2)"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E18,\"\")","v":""},null,3,{"$f":"\"\"","v":""},{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I18,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M18,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G19,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M18,\n\"\"))))","v":""},null,null,null,"What is the name of the fluid?",{"$f":"IF(Basic!D17=\"Gas\",\"Select the name of the fluid in the dropdown menu\"&\"                                                                                                     \"&\"                                                                                                     \"&\"Use 'Other' if you cannot find the name of the gas                                                                                                           \",\nIF(Basic!D17=\"Liquid\",\"Select the name of the fluid in the dropdown menu\"&\"                                                                                               \"&\"                                                                                                         \"&\"                                                                                      Potable Water is drinking water and has a Density of 1 g/mL and a Viscosity of 1 cP\",\"\"))","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E19,\"\")","v":""},null,4,{"$f":"\"\"","v":""},{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I19,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M19,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G20,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M19,\n\"\"))))","v":""},null,null,null,"Is this gas being measured at actual or reference conditions?","Use 'Actual' when the flowrate is in mass units (ex. lb/hr)                    or when an \"A\" precedes the flowrate units (ex. ACFM)\n\nUse 'Reference' for all other cases"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E20,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I20,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M20,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G21,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M20,\n\"\"))))","v":""},null,null,null,"What is the operating pressure in the line? (Optional)","This selection is optional but it is recommended all process information is gathered for safety measures"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E21,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I21,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M21,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G22,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M21,\n\"\"))))","v":""},null,null,null,"What is the viscosity of this fluid?","The viscosity of the fluid is a critical parameter in the sizing calculation. The viscosity of water is 1 cP"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E22,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I22,\nIF(Basic!$L$8=\"What is the density of this fluid?\",BasicFluid!M22,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G23,\nIF(OR(Basic!$L$8=\"What is the density at operating conditions?\",Basic!$L$8=\"What is the density at reference/base conditions?\"),BasicFluid!M22,\n\"\"))))","v":""},null,null,null,"What density is provided by the customer?","The Operating Density is the density of the gas under the operating temperature and pressure\n\n\nThe Base/Reference Density is the density of the gas under a reference temperature and pressure (ex. 70 Deg. F and 14.7 psia)"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E23,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I23,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G24,\n\"\"))","v":""},null,null,null,"What density should be used for the sizing?","If given both the Operating  Density and Base/Reference Density, then select Operating Density"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E24,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I24,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G25,\n\"\"))","v":""},null,null,null,"What is the operating pressure in the line?","Enter the operating pressure of this application. VA Meters can only be sized to one operating condition\n\nNote:             psi(g) is also known as psi\n                    psi(a) is a separate unit\n\nThis is true for all units of pressure"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E25,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I25,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G26,\n\"\"))","v":""},null,null,null,"What is the operating temperature in the line? (Optional)","This selection is optional but it is recommended all process information is gathered for safety measures"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E26,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I26,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G27,\n\"\"))","v":""},null,null,null,"What is the density of this fluid?","The density of the fluid is a critical parameter in the sizing calculation. The density of water is 1 g/mL"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E27,\"\")","v":""},null,null,null,{"$f":"IF(OR(Basic!$L$8=\"What is the operating pressure in the line?\",Basic!$L$8=\"What is the operating pressure in the line? (Optional)\"),BasicFluid!I27,\nIF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G28,\n\"\"))","v":""},null,null,null,"What is the density at reference/base conditions?","Enter the density at Reference/Base Conditions"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E28,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G29,\"\")","v":""},null,null,null,"What is the density at operating conditions?","Enter the density at Operating Conditions"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E29,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G30,\"\")","v":""},null,null,null,"What is the operating temperature in the line?","Enter the operating temperature of this application. VA Meters can only be sized to one operating condition"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E30,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G31,\"\")","v":""},null,null,null,"What is the flowrate this meter should be sized to?","Enter the absolute maximum flowrate of the line so the full range can be measured\n\nThe number entered will not necessarily be the exact range of the meter but it will be included"]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E31,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G32,\"\")","v":""},null,null,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E32,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G33,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E33,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G34,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E34,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G35,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E35,\"\")","v":""},null,null,null,{"$f":"IF(Basic!$L$8=\"What is the flowrate this meter should be sized to?\",BasicFluid!G36,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E36,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E37,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E38,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E39,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E40,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E41,\"\")","v":""}]
[null,null,null,null,{"$f":"IF(Step<5,BasicFluid!E42,\"\")","v":""}]

{"sheet":"BasicMeter10A61 3 inch","index":26,"n_rows":54,"n_cols":35,"rows_kept":54,"cut":false,"hidden":true,"merged":[[2,3,2,6],[1,20,1,21],[1,24,1,25]]}
[]
[null,"Current Tab","Current Step",null,null,null,null,"3\" All",null,null,null,null,"3\" Range Limit",null,null,"3\" Range Limit",null,null,null,null,"Final Standard",null,null,null,"Final Alarm",null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},"Conditioned Output for ED3",null,null,null,"Tube/Float","Max Rounded","Tube/Float","Viscosity Warning",null,"Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded","Viscosity Warning","Alarm Capable?",null,"Tube/Float","Max","Error Reason",null,"Tube/Float","Max","Error Reason"]
[null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!F4+0.00000000001","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(D4>0.000975,D4<0.00974999),D4*10^5,\nIF(AND(D4>0.00975,D4<0.0974999),D4*10^4,\nIF(AND(D4>0.0975,D4<0.974999),D4*10^3,\nIF(AND(D4>0.975,D4<9.74999),D4*10^2,\nIF(AND(D4>9.75,D4<97.4999),D4*10^1,\nIF(AND(D4>97.5,D4<974.999),D4*10^0,\nIF(AND(D4>975,D4<9749.99),D4*10^-1,\nIF(AND(D4>9750,D4<97499.9),D4*10^-2,\nIF(AND(D4>97500,D4<974999),D4*10^-3,\"error\")))))))))","v":{"$error":"#VALUE!"}},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E4)),ABS($A$7:$A$54-E4),0))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(D4>0.000975,D4<0.00974999),F4*10^-5,\nIF(AND(D4>0.00975,D4<0.0974999),F4*10^-4,\nIF(AND(D4>0.0975,D4<0.974999),F4*10^-3,\nIF(AND(D4>0.975,D4<9.74999),F4*10^-2,\nIF(AND(D4>9.75,D4<97.4999),F4*10^-1,\nIF(AND(D4>97.5,D4<974.999),F4*10^0,\nIF(AND(D4>975,D4<9749.99),F4*10^1,\nIF(AND(D4>9750,D4<97499.9),F4*10^2,\nIF(AND(D4>97500,D4<974999),F4*10^3,\"error\")))))))))","v":{"$error":"#VALUE!"}},"1/8-08-BG",{"$f":"G4","v":{"$error":"#VALUE!"}},"1/8-08-BG",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E4,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I4*0.45),'BasicMeter10A61 3 inch'!I4+0.000001>'Modified Inputs'!$N$2),H4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I4*0.45),'BasicMeter10A61 3 inch'!I4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I4,0),0)","v":0},null,{"$f":"VLOOKUP(Q4,$I$4:$J$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($N$4:$N$33>0,N4:N33))","v":0},{"$f":"VLOOKUP(P4,$J$4:$K$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(OR(RIGHT(P4,2)=\"SS\",RIGHT(P4,2)=\"CA\"),\"yes\",\"no\")","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(IF($R$33=\"\",$P$33,1/0),\nIFERROR(IF($R$32=\"\",$P$32,1/0),\nIFERROR(IF($R$31=\"\",$P$31,1/0),\nIFERROR(IF($R$30=\"\",$P$30,1/0),\nIFERROR(IF($R$29=\"\",$P$29,1/0),\nIFERROR(IF($R$28=\"\",$P$28,1/0),\nIFERROR(IF($R$27=\"\",$P$27,1/0),\nIFERROR(IF($R$26=\"\",$P$26,1/0),\nIFERROR(IF($R$25=\"\",$P$25,1/0),\nIFERROR(IF($R$24=\"\",$P$24,1/0),\nIFERROR(IF($R$23=\"\",$P$23,1/0),\nIFERROR(IF($R$22=\"\",$P$22,1/0),\nIFERROR(IF($R$21=\"\",$P$21,1/0),\nIFERROR(IF($R$20=\"\",$P$20,1/0),\nIFERROR(IF($R$19=\"\",$P$19,1/0),\nIFERROR(IF($R$18=\"\",$P$18,1/0),\nIFERROR(IF($R$17=\"\",$P$17,1/0),\nIFERROR(IF($R$16=\"\",$P$16,1/0),\nIFERROR(IF($R$15=\"\",$P$15,1/0),\nIFERROR(IF($R$14=\"\",$P$14,1/0),\nIFERROR(IF($R$13=\"\",$P$13,1/0),\nIFERROR(IF($R$12=\"\",$P$12,1/0),\nIFERROR(IF($R$11=\"\",$P$11,1/0),\nIFERROR(IF($R$10=\"\",$P$10,1/0),\nIFERROR(IF($R$9=\"\",$P$9,1/0),\nIFERROR(IF($R$8=\"\",$P$8,1/0),\nIFERROR(IF($R$7=\"\",$P$7,1/0),\nIFERROR(IF($R$6=\"\",$P$6,1/0),\nIFERROR(IF($R$5=\"\",$P$5,1/0),\nIFERROR(IF($R$4=\"\",$P$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(U4,$P$4:$Q$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(AND(U4=\"none\",R4=\"viscosity\"),\"viscosity\",\"\"),\"sizing\")","v":"sizing"},null,{"$f":"IFERROR(IF(AND($R$33=\"\",$S$33=\"yes\"),$P$33,1/0),\nIFERROR(IF(AND($R$32=\"\",$S$32=\"yes\"),$P$32,1/0),\nIFERROR(IF(AND($R$31=\"\",$S$31=\"yes\"),$P$31,1/0),\nIFERROR(IF(AND($R$30=\"\",$S$30=\"yes\"),$P$30,1/0),\nIFERROR(IF(AND($R$29=\"\",$S$29=\"yes\"),$P$29,1/0),\nIFERROR(IF(AND($R$28=\"\",$S$28=\"yes\"),$P$28,1/0),\nIFERROR(IF(AND($R$27=\"\",$S$27=\"yes\"),$P$27,1/0),\nIFERROR(IF(AND($R$26=\"\",$S$26=\"yes\"),$P$26,1/0),\nIFERROR(IF(AND($R$25=\"\",$S$25=\"yes\"),$P$25,1/0),\nIFERROR(IF(AND($R$24=\"\",$S$24=\"yes\"),$P$24,1/0),\nIFERROR(IF(AND($R$23=\"\",$S$23=\"yes\"),$P$23,1/0),\nIFERROR(IF(AND($R$22=\"\",$S$22=\"yes\"),$P$22,1/0),\nIFERROR(IF(AND($R$21=\"\",$S$21=\"yes\"),$P$21,1/0),\nIFERROR(IF(AND($R$20=\"\",$S$20=\"yes\"),$P$20,1/0),\nIFERROR(IF(AND($R$19=\"\",$S$19=\"yes\"),$P$19,1/0),\nIFERROR(IF(AND($R$18=\"\",$S$18=\"yes\"),$P$18,1/0),\nIFERROR(IF(AND($R$17=\"\",$S$17=\"yes\"),$P$17,1/0),\nIFERROR(IF(AND($R$16=\"\",$S$16=\"yes\"),$P$16,1/0),\nIFERROR(IF(AND($R$15=\"\",$S$15=\"yes\"),$P$15,1/0),\nIFERROR(IF(AND($R$14=\"\",$S$14=\"yes\"),$P$14,1/0),\nIFERROR(IF(AND($R$13=\"\",$S$13=\"yes\"),$P$13,1/0),\nIFERROR(IF(AND($R$12=\"\",$S$12=\"yes\"),$P$12,1/0),\nIFERROR(IF(AND($R$11=\"\",$S$11=\"yes\"),$P$11,1/0),\nIFERROR(IF(AND($R$10=\"\",$S$10=\"yes\"),$P$10,1/0),\nIFERROR(IF(AND($R$9=\"\",$S$9=\"yes\"),$P$9,1/0),\nIFERROR(IF(AND($R$8=\"\",$S$8=\"yes\"),$P$8,1/0),\nIFERROR(IF(AND($R$7=\"\",$S$7=\"yes\"),$P$7,1/0),\nIFERROR(IF(AND($R$6=\"\",$S$6=\"yes\"),$P$6,1/0),\nIFERROR(IF(AND($R$5=\"\",$S$5=\"yes\"),$P$5,1/0),\nIFERROR(IF(AND($R$4=\"\",$S$4=\"yes\"),$P$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(Y4,$P$4:$Q$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(AND(Y4=\"none\",R4=\"viscosity\"),\"viscosity\",\nIF(Y4=\"none\",\"sizing\",\"\")),\"sizing\")","v":"sizing"}]
[null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!F5+0.00000000001","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(D5>0.000975,D5<0.00974999),D5*10^5,\nIF(AND(D5>0.00975,D5<0.0974999),D5*10^4,\nIF(AND(D5>0.0975,D5<0.974999),D5*10^3,\nIF(AND(D5>0.975,D5<9.74999),D5*10^2,\nIF(AND(D5>9.75,D5<97.4999),D5*10^1,\nIF(AND(D5>97.5,D5<974.999),D5*10^0,\nIF(AND(D5>975,D5<9749.99),D5*10^-1,\nIF(AND(D5>9750,D5<97499.9),D5*10^-2,\nIF(AND(D5>97500,D5<974999),D5*10^-3,\"error\")))))))))","v":{"$error":"#VALUE!"}},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E5)),ABS($A$7:$A$54-E5),0))","v":{"$error":"#VALUE!"}},{"$f":"IF(AND(D5>0.000975,D5<0.00974999),F5*10^-5,\nIF(AND(D5>0.00975,D5<0.0974999),F5*10^-4,\nIF(AND(D5>0.0975,D5<0.974999),F5*10^-3,\nIF(AND(D5>0.975,D5<9.74999),F5*10^-2,\nIF(AND(D5>9.75,D5<97.4999),F5*10^-1,\nIF(AND(D5>97.5,D5<974.999),F5*10^0,\nIF(AND(D5>975,D5<9749.99),F5*10^1,\nIF(AND(D5>9750,D5<97499.9),F5*10^2,\nIF(AND(D5>97500,D5<974999),F5*10^3,\"error\")))))))))","v":{"$error":"#VALUE!"}},"1/8-08-SA",{"$f":"G5","v":{"$error":"#VALUE!"}},"1/8-08-SA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E5,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I5*0.45),'BasicMeter10A61 3 inch'!I5+0.000001>'Modified Inputs'!$N$2),H5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I5*0.45),'BasicMeter10A61 3 inch'!I5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I5,0),0)","v":0},null,{"$f":"VLOOKUP(Q5,$I$4:$J$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($N$4:$N$33<Q4,$N$4:$N$33))","v":0},{"$f":"VLOOKUP(P5,$J$4:$K$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(OR(RIGHT(P5,2)=\"SS\",RIGHT(P5,2)=\"CA\"),\"yes\",\"no\")","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
["Range","Name",null,{"$f":"'10A61 3\" Gas+liquid Results'!F6+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E6)),ABS($A$7:$A$54-E6),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-08-SS",{"$error":"#VALUE!"},"1/8-08-SS",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E6,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I6*0.45),'BasicMeter10A61 3 inch'!I6+0.000001>'Modified Inputs'!$N$2),H6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I6*0.45),'BasicMeter10A61 3 inch'!I6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q5,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[100,"ED-3-100",null,{"$f":"'10A61 3\" Gas+liquid Results'!F7+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E7)),ABS($A$7:$A$54-E7),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-08-CA",{"$error":"#VALUE!"},"1/8-08-CA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E7,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I7*0.45),'BasicMeter10A61 3 inch'!I7+0.000001>'Modified Inputs'!$N$2),H7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I7*0.45),'BasicMeter10A61 3 inch'!I7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q6,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[105,"ED-3-105",null,{"$f":"'10A61 3\" Gas+liquid Results'!F8+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E8)),ABS($A$7:$A$54-E8),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-08-TA",{"$error":"#VALUE!"},"1/8-08-TA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E8,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I8*0.45),'BasicMeter10A61 3 inch'!I8+0.000001>'Modified Inputs'!$N$2),H8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I8*0.45),'BasicMeter10A61 3 inch'!I8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q7,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[110,"ED-3-110",null,{"$f":"'10A61 3\" Gas+liquid Results'!F9+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E9)),ABS($A$7:$A$54-E9),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-20-BG",{"$error":"#VALUE!"},"1/8-20-BG",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E9,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I9*0.45),'BasicMeter10A61 3 inch'!I9+0.000001>'Modified Inputs'!$N$2),H9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I9*0.45),'BasicMeter10A61 3 inch'!I9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q8,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[115,"ED-3-115",null,{"$f":"'10A61 3\" Gas+liquid Results'!F10+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E10)),ABS($A$7:$A$54-E10),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-20-SA",{"$error":"#VALUE!"},"1/8-20-SA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E10,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I10*0.45),'BasicMeter10A61 3 inch'!I10+0.000001>'Modified Inputs'!$N$2),H10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I10*0.45),'BasicMeter10A61 3 inch'!I10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I10,0),0)","v":0},null,{"$f":"VLOOKUP(Q10,$I$4:$J$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($N$4:$N$33<Q9,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[120,"ED-3-120",null,{"$f":"'10A61 3\" Gas+liquid Results'!F11+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E11)),ABS($A$7:$A$54-E11),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-20-SS",{"$error":"#VALUE!"},"1/8-20-SS",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E11,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I11*0.45),'BasicMeter10A61 3 inch'!I11+0.000001>'Modified Inputs'!$N$2),H11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I11*0.45),'BasicMeter10A61 3 inch'!I11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q10,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[125,"ED-3-125",null,{"$f":"'10A61 3\" Gas+liquid Results'!F12+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E12)),ABS($A$7:$A$54-E12),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-20-CA",{"$error":"#VALUE!"},"1/8-20-CA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E12,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I12*0.45),'BasicMeter10A61 3 inch'!I12+0.000001>'Modified Inputs'!$N$2),H12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I12*0.45),'BasicMeter10A61 3 inch'!I12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q11,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[130,"ED-3-130",null,{"$f":"'10A61 3\" Gas+liquid Results'!F13+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E13)),ABS($A$7:$A$54-E13),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/8-20-TA",{"$error":"#VALUE!"},"1/8-20-TA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E13,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I13*0.45),'BasicMeter10A61 3 inch'!I13+0.000001>'Modified Inputs'!$N$2),H13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I13*0.45),'BasicMeter10A61 3 inch'!I13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q12,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[135,"ED-3-135",null,{"$f":"'10A61 3\" Gas+liquid Results'!F14+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E14)),ABS($A$7:$A$54-E14),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-15-BG",{"$error":"#VALUE!"},"1/4-15-BG",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E14,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I14*0.45),'BasicMeter10A61 3 inch'!I14+0.000001>'Modified Inputs'!$N$2),H14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I14*0.45),'BasicMeter10A61 3 inch'!I14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q13,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[140,"ED-3-140",null,{"$f":"'10A61 3\" Gas+liquid Results'!F15+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E15)),ABS($A$7:$A$54-E15),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-15-SA",{"$error":"#VALUE!"},"1/4-15-SA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E15,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I15*0.45),'BasicMeter10A61 3 inch'!I15+0.000001>'Modified Inputs'!$N$2),H15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I15*0.45),'BasicMeter10A61 3 inch'!I15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q14,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"No"]
[145,"ED-3-145",null,{"$f":"'10A61 3\" Gas+liquid Results'!F16+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E16)),ABS($A$7:$A$54-E16),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-15-SS",{"$error":"#VALUE!"},"1/4-15-SS",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E16,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I16*0.45),'BasicMeter10A61 3 inch'!I16+0.000001>'Modified Inputs'!$N$2),H16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I16*0.45),'BasicMeter10A61 3 inch'!I16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q15,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[150,"ED-3-150",null,{"$f":"'10A61 3\" Gas+liquid Results'!F17+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E17)),ABS($A$7:$A$54-E17),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-15-CA",{"$error":"#VALUE!"},"1/4-15-CA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E17,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I17*0.45),'BasicMeter10A61 3 inch'!I17+0.000001>'Modified Inputs'!$N$2),H17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I17*0.45),'BasicMeter10A61 3 inch'!I17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q16,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[160,"ED-3-160",null,{"$f":"'10A61 3\" Gas+liquid Results'!F18+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E18)),ABS($A$7:$A$54-E18),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-15-TA",{"$error":"#VALUE!"},"1/4-15-TA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E18,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I18*0.45),'BasicMeter10A61 3 inch'!I18+0.000001>'Modified Inputs'!$N$2),H18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I18*0.45),'BasicMeter10A61 3 inch'!I18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q17,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[170,"ED-3-170",null,{"$f":"'10A61 3\" Gas+liquid Results'!F19+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E19)),ABS($A$7:$A$54-E19),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-20-BG",{"$error":"#VALUE!"},"1/4-20-BG",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E19,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I19*0.45),'BasicMeter10A61 3 inch'!I19+0.000001>'Modified Inputs'!$N$2),H19,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I19*0.45),'BasicMeter10A61 3 inch'!I19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q18,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[180,"ED-3-180",null,{"$f":"'10A61 3\" Gas+liquid Results'!F20+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E20)),ABS($A$7:$A$54-E20),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-20-SA",{"$error":"#VALUE!"},"1/4-20-SA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E20,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I20*0.45),'BasicMeter10A61 3 inch'!I20+0.000001>'Modified Inputs'!$N$2),H20,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I20*0.45),'BasicMeter10A61 3 inch'!I20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q19,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[190,"ED-3-190",null,{"$f":"'10A61 3\" Gas+liquid Results'!F21+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E21)),ABS($A$7:$A$54-E21),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-20-SS",{"$error":"#VALUE!"},"1/4-20-SS",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E21,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I21*0.45),'BasicMeter10A61 3 inch'!I21+0.000001>'Modified Inputs'!$N$2),H21,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I21*0.45),'BasicMeter10A61 3 inch'!I21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q20,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[200,"ED-3-200",null,{"$f":"'10A61 3\" Gas+liquid Results'!F22+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E22)),ABS($A$7:$A$54-E22),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-20-CA",{"$error":"#VALUE!"},"1/4-20-CA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E22,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I22*0.45),'BasicMeter10A61 3 inch'!I22+0.000001>'Modified Inputs'!$N$2),H22,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I22*0.45),'BasicMeter10A61 3 inch'!I22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q21,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[210,"ED-3-210",null,{"$f":"'10A61 3\" Gas+liquid Results'!F23+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E23)),ABS($A$7:$A$54-E23),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-20-TA",{"$error":"#VALUE!"},"1/4-20-TA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E23,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I23*0.45),'BasicMeter10A61 3 inch'!I23+0.000001>'Modified Inputs'!$N$2),H23,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I23*0.45),'BasicMeter10A61 3 inch'!I23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q22,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[220,"ED-3-220",null,{"$f":"'10A61 3\" Gas+liquid Results'!F24+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E24)),ABS($A$7:$A$54-E24),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-G-BG",{"$error":"#VALUE!"},"1/4-41-G-BG",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E24,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I24*0.45),'BasicMeter10A61 3 inch'!I24+0.000001>'Modified Inputs'!$N$2),H24,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I24*0.45),'BasicMeter10A61 3 inch'!I24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q23,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[230,"ED-3-230",null,{"$f":"'10A61 3\" Gas+liquid Results'!F25+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E25)),ABS($A$7:$A$54-E25),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-G-SA",{"$error":"#VALUE!"},"1/4-41-G-SA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E25,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I25*0.45),'BasicMeter10A61 3 inch'!I25+0.000001>'Modified Inputs'!$N$2),H25,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I25*0.45),'BasicMeter10A61 3 inch'!I25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q24,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[240,"ED-3-240",null,{"$f":"'10A61 3\" Gas+liquid Results'!F26+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E26)),ABS($A$7:$A$54-E26),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-G-SS",{"$error":"#VALUE!"},"1/4-41-G-SS",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E26,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I26*0.45),'BasicMeter10A61 3 inch'!I26+0.000001>'Modified Inputs'!$N$2),H26,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I26*0.45),'BasicMeter10A61 3 inch'!I26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q25,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[250,"ED-3-250",null,{"$f":"'10A61 3\" Gas+liquid Results'!F27+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E27)),ABS($A$7:$A$54-E27),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-G-CA",{"$error":"#VALUE!"},"1/4-41-G-CA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E27,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I27*0.45),'BasicMeter10A61 3 inch'!I27+0.000001>'Modified Inputs'!$N$2),H27,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I27*0.45),'BasicMeter10A61 3 inch'!I27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q26,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[260,"ED-3-260",null,{"$f":"'10A61 3\" Gas+liquid Results'!F28+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E28)),ABS($A$7:$A$54-E28),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-G-TA",{"$error":"#VALUE!"},"1/4-41-G-TA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E28,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I28*0.45),'BasicMeter10A61 3 inch'!I28+0.000001>'Modified Inputs'!$N$2),H28,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I28*0.45),'BasicMeter10A61 3 inch'!I28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q27,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[270,"ED-3-270",null,{"$f":"'10A61 3\" Gas+liquid Results'!F29+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E29)),ABS($A$7:$A$54-E29),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-P-BG",{"$error":"#VALUE!"},"1/4-41-P-BG",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E29,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I29*0.45),'BasicMeter10A61 3 inch'!I29+0.000001>'Modified Inputs'!$N$2),H29,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I29*0.45),'BasicMeter10A61 3 inch'!I29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q28,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[280,"ED-3-280",null,{"$f":"'10A61 3\" Gas+liquid Results'!F30+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E30)),ABS($A$7:$A$54-E30),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-P-SA",{"$error":"#VALUE!"},"1/4-41-P-SA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E30,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I30*0.45),'BasicMeter10A61 3 inch'!I30+0.000001>'Modified Inputs'!$N$2),H30,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I30*0.45),'BasicMeter10A61 3 inch'!I30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q29,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[290,"ED-3-290",null,{"$f":"'10A61 3\" Gas+liquid Results'!F31+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E31)),ABS($A$7:$A$54-E31),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-P-SS",{"$error":"#VALUE!"},"1/4-41-P-SS",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E31,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I31*0.45),'BasicMeter10A61 3 inch'!I31+0.000001>'Modified Inputs'!$N$2),H31,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I31*0.45),'BasicMeter10A61 3 inch'!I31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q30,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[300,"ED-3-300",null,{"$f":"'10A61 3\" Gas+liquid Results'!F32+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E32)),ABS($A$7:$A$54-E32),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-P-CA",{"$error":"#VALUE!"},"1/4-41-P-CA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E32,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I32*0.45),'BasicMeter10A61 3 inch'!I32+0.000001>'Modified Inputs'!$N$2),H32,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I32*0.45),'BasicMeter10A61 3 inch'!I32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q31,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[320,"ED-3-320",null,{"$f":"'10A61 3\" Gas+liquid Results'!F33+0.00000000001","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"INDEX($A$7:$A$54,MATCH(MIN(ABS($A$7:$A$54-E33)),ABS($A$7:$A$54-E33),0))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},"1/4-41-P-TA",{"$error":"#VALUE!"},"1/4-41-P-TA",{"$f":"IF(LEFT('10A61 3\" Gas+liquid Results'!E33,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I33*0.45),'BasicMeter10A61 3 inch'!I33+0.000001>'Modified Inputs'!$N$2),H33,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 3 inch'!I33*0.45),'BasicMeter10A61 3 inch'!I33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 3 inch'!I33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$33<Q32,$N$4:$N$33))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[240,"ED-3-340"]
[360,"ED-3-360"]
[380,"ED-3-380"]
[400,"ED-3-400"]
[420,"ED-3-420"]
[440,"ED-3-440"]
[460,"ED-3-460"]
[480,"ED-3-480"]
[500,"ED-3-500"]
[520,"ED-3-520"]
[540,"ED-3-540"]
[560,"ED-3-560"]
[580,"ED-3-580"]
[600,"ED-3-600"]
[650,"ED-3-650"]
[700,"ED-3-700"]
[750,"ED-3-750"]
[800,"ED-3-800"]
[850,"ED-3-850"]
[900,"ED-3-900"]
[950,"ED-3-950"]

{"sheet":"BasicMeter10A61 5 inch","index":27,"n_rows":72,"n_cols":35,"rows_kept":72,"cut":false,"hidden":true,"merged":[[2,3,2,6],[2,21,2,22],[2,25,2,26]]}
[]
[null,"Current Tab","Current Step",null,null,null,null,"5\" All",null,null,null,null,"5\" Range Limit",null,null,"5\" Range Limit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,null,null,null,"Tube/Float","Max Rounded","Tube/Float","Viscosity Warning",null,"Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded","Viscosity Warning","Alarm Capable?",null,null,"Final Standard",null,null,null,"Final Alarm"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C3*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-25-CD",{"$f":"IF(G4<0.00000099999,ROUND(G4,7),\nIF(G4<0.0000099999,ROUND(G4,6),\nIF(G4<0.000099999,ROUND(G4,5),\nIF(G4<0.00099999,ROUND(G4,4),\nIF(G4<0.0099999,ROUND(G4,3),\nIF(G4<0.099999,ROUND(G4,2),\nIF(G4<0.99999,ROUND(G4,2),\nIF(G4<9.999,ROUND(G4,2),\nIF(G4<99.99,ROUND(G4,1),\nIF(G4<999.99,ROUND(G4,0),\nIF(G4<9999.99,ROUND(G4,-1),\nIF(G4<99999,ROUND(G4,-2),ROUND(G4,2)))))))))))))","v":{"$error":"#VALUE!"}},"1/4-25-CD",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E3,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I4*0.45),'BasicMeter10A61 5 inch'!I4+0.000001>'Modified Inputs'!$N$2),H4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I4*0.45),'BasicMeter10A61 5 inch'!I4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I4,0),0)","v":0},{"$f":"LEFT(P4,4)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Q4,$I$4:$J$72,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($N$4:$N$72>0,N4:N72))","v":0},{"$f":"VLOOKUP(P4,$J$4:$K$72,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(AND(NOT(O4=\"1/16\"),OR(RIGHT(P4,2)=\"SS\",RIGHT(P4,2)=\"CA\")),\"yes\",\"no\")","v":{"$error":"#N/A"}},null,null,"Tube/Float","Max","Error Reason",null,"Tube/Float","Max","Error Reason"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C4*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-25-SA",{"$f":"IF(G5<0.00000099999,ROUND(G5,7),\nIF(G5<0.0000099999,ROUND(G5,6),\nIF(G5<0.000099999,ROUND(G5,5),\nIF(G5<0.00099999,ROUND(G5,4),\nIF(G5<0.0099999,ROUND(G5,3),\nIF(G5<0.099999,ROUND(G5,2),\nIF(G5<0.99999,ROUND(G5,2),\nIF(G5<9.999,ROUND(G5,2),\nIF(G5<99.99,ROUND(G5,1),\nIF(G5<999.99,ROUND(G5,0),\nIF(G5<9999.99,ROUND(G5,-1),\nIF(G5<99999,ROUND(G5,-2),ROUND(G5,2)))))))))))))","v":{"$error":"#VALUE!"}},"1/4-25-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E4,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I5*0.45),'BasicMeter10A61 5 inch'!I5+0.000001>'Modified Inputs'!$N$2),H5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I5*0.45),'BasicMeter10A61 5 inch'!I5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I5,0),0)","v":0},{"$f":"LEFT(P5,4)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Q5,$I$4:$J$72,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($N$4:$N$72<Q4,$N$4:$N$72))","v":0},{"$f":"VLOOKUP(P5,$J$4:$K$72,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,null,{"$f":"IFERROR(IF($R$33=\"\",$P$33,1/0),\nIFERROR(IF($R$32=\"\",$P$32,1/0),\nIFERROR(IF($R$31=\"\",$P$31,1/0),\nIFERROR(IF($R$30=\"\",$P$30,1/0),\nIFERROR(IF($R$29=\"\",$P$29,1/0),\nIFERROR(IF($R$28=\"\",$P$28,1/0),\nIFERROR(IF($R$27=\"\",$P$27,1/0),\nIFERROR(IF($R$26=\"\",$P$26,1/0),\nIFERROR(IF($R$25=\"\",$P$25,1/0),\nIFERROR(IF($R$24=\"\",$P$24,1/0),\nIFERROR(IF($R$23=\"\",$P$23,1/0),\nIFERROR(IF($R$22=\"\",$P$22,1/0),\nIFERROR(IF($R$21=\"\",$P$21,1/0),\nIFERROR(IF($R$20=\"\",$P$20,1/0),\nIFERROR(IF($R$19=\"\",$P$19,1/0),\nIFERROR(IF($R$18=\"\",$P$18,1/0),\nIFERROR(IF($R$17=\"\",$P$17,1/0),\nIFERROR(IF($R$16=\"\",$P$16,1/0),\nIFERROR(IF($R$15=\"\",$P$15,1/0),\nIFERROR(IF($R$14=\"\",$P$14,1/0),\nIFERROR(IF($R$13=\"\",$P$13,1/0),\nIFERROR(IF($R$12=\"\",$P$12,1/0),\nIFERROR(IF($R$11=\"\",$P$11,1/0),\nIFERROR(IF($R$10=\"\",$P$10,1/0),\nIFERROR(IF($R$9=\"\",$P$9,1/0),\nIFERROR(IF($R$8=\"\",$P$8,1/0),\nIFERROR(IF($R$7=\"\",$P$7,1/0),\nIFERROR(IF($R$6=\"\",$P$6,1/0),\nIFERROR(IF($R$5=\"\",$P$5,1/0),\nIFERROR(IF($R$4=\"\",$P$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(V5,$P$4:$Q$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(AND(V5=\"none\",R4=\"viscosity\"),\"viscosity\",\"\"),\"sizing\")","v":"sizing"},null,{"$f":"IFERROR(IF(AND($R$33=\"\",$S$33=\"yes\"),$P$33,1/0),\nIFERROR(IF(AND($R$32=\"\",$S$32=\"yes\"),$P$32,1/0),\nIFERROR(IF(AND($R$31=\"\",$S$31=\"yes\"),$P$31,1/0),\nIFERROR(IF(AND($R$30=\"\",$S$30=\"yes\"),$P$30,1/0),\nIFERROR(IF(AND($R$29=\"\",$S$29=\"yes\"),$P$29,1/0),\nIFERROR(IF(AND($R$28=\"\",$S$28=\"yes\"),$P$28,1/0),\nIFERROR(IF(AND($R$27=\"\",$S$27=\"yes\"),$P$27,1/0),\nIFERROR(IF(AND($R$26=\"\",$S$26=\"yes\"),$P$26,1/0),\nIFERROR(IF(AND($R$25=\"\",$S$25=\"yes\"),$P$25,1/0),\nIFERROR(IF(AND($R$24=\"\",$S$24=\"yes\"),$P$24,1/0),\nIFERROR(IF(AND($R$23=\"\",$S$23=\"yes\"),$P$23,1/0),\nIFERROR(IF(AND($R$22=\"\",$S$22=\"yes\"),$P$22,1/0),\nIFERROR(IF(AND($R$21=\"\",$S$21=\"yes\"),$P$21,1/0),\nIFERROR(IF(AND($R$20=\"\",$S$20=\"yes\"),$P$20,1/0),\nIFERROR(IF(AND($R$19=\"\",$S$19=\"yes\"),$P$19,1/0),\nIFERROR(IF(AND($R$18=\"\",$S$18=\"yes\"),$P$18,1/0),\nIFERROR(IF(AND($R$17=\"\",$S$17=\"yes\"),$P$17,1/0),\nIFERROR(IF(AND($R$16=\"\",$S$16=\"yes\"),$P$16,1/0),\nIFERROR(IF(AND($R$15=\"\",$S$15=\"yes\"),$P$15,1/0),\nIFERROR(IF(AND($R$14=\"\",$S$14=\"yes\"),$P$14,1/0),\nIFERROR(IF(AND($R$13=\"\",$S$13=\"yes\"),$P$13,1/0),\nIFERROR(IF(AND($R$12=\"\",$S$12=\"yes\"),$P$12,1/0),\nIFERROR(IF(AND($R$11=\"\",$S$11=\"yes\"),$P$11,1/0),\nIFERROR(IF(AND($R$10=\"\",$S$10=\"yes\"),$P$10,1/0),\nIFERROR(IF(AND($R$9=\"\",$S$9=\"yes\"),$P$9,1/0),\nIFERROR(IF(AND($R$8=\"\",$S$8=\"yes\"),$P$8,1/0),\nIFERROR(IF(AND($R$7=\"\",$S$7=\"yes\"),$P$7,1/0),\nIFERROR(IF(AND($R$6=\"\",$S$6=\"yes\"),$P$6,1/0),\nIFERROR(IF(AND($R$5=\"\",$S$5=\"yes\"),$P$5,1/0),\nIFERROR(IF(AND($R$4=\"\",$S$4=\"yes\"),$P$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(Z5,$P$4:$Q$33,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IFERROR(IF(AND(Z5=\"none\",R4=\"viscosity\"),\"viscosity\",\nIF(Z5=\"none\",\"sizing\",\"\")),\"sizing\")","v":"sizing"},null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C5*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-25-SS",{"$error":"#VALUE!"},"1/4-25-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E5,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I6*0.45),'BasicMeter10A61 5 inch'!I6+0.000001>'Modified Inputs'!$N$2),H6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I6*0.45),'BasicMeter10A61 5 inch'!I6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I6,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q5,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C6*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-25-CA",{"$error":"#VALUE!"},"1/4-25-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E6,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I7*0.45),'BasicMeter10A61 5 inch'!I7+0.000001>'Modified Inputs'!$N$2),H7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I7*0.45),'BasicMeter10A61 5 inch'!I7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I7,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q6,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C7*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-25-TA",{"$error":"#VALUE!"},"1/4-25-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E7,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I8*0.45),'BasicMeter10A61 5 inch'!I8+0.000001>'Modified Inputs'!$N$2),H8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I8*0.45),'BasicMeter10A61 5 inch'!I8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I8,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q7,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C8*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-25-BG",{"$error":"#VALUE!"},"1/4-25-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E8,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I9*0.45),'BasicMeter10A61 5 inch'!I9+0.000001>'Modified Inputs'!$N$2),H9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I9*0.45),'BasicMeter10A61 5 inch'!I9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I9,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q8,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C9*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-20-CD",{"$error":"#VALUE!"},"1/4-20-CD",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E9,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I10*0.45),'BasicMeter10A61 5 inch'!I10+0.000001>'Modified Inputs'!$N$2),H10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I10*0.45),'BasicMeter10A61 5 inch'!I10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I10,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q9,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C10*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-20-SA",{"$error":"#VALUE!"},"1/4-20-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E10,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I11*0.45),'BasicMeter10A61 5 inch'!I11+0.000001>'Modified Inputs'!$N$2),H11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I11*0.45),'BasicMeter10A61 5 inch'!I11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I11,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q10,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C11*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-20-SS",{"$error":"#VALUE!"},"1/4-20-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E11,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I12*0.45),'BasicMeter10A61 5 inch'!I12+0.000001>'Modified Inputs'!$N$2),H12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I12*0.45),'BasicMeter10A61 5 inch'!I12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I12,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q11,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C12*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-20-CA",{"$error":"#VALUE!"},"1/4-20-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E12,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I13*0.45),'BasicMeter10A61 5 inch'!I13+0.000001>'Modified Inputs'!$N$2),H13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I13*0.45),'BasicMeter10A61 5 inch'!I13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I13,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q12,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$f":"IF(AND(NOT(O13=\"1/16\"),OR(RIGHT(P13,2)=\"SS\",RIGHT(P13,2)=\"CA\")),\"yes\",\"no\")","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C13*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-20-TA",{"$error":"#VALUE!"},"1/4-20-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E13,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I14*0.45),'BasicMeter10A61 5 inch'!I14+0.000001>'Modified Inputs'!$N$2),H14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I14*0.45),'BasicMeter10A61 5 inch'!I14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I14,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q13,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C14*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-20-BG",{"$error":"#VALUE!"},"1/4-20-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E14,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I15*0.45),'BasicMeter10A61 5 inch'!I15+0.000001>'Modified Inputs'!$N$2),H15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I15*0.45),'BasicMeter10A61 5 inch'!I15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I15,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q14,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-16-CD",{"$error":"#VALUE!"},"1/4-16-CD",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E15,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I16*0.45),'BasicMeter10A61 5 inch'!I16+0.000001>'Modified Inputs'!$N$2),H16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I16*0.45),'BasicMeter10A61 5 inch'!I16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I16,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q15,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C16*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-16-SA",{"$error":"#VALUE!"},"1/4-16-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E16,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I17*0.45),'BasicMeter10A61 5 inch'!I17+0.000001>'Modified Inputs'!$N$2),H17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I17*0.45),'BasicMeter10A61 5 inch'!I17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I17,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q16,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C17*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-16-SS",{"$error":"#VALUE!"},"1/4-16-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E17,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I18*0.45),'BasicMeter10A61 5 inch'!I18+0.000001>'Modified Inputs'!$N$2),H18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I18*0.45),'BasicMeter10A61 5 inch'!I18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I18,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q17,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C18*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-16-CA",{"$error":"#VALUE!"},"1/4-16-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E18,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I19*0.45),'BasicMeter10A61 5 inch'!I19+0.000001>'Modified Inputs'!$N$2),H19,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I19*0.45),'BasicMeter10A61 5 inch'!I19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I19,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q18,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C19*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-16-TA",{"$error":"#VALUE!"},"1/4-16-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E19,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I20*0.45),'BasicMeter10A61 5 inch'!I20+0.000001>'Modified Inputs'!$N$2),H20,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I20*0.45),'BasicMeter10A61 5 inch'!I20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I20,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q19,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C20*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-16-BG",{"$error":"#VALUE!"},"1/4-16-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E20,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I21*0.45),'BasicMeter10A61 5 inch'!I21+0.000001>'Modified Inputs'!$N$2),H21,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I21*0.45),'BasicMeter10A61 5 inch'!I21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I21,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q20,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C21*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-10-CD",{"$error":"#VALUE!"},"1/4-10-CD",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E21,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I22*0.45),'BasicMeter10A61 5 inch'!I22+0.000001>'Modified Inputs'!$N$2),H22,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I22*0.45),'BasicMeter10A61 5 inch'!I22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I22,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q21,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C22*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-10-SA",{"$error":"#VALUE!"},"1/4-10-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E22,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I23*0.45),'BasicMeter10A61 5 inch'!I23+0.000001>'Modified Inputs'!$N$2),H23,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I23*0.45),'BasicMeter10A61 5 inch'!I23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I23,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q22,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-10-SS",{"$error":"#VALUE!"},"1/4-10-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E23,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I24*0.45),'BasicMeter10A61 5 inch'!I24+0.000001>'Modified Inputs'!$N$2),H24,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I24*0.45),'BasicMeter10A61 5 inch'!I24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I24,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q23,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C24*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-10-CA",{"$error":"#VALUE!"},"1/4-10-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E24,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I25*0.45),'BasicMeter10A61 5 inch'!I25+0.000001>'Modified Inputs'!$N$2),H25,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I25*0.45),'BasicMeter10A61 5 inch'!I25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I25,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q24,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C25*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-10-TA",{"$error":"#VALUE!"},"1/4-10-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E25,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I26*0.45),'BasicMeter10A61 5 inch'!I26+0.000001>'Modified Inputs'!$N$2),H26,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I26*0.45),'BasicMeter10A61 5 inch'!I26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I26,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q25,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C26*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-10-BG",{"$error":"#VALUE!"},"1/4-10-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E26,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I27*0.45),'BasicMeter10A61 5 inch'!I27+0.000001>'Modified Inputs'!$N$2),H27,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I27*0.45),'BasicMeter10A61 5 inch'!I27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I27,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q26,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C27*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-12-SA",{"$error":"#VALUE!"},"1/8-12-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E27,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I28*0.45),'BasicMeter10A61 5 inch'!I28+0.000001>'Modified Inputs'!$N$2),H28,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I28*0.45),'BasicMeter10A61 5 inch'!I28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I28,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q27,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C28*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-12-SS",{"$error":"#VALUE!"},"1/8-12-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E28,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I29*0.45),'BasicMeter10A61 5 inch'!I29+0.000001>'Modified Inputs'!$N$2),H29,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I29*0.45),'BasicMeter10A61 5 inch'!I29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I29,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q28,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C29*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-12-CA",{"$error":"#VALUE!"},"1/8-12-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E29,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I30*0.45),'BasicMeter10A61 5 inch'!I30+0.000001>'Modified Inputs'!$N$2),H30,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I30*0.45),'BasicMeter10A61 5 inch'!I30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I30,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q29,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C30*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-12-TA",{"$error":"#VALUE!"},"1/8-12-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E30,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I31*0.45),'BasicMeter10A61 5 inch'!I31+0.000001>'Modified Inputs'!$N$2),H31,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I31*0.45),'BasicMeter10A61 5 inch'!I31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I31,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q30,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C31*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-12-BG",{"$error":"#VALUE!"},"1/8-12-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E31,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I32*0.45),'BasicMeter10A61 5 inch'!I32+0.000001>'Modified Inputs'!$N$2),H32,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I32*0.45),'BasicMeter10A61 5 inch'!I32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I32,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q31,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C32*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-08-SA",{"$error":"#VALUE!"},"1/8-08-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E32,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I33*0.45),'BasicMeter10A61 5 inch'!I33+0.000001>'Modified Inputs'!$N$2),H33,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I33*0.45),'BasicMeter10A61 5 inch'!I33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I33,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q32,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C33*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-08-SS",{"$error":"#VALUE!"},"1/8-08-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E33,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I34*0.45),'BasicMeter10A61 5 inch'!I34+0.000001>'Modified Inputs'!$N$2),H34,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I34*0.45),'BasicMeter10A61 5 inch'!I34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I34,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q33,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C34*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-08-CA",{"$error":"#VALUE!"},"1/8-08-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E34,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I35*0.45),'BasicMeter10A61 5 inch'!I35+0.000001>'Modified Inputs'!$N$2),H35,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I35*0.45),'BasicMeter10A61 5 inch'!I35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I35,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q34,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C35*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-08-TA",{"$error":"#VALUE!"},"1/8-08-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E35,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I36*0.45),'BasicMeter10A61 5 inch'!I36+0.000001>'Modified Inputs'!$N$2),H36,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I36*0.45),'BasicMeter10A61 5 inch'!I36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I36,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q35,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C36*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-08-BG",{"$error":"#VALUE!"},"1/8-08-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E36,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I37*0.45),'BasicMeter10A61 5 inch'!I37+0.000001>'Modified Inputs'!$N$2),H37,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I37*0.45),'BasicMeter10A61 5 inch'!I37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I37,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q36,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C37*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-12-SA",{"$error":"#VALUE!"},"1/16-12-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E37,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I38*0.45),'BasicMeter10A61 5 inch'!I38+0.000001>'Modified Inputs'!$N$2),H38,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I38*0.45),'BasicMeter10A61 5 inch'!I38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I38,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q37,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C38*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-12-SS",{"$error":"#VALUE!"},"1/16-12-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E38,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I39*0.45),'BasicMeter10A61 5 inch'!I39+0.000001>'Modified Inputs'!$N$2),H39,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I39*0.45),'BasicMeter10A61 5 inch'!I39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I39,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q38,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C39*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-12-CA",{"$error":"#VALUE!"},"1/16-12-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E39,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I40*0.45),'BasicMeter10A61 5 inch'!I40+0.000001>'Modified Inputs'!$N$2),H40,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I40*0.45),'BasicMeter10A61 5 inch'!I40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I40,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q39,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C40*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-12-TA",{"$error":"#VALUE!"},"1/16-12-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E40,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I41*0.45),'BasicMeter10A61 5 inch'!I41+0.000001>'Modified Inputs'!$N$2),H41,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I41*0.45),'BasicMeter10A61 5 inch'!I41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I41,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q40,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C41*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-12-BG",{"$error":"#VALUE!"},"1/16-12-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E41,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I42*0.45),'BasicMeter10A61 5 inch'!I42+0.000001>'Modified Inputs'!$N$2),H42,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I42*0.45),'BasicMeter10A61 5 inch'!I42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I42,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q41,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C42*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-16-SA",{"$error":"#VALUE!"},"1/16-16-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E42,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I43*0.45),'BasicMeter10A61 5 inch'!I43+0.000001>'Modified Inputs'!$N$2),H43,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I43*0.45),'BasicMeter10A61 5 inch'!I43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I43,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q42,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C43*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-16-SS",{"$error":"#VALUE!"},"1/16-16-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E43,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I44*0.45),'BasicMeter10A61 5 inch'!I44+0.000001>'Modified Inputs'!$N$2),H44,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I44*0.45),'BasicMeter10A61 5 inch'!I44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I44,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q43,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C44*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-16-CA",{"$error":"#VALUE!"},"1/16-16-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E44,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I45*0.45),'BasicMeter10A61 5 inch'!I45+0.000001>'Modified Inputs'!$N$2),H45,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I45*0.45),'BasicMeter10A61 5 inch'!I45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I45,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q44,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C45*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-16-TA",{"$error":"#VALUE!"},"1/16-16-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E45,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I46*0.45),'BasicMeter10A61 5 inch'!I46+0.000001>'Modified Inputs'!$N$2),H46,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I46*0.45),'BasicMeter10A61 5 inch'!I46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I46,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q45,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C46*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-16-BG",{"$error":"#VALUE!"},"1/16-16-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E46,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I47*0.45),'BasicMeter10A61 5 inch'!I47+0.000001>'Modified Inputs'!$N$2),H47,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I47*0.45),'BasicMeter10A61 5 inch'!I47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I47,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q46,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C47*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-20-SA",{"$error":"#VALUE!"},"1/16-20-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E47,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I48*0.45),'BasicMeter10A61 5 inch'!I48+0.000001>'Modified Inputs'!$N$2),H48,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I48*0.45),'BasicMeter10A61 5 inch'!I48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I48,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q47,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C48*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-20-SS",{"$error":"#VALUE!"},"1/16-20-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E48,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I49*0.45),'BasicMeter10A61 5 inch'!I49+0.000001>'Modified Inputs'!$N$2),H49,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I49*0.45),'BasicMeter10A61 5 inch'!I49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I49,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q48,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C49*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-20-CA",{"$error":"#VALUE!"},"1/16-20-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E49,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I50*0.45),'BasicMeter10A61 5 inch'!I50+0.000001>'Modified Inputs'!$N$2),H50,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I50*0.45),'BasicMeter10A61 5 inch'!I50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I50,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q49,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C50*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-20-TA",{"$error":"#VALUE!"},"1/16-20-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E50,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I51*0.45),'BasicMeter10A61 5 inch'!I51+0.000001>'Modified Inputs'!$N$2),H51,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I51*0.45),'BasicMeter10A61 5 inch'!I51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I51,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q50,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C51*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/16-20-BG",{"$error":"#VALUE!"},"1/16-20-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E51,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I52*0.45),'BasicMeter10A61 5 inch'!I52+0.000001>'Modified Inputs'!$N$2),H52,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I52*0.45),'BasicMeter10A61 5 inch'!I52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I52,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q51,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C52*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-25-SA",{"$error":"#VALUE!"},"1/8-25-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E52,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I53*0.45),'BasicMeter10A61 5 inch'!I53+0.000001>'Modified Inputs'!$N$2),H53,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I53*0.45),'BasicMeter10A61 5 inch'!I53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I53,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q52,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C53*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-25-SS",{"$error":"#VALUE!"},"1/8-25-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E53,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I54*0.45),'BasicMeter10A61 5 inch'!I54+0.000001>'Modified Inputs'!$N$2),H54,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I54*0.45),'BasicMeter10A61 5 inch'!I54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I54,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q53,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C54*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-25-CA",{"$error":"#VALUE!"},"1/8-25-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E54,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I55*0.45),'BasicMeter10A61 5 inch'!I55+0.000001>'Modified Inputs'!$N$2),H55,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I55*0.45),'BasicMeter10A61 5 inch'!I55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I55,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q54,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C55*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-25-TA",{"$error":"#VALUE!"},"1/8-25-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E55,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I56*0.45),'BasicMeter10A61 5 inch'!I56+0.000001>'Modified Inputs'!$N$2),H56,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I56*0.45),'BasicMeter10A61 5 inch'!I56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I56,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q55,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C56*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-25-BG",{"$error":"#VALUE!"},"1/8-25-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E56,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I57*0.45),'BasicMeter10A61 5 inch'!I57+0.000001>'Modified Inputs'!$N$2),H57,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I57*0.45),'BasicMeter10A61 5 inch'!I57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I57,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q56,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C57*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-20-SA",{"$error":"#VALUE!"},"1/8-20-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E57,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I58*0.45),'BasicMeter10A61 5 inch'!I58+0.000001>'Modified Inputs'!$N$2),H58,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I58*0.45),'BasicMeter10A61 5 inch'!I58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I58,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q57,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C58*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-20-SS",{"$error":"#VALUE!"},"1/8-20-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E58,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I59*0.45),'BasicMeter10A61 5 inch'!I59+0.000001>'Modified Inputs'!$N$2),H59,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I59*0.45),'BasicMeter10A61 5 inch'!I59+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I59,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q58,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C59*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-20-CA",{"$error":"#VALUE!"},"1/8-20-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E59,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I60*0.45),'BasicMeter10A61 5 inch'!I60+0.000001>'Modified Inputs'!$N$2),H60,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I60*0.45),'BasicMeter10A61 5 inch'!I60+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I60,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q59,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C60*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-20-TA",{"$error":"#VALUE!"},"1/8-20-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E60,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I61*0.45),'BasicMeter10A61 5 inch'!I61+0.000001>'Modified Inputs'!$N$2),H61,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I61*0.45),'BasicMeter10A61 5 inch'!I61+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I61,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q60,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C61*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-20-BG",{"$error":"#VALUE!"},"1/8-20-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E61,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I62*0.45),'BasicMeter10A61 5 inch'!I62+0.000001>'Modified Inputs'!$N$2),H62,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I62*0.45),'BasicMeter10A61 5 inch'!I62+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I62,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q61,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C62*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-16-SA",{"$error":"#VALUE!"},"1/8-16-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E62,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I63*0.45),'BasicMeter10A61 5 inch'!I63+0.000001>'Modified Inputs'!$N$2),H63,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I63*0.45),'BasicMeter10A61 5 inch'!I63+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I63,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q62,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C63*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-16-SS",{"$error":"#VALUE!"},"1/8-16-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E63,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I64*0.45),'BasicMeter10A61 5 inch'!I64+0.000001>'Modified Inputs'!$N$2),H64,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I64*0.45),'BasicMeter10A61 5 inch'!I64+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I64,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q63,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C64*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-16-CA",{"$error":"#VALUE!"},"1/8-16-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E64,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I65*0.45),'BasicMeter10A61 5 inch'!I65+0.000001>'Modified Inputs'!$N$2),H65,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I65*0.45),'BasicMeter10A61 5 inch'!I65+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I65,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q64,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C65*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-16-TA",{"$error":"#VALUE!"},"1/8-16-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E65,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I66*0.45),'BasicMeter10A61 5 inch'!I66+0.000001>'Modified Inputs'!$N$2),H66,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I66*0.45),'BasicMeter10A61 5 inch'!I66+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I66,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q65,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C66*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/8-16-BG",{"$error":"#VALUE!"},"1/8-16-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E66,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I67*0.45),'BasicMeter10A61 5 inch'!I67+0.000001>'Modified Inputs'!$N$2),H67,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I67*0.45),'BasicMeter10A61 5 inch'!I67+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I67,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q66,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C67*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-40-G-6-BG",{"$error":"#VALUE!"},"1/4-40-G-6-BG",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E67,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I68*0.45),'BasicMeter10A61 5 inch'!I68+0.000001>'Modified Inputs'!$N$2),H68,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I68*0.45),'BasicMeter10A61 5 inch'!I68+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I68,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q67,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C68*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-40-G-6-SA",{"$f":"IF(G69<0.00000099999,ROUND(G69,7),\nIF(G69<0.0000099999,ROUND(G69,6),\nIF(G69<0.000099999,ROUND(G69,5),\nIF(G69<0.00099999,ROUND(G69,4),\nIF(G69<0.0099999,ROUND(G69,3),\nIF(G69<0.099999,ROUND(G69,2),\nIF(G69<0.99999,ROUND(G69,2),\nIF(G69<9.999,ROUND(G69,2),\nIF(G69<99.99,ROUND(G69,1),\nIF(G69<999.99,ROUND(G69,0),\nIF(G69<9999.99,ROUND(G69,-1),\nIF(G69<99999,ROUND(G69,-2),ROUND(G69,2)))))))))))))","v":{"$error":"#VALUE!"}},"1/4-40-G-6-SA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E68,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I69*0.45),'BasicMeter10A61 5 inch'!I69+0.000001>'Modified Inputs'!$N$2),H69,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I69*0.45),'BasicMeter10A61 5 inch'!I69+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I69,0),0)","v":0},{"$f":"LEFT(P69,4)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(Q69,$I$4:$J$72,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($N$4:$N$72<Q68,$N$4:$N$72))","v":0},{"$f":"VLOOKUP(P69,$J$4:$K$72,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C69*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-40-G-6-SS",{"$error":"#VALUE!"},"1/4-40-G-6-SS",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E69,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I70*0.45),'BasicMeter10A61 5 inch'!I70+0.000001>'Modified Inputs'!$N$2),H70,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I70*0.45),'BasicMeter10A61 5 inch'!I70+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I70,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q69,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C70*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-40-G-6-CA",{"$error":"#VALUE!"},"1/4-40-G-6-CA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E70,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I71*0.45),'BasicMeter10A61 5 inch'!I71+0.000001>'Modified Inputs'!$N$2),H71,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I71*0.45),'BasicMeter10A61 5 inch'!I71+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I71,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q70,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!C71*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},"1/4-40-G-6-TA",{"$error":"#VALUE!"},"1/4-40-G-6-TA",{"$f":"IF(LEFT('10A61 5\" + 6\" Results'!E71,1)=\" \",\"viscosity\",\"\")","v":{"$error":"#DIV/0!"}},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I72*0.45),'BasicMeter10A61 5 inch'!I72+0.000001>'Modified Inputs'!$N$2),H72,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A61 5 inch'!I72*0.45),'BasicMeter10A61 5 inch'!I72+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A61 5 inch'!I72,0),0)","v":0},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($N$4:$N$72<Q71,$N$4:$N$72))","v":0},{"$error":"#N/A"},{"$error":"#N/A"}]

{"sheet":"BasicMeter10A4 Standard","index":28,"n_rows":58,"n_cols":42,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,4,1,10],[2,28,2,29]]}
[]
[null,"Current Tab","Current Step",null,"Standard Floats",null,null,null,null,null,null,null,null,null,null,"10A4 All",null,null,null,null,"10A4\" Range Limit",null,null,"10A4\" Range Limit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,"Water GPM","Air SCFM","Tube","Float (SST)","VIC","psia Critical","Pressure Drop (in. H2O)",null,null,"Liquid + Gas",null,"Tube/Float","Max Rounded","Tube/Float","Viscosity / Pressure Warning","size","Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded","Viscosity / Pressure Warning",null,null,"Final Standard"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A",0.26700000000000002,1.1000000000000001,"FP-1/2-17-G-10","1/2-GUSVT-40A",2.9,5.5,1.2,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E4/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G4,\"                                                                                                  \",H4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A"},{"$f":"IF(N4<0.00000099999,ROUND(N4,7),\nIF(N4<0.0000099999,ROUND(N4,6),\nIF(N4<0.000099999,ROUND(N4,5),\nIF(N4<0.00099999,ROUND(N4,4),\nIF(N4<0.0099999,ROUND(N4,3),\nIF(N4<0.099999,ROUND(N4,2),\nIF(N4<0.99999,ROUND(N4,2),\nIF(N4<9.999,ROUND(N4,2),\nIF(N4<99.99,ROUND(N4,1),\nIF(N4<999.99,ROUND(N4,0),\nIF(N4<9999.99,ROUND(N4,-1),\nIF(N4<99999,ROUND(N4,-2),ROUND(N4,2)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"P4","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I4),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J4),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q4*0.45),'BasicMeter10A4 Standard'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q4*0.45),'BasicMeter10A4 Standard'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(Y4,$Q$4:$R$57,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($V$4:$V$58>0,V4:V58))","v":0},{"$f":"VLOOKUP(X4,$R$4:$S$58,2,FALSE)","v":{"$error":"#N/A"}},null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A",0.32800000000000001,1.35,"FP-1/2-21-G-10","1/2-GUSVT-40A",2.9,3.5,1.4,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G5,\"                                                                                                  \",H5)","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A"},{"$f":"IF(N5<0.00000099999,ROUND(N5,7),\nIF(N5<0.0000099999,ROUND(N5,6),\nIF(N5<0.000099999,ROUND(N5,5),\nIF(N5<0.00099999,ROUND(N5,4),\nIF(N5<0.0099999,ROUND(N5,3),\nIF(N5<0.099999,ROUND(N5,2),\nIF(N5<0.99999,ROUND(N5,2),\nIF(N5<9.999,ROUND(N5,2),\nIF(N5<99.99,ROUND(N5,1),\nIF(N5<999.99,ROUND(N5,0),\nIF(N5<9999.99,ROUND(N5,-1),\nIF(N5<99999,ROUND(N5,-2),ROUND(N5,2)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"P5","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I5),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J5),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q5*0.45),'BasicMeter10A4 Standard'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q5*0.45),'BasicMeter10A4 Standard'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(Y5,$Q$4:$R$57,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($V$4:$V$58<Y4,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$X$33,1/0),\nIFERROR(IF($Z$32=\"\",$X$32,1/0),\nIFERROR(IF($Z$31=\"\",$X$31,1/0),\nIFERROR(IF($Z$30=\"\",$X$30,1/0),\nIFERROR(IF($Z$29=\"\",$X$29,1/0),\nIFERROR(IF($Z$28=\"\",$X$28,1/0),\nIFERROR(IF($Z$27=\"\",$X$27,1/0),\nIFERROR(IF($Z$26=\"\",$X$26,1/0),\nIFERROR(IF($Z$25=\"\",$X$25,1/0),\nIFERROR(IF($Z$24=\"\",$X$24,1/0),\nIFERROR(IF($Z$23=\"\",$X$23,1/0),\nIFERROR(IF($Z$22=\"\",$X$22,1/0),\nIFERROR(IF($Z$21=\"\",$X$21,1/0),\nIFERROR(IF($Z$20=\"\",$X$20,1/0),\nIFERROR(IF($Z$19=\"\",$X$19,1/0),\nIFERROR(IF($Z$18=\"\",$X$18,1/0),\nIFERROR(IF($Z$17=\"\",$X$17,1/0),\nIFERROR(IF($Z$16=\"\",$X$16,1/0),\nIFERROR(IF($Z$15=\"\",$X$15,1/0),\nIFERROR(IF($Z$14=\"\",$X$14,1/0),\nIFERROR(IF($Z$13=\"\",$X$13,1/0),\nIFERROR(IF($Z$12=\"\",$X$12,1/0),\nIFERROR(IF($Z$11=\"\",$X$11,1/0),\nIFERROR(IF($Z$10=\"\",$X$10,1/0),\nIFERROR(IF($Z$9=\"\",$X$9,1/0),\nIFERROR(IF($Z$8=\"\",$X$8,1/0),\nIFERROR(IF($Z$7=\"\",$X$7,1/0),\nIFERROR(IF($Z$6=\"\",$X$6,1/0),\nIFERROR(IF($Z$5=\"\",$X$5,1/0),\nIFERROR(IF($Z$4=\"\",$X$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AC5,$X$4:$Y$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(IF(AND(AC5=\"none\",NOT(Z4=\"\")),Z4,\"\"),\"sizing\")","v":"sizing"},null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A",0.442,1.82,"FP-1/2-27-G-10","1/2-GUSVT-40A",2.9,2.7,2,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I6),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J6),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q6*0.45),'BasicMeter10A4 Standard'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q6*0.45),'BasicMeter10A4 Standard'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y5,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A",0.48,1.92,"FP-1/2-17-G-10","1/2-GSVT-45A",5.0999999999999996,17.899999999999999,3.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A",{"$error":"#VALUE!"},"FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I7),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J7),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q7*0.45),'BasicMeter10A4 Standard'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q7*0.45),'BasicMeter10A4 Standard'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y6,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A",0.6,2.4700000000000002,"FP-1/2-21-G-10","1/2-GSVT-45A",5.0999999999999996,11.5,4.5999999999999996,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I8),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J8),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q8*0.45),'BasicMeter10A4 Standard'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q8*0.45),'BasicMeter10A4 Standard'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y7,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A",0.61899999999999999,2.5499999999999998,"FP-1/2-35-G-10","1/2-GUSVT-40A",2.9,2,3.1,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I9),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J9),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q9*0.45),'BasicMeter10A4 Standard'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q9*0.45),'BasicMeter10A4 Standard'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y8,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A",0.67,2.76,"FP-1/2-17-G-10","1/2-GSVT-44A",7.1,33.4,6.4,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A",{"$error":"#VALUE!"},"FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I10),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J10),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q10*0.45),'BasicMeter10A4 Standard'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q10*0.45),'BasicMeter10A4 Standard'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y9,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A",0.69,2.85,"FP-1/2-17-G-10","1/2-GSVT-48A",7.6,39,7.3,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A",{"$error":"#VALUE!"},"FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I11),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J11),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q11*0.45),'BasicMeter10A4 Standard'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q11*0.45),'BasicMeter10A4 Standard'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y10,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A",0.81,3.35,"FP-1/2-27-G-10","1/2-GSVT-45A",4.0999999999999996,8.4,6.8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I12),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J12),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q12*0.45),'BasicMeter10A4 Standard'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q12*0.45),'BasicMeter10A4 Standard'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y11,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A",0.83,3.42,"FP-1/2-21-G-10","1/2-GSVT-44A",7.1,33.799999999999997,7.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I13),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J13),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q13*0.45),'BasicMeter10A4 Standard'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q13*0.45),'BasicMeter10A4 Standard'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y12,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A",0.88,3.62,"FP-1/2-21-G-10","1/2-GSVT-48A",7.6,24.6,8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I14),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J14),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q14*0.45),'BasicMeter10A4 Standard'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q14*0.45),'BasicMeter10A4 Standard'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y13,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A",0.88500000000000001,3.65,"FP-1/2-17-G-10","1/2-GNSVT-48A",1.1000000000000001,19.8,8.1999999999999993,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E15/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A",{"$error":"#VALUE!"},"FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I15),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J15),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q15*0.45),'BasicMeter10A4 Standard'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q15*0.45),'BasicMeter10A4 Standard'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y14,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A",1.1000000000000001,4.5199999999999996,"FP-1/2-21-G-10","1/2-GNSVT-48A",1.1000000000000001,20,9.9,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E16/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I16),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J16),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q16*0.45),'BasicMeter10A4 Standard'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q16*0.45),'BasicMeter10A4 Standard'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y15,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A",1.1200000000000001,4.5999999999999996,"FP-1/2-27-G-10","1/2-GSVT-44A",7.1,16.2,12.3,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E17/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I17),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J17),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q17*0.45),'BasicMeter10A4 Standard'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q17*0.45),'BasicMeter10A4 Standard'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y16,$V$4:$V$58))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A",1.1499999999999999,4.74,"FP-1/2-35-G-10","1/2-GSVT-45A",5.0999999999999996,8.5,8.1999999999999993,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E18/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I18),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J18),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q18*0.45),'BasicMeter10A4 Standard'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q18*0.45),'BasicMeter10A4 Standard'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y17,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A",1.19,4.9000000000000004,"FP-1/2-27-G-10","1/2-GSVT-48A",7.6,18.600000000000001,13.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E19/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I19),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J19),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q19*0.45),'BasicMeter10A4 Standard'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q19*0.45),'BasicMeter10A4 Standard'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y18,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A",1.44,5.93,"FP-1/2-27-G-10","1/2-GNSVT-48A",1.1000000000000001,16.5,15.8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E20/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I20),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J20),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q20*0.45),'BasicMeter10A4 Standard'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q20*0.45),'BasicMeter10A4 Standard'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y19,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A",1.56,6.43,"FP-1/2-35-G-10","1/2-GSVT-44A",7.1,16.5,14.8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E21/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I21),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J21),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q21*0.45),'BasicMeter10A4 Standard'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q21*0.45),'BasicMeter10A4 Standard'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y20,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A",1.66,6.85,"FP-1/2-35-G-10","1/2-GSVT-48A",7.6,18.8,17.2,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E22/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I22),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J22),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q22*0.45),'BasicMeter10A4 Standard'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q22*0.45),'BasicMeter10A4 Standard'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y21,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A",2,8.24,"FP-1/2-50-G-9","1/2-GSVT-45A",5.0999999999999996,4,12,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E23/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I23),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J23),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q23*0.45),'BasicMeter10A4 Standard'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q23*0.45),'BasicMeter10A4 Standard'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y22,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A",2.76,11.4,"FP-1/2-50-G-9","1/2-GSVT-44A",7.1,7.7,31,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E24/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I24),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J24),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q24*0.45),'BasicMeter10A4 Standard'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q24*0.45),'BasicMeter10A4 Standard'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y23,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A",2.9,12,"FP-1/2-50-G-9","1/2-GSVT-48A",7.6,8.9,35.200000000000003,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E25/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I25),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J25),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q25*0.45),'BasicMeter10A4 Standard'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q25*0.45),'BasicMeter10A4 Standard'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y24,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A",3.52,14.5,"FP-1/2-50-G-9","1/2-GNSVT-48A",1.1000000000000001,8.8000000000000007,52,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E26/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I26),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J26),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q26*0.45),'BasicMeter10A4 Standard'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q26*0.45),'BasicMeter10A4 Standard'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y25,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A",1.96,8.1,"FP-3/4-21-G-10","3/4-GSVGT-54A",10.4,13.9,5.3,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E27/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I27),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J27),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q27*0.45),'BasicMeter10A4 Standard'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q27*0.45),'BasicMeter10A4 Standard'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y26,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A",2.4900000000000002,10.199999999999999,"FP-3/4-21-G-10","3/4-GNSVGT-54A",1.6,13.9,6.8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E28/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I28),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J28),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q28*0.45),'BasicMeter10A4 Standard'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q28*0.45),'BasicMeter10A4 Standard'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y27,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A",2.66,11,"FP-3/4-21-G-10","3/4-GSVGT-59A",14.1,28.7,7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E29/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I29),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J29),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q29*0.45),'BasicMeter10A4 Standard'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q29*0.45),'BasicMeter10A4 Standard'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y28,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A",2.7,11.1,"FP-3/4-27-G-10","3/4-GSVGT-54A",10.4,9.6,7.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E30/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I30),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J30),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q30*0.45),'BasicMeter10A4 Standard'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q30*0.45),'BasicMeter10A4 Standard'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y29,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A",3.37,13.9,"FP-3/4-21-G-10","3/4-GNSVGT-59A",2.1,25.3,11.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E31/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I31),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J31),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q31*0.45),'BasicMeter10A4 Standard'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q31*0.45),'BasicMeter10A4 Standard'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y30,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A",3.55,14.6,"FP-3/4-27-G-10","3/4-GNSVGT-54A",1.6,9.6,11.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E32/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I32),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J32),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q32*0.45),'BasicMeter10A4 Standard'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q32*0.45),'BasicMeter10A4 Standard'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y31,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A",3.67,15.1,"FP-3/4-27-G-10","3/4-GSVGT-59A",14,19.8,13.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E33/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I33),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J33),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q33*0.45),'BasicMeter10A4 Standard'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q33*0.45),'BasicMeter10A4 Standard'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y32,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A",4.8,19.8,"FP-3/4-27-G-10","3/4-GNSVGT-59A",2.1,19.8,20.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E34/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I34),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J34),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q34*0.45),'BasicMeter10A4 Standard'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q34*0.45),'BasicMeter10A4 Standard'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y33,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GSVGT-64A",4.25,17.5,"FP-1-27-G-10","1-GSVGT-64A",14.8,11.5,12.9,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E35/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GSVGT-64A",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GSVGT-64A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I35),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J35),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q35*0.45),'BasicMeter10A4 Standard'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q35*0.45),'BasicMeter10A4 Standard'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y34,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GSVGT-68A",4.82,19.899999999999999,"FP-1-27-G-10","1-GSVGT-68A",16.899999999999999,15.6,18.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E36/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GSVGT-68A",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GSVGT-68A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I36),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J36),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q36*0.45),'BasicMeter10A4 Standard'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q36*0.45),'BasicMeter10A4 Standard'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y35,$V$4:$V$58))","v":0},{"$f":"VLOOKUP(X36,$R$4:$S$58,2,FALSE)","v":{"$error":"#N/A"}}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-64A",5.63,23.2,"FP-1-27-G-10","1-GNSVGT-64A",2.2000000000000002,11.3,20.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E37/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GNSVGT-64A",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GNSVGT-64A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I37),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J37),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q37*0.45),'BasicMeter10A4 Standard'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q37*0.45),'BasicMeter10A4 Standard'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y36,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-64A",6,24.7,"FP-1-35-G-10","1-GSVGT-64A",14.8,6.8,24.6,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E38/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVGT-64A",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVGT-64A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I38),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J38),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q38*0.45),'BasicMeter10A4 Standard'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q38*0.45),'BasicMeter10A4 Standard'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y37,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-68A",6.46,26.6,"FP-1-27-G-10","1-GNSVGT-68A",2.5,15.6,32.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E39/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GNSVGT-68A",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GNSVGT-68A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I39),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J39),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q39*0.45),'BasicMeter10A4 Standard'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q39*0.45),'BasicMeter10A4 Standard'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y38,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-68A",6.8,28,"FP-1-35-G-10","1-GSVGT-68A",16.899999999999999,8.9,37,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E40/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVGT-68A",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVGT-68A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I40),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J40),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q40*0.45),'BasicMeter10A4 Standard'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q40*0.45),'BasicMeter10A4 Standard'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y39,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-69A",7.62,31.4,"FP-1-27-G-10","1-GNSVGT-69A",1.5,22.2,75,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E41/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GNSVGT-69A",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GNSVGT-69A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I41),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J41),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q41*0.45),'BasicMeter10A4 Standard'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q41*0.45),'BasicMeter10A4 Standard'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y40,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-64A",7.84,32.4,"FP-1-35-G-10","1-GNSVGT-64A",2.2000000000000002,6.8,37.700000000000003,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E42/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GNSVGT-64A",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GNSVGT-64A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I42),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J42),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q42*0.45),'BasicMeter10A4 Standard'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q42*0.45),'BasicMeter10A4 Standard'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y41,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-68A",9,37,"FP-1-35-G-10","1-GNSVGT-68A",2.5,8.9,62.8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E43/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GNSVGT-68A",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GNSVGT-68A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I43),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J43),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q43*0.45),'BasicMeter10A4 Standard'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q43*0.45),'BasicMeter10A4 Standard'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y42,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-69A",9.5,39.200000000000003,"FP-1-35-G-10","1-GSVGT-69A",8.5,13.4,65.3,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E44/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVGT-69A",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVGT-69A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I44),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J44),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q44*0.45),'BasicMeter10A4 Standard'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q44*0.45),'BasicMeter10A4 Standard'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y43,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-69A",11,45.3,"FP-1-35-G-10","1-GNSVGT-69A",1.5,13.4,112,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E45/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GNSVGT-69A",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GNSVGT-69A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I45),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J45),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q45*0.45),'BasicMeter10A4 Standard'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q45*0.45),'BasicMeter10A4 Standard'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y44,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A",13.2,54.4,"FP-1-1/2-27-G-10","1-1/2-GSVGT-87A",27.6,15.4,9.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E46/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I46),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J46),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q46*0.45),'BasicMeter10A4 Standard'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q46*0.45),'BasicMeter10A4 Standard'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y45,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A",14.6,60,"FP-1-1/2-27-G-10","1-1/2-GSVGT-86A",31,22,13.5,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E47/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I47),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J47),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q47*0.45),'BasicMeter10A4 Standard'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q47*0.45),'BasicMeter10A4 Standard'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y46,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A",17.600000000000001,72,"FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A",4.2,15.4,12.8,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E48/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I48),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J48),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q48*0.45),'BasicMeter10A4 Standard'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q48*0.45),'BasicMeter10A4 Standard'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y47,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A",18.600000000000001,76.5,"FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A",4.8,22,15.2,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E49/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I49),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J49),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q49*0.45),'BasicMeter10A4 Standard'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q49*0.45),'BasicMeter10A4 Standard'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y48,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GSVGT-97A",24,99,"FP-2-27-G-10","2-GSVGT-97A",26.5,16.399999999999999,24,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E50/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GSVGT-97A",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GSVGT-97A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I50),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J50),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q50*0.45),'BasicMeter10A4 Standard'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q50*0.45),'BasicMeter10A4 Standard'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y49,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GSVGT-98A",30,123.8,"FP-2-27-G-10","2-GSVGT-98A",18.5,21.2,34,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E51/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GSVGT-98A",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GSVGT-98A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I51),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J51),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q51*0.45),'BasicMeter10A4 Standard'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q51*0.45),'BasicMeter10A4 Standard'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y50,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVGT-97A",32,132,"FP-2-27-G-10","2-GNSVGT-97A",3,16.399999999999999,32,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E52/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GNSVGT-97A",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GNSVGT-97A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I52),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J52),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q52*0.45),'BasicMeter10A4 Standard'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q52*0.45),'BasicMeter10A4 Standard'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y51,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVGT-98A",36.1,149,"FP-2-27-G-10","2-GNSVGT-98A",3.3,21.2,45,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E53/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GNSVGT-98A",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GNSVGT-98A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I53),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J53),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q53*0.45),'BasicMeter10A4 Standard'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q53*0.45),'BasicMeter10A4 Standard'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y52,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  BL-954",48,null,"FP-2-27-G-10","BL-954",2,null,70,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"\",\nIF('VA Sizing'!$C$3=\"Liquid\",E54/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":""},null,"FP-2-27-G-10                                                                                                  BL-954",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  BL-954",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I54),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J54),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q54*0.45),'BasicMeter10A4 Standard'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q54*0.45),'BasicMeter10A4 Standard'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y53,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  BL-953",60,null,"FP-2-27-G-10","BL-953",2,null,95,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"\",\nIF('VA Sizing'!$C$3=\"Liquid\",E55/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":""},null,"FP-2-27-G-10                                                                                                  BL-953",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  BL-953",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I55),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J55),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q55*0.45),'BasicMeter10A4 Standard'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q55*0.45),'BasicMeter10A4 Standard'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y54,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  BL-950",68,null,"FP-2-27-G-10","BL-950",2,null,110,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"\",\nIF('VA Sizing'!$C$3=\"Liquid\",E56/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":""},null,"FP-2-27-G-10                                                                                                  BL-950",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  BL-950",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I56),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J56),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q56*0.45),'BasicMeter10A4 Standard'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q56*0.45),'BasicMeter10A4 Standard'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y55,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  BL-951",90,null,"FP-2-27-G-10","BL-951",1,null,192.7,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"\",\nIF('VA Sizing'!$C$3=\"Liquid\",E57/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))))","v":""},null,"FP-2-27-G-10                                                                                                  BL-951",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  BL-951",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I57),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J57),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q57*0.45),'BasicMeter10A4 Standard'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q57*0.45),'BasicMeter10A4 Standard'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y56,$V$4:$V$58))","v":0},{"$error":"#N/A"}]
[null,null,null,null,0,null,null,null,0,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E58/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I58),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J58),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q58*0.45),'BasicMeter10A4 Standard'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Standard'!Q58*0.45),'BasicMeter10A4 Standard'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Standard'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$58<Y57,$V$4:$V$58))","v":0},{"$error":"#N/A"}]

{"sheet":"BasicMeter10A4 Low Pressure Dro","index":29,"n_rows":58,"n_cols":42,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,4,1,10],[2,28,2,29]]}
[]
[null,"Current Tab","Current Step",null,"Low Pressure Drop",null,null,null,null,null,null,null,null,null,null,"10A4 All",null,null,null,null,"10A4\" Range Limit",null,null,"10A4\" Range Limit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,"Water GPM","Air SCFM","Tube","Float (SST)","VIC","psia Critical","Pressure Drop (in. H2O)",null,null,"Liquid + Gas",null,"Tube/Float","Max Rounded","Tube/Float","Viscosity / Pressure Warning","size","Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded","Viscosity / Pressure Warning",null,null,"Final Standard"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410",0.19800000000000001,0.8,"FP-1/2-17-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,0.53,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E4/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G4,\"                                                                                                  \",H4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410"},{"$f":"IF(N4<0.00000099999,ROUND(N4,7),\nIF(N4<0.0000099999,ROUND(N4,6),\nIF(N4<0.000099999,ROUND(N4,5),\nIF(N4<0.00099999,ROUND(N4,4),\nIF(N4<0.0099999,ROUND(N4,3),\nIF(N4<0.099999,ROUND(N4,2),\nIF(N4<0.99999,ROUND(N4,2),\nIF(N4<9.999,ROUND(N4,2),\nIF(N4<99.99,ROUND(N4,1),\nIF(N4<999.99,ROUND(N4,0),\nIF(N4<9999.99,ROUND(N4,-1),\nIF(N4<99999,ROUND(N4,-2),ROUND(N4,2)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"P4","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I4),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J4),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q4*0.45),'BasicMeter10A4 Low Pressure Dro'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q4*0.45),'BasicMeter10A4 Low Pressure Dro'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(Y4,$Q$4:$R$20,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($V$4:$V$20>0,V4:V20))","v":0},{"$f":"VLOOKUP(X4,$R$4:$S$20,2,FALSE)","v":{"$error":"#N/A"}},null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410",0.23799999999999999,0.98199999999999998,"FP-1/2-21-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,0.53,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G5,\"                                                                                                  \",H5)","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410"},{"$f":"IF(N5<0.00000099999,ROUND(N5,7),\nIF(N5<0.0000099999,ROUND(N5,6),\nIF(N5<0.000099999,ROUND(N5,5),\nIF(N5<0.00099999,ROUND(N5,4),\nIF(N5<0.0099999,ROUND(N5,3),\nIF(N5<0.099999,ROUND(N5,2),\nIF(N5<0.99999,ROUND(N5,2),\nIF(N5<9.999,ROUND(N5,2),\nIF(N5<99.99,ROUND(N5,1),\nIF(N5<999.99,ROUND(N5,0),\nIF(N5<9999.99,ROUND(N5,-1),\nIF(N5<99999,ROUND(N5,-2),ROUND(N5,2)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"P5","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I5),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J5),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q5*0.45),'BasicMeter10A4 Low Pressure Dro'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q5*0.45),'BasicMeter10A4 Low Pressure Dro'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(Y5,$Q$4:$R$20,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($V$4:$V$20<Y4,$V$4:$V$20))","v":0},{"$f":"VLOOKUP(X5,$R$4:$S$20,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$X$33,1/0),\nIFERROR(IF($Z$32=\"\",$X$32,1/0),\nIFERROR(IF($Z$31=\"\",$X$31,1/0),\nIFERROR(IF($Z$30=\"\",$X$30,1/0),\nIFERROR(IF($Z$29=\"\",$X$29,1/0),\nIFERROR(IF($Z$28=\"\",$X$28,1/0),\nIFERROR(IF($Z$27=\"\",$X$27,1/0),\nIFERROR(IF($Z$26=\"\",$X$26,1/0),\nIFERROR(IF($Z$25=\"\",$X$25,1/0),\nIFERROR(IF($Z$24=\"\",$X$24,1/0),\nIFERROR(IF($Z$23=\"\",$X$23,1/0),\nIFERROR(IF($Z$22=\"\",$X$22,1/0),\nIFERROR(IF($Z$21=\"\",$X$21,1/0),\nIFERROR(IF($Z$20=\"\",$X$20,1/0),\nIFERROR(IF($Z$19=\"\",$X$19,1/0),\nIFERROR(IF($Z$18=\"\",$X$18,1/0),\nIFERROR(IF($Z$17=\"\",$X$17,1/0),\nIFERROR(IF($Z$16=\"\",$X$16,1/0),\nIFERROR(IF($Z$15=\"\",$X$15,1/0),\nIFERROR(IF($Z$14=\"\",$X$14,1/0),\nIFERROR(IF($Z$13=\"\",$X$13,1/0),\nIFERROR(IF($Z$12=\"\",$X$12,1/0),\nIFERROR(IF($Z$11=\"\",$X$11,1/0),\nIFERROR(IF($Z$10=\"\",$X$10,1/0),\nIFERROR(IF($Z$9=\"\",$X$9,1/0),\nIFERROR(IF($Z$8=\"\",$X$8,1/0),\nIFERROR(IF($Z$7=\"\",$X$7,1/0),\nIFERROR(IF($Z$6=\"\",$X$6,1/0),\nIFERROR(IF($Z$5=\"\",$X$5,1/0),\nIFERROR(IF($Z$4=\"\",$X$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AC5,$X$4:$Y$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(IF(AND(AC5=\"none\",NOT(Z4=\"\")),Z4,\"\"),\"sizing\")","v":"sizing"},null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410",0.32400000000000001,1.339,"FP-1/2-27-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,0.57999999999999996,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I6),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J6),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q6*0.45),'BasicMeter10A4 Low Pressure Dro'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q6*0.45),'BasicMeter10A4 Low Pressure Dro'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y5,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410",0.436,1.796,"FP-1/2-35-G-10","1/2-GUSVT-410",2.2000000000000002,3.6,1,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I7),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J7),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q7*0.45),'BasicMeter10A4 Low Pressure Dro'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q7*0.45),'BasicMeter10A4 Low Pressure Dro'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y6,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410",0.82499999999999996,3.4,"FP-1/2-50-G-9","1/2-GUSVT-410",2.2000000000000002,3.6,2,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I8),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J8),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q8*0.45),'BasicMeter10A4 Low Pressure Dro'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q8*0.45),'BasicMeter10A4 Low Pressure Dro'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y7,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510",0.63300000000000001,2.62,"FP-3/4-21-G-10","3/4-GUSVT-510",3.3,3.1,0.6,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I9),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J9),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q9*0.45),'BasicMeter10A4 Low Pressure Dro'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q9*0.45),'BasicMeter10A4 Low Pressure Dro'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y8,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510",0.86,3.54,"FP-3/4-27-G-10","3/4-GUSVT-510",3.3,1.5,0.71,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I10),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J10),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q10*0.45),'BasicMeter10A4 Low Pressure Dro'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q10*0.45),'BasicMeter10A4 Low Pressure Dro'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y9,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GUSVT-611",1.2050000000000001,4.9800000000000004,"FP-1-27-G-10","1-GUSVT-611",4,1,1.28,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GUSVT-611",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GUSVT-611",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I11),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J11),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q11*0.45),'BasicMeter10A4 Low Pressure Dro'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q11*0.45),'BasicMeter10A4 Low Pressure Dro'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y10,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GUSVT-611",1.67,6.9,"FP-1-35-G-10","1-GUSVT-611",4,0.75,1.83,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GUSVT-611",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GUSVT-611",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I12),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J12),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q12*0.45),'BasicMeter10A4 Low Pressure Dro'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q12*0.45),'BasicMeter10A4 Low Pressure Dro'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y11,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GUSVT-610",2.58,10.7,"FP-1-27-G-10","1-GUSVT-610",8.6,4.5,5.47,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GUSVT-610",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GUSVT-610",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I13),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J13),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q13*0.45),'BasicMeter10A4 Low Pressure Dro'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q13*0.45),'BasicMeter10A4 Low Pressure Dro'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y12,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GUSVT-610",3.6,14.84,"FP-1-35-G-10","1-GUSVT-610",8.6,3.4,7.97,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GUSVT-610",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GUSVT-610",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I14),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J14),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q14*0.45),'BasicMeter10A4 Low Pressure Dro'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q14*0.45),'BasicMeter10A4 Low Pressure Dro'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y13,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867",2.4500000000000002,10.3,"FP-1-1/2-21-G-10","1-1/2-GUSVT-867",6.5,1,0.92,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E15/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867",{"$error":"#VALUE!"},"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I15),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J15),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q15*0.45),'BasicMeter10A4 Low Pressure Dro'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q15*0.45),'BasicMeter10A4 Low Pressure Dro'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y14,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867",3.33,13.8,"FP-1-1/2-27-G-10","1-1/2-GUSVT-867",6.5,1,1.24,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E16/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I16),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J16),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q16*0.45),'BasicMeter10A4 Low Pressure Dro'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q16*0.45),'BasicMeter10A4 Low Pressure Dro'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y15,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814",6.5,27,"FP-1-1/2-21-G-10","1-1/2-GUSVGT-814",16.2,6.8,5.75,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E17/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814",{"$error":"#VALUE!"},"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I17),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J17),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q17*0.45),'BasicMeter10A4 Low Pressure Dro'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q17*0.45),'BasicMeter10A4 Low Pressure Dro'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y16,$V$4:$V$20))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814",8.6999999999999993,36,"FP-1-1/2-27-G-10","1-1/2-GUSVGT-814",16.2,6.8,7.2,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E18/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I18),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J18),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q18*0.45),'BasicMeter10A4 Low Pressure Dro'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q18*0.45),'BasicMeter10A4 Low Pressure Dro'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y17,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GUSVT-913",5.54,22.9,"FP-2-27-G-10","2-GUSVT-913",8.9,1,1.65,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E19/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GUSVT-913",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GUSVT-913",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I19),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J19),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q19*0.45),'BasicMeter10A4 Low Pressure Dro'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q19*0.45),'BasicMeter10A4 Low Pressure Dro'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y18,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GUSVGT-914",13.75,56.7,"FP-2-27-G-10","2-GUSVGT-914",22,6.2,9,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E20/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GUSVGT-914",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GUSVGT-914",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I20),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J20),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q20*0.45),'BasicMeter10A4 Low Pressure Dro'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q20*0.45),'BasicMeter10A4 Low Pressure Dro'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y19,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E21/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I21),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J21),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q21*0.45),'BasicMeter10A4 Low Pressure Dro'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q21*0.45),'BasicMeter10A4 Low Pressure Dro'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y20,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E22/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I22),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J22),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q22*0.45),'BasicMeter10A4 Low Pressure Dro'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q22*0.45),'BasicMeter10A4 Low Pressure Dro'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y21,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E23/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I23),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J23),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q23*0.45),'BasicMeter10A4 Low Pressure Dro'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q23*0.45),'BasicMeter10A4 Low Pressure Dro'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y22,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E24/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I24),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J24),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q24*0.45),'BasicMeter10A4 Low Pressure Dro'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q24*0.45),'BasicMeter10A4 Low Pressure Dro'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y23,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E25/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I25),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J25),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q25*0.45),'BasicMeter10A4 Low Pressure Dro'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q25*0.45),'BasicMeter10A4 Low Pressure Dro'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y24,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E26/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I26),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J26),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q26*0.45),'BasicMeter10A4 Low Pressure Dro'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q26*0.45),'BasicMeter10A4 Low Pressure Dro'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y25,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E27/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I27),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J27),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q27*0.45),'BasicMeter10A4 Low Pressure Dro'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q27*0.45),'BasicMeter10A4 Low Pressure Dro'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y26,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E28/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I28),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J28),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q28*0.45),'BasicMeter10A4 Low Pressure Dro'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q28*0.45),'BasicMeter10A4 Low Pressure Dro'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y27,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E29/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I29),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J29),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q29*0.45),'BasicMeter10A4 Low Pressure Dro'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q29*0.45),'BasicMeter10A4 Low Pressure Dro'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y28,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E30/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I30),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J30),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q30*0.45),'BasicMeter10A4 Low Pressure Dro'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q30*0.45),'BasicMeter10A4 Low Pressure Dro'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y29,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E31/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I31),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J31),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q31*0.45),'BasicMeter10A4 Low Pressure Dro'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q31*0.45),'BasicMeter10A4 Low Pressure Dro'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y30,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E32/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I32),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J32),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q32*0.45),'BasicMeter10A4 Low Pressure Dro'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q32*0.45),'BasicMeter10A4 Low Pressure Dro'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y31,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E33/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I33),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J33),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q33*0.45),'BasicMeter10A4 Low Pressure Dro'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q33*0.45),'BasicMeter10A4 Low Pressure Dro'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y32,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E34/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I34),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J34),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q34*0.45),'BasicMeter10A4 Low Pressure Dro'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q34*0.45),'BasicMeter10A4 Low Pressure Dro'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y33,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E35/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I35),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J35),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q35*0.45),'BasicMeter10A4 Low Pressure Dro'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q35*0.45),'BasicMeter10A4 Low Pressure Dro'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y34,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E36/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I36),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J36),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q36*0.45),'BasicMeter10A4 Low Pressure Dro'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q36*0.45),'BasicMeter10A4 Low Pressure Dro'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y35,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E37/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I37),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J37),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q37*0.45),'BasicMeter10A4 Low Pressure Dro'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q37*0.45),'BasicMeter10A4 Low Pressure Dro'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y36,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E38/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I38),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J38),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q38*0.45),'BasicMeter10A4 Low Pressure Dro'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q38*0.45),'BasicMeter10A4 Low Pressure Dro'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y37,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E39/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I39),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J39),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q39*0.45),'BasicMeter10A4 Low Pressure Dro'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q39*0.45),'BasicMeter10A4 Low Pressure Dro'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y38,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E40/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I40),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J40),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q40*0.45),'BasicMeter10A4 Low Pressure Dro'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q40*0.45),'BasicMeter10A4 Low Pressure Dro'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y39,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E41/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I41),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J41),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q41*0.45),'BasicMeter10A4 Low Pressure Dro'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q41*0.45),'BasicMeter10A4 Low Pressure Dro'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y40,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E42/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I42),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J42),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q42*0.45),'BasicMeter10A4 Low Pressure Dro'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q42*0.45),'BasicMeter10A4 Low Pressure Dro'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y41,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E43/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I43),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J43),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q43*0.45),'BasicMeter10A4 Low Pressure Dro'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q43*0.45),'BasicMeter10A4 Low Pressure Dro'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y42,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E44/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I44),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J44),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q44*0.45),'BasicMeter10A4 Low Pressure Dro'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q44*0.45),'BasicMeter10A4 Low Pressure Dro'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y43,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E45/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I45),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J45),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q45*0.45),'BasicMeter10A4 Low Pressure Dro'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q45*0.45),'BasicMeter10A4 Low Pressure Dro'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y44,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E46/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I46),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J46),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q46*0.45),'BasicMeter10A4 Low Pressure Dro'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q46*0.45),'BasicMeter10A4 Low Pressure Dro'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y45,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E47/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I47),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J47),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q47*0.45),'BasicMeter10A4 Low Pressure Dro'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q47*0.45),'BasicMeter10A4 Low Pressure Dro'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y46,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E48/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I48),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J48),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q48*0.45),'BasicMeter10A4 Low Pressure Dro'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q48*0.45),'BasicMeter10A4 Low Pressure Dro'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y47,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E49/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I49),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J49),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q49*0.45),'BasicMeter10A4 Low Pressure Dro'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q49*0.45),'BasicMeter10A4 Low Pressure Dro'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y48,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E50/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I50),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J50),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q50*0.45),'BasicMeter10A4 Low Pressure Dro'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q50*0.45),'BasicMeter10A4 Low Pressure Dro'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y49,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E51/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I51),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J51),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q51*0.45),'BasicMeter10A4 Low Pressure Dro'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q51*0.45),'BasicMeter10A4 Low Pressure Dro'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y50,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E52/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I52),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J52),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q52*0.45),'BasicMeter10A4 Low Pressure Dro'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q52*0.45),'BasicMeter10A4 Low Pressure Dro'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y51,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E53/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I53),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J53),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q53*0.45),'BasicMeter10A4 Low Pressure Dro'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q53*0.45),'BasicMeter10A4 Low Pressure Dro'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y52,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E54/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I54),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J54),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q54*0.45),'BasicMeter10A4 Low Pressure Dro'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q54*0.45),'BasicMeter10A4 Low Pressure Dro'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y53,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E55/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I55),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J55),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q55*0.45),'BasicMeter10A4 Low Pressure Dro'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q55*0.45),'BasicMeter10A4 Low Pressure Dro'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y54,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E56/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I56),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J56),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q56*0.45),'BasicMeter10A4 Low Pressure Dro'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q56*0.45),'BasicMeter10A4 Low Pressure Dro'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y55,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E57/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I57),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J57),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q57*0.45),'BasicMeter10A4 Low Pressure Dro'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q57*0.45),'BasicMeter10A4 Low Pressure Dro'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y56,$V$4:$V$20))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E58/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I58),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J58),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q58*0.45),'BasicMeter10A4 Low Pressure Dro'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Low Pressure Dro'!Q58*0.45),'BasicMeter10A4 Low Pressure Dro'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Low Pressure Dro'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$20<Y57,$V$4:$V$20))","v":0},{"$error":"#N/A"}]

{"sheet":"BasicMeter10A4 Alarm","index":30,"n_rows":58,"n_cols":42,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,4,1,10],[2,28,2,29]]}
[]
[null,"Current Tab","Current Step",null,"Alarm Floats",null,null,null,null,null,null,null,null,null,null,"10A4 All",null,null,null,null,"10A4\" Range Limit",null,null,"10A4\" Range Limit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,"Water GPM","Air SCFM","Tube","Float (SST)","VIC","psia Critical","Pressure Drop (in. H2O)",null,null,"Liquid + Gas",null,"Tube/Float","Max Rounded","Tube/Float","Viscosity / Pressure Warning","size","Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded","Viscosity Pressure Warning",null,null,"Final Standard"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44",0.67,2.76,"FP-1/2-17-G-10","1/2-GSVTA-44",7.1,33.4,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E4/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G4,\"                                                                                                  \",H4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44"},{"$f":"IF(N4<0.00000099999,ROUND(N4,7),\nIF(N4<0.0000099999,ROUND(N4,6),\nIF(N4<0.000099999,ROUND(N4,5),\nIF(N4<0.00099999,ROUND(N4,4),\nIF(N4<0.0099999,ROUND(N4,3),\nIF(N4<0.099999,ROUND(N4,2),\nIF(N4<0.99999,ROUND(N4,2),\nIF(N4<9.999,ROUND(N4,2),\nIF(N4<99.99,ROUND(N4,1),\nIF(N4<999.99,ROUND(N4,0),\nIF(N4<9999.99,ROUND(N4,-1),\nIF(N4<99999,ROUND(N4,-2),ROUND(N4,2)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"P4","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I4),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J4),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q4*0.45),'BasicMeter10A4 Alarm'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q4*0.45),'BasicMeter10A4 Alarm'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(Y4,$Q$4:$R$52,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($V$4:$V$52>0,V4:V52))","v":0},{"$f":"VLOOKUP(X4,$R$4:$S$52,2,FALSE)","v":{"$error":"#N/A"}},null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48",0.69,2.85,"FP-1/2-17-G-10","1/2-GSVTA-48",7.6,39,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G5,\"                                                                                                  \",H5)","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48"},{"$f":"IF(N5<0.00000099999,ROUND(N5,7),\nIF(N5<0.0000099999,ROUND(N5,6),\nIF(N5<0.000099999,ROUND(N5,5),\nIF(N5<0.00099999,ROUND(N5,4),\nIF(N5<0.0099999,ROUND(N5,3),\nIF(N5<0.099999,ROUND(N5,2),\nIF(N5<0.99999,ROUND(N5,2),\nIF(N5<9.999,ROUND(N5,2),\nIF(N5<99.99,ROUND(N5,1),\nIF(N5<999.99,ROUND(N5,0),\nIF(N5<9999.99,ROUND(N5,-1),\nIF(N5<99999,ROUND(N5,-2),ROUND(N5,2)))))))))))))","v":{"$error":"#VALUE!"}},{"$f":"P5","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I5),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J5),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q5*0.45),'BasicMeter10A4 Alarm'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q5*0.45),'BasicMeter10A4 Alarm'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(Y5,$Q$4:$R$52,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($V$4:$V$52<Y4,$V$4:$V$52))","v":0},{"$f":"VLOOKUP(X5,$R$4:$S$52,2,FALSE)","v":{"$error":"#N/A"}},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$X$33,1/0),\nIFERROR(IF($Z$32=\"\",$X$32,1/0),\nIFERROR(IF($Z$31=\"\",$X$31,1/0),\nIFERROR(IF($Z$30=\"\",$X$30,1/0),\nIFERROR(IF($Z$29=\"\",$X$29,1/0),\nIFERROR(IF($Z$28=\"\",$X$28,1/0),\nIFERROR(IF($Z$27=\"\",$X$27,1/0),\nIFERROR(IF($Z$26=\"\",$X$26,1/0),\nIFERROR(IF($Z$25=\"\",$X$25,1/0),\nIFERROR(IF($Z$24=\"\",$X$24,1/0),\nIFERROR(IF($Z$23=\"\",$X$23,1/0),\nIFERROR(IF($Z$22=\"\",$X$22,1/0),\nIFERROR(IF($Z$21=\"\",$X$21,1/0),\nIFERROR(IF($Z$20=\"\",$X$20,1/0),\nIFERROR(IF($Z$19=\"\",$X$19,1/0),\nIFERROR(IF($Z$18=\"\",$X$18,1/0),\nIFERROR(IF($Z$17=\"\",$X$17,1/0),\nIFERROR(IF($Z$16=\"\",$X$16,1/0),\nIFERROR(IF($Z$15=\"\",$X$15,1/0),\nIFERROR(IF($Z$14=\"\",$X$14,1/0),\nIFERROR(IF($Z$13=\"\",$X$13,1/0),\nIFERROR(IF($Z$12=\"\",$X$12,1/0),\nIFERROR(IF($Z$11=\"\",$X$11,1/0),\nIFERROR(IF($Z$10=\"\",$X$10,1/0),\nIFERROR(IF($Z$9=\"\",$X$9,1/0),\nIFERROR(IF($Z$8=\"\",$X$8,1/0),\nIFERROR(IF($Z$7=\"\",$X$7,1/0),\nIFERROR(IF($Z$6=\"\",$X$6,1/0),\nIFERROR(IF($Z$5=\"\",$X$5,1/0),\nIFERROR(IF($Z$4=\"\",$X$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AC5,$X$4:$Y$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(IF(AND(AC5=\"none\",NOT(Z4=\"\")),Z4,\"\"),\"sizing\")","v":"sizing"},null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44",0.83,3.42,"FP-1/2-21-G-10","1/2-GSVTA-44",7.1,33.799999999999997,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I6),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J6),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q6*0.45),'BasicMeter10A4 Alarm'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q6*0.45),'BasicMeter10A4 Alarm'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y5,$V$4:$V$52))","v":0},{"$f":"VLOOKUP(X6,$R$4:$S$52,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48",0.88,3.62,"FP-1/2-21-G-10","1/2-GSVTA-48",7.6,24.6,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I7),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J7),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q7*0.45),'BasicMeter10A4 Alarm'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q7*0.45),'BasicMeter10A4 Alarm'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y6,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48",0.88500000000000001,3.65,"FP-1/2-17-G-10","1/2-GNSVTA-48",1.1000000000000001,19.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48",{"$error":"#VALUE!"},"FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I8),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J8),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q8*0.45),'BasicMeter10A4 Alarm'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q8*0.45),'BasicMeter10A4 Alarm'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y7,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44",1.03,4.24,"FP-1/2-21-G-10","1/2-GNSVTA-44",1.1000000000000001,33.4,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I9),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J9),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q9*0.45),'BasicMeter10A4 Alarm'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q9*0.45),'BasicMeter10A4 Alarm'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y8,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48",1.1000000000000001,4.5199999999999996,"FP-1/2-21-G-10","1/2-GNSVTA-48",1.1000000000000001,20,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48",{"$error":"#VALUE!"},"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I10),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J10),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q10*0.45),'BasicMeter10A4 Alarm'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q10*0.45),'BasicMeter10A4 Alarm'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y9,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44",1.1200000000000001,4.5999999999999996,"FP-1/2-27-G-10","1/2-GSVTA-44",7.1,16.2,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I11),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J11),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q11*0.45),'BasicMeter10A4 Alarm'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q11*0.45),'BasicMeter10A4 Alarm'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y10,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48",1.19,4.9000000000000004,"FP-1/2-27-G-10","1/2-GSVTA-48",7.6,18.600000000000001,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I12),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J12),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q12*0.45),'BasicMeter10A4 Alarm'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q12*0.45),'BasicMeter10A4 Alarm'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y11,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48",1.44,5.93,"FP-1/2-27-G-10","1/2-GNSVTA-48",1.1000000000000001,16.5,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I13),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J13),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q13*0.45),'BasicMeter10A4 Alarm'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q13*0.45),'BasicMeter10A4 Alarm'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y12,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44",1.56,6.43,"FP-1/2-35-G-10","1/2-GSVTA-44",7.1,16.5,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I14),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J14),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q14*0.45),'BasicMeter10A4 Alarm'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q14*0.45),'BasicMeter10A4 Alarm'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y13,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48",1.66,6.85,"FP-1/2-35-G-10","1/2-GSVTA-48",7.3,18.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E15/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I15),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J15),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q15*0.45),'BasicMeter10A4 Alarm'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q15*0.45),'BasicMeter10A4 Alarm'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y14,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43",1.84,7.6,"FP-1/2-27-G-10","1/2-GNSVTA-43",1.3,27.5,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E16/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43",{"$error":"#VALUE!"},"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I16),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J16),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q16*0.45),'BasicMeter10A4 Alarm'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q16*0.45),'BasicMeter10A4 Alarm'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y15,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48",2,8.24,"FP-1/2-35-G-10","1/2-GNSVTA-48",1.1000000000000001,8.8000000000000007,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E17/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I17),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J17),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q17*0.45),'BasicMeter10A4 Alarm'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q17*0.45),'BasicMeter10A4 Alarm'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y16,$V$4:$V$52))","v":0},{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43",2.4300000000000002,10,"FP-1/2-35-G-10","1/2-GNSVTA-43",1.3,22.7,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E18/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F18/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43",{"$error":"#VALUE!"},"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I18),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J18),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q18*0.45),'BasicMeter10A4 Alarm'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q18*0.45),'BasicMeter10A4 Alarm'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y17,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44",2.76,11.4,"FP-1/2-50-G-9","1/2-GSVTA-44",7,7.7,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E19/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F19/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I19),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J19),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q19*0.45),'BasicMeter10A4 Alarm'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q19*0.45),'BasicMeter10A4 Alarm'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y18,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48",2.9,12,"FP-1/2-50-G-9","1/2-GSVTA-48",7.6,8.9,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E20/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F20/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I20),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J20),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q20*0.45),'BasicMeter10A4 Alarm'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q20*0.45),'BasicMeter10A4 Alarm'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y19,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48",3.52,14.5,"FP-1/2-50-G-9","1/2-GNSVTA-48",1.1000000000000001,8.8000000000000007,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E21/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F21/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I21),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J21),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q21*0.45),'BasicMeter10A4 Alarm'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q21*0.45),'BasicMeter10A4 Alarm'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y20,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43",4,16,"FP-1/2-50-G-9","1/2-GNSVTA-43",1.3,12.3,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E22/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F22/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43",{"$error":"#VALUE!"},"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I22),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J22),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q22*0.45),'BasicMeter10A4 Alarm'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q22*0.45),'BasicMeter10A4 Alarm'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y21,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54",1.96,8.1,"FP-3/4-21-G-10","3/4-GSVTA-54",10.4,13.9,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E23/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F23/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I23),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J23),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q23*0.45),'BasicMeter10A4 Alarm'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q23*0.45),'BasicMeter10A4 Alarm'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y22,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54",2.4900000000000002,10.199999999999999,"FP-3/4-21-G-10","3/4-GNSVTA-54",1.6,13.9,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E24/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F24/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I24),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J24),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q24*0.45),'BasicMeter10A4 Alarm'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q24*0.45),'BasicMeter10A4 Alarm'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y23,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54",2.7,11.1,"FP-3/4-27-G-10","3/4-GSVTA-54",10.4,9.6,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E25/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F25/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I25),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J25),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q25*0.45),'BasicMeter10A4 Alarm'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q25*0.45),'BasicMeter10A4 Alarm'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y24,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53",3.15,13,"FP-3/4-21-G-10","3/4-GSVTA-53",16.600000000000001,36,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E26/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F26/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53",{"$error":"#VALUE!"},"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I26),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J26),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q26*0.45),'BasicMeter10A4 Alarm'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q26*0.45),'BasicMeter10A4 Alarm'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y25,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54",3.55,14.6,"FP-3/4-27-G-10","3/4-GNSVTA-54",1.6,9.6,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E27/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F27/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I27),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J27),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q27*0.45),'BasicMeter10A4 Alarm'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q27*0.45),'BasicMeter10A4 Alarm'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y26,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56",3.85,15.8,"FP-3/4-27-G-10","3/4-GSVTA-56",14.9,19.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E28/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F28/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I28),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J28),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q28*0.45),'BasicMeter10A4 Alarm'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q28*0.45),'BasicMeter10A4 Alarm'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y27,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53",4.3499999999999996,18,"FP-3/4-27-G-10","3/4-GSVTA-53",16.8,25,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E29/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F29/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I29),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J29),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q29*0.45),'BasicMeter10A4 Alarm'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q29*0.45),'BasicMeter10A4 Alarm'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y28,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56",5.05,20.8,"FP-3/4-27-G-10","3/4-GNSVTA-56",2.2000000000000002,19.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E30/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F30/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I30),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J30),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q30*0.45),'BasicMeter10A4 Alarm'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q30*0.45),'BasicMeter10A4 Alarm'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y29,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53",5.7,23.6,"FP-3/4-27-G-10","3/4-GNSVTA-53",2.5,25,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E31/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F31/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53",{"$error":"#VALUE!"},"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I31),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J31),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"3/4",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q31*0.45),'BasicMeter10A4 Alarm'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q31*0.45),'BasicMeter10A4 Alarm'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y30,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GSVTA-64",4.25,17.5,"FP-1-27-G-10","1-GSVTA-64",14.8,11.5,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E32/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F32/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GSVTA-64",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GSVTA-64",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I32),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J32),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q32*0.45),'BasicMeter10A4 Alarm'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q32*0.45),'BasicMeter10A4 Alarm'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y31,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GSVTA-65",4.82,19.8,"FP-1-27-G-10","1-GSVTA-65",16.899999999999999,14.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E33/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F33/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GSVTA-65",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GSVTA-65",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I33),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J33),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q33*0.45),'BasicMeter10A4 Alarm'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q33*0.45),'BasicMeter10A4 Alarm'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y32,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVTA-64",5.63,23.2,"FP-1-27-G-10","1-GNSVTA-64",2.2000000000000002,11.3,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E34/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F34/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-27-G-10                                                                                                  1-GNSVTA-64",{"$error":"#VALUE!"},"FP-1-27-G-10                                                                                                  1-GNSVTA-64",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I34),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J34),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q34*0.45),'BasicMeter10A4 Alarm'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q34*0.45),'BasicMeter10A4 Alarm'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y33,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-64",6,24.7,"FP-1-35-G-10","1-GSVTA-64",14.8,6.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E35/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F35/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVTA-64",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVTA-64",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I35),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J35),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q35*0.45),'BasicMeter10A4 Alarm'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q35*0.45),'BasicMeter10A4 Alarm'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y34,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-65",6.75,27.9,"FP-1-35-G-10","1-GSVTA-65",16.899999999999999,8.9,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E36/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F36/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVTA-65",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVTA-65",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I36),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J36),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q36*0.45),'BasicMeter10A4 Alarm'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q36*0.45),'BasicMeter10A4 Alarm'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y35,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-64",7.84,32.4,"FP-1-35-G-10","1-GNSVTA-64",2.2000000000000002,6.8,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E37/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F37/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GNSVTA-64",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GNSVTA-64",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I37),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J37),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q37*0.45),'BasicMeter10A4 Alarm'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q37*0.45),'BasicMeter10A4 Alarm'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y36,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-63",8.4600000000000009,35.1,"FP-1-35-G-10","1-GSVTA-63",20.8,13.9,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E38/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F38/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVTA-63",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVTA-63",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I38),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J38),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q38*0.45),'BasicMeter10A4 Alarm'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q38*0.45),'BasicMeter10A4 Alarm'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y37,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-65",9,36.9,"FP-1-35-G-10","1-GNSVTA-65",2.5,8.9,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E39/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F39/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GNSVTA-65",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GNSVTA-65",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I39),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J39),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q39*0.45),'BasicMeter10A4 Alarm'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q39*0.45),'BasicMeter10A4 Alarm'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y38,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-66",9.9,10.6,"FP-1-35-G-10","1-GSVTA-66",8.5,13.4,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E40/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F40/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-35-G-10                                                                                                  1-GSVTA-66",{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GSVTA-66",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I40),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J40),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q40*0.45),'BasicMeter10A4 Alarm'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q40*0.45),'BasicMeter10A4 Alarm'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y39,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-63",11.1,45.7,"FP-1-35-G-10","1-GNSVTA-63",2.9,13.1,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E41/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F41/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,{"$f":"CONCATENATE(G41,\"                                                                                                  \",H41)","v":"FP-1-35-G-10                                                                                                  1-GNSVTA-63"},{"$error":"#VALUE!"},"FP-1-35-G-10                                                                                                  1-GNSVTA-63",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I41),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J41),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q41*0.45),'BasicMeter10A4 Alarm'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q41*0.45),'BasicMeter10A4 Alarm'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y40,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84",13.4,55,"FP-1-1/2-27-G-10","1-1/2-GSVTA-84",27.6,15.4,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E42/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F42/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I42),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J42),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q42*0.45),'BasicMeter10A4 Alarm'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q42*0.45),'BasicMeter10A4 Alarm'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y41,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85",15.4,63.5,"FP-1-1/2-27-G-10","1-1/2-GSVTA-85",32,20.3,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E43/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F43/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I43),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J43),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q43*0.45),'BasicMeter10A4 Alarm'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q43*0.45),'BasicMeter10A4 Alarm'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y42,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83",16,66,"FP-1-1/2-27-G-10","1-1/2-GSVTA-83",33,22,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E44/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F44/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I44),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J44),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q44*0.45),'BasicMeter10A4 Alarm'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q44*0.45),'BasicMeter10A4 Alarm'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y43,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84",17.600000000000001,72,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-84",4.2,15.4,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E45/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F45/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I45),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J45),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q45*0.45),'BasicMeter10A4 Alarm'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q45*0.45),'BasicMeter10A4 Alarm'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y44,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85",20.399999999999999,84,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-85",5,20.3,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E46/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F46/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I46),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J46),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q46*0.45),'BasicMeter10A4 Alarm'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q46*0.45),'BasicMeter10A4 Alarm'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y45,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83",21.2,87,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-83",4.9000000000000004,22,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E47/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F47/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83",{"$error":"#VALUE!"},"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I47),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J47),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"1-1/2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q47*0.45),'BasicMeter10A4 Alarm'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q47*0.45),'BasicMeter10A4 Alarm'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y46,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GSVTA-94",23.9,99,"FP-2-27-G-10","2-GSVTA-94",40.5,16.399999999999999,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E48/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F48/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GSVTA-94",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GSVTA-94",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I48),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J48),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q48*0.45),'BasicMeter10A4 Alarm'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q48*0.45),'BasicMeter10A4 Alarm'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y47,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GSVTA-93",27.9,115.2,"FP-2-27-G-10","2-GSVTA-93",49,24,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E49/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F49/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GSVTA-93",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GSVTA-93",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I49),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J49),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q49*0.45),'BasicMeter10A4 Alarm'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q49*0.45),'BasicMeter10A4 Alarm'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y48,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-94",31.5,129.80000000000001,"FP-2-27-G-10","2-GNSVTA-94",6.1,17.399999999999999,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E50/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F50/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GNSVTA-94",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GNSVTA-94",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I50),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J50),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q50*0.45),'BasicMeter10A4 Alarm'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q50*0.45),'BasicMeter10A4 Alarm'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y49,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-96",36.9,152.1,"FP-2-27-G-10","2-GNSVTA-96",7.6,21.2,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E51/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F51/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GNSVTA-96",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GNSVTA-96",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I51),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J51),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q51*0.45),'BasicMeter10A4 Alarm'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q51*0.45),'BasicMeter10A4 Alarm'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y50,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-93",38.200000000000003,156.6,"FP-2-27-G-10","2-GNSVTA-93",7.3,24,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E52/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F52/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"FP-2-27-G-10                                                                                                  2-GNSVTA-93",{"$error":"#VALUE!"},"FP-2-27-G-10                                                                                                  2-GNSVTA-93",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I52),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J52),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},"2",{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q52*0.45),'BasicMeter10A4 Alarm'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q52*0.45),'BasicMeter10A4 Alarm'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y51,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E53/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F53/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I53),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J53),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q53*0.45),'BasicMeter10A4 Alarm'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q53*0.45),'BasicMeter10A4 Alarm'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y52,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E54/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F54/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I54),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J54),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q54*0.45),'BasicMeter10A4 Alarm'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q54*0.45),'BasicMeter10A4 Alarm'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y53,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E55/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F55/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I55),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J55),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q55*0.45),'BasicMeter10A4 Alarm'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q55*0.45),'BasicMeter10A4 Alarm'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y54,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E56/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F56/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I56),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J56),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q56*0.45),'BasicMeter10A4 Alarm'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q56*0.45),'BasicMeter10A4 Alarm'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y55,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E57/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F57/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I57),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J57),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q57*0.45),'BasicMeter10A4 Alarm'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q57*0.45),'BasicMeter10A4 Alarm'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y56,$V$4:$V$52))","v":0},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",E58/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2)),\nIF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F58/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\"))))","v":""},null,"                                                                                                  ",{"$error":"#VALUE!"},"                                                                                                  ",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>I58),\"viscosity\",\nIF('VA Sizing'!$C$3=\"Liquid\",\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<J58),\"pressure\",\nIF('VA Sizing'!$C$3=\"Gas\",\"\",))))","v":0},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q58*0.45),'BasicMeter10A4 Alarm'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A4 Alarm'!Q58*0.45),'BasicMeter10A4 Alarm'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A4 Alarm'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($V$4:$V$52<Y57,$V$4:$V$52))","v":0},{"$error":"#N/A"}]

{"sheet":"BasicResults","index":31,"n_rows":23,"n_cols":20,"rows_kept":23,"cut":false,"hidden":true,"merged":[[6,1,7,3],[12,16,13,17],[6,19,7,19],[8,19,9,19],[10,19,11,19],[12,19,13,19],[3,6,3,13],[5,16,5,19],[6,16,7,17],[8,16,9,17],[10,16,11,17]]}
[]
[null,"Current Tab","Current Step"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1}]
[null,null,null,null,null,null,"Available Meters"]
[]
[null,null,null,null,null,{"$f":"'BasicMeter Consolidation'!B36","v":""},null,null,{"$f":"'BasicMeter Consolidation'!B37","v":""},null,null,{"$f":"'BasicMeter Consolidation'!B38","v":""},null,null,{"$f":"'BasicMeter Consolidation'!B39","v":""},null,"Unavailable Meters"]
[null,"VA Sizing Tool",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'BasicMeter Consolidation'!A49","v":"10A61"},null,null,{"$f":"IF(Q7=\"\",\"\",\"REASON\")","v":"REASON"}]
[]
[null," Version 3.0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'BasicMeter Consolidation'!A50","v":"10A4"},null,null,{"$f":"IF(Q9=\"\",\"\",\"REASON\")","v":"REASON"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'BasicMeter Consolidation'!A51","v":"10A22"},null,null,{"$f":"IF(Q11=\"\",\"\",\"REASON\")","v":"REASON"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'BasicMeter Consolidation'!A52","v":"10A32"},null,null,{"$f":"IF(Q13=\"\",\"\",\"REASON\")","v":"REASON"}]
[]
[]
[null,null,null,"Connection Size",null,{"$f":"'BasicMeter Consolidation'!G36","v":""},null,null,{"$f":"'BasicMeter Consolidation'!G37","v":""},null,null,{"$f":"'BasicMeter Consolidation'!G38","v":""},null,null,{"$f":"'BasicMeter Consolidation'!G39","v":""}]
[null,null,null,"Connection Type",null,{"$f":"IF($F$6=\"\",\"\",\nIF($F$6=\"10A61\",\"NPT Threaded\",\nIF($F$6=\"10A4\",\"NPT Threaded or Flanged\",\nIF($F$6=\"10A32\",\"NPT Threaded\",\nIF($F$6=\"10A22\",\"NPT Threaded\",\"\")))))","v":""},null,null,{"$f":"IF($I$6=\"\",\"\",\nIF($I$6=\"10A61\",\"NPT Threaded\",\nIF($I$6=\"10A4\",\"NPT Threaded or Flanged\",\nIF($I$6=\"10A32\",\"NPT Threaded\",\nIF($I$6=\"10A22\",\"NPT Threaded\",\"\")))))","v":""},null,null,{"$f":"IF($L$6=\"\",\"\",\nIF($L$6=\"10A61\",\"NPT Threaded\",\nIF($L$6=\"10A4\",\"NPT Threaded or Flanged\",\nIF($L$6=\"10A32\",\"NPT Threaded\",\nIF($L$6=\"10A22\",\"NPT Threaded\",\"\")))))","v":""},null,null,{"$f":"IF($O$6=\"\",\"\",\nIF($O$6=\"10A61\",\"NPT Threaded\",\nIF($O$6=\"10A4\",\"NPT Threaded or Flanged\",\nIF($O$6=\"10A32\",\"NPT Threaded\",\nIF($O$6=\"10A22\",\"NPT Threaded\",\"\")))))","v":""}]
[null,null,null,"Tube Material",null,{"$f":"IF($F$6=\"\",\"\",\nIF($F$6=\"10A61\",\"Glass\",\nIF($F$6=\"10A4\",\"Glass\",\nIF($F$6=\"10A32\",\"Metal\",\nIF($F$6=\"10A22\",\"Glass\",\"\")))))","v":""},null,null,{"$f":"IF($I$6=\"\",\"\",\nIF($I$6=\"10A61\",\"Glass\",\nIF($I$6=\"10A4\",\"Glass\",\nIF($I$6=\"10A32\",\"Metal\",\nIF($I$6=\"10A22\",\"Glass\",\"\")))))","v":""},null,null,{"$f":"IF($L$6=\"\",\"\",\nIF($L$6=\"10A61\",\"Glass\",\nIF($L$6=\"10A4\",\"Glass\",\nIF($L$6=\"10A32\",\"Metal\",\nIF($L$6=\"10A22\",\"Glass\",\"\")))))","v":""},null,null,{"$f":"IF($O$6=\"\",\"\",\nIF($O$6=\"10A61\",\"Glass\",\nIF($O$6=\"10A4\",\"Glass\",\nIF($O$6=\"10A32\",\"Metal\",\nIF($O$6=\"10A22\",\"Glass\",\"\")))))","v":""}]
[null,null,null,"Integral Needle Valve",null,{"$f":"IF($F$6=\"\",\"\",\nIF($F$6=\"10A61\",\"Yes\",\nIF($F$6=\"10A4\",\"No\",\nIF($F$6=\"10A32\",\"Yes\",\nIF($F$6=\"10A22\",\"No\",\"\")))))","v":""},null,null,{"$f":"IF($I$6=\"\",\"\",\nIF($I$6=\"10A61\",\"Yes\",\nIF($I$6=\"10A4\",\"No\",\nIF($I$6=\"10A32\",\"Yes\",\nIF($I$6=\"10A22\",\"No\",\"\")))))","v":""},null,null,{"$f":"IF($L$6=\"\",\"\",\nIF($L$6=\"10A61\",\"Yes\",\nIF($L$6=\"10A4\",\"No\",\nIF($L$6=\"10A32\",\"Yes\",\nIF($L$6=\"10A22\",\"No\",\"\")))))","v":""},null,null,{"$f":"IF($O$6=\"\",\"\",\nIF($O$6=\"10A61\",\"Yes\",\nIF($O$6=\"10A4\",\"No\",\nIF($O$6=\"10A32\",\"Yes\",\nIF($O$6=\"10A22\",\"No\",\"\")))))","v":""}]
[null,null,null,"Transmit (4-20mA)",null,{"$f":"IF($F$6=\"\",\"\",\nIF($F$6=\"10A61\",\"No\",\nIF($F$6=\"10A4\",\"No\",\nIF($F$6=\"10A32\",\"Yes\",\nIF($F$6=\"10A22\",\"No\",\"\")))))","v":""},null,null,{"$f":"IF($I$6=\"\",\"\",\nIF($I$6=\"10A61\",\"No\",\nIF($I$6=\"10A4\",\"No\",\nIF($I$6=\"10A32\",\"Yes\",\nIF($I$6=\"10A22\",\"No\",\"\")))))","v":""},null,null,{"$f":"IF($L$6=\"\",\"\",\nIF($L$6=\"10A61\",\"No\",\nIF($L$6=\"10A4\",\"No\",\nIF($L$6=\"10A32\",\"Yes\",\nIF($L$6=\"10A22\",\"No\",\"\")))))","v":""},null,null,{"$f":"IF($O$6=\"\",\"\",\nIF($O$6=\"10A61\",\"No\",\nIF($O$6=\"10A4\",\"No\",\nIF($O$6=\"10A32\",\"Yes\",\nIF($O$6=\"10A22\",\"No\",\"\")))))","v":""}]
[null,null,null,"Alarm Availability",null,{"$f":"IF(F6=\"\",\"\",\nIF(AND(F6=\"10A61\",OR('BasicMeter Consolidation'!$B$43=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A61 Alarm\")),\"Yes\",\nIF(AND(F6=\"10A4\",OR('BasicMeter Consolidation'!$B$43=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A4 Alarm\")),\"Yes\",\nIF(AND(F6=\"10A22\",OR('BasicMeter Consolidation'!$B$43=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A22 Alarm\")),\"Yes\",\nIF(BasicResults!F6=\"10A32\",\"Yes\",\"No\")))))","v":""},null,null,{"$f":"IF(I6=\"\",\"\",\nIF(AND(I6=\"10A61\",OR('BasicMeter Consolidation'!$B$43=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A61 Alarm\")),\"Yes\",\nIF(AND(I6=\"10A4\",OR('BasicMeter Consolidation'!$B$43=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A4 Alarm\")),\"Yes\",\nIF(AND(I6=\"10A22\",OR('BasicMeter Consolidation'!$B$43=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A22 Alarm\")),\"Yes\",\nIF(BasicResults!I6=\"10A32\",\"Yes\",\"No\")))))","v":""},null,null,{"$f":"IF(L6=\"\",\"\",\nIF(AND(L6=\"10A61\",OR('BasicMeter Consolidation'!$B$43=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A61 Alarm\")),\"Yes\",\nIF(AND(L6=\"10A4\",OR('BasicMeter Consolidation'!$B$43=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A4 Alarm\")),\"Yes\",\nIF(AND(L6=\"10A22\",OR('BasicMeter Consolidation'!$B$43=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A22 Alarm\")),\"Yes\",\nIF(BasicResults!L6=\"10A32\",\"Yes\",\"No\")))))","v":""},{"$f":"IF(M6=\"\",\"\",\nIF(AND(M6=\"10A61\",OR('BasicMeter Consolidation'!$B$43=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A61 Alarm\")),\"Yes\",\nIF(AND(M6=\"10A4\",OR('BasicMeter Consolidation'!$B$43=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A4 Alarm\")),\"Yes\",\nIF(AND(M6=\"10A22\",OR('BasicMeter Consolidation'!$B$43=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A22 Alarm\")),\"Yes\",\nIF(BasicResults!M6=\"10A32\",\"Yes\",\"No\")))))","v":""},{"$f":"IF(N6=\"\",\"\",\nIF(AND(N6=\"10A61\",OR('BasicMeter Consolidation'!$B$43=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A61 Alarm\")),\"Yes\",\nIF(AND(N6=\"10A4\",OR('BasicMeter Consolidation'!$B$43=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A4 Alarm\")),\"Yes\",\nIF(AND(N6=\"10A22\",OR('BasicMeter Consolidation'!$B$43=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A22 Alarm\")),\"Yes\",\nIF(BasicResults!N6=\"10A32\",\"Yes\",\"No\")))))","v":""},{"$f":"IF(O6=\"\",\"\",\nIF(AND(O6=\"10A61\",OR('BasicMeter Consolidation'!$B$43=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A61 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A61 Alarm\")),\"Yes\",\nIF(AND(O6=\"10A4\",OR('BasicMeter Consolidation'!$B$43=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A4 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A4 Alarm\")),\"Yes\",\nIF(AND(O6=\"10A22\",OR('BasicMeter Consolidation'!$B$43=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$44=\"10A22 Alarm\",'BasicMeter Consolidation'!$B$45=\"10A22 Alarm\")),\"Yes\",\nIF(BasicResults!O6=\"10A32\",\"Yes\",\"No\")))))","v":""}]
[]
[null,null,null,null,null,{"$f":"IF(F6=\"\",\"\",\" SELECT\")","v":""},null,null,{"$f":"IF(I6=\"\",\"\",\"SELECT\")","v":""},null,null,"",null,null,{"$f":"IF(O6=\"\",\"\",\"SELECT \")","v":""}]

{"sheet":"VA Sizing","index":32,"n_rows":32,"n_cols":26,"rows_kept":32,"cut":false,"hidden":false,"merged":[[27,15,27,17],[26,15,26,17],[31,9,31,25],[29,9,29,25],[23,18,23,19],[23,24,23,25],[24,21,24,23],[25,21,25,23],[26,21,26,23],[27,21,27,23],[23,12,23,13],[24,9,24,11],[25,9,25,11],[26,9,26,11],[27,9,27,11],[24,15,24,17],[25,15,25,17],[13,15,15,19],[13,20,15,25],[21,9,22,13],[21,15,22,19],[23,9,23,11],[23,15,23,17],[23,21,23,23],[21,21,21,25],[22,21,22,25],[15,1,20,2],[1,10,2,12],[1,13,2,16],[6,5,7,7],[10,5,11,7],[5,15,5,25],[6,15,10,25],[12,15,12,25],[17,9,17,25],[18,9,19,25],[2,4,3,5],[2,7,3,7]]}
[]
[null,null,null,null,null,null,null,null,null,null,"Select Meter"]
[null,"Fluid Type",null,null,{"$f":"IF(C3=\"Gas\",\"Mixed Gas\",\"\")","v":""},null,null,{"$f":"IF(C3=\"Gas\",\"Steam\",\"\")","v":""}]
[null,"Fluid Name"]
[null,"Reference Condition"]
[null,"Type of Density",null,null,null,null,null,null,null,"PHOTO",null,null,null,null,null,"Description"]
[null,"Density at Reference Conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(N2,Descriptions!$B$6:$E$10,2,FALSE),\"\")","v":""}]
[null,"Viscosity at Operating Conditions"]
[null,"Operating Pressure"]
[null,"Operating Temperature"]
[null,"Density at Operating Conditions"]
[null,"Maximum Flowrate"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Features"]
[null,"Calculated Operating Density",{"$f":"IFERROR(ROUND('10A61 5\" Calcs'!O46/VLOOKUP(D14,'Modified Inputs'!$L$15:$M$20,2,FALSE),4),\"\")","v":""},"kg/m3",null,null,null,"$B$16:$C$21",null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(N2,Descriptions!$B$6:$E$10,3,FALSE),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(VLOOKUP(N2,Descriptions!$B$6:$F$10,5,FALSE),\"\")","v":""}]
[]
[null,{"$f":"IF(C3=\"\",Assistant!G9,\nIF(AND(C3=\"Liquid\",C4=\"\"),Assistant!G10,\nIF(AND(C3=\"Gas\",C4=\"\"),Assistant!G10,\nIF(AND(C4=\"Potable Water\",C12=\"\"),Assistant!G18,\nIF(AND(OR(C4=\"Other Water\",C4=\"Other Liquid\"),C8=\"\"),Assistant!G14,\nIF(AND(OR(C4=\"Other Water\",C4=\"Other Liquid\"),C11=\"\"),Assistant!G17,\nIF(AND(OR(C4=\"Other Water\",C4=\"Other Liquid\"),C12=\"\"),Assistant!G18,\nIF(AND(C3=\"Gas\",C5=\"\"),Assistant!G11,\nIF(AND(C3=\"Gas\",C9=\"\"),Assistant!G15,\nIF(AND(C3=\"Gas\",C10=\"\"),Assistant!G16,\nIF(AND(C3=\"Gas\",C12=\"\"),Assistant!G18,\nIF(AND(NOT(C12=\"\"),N2=\"\"),\"Select Meter\",\"\"))))))))))))","v":"Select if the fluid is either a liquid or gas"}]
[]
[null,null,null,null,null,null,null,null,null,"NOTES"]
[null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(N2,Descriptions!$B$6:$E$10,4,FALSE),\"\")","v":""}]
[]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"IF(N2=\"10A61\",'10A61 Naming'!O3,\nIF('VA Sizing'!N2=\"10A4\",\"Standard Floats\",\nIF('VA Sizing'!N2=\"10A22\",\"Standard Floats\",\nIF('VA Sizing'!N2=\"10A32\",\"Standard Floats\",\"\"))))","v":""},null,null,null,null,null,{"$f":"IF(N2=\"10A61\",'10A61 Naming'!P3,\nIF('VA Sizing'!N2=\"10A4\",\"Low Pressure Drop Floats\",\nIF('VA Sizing'!N2=\"10A22\",\"Alarm Floats\",\"\")))","v":""},null,null,null,null,null,{"$f":"IF(N2=\"10A61\",'10A61 Naming'!Q3,\nIF('VA Sizing'!N2=\"10A4\",\"Additional Floats\",\nIF('VA Sizing'!N2=\"10A22\",\"\",\"\")))","v":""}]
[]
[null,null,null,null,null,null,null,null,null,"Tube/Float",null,null,"Range",null,null,"Tube/Float",null,null,"Range",null,null,"Tube/Float",null,null,"Range"]
[null,null,null,null,null,null,null,null,null,{"$f":"IF($N$2=\"10A61\",'10A61 3\" Gas+liquid Results'!H16,\nIF($N$2=\"10A4\",'10A4 Standard Floats Results'!D26,\nIF('VA Sizing'!$N$2=\"10A22\",'10A22 Standard Results'!D26,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BF26,\"\"))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 3\" Gas+liquid Results'!I16,\nIF(N2=\"10A4\",'10A4 Standard Floats Results'!E26,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Standard Results'!E26,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BG26,\"\"))))","v":""},{"$f":"IF(M25=\"\",\"\",$D$12)","v":""},null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!H13,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!D26,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!D26,\"\")))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!I13,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!E26,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!E26,\"\")))","v":""},{"$f":"IF(S25=\"\",\"\",$D$12)","v":""},null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!I16,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!D26,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!D26,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!D26,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!D26,\"\")))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!J16,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!E26,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!E26,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!E26,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!E26,\"\")))))","v":""},{"$f":"IF(Y25=\"\",\"\",$D$12)","v":""}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF($N$2=\"10A61\",'10A61 3\" Gas+liquid Results'!H17,\nIF($N$2=\"10A4\",'10A4 Standard Floats Results'!D27,\nIF('VA Sizing'!$N$2=\"10A22\",'10A22 Standard Results'!D27,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BF27,\"\"))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 3\" Gas+liquid Results'!I17,\nIF(N2=\"10A4\",'10A4 Standard Floats Results'!E27,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Standard Results'!E27,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BG27,\"\"))))","v":""},{"$f":"IF(M26=\"\",\"\",$D$12)","v":""},null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!H14,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!D27,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!D27,\"\")))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!I14,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!E27,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!E27,\"\")))","v":""},{"$f":"IF(S26=\"\",\"\",$D$12)","v":""},null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!I17,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!D27,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!D27,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!D27,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!D27,\"\")))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!J17,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!E27,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!E27,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!E27,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!E27,\"\")))))","v":""},{"$f":"IF(Y26=\"\",\"\",$D$12)","v":""}]
[null,null,null,null,null,null,null,null,null,{"$f":"IF($N$2=\"10A61\",'10A61 3\" Gas+liquid Results'!H18,\nIF($N$2=\"10A4\",'10A4 Standard Floats Results'!D28,\nIF('VA Sizing'!$N$2=\"10A22\",'10A22 Standard Results'!D28,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BF28,\"\"))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 3\" Gas+liquid Results'!I18,\nIF(N2=\"10A4\",'10A4 Standard Floats Results'!E28,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Standard Results'!E28,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BG28,\"\"))))","v":""},"",null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!H15,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!D28,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!D28,\"\")))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!I15,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!E28,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!E28,\"\")))","v":""},"",null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!I18,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!D28,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!D28,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!D28,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!D28,\"\")))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!J18,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!E28,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!E28,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!E28,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!E28,\"\")))))","v":""},""]
[null,"ABB VA Sizing V4.0",null,null,null,null,null,null,null,{"$f":"IF($N$2=\"10A61\",'10A61 3\" Gas+liquid Results'!H19,\nIF($N$2=\"10A4\",'10A4 Standard Floats Results'!D29,\nIF('VA Sizing'!$N$2=\"10A22\",'10A22 Standard Results'!D29,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BF29,\"\"))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 3\" Gas+liquid Results'!I19,\nIF(N2=\"10A4\",'10A4 Standard Floats Results'!E29,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Standard Results'!E29,\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BG29,\"\"))))","v":""},"",null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!H16,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!D29,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!D29,\"\")))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 5\" + 6\" Results'!I16,\nIF(N2=\"10A4\",'10A4 Low PSI Drop Floats Result'!E29,\nIF('VA Sizing'!N2=\"10A22\",'10A22 Alarm Results'!E29,\"\")))","v":""},"",null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!I19,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!D29,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!D29,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!D29,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!D29,\"\")))))","v":""},null,null,{"$f":"IF(N2=\"10A61\",'10A61 10\" Results'!J19,\nIF(AND(N2=\"10A4\",V23=\"Alarm Floats\"),'10A4 Alarm Floats Results'!E29,\nIF(AND(N2=\"10A4\",V23=\"Tantalum Floats (TA)\"),'10A4 TA Floats Results'!E29,\nIF(AND(N2=\"10A4\",V23=\"Teflon Floats (PTFE)\"),'10A4 PTFE Floats Results'!E29,\nIF(AND(N2=\"10A4\",V23=\"PVC Floats\"),'10A4 PVC Floats Results'!E29,\"\")))))","v":""},""]
[null,"© 2015, 2018 ABB Inc."]
[null,null,null,null,null,null,null,null,null,"Highlighted combinations may require a viscosity calibration. Please contact ABB for more information."]
[]
[null,null,null,null,null,null,null,null,null,"Highlighted combinations require a greater operating pressure."]

{"sheet":"Calculating","index":33,"n_rows":14,"n_cols":13,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Loading…"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Please Wait"]

{"sheet":"Bulk Sizing","index":34,"n_rows":35,"n_cols":22,"rows_kept":35,"cut":false,"hidden":true,"merged":[[5,14,5,18],[5,1,5,11],[5,12,5,13]]}
[]
[null,"Temp Units",null,null,null,null,null,null,null,null,"Total Lines",{"$f":"COUNTA(C8:C35)","v":0}]
[null,"Pressure Units",null,"\n"]
[]
[null,null,null,null,null,null,null,null,null,null," "]
["\n","Input",null,null,null,null,null,null,null,null,null,null,"Output",null,"Warnings",null,null,null,null,null,"$B$12:$L$12","$B$12:$L$12"]
[null,"Tag","Fluid","Density","Density Units","Viscosity (cP)","Ref. Condition","Temp.","Pressure","Flowrate","Flow Units","Meter","Part Number","List Price","Flow","Press./Temp","Haz. Gas","Press. Drop","High Viscosity",null,null,"Potable Water"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other Liquid"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"------------------"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Air"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Argon (Ar)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Butane (C4H10)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Acetylene (C2H2)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ammonia (NH3)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Carbon Monoxide (CO)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Carbon Dioxide (CO2)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chlorine (Cl2)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ethane (C2H6)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ethylene (C2H4)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Helium (He)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hydrochloric Acid (HCl)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hydrogen (H2)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hydrogen Sulfide (H2S)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Krypton (Kr)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane (CH4)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methyl Chloride (CH3Cl)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Natural Gas"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Neon (Ne)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nitric Oxide (NO)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nitrogen (N2)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nitrous Oxide (N2O)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oxygen (O2)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Propane (C3H8)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Propylene (C3H6)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sulfur Dioxide (SO2)"]

{"sheet":"Graphics","index":35,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[[24,75,27,75],[24,76,27,76],[24,77,27,77],[24,69,27,69],[24,70,27,70],[24,71,27,71],[24,72,27,72],[24,73,27,73],[24,74,27,74],[24,68,27,68],[24,57,27,57],[24,58,27,58],[24,59,27,59],[24,60,27,60],[24,61,27,61],[24,62,27,62],[24,63,27,63],[24,64,27,64],[24,65,27,65],[24,66,27,66],[24,67,27,67],[24,56,27,56],[24,51,27,51],[24,52,27,52],[24,53,27,53],[24,54,27,54],[24,55,27,55]]}

{"sheet":"Sheet3","index":36,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
[]
[null,"1st","2nd","3rd","4th","5th"]
[null,{"$f":"RANDBETWEEN(0,9)","v":4},{"$f":"RANDBETWEEN(0,9)","v":0},{"$f":"RANDBETWEEN(0,9)","v":0},{"$f":"RANDBETWEEN(0,9)","v":6},{"$f":"RANDBETWEEN(0,9)","v":6}]
[null,{"$f":"CHAR(RANDBETWEEN(65,90))","v":"Q"},{"$f":"CHAR(RANDBETWEEN(65,90))","v":"F"},{"$f":"CHAR(RANDBETWEEN(65,90))","v":"R"},{"$f":"CHAR(RANDBETWEEN(65,90))","v":"K"},{"$f":"CHAR(RANDBETWEEN(65,90))","v":"U"}]
[]
[null,{"$f":"RANDBETWEEN(0,1)","v":1},{"$f":"RANDBETWEEN(0,1)","v":1},1,0,1]
[null,null,null,null,null,null,null,"Random Identifier",null,"User Reference#"]
[null,{"$f":"IF(B6=0,B3,B4)","v":"Q"},{"$f":"IF(C6=0,C3,C4)","v":"F"},"R",6,"U",null,{"$f":"B8&C8&D8&E8&F8","v":"QFR6U"}]

{"sheet":"Log","index":37,"n_rows":30,"n_cols":2,"rows_kept":30,"cut":false,"hidden":true,"merged":[]}
[]
[]
["Version","Changes"]
[1.41,"Natural Gas Sizing Density at Operating Conditions Fixed"]
[null,"Chlorine Density Updated"]
[1.42,"10A32 sizing fixed when for flowrates exactly matching standard ranges"]
[1.43,"Fixed Error with Label56 on FormSizing for empty 10A32 Cells"]
[null,"Fixed Error with Config Preview Button for empty 10A32 Cells"]
[null,"Fixed Error with different tube/float selections within FormSizing for empty 10A32 Cells"]
[1.44,"Fixed error with 10A32 liquids above max VIC"]
[null,"Fixed error with other gas using standard viscosity instead of operating viscosity"]
[null,"Fixed error with 10A32 Configuration Preview of non-default sizings"]
["1.45/2.0","Changed graphic of meter and float in sizing record"]
[null,"Removed Gas Damping for 1/4\" 10A32"]
[2.2000000000000002,"Fixed high viscosity curve for 1/4-20-G5 and 1/8-20-G5 for the 10A61"]
[2.2999999999999998,"Added \"scfm, scfh, scfs, sccm\" as standard flowrate units"]
[null,"Added ED-Data for 3\" 10A61"]
[null,"Density units for \"other\" gases transferred to sizing record correctly"]
[null,"ED-Data updated when new tube/float selected from side bar"]
[2.4,"Added Selections for liquids"]
[null,"Potable water self populates density and viscosity"]
[null,"Pressure and Temperature for liquids is optional"]
[null,"other gas viscosity = 0.01 cP, hidden"]
[2.4300000000000002,"Basic Sizing"]
[3,"Eliminated Tantalum Float for 10A45 b/c of conflict minerals"]
[null,"Removed 1/8-32-TA combination b/c not possible"]
[null,"Operating Flowrate Float Feature Added"]
[null,"FAM54 w/ Link to PSA"]
[null,"Quick Navigation within Basic Sizing"]
[null,"Pressure and Temperature warning removed on sizing record when Optional no data entered"]

{"sheet":"10A61 5\" Calcs","index":38,"n_rows":107,"n_cols":43,"rows_kept":107,"cut":false,"hidden":true,"merged":[[44,1,44,2],[44,3,44,4],[44,5,44,6],[43,29,43,30],[43,34,43,35],[43,38,43,39],[43,41,43,42],[1,0,1,1],[1,3,1,5],[43,22,43,23],[43,26,43,27]]}
[]
["Float Densities",null,null,"Size Factor",null,null,null,null,null,"Gas","Density at Standard","Density at Normal/Actual","Viscosity","Temp Coeff. Deg F","Molecular Mass"]
["CD",2.2799999999999998,null,null,"A","B",null,null,null,"Air",1.1999999999999999E-3,1.2930000000000001E-3,1.8120000000000001E-2,2.5999999999999998E-5,28.97]
["SA",3.98,null,"1/16",143,13.6,null,null,null,"Argon (Ar)",1.66E-3,1.784E-3,2.2200000000000001E-2,3.1999999999999999E-5,39.948]
["SS",8.02,null,"1/8",404,76.8,null,null,null,"Butane (C4H10)",2.4840000000000001E-3,2.6679999999999998E-3,8.4799999999999997E-3,1.4E-5,58.12]
["CA",15,null,"1/4",1142,434,null,null,null,"Carbon Monoxide (CO)",1.163E-3,1.25E-3,1.7500000000000002E-2,2.4000000000000001E-5,28.01]
["TA",16.600000000000001,null,"3/8",2095,1200,null,null,null,"Ethane (C2H6)",1.2600000000000001E-3,1.3569999999999999E-3,9.0100000000000006E-3,1.2999999999999999E-5,30.07]
["BG",2.54,null,null,null,null,null,null,null,"Ethylene (C2H4)",1.17E-3,1.2600000000000001E-3,1.01E-2,1.8E-5,28.05]
[null,null,null,null,null,null,null,null,null,"Helium (He)",1.6559999999999999E-4,1.785E-4,1.9800000000000002E-2,2.4000000000000001E-5,4.0030000000000001]
[null,null,null,null,null,null,null,null,null,"Ammonia (NH3)",7.0899999999999999E-4,7.6499999999999995E-4,9.7999999999999997E-3,{"$f":"1.9898*10^-5","v":1.9898000000000002E-5},17.030999999999999]
[null,null,null,null,null,null,null,null,null,"Chlorine (Cl2)",2.983E-3,3.2139999999999998E-3,1.32E-2,{"$f":"2.17*10^-5","v":2.1700000000000002E-5},35.453000000000003]
[null,null,null,null,null,null,null,null,null,"Sulfur Dioxide (SO2)",2.6779999999999998E-3,2.8900000000000002E-3,1.2500000000000001E-2,{"$f":"2.5848*10^-5","v":2.5848000000000001E-5},64.066000000000003]
[null,null,null,null,null,null,null,null,null,"Hydrochloric Acid (HCl)",1.5219999999999999E-3,1.639E-3,1.43E-2,2.9E-5,36.460940000000001]
[null,null,null,null,null,null,null,null,null,"Hydrogen (H2)",8.3399999999999994E-5,8.9900000000000003E-5,8.5000000000000006E-3,1.4E-5,2.02]
[null,null,null,null,null,null,null,null,null,"Carbon Dioxide (CO2)",{"$f":"IF('Modified Inputs'!$I$2>70,'10A61 5\" Calcs'!F19,0.001833784)","v":1.833784E-3},{"$f":"IF('Modified Inputs'!$I$2>70,'10A61 5\" Calcs'!G19,0.001978157)","v":1.9781569999999999E-3},1.4853282000000001E-2,2.4919599999999998E-5,44.01]
[null,null,null,null,null,null,null,null,null,"Krypton (Kr)",3.4788509999999998E-3,3.7479499999999999E-3,2.5736330000000002E-2,4.1090399999999975E-5,83.798000000000002]
[null,null,null,null,null,null,null,null,null,"Methyl Chloride (CH3Cl)",2.1277370000000002E-3,2.3022089999999999E-3,1.121953E-2,2.1580799999999998E-5,50.49]
[null,"Real Gases","a","b","MW","standard","normal",null,null,"Neon (Ne)",8.3569720000000001E-4,8.998144E-4,3.119272E-2,3.7229100000000026E-5,20.1797]
[null,"Carbon Dioxide",0.36430000000000001,4.2700000000000001E-5,44.01,1.8309999999999999E-3,1.9740000000000001E-3,null,null,"Acetylene (C2H2)",1.0864869999999999E-3,1.172225E-3,9.9490829999999992E-3,1.7952870000000014E-5,26.04]
[null,"Ammonia",0.42330000000000001,3.7299999999999999E-5,17.030999999999999,7.0899999999999999E-4,7.6499999999999995E-4,null,null,"Mixed Gas",{"$f":"IF(MixedGas!E2=\"Volume %\",MixedGas!A15,\nIF(MixedGas!E2=\"Mass %\",MixedGas!B15,\"\"))","v":""},{"$f":"IF(MixedGas!E2=\"Volume %\",MixedGas!C15,\nIF(MixedGas!E2=\"Mass %\",MixedGas!D15,\"\"))","v":""},{"$f":"MixedGas!E15","v":1},{"$f":"MixedGas!F15","v":false}]
[null,"Chlorine",0.65790000000000004,5.622E-5,35.453000000000003,1.482E-3,1.5989999999999999E-3,null,null,"Hydrogen Sulfide (H2S)",1.426E-3,1.536E-3,1.24E-2,2.3E-5,34.0809]
[null,"Sulfur Dioxide",0.68030000000000002,5.6360000000000002E-5,64.066000000000003,2.6779999999999998E-3,2.8900000000000002E-3,null,null,"Methane (CH4)",6.6529999999999996E-4,7.1679999999999997E-4,1.099E-2,1.8E-5,16.04]
[null,null,null,null,null,null,null,null,null,"Natural Gas",{"$f":"IF(AND('VA Sizing'!$C$4=\"Natural Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!$O$46/'10A61 5\" Calcs'!$M$46,0.0007704)","v":7.7039999999999997E-4},{"$f":"IF(AND('VA Sizing'!$C$4=\"Natural Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!$O$46/'10A61 5\" Calcs'!$N$46,0.00083)","v":8.3000000000000001E-4},1.04E-2,1.7E-5,19]
["Pressure (Pa)","Temp (K)","MW (g/mol)","R","a","b",null,null,null,"Nitric Oxide (NO)",1.2440000000000001E-3,1.34E-3,1.8800000000000001E-2,2.5999999999999998E-5,30.006]
[{"$f":"'Modified Inputs'!$I$2*6894.75729","v":0},{"$f":"('Modified Inputs'!$K$2-32)*5/9+273.15","v":255.37222222222221},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$B$19:$E$22,4,FALSE)","v":{"$error":"#N/A"}},8.3145100000000003,{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$B$19:$E$22,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$B$19:$E$22,3,FALSE)","v":{"$error":"#N/A"}},null,null,null,"Nitrogen (N2)",1.16E-3,1.2509999999999999E-3,1.7559999999999999E-2,2.4000000000000001E-5,28.013400000000001]
[null,null,null,null,null,null,"g/mL",null,null,"Nitrous Oxide (N2O)",1.838E-3,1.98E-3,1.46E-2,2.5999999999999998E-5,44.012999999999998]
[{"$f":"(D25^3)*B25^3","v":9572622815.572525},{"$f":"(D25^2)*A25*(B25^2)+E25*(A25^2)","v":{"$error":"#N/A"}},{"$f":"(A27/B27)+F25","v":{"$error":"#N/A"}},{"$f":"C27/C25","v":{"$error":"#N/A"}},{"$f":"1/D27","v":{"$error":"#N/A"}},{"$f":"E27/1000","v":{"$error":"#N/A"}},{"$f":"F27/1000","v":{"$error":"#N/A"}},null,null,"Oxygen (O2)",1.3259999999999999E-3,1.4289999999999999E-3,2.0299999999999999E-2,2.9E-5,32]
[null,null,null,null,null,null,null,null,null,"Propane (C3H8)",1.8649999999999999E-3,2.0100000000000001E-3,8.0499999999999999E-3,1.4E-5,44.1]
[null,null,null,null,null,null,null,null,null,"Propylene (C3H6)",1.7769999999999999E-3,1.9139999999999999E-3,8.3999999999999995E-3,1.5999999999999999E-5,42.08]
[null,null,null,null,null,null,null,null,null,0,0,0,1,0,1]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["LINEST",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS",null,null,null,"LIQUID",null,null,"RESULTS",null,null,null,null,"GAS",null,null,null,"LIQUID",null,null,"RESULTS"]
[null,"FIRST",null,"MIDDLE",null,"LAST",null,null,"Float","Operating Temp Deg F","Operating Pressure psia","Standard Density","R Standard","R Normal/Actual","Operating Density","Standard Viscosity","temp coeff","t-32","t-70","Operating Viscosity","N","C","W (g/min)","(mL/min)","N","C","W (g/min)","(mL/min)",null,"(mL/min)","Tube/Float",null,"N","C","W","ml/min","N","C","W (g/min)","(mL/min)",null,"(mL/min)","Tube/Float"]
["1/4-25",{"$f":"LINEST('10A61 5\" Curves'!C4:I4,LN('10A61 5\" Curves'!C3:I3))","v":0.13693027110752118},-0.39603758830901137,{"$f":"LINEST('10A61 5\" Curves'!I4:M4,LN('10A61 5\" Curves'!I3:M3))","v":7.4354677851053805E-2},2.1796982542503951E-2,{"$f":"LINEST('10A61 5\" Curves'!M4:Q4,LN('10A61 5\" Curves'!M3:Q3))","v":3.4127758675246346E-2},0.38541445135148822,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},{"$f":"(K46/14.7)*(530/(460+J46))","v":0},{"$f":"(K46/14.7)*(492/(460+J46))","v":0},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M46*'10A61 5\" Calcs'!L46,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N46*'10A61 5\" Calcs'!L46,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"J46-32","v":-32},{"$f":"J46-70","v":-70},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P46+'10A61 5\" Calcs'!Q46*'10A61 5\" Calcs'!S46,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P46+'10A61 5\" Calcs'!Q46*'10A61 5\" Calcs'!R46,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$6/T46)*SQRT((VLOOKUP(I46,$A$3:$B$8,2,FALSE)-O46)*O46)","v":{"$error":"#VALUE!"}},{"$f":"IF(U46<($C$47+0.00001),$B$46*LN(U46)+$C$46,\nIF(U46<($E$47+0.00001),$D$46*LN(U46)+$E$46,\nIF(U46<($G$47+0.0001),$F$46*LN(U46)+$G$46,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(V46*$F$6)*SQRT((VLOOKUP(I46,$A$3:$B$8,2,FALSE)-O46)*O46)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W46/'10A61 5\" Calcs'!L46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W46/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W46/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W46/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W46/'10A61 5\" Calcs'!O46,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I46,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y46<700.00001,$B$46*LN(Y46)+$C$46,\nIF(Y46<10000.00001,$D$46*LN(Y46)+$E$46,\nIF(Y46<200000.0001,$F$46*LN(Y46)+$G$46,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z46*$F$6*SQRT((VLOOKUP(I46,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA46/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X46,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB46,\"\"))","v":""},{"$f":"CONCATENATE($A$46,\"-\",I46)","v":"1/4-25-CD"},null,{"$f":"($E$5/T46)*SQRT((VLOOKUP(I46,$A$3:$B$8,2,FALSE)-O46)*O46)","v":{"$error":"#VALUE!"}},{"$f":"IF(AG46<($C$47+0.00001),$B$46*LN(AG46)+$C$46,\nIF(AG46<($E$47+0.00001),$D$46*LN(AG46)+$E$46,\nIF(AG46<($G$47+0.0001),$F$46*LN(AG46)+$G$46,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(AH46*$F$5)*SQRT((VLOOKUP(I46,$A$3:$B$8,2,FALSE)-O46)*O46)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI46/'10A61 5\" Calcs'!L46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI46/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI46/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI46/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI46/'10A61 5\" Calcs'!O46,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I46,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK46<700.00001,$B$46*LN(AK46)+$C$46,\nIF(AK46<10000.00001,$D$46*LN(AK46)+$E$46,\nIF(AK46<200000.0001,$F$46*LN(AK46)+$G$46,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"AL46*$F$5*SQRT((VLOOKUP(I46,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM46/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ46,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN46,\"\"))","v":""},"1/8-25-CD"]
["ranges",30,700,700,10000,10000,200000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O47/'10A61 5\" Calcs'!M47,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O47/N47,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},{"$f":"(K47/14.7)*(530/(460+J47))","v":0},{"$f":"(K47/14.7)*(492/(460+J47))","v":0},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M47*'10A61 5\" Calcs'!L47,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N47*'10A61 5\" Calcs'!L47,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"J47-32","v":-32},{"$f":"J47-70","v":-70},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P47+'10A61 5\" Calcs'!Q47*'10A61 5\" Calcs'!S47,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P47+'10A61 5\" Calcs'!Q47*'10A61 5\" Calcs'!R47,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U47<($C$47+0.00001),$B$46*LN(U47)+$C$46,\nIF(U47<($E$47+0.00001),$D$46*LN(U47)+$E$46,\nIF(U47<($G$47+0.0001),$F$46*LN(U47)+$G$46,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W47/'10A61 5\" Calcs'!L47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W47/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W47/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W47/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W47/'10A61 5\" Calcs'!O47,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I47,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y47<700.00001,$B$46*LN(Y47)+$C$46,\nIF(Y47<10000.00001,$D$46*LN(Y47)+$E$46,\nIF(Y47<200000.0001,$F$46*LN(Y47)+$G$46,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z47*$F$6*SQRT((VLOOKUP(I47,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA47/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X47,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB47,\"\"))","v":""},{"$f":"CONCATENATE($A$46,\"-\",I47)","v":"1/4-25-SA"},null,{"$f":"($E$5/T47)*SQRT((VLOOKUP(I47,$A$3:$B$8,2,FALSE)-O47)*O47)","v":{"$error":"#VALUE!"}},{"$f":"IF(AG47<($C$47+0.00001),$B$46*LN(AG47)+$C$46,\nIF(AG47<($E$47+0.00001),$D$46*LN(AG47)+$E$46,\nIF(AG47<($G$47+0.0001),$F$46*LN(AG47)+$G$46,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(AH47*$F$5)*SQRT((VLOOKUP(I47,$A$3:$B$8,2,FALSE)-O47)*O47)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI47/'10A61 5\" Calcs'!L47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI47/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI47/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI47/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI47/'10A61 5\" Calcs'!O47,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I47,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK47<700.00001,$B$46*LN(AK47)+$C$46,\nIF(AK47<10000.00001,$D$46*LN(AK47)+$E$46,\nIF(AK47<200000.0001,$F$46*LN(AK47)+$G$46,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"AL47*$F$5*SQRT((VLOOKUP(I47,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM47/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ47,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN47,\"\"))","v":""},"1/8-25-SA"]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O48/'10A61 5\" Calcs'!M48,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O48/N48,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},{"$f":"(K48/14.7)*(530/(460+J48))","v":0},{"$f":"(K48/14.7)*(492/(460+J48))","v":0},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M48*'10A61 5\" Calcs'!L48,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N48*'10A61 5\" Calcs'!L48,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"J48-32","v":-32},{"$f":"J48-70","v":-70},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P48+'10A61 5\" Calcs'!Q48*'10A61 5\" Calcs'!S48,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P48+'10A61 5\" Calcs'!Q48*'10A61 5\" Calcs'!R48,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W48/'10A61 5\" Calcs'!L48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W48/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W48/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W48/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W48/'10A61 5\" Calcs'!O48,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I48,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z48*$F$6*SQRT((VLOOKUP(I48,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA48/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X48,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB48,\"\"))","v":""},"1/4-25-SS",null,{"$f":"($E$5/T48)*SQRT((VLOOKUP(I48,$A$3:$B$8,2,FALSE)-O48)*O48)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI48/'10A61 5\" Calcs'!L48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI48/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI48/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI48/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI48/'10A61 5\" Calcs'!O48,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I48,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL48*$F$5*SQRT((VLOOKUP(I48,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM48/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ48,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN48,\"\"))","v":""},"1/8-25-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O49/'10A61 5\" Calcs'!M49,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O49/N49,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M49*'10A61 5\" Calcs'!L49,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N49*'10A61 5\" Calcs'!L49,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P49+'10A61 5\" Calcs'!Q49*'10A61 5\" Calcs'!S49,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P49+'10A61 5\" Calcs'!Q49*'10A61 5\" Calcs'!R49,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W49/'10A61 5\" Calcs'!L49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W49/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W49/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W49/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W49/'10A61 5\" Calcs'!O49,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I49,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z49*$F$6*SQRT((VLOOKUP(I49,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA49/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X49,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB49,\"\"))","v":""},"1/4-25-CA",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI49/'10A61 5\" Calcs'!L49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI49/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI49/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI49/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI49/'10A61 5\" Calcs'!O49,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I49,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL49*$F$5*SQRT((VLOOKUP(I49,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM49/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ49,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN49,\"\"))","v":""},"1/8-25-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O50/'10A61 5\" Calcs'!M50,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O50/N50,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M50*'10A61 5\" Calcs'!L50,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N50*'10A61 5\" Calcs'!L50,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P50+'10A61 5\" Calcs'!Q50*'10A61 5\" Calcs'!S50,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P50+'10A61 5\" Calcs'!Q50*'10A61 5\" Calcs'!R50,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W50/'10A61 5\" Calcs'!L50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W50/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W50/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W50/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W50/'10A61 5\" Calcs'!O50,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I50,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z50*$F$6*SQRT((VLOOKUP(I50,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA50/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X50,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB50,\"\"))","v":""},"1/4-25-TA",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI50/'10A61 5\" Calcs'!L50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI50/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI50/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI50/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI50/'10A61 5\" Calcs'!O50,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I50,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL50*$F$5*SQRT((VLOOKUP(I50,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM50/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ50,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN50,\"\"))","v":""},"1/8-25-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O51/'10A61 5\" Calcs'!M51,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O51/N51,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M51*'10A61 5\" Calcs'!L51,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N51*'10A61 5\" Calcs'!L51,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P51+'10A61 5\" Calcs'!Q51*'10A61 5\" Calcs'!S51,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P51+'10A61 5\" Calcs'!Q51*'10A61 5\" Calcs'!R51,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W51/'10A61 5\" Calcs'!L51,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W51/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W51/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W51/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W51/'10A61 5\" Calcs'!O51,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I51,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y51<700.00001,$B$46*LN(Y51)+$C$46,\nIF(Y51<10000.00001,$D$46*LN(Y51)+$E$46,\nIF(Y51<200000.0001,$F$46*LN(Y51)+$G$46,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z51*$F$6*SQRT((VLOOKUP(I51,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA51/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X51,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB51,\"\"))","v":""},"1/4-25-BG",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI51/'10A61 5\" Calcs'!L51,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI51/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI51/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI51/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI51/'10A61 5\" Calcs'!O51,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I51,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL51*$F$5*SQRT((VLOOKUP(I51,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM51/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ51,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN51,\"\"))","v":""},"1/8-25-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M52*'10A61 5\" Calcs'!L52,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N52*'10A61 5\" Calcs'!L52,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P52+'10A61 5\" Calcs'!Q52*'10A61 5\" Calcs'!S52,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P52+'10A61 5\" Calcs'!Q52*'10A61 5\" Calcs'!R52,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/4-20",{"$f":"LINEST('10A61 5\" Curves'!C11:J11,LN('10A61 5\" Curves'!C10:J10))","v":0.10605421214896053},-0.33053529151511751,{"$f":"LINEST('10A61 5\" Curves'!J11:N11,LN('10A61 5\" Curves'!J10:N10))","v":7.2043715615787665E-2},-0.10291419257850365,{"$f":"LINEST('10A61 5\" Curves'!N11:R11,LN('10A61 5\" Curves'!N10:R10))","v":2.1074154591499333E-2},0.35692031852738559,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O53/'10A61 5\" Calcs'!M53,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O53/N53,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M53*'10A61 5\" Calcs'!L53,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N53*'10A61 5\" Calcs'!L53,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P53+'10A61 5\" Calcs'!Q53*'10A61 5\" Calcs'!S53,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P53+'10A61 5\" Calcs'!Q53*'10A61 5\" Calcs'!R53,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$6/T53)*SQRT((VLOOKUP(I53,$A$3:$B$8,2,FALSE)-O53)*O53)","v":{"$error":"#VALUE!"}},{"$f":"IF(U53<($C$54+0.00001),$B$53*LN(U53)+$C$53,\nIF(U53<($E$54+0.00001),$D$53*LN(U53)+$E$53,\nIF(U53<($G$54+0.0001),$F$53*LN(U53)+$G$53,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(V53*$F$6)*SQRT((VLOOKUP(I53,$A$3:$B$8,2,FALSE)-O53)*O53)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W53/'10A61 5\" Calcs'!L53,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W53/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W53/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W53/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W53/'10A61 5\" Calcs'!O53,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I53,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y53<600.00001,$B$53*LN(Y53)+$C$53,\nIF(Y53<8500.00001,$D$53*LN(Y53)+$E$53,\nIF(Y53<140000.0001,$F$53*LN(Y53)+$G$53,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z53*$F$6*SQRT((VLOOKUP(I53,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA53/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X53,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB53,\"\"))","v":""},{"$f":"CONCATENATE($A$53,\"-\",I53)","v":"1/4-20-CD"},null,{"$f":"($E$5/T53)*SQRT((VLOOKUP(I53,$A$3:$B$8,2,FALSE)-O53)*O53)","v":{"$error":"#VALUE!"}},{"$f":"IF(AG53<($C$54+0.00001),$B$53*LN(AG53)+$C$53,\nIF(AG53<($E$54+0.00001),$D$53*LN(AG53)+$E$53,\nIF(AG53<($G$54+0.0001),$F$53*LN(AG53)+$G$53,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(AH53*$F$5)*SQRT((VLOOKUP(I53,$A$3:$B$8,2,FALSE)-O53)*O53)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI53/'10A61 5\" Calcs'!L53,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI53/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI53/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI53/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI53/'10A61 5\" Calcs'!O53,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I53,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK53<600.00001,$B$53*LN(AK53)+$C$53,\nIF(AK53<8500.00001,$D$53*LN(AK53)+$E$53,\nIF(AK53<140000.0001,$F$53*LN(AK53)+$G$53,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"AL53*$F$5*SQRT((VLOOKUP(I53,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM53/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ53,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN53,\"\"))","v":""},"1/8-20-CD"]
["ranges",30,600,600,8500,8500,140000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O54/'10A61 5\" Calcs'!M54,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O54/N54,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M54*'10A61 5\" Calcs'!L54,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N54*'10A61 5\" Calcs'!L54,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P54+'10A61 5\" Calcs'!Q54*'10A61 5\" Calcs'!S54,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P54+'10A61 5\" Calcs'!Q54*'10A61 5\" Calcs'!R54,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U54<($C$54+0.00001),$B$53*LN(U54)+$C$53,\nIF(U54<($E$54+0.00001),$D$53*LN(U54)+$E$53,\nIF(U54<($G$54+0.0001),$F$53*LN(U54)+$G$53,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W54/'10A61 5\" Calcs'!L54,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W54/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W54/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W54/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W54/'10A61 5\" Calcs'!O54,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I54,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y54<600.00001,$B$53*LN(Y54)+$C$53,\nIF(Y54<8500.00001,$D$53*LN(Y54)+$E$53,\nIF(Y54<140000.0001,$F$53*LN(Y54)+$G$53,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z54*$F$6*SQRT((VLOOKUP(I54,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA54/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X54,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB54,\"\"))","v":""},{"$f":"CONCATENATE($A$53,\"-\",I54)","v":"1/4-20-SA"},null,{"$error":"#VALUE!"},{"$f":"IF(AG54<($C$54+0.00001),$B$53*LN(AG54)+$C$53,\nIF(AG54<($E$54+0.00001),$D$53*LN(AG54)+$E$53,\nIF(AG54<($G$54+0.0001),$F$53*LN(AG54)+$G$53,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(AH54*$F$5)*SQRT((VLOOKUP(I54,$A$3:$B$8,2,FALSE)-O54)*O54)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI54/'10A61 5\" Calcs'!L54,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI54/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI54/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI54/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI54/'10A61 5\" Calcs'!O54,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I54,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK54<600.00001,$B$53*LN(AK54)+$C$53,\nIF(AK54<8500.00001,$D$53*LN(AK54)+$E$53,\nIF(AK54<140000.0001,$F$53*LN(AK54)+$G$53,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"AL54*$F$5*SQRT((VLOOKUP(I54,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM54/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ54,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN54,\"\"))","v":""},"1/8-20-SA"]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O55/'10A61 5\" Calcs'!M55,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O55/N55,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M55*'10A61 5\" Calcs'!L55,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N55*'10A61 5\" Calcs'!L55,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P55+'10A61 5\" Calcs'!Q55*'10A61 5\" Calcs'!S55,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P55+'10A61 5\" Calcs'!Q55*'10A61 5\" Calcs'!R55,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$6/T55)*SQRT((VLOOKUP(I55,$A$3:$B$8,2,FALSE)-O55)*O55)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W55/'10A61 5\" Calcs'!L55,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W55/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W55/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W55/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W55/'10A61 5\" Calcs'!O55,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I55,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z55*$F$6*SQRT((VLOOKUP(I55,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA55/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X55,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB55,\"\"))","v":""},"1/4-20-SS",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI55/'10A61 5\" Calcs'!L55,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI55/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI55/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI55/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI55/'10A61 5\" Calcs'!O55,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I55,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK55<200.00001,(10^-8)*('10A61 5\" Calcs'!$AK$55^3)-(7*(10^-6))*($AK$55^2)+(0.0022*$AK$55)-0.0175,\nIF(AK55<600.00001,$B$53*LN(AK55)+$C$53,\nIF(AK55<8500.00001,$D$53*LN(AK55)+$E$53,\nIF(AK55<140000.0001,$F$53*LN(AK55)+$G$53,\"\"))))","v":{"$error":"#DIV/0!"}},{"$f":"AL55*$F$5*SQRT((VLOOKUP(I55,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM55/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ55,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN55,\"\"))","v":""},"1/8-20-SS"]
[null,30,200,200,600,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O56/'10A61 5\" Calcs'!M56,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O56/N56,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M56*'10A61 5\" Calcs'!L56,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N56*'10A61 5\" Calcs'!L56,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P56+'10A61 5\" Calcs'!Q56*'10A61 5\" Calcs'!S56,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P56+'10A61 5\" Calcs'!Q56*'10A61 5\" Calcs'!R56,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W56/'10A61 5\" Calcs'!L56,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W56/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W56/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W56/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W56/'10A61 5\" Calcs'!O56,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I56,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z56*$F$6*SQRT((VLOOKUP(I56,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA56/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X56,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB56,\"\"))","v":""},"1/4-20-CA",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI56/'10A61 5\" Calcs'!L56,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI56/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI56/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI56/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI56/'10A61 5\" Calcs'!O56,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I56,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL56*$F$5*SQRT((VLOOKUP(I56,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM56/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ56,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN56,\"\"))","v":""},"1/8-20-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O57/'10A61 5\" Calcs'!M57,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O57/N57,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M57*'10A61 5\" Calcs'!L57,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N57*'10A61 5\" Calcs'!L57,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P57+'10A61 5\" Calcs'!Q57*'10A61 5\" Calcs'!S57,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P57+'10A61 5\" Calcs'!Q57*'10A61 5\" Calcs'!R57,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W57/'10A61 5\" Calcs'!L57,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W57/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W57/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W57/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W57/'10A61 5\" Calcs'!O57,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I57,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z57*$F$6*SQRT((VLOOKUP(I57,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA57/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X57,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB57,\"\"))","v":""},"1/4-20-TA",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI57/'10A61 5\" Calcs'!L57,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI57/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI57/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI57/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI57/'10A61 5\" Calcs'!O57,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I57,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL57*$F$5*SQRT((VLOOKUP(I57,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM57/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ57,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN57,\"\"))","v":""},"1/8-20-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O58/'10A61 5\" Calcs'!M58,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O58/N58,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M58*'10A61 5\" Calcs'!L58,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N58*'10A61 5\" Calcs'!L58,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P58+'10A61 5\" Calcs'!Q58*'10A61 5\" Calcs'!S58,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P58+'10A61 5\" Calcs'!Q58*'10A61 5\" Calcs'!R58,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$6/T58)*SQRT((VLOOKUP(I58,$A$3:$B$8,2,FALSE)-O58)*O58)","v":{"$error":"#VALUE!"}},{"$f":"IF(U58<($C$54+0.00001),$B$53*LN(U58)+$C$53,\nIF(U58<($E$54+0.00001),$D$53*LN(U58)+$E$53,\nIF(U58<($G$54+0.0001),$F$53*LN(U58)+$G$53,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W58/'10A61 5\" Calcs'!L58,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W58/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W58/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W58/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W58/'10A61 5\" Calcs'!O58,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I58,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z58*$F$6*SQRT((VLOOKUP(I58,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA58/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X58,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB58,\"\"))","v":""},"1/4-20-BG",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI58/'10A61 5\" Calcs'!L58,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI58/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI58/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI58/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI58/'10A61 5\" Calcs'!O58,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I58,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL58*$F$5*SQRT((VLOOKUP(I58,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM58/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ58,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN58,\"\"))","v":""},"1/8-20-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M59*'10A61 5\" Calcs'!L59,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N59*'10A61 5\" Calcs'!L59,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P59+'10A61 5\" Calcs'!Q59*'10A61 5\" Calcs'!S59,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P59+'10A61 5\" Calcs'!Q59*'10A61 5\" Calcs'!R59,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/4-16",{"$f":"LINEST('10A61 5\" Curves'!C18:I18,LN('10A61 5\" Curves'!C17:I17))","v":7.6534645743448371E-2},-0.25200878207267718,{"$f":"LINEST('10A61 5\" Curves'!H18:M18,LN('10A61 5\" Curves'!H17:M17))","v":6.721366903477323E-2},-0.18174281222972793,{"$f":"LINEST('10A61 5\" Curves'!M18:Q18,LN('10A61 5\" Curves'!M17:Q17))","v":2.586865038101787E-2},0.18081707489285032,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O60/'10A61 5\" Calcs'!M60,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O60/N60,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M60*'10A61 5\" Calcs'!L60,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N60*'10A61 5\" Calcs'!L60,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P60+'10A61 5\" Calcs'!Q60*'10A61 5\" Calcs'!S60,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P60+'10A61 5\" Calcs'!Q60*'10A61 5\" Calcs'!R60,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$6/T60)*SQRT((VLOOKUP(I60,$A$3:$B$8,2,FALSE)-O60)*O60)","v":{"$error":"#VALUE!"}},{"$f":"IF(U60<($C$61+0.00001),-0.00000130626*(U60^2)+0.001049*U60-0.0068,\nIF(U60<($E$61+0.00001),$D$60*LN(U60)+$E$60,\nIF(U60<($G$61+0.0001),$F$60*LN(U60)+$G$60,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W60/'10A61 5\" Calcs'!L60,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W60/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W60/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W60/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W60/'10A61 5\" Calcs'!O60,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I60,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y60<($C$61+0.00001),-0.00000130626*(Y60^2)+0.001049*Y60-0.0068,\nIF(Y60<($E$61+0.00001),$D$60*LN(Y60)+$E$60,\nIF(Y60<($G$61+0.0001),$F$60*LN(Y60)+$G$60,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z60*$F$6*SQRT((VLOOKUP(I60,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA60/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X60,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB60,\"\"))","v":""},{"$f":"CONCATENATE($A$60,\"-\",I60)","v":"1/4-16-CD"},null,{"$f":"($E$5/T60)*SQRT((VLOOKUP(I60,$A$3:$B$8,2,FALSE)-O60)*O60)","v":{"$error":"#VALUE!"}},{"$f":"IF(AG60<($C$61+0.00001),0.0012*(AG60^(0.9159)),\nIF(AG60<($E$61+0.00001),$D$60*LN(AG60)+$E$60,\nIF(AG60<($G$61+0.0001),$F$60*LN(AG60)+$G$60,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(AH60*$F$5)*SQRT((VLOOKUP(I60,$A$3:$B$8,2,FALSE)-O60)*O60)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI60/'10A61 5\" Calcs'!L60,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI60/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI60/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI60/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI60/'10A61 5\" Calcs'!O60,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I60,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK60<($C$61+0.00001),-0.00000130626*(AK60^2)+0.001049*AK60-0.0068,\nIF(AK60<($E$61+0.00001),$D$60*LN(AK60)+$E$60,\nIF(AK60<($G$61+0.0001),$F$60*LN(AK60)+$G$60,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"AL60*$F$5*SQRT((VLOOKUP(I60,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM60/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ60,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN60,\"\"))","v":""},"1/8-16-CD"]
["ranges",30,300,300,8000,8000,75000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O61/'10A61 5\" Calcs'!M61,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O61/N61,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M61*'10A61 5\" Calcs'!L61,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N61*'10A61 5\" Calcs'!L61,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P61+'10A61 5\" Calcs'!Q61*'10A61 5\" Calcs'!S61,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P61+'10A61 5\" Calcs'!Q61*'10A61 5\" Calcs'!R61,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U61<($C$61+0.00001),-0.00000130626*(U61^2)+0.001049*U61-0.0068,\nIF(U61<($E$61+0.00001),$D$60*LN(U61)+$E$60,\nIF(U61<($G$61+0.0001),$F$60*LN(U61)+$G$60,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W61/'10A61 5\" Calcs'!L61,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W61/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W61/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W61/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W61/'10A61 5\" Calcs'!O61,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I61,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y61<($C$61+0.00001),-0.00000130626*(Y61^2)+0.001049*Y61-0.0068,\nIF(Y61<($E$61+0.00001),$D$60*LN(Y61)+$E$60,\nIF(Y61<($G$61+0.0001),$F$60*LN(Y61)+$G$60,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z61*$F$6*SQRT((VLOOKUP(I61,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA61/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X61,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB61,\"\"))","v":""},{"$f":"CONCATENATE($A$60,\"-\",I61)","v":"1/4-16-SA"},null,{"$error":"#VALUE!"},{"$f":"IF(AG61<($C$61+0.00001),0.0012*(AG61^(0.9159)),\nIF(AG61<($E$61+0.00001),$D$60*LN(AG61)+$E$60,\nIF(AG61<($G$61+0.0001),$F$60*LN(AG61)+$G$60,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI61/'10A61 5\" Calcs'!L61,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI61/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI61/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI61/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI61/'10A61 5\" Calcs'!O61,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I61,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(AK61<($C$61+0.00001),-0.00000130626*(AK61^2)+0.001049*AK61-0.0068,\nIF(AK61<($E$61+0.00001),$D$60*LN(AK61)+$E$60,\nIF(AK61<($G$61+0.0001),$F$60*LN(AK61)+$G$60,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"AL61*$F$5*SQRT((VLOOKUP(I61,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM61/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ61,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN61,\"\"))","v":""},"1/8-16-SA"]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O62/'10A61 5\" Calcs'!M62,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O62/N62,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M62*'10A61 5\" Calcs'!L62,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N62*'10A61 5\" Calcs'!L62,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P62+'10A61 5\" Calcs'!Q62*'10A61 5\" Calcs'!S62,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P62+'10A61 5\" Calcs'!Q62*'10A61 5\" Calcs'!R62,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W62/'10A61 5\" Calcs'!L62,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W62/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W62/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W62/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W62/'10A61 5\" Calcs'!O62,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I62,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z62*$F$6*SQRT((VLOOKUP(I62,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA62/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X62,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB62,\"\"))","v":""},"1/4-16-SS",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI62/'10A61 5\" Calcs'!L62,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI62/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI62/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI62/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI62/'10A61 5\" Calcs'!O62,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I62,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL62*$F$5*SQRT((VLOOKUP(I62,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM62/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ62,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN62,\"\"))","v":""},"1/8-16-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O63/'10A61 5\" Calcs'!M63,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O63/N63,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M63*'10A61 5\" Calcs'!L63,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N63*'10A61 5\" Calcs'!L63,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P63+'10A61 5\" Calcs'!Q63*'10A61 5\" Calcs'!S63,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P63+'10A61 5\" Calcs'!Q63*'10A61 5\" Calcs'!R63,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U63<($C$61+0.00001),-0.00000130626*(U63^2)+0.001049*U63-0.0068,\nIF(U63<($E$61+0.00001),$D$60*LN(U63)+$E$60,\nIF(U63<(80000+0.0001),$F$60*LN(U63)+$G$60,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W63/'10A61 5\" Calcs'!L63,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W63/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W63/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W63/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W63/'10A61 5\" Calcs'!O63,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I63,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z63*$F$6*SQRT((VLOOKUP(I63,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA63/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X63,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB63,\"\"))","v":""},"1/4-16-CA",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI63/'10A61 5\" Calcs'!L63,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI63/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI63/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI63/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI63/'10A61 5\" Calcs'!O63,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I63,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL63*$F$5*SQRT((VLOOKUP(I63,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM63/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ63,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN63,\"\"))","v":""},"1/8-16-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O64/'10A61 5\" Calcs'!M64,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O64/N64,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M64*'10A61 5\" Calcs'!L64,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N64*'10A61 5\" Calcs'!L64,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P64+'10A61 5\" Calcs'!Q64*'10A61 5\" Calcs'!S64,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P64+'10A61 5\" Calcs'!Q64*'10A61 5\" Calcs'!R64,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U64<($C$61+0.00001),-0.00000130626*(U64^2)+0.001049*U64-0.0068,\nIF(U64<($E$61+0.00001),$D$60*LN(U64)+$E$60,\nIF(U64<(80000+0.0001),$F$60*LN(U64)+$G$60,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W64/'10A61 5\" Calcs'!L64,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W64/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W64/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W64/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W64/'10A61 5\" Calcs'!O64,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I64,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z64*$F$6*SQRT((VLOOKUP(I64,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA64/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X64,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB64,\"\"))","v":""},"1/4-16-TA",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI64/'10A61 5\" Calcs'!L64,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI64/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI64/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI64/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI64/'10A61 5\" Calcs'!O64,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I64,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL64*$F$5*SQRT((VLOOKUP(I64,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM64/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ64,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN64,\"\"))","v":""},"1/8-16-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O65/'10A61 5\" Calcs'!M65,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O65/N65,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M65*'10A61 5\" Calcs'!L65,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N65*'10A61 5\" Calcs'!L65,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P65+'10A61 5\" Calcs'!Q65*'10A61 5\" Calcs'!S65,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P65+'10A61 5\" Calcs'!Q65*'10A61 5\" Calcs'!R65,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W65/'10A61 5\" Calcs'!L65,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W65/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W65/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W65/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W65/'10A61 5\" Calcs'!O65,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I65,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z65*$F$6*SQRT((VLOOKUP(I65,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA65/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X65,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB65,\"\"))","v":""},"1/4-16-BG",null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!AI65/'10A61 5\" Calcs'!L65,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!AI65/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",AI65/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!AI65/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!AI65/'10A61 5\" Calcs'!O65,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I65,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"AL65*$F$5*SQRT((VLOOKUP(I65,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AM65/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!AJ65,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AN65,\"\"))","v":""},"1/8-16-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M66*'10A61 5\" Calcs'!L66,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N66*'10A61 5\" Calcs'!L66,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P66+'10A61 5\" Calcs'!Q66*'10A61 5\" Calcs'!S66,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P66+'10A61 5\" Calcs'!Q66*'10A61 5\" Calcs'!R66,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/4-10",{"$f":"LINEST('10A61 5\" Curves'!C25:I25,LN('10A61 5\" Curves'!C24:I24))","v":3.8881296361878995E-2},-0.13870160570633588,{"$f":"LINEST('10A61 5\" Curves'!H25:M25,LN('10A61 5\" Curves'!H24:M24))","v":4.6536783643606437E-2},-0.17698438438977909,{"$f":"LINEST('10A61 5\" Curves'!M25:Q25,LN('10A61 5\" Curves'!M24:Q24))","v":1.764149215888693E-2},7.6956909161375597E-2,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O67/'10A61 5\" Calcs'!M67,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O67/N67,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M67*'10A61 5\" Calcs'!L67,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N67*'10A61 5\" Calcs'!L67,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P67+'10A61 5\" Calcs'!Q67*'10A61 5\" Calcs'!S67,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P67+'10A61 5\" Calcs'!Q67*'10A61 5\" Calcs'!R67,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U67<($C$68+0.00001),-0.000000136062*(U67^2)+0.000276*U67-0.00185,\nIF(U67<($E$68+0.00001),$D$67*LN(U67)+$E$67,\nIF(U67<($G$68+0.0001),$F$67*LN(U67)+$G$67,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W67/'10A61 5\" Calcs'!L67,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W67/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W67/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W67/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W67/'10A61 5\" Calcs'!O67,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I67,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y67<($C$68+0.00001),-0.000000136062*(Y67^2)+0.000276*Y67-0.00185,\nIF(Y67<($E$68+0.00001),$D$67*LN(Y67)+$E$67,\nIF(Y67<($G$68+0.0001),$F$67*LN(Y67)+$G$67,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z67*$F$6*SQRT((VLOOKUP(I67,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA67/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X67,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB67,\"\"))","v":""},{"$f":"CONCATENATE($A$67,\"-\",I67)","v":"1/4-10-CD"}]
["ranges",30,650,650,7000,7000,120000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O68/'10A61 5\" Calcs'!M68,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O68/N68,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M68*'10A61 5\" Calcs'!L68,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N68*'10A61 5\" Calcs'!L68,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P68+'10A61 5\" Calcs'!Q68*'10A61 5\" Calcs'!S68,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P68+'10A61 5\" Calcs'!Q68*'10A61 5\" Calcs'!R68,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U68<($C$68+0.00001),-0.000000136062*(U68^2)+0.000276*U68-0.00185,\nIF(U68<($E$68+0.00001),$D$67*LN(U68)+$E$67,\nIF(U68<($G$68+0.0001),$F$67*LN(U68)+$G$67,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W68/'10A61 5\" Calcs'!L68,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W68/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W68/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W68/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W68/'10A61 5\" Calcs'!O68,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I68,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y68<($C$68+0.00001),-0.000000136062*(Y68^2)+0.000276*Y68-0.00185,\nIF(Y68<($E$68+0.00001),$D$67*LN(Y68)+$E$67,\nIF(Y68<($G$68+0.0001),$F$67*LN(Y68)+$G$67,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z68*$F$6*SQRT((VLOOKUP(I68,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA68/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X68,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB68,\"\"))","v":""},{"$f":"CONCATENATE($A$67,\"-\",I68)","v":"1/4-10-SA"}]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O69/'10A61 5\" Calcs'!M69,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O69/N69,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M69*'10A61 5\" Calcs'!L69,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N69*'10A61 5\" Calcs'!L69,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P69+'10A61 5\" Calcs'!Q69*'10A61 5\" Calcs'!S69,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P69+'10A61 5\" Calcs'!Q69*'10A61 5\" Calcs'!R69,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W69/'10A61 5\" Calcs'!L69,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W69/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W69/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W69/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W69/'10A61 5\" Calcs'!O69,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I69,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z69*$F$6*SQRT((VLOOKUP(I69,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA69/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X69,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB69,\"\"))","v":""},"1/4-10-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O70/'10A61 5\" Calcs'!M70,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O70/N70,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M70*'10A61 5\" Calcs'!L70,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N70*'10A61 5\" Calcs'!L70,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P70+'10A61 5\" Calcs'!Q70*'10A61 5\" Calcs'!S70,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P70+'10A61 5\" Calcs'!Q70*'10A61 5\" Calcs'!R70,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W70/'10A61 5\" Calcs'!L70,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W70/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W70/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W70/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W70/'10A61 5\" Calcs'!O70,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I70,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z70*$F$6*SQRT((VLOOKUP(I70,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA70/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X70,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB70,\"\"))","v":""},"1/4-10-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O71/'10A61 5\" Calcs'!M71,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O71/N71,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M71*'10A61 5\" Calcs'!L71,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N71*'10A61 5\" Calcs'!L71,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P71+'10A61 5\" Calcs'!Q71*'10A61 5\" Calcs'!S71,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P71+'10A61 5\" Calcs'!Q71*'10A61 5\" Calcs'!R71,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W71/'10A61 5\" Calcs'!L71,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W71/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W71/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W71/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W71/'10A61 5\" Calcs'!O71,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I71,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z71*$F$6*SQRT((VLOOKUP(I71,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA71/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X71,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB71,\"\"))","v":""},"1/4-10-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O72/'10A61 5\" Calcs'!M72,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O72/N72,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M72*'10A61 5\" Calcs'!L72,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N72*'10A61 5\" Calcs'!L72,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P72+'10A61 5\" Calcs'!Q72*'10A61 5\" Calcs'!S72,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P72+'10A61 5\" Calcs'!Q72*'10A61 5\" Calcs'!R72,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W72/'10A61 5\" Calcs'!L72,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W72/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W72/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W72/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W72/'10A61 5\" Calcs'!O72,\"\")))))","v":""},{"$f":"($E$6/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I72,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z72*$F$6*SQRT((VLOOKUP(I72,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA72/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X72,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB72,\"\"))","v":""},"1/4-10-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M73*'10A61 5\" Calcs'!L73,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N73*'10A61 5\" Calcs'!L73,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P73+'10A61 5\" Calcs'!Q73*'10A61 5\" Calcs'!S73,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P73+'10A61 5\" Calcs'!Q73*'10A61 5\" Calcs'!R73,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/8-12",{"$f":"LINEST('10A61 5\" Curves'!C32:G32,LN('10A61 5\" Curves'!C31:G31))","v":4.7255852732625454E-2},-0.16646068504766809,{"$f":"LINEST('10A61 5\" Curves'!G32:L32,LN('10A61 5\" Curves'!G31:L31))","v":5.5560320912742454E-2},-0.19661152684529073,{"$f":"LINEST('10A61 5\" Curves'!L32:Q32,LN('10A61 5\" Curves'!L31:Q31))","v":2.3705608932839174E-2},7.7415135109961536E-2,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O74/'10A61 5\" Calcs'!M74,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O74/N74,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M74*'10A61 5\" Calcs'!L74,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N74*'10A61 5\" Calcs'!L74,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P74+'10A61 5\" Calcs'!Q74*'10A61 5\" Calcs'!S74,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P74+'10A61 5\" Calcs'!Q74*'10A61 5\" Calcs'!R74,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$5/T74)*SQRT((VLOOKUP(I74,$A$3:$B$8,2,FALSE)-O74)*O74)","v":{"$error":"#VALUE!"}},{"$f":"IF(U74<($C$75+0.00001),-0.000000388581*(U74^2)+0.000491-0.0039,\nIF(U74<($E$75+0.00001),$D$74*LN(U74)+$E$74,\nIF(U74<($G$75+0.0001),$F$74*LN(U74)+$G$74,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(V74*$F$5)*SQRT((VLOOKUP(I74,$A$3:$B$8,2,FALSE)-O74)*O74)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W74/'10A61 5\" Calcs'!L74,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W74/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W74/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W74/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W74/'10A61 5\" Calcs'!O74,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I74,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y74<($C$75+0.00001),-0.000000388581*(Y74^2)+0.000491*Y74-0.0039,\nIF(Y74<($E$75+0.00001),$D$74*LN(Y74)+$E$74,\nIF(Y74<($G$75+0.0001),$F$74*LN(Y74)+$G$74,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z74*$F$5*SQRT((VLOOKUP(I74,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA74/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X74,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB74,\"\"))","v":""},{"$f":"CONCATENATE($A$74,\"-\",I74)","v":"1/8-12-CD"}]
["ranges",36,400,400,6000,6000,120000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O75/'10A61 5\" Calcs'!M75,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O75/N75,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M75*'10A61 5\" Calcs'!L75,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N75*'10A61 5\" Calcs'!L75,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P75+'10A61 5\" Calcs'!Q75*'10A61 5\" Calcs'!S75,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P75+'10A61 5\" Calcs'!Q75*'10A61 5\" Calcs'!R75,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$5/T75)*SQRT((VLOOKUP(I75,$A$3:$B$8,2,FALSE)-O75)*O75)","v":{"$error":"#VALUE!"}},{"$f":"IF(U75<($C$75+0.00001),-0.000000388581*(U75^2)+0.000491-0.0039,\nIF(U75<($E$75+0.00001),$D$74*LN(U75)+$E$74,\nIF(U75<($G$75+0.0001),$F$74*LN(U75)+$G$74,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(V75*$F$5)*SQRT((VLOOKUP(I75,$A$3:$B$8,2,FALSE)-O75)*O75)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W75/'10A61 5\" Calcs'!L75,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W75/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W75/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W75/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W75/'10A61 5\" Calcs'!O75,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I75,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y75<($C$75+0.00001),-0.000000388581*(Y75^2)+0.000491*Y75-0.0039,\nIF(Y75<($E$75+0.00001),$D$74*LN(Y75)+$E$74,\nIF(Y75<($G$75+0.0001),$F$74*LN(Y75)+$G$74,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z75*$F$5*SQRT((VLOOKUP(I75,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA75/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X75,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB75,\"\"))","v":""},{"$f":"CONCATENATE($A$74,\"-\",I75)","v":"1/8-12-SA"}]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O76/'10A61 5\" Calcs'!M76,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O76/N76,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M76*'10A61 5\" Calcs'!L76,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N76*'10A61 5\" Calcs'!L76,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P76+'10A61 5\" Calcs'!Q76*'10A61 5\" Calcs'!S76,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P76+'10A61 5\" Calcs'!Q76*'10A61 5\" Calcs'!R76,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W76/'10A61 5\" Calcs'!L76,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W76/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W76/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W76/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W76/'10A61 5\" Calcs'!O76,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I76,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z76*$F$5*SQRT((VLOOKUP(I76,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA76/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X76,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB76,\"\"))","v":""},"1/8-12-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O77/'10A61 5\" Calcs'!M77,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O77/N77,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M77*'10A61 5\" Calcs'!L77,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N77*'10A61 5\" Calcs'!L77,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P77+'10A61 5\" Calcs'!Q77*'10A61 5\" Calcs'!S77,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P77+'10A61 5\" Calcs'!Q77*'10A61 5\" Calcs'!R77,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W77/'10A61 5\" Calcs'!L77,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W77/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W77/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W77/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W77/'10A61 5\" Calcs'!O77,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I77,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z77*$F$5*SQRT((VLOOKUP(I77,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA77/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X77,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB77,\"\"))","v":""},"1/8-12-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O78/'10A61 5\" Calcs'!M78,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O78/N78,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M78*'10A61 5\" Calcs'!L78,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N78*'10A61 5\" Calcs'!L78,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P78+'10A61 5\" Calcs'!Q78*'10A61 5\" Calcs'!S78,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P78+'10A61 5\" Calcs'!Q78*'10A61 5\" Calcs'!R78,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W78/'10A61 5\" Calcs'!L78,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W78/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W78/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W78/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W78/'10A61 5\" Calcs'!O78,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I78,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z78*$F$5*SQRT((VLOOKUP(I78,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA78/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X78,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB78,\"\"))","v":""},"1/8-12-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O79/'10A61 5\" Calcs'!M79,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O79/N79,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M79*'10A61 5\" Calcs'!L79,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N79*'10A61 5\" Calcs'!L79,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P79+'10A61 5\" Calcs'!Q79*'10A61 5\" Calcs'!S79,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P79+'10A61 5\" Calcs'!Q79*'10A61 5\" Calcs'!R79,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W79/'10A61 5\" Calcs'!L79,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W79/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W79/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W79/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W79/'10A61 5\" Calcs'!O79,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I79,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z79*$F$5*SQRT((VLOOKUP(I79,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA79/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X79,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB79,\"\"))","v":""},"1/8-12-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M80*'10A61 5\" Calcs'!L80,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N80*'10A61 5\" Calcs'!L80,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P80+'10A61 5\" Calcs'!Q80*'10A61 5\" Calcs'!S80,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P80+'10A61 5\" Calcs'!Q80*'10A61 5\" Calcs'!R80,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/8-08",{"$f":"LINEST('10A61 5\" Curves'!C39:I39,LN('10A61 5\" Curves'!C38:I38))","v":2.7090217810864719E-2},-0.10552270173101685,{"$f":"LINEST('10A61 5\" Curves'!I39:N39,LN('10A61 5\" Curves'!I38:N38))","v":3.6864230379455472E-2},-0.15303689113769881,{"$f":"LINEST('10A61 5\" Curves'!N39:Q39,LN('10A61 5\" Curves'!N38:Q38))","v":1.5449270343535326E-2},4.1407611540326239E-2,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O81/'10A61 5\" Calcs'!M81,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O81/N81,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M81*'10A61 5\" Calcs'!L81,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N81*'10A61 5\" Calcs'!L81,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P81+'10A61 5\" Calcs'!Q81*'10A61 5\" Calcs'!S81,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P81+'10A61 5\" Calcs'!Q81*'10A61 5\" Calcs'!R81,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$5/T81)*SQRT((VLOOKUP(I81,$A$3:$B$8,2,FALSE)-O81)*O81)","v":{"$error":"#VALUE!"}},{"$f":"IF(U81<($C$82+0.00001),-5.28542*(10^(-8))*('10A61 5\" Calcs'!U81^2)+(0.000153*'10A61 5\" Calcs'!U81)-0.00184,\nIF(U81<($E$82+0.00001),$D$81*LN(U81)+$E$81,\nIF(U81<($G$82+0.0001),$F$81*LN(U81)+$G$81,\"\")))","v":{"$error":"#VALUE!"}},{"$f":"(V81*$F$5)*SQRT((VLOOKUP(I81,$A$3:$B$8,2,FALSE)-O81)*O81)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W81/'10A61 5\" Calcs'!L81,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W81/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W81/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W81/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W81/'10A61 5\" Calcs'!O81,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I81,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y81<($C$82+0.00001),(-5.28542*(10^(-8))*('10A61 5\" Calcs'!Y81^2)+(0.000153*'10A61 5\" Calcs'!Y81)-0.00184),\nIF(Y81<($E$82+0.00001),$D$81*LN(Y81)+$E$81,\nIF(Y81<($G$82+0.0001),$F$81*LN(Y81)+$G$81,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z81*$F$5*SQRT((VLOOKUP(I81,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA81/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X81,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB81,\"\"))","v":""},{"$f":"CONCATENATE($A$81,\"-\",I81)","v":"1/8-08-CD"}]
["ranges",32,1000,1000,9000,9000,120000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O82/'10A61 5\" Calcs'!M82,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O82/N82,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M82*'10A61 5\" Calcs'!L82,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N82*'10A61 5\" Calcs'!L82,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P82+'10A61 5\" Calcs'!Q82*'10A61 5\" Calcs'!S82,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P82+'10A61 5\" Calcs'!Q82*'10A61 5\" Calcs'!R82,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U82<($C$82+0.00001),-5.28542*(10^(-8))*('10A61 5\" Calcs'!U82^2)+(0.000153*'10A61 5\" Calcs'!U82)-0.00184,\nIF(U82<($E$82+0.00001),$D$81*LN(U82)+$E$81,\nIF(U82<($G$82+0.0001),$F$81*LN(U82)+$G$81,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W82/'10A61 5\" Calcs'!L82,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W82/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W82/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W82/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W82/'10A61 5\" Calcs'!O82,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I82,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y82<($C$82+0.00001),(-5.28542*(10^(-8))*('10A61 5\" Calcs'!Y82^2)+(0.000153*'10A61 5\" Calcs'!Y82)-0.00184),\nIF(Y82<($E$82+0.00001),$D$81*LN(Y82)+$E$81,\nIF(Y82<($G$82+0.0001),$F$81*LN(Y82)+$G$81,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z82*$F$5*SQRT((VLOOKUP(I82,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA82/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X82,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB82,\"\"))","v":""},{"$f":"CONCATENATE($A$81,\"-\",I82)","v":"1/8-08-SA"}]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O83/'10A61 5\" Calcs'!M83,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O83/N83,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M83*'10A61 5\" Calcs'!L83,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N83*'10A61 5\" Calcs'!L83,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P83+'10A61 5\" Calcs'!Q83*'10A61 5\" Calcs'!S83,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P83+'10A61 5\" Calcs'!Q83*'10A61 5\" Calcs'!R83,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U83<($C$82+0.00001),-5.28542*(10^(-8))*('10A61 5\" Calcs'!U83^2)+(0.000153*'10A61 5\" Calcs'!U83)-0.00184,\nIF(U83<($E$82+0.00001),$D$81*LN(U83)+$E$81,\nIF(U83<($G$82+0.0001),$F$81*LN(U83)+$G$81,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W83/'10A61 5\" Calcs'!L83,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W83/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W83/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W83/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W83/'10A61 5\" Calcs'!O83,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I83,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y83<($C$82+0.00001),(-5.28542*(10^(-8))*('10A61 5\" Calcs'!Y83^2)+(0.000153*'10A61 5\" Calcs'!Y83)-0.00184),\nIF(Y83<($E$82+0.00001),$D$81*LN(Y83)+$E$81,\nIF(Y83<($G$82+0.0001),$F$81*LN(Y83)+$G$81,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z83*$F$5*SQRT((VLOOKUP(I83,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA83/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X83,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB83,\"\"))","v":""},"1/8-08-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O84/'10A61 5\" Calcs'!M84,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O84/N84,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M84*'10A61 5\" Calcs'!L84,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N84*'10A61 5\" Calcs'!L84,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P84+'10A61 5\" Calcs'!Q84*'10A61 5\" Calcs'!S84,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P84+'10A61 5\" Calcs'!Q84*'10A61 5\" Calcs'!R84,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U84<($C$82+0.00001),-5.28542*(10^(-8))*('10A61 5\" Calcs'!U84^2)+(0.000153*'10A61 5\" Calcs'!U84)-0.00184,\nIF(U84<($E$82+0.00001),$D$81*LN(U84)+$E$81,\nIF(U84<($G$82+0.0001),$F$81*LN(U84)+$G$81,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W84/'10A61 5\" Calcs'!L84,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W84/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W84/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W84/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W84/'10A61 5\" Calcs'!O84,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I84,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y84<($C$82+0.00001),(-5.28542*(10^(-8))*('10A61 5\" Calcs'!Y84^2)+(0.000153*'10A61 5\" Calcs'!Y84)-0.00184),\nIF(Y84<($E$82+0.00001),$D$81*LN(Y84)+$E$81,\nIF(Y84<($G$82+0.0001),$F$81*LN(Y84)+$G$81,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z84*$F$5*SQRT((VLOOKUP(I84,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA84/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X84,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB84,\"\"))","v":""},"1/8-08-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O85/'10A61 5\" Calcs'!M85,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O85/N85,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M85*'10A61 5\" Calcs'!L85,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N85*'10A61 5\" Calcs'!L85,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P85+'10A61 5\" Calcs'!Q85*'10A61 5\" Calcs'!S85,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P85+'10A61 5\" Calcs'!Q85*'10A61 5\" Calcs'!R85,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U85<($C$82+0.00001),-5.28542*(10^(-8))*('10A61 5\" Calcs'!U85^2)+(0.000153*'10A61 5\" Calcs'!U85)-0.00184,\nIF(U85<($E$82+0.00001),$D$81*LN(U85)+$E$81,\nIF(U85<($G$82+0.0001),$F$81*LN(U85)+$G$81,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W85/'10A61 5\" Calcs'!L85,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W85/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W85/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W85/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W85/'10A61 5\" Calcs'!O85,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I85,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y85<($C$82+0.00001),(-5.28542*(10^(-8))*('10A61 5\" Calcs'!Y85^2)+(0.000153*'10A61 5\" Calcs'!Y85)-0.00184),\nIF(Y85<($E$82+0.00001),$D$81*LN(Y85)+$E$81,\nIF(Y85<($G$82+0.0001),$F$81*LN(Y85)+$G$81,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z85*$F$5*SQRT((VLOOKUP(I85,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA85/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X85,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB85,\"\"))","v":""},"1/8-08-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O86/'10A61 5\" Calcs'!M86,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O86/N86,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M86*'10A61 5\" Calcs'!L86,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N86*'10A61 5\" Calcs'!L86,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P86+'10A61 5\" Calcs'!Q86*'10A61 5\" Calcs'!S86,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P86+'10A61 5\" Calcs'!Q86*'10A61 5\" Calcs'!R86,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$5/T86)*SQRT((VLOOKUP(I86,$A$3:$B$8,2,FALSE)-O86)*O86)","v":{"$error":"#VALUE!"}},{"$f":"IF(U86<($C$82+0.00001),-5.28542*(10^(-8))*('10A61 5\" Calcs'!U86^2)+(0.000153*'10A61 5\" Calcs'!U86)-0.00184,\nIF(U86<($E$82+0.00001),$D$81*LN(U86)+$E$81,\nIF(U86<($G$82+0.0001),$F$81*LN(U86)+$G$81,\"\")))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W86/'10A61 5\" Calcs'!L86,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W86/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W86/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W86/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W86/'10A61 5\" Calcs'!O86,\"\")))))","v":""},{"$f":"($E$5/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I86,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y86<($C$82+0.00001),(-5.28542*(10^(-8))*('10A61 5\" Calcs'!Y86^2)+(0.000153*'10A61 5\" Calcs'!Y86)-0.00184),\nIF(Y86<($E$82+0.00001),$D$81*LN(Y86)+$E$81,\nIF(Y86<($G$82+0.0001),$F$81*LN(Y86)+$G$81,\"\")))","v":{"$error":"#DIV/0!"}},{"$f":"Z86*$F$5*SQRT((VLOOKUP(I86,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA86/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X86,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB86,\"\"))","v":""},"1/8-08-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M87*'10A61 5\" Calcs'!L87,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N87*'10A61 5\" Calcs'!L87,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P87+'10A61 5\" Calcs'!Q87*'10A61 5\" Calcs'!S87,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P87+'10A61 5\" Calcs'!Q87*'10A61 5\" Calcs'!R87,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/16-12",{"$f":"LINEST('10A61 5\" Curves'!C46:I46,LN('10A61 5\" Curves'!C45:I45))","v":4.300757436785712E-2},-0.15260497600639988,{"$f":"LINEST('10A61 5\" Curves'!I46:N46,LN('10A61 5\" Curves'!I45:N45))","v":7.0246648651037663E-2},-0.29094561446499306,{"$f":"LINEST('10A61 5\" Curves'!J46:Q46,LN('10A61 5\" Curves'!J45:Q45))","v":5.8483618301608302E-2},-0.20449305659111172,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O88/'10A61 5\" Calcs'!M88,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O88/N88,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M88*'10A61 5\" Calcs'!L88,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N88*'10A61 5\" Calcs'!L88,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P88+'10A61 5\" Calcs'!Q88*'10A61 5\" Calcs'!S88,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P88+'10A61 5\" Calcs'!Q88*'10A61 5\" Calcs'!R88,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$4/T88)*SQRT((VLOOKUP(I88,$A$3:$B$8,2,FALSE)-O88)*O88)","v":{"$error":"#VALUE!"}},{"$f":"IF(U88<($E$89+0.00001),-0.00000016607*(U88^2)+0.000372*U88-0.003,\nIF(U88<($G$89+0.00001),$F$88*LN(U88)+$G$88,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"(V88*$F$4)*SQRT((VLOOKUP(I88,$A$3:$B$8,2,FALSE)-O88)*O88)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W88/'10A61 5\" Calcs'!L88,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W88/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W88/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W88/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W88/'10A61 5\" Calcs'!O88,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I88,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y88<($E$89+0.00001),-0.00000016607*(Y88^2)+0.000372*Y88-0.003,\nIF(Y88<($G$89+0.00001),$F$88*LN(Y88)+$G$88,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"Z88*$F$4*SQRT((VLOOKUP(I88,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA88/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X88,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB88,\"\"))","v":""},{"$f":"CONCATENATE($A$88,\"-\",I88)","v":"1/16-12-CD"}]
["ranges",null,null,32,600,600,8500,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O89/'10A61 5\" Calcs'!M89,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O89/N89,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M89*'10A61 5\" Calcs'!L89,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N89*'10A61 5\" Calcs'!L89,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P89+'10A61 5\" Calcs'!Q89*'10A61 5\" Calcs'!S89,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P89+'10A61 5\" Calcs'!Q89*'10A61 5\" Calcs'!R89,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$f":"($E$4/T89)*SQRT((VLOOKUP(I89,$A$3:$B$8,2,FALSE)-O89)*O89)","v":{"$error":"#VALUE!"}},{"$f":"IF(U89<($E$89+0.00001),-0.00000016607*(U89^2)+0.000372*U89-0.003,\nIF(U89<($G$89+0.00001),$F$88*LN(U89)+$G$88,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"(V89*$F$4)*SQRT((VLOOKUP(I89,$A$3:$B$8,2,FALSE)-O89)*O89)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W89/'10A61 5\" Calcs'!L89,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W89/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W89/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W89/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W89/'10A61 5\" Calcs'!O89,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I89,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y89<($E$89+0.00001),-0.00000016607*(Y89^2)+0.000372*Y89-0.003,\nIF(Y89<($G$89+0.00001),$F$88*LN(Y89)+$G$88,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"Z89*$F$4*SQRT((VLOOKUP(I89,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA89/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X89,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB89,\"\"))","v":""},{"$f":"CONCATENATE($A$88,\"-\",I89)","v":"1/16-12-SA"}]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O90/'10A61 5\" Calcs'!M90,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O90/N90,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M90*'10A61 5\" Calcs'!L90,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N90*'10A61 5\" Calcs'!L90,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P90+'10A61 5\" Calcs'!Q90*'10A61 5\" Calcs'!S90,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P90+'10A61 5\" Calcs'!Q90*'10A61 5\" Calcs'!R90,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W90/'10A61 5\" Calcs'!L90,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W90/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W90/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W90/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W90/'10A61 5\" Calcs'!O90,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I90,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z90*$F$4*SQRT((VLOOKUP(I90,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA90/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X90,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB90,\"\"))","v":""},"1/16-12-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O91/'10A61 5\" Calcs'!M91,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O91/N91,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M91*'10A61 5\" Calcs'!L91,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N91*'10A61 5\" Calcs'!L91,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P91+'10A61 5\" Calcs'!Q91*'10A61 5\" Calcs'!S91,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P91+'10A61 5\" Calcs'!Q91*'10A61 5\" Calcs'!R91,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U91<($E$89+0.00001),-0.00000016607*(U91^2)+0.000372*U91-0.003,\nIF(U91<(10000+0.00001),$F$88*LN(U91)+$G$88,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W91/'10A61 5\" Calcs'!L91,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W91/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W91/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W91/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W91/'10A61 5\" Calcs'!O91,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I91,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z91*$F$4*SQRT((VLOOKUP(I91,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA91/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X91,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB91,\"\"))","v":""},"1/16-12-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O92/'10A61 5\" Calcs'!M92,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O92/N92,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M92*'10A61 5\" Calcs'!L92,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N92*'10A61 5\" Calcs'!L92,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P92+'10A61 5\" Calcs'!Q92*'10A61 5\" Calcs'!S92,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P92+'10A61 5\" Calcs'!Q92*'10A61 5\" Calcs'!R92,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U92<($E$89+0.00001),-0.00000016607*(U92^2)+0.000372*U92-0.003,\nIF(U92<(10000+0.00001),$F$88*LN(U92)+$G$88,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W92/'10A61 5\" Calcs'!L92,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W92/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W92/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W92/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W92/'10A61 5\" Calcs'!O92,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I92,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z92*$F$4*SQRT((VLOOKUP(I92,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA92/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X92,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB92,\"\"))","v":""},"1/16-12-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O93/'10A61 5\" Calcs'!M93,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O93/N93,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M93*'10A61 5\" Calcs'!L93,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N93*'10A61 5\" Calcs'!L93,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P93+'10A61 5\" Calcs'!Q93*'10A61 5\" Calcs'!S93,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P93+'10A61 5\" Calcs'!Q93*'10A61 5\" Calcs'!R93,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W93/'10A61 5\" Calcs'!L93,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W93/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W93/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W93/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W93/'10A61 5\" Calcs'!O93,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I93,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z93*$F$4*SQRT((VLOOKUP(I93,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA93/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X93,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB93,\"\"))","v":""},"1/16-12-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M94*'10A61 5\" Calcs'!L94,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N94*'10A61 5\" Calcs'!L94,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P94+'10A61 5\" Calcs'!Q94*'10A61 5\" Calcs'!S94,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P94+'10A61 5\" Calcs'!Q94*'10A61 5\" Calcs'!R94,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/16-16",{"$f":"LINEST('10A61 5\" Curves'!C53:I53,LN('10A61 5\" Curves'!C52:I52))","v":8.0860042972230498E-2},-0.30259454024760679,{"$f":"LINEST('10A61 5\" Curves'!I53:N53,LN('10A61 5\" Curves'!I52:N52))","v":9.6521584802503765E-2},-0.36161930881375187,{"$f":"LINEST('10A61 5\" Curves'!K53:Q53,LN('10A61 5\" Curves'!K52:Q52))","v":6.8878016634463177E-2},-0.16054852279840959,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O95/'10A61 5\" Calcs'!M95,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O95/N95,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M95*'10A61 5\" Calcs'!L95,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N95*'10A61 5\" Calcs'!L95,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P95+'10A61 5\" Calcs'!Q95*'10A61 5\" Calcs'!S95,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P95+'10A61 5\" Calcs'!Q95*'10A61 5\" Calcs'!R95,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U95<($E$96+0.00001),-0.000000349508*(U95^2)+0.000653*U95-0.00603,\nIF(U95<($G$96+0.00001),$F$95*LN(U95)+$G$95,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"(V95*$F$4)*SQRT((VLOOKUP(I95,$A$3:$B$8,2,FALSE)-O95)*O95)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W95/'10A61 5\" Calcs'!L95,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W95/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W95/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W95/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W95/'10A61 5\" Calcs'!O95,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I95,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y95<($E$96+0.00001),-0.000000349508*(Y95^2)+0.000653*Y95-0.00603,\nIF(Y95<($G$96+0.00001),$F$95*LN(Y95)+$G$95,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"Z95*$F$4*SQRT((VLOOKUP(I95,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA95/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X95,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB95,\"\"))","v":""},{"$f":"CONCATENATE($A$95,\"-\",I95)","v":"1/16-16-CD"}]
["ranges",null,null,45,700,700,6000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O96/'10A61 5\" Calcs'!M96,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O96/N96,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M96*'10A61 5\" Calcs'!L96,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N96*'10A61 5\" Calcs'!L96,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P96+'10A61 5\" Calcs'!Q96*'10A61 5\" Calcs'!S96,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P96+'10A61 5\" Calcs'!Q96*'10A61 5\" Calcs'!R96,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U96<($E$96+0.00001),-0.000000349508*(U96^2)+0.000653*U96-0.00603,\nIF(U96<($G$96+0.00001),$F$95*LN(U96)+$G$95,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W96/'10A61 5\" Calcs'!L96,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W96/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W96/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W96/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W96/'10A61 5\" Calcs'!O96,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I96,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y96<($E$96+0.00001),-0.000000349508*(Y96^2)+0.000653*Y96-0.00603,\nIF(Y96<($G$96+0.00001),$F$95*LN(Y96)+$G$95,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"Z96*$F$4*SQRT((VLOOKUP(I96,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA96/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X96,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB96,\"\"))","v":""},{"$f":"CONCATENATE($A$95,\"-\",I96)","v":"1/16-16-SA"}]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O97/'10A61 5\" Calcs'!M97,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O97/N97,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M97*'10A61 5\" Calcs'!L97,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N97*'10A61 5\" Calcs'!L97,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P97+'10A61 5\" Calcs'!Q97*'10A61 5\" Calcs'!S97,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P97+'10A61 5\" Calcs'!Q97*'10A61 5\" Calcs'!R97,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U97<($E$96+0.00001),-0.000000349508*(U97^2)+0.000653*U97-0.00603,\nIF(U97<(10000+0.00001),$F$95*LN(U97)+$G$95,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W97/'10A61 5\" Calcs'!L97,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W97/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W97/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W97/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W97/'10A61 5\" Calcs'!O97,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I97,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z97*$F$4*SQRT((VLOOKUP(I97,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA97/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X97,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB97,\"\"))","v":""},"1/16-16-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O98/'10A61 5\" Calcs'!M98,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O98/N98,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M98*'10A61 5\" Calcs'!L98,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N98*'10A61 5\" Calcs'!L98,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P98+'10A61 5\" Calcs'!Q98*'10A61 5\" Calcs'!S98,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P98+'10A61 5\" Calcs'!Q98*'10A61 5\" Calcs'!R98,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U98<($E$96+0.00001),-0.000000349508*(U98^2)+0.000653*U98-0.00603,\nIF(U98<(10000+0.00001),$F$95*LN(U98)+$G$95,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W98/'10A61 5\" Calcs'!L98,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W98/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W98/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W98/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W98/'10A61 5\" Calcs'!O98,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I98,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z98*$F$4*SQRT((VLOOKUP(I98,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA98/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X98,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB98,\"\"))","v":""},"1/16-16-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O99/'10A61 5\" Calcs'!M99,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O99/N99,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M99*'10A61 5\" Calcs'!L99,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N99*'10A61 5\" Calcs'!L99,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P99+'10A61 5\" Calcs'!Q99*'10A61 5\" Calcs'!S99,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P99+'10A61 5\" Calcs'!Q99*'10A61 5\" Calcs'!R99,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U99<($E$96+0.00001),-0.000000349508*(U99^2)+0.000653*U99-0.00603,\nIF(U99<(10000+0.00001),$F$95*LN(U99)+$G$95,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W99/'10A61 5\" Calcs'!L99,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W99/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W99/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W99/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W99/'10A61 5\" Calcs'!O99,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I99,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z99*$F$4*SQRT((VLOOKUP(I99,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA99/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X99,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB99,\"\"))","v":""},"1/16-16-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O100/'10A61 5\" Calcs'!M100,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O100/N100,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M100*'10A61 5\" Calcs'!L100,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N100*'10A61 5\" Calcs'!L100,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P100+'10A61 5\" Calcs'!Q100*'10A61 5\" Calcs'!S100,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P100+'10A61 5\" Calcs'!Q100*'10A61 5\" Calcs'!R100,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W100/'10A61 5\" Calcs'!L100,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W100/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W100/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W100/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W100/'10A61 5\" Calcs'!O100,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I100,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z100*$F$4*SQRT((VLOOKUP(I100,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA100/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X100,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB100,\"\"))","v":""},"1/16-16-BG"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M101*'10A61 5\" Calcs'!L101,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N101*'10A61 5\" Calcs'!L101,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},null,null,null,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P101+'10A61 5\" Calcs'!Q101*'10A61 5\" Calcs'!S101,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P101+'10A61 5\" Calcs'!Q101*'10A61 5\" Calcs'!R101,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""}]
["1/16-20",{"$f":"LINEST('10A61 5\" Curves'!C60:I60,LN('10A61 5\" Curves'!C59:I59))","v":9.6862819836838282E-2},-0.33868340717390177,{"$f":"LINEST('10A61 5\" Curves'!I60:N60,LN('10A61 5\" Curves'!I59:N59))","v":0.16040373817984574},-0.66463356035143339,{"$f":"LINEST('10A61 5\" Curves'!M60:Q60,LN('10A61 5\" Curves'!M59:Q59))","v":8.513160940324041E-2},-0.17613640636267758,null,"CD",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O102/'10A61 5\" Calcs'!M102,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O102/N102,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M102*'10A61 5\" Calcs'!L102,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N102*'10A61 5\" Calcs'!L102,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P102+'10A61 5\" Calcs'!Q102*'10A61 5\" Calcs'!S102,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P102+'10A61 5\" Calcs'!Q102*'10A61 5\" Calcs'!R102,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U102<($E$103+0.00001),-0.00000066163*(U102^2)+0.001036*U102-0.01083,\nIF(U102<($G$103+0.00001),$F$102*LN(U102)+$G$102,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"(V102*$F$4)*SQRT((VLOOKUP(I102,$A$3:$B$8,2,FALSE)-O102)*O102)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W102/'10A61 5\" Calcs'!L102,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W102/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W102/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W102/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W102/'10A61 5\" Calcs'!O102,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I102,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y102<($E$103+0.00001),-0.00000066163*(Y102^2)+0.001036*Y102-0.01083,\nIF(Y102<($G$103+0.00001),$F$102*LN(Y102)+$G$102,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"Z102*$F$4*SQRT((VLOOKUP(I102,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA102/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X102,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB102,\"\"))","v":""},{"$f":"CONCATENATE($A$102,\"-\",I102)","v":"1/16-20-CD"}]
["ranges",null,null,36,500,500,5000,null,"SA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O103/'10A61 5\" Calcs'!M103,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O103/N103,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M103*'10A61 5\" Calcs'!L103,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N103*'10A61 5\" Calcs'!L103,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P103+'10A61 5\" Calcs'!Q103*'10A61 5\" Calcs'!S103,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P103+'10A61 5\" Calcs'!Q103*'10A61 5\" Calcs'!R103,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U103<($E$103+0.00001),-0.00000066163*(U103^2)+0.001036*U103-0.01083,\nIF(U103<($G$103+0.00001),$F$102*LN(U103)+$G$102,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W103/'10A61 5\" Calcs'!L103,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W103/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W103/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W103/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W103/'10A61 5\" Calcs'!O103,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I103,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"IF(Y103<($E$103+0.00001),-0.00000066163*(Y103^2)+0.001036*Y103-0.01083,\nIF(Y103<($G$103+0.00001),$F$102*LN(Y103)+$G$102,\"\"))","v":{"$error":"#DIV/0!"}},{"$f":"Z103*$F$4*SQRT((VLOOKUP(I103,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA103/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X103,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB103,\"\"))","v":""},{"$f":"CONCATENATE($A$102,\"-\",I103)","v":"1/16-20-SA"}]
[null,null,null,null,null,null,null,null,"SS",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O104/'10A61 5\" Calcs'!M104,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O104/N104,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M104*'10A61 5\" Calcs'!L104,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N104*'10A61 5\" Calcs'!L104,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P104+'10A61 5\" Calcs'!Q104*'10A61 5\" Calcs'!S104,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P104+'10A61 5\" Calcs'!Q104*'10A61 5\" Calcs'!R104,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U104<($E$103+0.00001),-0.00000066163*(U104^2)+0.001036*U104-0.01083,\nIF(U104<(9000+0.00001),$F$102*LN(U104)+$G$102,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W104/'10A61 5\" Calcs'!L104,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W104/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W104/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W104/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W104/'10A61 5\" Calcs'!O104,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I104,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z104*$F$4*SQRT((VLOOKUP(I104,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA104/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X104,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB104,\"\"))","v":""},"1/16-20-SS"]
[null,null,null,null,null,null,null,null,"CA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O105/'10A61 5\" Calcs'!M105,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O105/N105,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M105*'10A61 5\" Calcs'!L105,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N105*'10A61 5\" Calcs'!L105,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P105+'10A61 5\" Calcs'!Q105*'10A61 5\" Calcs'!S105,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P105+'10A61 5\" Calcs'!Q105*'10A61 5\" Calcs'!R105,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U105<($E$103+0.00001),-0.00000066163*(U105^2)+0.001036*U105-0.01083,\nIF(U105<(10000+0.00001),$F$102*LN(U105)+$G$102,\"\"))","v":{"$error":"#VALUE!"}},{"$f":"(V105*$F$4)*SQRT((VLOOKUP(I105,$A$3:$B$8,2,FALSE)-O105)*O105)","v":{"$error":"#VALUE!"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W105/'10A61 5\" Calcs'!L105,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W105/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W105/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W105/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W105/'10A61 5\" Calcs'!O105,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I105,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z105*$F$4*SQRT((VLOOKUP(I105,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA105/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X105,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB105,\"\"))","v":""},"1/16-20-CA"]
[null,null,null,null,null,null,null,null,"TA",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O106/'10A61 5\" Calcs'!M106,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O106/N106,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M106*'10A61 5\" Calcs'!L106,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N106*'10A61 5\" Calcs'!L106,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P106+'10A61 5\" Calcs'!Q106*'10A61 5\" Calcs'!S106,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P106+'10A61 5\" Calcs'!Q106*'10A61 5\" Calcs'!R106,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U106<($E$103+0.00001),-0.00000066163*(U106^2)+0.001036*U106-0.01083,\nIF(U106<(10000+0.00001),$F$102*LN(U106)+$G$102,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W106/'10A61 5\" Calcs'!L106,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W106/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W106/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W106/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W106/'10A61 5\" Calcs'!O106,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I106,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z106*$F$4*SQRT((VLOOKUP(I106,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA106/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X106,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB106,\"\"))","v":""},"1/16-20-TA"]
[null,null,null,null,null,null,null,null,"BG",{"$f":"'Modified Inputs'!$K$2","v":0},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O107/'10A61 5\" Calcs'!M107,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O107/N107,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},0,0,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$6=\"at Operating Conditions\"),'Modified Inputs'!$M$2,\nIF(OR(AND('VA Sizing'!$C$4=\"Carbon Dioxide\",'Modified Inputs'!$I$2>70),'VA Sizing'!$C$4=\"Ammonia\",'VA Sizing'!$C$4=\"Chlorine\",'VA Sizing'!$C$4=\"Sulfur Dioxide\"),'10A61 5\" Calcs'!$G$27,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!M107*'10A61 5\" Calcs'!L107,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!N107*'10A61 5\" Calcs'!L107,\"\")))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$B$20,\"\"))","v":""},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$M$29,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$N$28,5,FALSE)","v":{"$error":"#N/A"}},-32,-70,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\"),'Modified Inputs'!$G$2,\nIF('VA Sizing'!$C$5=\"Standard\",'10A61 5\" Calcs'!P107+'10A61 5\" Calcs'!Q107*'10A61 5\" Calcs'!S107,\nIF(OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!P107+'10A61 5\" Calcs'!Q107*'10A61 5\" Calcs'!R107,\"\"))),IF('VA Sizing'!$C$4=\"Steam\",Steam!$C$20,\"\"))","v":""},{"$error":"#VALUE!"},{"$f":"IF(U107<($E$103+0.00001),-0.00000066163*(U107^2)+0.001036*U107-0.01083,\nIF(U107<($G$103+0.00001),$F$102*LN(U107)+$G$102,\"\"))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Operating Conditions\"),'10A61 5\" Calcs'!W107/'10A61 5\" Calcs'!L107,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$4=\" Other\",NOT('VA Sizing'!$C$5=\"Actual\"),'VA Sizing'!$C$6=\"at Reference Conditions\"),'10A61 5\" Calcs'!W107/'Modified Inputs'!$M$4,\nIF('VA Sizing'!$C$5=\"Standard\",W107/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF('VA Sizing'!$C$5=\"Normal\",'10A61 5\" Calcs'!W107/VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF('VA Sizing'!$C$5=\"Actual\",'10A61 5\" Calcs'!W107/'10A61 5\" Calcs'!O107,\"\")))))","v":""},{"$f":"($E$4/'Modified Inputs'!$G$2)*SQRT((VLOOKUP('10A61 5\" Calcs'!I107,'10A61 5\" Calcs'!$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$f":"Z107*$F$4*SQRT((VLOOKUP(I107,$A$3:$B$8,2,FALSE)-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)","v":{"$error":"#DIV/0!"}},{"$f":"AA107/'Modified Inputs'!$M$2","v":{"$error":"#DIV/0!"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",'10A61 5\" Calcs'!X107,\nIF('VA Sizing'!$C$3=\"Liquid\",'10A61 5\" Calcs'!AB107,\"\"))","v":""},"1/16-20-BG"]

{"sheet":"10A32 Capacity","index":39,"n_rows":62,"n_cols":73,"rows_kept":62,"cut":false,"hidden":true,"merged":[[3,22,3,24],[3,29,3,30],[3,37,3,39],[3,41,3,45],[23,57,23,59]]}
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liquid Flow",null,null,null,null,"Gas Flow",null,null,null,null,null,null,null,null,null,"Flow Outputs",null,null,null,"Modified Outputs"]
[null,null,"Equivalent Water L/h","Equivalent Air SCFM","Name","Mass","Density","Vstd","Vmax","Psta bar(g)","Code","Size","Description","W","N","N1","Pos(N1)","N2","K1","K2","K",null,"Q L/min","Q USGal/min","M3/h","Compress Normal","Compress Standard","Q M3/h",null,"Q M3/h","Scale Type",null,"BT","BU","BV","BZ",null,"Max\nM3/h","Min\nM3/h","Scale Type",null,"Max Specified Units","Min Specified Units","Max Rounded","Min Rounded","Concatenated","Code","Name","Scale Type","Size","Description","Vstd","Vmax","Psta bar(g)","Pmin bar(g)","Equivalent Water L/h",null,"Max","Range","Code","Name","Scale Type","Size","Flow Range","Vstd","Vmax","Psta bar(g)","Pmin bar(g)","Top Descriptor","Bottom Descriptor"]
[null,null,1,2.137431502212804E-2,"K-06-1.0",4.0599999999999996,7.31,4,8,-100,"01","1/4\"",{"$f":"K6&\" \"&\":\"&\" \"&L6&\" \"&\"Diameter Tube\"&\" \"&C6&\" \"&\"L/h\"","v":"01 : 1/4\" Diameter Tube 1 L/h"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F6*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G6)),\nSQRT(F6*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G6)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N6),cP/'10A32 Capacity'!N6),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N6),\"\"))","v":""},{"$f":"HLOOKUP(O6,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P6,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q6+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A24,0,'10A32 Capacity'!Q6)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A24,0,'10A32 Capacity'!Q6+1)","v":{"$error":"#N/A"}},{"$f":"EXP(LN(S6)-((LN(S6)-LN(T6))*(LN(O6)-LN(P6)))/(LN(R6)-LN(P6)))","v":{"$error":"#N/A"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U6*N6/(1000*'10A61 5\" Calcs'!$O$46),U6*N6/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"W6*0.2642","v":{"$error":"#N/A"}},{"$f":"W6*(60)/1000","v":{"$error":"#N/A"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y6/'10A32 Capacity'!AA6,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y6/'10A32 Capacity'!Z6,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y6,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB6,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O6>'10A32 Tables'!S24),'10A32 Tables'!T24,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O6>'10A32 Tables'!Q24),'10A32 Tables'!R24,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O6>'10A32 Tables'!O24),'10A32 Tables'!P24,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O6>'10A32 Tables'!M24),'10A32 Tables'!N24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB24),'10A32 Tables'!AC24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z24),'10A32 Tables'!AA24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X24),'10A32 Tables'!Y24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V24),'10A32 Tables'!W24,1))))))))","v":1},null,{"$f":"-2+INT(LOG10(AD6))","v":{"$error":"#VALUE!"}},{"$f":"AD6*(10^(0-AG6))","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP(AH6,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE6),VLOOKUP(AI6,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE6+3,TRUE),VLOOKUP(AI6,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$f":"AI6*(10^AG6)","v":{"$error":"#VALUE!"}},{"$f":"AJ6*(10^(AG6))","v":{"$error":"#VALUE!"}},{"$f":"AE6","v":1},null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA6-0.0000001)),\"\",AL6/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM6/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(AP6=\"\",0,\nIF(AP6<0.99999,ROUND(AP6,2),\nIF(AP6<9.999,ROUND(AP6,2),\nIF(AP6<99.99,ROUND(AP6,1),\nIF(AP6<999.99,ROUND(AP6,0),\nIF(AP6<9999.99,ROUND(AP6,-1),\nIF(AP6<99999,ROUND(AP6,-2),ROUND(AP6,2))))))))","v":0},{"$f":"IF(AR6=0,0,ROUND(AQ6,1))","v":0},{"$f":"AS6&\" \"&\"-\"&\" \"&AR6","v":"0 - 0"},{"$f":"K6","v":"01"},{"$f":"E6","v":"K-06-1.0"},{"$f":"AN6","v":1},{"$f":"L6","v":"1/4\""},{"$f":"M6","v":"01 : 1/4\" Diameter Tube 1 L/h"},{"$f":"H6","v":4},{"$f":"I6","v":8},-100,0,1,{"$f":"AU6&\" \"&\":\"&\" \"&AX6&\" \"&\"Diameter Tube\"","v":"01 : 1/4\" Diameter Tube"},{"$f":"MAX(IF($AP$6:$AP$32<('VA Sizing'!$C$12-0.00000000001),'10A32 Capacity'!$AP$6:$AP$32))","v":0},{"$f":"VLOOKUP(BF6,$AP$6:$AT$32,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"BH6&\" \"&\":\"&\" \"&BK6&\" \"&\"Dia. Tube\"","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(BF6,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(VLOOKUP(BF6,$AP$6:$AT$32,3,FALSE),0)","v":0},{"$f":"BF6","v":0}]
[null,null,1.6,3.2977514600140402E-2,"K-07-1.6",4.0599999999999996,7.31,4,8,-100,"02","1/4\"",{"$f":"K7&\" \"&\":\"&\" \"&L7&\" \"&\"Diameter Tube\"&\" \"&C7&\" \"&\"L/h\"","v":"02 : 1/4\" Diameter Tube 1.6 L/h"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F7*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G7)),\nSQRT(F7*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G7)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N7),cP/'10A32 Capacity'!N7),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N7),\"\"))","v":""},{"$f":"HLOOKUP(O7,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P7,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q7+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A25,0,'10A32 Capacity'!Q7)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A25,0,'10A32 Capacity'!Q7+1)","v":{"$error":"#N/A"}},{"$f":"EXP(LN(S7)-((LN(S7)-LN(T7))*(LN(O7)-LN(P7)))/(LN(R7)-LN(P7)))","v":{"$error":"#N/A"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U7*N7/(1000*'10A61 5\" Calcs'!$O$46),U7*N7/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"W7*0.2642","v":{"$error":"#N/A"}},{"$f":"W7*(60)/1000","v":{"$error":"#N/A"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y7/'10A32 Capacity'!AA7,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y7/'10A32 Capacity'!Z7,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y7,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB7,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O7>'10A32 Tables'!S25),'10A32 Tables'!T25,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O7>'10A32 Tables'!Q25),'10A32 Tables'!R25,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O7>'10A32 Tables'!O25),'10A32 Tables'!P25,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O7>'10A32 Tables'!M25),'10A32 Tables'!N25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB25),'10A32 Tables'!AC25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z25),'10A32 Tables'!AA25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X25),'10A32 Tables'!Y25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V25),'10A32 Tables'!W25,1))))))))","v":1},null,{"$f":"-2+INT(LOG10(AD7))","v":{"$error":"#VALUE!"}},{"$f":"AD7*(10^(0-AG7))","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP(AH7,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE7),VLOOKUP(AI7,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE7+3,TRUE),VLOOKUP(AI7,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"AE7","v":1},null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA7-0.0000001)),\"\",AL7/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM7/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(AP7=\"\",0,\nIF(AP7<0.99999,ROUND(AP7,2),\nIF(AP7<9.999,ROUND(AP7,2),\nIF(AP7<99.99,ROUND(AP7,1),\nIF(AP7<999.99,ROUND(AP7,0),\nIF(AP7<9999.99,ROUND(AP7,-1),\nIF(AP7<99999,ROUND(AP7,-2),ROUND(AP7,2))))))))","v":0},{"$f":"IF(AR7=0,0,ROUND(AQ7,1))","v":0},{"$f":"AS7&\" \"&\"-\"&\" \"&AR7","v":"0 - 0"},{"$f":"K7","v":"02"},{"$f":"E7","v":"K-07-1.6"},{"$f":"AN7","v":1},{"$f":"L7","v":"1/4\""},{"$f":"M7","v":"02 : 1/4\" Diameter Tube 1.6 L/h"},{"$f":"H7","v":4},{"$f":"I7","v":8},{"$f":"J7","v":-100},0,1.6,{"$f":"AU7&\" \"&\":\"&\" \"&AX7&\" \"&\"Diameter Tube\"","v":"02 : 1/4\" Diameter Tube"},{"$f":"MIN(IF($AP$6:$AP$32>=('VA Sizing'!$C$12-0.00000000001),'10A32 Capacity'!$AP$6:$AP$32))","v":0},{"$f":"VLOOKUP(BF7,$AP$6:$AT$32,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"BH7&\" \"&\":\"&\" \"&BK7&\" \"&\"Dia. Tube\"","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(BF7,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(VLOOKUP(BF7,$AP$6:$AT$32,3,FALSE),0)","v":0},{"$f":"BF7","v":0}]
[null,null,2.5,6.1069471473222961E-2,"K-08-2.5",4.0599999999999996,7.31,6,8,-100,"03","1/4\"","03 : 1/4\" Diameter Tube 2.5 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F8*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G8)),\nSQRT(F8*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G8)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N8),cP/'10A32 Capacity'!N8),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N8),\"\"))","v":""},{"$f":"HLOOKUP(O8,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P8,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q8+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A26,0,'10A32 Capacity'!Q8)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A26,0,'10A32 Capacity'!Q8+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U8*N8/(1000*'10A61 5\" Calcs'!$O$46),U8*N8/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y8/'10A32 Capacity'!AA8,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y8/'10A32 Capacity'!Z8,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y8,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB8,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O8>'10A32 Tables'!S26),'10A32 Tables'!T26,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O8>'10A32 Tables'!Q26),'10A32 Tables'!R26,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O8>'10A32 Tables'!O26),'10A32 Tables'!P26,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O8>'10A32 Tables'!M26),'10A32 Tables'!N26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB26),'10A32 Tables'!AC26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z26),'10A32 Tables'!AA26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X26),'10A32 Tables'!Y26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V26),'10A32 Tables'!W26,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH8,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE8),VLOOKUP(AI8,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE8+3,TRUE),VLOOKUP(AI8,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA8-0.0000001)),\"\",AL8/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM8/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","03","K-08-2.5",1,"1/4\"","03 : 1/4\" Diameter Tube 2.5 L/h",6,8,-100,0,2.5,"03 : 1/4\" Diameter Tube",{"$f":"MIN(IF($AP$6:$AP$32>BF7,'10A32 Capacity'!$AP$6:$AP$32))","v":0},{"$error":"#N/A"},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"VLOOKUP(BF8,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,0,0]
[null,null,4,9.7711154351156751E-2,"K-09-4",4.0599999999999996,7.31,6,8,-100,"04","1/4\"","04 : 1/4\" Diameter Tube 4 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F9*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G9)),\nSQRT(F9*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G9)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N9),cP/'10A32 Capacity'!N9),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N9),\"\"))","v":""},{"$f":"HLOOKUP(O9,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P9,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q9+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A27,0,'10A32 Capacity'!Q9)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A27,0,'10A32 Capacity'!Q9+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U9*N9/(1000*'10A61 5\" Calcs'!$O$46),U9*N9/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y9/'10A32 Capacity'!AA9,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y9/'10A32 Capacity'!Z9,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y9,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y9,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB9,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O9>'10A32 Tables'!S27),'10A32 Tables'!T27,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O9>'10A32 Tables'!Q27),'10A32 Tables'!R27,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O9>'10A32 Tables'!O27),'10A32 Tables'!P27,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O9>'10A32 Tables'!M27),'10A32 Tables'!N27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB27),'10A32 Tables'!AC27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z27),'10A32 Tables'!AA27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X27),'10A32 Tables'!Y27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V27),'10A32 Tables'!W27,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH9,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE9),VLOOKUP(AI9,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE9+3,TRUE),VLOOKUP(AI9,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA9-0.0000001)),\"\",AL9/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM9/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","04","K-09-4",1,"1/4\"","04 : 1/4\" Diameter Tube 4 L/h",6,8,-100,0,4,"04 : 1/4\" Diameter Tube",{"$f":"MIN(IF($AP$6:$AP$32>BF8,'10A32 Capacity'!$AP$6:$AP$32))","v":0},{"$error":"#N/A"},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"VLOOKUP(BF9,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,0,0]
[null,null,6,0.14045978437541282,"K-1-6",4.0599999999999996,7.31,18,24,-100,"05","1/4\"","05 : 1/4\" Diameter Tube 6 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F10*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G10)),\nSQRT(F10*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G10)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N10),cP/'10A32 Capacity'!N10),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N10),\"\"))","v":""},{"$f":"HLOOKUP(O10,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P10,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q10+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A28,0,'10A32 Capacity'!Q10)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A28,0,'10A32 Capacity'!Q10+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U10*N10/(1000*'10A61 5\" Calcs'!$O$46),U10*N10/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y10/'10A32 Capacity'!AA10,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y10/'10A32 Capacity'!Z10,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y10,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y10,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB10,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O10>'10A32 Tables'!S28),'10A32 Tables'!T28,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O10>'10A32 Tables'!Q28),'10A32 Tables'!R28,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O10>'10A32 Tables'!O28),'10A32 Tables'!P28,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O10>'10A32 Tables'!M28),'10A32 Tables'!N28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB28),'10A32 Tables'!AC28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z28),'10A32 Tables'!AA28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X28),'10A32 Tables'!Y28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V28),'10A32 Tables'!W28,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH10,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE10),VLOOKUP(AI10,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE10+3,TRUE),VLOOKUP(AI10,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA10-0.0000001)),\"\",AL10/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM10/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","05","K-1-6",1,"1/4\"","05 : 1/4\" Diameter Tube 6 L/h",18,24,-100,0,6,"05 : 1/4\" Diameter Tube"]
[null,null,10,0.2137431501312804,"K-2-10",4.0599999999999996,7.31,18,24,-100,"06","1/4\"","06 : 1/4\" Diameter Tube 10 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F11*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G11)),\nSQRT(F11*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G11)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N11),cP/'10A32 Capacity'!N11),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N11),\"\"))","v":""},{"$f":"HLOOKUP(O11,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P11,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q11+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A29,0,'10A32 Capacity'!Q11)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A29,0,'10A32 Capacity'!Q11+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U11*N11/(1000*'10A61 5\" Calcs'!$O$46),U11*N11/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y11/'10A32 Capacity'!AA11,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y11/'10A32 Capacity'!Z11,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y11,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y11,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB11,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O11>'10A32 Tables'!S29),'10A32 Tables'!T29,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O11>'10A32 Tables'!Q29),'10A32 Tables'!R29,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O11>'10A32 Tables'!O29),'10A32 Tables'!P29,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O11>'10A32 Tables'!M29),'10A32 Tables'!N29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB29),'10A32 Tables'!AC29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z29),'10A32 Tables'!AA29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X29),'10A32 Tables'!Y29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V29),'10A32 Tables'!W29,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH11,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE11),VLOOKUP(AI11,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE11+3,TRUE),VLOOKUP(AI11,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA11-0.0000001)),\"\",AL11/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM11/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","06","K-2-10",1,"1/4\"","06 : 1/4\" Diameter Tube 10 L/h",18,24,-100,0,10,"06 : 1/4\" Diameter Tube"]
[null,null,16,0.329775145911404,"K-3-13",4.0599999999999996,7.31,18,24,-100,"07","1/4\"","07 : 1/4\" Diameter Tube 16 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F12*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G12)),\nSQRT(F12*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G12)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N12),cP/'10A32 Capacity'!N12),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N12),\"\"))","v":""},{"$f":"HLOOKUP(O12,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P12,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q12+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A30,0,'10A32 Capacity'!Q12)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A30,0,'10A32 Capacity'!Q12+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U12*N12/(1000*'10A61 5\" Calcs'!$O$46),U12*N12/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y12/'10A32 Capacity'!AA12,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y12/'10A32 Capacity'!Z12,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y12,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y12,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB12,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O12>'10A32 Tables'!S30),'10A32 Tables'!T30,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O12>'10A32 Tables'!Q30),'10A32 Tables'!R30,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O12>'10A32 Tables'!O30),'10A32 Tables'!P30,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O12>'10A32 Tables'!M30),'10A32 Tables'!N30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB30),'10A32 Tables'!AC30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z30),'10A32 Tables'!AA30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X30),'10A32 Tables'!Y30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V30),'10A32 Tables'!W30,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH12,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE12),VLOOKUP(AI12,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE12+3,TRUE),VLOOKUP(AI12,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA12-0.0000001)),\"\",AL12/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM12/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","07","K-3-13",1,"1/4\"","07 : 1/4\" Diameter Tube 16 L/h",18,24,-100,0,16,"07 : 1/4\" Diameter Tube","Name / Size"]
[null,null,25,0.51909050744739527,"K-4-25",5.66,7.52,18,24,-100,"08","1/4\"","08 : 1/4\" Diameter Tube 25 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F13*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G13)),\nSQRT(F13*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G13)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N13),cP/'10A32 Capacity'!N13),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N13),\"\"))","v":""},{"$f":"HLOOKUP(O13,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P13,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q13+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A31,0,'10A32 Capacity'!Q13)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A31,0,'10A32 Capacity'!Q13+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U13*N13/(1000*'10A61 5\" Calcs'!$O$46),U13*N13/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y13/'10A32 Capacity'!AA13,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y13/'10A32 Capacity'!Z13,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y13,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y13,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB13,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O13>'10A32 Tables'!S31),'10A32 Tables'!T31,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O13>'10A32 Tables'!Q31),'10A32 Tables'!R31,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O13>'10A32 Tables'!O31),'10A32 Tables'!P31,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O13>'10A32 Tables'!M31),'10A32 Tables'!N31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB31),'10A32 Tables'!AC31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z31),'10A32 Tables'!AA31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X31),'10A32 Tables'!Y31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V31),'10A32 Tables'!W31,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH13,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE13),VLOOKUP(AI13,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE13+3,TRUE),VLOOKUP(AI13,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA13-0.0000001)),\"\",AL13/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM13/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","08","K-4-25",1,"1/4\"","08 : 1/4\" Diameter Tube 25 L/h",18,24,-100,0,25,"08 : 1/4\" Diameter Tube",{"$f":"BQ6&\"                                                                                                  \"&BR6","v":{"$error":"#N/A"}},null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Capacity'!BM6),\" \"&'10A32 Capacity'!BF13,\"false\")","v":{"$error":"#N/A"}}]
[null,null,40,0.76336839330028705,"K-5-40",4.0599999999999996,7.31,18,24,-100,"09","1/4\"","09 : 1/4\" Diameter Tube 40 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F14*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G14)),\nSQRT(F14*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G14)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N14),cP/'10A32 Capacity'!N14),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N14),\"\"))","v":""},{"$f":"HLOOKUP(O14,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P14,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q14+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A32,0,'10A32 Capacity'!Q14)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A32,0,'10A32 Capacity'!Q14+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U14*N14/(1000*'10A61 5\" Calcs'!$O$46),U14*N14/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y14/'10A32 Capacity'!AA14,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y14/'10A32 Capacity'!Z14,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y14,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y14,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB14,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O14>'10A32 Tables'!S32),'10A32 Tables'!T32,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O14>'10A32 Tables'!Q32),'10A32 Tables'!R32,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O14>'10A32 Tables'!O32),'10A32 Tables'!P32,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O14>'10A32 Tables'!M32),'10A32 Tables'!N32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB32),'10A32 Tables'!AC32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z32),'10A32 Tables'!AA32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X32),'10A32 Tables'!Y32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V32),'10A32 Tables'!W32,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH14,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE14),VLOOKUP(AI14,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE14+3,TRUE),VLOOKUP(AI14,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA14-0.0000001)),\"\",AL14/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM14/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","09","K-5-40",1,"1/4\"","09 : 1/4\" Diameter Tube 40 L/h",18,24,-100,0,40,"09 : 1/4\" Diameter Tube",{"$f":"BQ7&\"                                                                                                  \"&BR7","v":{"$error":"#N/A"}}]
[null,null,60,1.1603199578112362,"K-6-60",5.66,7.52,18,24,-100,"10","1/4\"","10 : 1/4\" Diameter Tube 60 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F15*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G15)),\nSQRT(F15*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G15)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N15),cP/'10A32 Capacity'!N15),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N15),\"\"))","v":""},{"$f":"HLOOKUP(O15,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P15,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q15+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A33,0,'10A32 Capacity'!Q15)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A33,0,'10A32 Capacity'!Q15+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U15*N15/(1000*'10A61 5\" Calcs'!$O$46),U15*N15/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y15/'10A32 Capacity'!AA15,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y15/'10A32 Capacity'!Z15,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y15,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y15,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB15,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O15>'10A32 Tables'!S33),'10A32 Tables'!T33,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O15>'10A32 Tables'!Q33),'10A32 Tables'!R33,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O15>'10A32 Tables'!O33),'10A32 Tables'!P33,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O15>'10A32 Tables'!M33),'10A32 Tables'!N33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB33),'10A32 Tables'!AC33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z33),'10A32 Tables'!AA33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X33),'10A32 Tables'!Y33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V33),'10A32 Tables'!W33,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH15,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE15),VLOOKUP(AI15,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE15+3,TRUE),VLOOKUP(AI15,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA15-0.0000001)),\"\",AL15/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM15/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","10","K-6-60",1,"1/4\"","10 : 1/4\" Diameter Tube 60 L/h",18,24,-100,0,60,"10 : 1/4\" Diameter Tube",{"$error":"#N/A"}]
[null,null,100,1.8931536153699118,"K-7-100",5.66,7.52,12,24,-100,"11","1/4\"","11 : 1/4\" Diameter Tube 100 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F16*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G16)),\nSQRT(F16*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G16)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N16),cP/'10A32 Capacity'!N16),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N16),\"\"))","v":""},{"$f":"HLOOKUP(O16,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P16,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q16+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A34,0,'10A32 Capacity'!Q16)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A34,0,'10A32 Capacity'!Q16+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U16*N16/(1000*'10A61 5\" Calcs'!$O$46),U16*N16/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y16/'10A32 Capacity'!AA16,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y16/'10A32 Capacity'!Z16,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y16,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y16,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB16,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O16>'10A32 Tables'!S34),'10A32 Tables'!T34,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O16>'10A32 Tables'!Q34),'10A32 Tables'!R34,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O16>'10A32 Tables'!O34),'10A32 Tables'!P34,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O16>'10A32 Tables'!M34),'10A32 Tables'!N34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB34),'10A32 Tables'!AC34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z34),'10A32 Tables'!AA34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X34),'10A32 Tables'!Y34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V34),'10A32 Tables'!W34,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH16,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE16),VLOOKUP(AI16,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE16+3,TRUE),VLOOKUP(AI16,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA16-0.0000001)),\"\",AL16/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM16/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","11","K-7-100",1,"1/4\"","11 : 1/4\" Diameter Tube 100 L/h",12,24,-100,0,100,"11 : 1/4\" Diameter Tube",{"$error":"#N/A"}]
[null,null,100,1.9542230868331347,"B-8 -100",29,7.77,8,10,4,"20","3/8\"","20 : 3/8\" Diameter Tube 100 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F17*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G17)),\nSQRT(F17*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G17)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N17),cP/'10A32 Capacity'!N17),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N17),\"\"))","v":""},{"$f":"HLOOKUP(O17,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P17,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q17+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A35,0,'10A32 Capacity'!Q17)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A35,0,'10A32 Capacity'!Q17+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U17*N17/(1000*'10A61 5\" Calcs'!$O$46),U17*N17/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y17/'10A32 Capacity'!AA17,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y17/'10A32 Capacity'!Z17,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y17,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y17,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB17,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O17>'10A32 Tables'!S35),'10A32 Tables'!T35,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O17>'10A32 Tables'!Q35),'10A32 Tables'!R35,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O17>'10A32 Tables'!O35),'10A32 Tables'!P35,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O17>'10A32 Tables'!M35),'10A32 Tables'!N35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB35),'10A32 Tables'!AC35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z35),'10A32 Tables'!AA35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X35),'10A32 Tables'!Y35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V35),'10A32 Tables'!W35,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH17,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE17),VLOOKUP(AI17,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE17+3,TRUE),VLOOKUP(AI17,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA17-0.0000001)),\"\",(0.0000001)+AL17/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM17/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","20","B-8 -100",1,"3/8\"","20 : 3/8\" Diameter Tube 100 L/h",8,10,4,0.3,100,"20 : 3/8\" Diameter Tube"]
[null,null,160,3.0534735731711482,"B-9 -160",27.56,7.74,8,10,4,"21","3/8\"","21 : 3/8\" Diameter Tube 160 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F18*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G18)),\nSQRT(F18*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G18)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N18),cP/'10A32 Capacity'!N18),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N18),\"\"))","v":""},{"$f":"HLOOKUP(O18,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P18,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q18+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A36,0,'10A32 Capacity'!Q18)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A36,0,'10A32 Capacity'!Q18+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U18*N18/(1000*'10A61 5\" Calcs'!$O$46),U18*N18/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y18/'10A32 Capacity'!AA18,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y18/'10A32 Capacity'!Z18,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y18,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y18,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB18,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O18>'10A32 Tables'!S36),'10A32 Tables'!T36,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O18>'10A32 Tables'!Q36),'10A32 Tables'!R36,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O18>'10A32 Tables'!O36),'10A32 Tables'!P36,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O18>'10A32 Tables'!M36),'10A32 Tables'!N36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB36),'10A32 Tables'!AC36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z36),'10A32 Tables'!AA36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X36),'10A32 Tables'!Y36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V36),'10A32 Tables'!W36,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH18,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE18),VLOOKUP(AI18,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE18+3,TRUE),VLOOKUP(AI18,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA18-0.0000001)),\"\",AL18/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM18/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","21","B-9 -160",1,"3/8\"","21 : 3/8\" Diameter Tube 160 L/h",8,10,4,0.3,160,"21 : 3/8\" Diameter Tube","Name / Size","Range","Sizing Summary Scale Type","Damping ?","Configuration Preview Flow Range","Sizing Summary Flow Range","Configuration Preview Scale Type",null,null,null,"Scale Type","Descriptor"]
[null,null,200,3.7863072307298236,"B-10-200",26.76,7.71,8,10,4,"22","3/8\"","22 : 3/8\" Diameter Tube 200 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F19*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G19)),\nSQRT(F19*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G19)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N19),cP/'10A32 Capacity'!N19),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N19),\"\"))","v":""},{"$f":"HLOOKUP(O19,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P19,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q19+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A37,0,'10A32 Capacity'!Q19)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A37,0,'10A32 Capacity'!Q19+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U19*N19/(1000*'10A61 5\" Calcs'!$O$46),U19*N19/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y19/'10A32 Capacity'!AA19,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y19/'10A32 Capacity'!Z19,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y19,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y19,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB19,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O19>'10A32 Tables'!S37),'10A32 Tables'!T37,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O19>'10A32 Tables'!Q37),'10A32 Tables'!R37,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O19>'10A32 Tables'!O37),'10A32 Tables'!P37,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O19>'10A32 Tables'!M37),'10A32 Tables'!N37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB37),'10A32 Tables'!AC37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z37),'10A32 Tables'!AA37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X37),'10A32 Tables'!Y37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V37),'10A32 Tables'!W37,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH19,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE19),VLOOKUP(AI19,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE19+3,TRUE),VLOOKUP(AI19,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA19-0.0000001)),\"\",AL19/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM19/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","22","B-10-200",1,"3/8\"","22 : 3/8\" Diameter Tube 200 L/h",8,10,4,0.3,200,"22 : 3/8\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Capacity'!BM6),\" \"&'10A32 Capacity'!BF13,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF13,4),3)=\"1/4\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO6),'10A32 Capacity'!BF13&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO6,'Modified Inputs'!$J$3>BP6),BF13,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP6),BF13&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),'10A32 Capacity'!BF13,\"\")))))","v":{"$error":"#N/A"}},{"$f":"BG6","v":{"$error":"#N/A"}},{"$f":"BJ6","v":{"$error":"#N/A"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO6),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$f":"BL6","v":{"$error":"#N/A"}},{"$f":"BH6&\" \"&\":\"&\" \"&BK6&\" \"&\"Dia. \"&VLOOKUP(BF6,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/HR\"","v":{"$error":"#N/A"}},{"$f":"BH19&\" \"&\":\"&\" \"&IFERROR(VLOOKUP(BH19,$BP$19:$BQ$23,2,FALSE),\"\")","v":{"$error":"#N/A"}},null,null,null,1,"Linear, Liq/Gas Visc <1.4 CPS"]
[null,null,250,4.7634187741413916,"B-11-250",25.9,7.71,8,10,4,"23","3/8\"","23 : 3/8\" Diameter Tube 250 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F20*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G20)),\nSQRT(F20*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G20)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N20),cP/'10A32 Capacity'!N20),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N20),\"\"))","v":""},{"$f":"HLOOKUP(O20,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P20,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q20+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A38,0,'10A32 Capacity'!Q20)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A38,0,'10A32 Capacity'!Q20+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U20*N20/(1000*'10A61 5\" Calcs'!$O$46),U20*N20/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y20/'10A32 Capacity'!AA20,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y20/'10A32 Capacity'!Z20,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y20,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y20,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB20,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O20>'10A32 Tables'!S38),'10A32 Tables'!T38,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O20>'10A32 Tables'!Q38),'10A32 Tables'!R38,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O20>'10A32 Tables'!O38),'10A32 Tables'!P38,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O20>'10A32 Tables'!M38),'10A32 Tables'!N38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB38),'10A32 Tables'!AC38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z38),'10A32 Tables'!AA38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X38),'10A32 Tables'!Y38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V38),'10A32 Tables'!W38,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH20,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE20),VLOOKUP(AI20,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE20+3,TRUE),VLOOKUP(AI20,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA20-0.0000001)),\"\",AL20/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM20/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","23","B-11-250",1,"3/8\"","23 : 3/8\" Diameter Tube 250 L/h",8,10,4,0.3,250,"23 : 3/8\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Capacity'!BM7),\" \"&'10A32 Capacity'!BF14,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF14,4),3)=\"1/4\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO7),'10A32 Capacity'!BF14&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO7,'Modified Inputs'!$J$3>BP7),BF14,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP7),BF14&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),'10A32 Capacity'!BF14,\"\")))))","v":{"$error":"#N/A"}},{"$f":"BG7","v":{"$error":"#N/A"}},{"$f":"BJ7","v":{"$error":"#N/A"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO7),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$f":"BL7","v":{"$error":"#N/A"}},{"$f":"BH7&\" \"&\":\"&\" \"&BK7&\" \"&\"Dia. \"&VLOOKUP(BF7,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/HR\"","v":{"$error":"#N/A"}},{"$f":"BH20&\" \"&\":\"&\" \"&IFERROR(VLOOKUP(BH20,$BP$19:$BQ$23,2,FALSE),\"\")","v":{"$error":"#N/A"}},null,null,null,2,"Linear Gas"]
[null,null,300,5.6183913746265128,"B-12-300",25,7.7,8,10,4,"24","3/8\"","24 : 3/8\" Diameter Tube 300 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F21*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G21)),\nSQRT(F21*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G21)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N21),cP/'10A32 Capacity'!N21),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N21),\"\"))","v":""},{"$f":"HLOOKUP(O21,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P21,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q21+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A39,0,'10A32 Capacity'!Q21)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A39,0,'10A32 Capacity'!Q21+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U21*N21/(1000*'10A61 5\" Calcs'!$O$46),U21*N21/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y21/'10A32 Capacity'!AA21,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y21/'10A32 Capacity'!Z21,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y21,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y21,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB21,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O21>'10A32 Tables'!S39),'10A32 Tables'!T39,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O21>'10A32 Tables'!Q39),'10A32 Tables'!R39,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O21>'10A32 Tables'!O39),'10A32 Tables'!P39,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O21>'10A32 Tables'!M39),'10A32 Tables'!N39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB39),'10A32 Tables'!AC39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z39),'10A32 Tables'!AA39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X39),'10A32 Tables'!Y39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V39),'10A32 Tables'!W39,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH21,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE21),VLOOKUP(AI21,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE21+3,TRUE),VLOOKUP(AI21,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA21-0.0000001)),\"\",AL21/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM21/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","24","B-12-300",1,"3/8\"","24 : 3/8\" Diameter Tube 300 L/h",8,10,4,0.3,300,"24 : 3/8\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Capacity'!BM8),\" \"&'10A32 Capacity'!BF15,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF15,4),3)=\"1/4\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO8),'10A32 Capacity'!BF15&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO8,'Modified Inputs'!$J$3>BP8),BF15,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP8),BF15&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),'10A32 Capacity'!BF15,\"\")))))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO8),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,3,"Linear Gas"]
[null,null,400,7.633683932912871,"B-13-400",35.6,7.7,8,10,4,"30","1/2\"","30 : 1/2\" Diameter Tube 400 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F22*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G22)),\nSQRT(F22*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G22)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N22),cP/'10A32 Capacity'!N22),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N22),\"\"))","v":""},{"$f":"HLOOKUP(O22,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P22,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q22+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A40,0,'10A32 Capacity'!Q22)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A40,0,'10A32 Capacity'!Q22+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U22*N22/(1000*'10A61 5\" Calcs'!$O$46),U22*N22/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y22/'10A32 Capacity'!AA22,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y22/'10A32 Capacity'!Z22,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y22,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y22,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB22,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O22>'10A32 Tables'!S40),'10A32 Tables'!T40,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O22>'10A32 Tables'!Q40),'10A32 Tables'!R40,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O22>'10A32 Tables'!O40),'10A32 Tables'!P40,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O22>'10A32 Tables'!M40),'10A32 Tables'!N40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB40),'10A32 Tables'!AC40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z40),'10A32 Tables'!AA40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X40),'10A32 Tables'!Y40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V40),'10A32 Tables'!W40,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH22,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE22),VLOOKUP(AI22,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE22+3,TRUE),VLOOKUP(AI22,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA22-0.0000001)),\"\",AL22/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM22/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","30","B-13-400",1,"1/2\"","30 : 1/2\" Diameter Tube 400 L/h",8,10,4,0.3,400,"30 : 1/2\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Capacity'!BM9),\" \"&'10A32 Capacity'!BF16,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF16,4),3)=\"1/4\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO9),'10A32 Capacity'!BF16&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO9,'Modified Inputs'!$J$3>BP9),BF16,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP9),BF16&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),'10A32 Capacity'!BF16,\"\")))))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<'10A32 Capacity'!BO9),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,4,"Non Linear Liq Visc >1.4 CPS"]
[null,null,500,9.1604207194934428,"B-14-500",34.200000000000003,7.7,8,10,4,"31","1/2\"","31 : 1/2\" Diameter Tube 500 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F23*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G23)),\nSQRT(F23*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G23)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N23),cP/'10A32 Capacity'!N23),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N23),\"\"))","v":""},{"$f":"HLOOKUP(O23,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P23,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q23+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A41,0,'10A32 Capacity'!Q23)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A41,0,'10A32 Capacity'!Q23+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U23*N23/(1000*'10A61 5\" Calcs'!$O$46),U23*N23/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y23/'10A32 Capacity'!AA23,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y23/'10A32 Capacity'!Z23,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y23,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y23,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB23,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O23>'10A32 Tables'!S41),'10A32 Tables'!T41,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O23>'10A32 Tables'!Q41),'10A32 Tables'!R41,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O23>'10A32 Tables'!O41),'10A32 Tables'!P41,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O23>'10A32 Tables'!M41),'10A32 Tables'!N41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB41),'10A32 Tables'!AC41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z41),'10A32 Tables'!AA41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X41),'10A32 Tables'!Y41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V41),'10A32 Tables'!W41,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH23,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE23),VLOOKUP(AI23,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE23+3,TRUE),VLOOKUP(AI23,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA23-0.0000001)),\"\",AL23/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM23/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","31","B-14-500",1,"1/2\"","31 : 1/2\" Diameter Tube 500 L/h",8,10,4,0.3,500,"31 : 1/2\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,5,"Non Linear Liq Visc >1.4 CPS"]
[null,null,600,10.992504863390133,"B-15-600",32.799999999999997,7.7,8,10,4,"32","1/2\"","32 : 1/2\" Diameter Tube 600 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F24*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G24)),\nSQRT(F24*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G24)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N24),cP/'10A32 Capacity'!N24),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N24),\"\"))","v":""},{"$f":"HLOOKUP(O24,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P24,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q24+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A42,0,'10A32 Capacity'!Q24)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A42,0,'10A32 Capacity'!Q24+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U24*N24/(1000*'10A61 5\" Calcs'!$O$46),U24*N24/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y24/'10A32 Capacity'!AA24,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y24/'10A32 Capacity'!Z24,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y24,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y24,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB24,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O24>'10A32 Tables'!S42),'10A32 Tables'!T42,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O24>'10A32 Tables'!Q42),'10A32 Tables'!R42,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O24>'10A32 Tables'!O42),'10A32 Tables'!P42,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O24>'10A32 Tables'!M42),'10A32 Tables'!N42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB42),'10A32 Tables'!AC42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z42),'10A32 Tables'!AA42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X42),'10A32 Tables'!Y42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V42),'10A32 Tables'!W42,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH24,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE24),VLOOKUP(AI24,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE24+3,TRUE),VLOOKUP(AI24,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA24-0.0000001)),\"\",AL24/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM24/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","32","B-15-600",1,"1/2\"","32 : 1/2\" Diameter Tube 600 L/h",8,10,4,0.3,600,"32 : 1/2\" Diameter Tube","Final Table"]
[null,null,700,12.824589007286821,"B-16-700",31.4,7.7,8,10,4,"33","1/2\"","33 : 1/2\" Diameter Tube 700 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F25*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G25)),\nSQRT(F25*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G25)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N25),cP/'10A32 Capacity'!N25),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N25),\"\"))","v":""},{"$f":"HLOOKUP(O25,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P25,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q25+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A43,0,'10A32 Capacity'!Q25)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A43,0,'10A32 Capacity'!Q25+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U25*N25/(1000*'10A61 5\" Calcs'!$O$46),U25*N25/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y25/'10A32 Capacity'!AA25,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y25/'10A32 Capacity'!Z25,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y25,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y25,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB25,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O25>'10A32 Tables'!S43),'10A32 Tables'!T43,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O25>'10A32 Tables'!Q43),'10A32 Tables'!R43,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O25>'10A32 Tables'!O43),'10A32 Tables'!P43,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O25>'10A32 Tables'!M43),'10A32 Tables'!N43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB43),'10A32 Tables'!AC43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z43),'10A32 Tables'!AA43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X43),'10A32 Tables'!Y43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V43),'10A32 Tables'!W43,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH25,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE25),VLOOKUP(AI25,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE25+3,TRUE),VLOOKUP(AI25,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA25-0.0000001)),\"\",AL25/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM25/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","33","B-16-700",1,"1/2\"","33 : 1/2\" Diameter Tube 700 L/h",8,10,4,0.3,700,"33 : 1/2\" Diameter Tube","Name / Size","Range","Sizing Summary Scale Type","Damping ?","Configuration Preview Flow Range","Sizing Summary Flow Range","Configuration Preview Scale Type"]
[null,null,800,14.656673151183512,"B-17-800",30.5,7.7,8,10,4,"34","1/2\"","34 : 1/2\" Diameter Tube 800 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F26*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G26)),\nSQRT(F26*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G26)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N26),cP/'10A32 Capacity'!N26),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N26),\"\"))","v":""},{"$f":"HLOOKUP(O26,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P26,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q26+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A44,0,'10A32 Capacity'!Q26)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A44,0,'10A32 Capacity'!Q26+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U26*N26/(1000*'10A61 5\" Calcs'!$O$46),U26*N26/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y26/'10A32 Capacity'!AA26,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y26/'10A32 Capacity'!Z26,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y26,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y26,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB26,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O26>'10A32 Tables'!S44),'10A32 Tables'!T44,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O26>'10A32 Tables'!Q44),'10A32 Tables'!R44,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O26>'10A32 Tables'!O44),'10A32 Tables'!P44,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O26>'10A32 Tables'!M44),'10A32 Tables'!N44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB44),'10A32 Tables'!AC44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z44),'10A32 Tables'!AA44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X44),'10A32 Tables'!Y44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V44),'10A32 Tables'!W44,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH26,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE26),VLOOKUP(AI26,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE26+3,TRUE),VLOOKUP(AI26,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA26-0.0000001)),\"\",(0.0000001)+AL26/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM26/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","34","B-17-800",1,"1/2\"","34 : 1/2\" Diameter Tube 800 L/h",8,10,4,0.3,800,"34 : 1/2\" Diameter Tube",{"$f":"IFERROR(BF19,\"\")","v":""},{"$f":"IF(BF26=\"\",\"\",BG19)","v":""},"","",{"$f":"IF($BH$26=\"\",\"\",BJ19)","v":""},{"$f":"IF($BH$26=\"\",\"\",BK19)","v":""},"",{"$f":"BJ26","v":""}]
[null,null,800,14.534534208257064,"B-18-800",216,7.81,3,10,16,"40","1\"","40 : 1\" Diameter Tube 800 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F27*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G27)),\nSQRT(F27*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G27)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N27),cP/'10A32 Capacity'!N27),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N27),\"\"))","v":""},{"$f":"HLOOKUP(O27,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P27,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q27+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A45,0,'10A32 Capacity'!Q27)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A45,0,'10A32 Capacity'!Q27+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U27*N27/(1000*'10A61 5\" Calcs'!$O$46),U27*N27/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y27/'10A32 Capacity'!AA27,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y27/'10A32 Capacity'!Z27,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y27,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y27,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB27,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O27>'10A32 Tables'!S45),'10A32 Tables'!T45,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O27>'10A32 Tables'!Q45),'10A32 Tables'!R45,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O27>'10A32 Tables'!O45),'10A32 Tables'!P45,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O27>'10A32 Tables'!M45),'10A32 Tables'!N45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB45),'10A32 Tables'!AC45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z45),'10A32 Tables'!AA45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X45),'10A32 Tables'!Y45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V45),'10A32 Tables'!W45,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH27,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE27),VLOOKUP(AI27,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE27+3,TRUE),VLOOKUP(AI27,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA27-0.0000001)),\"\",AL27/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM27/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","40","B-18-800",1,"1\"","40 : 1\" Diameter Tube 800 L/h",3,10,16,0.4,800,"40 : 1\" Diameter Tube",{"$f":"IFERROR(BF20,\"\")","v":""},"","",{"$f":"IF(BH27=\"\",\"\",BI20)","v":""},{"$f":"IF($BH$27=\"\",\"\",BJ20)","v":""},{"$f":"IF($BH$27=\"\",\"\",BK20)","v":""},{"$f":"IF($BH$27=\"\",\"\",BL20)","v":""},{"$f":"BJ27","v":""}]
[null,null,1000,18.13763302458722,"B-19-1000",210,7.8,3,10,16,"41","1\"","41 : 1\" Diameter Tube 1000 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F28*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G28)),\nSQRT(F28*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G28)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N28),cP/'10A32 Capacity'!N28),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N28),\"\"))","v":""},{"$f":"HLOOKUP(O28,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P28,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q28+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A46,0,'10A32 Capacity'!Q28)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A46,0,'10A32 Capacity'!Q28+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U28*N28/(1000*'10A61 5\" Calcs'!$O$46),U28*N28/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y28/'10A32 Capacity'!AA28,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y28/'10A32 Capacity'!Z28,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y28,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y28,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB28,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O28>'10A32 Tables'!S46),'10A32 Tables'!T46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O28>'10A32 Tables'!Q46),'10A32 Tables'!R46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O28>'10A32 Tables'!O46),'10A32 Tables'!P46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O28>'10A32 Tables'!M46),'10A32 Tables'!N46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB46),'10A32 Tables'!AC46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z46),'10A32 Tables'!AA46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X46),'10A32 Tables'!Y46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V46),'10A32 Tables'!W46,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH28,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE28),VLOOKUP(AI28,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE28+3,TRUE),VLOOKUP(AI28,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA28-0.0000001)),\"\",AL28/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM28/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","41","B-19-1000",1,"1\"","41 : 1\" Diameter Tube 1000 L/h",3,10,16,0.4,1000,"41 : 1\" Diameter Tube",{"$f":"IFERROR(IF(BF27=\"\",\"\",BF21),\"\")","v":""},"","",{"$f":"IF(BH28=\"\",\"\",BI21)","v":""},{"$f":"IF($BH$28=\"\",\"\",BJ21)","v":""},{"$f":"IF($BH$28=\"\",\"\",BK21)","v":""},{"$f":"IF($BH$28=\"\",\"\",BL21)","v":""},""]
[null,null,1600,29.06906841650413,"B-20-1600",195,7.8,3,10,16,"42","1\"","42 : 1\" Diameter Tube 1600 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F29*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G29)),\nSQRT(F29*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G29)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N29),cP/'10A32 Capacity'!N29),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N29),\"\"))","v":""},{"$f":"HLOOKUP(O29,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P29,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q29+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A47,0,'10A32 Capacity'!Q29)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A47,0,'10A32 Capacity'!Q29+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U29*N29/(1000*'10A61 5\" Calcs'!$O$46),U29*N29/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y29/'10A32 Capacity'!AA29,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y29/'10A32 Capacity'!Z29,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y29,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y29,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB29,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O29>'10A32 Tables'!S47),'10A32 Tables'!T47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O29>'10A32 Tables'!Q47),'10A32 Tables'!R47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O29>'10A32 Tables'!O47),'10A32 Tables'!P47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O29>'10A32 Tables'!M47),'10A32 Tables'!N47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB47),'10A32 Tables'!AC47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z47),'10A32 Tables'!AA47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X47),'10A32 Tables'!Y47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V47),'10A32 Tables'!W47,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH29,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE29),VLOOKUP(AI29,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE29+3,TRUE),VLOOKUP(AI29,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA29-0.0000001)),\"\",AL29/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM29/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","42","B-20-1600",1,"1\"","42 : 1\" Diameter Tube 1600 L/h",3,10,16,0.4,1600,"42 : 1\" Diameter Tube",{"$f":"IFERROR(IF(OR(BF27=\"\",BF28=\"\"),\"\",BF22),\"\")","v":""},"","",{"$f":"IF(BH29=\"\",\"\",BI22)","v":""},{"$f":"IF($BH$29=\"\",\"\",BJ22)","v":""},{"$f":"IF($BH$29=\"\",\"\",BK22)","v":""},{"$f":"IF($BH$29=\"\",\"\",BL22)","v":""},""]
[null,null,2000,36.336335520627657,"B-21-2000",185,7.79,3,10,16,"43","1\"","43 : 1\" Diameter Tube 2000 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F30*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G30)),\nSQRT(F30*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G30)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N30),cP/'10A32 Capacity'!N30),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N30),\"\"))","v":""},{"$f":"HLOOKUP(O30,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P30,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q30+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A48,0,'10A32 Capacity'!Q30)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A48,0,'10A32 Capacity'!Q30+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U30*N30/(1000*'10A61 5\" Calcs'!$O$46),U30*N30/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y30/'10A32 Capacity'!AA30,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y30/'10A32 Capacity'!Z30,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y30,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y30,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB30,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O30>'10A32 Tables'!S48),'10A32 Tables'!T48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O30>'10A32 Tables'!Q48),'10A32 Tables'!R48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O30>'10A32 Tables'!O48),'10A32 Tables'!P48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O30>'10A32 Tables'!M48),'10A32 Tables'!N48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB48),'10A32 Tables'!AC48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z48),'10A32 Tables'!AA48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X48),'10A32 Tables'!Y48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V48),'10A32 Tables'!W48,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH30,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE30),VLOOKUP(AI30,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE30+3,TRUE),VLOOKUP(AI30,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA30-0.0000001)),\"\",AL30/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM30/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","43","B-21-2000",1,"1\"","43 : 1\" Diameter Tube 2000 L/h",3,10,16,0.4,2000,"43 : 1\" Diameter Tube"]
[null,null,2500,45.435686768647884,"B-22-2500",176,7.79,3,10,16,"44","1\"","44 : 1\" Diameter Tube 2500 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F31*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G31)),\nSQRT(F31*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G31)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N31),cP/'10A32 Capacity'!N31),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N31),\"\"))","v":""},{"$f":"HLOOKUP(O31,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P31,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q31+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A49,0,'10A32 Capacity'!Q31)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A49,0,'10A32 Capacity'!Q31+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U31*N31/(1000*'10A61 5\" Calcs'!$O$46),U31*N31/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y31/'10A32 Capacity'!AA31,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y31/'10A32 Capacity'!Z31,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y31,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y31,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB31,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O31>'10A32 Tables'!S49),'10A32 Tables'!T49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O31>'10A32 Tables'!Q49),'10A32 Tables'!R49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O31>'10A32 Tables'!O49),'10A32 Tables'!P49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O31>'10A32 Tables'!M49),'10A32 Tables'!N49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB49),'10A32 Tables'!AC49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z49),'10A32 Tables'!AA49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X49),'10A32 Tables'!Y49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V49),'10A32 Tables'!W49,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH31,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE31),VLOOKUP(AI31,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE31+3,TRUE),VLOOKUP(AI31,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA31-0.0000001)),\"\",AL31/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM31/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","44","B-22-2500",1,"1\"","44 : 1\" Diameter Tube 2500 L/h",3,10,16,0.4,2500,"44 : 1\" Diameter Tube"]
[null,null,3000,54.535038016668103,"B-23-3000",177,7.79,3,10,16,"45","1\"","45 : 1\" Diameter Tube 3000 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F32*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/'10A32 Capacity'!G32)),\nSQRT(F32*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/'10A32 Capacity'!G32)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N32),cP/'10A32 Capacity'!N32),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/'10A32 Capacity'!N32),\"\"))","v":""},{"$f":"HLOOKUP(O32,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P32,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,'10A32 Capacity'!Q32+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A50,0,'10A32 Capacity'!Q32)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A50,0,'10A32 Capacity'!Q32+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U32*N32/(1000*'10A61 5\" Calcs'!$O$46),U32*N32/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",'10A32 Capacity'!Y32/'10A32 Capacity'!AA32,\nIF('VA Sizing'!$C$5=\"Normal\",'10A32 Capacity'!Y32/'10A32 Capacity'!Z32,\nIF('VA Sizing'!$C$5=\"Actual\",'10A32 Capacity'!Y32,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A32 Capacity'!Y32,\nIF('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!AB32,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O32>'10A32 Tables'!S50),'10A32 Tables'!T50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O32>'10A32 Tables'!Q50),'10A32 Tables'!R50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O32>'10A32 Tables'!O50),'10A32 Tables'!P50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'10A32 Capacity'!O32>'10A32 Tables'!M50),'10A32 Tables'!N50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB50),'10A32 Tables'!AC50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z50),'10A32 Tables'!AA50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X50),'10A32 Tables'!Y50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V50),'10A32 Tables'!W50,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH32,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE32),VLOOKUP(AI32,'10A32 Tables'!$D$53:$L$118,'10A32 Capacity'!AE32+3,TRUE),VLOOKUP(AI32,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,null,{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>('10A32 Capacity'!BA32-0.0000001)),\"\",AL32/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM32/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","45","B-23-3000",1,"1\"","45 : 1\" Diameter Tube 3000 L/h",3,10,16,0.4,3000,"45 : 1\" Diameter Tube"]
[null,null,0,null,null,null,null,0,0]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"01 : 1/4\" Dia. 1 L/HR","01 : 1/4\" Diameter Tube 1 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"02 : 1/4\" Dia. 1.6 L/HR","02 : 1/4\" Diameter Tube 1.6 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"03 : 1/4\" Dia. 2.5 L/HR","03 : 1/4\" Diameter Tube 2.5 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"04 : 1/4\" Dia. 4 L/HR","04 : 1/4\" Diameter Tube 4 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"05 : 1/4\" Dia. 6 L/HR","05 : 1/4\" Diameter Tube 6 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"06 : 1/4\" Dia. 10 L/HR","06 : 1/4\" Diameter Tube 10 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"07 : 1/4\" Dia. 16 L/HR","07 : 1/4\" Diameter Tube 16 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"08 : 1/4\" Dia. 25 L/HR","08 : 1/4\" Diameter Tube 25 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"09 : 1/4\" Dia. 40 L/HR","09 : 1/4\" Diameter Tube 40 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 : 1/4\" Dia. 60 L/HR","10 : 1/4\" Diameter Tube 60 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"11 : 1/4\" Dia. 100 L/HR","11 : 1/4\" Diameter Tube 100 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 : 3/8\" Dia. 100 L/HR","20 : 3/8\" Diameter Tube 100 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"21 : 3/8\" Dia. 160 L/HR","21 : 3/8\" Diameter Tube 160 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"22 : 3/8\" Dia. 200 L/HR","22 : 3/8\" Diameter Tube 200 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"23 : 3/8\" Dia. 250 L/HR","23 : 3/8\" Diameter Tube 250 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 : 3/8\" Dia. 300 L/HR","24 : 3/8\" Diameter Tube 300 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 : 1/2\" Dia. 400 L/HR","30 : 1/2\" Diameter Tube 400 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"31 : 1/2\" Dia. 500 L/HR","31 : 1/2\" Diameter Tube 500 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 : 1/2\" Dia. 600 L/HR","32 : 1/2\" Diameter Tube 600 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"33 : 1/2\" Dia. 700 L/HR","33 : 1/2\" Diameter Tube 700 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 : 1/2\" Dia. 800 L/HR","34 : 1/2\" Diameter Tube 800 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 : 1\" Dia. 800 L/HR","40 : 1\" Diameter Tube 800 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"41 : 1\" Dia. 1000 L/HR","41 : 1\" Diameter Tube 1000 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 : 1\" Dia. 1600 L/HR","42 : 1\" Diameter Tube 1600 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"43 : 1\" Dia. 2000 L/HR","43 : 1\" Diameter Tube 2000 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"44 : 1\" Dia. 2500 L/HR","44 : 1\" Diameter Tube 2500 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"45 : 1\" Dia. 3000 L/HR","45 : 1\" Diameter Tube 3000 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]

{"sheet":"Basic10A32","index":40,"n_rows":62,"n_cols":93,"rows_kept":62,"cut":false,"hidden":true,"merged":[[23,57,23,59],[4,89,4,90],[3,22,3,24],[3,29,3,30],[3,37,3,39],[3,41,3,45]]}
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liquid Flow",null,null,null,null,"Gas Flow",null,null,null,null,null,null,null,null,null,"Flow Outputs",null,null,null,"Modified Outputs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"All",null,null,null,"Range Limit"]
[null,null,"Equivalent Water L/h","Equivalent Air SCFM","Name","Mass","Density","Vstd","Vmax","Psta bar(g)","Code","Size","Description","W","N","N1","Pos(N1)","N2","K1","K2","K",null,"Q L/min","Q USGal/min","M3/h","Compress Normal","Compress Standard","Q M3/h",null,"Q M3/h","Scale Type",null,"BT","BU","BV","BZ",null,"Max\nM3/h","Min\nM3/h","Scale Type",null,"Max Specified Units","Min Specified Units","Max Rounded","Min Rounded","Concatenated","Code","Name","Scale Type","Size","Description","Vstd","Vmax","Psta bar(g)","Pmin bar(g)","Equivalent Water L/h",null,"Max","Range","Code","Name","Scale Type","Size","Flow Range","Vstd","Vmax","Psta bar(g)","Pmin bar(g)","Top Descriptor","Bottom Descriptor",null,null,null,"Code","Max Rounded",null,null,"Code","Max Rounded",null,"Tube/Float","Code","Max Rounded","Vstd","Psta bar(g)","Pmin bar(g)","Viscosity / Pressure Warning",null,null,"Final Standard"]
[null,null,1,2.137431502212804E-2,"K-06-1.0",4.0599999999999996,7.31,4,8,-100,"01","1/4\"",{"$f":"K6&\" \"&\":\"&\" \"&L6&\" \"&\"Diameter Tube\"&\" \"&C6&\" \"&\"L/h\"","v":"01 : 1/4\" Diameter Tube 1 L/h"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F6*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G6)),\nSQRT(F6*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G6)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N6),cP/Basic10A32!N6),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N6),\"\"))","v":""},{"$f":"HLOOKUP(O6,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P6,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q6+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A24,0,Basic10A32!Q6)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A24,0,Basic10A32!Q6+1)","v":{"$error":"#N/A"}},{"$f":"EXP(LN(S6)-((LN(S6)-LN(T6))*(LN(O6)-LN(P6)))/(LN(R6)-LN(P6)))","v":{"$error":"#N/A"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U6*N6/(1000*'10A61 5\" Calcs'!$O$46),U6*N6/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"W6*0.2642","v":{"$error":"#N/A"}},{"$f":"W6*(60)/1000","v":{"$error":"#N/A"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y6/Basic10A32!AA6,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y6/Basic10A32!Z6,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y6,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y6,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB6,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O6>'10A32 Tables'!S24),'10A32 Tables'!T24,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O6>'10A32 Tables'!Q24),'10A32 Tables'!R24,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O6>'10A32 Tables'!O24),'10A32 Tables'!P24,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O6>'10A32 Tables'!M24),'10A32 Tables'!N24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB24),'10A32 Tables'!AC24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z24),'10A32 Tables'!AA24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X24),'10A32 Tables'!Y24,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V24),'10A32 Tables'!W24,1))))))))","v":1},null,{"$f":"-2+INT(LOG10(AD6))","v":{"$error":"#VALUE!"}},{"$f":"AD6*(10^(0-AG6))","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP(AH6,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE6),VLOOKUP(AI6,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE6+3,TRUE),VLOOKUP(AI6,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$f":"AI6*(10^AG6)","v":{"$error":"#VALUE!"}},{"$f":"AJ6*(10^(AG6))","v":{"$error":"#VALUE!"}},{"$f":"AE6","v":1},{"$f":"AY6","v":"01 : 1/4\" Diameter Tube 1 L/h"},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA6-0.0000001)),\"\",AL6/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM6/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(AP6=\"\",0,\nIF(AP6<0.00000099999,ROUND(AP6,7),\nIF(AP6<0.0000099999,ROUND(AP6,6),\nIF(AP6<0.000099999,ROUND(AP6,5),\nIF(AP6<0.00099999,ROUND(AP6,4),\nIF(AP6<0.0099999,ROUND(AP6,3),\nIF(AP6<0.099999,ROUND(AP6,2),\nIF(AP6<0.99999,ROUND(AP6,2),\nIF(AP6<9.999,ROUND(AP6,2),\nIF(AP6<99.99,ROUND(AP6,1),\nIF(AP6<999.99,ROUND(AP6,0),\nIF(AP6<9999.99,ROUND(AP6,-1),\nIF(AP6<99999,ROUND(AP6,-2),ROUND(AP6,2))))))))))))))","v":0},{"$f":"IF(AR6=0,0,ROUND(AQ6,1))","v":0},{"$f":"AS6&\" \"&\"-\"&\" \"&AR6","v":"0 - 0"},{"$f":"K6","v":"01"},{"$f":"E6","v":"K-06-1.0"},{"$f":"AN6","v":1},{"$f":"L6","v":"1/4\""},{"$f":"M6","v":"01 : 1/4\" Diameter Tube 1 L/h"},{"$f":"H6","v":4},{"$f":"I6","v":8},-100,0,1,{"$f":"AU6&\" \"&\":\"&\" \"&AX6&\" \"&\"Diameter Tube\"","v":"01 : 1/4\" Diameter Tube"},{"$f":"MAX(IF($AP$6:$AP$32<('VA Sizing'!$C$12-0.00000000001),Basic10A32!$AP$6:$AP$32))","v":0},{"$f":"VLOOKUP(BF6,$AP$6:$AT$32,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$6,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"BH6&\" \"&\":\"&\" \"&BK6&\" \"&\"Dia. Tube\"","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(BF6,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,null,null,{"$f":"AU6","v":"01"},{"$f":"IF(AR6=0,\"zero\",AR6)","v":"zero"},{"$f":"BV6","v":"01"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW6*0.45),BW6+0.000001>'Modified Inputs'!$N$2),BV6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW6*0.45),BW6+0.0000001>'Modified Inputs'!$N$2),BW6,0),0)","v":0},null,{"$f":"VLOOKUP(CD6,$AU$6:$AY$32,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(CE6,$BW$6:$BX$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($CA$6:$CA$54>0,$CA$6:$CA$54))","v":0},{"$f":"VLOOKUP(CE6,$AR$6:$BB$32,9,FALSE)","v":4},{"$f":"VLOOKUP(CE6,$AR$6:$BB$32,11,FALSE)","v":-100},{"$f":"VLOOKUP(CE6,$AR$6:$BC$32,12,FALSE)","v":0},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF6),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD6=\"01\",CD6=\"02\",CD6=\"03\",CD6=\"04\",CD6=\"05\",CD6=\"06\",CD6=\"07\",CD6=\"08\",CD6=\"09\",CD6=\"10\",CD6=\"11\"),'Modified Inputs'!$J$3<CG6),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH6),\"pressure\",\"\"))))","v":{"$error":"#N/A"}},null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,1.6,3.2977514600140402E-2,"K-07-1.6",4.0599999999999996,7.31,4,8,-100,"02","1/4\"",{"$f":"K7&\" \"&\":\"&\" \"&L7&\" \"&\"Diameter Tube\"&\" \"&C7&\" \"&\"L/h\"","v":"02 : 1/4\" Diameter Tube 1.6 L/h"},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F7*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G7)),\nSQRT(F7*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G7)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N7),cP/Basic10A32!N7),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N7),\"\"))","v":""},{"$f":"HLOOKUP(O7,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P7,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q7+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A25,0,Basic10A32!Q7)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A25,0,Basic10A32!Q7+1)","v":{"$error":"#N/A"}},{"$f":"EXP(LN(S7)-((LN(S7)-LN(T7))*(LN(O7)-LN(P7)))/(LN(R7)-LN(P7)))","v":{"$error":"#N/A"}},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U7*N7/(1000*'10A61 5\" Calcs'!$O$46),U7*N7/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"W7*0.2642","v":{"$error":"#N/A"}},{"$f":"W7*(60)/1000","v":{"$error":"#N/A"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y7/Basic10A32!AA7,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y7/Basic10A32!Z7,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y7,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y7,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB7,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O7>'10A32 Tables'!S25),'10A32 Tables'!T25,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O7>'10A32 Tables'!Q25),'10A32 Tables'!R25,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O7>'10A32 Tables'!O25),'10A32 Tables'!P25,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O7>'10A32 Tables'!M25),'10A32 Tables'!N25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB25),'10A32 Tables'!AC25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z25),'10A32 Tables'!AA25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X25),'10A32 Tables'!Y25,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V25),'10A32 Tables'!W25,1))))))))","v":1},null,{"$f":"-2+INT(LOG10(AD7))","v":{"$error":"#VALUE!"}},{"$f":"AD7*(10^(0-AG7))","v":{"$error":"#VALUE!"}},{"$f":"VLOOKUP(AH7,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE7),VLOOKUP(AI7,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE7+3,TRUE),VLOOKUP(AI7,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"AE7","v":1},{"$f":"AY7","v":"02 : 1/4\" Diameter Tube 1.6 L/h"},{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA7-0.0000001)),\"\",AL7/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM7/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},{"$f":"IF(AP7=\"\",0,\nIF(AP7<0.00000099999,ROUND(AP7,7),\nIF(AP7<0.0000099999,ROUND(AP7,6),\nIF(AP7<0.000099999,ROUND(AP7,5),\nIF(AP7<0.00099999,ROUND(AP7,4),\nIF(AP7<0.0099999,ROUND(AP7,3),\nIF(AP7<0.099999,ROUND(AP7,2),\nIF(AP7<0.99999,ROUND(AP7,2),\nIF(AP7<9.999,ROUND(AP7,2),\nIF(AP7<99.99,ROUND(AP7,1),\nIF(AP7<999.99,ROUND(AP7,0),\nIF(AP7<9999.99,ROUND(AP7,-1),\nIF(AP7<99999,ROUND(AP7,-2),ROUND(AP7,2))))))))))))))","v":0},{"$f":"IF(AR7=0,0,ROUND(AQ7,1))","v":0},{"$f":"AS7&\" \"&\"-\"&\" \"&AR7","v":"0 - 0"},{"$f":"K7","v":"02"},{"$f":"E7","v":"K-07-1.6"},{"$f":"AN7","v":1},{"$f":"L7","v":"1/4\""},"02 : 1/4\" Diameter Tube 1.6 L/h",{"$f":"H7","v":4},8,-100,0,1.6,{"$f":"AU7&\" \"&\":\"&\" \"&AX7&\" \"&\"Diameter Tube\"","v":"02 : 1/4\" Diameter Tube"},{"$f":"MIN(IF($AP$6:$AP$32>=('VA Sizing'!$C$12-0.00000000001),Basic10A32!$AP$6:$AP$32))","v":0},{"$f":"VLOOKUP(BF7,$AP$6:$AT$32,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$7,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$f":"BH7&\" \"&\":\"&\" \"&BK7&\" \"&\"Dia. Tube\"","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(BF7,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,null,null,{"$f":"AU7","v":"02"},{"$f":"IF(AR7=0,\"zero\",AR7)","v":"zero"},{"$f":"BV7","v":"02"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW7*0.45),BW7+0.000001>'Modified Inputs'!$N$2),BV7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW7*0.45),BW7+0.0000001>'Modified Inputs'!$N$2),BW7,0),0)","v":0},null,{"$f":"VLOOKUP(CD7,$AU$6:$AY$32,5,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(CE7,$BW$6:$BX$32,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($CA$6:$CA$32<CE6,$CA$6:$CA$32))","v":0},{"$f":"VLOOKUP(CE7,$AR$6:$BB$32,9,FALSE)","v":4},{"$f":"VLOOKUP(CE7,$AR$6:$BB$32,11,FALSE)","v":-100},{"$f":"VLOOKUP(CE7,$AR$6:$BC$32,12,FALSE)","v":0},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF7),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD7=\"01\",CD7=\"02\",CD7=\"03\",CD7=\"04\",CD7=\"05\",CD7=\"06\",CD7=\"07\",CD7=\"08\",CD7=\"09\",CD7=\"10\",CD7=\"11\"),'Modified Inputs'!$J$3<CG7),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH7),\"pressure\",\"\"))))","v":{"$error":"#N/A"}},null,null,{"$f":"IFERROR(IF($CI$35=\"\",$CC$35,1/0),\nIFERROR(IF($CI$34=\"\",$CC$34,1/0),\nIFERROR(IF($CI$33=\"\",$CC$33,1/0),\nIFERROR(IF($CI$32=\"\",$CC$32,1/0),\nIFERROR(IF($CI$31=\"\",$CC$31,1/0),\nIFERROR(IF($CI$30=\"\",$CC$30,1/0),\nIFERROR(IF($CI$29=\"\",$CC$29,1/0),\nIFERROR(IF($CI$28=\"\",$CC$28,1/0),\nIFERROR(IF($CI$27=\"\",$CC$27,1/0),\nIFERROR(IF($CI$26=\"\",$CC$26,1/0),\nIFERROR(IF($CI$25=\"\",$CC$25,1/0),\nIFERROR(IF($CI$24=\"\",$CC$24,1/0),\nIFERROR(IF($CI$23=\"\",$CC$23,1/0),\nIFERROR(IF($CI$22=\"\",$CC$22,1/0),\nIFERROR(IF($CI$21=\"\",$CC$21,1/0),\nIFERROR(IF($CI$20=\"\",$CC$20,1/0),\nIFERROR(IF($CI$19=\"\",$CC$19,1/0),\nIFERROR(IF($CI$18=\"\",$CC$18,1/0),\nIFERROR(IF($CI$17=\"\",$CC$17,1/0),\nIFERROR(IF($CI$16=\"\",$CC$16,1/0),\nIFERROR(IF($CI$15=\"\",$CC$15,1/0),\nIFERROR(IF($CI$14=\"\",$CC$14,1/0),\nIFERROR(IF($CI$13=\"\",$CC$16,1/0),\nIFERROR(IF($CI$12=\"\",$CC$12,1/0),\nIFERROR(IF($CI$11=\"\",$CC$11,1/0),\nIFERROR(IF($CI$10=\"\",$CC$10,1/0),\nIFERROR(IF($CI$9=\"\",$CC$9,1/0),\nIFERROR(IF($CI$8=\"\",$CC$8,1/0),\nIFERROR(IF($CI$7=\"\",$CC$7,1/0),\nIFERROR(IF($CI$6=\"\",$CC$6,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(CL7,$CC$6:$CE$35,3,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IFERROR(IF(AND(CL7=\"none\",NOT(CI6=\"\")),CI6,\"\"),\"sizing\")","v":"sizing"}]
[null,null,2.5,6.1069471473222961E-2,"K-08-2.5",4.0599999999999996,7.31,6,8,-100,"03","1/4\"","03 : 1/4\" Diameter Tube 2.5 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F8*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G8)),\nSQRT(F8*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G8)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N8),cP/Basic10A32!N8),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N8),\"\"))","v":""},{"$f":"HLOOKUP(O8,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P8,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q8+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A26,0,Basic10A32!Q8)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A26,0,Basic10A32!Q8+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U8*N8/(1000*'10A61 5\" Calcs'!$O$46),U8*N8/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y8/Basic10A32!AA8,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y8/Basic10A32!Z8,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y8,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y8,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB8,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O8>'10A32 Tables'!S26),'10A32 Tables'!T26,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O8>'10A32 Tables'!Q26),'10A32 Tables'!R26,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O8>'10A32 Tables'!O26),'10A32 Tables'!P26,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O8>'10A32 Tables'!M26),'10A32 Tables'!N26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB26),'10A32 Tables'!AC26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z26),'10A32 Tables'!AA26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X26),'10A32 Tables'!Y26,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V26),'10A32 Tables'!W26,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH8,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE8),VLOOKUP(AI8,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE8+3,TRUE),VLOOKUP(AI8,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"03 : 1/4\" Diameter Tube 2.5 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA8-0.0000001)),\"\",AL8/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM8/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","03","K-08-2.5",1,"1/4\"","03 : 1/4\" Diameter Tube 2.5 L/h",6,8,-100,0,2.5,"03 : 1/4\" Diameter Tube",{"$f":"MIN(IF($AP$6:$AP$32>BF7,Basic10A32!$AP$6:$AP$32))","v":0},{"$error":"#N/A"},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$8,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"VLOOKUP(BF8,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,null,null,"03","zero","03",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW8*0.45),BW8+0.000001>'Modified Inputs'!$N$2),BV8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW8*0.45),BW8+0.0000001>'Modified Inputs'!$N$2),BW8,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE7,$CA$6:$CA$32))","v":0},{"$f":"VLOOKUP(CE8,$AR$6:$BB$32,9,FALSE)","v":4},-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF8),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD8=\"01\",CD8=\"02\",CD8=\"03\",CD8=\"04\",CD8=\"05\",CD8=\"06\",CD8=\"07\",CD8=\"08\",CD8=\"09\",CD8=\"10\",CD8=\"11\"),'Modified Inputs'!$J$3<CG8),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH8),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,4,9.7711154351156751E-2,"K-09-4",4.0599999999999996,7.31,6,8,-100,"04","1/4\"","04 : 1/4\" Diameter Tube 4 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F9*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G9)),\nSQRT(F9*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G9)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N9),cP/Basic10A32!N9),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N9),\"\"))","v":""},{"$f":"HLOOKUP(O9,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P9,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q9+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A27,0,Basic10A32!Q9)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A27,0,Basic10A32!Q9+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U9*N9/(1000*'10A61 5\" Calcs'!$O$46),U9*N9/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y9/Basic10A32!AA9,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y9/Basic10A32!Z9,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y9,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y9,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB9,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O9>'10A32 Tables'!S27),'10A32 Tables'!T27,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O9>'10A32 Tables'!Q27),'10A32 Tables'!R27,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O9>'10A32 Tables'!O27),'10A32 Tables'!P27,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O9>'10A32 Tables'!M27),'10A32 Tables'!N27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB27),'10A32 Tables'!AC27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z27),'10A32 Tables'!AA27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X27),'10A32 Tables'!Y27,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V27),'10A32 Tables'!W27,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH9,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE9),VLOOKUP(AI9,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE9+3,TRUE),VLOOKUP(AI9,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"04 : 1/4\" Diameter Tube 4 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA9-0.0000001)),\"\",AL9/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM9/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","04","K-09-4",1,"1/4\"","04 : 1/4\" Diameter Tube 4 L/h",6,8,-100,0,4,"04 : 1/4\" Diameter Tube",{"$f":"MIN(IF($AP$6:$AP$32>BF8,Basic10A32!$AP$6:$AP$32))","v":0},{"$error":"#N/A"},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,6,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,7,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,8,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,9,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,10,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,11,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,12,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BB$32,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP($BF$9,$AP$6:$BC$32,14,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"VLOOKUP(BF9,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/H Capacity\"","v":{"$error":"#N/A"}},null,null,null,"04","zero","04",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW9*0.45),BW9+0.000001>'Modified Inputs'!$N$2),BV9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW9*0.45),BW9+0.0000001>'Modified Inputs'!$N$2),BW9,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE8,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF9),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD9=\"01\",CD9=\"02\",CD9=\"03\",CD9=\"04\",CD9=\"05\",CD9=\"06\",CD9=\"07\",CD9=\"08\",CD9=\"09\",CD9=\"10\",CD9=\"11\"),'Modified Inputs'!$J$3<CG9),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH9),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,6,0.14045978437541282,"K-1-6",4.0599999999999996,7.31,18,24,-100,"05","1/4\"","05 : 1/4\" Diameter Tube 6 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F10*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G10)),\nSQRT(F10*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G10)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N10),cP/Basic10A32!N10),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N10),\"\"))","v":""},{"$f":"HLOOKUP(O10,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P10,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q10+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A28,0,Basic10A32!Q10)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A28,0,Basic10A32!Q10+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U10*N10/(1000*'10A61 5\" Calcs'!$O$46),U10*N10/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y10/Basic10A32!AA10,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y10/Basic10A32!Z10,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y10,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y10,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB10,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O10>'10A32 Tables'!S28),'10A32 Tables'!T28,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O10>'10A32 Tables'!Q28),'10A32 Tables'!R28,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O10>'10A32 Tables'!O28),'10A32 Tables'!P28,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O10>'10A32 Tables'!M28),'10A32 Tables'!N28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB28),'10A32 Tables'!AC28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z28),'10A32 Tables'!AA28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X28),'10A32 Tables'!Y28,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V28),'10A32 Tables'!W28,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH10,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE10),VLOOKUP(AI10,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE10+3,TRUE),VLOOKUP(AI10,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"05 : 1/4\" Diameter Tube 6 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA10-0.0000001)),\"\",AL10/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM10/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","05","K-1-6",1,"1/4\"","05 : 1/4\" Diameter Tube 6 L/h",18,24,-100,0,6,"05 : 1/4\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"05","zero","05",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW10*0.45),BW10+0.000001>'Modified Inputs'!$N$2),BV10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW10*0.45),BW10+0.0000001>'Modified Inputs'!$N$2),BW10,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE9,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF10),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD10=\"01\",CD10=\"02\",CD10=\"03\",CD10=\"04\",CD10=\"05\",CD10=\"06\",CD10=\"07\",CD10=\"08\",CD10=\"09\",CD10=\"10\",CD10=\"11\"),'Modified Inputs'!$J$3<CG10),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH10),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,10,0.2137431501312804,"K-2-10",4.0599999999999996,7.31,18,24,-100,"06","1/4\"","06 : 1/4\" Diameter Tube 10 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F11*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G11)),\nSQRT(F11*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G11)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N11),cP/Basic10A32!N11),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N11),\"\"))","v":""},{"$f":"HLOOKUP(O11,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P11,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q11+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A29,0,Basic10A32!Q11)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A29,0,Basic10A32!Q11+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U11*N11/(1000*'10A61 5\" Calcs'!$O$46),U11*N11/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y11/Basic10A32!AA11,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y11/Basic10A32!Z11,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y11,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y11,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB11,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O11>'10A32 Tables'!S29),'10A32 Tables'!T29,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O11>'10A32 Tables'!Q29),'10A32 Tables'!R29,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O11>'10A32 Tables'!O29),'10A32 Tables'!P29,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O11>'10A32 Tables'!M29),'10A32 Tables'!N29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB29),'10A32 Tables'!AC29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z29),'10A32 Tables'!AA29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X29),'10A32 Tables'!Y29,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V29),'10A32 Tables'!W29,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH11,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE11),VLOOKUP(AI11,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE11+3,TRUE),VLOOKUP(AI11,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"06 : 1/4\" Diameter Tube 10 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA11-0.0000001)),\"\",AL11/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM11/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","06","K-2-10",1,"1/4\"","06 : 1/4\" Diameter Tube 10 L/h",18,24,-100,0,10,"06 : 1/4\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"06","zero","06",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW11*0.45),BW11+0.000001>'Modified Inputs'!$N$2),BV11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW11*0.45),BW11+0.0000001>'Modified Inputs'!$N$2),BW11,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE10,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF11),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD11=\"01\",CD11=\"02\",CD11=\"03\",CD11=\"04\",CD11=\"05\",CD11=\"06\",CD11=\"07\",CD11=\"08\",CD11=\"09\",CD11=\"10\",CD11=\"11\"),'Modified Inputs'!$J$3<CG11),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH11),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,16,0.329775145911404,"K-3-13",4.0599999999999996,7.31,18,24,-100,"07","1/4\"","07 : 1/4\" Diameter Tube 16 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F12*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G12)),\nSQRT(F12*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G12)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N12),cP/Basic10A32!N12),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N12),\"\"))","v":""},{"$f":"HLOOKUP(O12,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P12,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q12+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A30,0,Basic10A32!Q12)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A30,0,Basic10A32!Q12+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U12*N12/(1000*'10A61 5\" Calcs'!$O$46),U12*N12/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y12/Basic10A32!AA12,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y12/Basic10A32!Z12,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y12,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y12,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB12,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O12>'10A32 Tables'!S30),'10A32 Tables'!T30,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O12>'10A32 Tables'!Q30),'10A32 Tables'!R30,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O12>'10A32 Tables'!O30),'10A32 Tables'!P30,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O12>'10A32 Tables'!M30),'10A32 Tables'!N30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB30),'10A32 Tables'!AC30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z30),'10A32 Tables'!AA30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X30),'10A32 Tables'!Y30,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V30),'10A32 Tables'!W30,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH12,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE12),VLOOKUP(AI12,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE12+3,TRUE),VLOOKUP(AI12,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"07 : 1/4\" Diameter Tube 16 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA12-0.0000001)),\"\",AL12/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM12/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","07","K-3-13",1,"1/4\"","07 : 1/4\" Diameter Tube 16 L/h",18,24,-100,0,16,"07 : 1/4\" Diameter Tube","Name / Size",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"07","zero","07",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW12*0.45),BW12+0.000001>'Modified Inputs'!$N$2),BV12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW12*0.45),BW12+0.0000001>'Modified Inputs'!$N$2),BW12,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE11,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF12),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD12=\"01\",CD12=\"02\",CD12=\"03\",CD12=\"04\",CD12=\"05\",CD12=\"06\",CD12=\"07\",CD12=\"08\",CD12=\"09\",CD12=\"10\",CD12=\"11\"),'Modified Inputs'!$J$3<CG12),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH12),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,25,0.51909050744739527,"K-4-25",5.66,7.52,18,24,-100,"08","1/4\"","08 : 1/4\" Diameter Tube 25 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F13*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G13)),\nSQRT(F13*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G13)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N13),cP/Basic10A32!N13),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N13),\"\"))","v":""},{"$f":"HLOOKUP(O13,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P13,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q13+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A31,0,Basic10A32!Q13)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A31,0,Basic10A32!Q13+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U13*N13/(1000*'10A61 5\" Calcs'!$O$46),U13*N13/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y13/Basic10A32!AA13,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y13/Basic10A32!Z13,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y13,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y13,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB13,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O13>'10A32 Tables'!S31),'10A32 Tables'!T31,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O13>'10A32 Tables'!Q31),'10A32 Tables'!R31,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O13>'10A32 Tables'!O31),'10A32 Tables'!P31,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O13>'10A32 Tables'!M31),'10A32 Tables'!N31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB31),'10A32 Tables'!AC31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z31),'10A32 Tables'!AA31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X31),'10A32 Tables'!Y31,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V31),'10A32 Tables'!W31,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH13,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE13),VLOOKUP(AI13,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE13+3,TRUE),VLOOKUP(AI13,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"08 : 1/4\" Diameter Tube 25 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA13-0.0000001)),\"\",AL13/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM13/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","08","K-4-25",1,"1/4\"","08 : 1/4\" Diameter Tube 25 L/h",18,24,-100,0,25,"08 : 1/4\" Diameter Tube",{"$f":"BQ6&\"                                                                                                  \"&BR6","v":{"$error":"#N/A"}},null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>Basic10A32!BM6),\" \"&Basic10A32!BF13,\"false\")","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,"08","zero","08",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW13*0.45),BW13+0.000001>'Modified Inputs'!$N$2),BV13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW13*0.45),BW13+0.0000001>'Modified Inputs'!$N$2),BW13,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE12,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF13),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD13=\"01\",CD13=\"02\",CD13=\"03\",CD13=\"04\",CD13=\"05\",CD13=\"06\",CD13=\"07\",CD13=\"08\",CD13=\"09\",CD13=\"10\",CD13=\"11\"),'Modified Inputs'!$J$3<CG13),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH13),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,40,0.76336839330028705,"K-5-40",4.0599999999999996,7.31,18,24,-100,"09","1/4\"","09 : 1/4\" Diameter Tube 40 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F14*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G14)),\nSQRT(F14*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G14)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N14),cP/Basic10A32!N14),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N14),\"\"))","v":""},{"$f":"HLOOKUP(O14,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P14,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q14+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A32,0,Basic10A32!Q14)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A32,0,Basic10A32!Q14+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U14*N14/(1000*'10A61 5\" Calcs'!$O$46),U14*N14/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y14/Basic10A32!AA14,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y14/Basic10A32!Z14,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y14,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y14,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB14,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O14>'10A32 Tables'!S32),'10A32 Tables'!T32,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O14>'10A32 Tables'!Q32),'10A32 Tables'!R32,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O14>'10A32 Tables'!O32),'10A32 Tables'!P32,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O14>'10A32 Tables'!M32),'10A32 Tables'!N32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB32),'10A32 Tables'!AC32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z32),'10A32 Tables'!AA32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X32),'10A32 Tables'!Y32,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V32),'10A32 Tables'!W32,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH14,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE14),VLOOKUP(AI14,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE14+3,TRUE),VLOOKUP(AI14,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"09 : 1/4\" Diameter Tube 40 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA14-0.0000001)),\"\",AL14/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM14/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","09","K-5-40",1,"1/4\"","09 : 1/4\" Diameter Tube 40 L/h",18,24,-100,0,40,"09 : 1/4\" Diameter Tube",{"$f":"BQ7&\"                                                                                                  \"&BR7","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"09","zero","09",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW14*0.45),BW14+0.000001>'Modified Inputs'!$N$2),BV14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW14*0.45),BW14+0.0000001>'Modified Inputs'!$N$2),BW14,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE13,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF14),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD14=\"01\",CD14=\"02\",CD14=\"03\",CD14=\"04\",CD14=\"05\",CD14=\"06\",CD14=\"07\",CD14=\"08\",CD14=\"09\",CD14=\"10\",CD14=\"11\"),'Modified Inputs'!$J$3<CG14),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH14),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,60,1.1603199578112362,"K-6-60",5.66,7.52,18,24,-100,"10","1/4\"","10 : 1/4\" Diameter Tube 60 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F15*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G15)),\nSQRT(F15*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G15)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N15),cP/Basic10A32!N15),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N15),\"\"))","v":""},{"$f":"HLOOKUP(O15,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P15,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q15+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A33,0,Basic10A32!Q15)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A33,0,Basic10A32!Q15+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U15*N15/(1000*'10A61 5\" Calcs'!$O$46),U15*N15/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y15/Basic10A32!AA15,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y15/Basic10A32!Z15,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y15,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y15,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB15,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O15>'10A32 Tables'!S33),'10A32 Tables'!T33,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O15>'10A32 Tables'!Q33),'10A32 Tables'!R33,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O15>'10A32 Tables'!O33),'10A32 Tables'!P33,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O15>'10A32 Tables'!M33),'10A32 Tables'!N33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB33),'10A32 Tables'!AC33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z33),'10A32 Tables'!AA33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X33),'10A32 Tables'!Y33,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V33),'10A32 Tables'!W33,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH15,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE15),VLOOKUP(AI15,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE15+3,TRUE),VLOOKUP(AI15,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"10 : 1/4\" Diameter Tube 60 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA15-0.0000001)),\"\",AL15/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM15/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","10","K-6-60",1,"1/4\"","10 : 1/4\" Diameter Tube 60 L/h",18,24,-100,0,60,"10 : 1/4\" Diameter Tube",{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10","zero","10",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW15*0.45),BW15+0.000001>'Modified Inputs'!$N$2),BV15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW15*0.45),BW15+0.0000001>'Modified Inputs'!$N$2),BW15,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE14,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF15),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD15=\"01\",CD15=\"02\",CD15=\"03\",CD15=\"04\",CD15=\"05\",CD15=\"06\",CD15=\"07\",CD15=\"08\",CD15=\"09\",CD15=\"10\",CD15=\"11\"),'Modified Inputs'!$J$3<CG15),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH15),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,100,1.8931536153699118,"K-7-100",5.66,7.52,12,24,-100,"11","1/4\"","11 : 1/4\" Diameter Tube 100 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F16*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G16)),\nSQRT(F16*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G16)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N16),cP/Basic10A32!N16),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N16),\"\"))","v":""},{"$f":"HLOOKUP(O16,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P16,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q16+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A34,0,Basic10A32!Q16)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A34,0,Basic10A32!Q16+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U16*N16/(1000*'10A61 5\" Calcs'!$O$46),U16*N16/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y16/Basic10A32!AA16,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y16/Basic10A32!Z16,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y16,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y16,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB16,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O16>'10A32 Tables'!S34),'10A32 Tables'!T34,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O16>'10A32 Tables'!Q34),'10A32 Tables'!R34,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O16>'10A32 Tables'!O34),'10A32 Tables'!P34,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O16>'10A32 Tables'!M34),'10A32 Tables'!N34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB34),'10A32 Tables'!AC34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z34),'10A32 Tables'!AA34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X34),'10A32 Tables'!Y34,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V34),'10A32 Tables'!W34,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH16,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE16),VLOOKUP(AI16,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE16+3,TRUE),VLOOKUP(AI16,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"11 : 1/4\" Diameter Tube 100 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA16-0.0000001)),\"\",AL16/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM16/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","11","K-7-100",1,"1/4\"","11 : 1/4\" Diameter Tube 100 L/h",12,24,-100,0,100,"11 : 1/4\" Diameter Tube",{"$error":"#N/A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"11","zero","11",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW16*0.45),BW16+0.000001>'Modified Inputs'!$N$2),BV16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW16*0.45),BW16+0.0000001>'Modified Inputs'!$N$2),BW16,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE15,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF16),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD16=\"01\",CD16=\"02\",CD16=\"03\",CD16=\"04\",CD16=\"05\",CD16=\"06\",CD16=\"07\",CD16=\"08\",CD16=\"09\",CD16=\"10\",CD16=\"11\"),'Modified Inputs'!$J$3<CG16),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH16),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,100,1.9542230868331347,"B-8 -100",29,7.77,8,10,4,"20","3/8\"","20 : 3/8\" Diameter Tube 100 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F17*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G17)),\nSQRT(F17*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G17)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N17),cP/Basic10A32!N17),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N17),\"\"))","v":""},{"$f":"HLOOKUP(O17,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P17,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q17+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A35,0,Basic10A32!Q17)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A35,0,Basic10A32!Q17+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U17*N17/(1000*'10A61 5\" Calcs'!$O$46),U17*N17/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y17/Basic10A32!AA17,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y17/Basic10A32!Z17,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y17,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y17,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB17,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O17>'10A32 Tables'!S35),'10A32 Tables'!T35,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O17>'10A32 Tables'!Q35),'10A32 Tables'!R35,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O17>'10A32 Tables'!O35),'10A32 Tables'!P35,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O17>'10A32 Tables'!M35),'10A32 Tables'!N35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB35),'10A32 Tables'!AC35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z35),'10A32 Tables'!AA35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X35),'10A32 Tables'!Y35,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V35),'10A32 Tables'!W35,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH17,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE17),VLOOKUP(AI17,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE17+3,TRUE),VLOOKUP(AI17,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"20 : 3/8\" Diameter Tube 100 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA17-0.0000001)),\"\",(0.0000001)+AL17/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM17/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","20","B-8 -100",1,"3/8\"","20 : 3/8\" Diameter Tube 100 L/h",8,10,4,0.3,100,"20 : 3/8\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20","zero","20",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW17*0.45),BW17+0.000001>'Modified Inputs'!$N$2),BV17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW17*0.45),BW17+0.0000001>'Modified Inputs'!$N$2),BW17,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE16,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF17),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD17=\"01\",CD17=\"02\",CD17=\"03\",CD17=\"04\",CD17=\"05\",CD17=\"06\",CD17=\"07\",CD17=\"08\",CD17=\"09\",CD17=\"10\",CD17=\"11\"),'Modified Inputs'!$J$3<CG17),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH17),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,160,3.0534735731711482,"B-9 -160",27.56,7.74,8,10,4,"21","3/8\"","21 : 3/8\" Diameter Tube 160 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F18*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G18)),\nSQRT(F18*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G18)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N18),cP/Basic10A32!N18),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N18),\"\"))","v":""},{"$f":"HLOOKUP(O18,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P18,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q18+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A36,0,Basic10A32!Q18)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A36,0,Basic10A32!Q18+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U18*N18/(1000*'10A61 5\" Calcs'!$O$46),U18*N18/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y18/Basic10A32!AA18,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y18/Basic10A32!Z18,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y18,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y18,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB18,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O18>'10A32 Tables'!S36),'10A32 Tables'!T36,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O18>'10A32 Tables'!Q36),'10A32 Tables'!R36,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O18>'10A32 Tables'!O36),'10A32 Tables'!P36,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O18>'10A32 Tables'!M36),'10A32 Tables'!N36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB36),'10A32 Tables'!AC36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z36),'10A32 Tables'!AA36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X36),'10A32 Tables'!Y36,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V36),'10A32 Tables'!W36,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH18,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE18),VLOOKUP(AI18,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE18+3,TRUE),VLOOKUP(AI18,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"21 : 3/8\" Diameter Tube 160 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA18-0.0000001)),\"\",AL18/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM18/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","21","B-9 -160",1,"3/8\"","21 : 3/8\" Diameter Tube 160 L/h",8,10,4,0.3,160,"21 : 3/8\" Diameter Tube","Name / Size","Range","Sizing Summary Scale Type","Damping ?","Configuration Preview Flow Range","Sizing Summary Flow Range","Configuration Preview Scale Type",null,null,null,"Scale Type","Descriptor",null,null,null,null,"21","zero","21",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW18*0.45),BW18+0.000001>'Modified Inputs'!$N$2),BV18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW18*0.45),BW18+0.0000001>'Modified Inputs'!$N$2),BW18,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE17,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF18),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD18=\"01\",CD18=\"02\",CD18=\"03\",CD18=\"04\",CD18=\"05\",CD18=\"06\",CD18=\"07\",CD18=\"08\",CD18=\"09\",CD18=\"10\",CD18=\"11\"),'Modified Inputs'!$J$3<CG18),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH18),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,200,3.7863072307298236,"B-10-200",26.76,7.71,8,10,4,"22","3/8\"","22 : 3/8\" Diameter Tube 200 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F19*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G19)),\nSQRT(F19*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G19)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N19),cP/Basic10A32!N19),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N19),\"\"))","v":""},{"$f":"HLOOKUP(O19,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P19,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q19+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A37,0,Basic10A32!Q19)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A37,0,Basic10A32!Q19+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U19*N19/(1000*'10A61 5\" Calcs'!$O$46),U19*N19/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y19/Basic10A32!AA19,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y19/Basic10A32!Z19,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y19,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y19,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB19,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O19>'10A32 Tables'!S37),'10A32 Tables'!T37,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O19>'10A32 Tables'!Q37),'10A32 Tables'!R37,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O19>'10A32 Tables'!O37),'10A32 Tables'!P37,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O19>'10A32 Tables'!M37),'10A32 Tables'!N37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB37),'10A32 Tables'!AC37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z37),'10A32 Tables'!AA37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X37),'10A32 Tables'!Y37,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V37),'10A32 Tables'!W37,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH19,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE19),VLOOKUP(AI19,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE19+3,TRUE),VLOOKUP(AI19,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"22 : 3/8\" Diameter Tube 200 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA19-0.0000001)),\"\",AL19/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM19/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","22","B-10-200",1,"3/8\"","22 : 3/8\" Diameter Tube 200 L/h",8,10,4,0.3,200,"22 : 3/8\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>Basic10A32!BM6),\" \"&Basic10A32!BF13,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF13,4),3)=\"1/4\",'Modified Inputs'!$J$3<Basic10A32!BO6),Basic10A32!BF13&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO6,'Modified Inputs'!$J$3>BP6),BF13,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP6),BF13&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),Basic10A32!BF13,\"\")))))","v":{"$error":"#N/A"}},{"$f":"BG6","v":{"$error":"#N/A"}},{"$f":"BJ6","v":{"$error":"#N/A"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO6),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$f":"BL6","v":{"$error":"#N/A"}},{"$f":"BH6&\" \"&\":\"&\" \"&BK6&\" \"&\"Dia. \"&VLOOKUP(BF6,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/HR\"","v":{"$error":"#N/A"}},{"$f":"BH19&\" \"&\":\"&\" \"&IFERROR(VLOOKUP(BH19,$BP$19:$BQ$23,2,FALSE),\"\")","v":{"$error":"#N/A"}},null,null,null,1,"Linear, Liq/Gas Visc <1.4 CPS",null,null,null,null,"22","zero","22",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW19*0.45),BW19+0.000001>'Modified Inputs'!$N$2),BV19,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW19*0.45),BW19+0.0000001>'Modified Inputs'!$N$2),BW19,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE18,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF19),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD19=\"01\",CD19=\"02\",CD19=\"03\",CD19=\"04\",CD19=\"05\",CD19=\"06\",CD19=\"07\",CD19=\"08\",CD19=\"09\",CD19=\"10\",CD19=\"11\"),'Modified Inputs'!$J$3<CG19),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH19),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,250,4.7634187741413916,"B-11-250",25.9,7.71,8,10,4,"23","3/8\"","23 : 3/8\" Diameter Tube 250 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F20*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G20)),\nSQRT(F20*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G20)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N20),cP/Basic10A32!N20),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N20),\"\"))","v":""},{"$f":"HLOOKUP(O20,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P20,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q20+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A38,0,Basic10A32!Q20)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A38,0,Basic10A32!Q20+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U20*N20/(1000*'10A61 5\" Calcs'!$O$46),U20*N20/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y20/Basic10A32!AA20,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y20/Basic10A32!Z20,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y20,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y20,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB20,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O20>'10A32 Tables'!S38),'10A32 Tables'!T38,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O20>'10A32 Tables'!Q38),'10A32 Tables'!R38,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O20>'10A32 Tables'!O38),'10A32 Tables'!P38,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O20>'10A32 Tables'!M38),'10A32 Tables'!N38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB38),'10A32 Tables'!AC38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z38),'10A32 Tables'!AA38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X38),'10A32 Tables'!Y38,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V38),'10A32 Tables'!W38,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH20,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE20),VLOOKUP(AI20,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE20+3,TRUE),VLOOKUP(AI20,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"23 : 3/8\" Diameter Tube 250 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA20-0.0000001)),\"\",AL20/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM20/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","23","B-11-250",1,"3/8\"","23 : 3/8\" Diameter Tube 250 L/h",8,10,4,0.3,250,"23 : 3/8\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>Basic10A32!BM7),\" \"&Basic10A32!BF14,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF14,4),3)=\"1/4\",'Modified Inputs'!$J$3<Basic10A32!BO7),Basic10A32!BF14&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO7,'Modified Inputs'!$J$3>BP7),BF14,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP7),BF14&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),Basic10A32!BF14,\"\")))))","v":{"$error":"#N/A"}},{"$f":"BG7","v":{"$error":"#N/A"}},{"$f":"BJ7","v":{"$error":"#N/A"}},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO7),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$f":"BL7","v":{"$error":"#N/A"}},{"$f":"BH7&\" \"&\":\"&\" \"&BK7&\" \"&\"Dia. \"&VLOOKUP(BF7,$AP$6:$BD$32,15,FALSE)&\" \"&\"L/HR\"","v":{"$error":"#N/A"}},{"$f":"BH20&\" \"&\":\"&\" \"&IFERROR(VLOOKUP(BH20,$BP$19:$BQ$23,2,FALSE),\"\")","v":{"$error":"#N/A"}},null,null,null,2,"Linear Gas",null,null,null,null,"23","zero","23",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW20*0.45),BW20+0.000001>'Modified Inputs'!$N$2),BV20,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW20*0.45),BW20+0.0000001>'Modified Inputs'!$N$2),BW20,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE19,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF20),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD20=\"01\",CD20=\"02\",CD20=\"03\",CD20=\"04\",CD20=\"05\",CD20=\"06\",CD20=\"07\",CD20=\"08\",CD20=\"09\",CD20=\"10\",CD20=\"11\"),'Modified Inputs'!$J$3<CG20),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH20),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,300,5.6183913746265128,"B-12-300",25,7.7,8,10,4,"24","3/8\"","24 : 3/8\" Diameter Tube 300 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F21*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G21)),\nSQRT(F21*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G21)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N21),cP/Basic10A32!N21),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N21),\"\"))","v":""},{"$f":"HLOOKUP(O21,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P21,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q21+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A39,0,Basic10A32!Q21)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A39,0,Basic10A32!Q21+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U21*N21/(1000*'10A61 5\" Calcs'!$O$46),U21*N21/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y21/Basic10A32!AA21,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y21/Basic10A32!Z21,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y21,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y21,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB21,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O21>'10A32 Tables'!S39),'10A32 Tables'!T39,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O21>'10A32 Tables'!Q39),'10A32 Tables'!R39,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O21>'10A32 Tables'!O39),'10A32 Tables'!P39,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O21>'10A32 Tables'!M39),'10A32 Tables'!N39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB39),'10A32 Tables'!AC39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z39),'10A32 Tables'!AA39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X39),'10A32 Tables'!Y39,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V39),'10A32 Tables'!W39,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH21,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE21),VLOOKUP(AI21,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE21+3,TRUE),VLOOKUP(AI21,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"24 : 3/8\" Diameter Tube 300 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA21-0.0000001)),\"\",AL21/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM21/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","24","B-12-300",1,"3/8\"","24 : 3/8\" Diameter Tube 300 L/h",8,10,4,0.3,300,"24 : 3/8\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>Basic10A32!BM8),\" \"&Basic10A32!BF15,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF15,4),3)=\"1/4\",'Modified Inputs'!$J$3<Basic10A32!BO8),Basic10A32!BF15&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO8,'Modified Inputs'!$J$3>BP8),BF15,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP8),BF15&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),Basic10A32!BF15,\"\")))))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO8),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,3,"Linear Gas",null,null,null,null,"24","zero","24",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW21*0.45),BW21+0.000001>'Modified Inputs'!$N$2),BV21,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW21*0.45),BW21+0.0000001>'Modified Inputs'!$N$2),BW21,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE20,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF21),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD21=\"01\",CD21=\"02\",CD21=\"03\",CD21=\"04\",CD21=\"05\",CD21=\"06\",CD21=\"07\",CD21=\"08\",CD21=\"09\",CD21=\"10\",CD21=\"11\"),'Modified Inputs'!$J$3<CG21),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH21),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,400,7.633683932912871,"B-13-400",35.6,7.7,8,10,4,"30","1/2\"","30 : 1/2\" Diameter Tube 400 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F22*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G22)),\nSQRT(F22*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G22)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N22),cP/Basic10A32!N22),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N22),\"\"))","v":""},{"$f":"HLOOKUP(O22,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P22,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q22+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A40,0,Basic10A32!Q22)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A40,0,Basic10A32!Q22+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U22*N22/(1000*'10A61 5\" Calcs'!$O$46),U22*N22/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y22/Basic10A32!AA22,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y22/Basic10A32!Z22,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y22,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y22,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB22,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O22>'10A32 Tables'!S40),'10A32 Tables'!T40,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O22>'10A32 Tables'!Q40),'10A32 Tables'!R40,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O22>'10A32 Tables'!O40),'10A32 Tables'!P40,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O22>'10A32 Tables'!M40),'10A32 Tables'!N40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB40),'10A32 Tables'!AC40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z40),'10A32 Tables'!AA40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X40),'10A32 Tables'!Y40,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V40),'10A32 Tables'!W40,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH22,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE22),VLOOKUP(AI22,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE22+3,TRUE),VLOOKUP(AI22,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"30 : 1/2\" Diameter Tube 400 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA22-0.0000001)),\"\",AL22/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM22/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","30","B-13-400",1,"1/2\"","30 : 1/2\" Diameter Tube 400 L/h",8,10,4,0.3,400,"30 : 1/2\" Diameter Tube",{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>Basic10A32!BM9),\" \"&Basic10A32!BF16,\nIF(AND('VA Sizing'!$C$3=\"Gas\",LEFT(RIGHT(BF16,4),3)=\"1/4\",'Modified Inputs'!$J$3<Basic10A32!BO9),Basic10A32!BF16&\" \",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO9,'Modified Inputs'!$J$3>BP9),BF16,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<BP9),BF16&\" \",\nIF(OR('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$3=\"Liquid\"),Basic10A32!BF16,\"\")))))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<Basic10A32!BO9),\"With Damping\",\"\")","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,4,"Non Linear Liq Visc >1.4 CPS",null,null,null,null,"30","zero","30",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW22*0.45),BW22+0.000001>'Modified Inputs'!$N$2),BV22,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW22*0.45),BW22+0.0000001>'Modified Inputs'!$N$2),BW22,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE21,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF22),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD22=\"01\",CD22=\"02\",CD22=\"03\",CD22=\"04\",CD22=\"05\",CD22=\"06\",CD22=\"07\",CD22=\"08\",CD22=\"09\",CD22=\"10\",CD22=\"11\"),'Modified Inputs'!$J$3<CG22),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH22),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,500,9.1604207194934428,"B-14-500",34.200000000000003,7.7,8,10,4,"31","1/2\"","31 : 1/2\" Diameter Tube 500 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F23*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G23)),\nSQRT(F23*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G23)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N23),cP/Basic10A32!N23),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N23),\"\"))","v":""},{"$f":"HLOOKUP(O23,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P23,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q23+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A41,0,Basic10A32!Q23)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A41,0,Basic10A32!Q23+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U23*N23/(1000*'10A61 5\" Calcs'!$O$46),U23*N23/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y23/Basic10A32!AA23,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y23/Basic10A32!Z23,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y23,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y23,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB23,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O23>'10A32 Tables'!S41),'10A32 Tables'!T41,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O23>'10A32 Tables'!Q41),'10A32 Tables'!R41,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O23>'10A32 Tables'!O41),'10A32 Tables'!P41,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O23>'10A32 Tables'!M41),'10A32 Tables'!N41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB41),'10A32 Tables'!AC41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z41),'10A32 Tables'!AA41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X41),'10A32 Tables'!Y41,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V41),'10A32 Tables'!W41,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH23,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE23),VLOOKUP(AI23,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE23+3,TRUE),VLOOKUP(AI23,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"31 : 1/2\" Diameter Tube 500 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA23-0.0000001)),\"\",AL23/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM23/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","31","B-14-500",1,"1/2\"","31 : 1/2\" Diameter Tube 500 L/h",8,10,4,0.3,500,"31 : 1/2\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,5,"Non Linear Liq Visc >1.4 CPS",null,null,null,null,"31","zero","31",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW23*0.45),BW23+0.000001>'Modified Inputs'!$N$2),BV23,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW23*0.45),BW23+0.0000001>'Modified Inputs'!$N$2),BW23,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE22,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF23),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD23=\"01\",CD23=\"02\",CD23=\"03\",CD23=\"04\",CD23=\"05\",CD23=\"06\",CD23=\"07\",CD23=\"08\",CD23=\"09\",CD23=\"10\",CD23=\"11\"),'Modified Inputs'!$J$3<CG23),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH23),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,600,10.992504863390133,"B-15-600",32.799999999999997,7.7,8,10,4,"32","1/2\"","32 : 1/2\" Diameter Tube 600 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F24*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G24)),\nSQRT(F24*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G24)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N24),cP/Basic10A32!N24),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N24),\"\"))","v":""},{"$f":"HLOOKUP(O24,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P24,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q24+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A42,0,Basic10A32!Q24)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A42,0,Basic10A32!Q24+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U24*N24/(1000*'10A61 5\" Calcs'!$O$46),U24*N24/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y24/Basic10A32!AA24,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y24/Basic10A32!Z24,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y24,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y24,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB24,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O24>'10A32 Tables'!S42),'10A32 Tables'!T42,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O24>'10A32 Tables'!Q42),'10A32 Tables'!R42,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O24>'10A32 Tables'!O42),'10A32 Tables'!P42,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O24>'10A32 Tables'!M42),'10A32 Tables'!N42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB42),'10A32 Tables'!AC42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z42),'10A32 Tables'!AA42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X42),'10A32 Tables'!Y42,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V42),'10A32 Tables'!W42,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH24,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE24),VLOOKUP(AI24,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE24+3,TRUE),VLOOKUP(AI24,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"32 : 1/2\" Diameter Tube 600 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA24-0.0000001)),\"\",AL24/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM24/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","32","B-15-600",1,"1/2\"","32 : 1/2\" Diameter Tube 600 L/h",8,10,4,0.3,600,"32 : 1/2\" Diameter Tube","Final Table",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32","zero","32",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW24*0.45),BW24+0.000001>'Modified Inputs'!$N$2),BV24,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW24*0.45),BW24+0.0000001>'Modified Inputs'!$N$2),BW24,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE23,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF24),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD24=\"01\",CD24=\"02\",CD24=\"03\",CD24=\"04\",CD24=\"05\",CD24=\"06\",CD24=\"07\",CD24=\"08\",CD24=\"09\",CD24=\"10\",CD24=\"11\"),'Modified Inputs'!$J$3<CG24),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH24),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,700,12.824589007286821,"B-16-700",31.4,7.7,8,10,4,"33","1/2\"","33 : 1/2\" Diameter Tube 700 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F25*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G25)),\nSQRT(F25*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G25)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N25),cP/Basic10A32!N25),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N25),\"\"))","v":""},{"$f":"HLOOKUP(O25,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P25,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q25+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A43,0,Basic10A32!Q25)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A43,0,Basic10A32!Q25+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U25*N25/(1000*'10A61 5\" Calcs'!$O$46),U25*N25/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y25/Basic10A32!AA25,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y25/Basic10A32!Z25,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y25,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y25,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB25,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O25>'10A32 Tables'!S43),'10A32 Tables'!T43,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O25>'10A32 Tables'!Q43),'10A32 Tables'!R43,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O25>'10A32 Tables'!O43),'10A32 Tables'!P43,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O25>'10A32 Tables'!M43),'10A32 Tables'!N43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB43),'10A32 Tables'!AC43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z43),'10A32 Tables'!AA43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X43),'10A32 Tables'!Y43,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V43),'10A32 Tables'!W43,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH25,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE25),VLOOKUP(AI25,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE25+3,TRUE),VLOOKUP(AI25,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"33 : 1/2\" Diameter Tube 700 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA25-0.0000001)),\"\",AL25/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM25/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","33","B-16-700",1,"1/2\"","33 : 1/2\" Diameter Tube 700 L/h",8,10,4,0.3,700,"33 : 1/2\" Diameter Tube","Name / Size","Range","Sizing Summary Scale Type","Damping ?","Configuration Preview Flow Range","Sizing Summary Flow Range","Configuration Preview Scale Type",null,null,null,null,null,null,null,null,null,"33","zero","33",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW25*0.45),BW25+0.000001>'Modified Inputs'!$N$2),BV25,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW25*0.45),BW25+0.0000001>'Modified Inputs'!$N$2),BW25,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE24,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF25),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD25=\"01\",CD25=\"02\",CD25=\"03\",CD25=\"04\",CD25=\"05\",CD25=\"06\",CD25=\"07\",CD25=\"08\",CD25=\"09\",CD25=\"10\",CD25=\"11\"),'Modified Inputs'!$J$3<CG25),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH25),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,800,14.656673151183512,"B-17-800",30.5,7.7,8,10,4,"34","1/2\"","34 : 1/2\" Diameter Tube 800 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F26*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G26)),\nSQRT(F26*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G26)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N26),cP/Basic10A32!N26),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N26),\"\"))","v":""},{"$f":"HLOOKUP(O26,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P26,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q26+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A44,0,Basic10A32!Q26)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A44,0,Basic10A32!Q26+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U26*N26/(1000*'10A61 5\" Calcs'!$O$46),U26*N26/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y26/Basic10A32!AA26,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y26/Basic10A32!Z26,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y26,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y26,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB26,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O26>'10A32 Tables'!S44),'10A32 Tables'!T44,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O26>'10A32 Tables'!Q44),'10A32 Tables'!R44,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O26>'10A32 Tables'!O44),'10A32 Tables'!P44,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O26>'10A32 Tables'!M44),'10A32 Tables'!N44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB44),'10A32 Tables'!AC44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z44),'10A32 Tables'!AA44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X44),'10A32 Tables'!Y44,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V44),'10A32 Tables'!W44,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH26,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE26),VLOOKUP(AI26,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE26+3,TRUE),VLOOKUP(AI26,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"34 : 1/2\" Diameter Tube 800 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA26-0.0000001)),\"\",(0.0000001)+AL26/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM26/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","34","B-17-800",1,"1/2\"","34 : 1/2\" Diameter Tube 800 L/h",8,10,4,0.3,800,"34 : 1/2\" Diameter Tube",{"$f":"IFERROR(BF19,\"\")","v":""},{"$f":"IF(BF26=\"\",\"\",BG19)","v":""},"","",{"$f":"IF($BH$26=\"\",\"\",BJ19)","v":""},{"$f":"IF($BH$26=\"\",\"\",BK19)","v":""},"",{"$f":"BJ26","v":""},null,null,null,null,null,null,null,null,"34","zero","34",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW26*0.45),BW26+0.000001>'Modified Inputs'!$N$2),BV26,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW26*0.45),BW26+0.0000001>'Modified Inputs'!$N$2),BW26,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE25,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF26),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD26=\"01\",CD26=\"02\",CD26=\"03\",CD26=\"04\",CD26=\"05\",CD26=\"06\",CD26=\"07\",CD26=\"08\",CD26=\"09\",CD26=\"10\",CD26=\"11\"),'Modified Inputs'!$J$3<CG26),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH26),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,800,14.534534208257064,"B-18-800",216,7.81,3,10,16,"40","1\"","40 : 1\" Diameter Tube 800 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F27*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G27)),\nSQRT(F27*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G27)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N27),cP/Basic10A32!N27),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N27),\"\"))","v":""},{"$f":"HLOOKUP(O27,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P27,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q27+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A45,0,Basic10A32!Q27)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A45,0,Basic10A32!Q27+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U27*N27/(1000*'10A61 5\" Calcs'!$O$46),U27*N27/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y27/Basic10A32!AA27,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y27/Basic10A32!Z27,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y27,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y27,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB27,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O27>'10A32 Tables'!S45),'10A32 Tables'!T45,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O27>'10A32 Tables'!Q45),'10A32 Tables'!R45,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O27>'10A32 Tables'!O45),'10A32 Tables'!P45,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O27>'10A32 Tables'!M45),'10A32 Tables'!N45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB45),'10A32 Tables'!AC45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z45),'10A32 Tables'!AA45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X45),'10A32 Tables'!Y45,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V45),'10A32 Tables'!W45,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH27,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE27),VLOOKUP(AI27,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE27+3,TRUE),VLOOKUP(AI27,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"40 : 1\" Diameter Tube 800 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA27-0.0000001)),\"\",AL27/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM27/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","40","B-18-800",1,"1\"","40 : 1\" Diameter Tube 800 L/h",3,10,16,0.4,800,"40 : 1\" Diameter Tube",{"$f":"IFERROR(BF20,\"\")","v":""},"","","",{"$f":"IF($BH$27=\"\",\"\",BJ20)","v":""},{"$f":"IF($BH$27=\"\",\"\",BK20)","v":""},{"$f":"IF($BH$27=\"\",\"\",BL20)","v":""},{"$f":"BJ27","v":""},null,null,null,null,null,null,null,null,"40","zero","40",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW27*0.45),BW27+0.000001>'Modified Inputs'!$N$2),BV27,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW27*0.45),BW27+0.0000001>'Modified Inputs'!$N$2),BW27,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE26,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF27),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD27=\"01\",CD27=\"02\",CD27=\"03\",CD27=\"04\",CD27=\"05\",CD27=\"06\",CD27=\"07\",CD27=\"08\",CD27=\"09\",CD27=\"10\",CD27=\"11\"),'Modified Inputs'!$J$3<CG27),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH27),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,1000,18.13763302458722,"B-19-1000",210,7.8,3,10,16,"41","1\"","41 : 1\" Diameter Tube 1000 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F28*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G28)),\nSQRT(F28*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G28)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N28),cP/Basic10A32!N28),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N28),\"\"))","v":""},{"$f":"HLOOKUP(O28,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P28,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q28+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A46,0,Basic10A32!Q28)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A46,0,Basic10A32!Q28+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U28*N28/(1000*'10A61 5\" Calcs'!$O$46),U28*N28/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y28/Basic10A32!AA28,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y28/Basic10A32!Z28,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y28,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y28,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB28,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O28>'10A32 Tables'!S46),'10A32 Tables'!T46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O28>'10A32 Tables'!Q46),'10A32 Tables'!R46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O28>'10A32 Tables'!O46),'10A32 Tables'!P46,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O28>'10A32 Tables'!M46),'10A32 Tables'!N46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB46),'10A32 Tables'!AC46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z46),'10A32 Tables'!AA46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X46),'10A32 Tables'!Y46,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V46),'10A32 Tables'!W46,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH28,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE28),VLOOKUP(AI28,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE28+3,TRUE),VLOOKUP(AI28,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"41 : 1\" Diameter Tube 1000 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA28-0.0000001)),\"\",AL28/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM28/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","41","B-19-1000",1,"1\"","41 : 1\" Diameter Tube 1000 L/h",3,10,16,0.4,1000,"41 : 1\" Diameter Tube",{"$f":"IFERROR(IF(BF27=\"\",\"\",BF21),\"\")","v":""},"","","",{"$f":"IF($BH$28=\"\",\"\",BJ21)","v":""},{"$f":"IF($BH$28=\"\",\"\",BK21)","v":""},{"$f":"IF($BH$28=\"\",\"\",BL21)","v":""},"",null,null,null,null,null,null,null,null,"41","zero","41",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW28*0.45),BW28+0.000001>'Modified Inputs'!$N$2),BV28,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW28*0.45),BW28+0.0000001>'Modified Inputs'!$N$2),BW28,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE27,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF28),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD28=\"01\",CD28=\"02\",CD28=\"03\",CD28=\"04\",CD28=\"05\",CD28=\"06\",CD28=\"07\",CD28=\"08\",CD28=\"09\",CD28=\"10\",CD28=\"11\"),'Modified Inputs'!$J$3<CG28),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH28),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,1600,29.06906841650413,"B-20-1600",195,7.8,3,10,16,"42","1\"","42 : 1\" Diameter Tube 1600 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F29*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G29)),\nSQRT(F29*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G29)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N29),cP/Basic10A32!N29),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N29),\"\"))","v":""},{"$f":"HLOOKUP(O29,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P29,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q29+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A47,0,Basic10A32!Q29)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A47,0,Basic10A32!Q29+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U29*N29/(1000*'10A61 5\" Calcs'!$O$46),U29*N29/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y29/Basic10A32!AA29,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y29/Basic10A32!Z29,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y29,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y29,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB29,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O29>'10A32 Tables'!S47),'10A32 Tables'!T47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O29>'10A32 Tables'!Q47),'10A32 Tables'!R47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O29>'10A32 Tables'!O47),'10A32 Tables'!P47,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O29>'10A32 Tables'!M47),'10A32 Tables'!N47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB47),'10A32 Tables'!AC47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z47),'10A32 Tables'!AA47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X47),'10A32 Tables'!Y47,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V47),'10A32 Tables'!W47,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH29,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE29),VLOOKUP(AI29,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE29+3,TRUE),VLOOKUP(AI29,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"42 : 1\" Diameter Tube 1600 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA29-0.0000001)),\"\",AL29/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM29/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","42","B-20-1600",1,"1\"","42 : 1\" Diameter Tube 1600 L/h",3,10,16,0.4,1600,"42 : 1\" Diameter Tube",{"$f":"IFERROR(IF(OR(BF27=\"\",BF28=\"\"),\"\",BF22),\"\")","v":""},"","","",{"$f":"IF($BH$29=\"\",\"\",BJ22)","v":""},{"$f":"IF($BH$29=\"\",\"\",BK22)","v":""},{"$f":"IF($BH$29=\"\",\"\",BL22)","v":""},"",null,null,null,null,null,null,null,null,"42","zero","42",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW29*0.45),BW29+0.000001>'Modified Inputs'!$N$2),BV29,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW29*0.45),BW29+0.0000001>'Modified Inputs'!$N$2),BW29,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE28,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF29),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD29=\"01\",CD29=\"02\",CD29=\"03\",CD29=\"04\",CD29=\"05\",CD29=\"06\",CD29=\"07\",CD29=\"08\",CD29=\"09\",CD29=\"10\",CD29=\"11\"),'Modified Inputs'!$J$3<CG29),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH29),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,2000,36.336335520627657,"B-21-2000",185,7.79,3,10,16,"43","1\"","43 : 1\" Diameter Tube 2000 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F30*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G30)),\nSQRT(F30*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G30)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N30),cP/Basic10A32!N30),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N30),\"\"))","v":""},{"$f":"HLOOKUP(O30,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P30,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q30+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A48,0,Basic10A32!Q30)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A48,0,Basic10A32!Q30+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U30*N30/(1000*'10A61 5\" Calcs'!$O$46),U30*N30/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y30/Basic10A32!AA30,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y30/Basic10A32!Z30,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y30,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y30,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB30,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O30>'10A32 Tables'!S48),'10A32 Tables'!T48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O30>'10A32 Tables'!Q48),'10A32 Tables'!R48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O30>'10A32 Tables'!O48),'10A32 Tables'!P48,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O30>'10A32 Tables'!M48),'10A32 Tables'!N48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB48),'10A32 Tables'!AC48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z48),'10A32 Tables'!AA48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X48),'10A32 Tables'!Y48,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V48),'10A32 Tables'!W48,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH30,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE30),VLOOKUP(AI30,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE30+3,TRUE),VLOOKUP(AI30,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"43 : 1\" Diameter Tube 2000 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA30-0.0000001)),\"\",AL30/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM30/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","43","B-21-2000",1,"1\"","43 : 1\" Diameter Tube 2000 L/h",3,10,16,0.4,2000,"43 : 1\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AU30","v":"43"},"zero","43",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW30*0.45),BW30+0.000001>'Modified Inputs'!$N$2),BV30,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW30*0.45),BW30+0.0000001>'Modified Inputs'!$N$2),BW30,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE29,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF30),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD30=\"01\",CD30=\"02\",CD30=\"03\",CD30=\"04\",CD30=\"05\",CD30=\"06\",CD30=\"07\",CD30=\"08\",CD30=\"09\",CD30=\"10\",CD30=\"11\"),'Modified Inputs'!$J$3<CG30),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH30),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,2500,45.435686768647884,"B-22-2500",176,7.79,3,10,16,"44","1\"","44 : 1\" Diameter Tube 2500 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F31*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G31)),\nSQRT(F31*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G31)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N31),cP/Basic10A32!N31),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N31),\"\"))","v":""},{"$f":"HLOOKUP(O31,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P31,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q31+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A49,0,Basic10A32!Q31)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A49,0,Basic10A32!Q31+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U31*N31/(1000*'10A61 5\" Calcs'!$O$46),U31*N31/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y31/Basic10A32!AA31,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y31/Basic10A32!Z31,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y31,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y31,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB31,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O31>'10A32 Tables'!S49),'10A32 Tables'!T49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O31>'10A32 Tables'!Q49),'10A32 Tables'!R49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O31>'10A32 Tables'!O49),'10A32 Tables'!P49,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O31>'10A32 Tables'!M49),'10A32 Tables'!N49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB49),'10A32 Tables'!AC49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z49),'10A32 Tables'!AA49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X49),'10A32 Tables'!Y49,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V49),'10A32 Tables'!W49,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH31,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE31),VLOOKUP(AI31,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE31+3,TRUE),VLOOKUP(AI31,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"44 : 1\" Diameter Tube 2500 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA31-0.0000001)),\"\",AL31/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM31/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","44","B-22-2500",1,"1\"","44 : 1\" Diameter Tube 2500 L/h",3,10,16,0.4,2500,"44 : 1\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"44","zero","44",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW31*0.45),BW31+0.000001>'Modified Inputs'!$N$2),BV31,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW31*0.45),BW31+0.0000001>'Modified Inputs'!$N$2),BW31,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE30,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF31),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD31=\"01\",CD31=\"02\",CD31=\"03\",CD31=\"04\",CD31=\"05\",CD31=\"06\",CD31=\"07\",CD31=\"08\",CD31=\"09\",CD31=\"10\",CD31=\"11\"),'Modified Inputs'!$J$3<CG31),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH31),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,3000,54.535038016668103,"B-23-3000",177,7.79,3,10,16,"45","1\"","45 : 1\" Diameter Tube 3000 L/h",{"$f":"IF('VA Sizing'!$C$3=\"Gas\",SQRT(F32*'10A61 5\" Calcs'!$O$46*(1-'10A61 5\" Calcs'!$O$46/Basic10A32!G32)),\nSQRT(F32*'Modified Inputs'!$M$2*(1-'Modified Inputs'!$M$2/Basic10A32!G32)))","v":0},{"$f":"IFERROR(IF('VA Sizing'!$C$3=\"Gas\",('10A61 5\" Calcs'!$T$46/Basic10A32!N32),cP/Basic10A32!N32),IF('VA Sizing'!$C$4=\"Steam\",('10A61 5\" Calcs'!$T$46/Basic10A32!N32),\"\"))","v":""},{"$f":"HLOOKUP(O32,'10A32 Tables'!$B$23:$K$23,1,TRUE)","v":{"$error":"#N/A"}},{"$f":"MATCH(P32,'10A32 Tables'!$B$23:$K$23,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A$23,0,Basic10A32!Q32+1)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A50,0,Basic10A32!Q32)","v":{"$error":"#N/A"}},{"$f":"OFFSET('10A32 Tables'!$A50,0,Basic10A32!Q32+1)","v":{"$error":"#N/A"}},{"$error":"#N/A"},null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",U32*N32/(1000*'10A61 5\" Calcs'!$O$46),U32*N32/(1000*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/273)","v":{"$error":"#DIV/0!"}},{"$f":"(14.7/'Modified Inputs'!$I$2)*('Modified Inputs'!$K$3/294)","v":{"$error":"#DIV/0!"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",Basic10A32!Y32/Basic10A32!AA32,\nIF('VA Sizing'!$C$5=\"Normal\",Basic10A32!Y32/Basic10A32!Z32,\nIF('VA Sizing'!$C$5=\"Actual\",Basic10A32!Y32,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",Basic10A32!Y32,\nIF('VA Sizing'!$C$3=\"Gas\",Basic10A32!AB32,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O32>'10A32 Tables'!S50),'10A32 Tables'!T50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O32>'10A32 Tables'!Q50),'10A32 Tables'!R50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O32>'10A32 Tables'!O50),'10A32 Tables'!P50,\nIF(AND('VA Sizing'!$C$3=\"Gas\",Basic10A32!O32>'10A32 Tables'!M50),'10A32 Tables'!N50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!AB50),'10A32 Tables'!AC50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!Z50),'10A32 Tables'!AA50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!X50),'10A32 Tables'!Y50,\nIF(AND('VA Sizing'!$C$3=\"Liquid\",cP>'10A32 Tables'!V50),'10A32 Tables'!W50,1))))))))","v":1},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$f":"VLOOKUP(AH32,'10A32 Tables'!$B$53:$D$118,3,TRUE)","v":{"$error":"#VALUE!"}},{"$f":"IF(ISNUMBER(AE32),VLOOKUP(AI32,'10A32 Tables'!$D$53:$L$118,Basic10A32!AE32+3,TRUE),VLOOKUP(AI32,'10A32 Tables'!$D$53:$L$118,9,TRUE))","v":{"$error":"#VALUE!"}},null,{"$error":"#VALUE!"},{"$error":"#VALUE!"},1,"45 : 1\" Diameter Tube 3000 L/h",{"$f":"IFERROR(IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>(Basic10A32!BA32-0.0000001)),\"\",AL32/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)),\"\")","v":""},{"$f":"AM32/'Modified Inputs'!$J$15*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)","v":{"$error":"#VALUE!"}},0,0,"0 - 0","45","B-23-3000",1,"1\"","45 : 1\" Diameter Tube 3000 L/h",3,10,16,0.4,3000,"45 : 1\" Diameter Tube",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"45","zero","45",null,{"$f":"IF(AND('Modified Inputs'!$N$2>(BW32*0.45),BW32+0.000001>'Modified Inputs'!$N$2),BV32,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>(BW32*0.45),BW32+0.0000001>'Modified Inputs'!$N$2),BW32,0),0)","v":0},null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE31,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF32),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD32=\"01\",CD32=\"02\",CD32=\"03\",CD32=\"04\",CD32=\"05\",CD32=\"06\",CD32=\"07\",CD32=\"08\",CD32=\"09\",CD32=\"10\",CD32=\"11\"),'Modified Inputs'!$J$3<CG32),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH32),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,0,null,null,null,null,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE32,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF33),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD33=\"01\",CD33=\"02\",CD33=\"03\",CD33=\"04\",CD33=\"05\",CD33=\"06\",CD33=\"07\",CD33=\"08\",CD33=\"09\",CD33=\"10\",CD33=\"11\"),'Modified Inputs'!$J$3<CG33),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH33),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE33,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF34),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD34=\"01\",CD34=\"02\",CD34=\"03\",CD34=\"04\",CD34=\"05\",CD34=\"06\",CD34=\"07\",CD34=\"08\",CD34=\"09\",CD34=\"10\",CD34=\"11\"),'Modified Inputs'!$J$3<CG34),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH34),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"01 : 1/4\" Dia. 1 L/HR","01 : 1/4\" Diameter Tube 1 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE34,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF35),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD35=\"01\",CD35=\"02\",CD35=\"03\",CD35=\"04\",CD35=\"05\",CD35=\"06\",CD35=\"07\",CD35=\"08\",CD35=\"09\",CD35=\"10\",CD35=\"11\"),'Modified Inputs'!$J$3<CG35),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH35),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"02 : 1/4\" Dia. 1.6 L/HR","02 : 1/4\" Diameter Tube 1.6 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE35,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF36),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD36=\"01\",CD36=\"02\",CD36=\"03\",CD36=\"04\",CD36=\"05\",CD36=\"06\",CD36=\"07\",CD36=\"08\",CD36=\"09\",CD36=\"10\",CD36=\"11\"),'Modified Inputs'!$J$3<CG36),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH36),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"03 : 1/4\" Dia. 2.5 L/HR","03 : 1/4\" Diameter Tube 2.5 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE36,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF37),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD37=\"01\",CD37=\"02\",CD37=\"03\",CD37=\"04\",CD37=\"05\",CD37=\"06\",CD37=\"07\",CD37=\"08\",CD37=\"09\",CD37=\"10\",CD37=\"11\"),'Modified Inputs'!$J$3<CG37),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH37),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"04 : 1/4\" Dia. 4 L/HR","04 : 1/4\" Diameter Tube 4 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE37,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF38),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD38=\"01\",CD38=\"02\",CD38=\"03\",CD38=\"04\",CD38=\"05\",CD38=\"06\",CD38=\"07\",CD38=\"08\",CD38=\"09\",CD38=\"10\",CD38=\"11\"),'Modified Inputs'!$J$3<CG38),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH38),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"05 : 1/4\" Dia. 6 L/HR","05 : 1/4\" Diameter Tube 6 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE38,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF39),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD39=\"01\",CD39=\"02\",CD39=\"03\",CD39=\"04\",CD39=\"05\",CD39=\"06\",CD39=\"07\",CD39=\"08\",CD39=\"09\",CD39=\"10\",CD39=\"11\"),'Modified Inputs'!$J$3<CG39),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH39),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"06 : 1/4\" Dia. 10 L/HR","06 : 1/4\" Diameter Tube 10 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE39,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF40),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD40=\"01\",CD40=\"02\",CD40=\"03\",CD40=\"04\",CD40=\"05\",CD40=\"06\",CD40=\"07\",CD40=\"08\",CD40=\"09\",CD40=\"10\",CD40=\"11\"),'Modified Inputs'!$J$3<CG40),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH40),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"07 : 1/4\" Dia. 16 L/HR","07 : 1/4\" Diameter Tube 16 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE40,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF41),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD41=\"01\",CD41=\"02\",CD41=\"03\",CD41=\"04\",CD41=\"05\",CD41=\"06\",CD41=\"07\",CD41=\"08\",CD41=\"09\",CD41=\"10\",CD41=\"11\"),'Modified Inputs'!$J$3<CG41),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH41),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"08 : 1/4\" Dia. 25 L/HR","08 : 1/4\" Diameter Tube 25 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE41,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF42),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD42=\"01\",CD42=\"02\",CD42=\"03\",CD42=\"04\",CD42=\"05\",CD42=\"06\",CD42=\"07\",CD42=\"08\",CD42=\"09\",CD42=\"10\",CD42=\"11\"),'Modified Inputs'!$J$3<CG42),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH42),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"09 : 1/4\" Dia. 40 L/HR","09 : 1/4\" Diameter Tube 40 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE42,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF43),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD43=\"01\",CD43=\"02\",CD43=\"03\",CD43=\"04\",CD43=\"05\",CD43=\"06\",CD43=\"07\",CD43=\"08\",CD43=\"09\",CD43=\"10\",CD43=\"11\"),'Modified Inputs'!$J$3<CG43),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH43),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10 : 1/4\" Dia. 60 L/HR","10 : 1/4\" Diameter Tube 60 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE43,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF44),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD44=\"01\",CD44=\"02\",CD44=\"03\",CD44=\"04\",CD44=\"05\",CD44=\"06\",CD44=\"07\",CD44=\"08\",CD44=\"09\",CD44=\"10\",CD44=\"11\"),'Modified Inputs'!$J$3<CG44),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH44),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"11 : 1/4\" Dia. 100 L/HR","11 : 1/4\" Diameter Tube 100 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE44,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF45),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD45=\"01\",CD45=\"02\",CD45=\"03\",CD45=\"04\",CD45=\"05\",CD45=\"06\",CD45=\"07\",CD45=\"08\",CD45=\"09\",CD45=\"10\",CD45=\"11\"),'Modified Inputs'!$J$3<CG45),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH45),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20 : 3/8\" Dia. 100 L/HR","20 : 3/8\" Diameter Tube 100 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE45,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF46),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD46=\"01\",CD46=\"02\",CD46=\"03\",CD46=\"04\",CD46=\"05\",CD46=\"06\",CD46=\"07\",CD46=\"08\",CD46=\"09\",CD46=\"10\",CD46=\"11\"),'Modified Inputs'!$J$3<CG46),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH46),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"21 : 3/8\" Dia. 160 L/HR","21 : 3/8\" Diameter Tube 160 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE46,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF47),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD47=\"01\",CD47=\"02\",CD47=\"03\",CD47=\"04\",CD47=\"05\",CD47=\"06\",CD47=\"07\",CD47=\"08\",CD47=\"09\",CD47=\"10\",CD47=\"11\"),'Modified Inputs'!$J$3<CG47),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH47),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"22 : 3/8\" Dia. 200 L/HR","22 : 3/8\" Diameter Tube 200 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE47,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF48),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD48=\"01\",CD48=\"02\",CD48=\"03\",CD48=\"04\",CD48=\"05\",CD48=\"06\",CD48=\"07\",CD48=\"08\",CD48=\"09\",CD48=\"10\",CD48=\"11\"),'Modified Inputs'!$J$3<CG48),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH48),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"23 : 3/8\" Dia. 250 L/HR","23 : 3/8\" Diameter Tube 250 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE48,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF49),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD49=\"01\",CD49=\"02\",CD49=\"03\",CD49=\"04\",CD49=\"05\",CD49=\"06\",CD49=\"07\",CD49=\"08\",CD49=\"09\",CD49=\"10\",CD49=\"11\"),'Modified Inputs'!$J$3<CG49),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH49),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24 : 3/8\" Dia. 300 L/HR","24 : 3/8\" Diameter Tube 300 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE49,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF50),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD50=\"01\",CD50=\"02\",CD50=\"03\",CD50=\"04\",CD50=\"05\",CD50=\"06\",CD50=\"07\",CD50=\"08\",CD50=\"09\",CD50=\"10\",CD50=\"11\"),'Modified Inputs'!$J$3<CG50),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH50),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30 : 1/2\" Dia. 400 L/HR","30 : 1/2\" Diameter Tube 400 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE50,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF51),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD51=\"01\",CD51=\"02\",CD51=\"03\",CD51=\"04\",CD51=\"05\",CD51=\"06\",CD51=\"07\",CD51=\"08\",CD51=\"09\",CD51=\"10\",CD51=\"11\"),'Modified Inputs'!$J$3<CG51),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH51),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"31 : 1/2\" Dia. 500 L/HR","31 : 1/2\" Diameter Tube 500 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE51,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF52),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD52=\"01\",CD52=\"02\",CD52=\"03\",CD52=\"04\",CD52=\"05\",CD52=\"06\",CD52=\"07\",CD52=\"08\",CD52=\"09\",CD52=\"10\",CD52=\"11\"),'Modified Inputs'!$J$3<CG52),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH52),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32 : 1/2\" Dia. 600 L/HR","32 : 1/2\" Diameter Tube 600 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE52,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF53),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD53=\"01\",CD53=\"02\",CD53=\"03\",CD53=\"04\",CD53=\"05\",CD53=\"06\",CD53=\"07\",CD53=\"08\",CD53=\"09\",CD53=\"10\",CD53=\"11\"),'Modified Inputs'!$J$3<CG53),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH53),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"33 : 1/2\" Dia. 700 L/HR","33 : 1/2\" Diameter Tube 700 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE53,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF54),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD54=\"01\",CD54=\"02\",CD54=\"03\",CD54=\"04\",CD54=\"05\",CD54=\"06\",CD54=\"07\",CD54=\"08\",CD54=\"09\",CD54=\"10\",CD54=\"11\"),'Modified Inputs'!$J$3<CG54),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH54),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34 : 1/2\" Dia. 800 L/HR","34 : 1/2\" Diameter Tube 800 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE54,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF55),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD55=\"01\",CD55=\"02\",CD55=\"03\",CD55=\"04\",CD55=\"05\",CD55=\"06\",CD55=\"07\",CD55=\"08\",CD55=\"09\",CD55=\"10\",CD55=\"11\"),'Modified Inputs'!$J$3<CG55),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH55),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"40 : 1\" Dia. 800 L/HR","40 : 1\" Diameter Tube 800 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE55,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF56),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD56=\"01\",CD56=\"02\",CD56=\"03\",CD56=\"04\",CD56=\"05\",CD56=\"06\",CD56=\"07\",CD56=\"08\",CD56=\"09\",CD56=\"10\",CD56=\"11\"),'Modified Inputs'!$J$3<CG56),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH56),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"41 : 1\" Dia. 1000 L/HR","41 : 1\" Diameter Tube 1000 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE56,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF57),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD57=\"01\",CD57=\"02\",CD57=\"03\",CD57=\"04\",CD57=\"05\",CD57=\"06\",CD57=\"07\",CD57=\"08\",CD57=\"09\",CD57=\"10\",CD57=\"11\"),'Modified Inputs'!$J$3<CG57),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH57),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"42 : 1\" Dia. 1600 L/HR","42 : 1\" Diameter Tube 1600 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE57,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF58),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD58=\"01\",CD58=\"02\",CD58=\"03\",CD58=\"04\",CD58=\"05\",CD58=\"06\",CD58=\"07\",CD58=\"08\",CD58=\"09\",CD58=\"10\",CD58=\"11\"),'Modified Inputs'!$J$3<CG58),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH58),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"43 : 1\" Dia. 2000 L/HR","43 : 1\" Diameter Tube 2000 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE58,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF59),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD59=\"01\",CD59=\"02\",CD59=\"03\",CD59=\"04\",CD59=\"05\",CD59=\"06\",CD59=\"07\",CD59=\"08\",CD59=\"09\",CD59=\"10\",CD59=\"11\"),'Modified Inputs'!$J$3<CG59),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH59),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"44 : 1\" Dia. 2500 L/HR","44 : 1\" Diameter Tube 2500 L/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"MAX(IF($CA$6:$CA$32<CE59,$CA$6:$CA$32))","v":0},4,-100,0,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>CF60),\"viscosity\",\nIF(AND('VA Sizing'!$C$3=\"Liquid\"),\"\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR(CD60=\"01\",CD60=\"02\",CD60=\"03\",CD60=\"04\",CD60=\"05\",CD60=\"06\",CD60=\"07\",CD60=\"08\",CD60=\"09\",CD60=\"10\",CD60=\"11\"),'Modified Inputs'!$J$3<CG60),\"pressure\",\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<CH60),\"pressure\",\"\"))))","v":{"$error":"#N/A"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"45 : 1\" Dia. 3000 L/HR","45 : 1\" Diameter Tube 3000 L/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]

{"sheet":"10A32 Tables","index":41,"n_rows":118,"n_cols":29,"rows_kept":118,"cut":false,"hidden":true,"merged":[[21,12,21,19],[21,21,21,28]]}
[]
["N",null,null,0.01,0.05,0.1,0.2,0.5,1,2,5,10,null,null,14]
[]
[null,null,null,0.01,0.05,0.1,0.2,0.4,0.5,0.8,1,1.1000000000000001,null,null,2,5,10,14]
["K","1 L/H",null,25.4,23.3,20.7,15.5,11,9.6,6,4.0999999999999996,1.5,null,null,2.4,1.2,1,1]
[]
[null,null,null,null,{"$f":"LINEST(D5:K5,D4:K4^{1;2;3})","v":-35.612702677172237},76.664843741257897,-63.15984463198248,26.071979112749926]
[null,null,null,null,{"$f":"'10A32 Tables'!E7*'10A32 Capacity'!O6^3+'10A32 Tables'!F7*'10A32 Capacity'!O6^2+'10A32 Tables'!G7*'10A32 Capacity'!O6+'10A32 Tables'!H7","v":{"$error":"#VALUE!"}}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"LINEST(LN(D5:R5),LN(D4:R4))","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"EXP(U11)","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U12*'10A32 Capacity'!O6^T11","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Gas Scales",null,null,null,null,null,null,null,null,"Liquid Scales"]
[null,1E-3,0.05,0.1,0.2,0.5,1,2,5,10,14,null,null,null,null,null,null,null,null,null,null,null,null,"Vstd",null,"Vmax"]
["01H",25.4,23.3,20.7,15.5,9.6,4.0999999999999996,2.4,1.2,1,1,"01H",0,4,1E-3,3,0.2,2,50000,"---",null,1.4,4,4,"NS",8,"---",50000,"---"]
["02H",34.200000000000003,31.6,28.4,22,14.7,8.4,5,2,1,1,"02H",0,4,1E-3,3,0.2,2,50000,"---",null,1.4,4,4,"NS",8,"---",50000,"---"]
["03H",48,47,41,32,23.5,12.5,8.3000000000000007,4,1,1,"03H",0,4,1E-3,3,0.2,2,50000,"---",null,1.4,4,6,"NS",8,"---",50000,"---"]
["04H",66,65,59,51,37,24,15,7,1,1,"04H",0,4,1E-3,3,0.15,2,50000,"---",null,1.4,4,6,"NS",8,"---",50000,"---"]
["05H",83,80,77,72,55,38,24.3,11,5.5,4,"05H",0,1,1E-3,2,0.1,3,50000,"---",null,1.4,4,18,"NS",24,"---",50000,"---"]
["06H",116,113,110,106,91.3,64,46,24.3,12,9,"06H",0,1,1E-3,2,0.1,3,50000,"---",null,1.4,4,18,"NS",24,"---",50000,"---"]
["07H",177,174,170,163,142,107,84,50,33,26,"07H",0,1,1E-3,2,0.15,3,50000,"---",null,1.4,4,18,"NS",24,"---",50000,"---"]
["08H",230,225,220,211,182,160,130,88,63,53,"08H",0,1,1E-3,2,0.1,3,50000,"---",null,1.4,4,18,"NS",24,"---",50000,"---"]
["09H",396,392,388,381,357,351,337,297,230,177,"09H",0,1,0.1,2,1,3,50000,"---",null,1.4,4,18,"NS",24,"---",50000,"---"]
["10H",505,499,494,483,449,393,403,348,255,181,"10H",0,1,0.1,2,1,3,50000,"---",null,1.4,4,18,"NS",24,"---",50000,"---"]
["11H",819,811,804,789,744,670,545,542,535,530,"11H",0,1,0.15,2,1,3,50000,"---",null,1.4,5,8,1,12,"NS",24,"---"]
["20H",373,367,356,331,306,280,235,208,164,128,"20H",0,1,1E-3,2,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["21H",578,571,566,545,512,475,420,387,334,291,"21H",0,1,1E-3,2,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["22H",724,716,710,690,645,595,550,525,482,452,"22H",0,1,2.5000000000000001E-2,2,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["23H",943,935,924,877,815,760,705,672,616,571,"23H",0,1,1E-3,1,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["24H",1114,1102,1094,1070,1000,930,870,828,757,700,"24H",0,1,1E-3,1,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["30H",1250,1248,1233,1204,1100,1000,922,845,730,665,"30H",0,1,1E-3,2,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["31H",1565,1562,1553,1535,1350,1170,1090,1007,837,752,"31H",0,1,1E-3,2,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["32H",1890,1887,1883,1877,1600,1360,1220,1125,960,833,"32H",0,1,1E-3,1,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["33H",2310,2307,2282,2233,1800,1490,1370,1236,1045,905,"33H",0,1,1E-3,1,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["34H",2600,2600,2598,2594,2100,1610,1418,1310,1120,965,"34H",0,1,1E-3,1,1,3,50000,"---",null,1.4,4,8,"NS",10,"---",50000,"---"]
["40H",972,972,972,950,910,850,"-","-","-","-","40H",0,1,0.1,2,1,3,50000,"---",null,1.4,1,2,"NS",10,"---",50000,"---"]
["41H",1232,1232,1232,1195,1135,1055,"-","-","-","-","41H",0,1,0.1,2,1,3,50000,"---",null,1.4,1,2,"NS",10,"---",50000,"---"]
["42H",2045,2045,2045,1984,1884,1750,"-","-","-","-","42H",0,1,1E-3,1,1,3,50000,"---",null,1.4,1,3,"NS",10,"---",50000,"---"]
["43H",2625,2625,2625,2546,2425,2245,"-","-","-","-","43H",0,1,1E-3,1,1,3,50000,"---",null,1.4,1,4,"NS",10,"---",50000,"---"]
["44H",3364,3364,3364,3263,3063,2750,"-","-","-","-","44H",0,1,1E-3,1,1,3,50000,"---",null,1.4,1,5,"NS",10,"---",50000,"---"]
["45H",4025,4025,4025,3905,3755,3555,"-","-","-","-","45H",0,1,1E-3,1,1,3,50000,"---",null,1.4,1,6,"NS",10,"---",50000,"---"]
[]
[null,"max(u)","max(o)","max","Intervall (max)","Rundungsfaktor","min (Typ 1)","min (Typ 2)","min (Typ 3)","min (Typ 4)","min (Typ 5)","min (Typ NS)"]
[null,97.5,102.499999,100,"[97,5; 102,499999]",5,"10","20","25","10","10","10"]
[null,102.5,107.499999,105,"[102,5; 107,499999]",5,"10","20","25","10","10","10"]
[null,107.5,112.499999,110,"[107,5; 112,499999]",5,"10","20","25","10","10","10"]
[null,112.5,117.499999,115,"[112,5; 117,499999]",5,"10","20","25","10","10","10"]
[null,117.5,122.499999,120,"[117,5; 122,499999]",5,"10","20","30","10","10","10"]
[null,122.5,127.499999,125,"[122,5; 127,499999]",5,"10","20","30","10","10","10"]
[null,127.5,132.499999,130,"[127,5; 132,499999]",5,"10","20","30","10","10","10"]
[null,132.5,137.499999,135,"[132,5; 137,499999]",5,"10","25","30","10","10","10"]
[null,137.5,142.499999,140,"[137,5; 142,499999]",5,"10","25","30","10","10","10"]
[null,142.5,147.499999,145,"[142,5; 147,499999]",5,"10","25","35","10","10","10"]
[null,147.5,154.999999,150,"[147,5; 154,999999]",10,"20","30","40","20","20","20"]
[null,155,164.999999,160,"[155,0; 164,999999]",10,"20","30","40","20","20","20"]
[null,165,174.999999,170,"[165,0; 174,999999]",10,"20","30","40","20","20","20"]
[null,175,184.999999,180,"[175,0; 184,999999]",10,"20","30","40","20","20","20"]
[null,185,194.999999,190,"[185,0; 194,999999]",10,"20","30","50","20","20","20"]
[null,195,204.999999,200,"[195,0; 204,999999]",10,"20","40","50","20","20","20"]
[null,205,214.999999,210,"[205,0; 214,999999]",10,"20","40","50","20","20","20"]
[null,215,224.999999,220,"[215,0; 224,999999]",10,"20","40","50","20","20","20"]
[null,225,234.999999,230,"[225,0; 234,999999]",10,"20","40","50","20","20","20"]
[null,235,244.999999,240,"[235,0; 244,999999]",10,"20","40","60","20","20","20"]
[null,245,254.999999,250,"[245,0; 254,999999]",10,"20","40","60","20","20","20"]
[null,255,264.999999,260,"[255,0; 264,999999]",10,"20","40","60","20","20","20"]
[null,265,274.999999,270,"[265,0; 274,999999]",10,"20","50","60","20","20","20"]
[null,275,284.999999,280,"[275,0; 284,999999]",10,"20","50","60","20","20","20"]
[null,285,294.999999,290,"[285,0; 294,999999]",10,"20","50","70","20","20","20"]
[null,295,304.999999,300,"[295,0; 304,999999]",10,"30","50","70","30","30","30"]
[null,305,314.999999,310,"[305,0; 314,999999]",10,"30","50","70","30","30","30"]
[null,315,324.999999,320,"[315,0; 324,999999]",10,"30","50","70","30","30","30"]
[null,325,334.999999,330,"[325,0; 334,999999]",10,"30","60","80","30","30","30"]
[null,335,344.999999,340,"[335,0; 344,999999]",10,"30","60","80","30","30","30"]
[null,345,354.999999,350,"[345,0; 354,999999]",10,"30","60","80","30","30","30"]
[null,355,364.999999,360,"[355,0; 364,999999]",10,"30","60","80","30","30","30"]
[null,365,374.999999,370,"[365,0; 374,999999]",10,"30","60","80","30","30","30"]
[null,375,384.999999,380,"[375,0; 384,999999]",10,"30","60","90","30","30","30"]
[null,385,394.999999,390,"[385,0; 394,999999]",10,"30","60","90","30","30","30"]
[null,395,409.999999,400,"[395,0; 409,999999]",20,"40","80","100","40","40","40"]
[null,410,429.999999,420,"[410,0; 429,999999]",20,"40","80","100","40","40","40"]
[null,430,449.999999,440,"[430,0; 449,999999]",20,"40","80","100","40","40","40"]
[null,450,469.999999,460,"[450,0; 469,999999]",20,"40","80","100","40","40","40"]
[null,470,489.999999,480,"[470,0; 489,999999]",20,"40","80","120","40","40","40"]
[null,490,509.999999,500,"[490,0; 509,999999]",20,"40","80","120","40","40","40"]
[null,510,529.999999,520,"[510,0; 529,999999]",20,"40","80","120","40","40","40"]
[null,530,549.999999,540,"[530,0; 549,999999]",20,"40","100","120","40","40","40"]
[null,550,569.999999,560,"[550,0; 569,999999]",20,"40","100","120","40","40","40"]
[null,570,589.999999,580,"[570,0; 589,999999]",20,"40","100","140","40","40","40"]
[null,590,609.999999,600,"[590,0; 609,999999]",20,"60","100","140","60","60","60"]
[null,610,629.999999,620,"[610,0; 629,999999]",20,"60","100","140","60","60","60"]
[null,630,649.999999,640,"[630,0; 649,999999]",20,"60","100","140","60","60","60"]
[null,650,669.999999,660,"[650,0; 669,999999]",20,"60","120","160","60","60","60"]
[null,670,689.999999,680,"[670,0; 689,999999]",20,"60","120","160","60","60","60"]
[null,690,709.999999,700,"[690,0; 709,999999]",20,"60","120","160","60","60","60"]
[null,710,729.999999,720,"[710,0; 729,999999]",20,"60","120","160","60","60","60"]
[null,730,749.999999,740,"[730,0; 749,999999]",20,"60","120","160","60","60","60"]
[null,750,769.999999,760,"[750,0; 769,999999]",20,"60","120","180","60","60","60"]
[null,770,789.999999,780,"[770,0; 789,999999]",20,"60","120","180","60","60","60"]
[null,790,809.999999,800,"[790,0; 809,999999]",20,"80","140","180","80","80","80"]
[null,810,829.999999,820,"[810,0; 829,999999]",20,"80","140","180","80","80","80"]
[null,830,849.999999,840,"[830,0; 849,999999]",20,"80","140","180","80","80","80"]
[null,850,869.999999,860,"[850,0; 869,999999]",20,"80","140","200","80","80","80"]
[null,870,889.999999,880,"[870,0; 889,999999]",20,"80","140","200","80","80","80"]
[null,890,909.999999,900,"[890,0; 909,999999]",20,"80","140","200","80","80","80"]
[null,910,929.999999,920,"[910,0; 929,999999]",20,"80","140","200","80","80","80"]
[null,930,949.999999,940,"[930,0; 949,999999]",20,"80","160","220","80","80","80"]
[null,950,969.999999,960,"[950,0; 969,999999]",20,"80","160","220","80","80","80"]
[null,970,989.999999,980,"[970,0; 989,999999]",20,"80","160","220","80","80","80"]
[null,990,1024.9999990000001,1000,"[990,0; 1024,999999]",50,"100","200","250","100","100","100"]

{"sheet":"IX Preview","index":42,"n_rows":102,"n_cols":15,"rows_kept":102,"cut":false,"hidden":true,"merged":[]}
[null,"Application",{"$f":"'VA Sizing'!C3","v":0}]
[null,"Fluid",{"$f":"IF(RIGHT('VA Sizing'!B4,1)=\" \",\"Mixed Gas\",'VA Sizing'!C4)","v":0},null,null,null,null,"Flowrate","Actual","Normal","Standard",null,null,"Density","Display"]
["0.3 - 2.9","Flowrate",{"$f":"IFERROR(RIGHT(A3,E3),\"\")","v":" 2.9"},{"$f":"IFERROR(IF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C5=\"Standard\"),VLOOKUP('IX Preview'!A4,'IX Preview'!H3:K31,4,FALSE),\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C5=\"Normal\"),VLOOKUP('IX Preview'!A4,'IX Preview'!H3:K31,3,FALSE),\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C5=\"Actual\"),VLOOKUP('IX Preview'!A4,'IX Preview'!H3:K31,2,FALSE),VLOOKUP('IX Preview'!A4,'IX Preview'!H3:K31,2,FALSE)))),\"\")","v":"scfh"},{"$f":"LEN(A3)-FIND(\"-\",A3&\"-\")","v":4},null,null,"cc/min","ml/min","ml/min(qn)","sccm",null,null,"S.G.","g/ml"]
["scfh","Density",{"$f":"IF('VA Sizing'!C3=\"Gas\",'IX Preview'!A5,\nIF('VA Sizing'!C3=\"Liquid\",'IX Preview'!A7,\"\"))","v":""},{"$f":"IF('VA Sizing'!C3=\"Gas\",VLOOKUP('IX Preview'!A6,N3:O9,2,FALSE),\nIF('VA Sizing'!C3=\"Liquid\",VLOOKUP('IX Preview'!A8,N3:O9,2,FALSE),\"\"))","v":""},{"$f":"IFERROR(LEFT(A3,LEN(A3)-E3-2),\"\")","v":"0.3"},null,null,"mL/min","ml/min","ml/min(qn)","sccm",null,null,"kg/m3","kg/m^3"]
["","Viscosity",{"$f":"IF('VA Sizing'!C3=\"Liquid\",'VA Sizing'!C8,\"\")","v":""},{"$f":"IF('VA Sizing'!C3=\"Liquid\",'VA Sizing'!D8,\"\")","v":""},null,null,null,"mL/h","ml/h","ml/h(qn)","ml/h",null,null,"kg/L","kg/l"]
["","Pressure",{"$f":"IF('VA Sizing'!$C$4=\"Steam\",ROUND(SizingSummary!C9,1),SizingSummary!C9)","v":0},{"$f":"IF(AND(C6=\"\",'VA Sizing'!C3=\"Liquid\"),\"\",\nIFERROR(VLOOKUP(A9,N14:O25,2,FALSE),\"\"))","v":""},null,null,null,"mL/s","ml/s","ml/s(qn)","ml/s",null,null,"g/mL","g/ml"]
[{"$f":"'VA Sizing'!C11","v":0},"Temperature",{"$f":"IF('VA Sizing'!$C$4=\"Steam\",ROUND(SizingSummary!C10,1),SizingSummary!C10)","v":0},{"$f":"IF(AND(C7=\"\",'VA Sizing'!C3=\"Liquid\"),\"\",\nIF(SizingSummary!D10=0,\"\",SizingSummary!D10))","v":""},null,null,null,"l/h","l/h","Nl/h","sl/h",null,null,"g/cm3","g/cm^3"]
[{"$f":"'VA Sizing'!D11","v":0},null,null,null,null,null,null,"l/min","l/min","Nl/min","sl/min",null,null,"lb/ft3","lb/ft^3"]
[{"$f":"SizingSummary!D9","v":""},null,null,null,null,null,null,"l/s","l/s","Nl/s","sl/s",null,null,"lb/USgal","lb/USgal"]
[null,null,null,null,null,null,null,"m3/h","m^3/h","Nm^3/h","sm^3/h"]
[null,null,null,null,null,null,null,"m3/min","m^3/min","Nm^3/min","sm^3/min"]
[null,null,null,null,null,null,null,"ft3/h","ft^3/h","ft^3/h(qn)","scfh"]
[null,null,null,null,null,null,null,"ft3/min","ft^3/min","ft^3/min(qn)","scfm",null,null,"Pressure Units","Display"]
[null,null,null,null,null,null,null,"ft3/s","ft^3/s","ft^3/s(qn)","scfs",null,null,"psi(a)","psi(a)"]
[null,null,null,null,null,null,null,"I GPH","UKgal/h","UKgal/h(qn)","UKgal/h",null,null,"psi(g)","psi"]
[null,null,null,null,null,null,null,"I GPM","UKgal/min","UKgal/min(qn)","UKgal/min",null,null,"bar(a)","bar(a)"]
[null,null,null,null,null,null,null,"US GPH","USgal/h","USgal/h(qn)","USgal/h",null,null,"bar(g)","bar"]
[null,null,null,null,null,null,null,"US GPM","USgal/min","USgal/min(qn)","USgal/min",null,null,"atm(a)","atm(a)"]
[null,null,null,null,null,null,null,"in3/h","in^3/h","in^3/h(qn)","in^3/h",null,null,"atm(g)","atm"]
[null,null,null,null,null,null,null,"in3/min","in^3/min","in^3/min(qn)","scinm",null,null,"kpa(a)","kPa(a)"]
[null,null,null,null,null,null,null,"in3/s","in^3/s","in^3/s(qn)","in^3/s",null,null,"kpa(g)","kPa"]
[null,null,null,null,null,null,null,"g/min","g/min","g/min","g/min",null,null,"inH2O(a)","inH2O(a)"]
[null,null,null,null,null,null,null,"g/h","g/h","g/h","g/h",null,null,"inH2O(g)","inH2O"]
[null,null,null,null,null,null,null,"kg/min","kg/min","kg/min","kg/min",null,null,"kg/cm2(a)","kg/cm^2(a)"]
[null,null,null,null,null,null,null,"kg/h","kg/h","kg/h","kg/h",null,null,"kg/cm2(g)","kg/cm^2"]
[null,null,null,null,null,null,null,"lb/min","lb/min","lb/min","lb/min"]
[null,null,null,null,null,null,null,"lb/h","lb/h","lb/h","lb/h"]
[null,null,null,null,null,null,null,"sccm","sccm","sccm","sccm"]
[null,"10A61","\"",null,null,null,null,"scfm","scfm","scfm","scfm"]
[null," 1 : 3\" Scale",null,null,null,null,null,"scfh","scfh","scfh","scfh"]
[null," 2 : 5\" Scale",null,null,null,null,null,"scfs","scfs","scfs","scfs"]
[null," 3 : 10\" Scale"]
[null,null,null,null,null,"(07) FP-1/8-08"]
[null,null,null,null,null,{"$f":"RIGHT(LEFT(F33,11),3)","v":"1/8"},null,{"$f":"RIGHT(G34,3)","v":""}]
[]
[]
[]
[]
[null,"10A4"]
[null,{"$f":"\"(66)\"","v":"(66)"},{"$f":"\"4 : \"&\"Tantalum\"","v":"4 : Tantalum"},null,"66",{"$f":"IFERROR(VLOOKUP(E41,B40:C56,2,FALSE),\"\")","v":"4 : Tantalum"}]
[null,{"$f":"\"(67)\"","v":"(67)"},{"$f":"\"4 : \"&\"Tantalum\"","v":"4 : Tantalum"},null,{"$f":"\"(\"&E40&\")\"","v":"(66)"}]
[null,{"$f":"\"(68)\"","v":"(68)"},"4 : Tantalum"]
[null,{"$f":"\"(69)\"","v":"(69)"},"4 : Tantalum"]
[null,{"$f":"\"(70)\"","v":"(70)"},"4 : Tantalum"]
[null,{"$f":"\"(71)\"","v":"(71)"},"4 : Tantalum"]
[null,{"$f":"\"(72)\"","v":"(72)"},"4 : Tantalum"]
[null,{"$f":"\"(73)\"","v":"(73)"},{"$f":"\"6 : PTFE - \"&D47","v":"6 : PTFE - 1/2\" size"},"1/2\" size"]
[null,{"$f":"\"(74)\"","v":"(74)"},{"$f":"\"5 : PVC - \"&D48","v":"5 : PVC - 1/2\" size"},"1/2\" size"]
[null,{"$f":"\"(75)\"","v":"(75)"},{"$f":"\"6 : PTFE - \"&D49","v":"6 : PTFE - 3/4\"-1\" size"},"3/4\"-1\" size"]
[null,{"$f":"\"(76)\"","v":"(76)"},{"$f":"\"5 : PVC - \"&D50","v":"5 : PVC - 3/4\"-1\" size"},"3/4\"-1\" size"]
[null,{"$f":"\"(77)\"","v":"(77)"},{"$f":"\"6 : PTFE - \"&D51","v":"6 : PTFE - 3/4\"-1\" size"},"3/4\"-1\" size"]
[null,{"$f":"\"(78)\"","v":"(78)"},{"$f":"\"5 : PVC - \"&D52","v":"5 : PVC - 3/4\"-1\" size"},"3/4\"-1\" size"]
[null,{"$f":"\"(79)\"","v":"(79)"},{"$f":"\"6 : PTFE - \"&D53","v":"6 : PTFE - 1-1/2-2\" size"},"1-1/2-2\" size"]
[null,{"$f":"\"(80)\"","v":"(80)"},{"$f":"\"5 : PVC - \"&D54","v":"5 : PVC - 1-1/2-2\" size"},"1-1/2-2\" size"]
[null,{"$f":"\"(81)\"","v":"(81)"},{"$f":"\"6 : PTFE - \"&D55","v":"6 : PTFE - 1-1/2-2\" size"},"1-1/2-2\" size"]
[null,{"$f":"\"(82)\"","v":"(82)"},{"$f":"\"5 : PVC - \"&D56","v":"5 : PVC - 1-1/2-2\" size"},"1-1/2-2\" size"]
[]
[]
[]
[null,"10A22"]
[null,"(2","2 : 1/4 in."]
[null,"(3","3 : 1/2 in."]
[null,"(4","4 : 1 in."]
[null,"(5","5 : 1-1/2 in."]
[null,"(6","6 : 2 in."]
[null,{"$f":"\"\"","v":""}]
[]
[]
[null,"1B",{"$f":"B69&\" : \"","v":"1B : "},"0.02 … 0.36 GPM Water",{"$f":"C69&D69","v":"1B : 0.02 … 0.36 GPM Water"}]
[null,"1C",{"$f":"B70&\" : \"","v":"1C : "},"0.05 … 0.60 GPM Water",{"$f":"C70&D70","v":"1C : 0.05 … 0.60 GPM Water"}]
[null,"1D","1D : ","0.1 … 1.0 GPM Water","1D : 0.1 … 1.0 GPM Water"]
[null,"1E","1E : ","0.1 … 1.3 GPM Water","1E : 0.1 … 1.3 GPM Water"]
[null,"1F","1F : ","0.2 … 2.0 GPM Water","1F : 0.2 … 2.0 GPM Water"]
[null,"1G","1G : ","0.4 … 3.0 GPM Water","1G : 0.4 … 3.0 GPM Water"]
[null,"1H","1H : ","0.6 … 4.0 GPM Water","1H : 0.6 … 4.0 GPM Water"]
[null,"1J","1J : ","0.5 … 6.0 GPM Water","1J : 0.5 … 6.0 GPM Water"]
[null,"1K","1K : ","0.5 … 8.0 GPM Water","1K : 0.5 … 8.0 GPM Water"]
[null,"1L","1L : ","1.0 … 11.0 GPM Water","1L : 1.0 … 11.0 GPM Water"]
[null,"1M","1M : ","1.0 … 15.0 GPM Water","1M : 1.0 … 15.0 GPM Water"]
[null,"1N","1N : ","2.0 … 20.0 GPM Water","1N : 2.0 … 20.0 GPM Water"]
[null,"1P","1P : ","2.0 … 24.0 GPM Water","1P : 2.0 … 24.0 GPM Water"]
[null,"1Q","1Q : ","3.0 … 35.0 GPM Water","1Q : 3.0 … 35.0 GPM Water"]
[null,"1R","1R : ","4.0 … 50.0 GPM Water","1R : 4.0 … 50.0 GPM Water"]
[null,"2B","2B : ","0.05 … 0.60 SCFM Air @ STP","2B : 0.05 … 0.60 SCFM Air @ STP"]
[null,"2C","2C : ","0.1 … 1.3 SCFM Air @ STP","2C : 0.1 … 1.3 SCFM Air @ STP"]
[null,"2D","2D : ","0.2 … 2.0 SCFM Air @ STP","2D : 0.2 … 2.0 SCFM Air @ STP"]
[null,"2E","2E : ","0.5 … 4.5 SCFM Air @ STP","2E : 0.5 … 4.5 SCFM Air @ STP"]
[null,"2F","2F : ","0.5 … 5.5 SCFM Air @ STP","2F : 0.5 … 5.5 SCFM Air @ STP"]
[null,"2G","2G : ","0.5 … 7.0 SCFM Air @ STP","2G : 0.5 … 7.0 SCFM Air @ STP"]
[null,"2H","2H : ","0.5 … 8.5 SCFM Air @ STP","2H : 0.5 … 8.5 SCFM Air @ STP"]
[null,"2J","2J : ","1.0 … 9.0 SCFM Air @ STP","2J : 1.0 … 9.0 SCFM Air @ STP"]
[null,"2K","2K : ","1.5 … 9.0 SCFM Air @ STP","2K : 1.5 … 9.0 SCFM Air @ STP"]
[null,"2L","2L : ","1.0 … 14.0 SCFM Air @ STP","2L : 1.0 … 14.0 SCFM Air @ STP"]
[null,"2M","2M : ","2.0 … 19.0 SCFM Air @ STP","2M : 2.0 … 19.0 SCFM Air @ STP"]
[null,"2N","2N : ","2.0 … 20.0 SCFM Air @ STP","2N : 2.0 … 20.0 SCFM Air @ STP"]
[null,"2P","2P : ","2.0 … 26.0 SCFM Air @ STP","2P : 2.0 … 26.0 SCFM Air @ STP"]
[null,"2Q","2Q : ","4.0 … 36.0 SCFM Air @ STP","2Q : 4.0 … 36.0 SCFM Air @ STP"]
[null,"2R","2R : ","5.0 … 50.0 SCFM Air @ STP","2R : 5.0 … 50.0 SCFM Air @ STP"]
[null,"2S","2S : ","5.0 … 60.0 SCFM Air @ STP","2S : 5.0 … 60.0 SCFM Air @ STP"]
[null,"2T","2T : ","8.0 … 80.0 SCFM Air @ STP","2T : 8.0 … 80.0 SCFM Air @ STP"]
[null,"2U","2U : ","10.0 … 110.0 SCFM Air @ STP","2U : 10.0 … 110.0 SCFM Air @ STP"]
[null,{"$f":"\"\"","v":""}]

{"sheet":"Temp-Press Limits","index":43,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":true,"merged":[[5,3,8,3],[9,3,11,3]]}
[]
[]
[]
[null,null,null,null,null,"Temp (F)","Pressure (psi)"]
[null,null,null,"10A61","10A61",150,150,"and/or"]
[null,null,null,"10A4","Universal",250]
[null,null,null,null,"1-1/2 higher",100,100]
[null,null,null,null,"1\", 3/4\"",100,200]
[null,null,null,null,"1/2\"",100,250]
[null,null,null,"10A22","1/2\" below",100,175]
[null,null,null,null,"1\", 1-1/2\"",100,100]
[null,null,null,null,"2\"",100,75]

{"sheet":"SizingSummary","index":44,"n_rows":108,"n_cols":8,"rows_kept":108,"cut":false,"hidden":true,"merged":[[0,5,0,6]]}
[null,null,null,null,null,"TOP LEFT"]
[null,"INPUTS",null,null,null,"METER DETAILS"]
[null,"Fluid Type",{"$f":"IF(RIGHT('VA Sizing'!B4,1)=\" \",\"Mixed Gas\",\nIF(RIGHT('VA Sizing'!B3,1)=\" \",\"Steam\",\n'VA Sizing'!C3))","v":0},null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,"Fluid Name",{"$f":"IF(RIGHT('VA Sizing'!B4,1)=\" \",MixedGas!A2,\n'VA Sizing'!C4)","v":0},{"$f":"IF(RIGHT('VA Sizing'!B4,1)=\" \",CONCATENATE(MixedGas!A3,E4),\"\")","v":""},"%","Details",{"$f":"'VA Sizing'!J22","v":""},{"$f":"LEFT(G4:G4,1)","v":""}]
[null,null,{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",NOT(MixedGas!B2=\"\")),MixedGas!B2,\n\"\")","v":""},{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",NOT(C5=\"\")),CONCATENATE(MixedGas!B3,E5),\"\")","v":""},"%",{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Flow Range\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J25,'10A61 Naming'!F3:L32,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J25,'10A45 Naming Standard'!K4:Q219,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J25,'10A22 Naming'!F3:H52,3,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BK26,\"\")))),\"\")","v":""}]
[null,null,{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",NOT(MixedGas!C2=\"\")),MixedGas!C2,\n\"\")","v":""},{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",NOT(C6=\"\")),CONCATENATE(MixedGas!C3,E6),\"\")","v":""},"%","Range",{"$f":"'VA Sizing'!M25","v":""},{"$f":"IF(NOT('VA Sizing'!N25=\"\"),'VA Sizing'!N25,\nIF(NOT(H15=\"\"),H15,\nIF(NOT(H24=\"\"),H24,\nIF(NOT(H33=\"\"),H33,\"\"))))","v":""}]
[null,null,{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",NOT(MixedGas!D2=\"\")),MixedGas!D2,\n\"\")","v":""},{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",NOT(C7=\"\")),CONCATENATE(MixedGas!D3,E7),\"\")","v":""},"%",{"$f":"IF(LEFT('VA Sizing'!J25,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!J25,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,{"$f":"IF('VA Sizing'!C3=\"Liquid\",\"Viscosity\",\"Ref. Condition\")","v":"Ref. Condition"},{"$f":"IF('VA Sizing'!C3=\"Liquid\",'VA Sizing'!$C$8,'VA Sizing'!C5)","v":0},{"$f":"IF(B8=\"Viscosity\",'VA Sizing'!$D$8,\"\")","v":""},null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G3=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G3=\"10A4\",OR(LEFT(G5,4)=\"(D1)\",LEFT(G5,4)=\"(D2)\",LEFT(G5,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G3=\"10A4\",OR(LEFT(G5,4)=\"(B1)\",LEFT(G5,4)=\"(B2)\",LEFT(G5,4)=\"(C1)\",LEFT(G5,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G3=\"10A4\",OR(LEFT(G5,4)=\"(A1)\",LEFT(G5,4)=\"(A2)\",LEFT(G5,4)=\"(A3)\",LEFT(G5,4)=\"(A4)\",LEFT(G5,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G3=\"10A22\",OR(LEFT(G5,3)=\"(2)\",LEFT(G5,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G3=\"10A22\",OR(LEFT(G5,3)=\"(4)\",LEFT(G5,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G3=\"10A22\",OR(LEFT(G5,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",\"\"))))))))),\"\")","v":""}]
[null,"Pressure",{"$f":"IF('VA Sizing'!C9 = \"Optional\",\"\",\nIF(RIGHT('VA Sizing'!B3,1)=\" \",Steam!C17-14.7,\n'VA Sizing'!C9))","v":0},{"$f":"IF(RIGHT('VA Sizing'!B3,1)=\" \",\"psi(g)\",\nIF('VA Sizing'!D9=\"\",\"\",\n'VA Sizing'!D9))","v":""},null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Scale Type\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J25,'10A61 Naming'!F3:L32,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J25,'10A45 Naming Standard'!K4:Q219,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J25,'10A22 Naming'!F3:H52,2,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BH26,\"\")))),\"\")","v":""}]
[null,"Temperature",{"$f":"IF('VA Sizing'!C10= \"Optional\",\"\",\nIF(RIGHT('VA Sizing'!B3,1)=\" \",Steam!B17,\n'VA Sizing'!C10))","v":0},{"$f":"IF(RIGHT('VA Sizing'!B3,1)=\" \",\"°C\",\nIF('VA Sizing'!D10=\"\",\"\",\n'VA Sizing'!D10))","v":""},null,"10A32 Damping?",{"$f":"IF(AND('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BI26=\"With Damping\"),\"Tube/Float Combination Requires Gas Damping\",\"\")","v":""}]
[null,"Oper. Density",{"$f":"IF(RIGHT('VA Sizing'!B3,1)=\" \",Steam!B20,\nIF('VA Sizing'!C3=\"Liquid\",'VA Sizing'!C11,\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Operating Conditions\"),'VA Sizing'!C11,\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Reference Conditions\"),B22,\nIF('VA Sizing'!C3=\"Gas\",ROUND('VA Sizing'!C14,5),\"\")))))","v":""},{"$f":"IF(RIGHT('VA Sizing'!B3,1)=\" \",'VA Sizing'!D14,\nIF('VA Sizing'!C3=\"Liquid\",'VA Sizing'!D11,\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Operating Conditions\"),'VA Sizing'!D11,\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Reference Conditions\"),C22,\nIF('VA Sizing'!C3=\"Gas\",'VA Sizing'!D14,\"\")))))","v":""},null,"METER DETAILS"]
[null,"Flowrate",{"$f":"'VA Sizing'!C12","v":0},{"$f":"'VA Sizing'!D12","v":0},null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"'VA Sizing'!J22","v":""}]
[null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Base Density\",\"\")","v":""},{"$f":"IF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Operating Conditions\"),B21,\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Reference Conditions\"),'VA Sizing'!C7,\nB17))","v":""},{"$f":"IF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Operating Conditions\"),C21,\nIF(AND('VA Sizing'!C3=\"Gas\",'VA Sizing'!C4=\" Other\", 'VA Sizing'!C6=\"at Reference Conditions\"),'VA Sizing'!D7,\nIF('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!D14,\"\")))","v":""},null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Flow Range\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J26,'10A61 Naming'!F3:L32,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J26,'10A45 Naming Standard'!K4:Q219,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J26,'10A22 Naming'!F3:H52,3,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BK27,\"\")))),\"\")","v":""}]
[null,null,{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Actual\",'VA Sizing'!$C$5=\"Normal\")),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\"\")))))","v":""},null,null,"Range",{"$f":"'VA Sizing'!M26","v":""},{"$f":"'VA Sizing'!N26","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!J26,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!J26,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,{"$f":"IFERROR(ROUND(B18/VLOOKUP('VA Sizing'!D14,'Modified Inputs'!$L$15:$M$20,2,FALSE),4),\"\")","v":""},"specified units",null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G12=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G12=\"10A4\",OR(LEFT(G14,4)=\"(D1)\",LEFT(G14,4)=\"(D2)\",LEFT(G14,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G12=\"10A4\",OR(LEFT(G14,4)=\"(B1)\",LEFT(G14,4)=\"(B2)\",LEFT(G14,4)=\"(C1)\",LEFT(G14,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G12=\"10A4\",OR(LEFT(G14,4)=\"(A1)\",LEFT(G14,4)=\"(A2)\",LEFT(G14,4)=\"(A3)\",LEFT(G14,4)=\"(A4)\",LEFT(G14,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G12=\"10A22\",OR(LEFT(G14,3)=\"(2)\",LEFT(G14,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G12=\"10A22\",OR(LEFT(G14,3)=\"(4)\",LEFT(G14,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G12=\"10A22\",OR(LEFT(G14,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,{"$f":"IFERROR(ROUND(C15,5),\"\")","v":""},"g/ml",null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Scale Type\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J26,'10A61 Naming'!F3:L32,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J26,'10A45 Naming Standard'!K4:Q219,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J26,'10A22 Naming'!F3:H52,2,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BH27,\"\")))),\"\")","v":""}]
[null,null,{"$f":"IF('VA Sizing'!N2=0,1,0)","v":1},null,null,"10A32 Damping?",{"$f":"IF(AND('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BI27=\"With Damping\"),\"Tube/Float Combination Requires Gas Damping\",\"\")","v":""}]
[null,null,null,null,null,"METER DETAILS"]
[null,{"$f":"IFERROR(ROUND(B18/VLOOKUP('VA Sizing'!D11,'Modified Inputs'!$L$15:$M$20,2,FALSE),4),\"\")","v":""},{"$f":"'VA Sizing'!D11","v":0},null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,{"$f":"IFERROR(ROUND('10A61 5\" Calcs'!O46/VLOOKUP(D14,'Modified Inputs'!$L$15:$M$20,2,FALSE),4),\"\")","v":""},{"$f":"'VA Sizing'!D7","v":0},null,null,"Details",{"$f":"'VA Sizing'!J22","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Flow Range\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J27,'10A61 Naming'!F3:L32,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J27,'10A45 Naming Standard'!K4:Q219,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J27,'10A22 Naming'!F3:H52,3,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BK28,\"\")))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!M27","v":""},{"$f":"'VA Sizing'!N27","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!J27,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!J27,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G21=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G21=\"10A4\",OR(LEFT(G23,4)=\"(D1)\",LEFT(G23,4)=\"(D2)\",LEFT(G23,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G21=\"10A4\",OR(LEFT(G23,4)=\"(B1)\",LEFT(G23,4)=\"(B2)\",LEFT(G23,4)=\"(C1)\",LEFT(G23,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G21=\"10A4\",OR(LEFT(G23,4)=\"(A1)\",LEFT(G23,4)=\"(A2)\",LEFT(G23,4)=\"(A3)\",LEFT(G23,4)=\"(A4)\",LEFT(G23,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G21=\"10A22\",OR(LEFT(G23,3)=\"(2)\",LEFT(G23,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G21=\"10A22\",OR(LEFT(G23,3)=\"(4)\",LEFT(G23,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G21=\"10A22\",OR(LEFT(G23,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Scale Type\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J27,'10A61 Naming'!F3:L32,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J27,'10A45 Naming Standard'!K4:Q219,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J27,'10A22 Naming'!F3:H52,2,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BH28,\"\")))),\"\")","v":""}]
[null,null,null,null,null,"10A32 Damping?",{"$f":"IF(AND('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BI28=\"With Damping\"),\"Tube/Float Combination Requires Gas Damping\",\"\")","v":""}]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"'VA Sizing'!J22","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Flow Range\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J28,'10A61 Naming'!F3:L32,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J28,'10A45 Naming Standard'!K4:Q219,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J28,'10A22 Naming'!F3:H52,3,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BK29,\"\")))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!M28","v":""},{"$f":"'VA Sizing'!N28","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!J28,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!J28,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G30=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G30=\"10A4\",OR(LEFT(G32,4)=\"(D1)\",LEFT(G32,4)=\"(D2)\",LEFT(G32,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G30=\"10A4\",OR(LEFT(G32,4)=\"(B1)\",LEFT(G32,4)=\"(B2)\",LEFT(G32,4)=\"(C1)\",LEFT(G32,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G30=\"10A4\",OR(LEFT(G32,4)=\"(A1)\",LEFT(G32,4)=\"(A2)\",LEFT(G32,4)=\"(A3)\",LEFT(G32,4)=\"(A4)\",LEFT(G32,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G30=\"10A22\",OR(LEFT(G32,3)=\"(2)\",LEFT(G32,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G30=\"10A22\",OR(LEFT(G32,3)=\"(4)\",LEFT(G32,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G30=\"10A22\",OR(LEFT(G32,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\nIF('VA Sizing'!$N$2=\"10A32\",\"Scale Type\",\"\"))))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!J28,'10A61 Naming'!F3:L32,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!J28,'10A45 Naming Standard'!K4:Q219,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!J28,'10A22 Naming'!F3:H52,2,FALSE),\nIF('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BH29,\"\")))),\"\")","v":""}]
[null,null,null,null,null,"10A32 Damping?",{"$f":"IF(AND('VA Sizing'!$N$2=\"10A32\",'10A32 Capacity'!BI29=\"With Damping\"),\"Tube/Float Combination Requires Gas Damping\",\"\")","v":""}]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"'VA Sizing'!P22","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P25,'10A61 Naming'!F33:L101,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P25,'10A45 Naming Low PSI'!K4:Q71,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P25,'10A22 Naming'!F3:H52,3,FALSE),\"\"))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!S25","v":""},{"$f":"'VA Sizing'!T25","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!P25,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!P25,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G39=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G39=\"10A4\",OR(LEFT(G41,4)=\"(D1)\",LEFT(G41,4)=\"(D2)\",LEFT(G41,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G39=\"10A4\",OR(LEFT(G41,4)=\"(B1)\",LEFT(G41,4)=\"(B2)\",LEFT(G41,4)=\"(C1)\",LEFT(G41,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G39=\"10A4\",OR(LEFT(G41,4)=\"(A1)\",LEFT(G41,4)=\"(A2)\",LEFT(G41,4)=\"(A3)\",LEFT(G41,4)=\"(A4)\",LEFT(G41,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G39=\"10A22\",OR(LEFT(G41,3)=\"(2)\",LEFT(G41,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G39=\"10A22\",OR(LEFT(G41,3)=\"(4)\",LEFT(G41,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G39=\"10A22\",OR(LEFT(G41,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P25,'10A61 Naming'!F33:L101,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P25,'10A45 Naming Low PSI'!K4:Q71,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P25,'10A22 Naming'!F3:H52,2,FALSE),\"\"))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"'VA Sizing'!P22","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P26,'10A61 Naming'!F33:L101,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P26,'10A45 Naming Low PSI'!K4:Q71,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P26,'10A22 Naming'!F3:H52,3,FALSE),\"\"))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!S26","v":""},{"$f":"'VA Sizing'!T26","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!P26,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!P26,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G48=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G48=\"10A4\",OR(LEFT(G50,4)=\"(D1)\",LEFT(G50,4)=\"(D2)\",LEFT(G50,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G48=\"10A4\",OR(LEFT(G50,4)=\"(B1)\",LEFT(G50,4)=\"(B2)\",LEFT(G50,4)=\"(C1)\",LEFT(G50,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G48=\"10A4\",OR(LEFT(G50,4)=\"(A1)\",LEFT(G50,4)=\"(A2)\",LEFT(G50,4)=\"(A3)\",LEFT(G50,4)=\"(A4)\",LEFT(G50,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G48=\"10A22\",OR(LEFT(G50,3)=\"(2)\",LEFT(G50,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G48=\"10A22\",OR(LEFT(G50,3)=\"(4)\",LEFT(G50,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G48=\"10A22\",OR(LEFT(G50,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P26,'10A61 Naming'!F33:L101,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P26,'10A45 Naming Low PSI'!K4:Q71,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P26,'10A22 Naming'!F3:H52,2,FALSE),\"\"))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"'VA Sizing'!P22","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P27,'10A61 Naming'!F33:L101,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P27,'10A45 Naming Low PSI'!K4:Q71,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P27,'10A22 Naming'!F3:H52,3,FALSE),\"\"))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!S27","v":""},{"$f":"'VA Sizing'!T27","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!P27,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!P27,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G57=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G57=\"10A4\",OR(LEFT(G59,4)=\"(D1)\",LEFT(G59,4)=\"(D2)\",LEFT(G59,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G57=\"10A4\",OR(LEFT(G59,4)=\"(B1)\",LEFT(G59,4)=\"(B2)\",LEFT(G59,4)=\"(C1)\",LEFT(G59,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G57=\"10A4\",OR(LEFT(G59,4)=\"(A1)\",LEFT(G59,4)=\"(A2)\",LEFT(G59,4)=\"(A3)\",LEFT(G59,4)=\"(A4)\",LEFT(G59,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G57=\"10A22\",OR(LEFT(G59,3)=\"(2)\",LEFT(G59,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G57=\"10A22\",OR(LEFT(G59,3)=\"(4)\",LEFT(G59,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G57=\"10A22\",OR(LEFT(G59,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P27,'10A61 Naming'!F33:L101,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P27,'10A45 Naming Low PSI'!K4:Q71,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P27,'10A22 Naming'!F3:H52,2,FALSE),\"\"))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"'VA Sizing'!P22","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P28,'10A61 Naming'!F33:L101,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P28,'10A45 Naming Low PSI'!K4:Q71,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P28,'10A22 Naming'!F3:H52,3,FALSE),\"\"))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!S28","v":""},{"$f":"'VA Sizing'!T28","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!P28,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!P28,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G66=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G66=\"10A4\",OR(LEFT(G68,4)=\"(D1)\",LEFT(G68,4)=\"(D2)\",LEFT(G68,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G66=\"10A4\",OR(LEFT(G68,4)=\"(B1)\",LEFT(G68,4)=\"(B2)\",LEFT(G68,4)=\"(C1)\",LEFT(G68,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G66=\"10A4\",OR(LEFT(G68,4)=\"(A1)\",LEFT(G68,4)=\"(A2)\",LEFT(G68,4)=\"(A3)\",LEFT(G68,4)=\"(A4)\",LEFT(G68,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G66=\"10A22\",OR(LEFT(G68,3)=\"(2)\",LEFT(G68,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G66=\"10A22\",OR(LEFT(G68,3)=\"(4)\",LEFT(G68,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G66=\"10A22\",OR(LEFT(G68,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!P28,'10A61 Naming'!F33:L101,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A4\",VLOOKUP('VA Sizing'!P28,'10A45 Naming Low PSI'!K4:Q71,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",VLOOKUP('VA Sizing'!P28,'10A22 Naming'!F3:H52,2,FALSE),\"\"))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"IF(AND('VA Sizing'!N2=\"10A4\",'VA Sizing'!V22=\"Additional Floats\"),'VA Sizing'!V23,'VA Sizing'!V22)","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V25,'10A61 Naming'!F102:L131,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming Alarm'!K4:Q203,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming TA'!K4:Q63,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming PTFE'!K4:Q43,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming PVC'!K4:Q51,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!Y25","v":""},{"$f":"'VA Sizing'!Z25","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!V25,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!V25,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G75=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G75=\"10A4\",OR(LEFT(G77,4)=\"(D1)\",LEFT(G77,4)=\"(D2)\",LEFT(G77,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G75=\"10A4\",OR(LEFT(G77,4)=\"(B1)\",LEFT(G77,4)=\"(B2)\",LEFT(G77,4)=\"(C1)\",LEFT(G77,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G75=\"10A4\",OR(LEFT(G77,4)=\"(A1)\",LEFT(G77,4)=\"(A2)\",LEFT(G77,4)=\"(A3)\",LEFT(G77,4)=\"(A4)\",LEFT(G77,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G75=\"10A22\",OR(LEFT(G77,3)=\"(2)\",LEFT(G77,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G75=\"10A22\",OR(LEFT(G77,3)=\"(4)\",LEFT(G77,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G75=\"10A22\",OR(LEFT(G77,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V25,'10A61 Naming'!F102:L131,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming Alarm'!K4:Q203,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming TA'!K4:Q63,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming PTFE'!K4:Q43,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V25,'10A45 Naming PVC'!K4:Q51,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"IF(AND('VA Sizing'!N2=\"10A4\",'VA Sizing'!V22=\"Additional Floats\"),'VA Sizing'!V23,'VA Sizing'!V22)","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V26,'10A61 Naming'!F102:L131,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming Alarm'!K4:Q203,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming TA'!K4:Q63,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming PTFE'!K4:Q43,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming PVC'!K4:Q51,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!Y26","v":""},{"$f":"'VA Sizing'!Z26","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!V26,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!V26,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G84=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G84=\"10A4\",OR(LEFT(G86,4)=\"(D1)\",LEFT(G86,4)=\"(D2)\",LEFT(G86,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G84=\"10A4\",OR(LEFT(G86,4)=\"(B1)\",LEFT(G86,4)=\"(B2)\",LEFT(G86,4)=\"(C1)\",LEFT(G86,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G84=\"10A4\",OR(LEFT(G86,4)=\"(A1)\",LEFT(G86,4)=\"(A2)\",LEFT(G86,4)=\"(A3)\",LEFT(G86,4)=\"(A4)\",LEFT(G86,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G84=\"10A22\",OR(LEFT(G86,3)=\"(2)\",LEFT(G86,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G84=\"10A22\",OR(LEFT(G86,3)=\"(4)\",LEFT(G86,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G84=\"10A22\",OR(LEFT(G86,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V26,'10A61 Naming'!F102:L131,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming Alarm'!K4:Q203,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming TA'!K4:Q63,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming PTFE'!K4:Q43,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V26,'10A45 Naming PVC'!K4:Q51,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"IF(AND('VA Sizing'!N2=\"10A4\",'VA Sizing'!V22=\"Additional Floats\"),'VA Sizing'!V23,'VA Sizing'!V22)","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V27,'10A61 Naming'!F102:L131,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming Alarm'!K4:Q203,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming TA'!K4:Q63,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming PTFE'!K4:Q43,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming PVC'!K4:Q51,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!Y27","v":""},{"$f":"'VA Sizing'!Z27","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!V27,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!V27,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G93=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G93=\"10A4\",OR(LEFT(G95,4)=\"(D1)\",LEFT(G95,4)=\"(D2)\",LEFT(G95,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G93=\"10A4\",OR(LEFT(G95,4)=\"(B1)\",LEFT(G95,4)=\"(B2)\",LEFT(G95,4)=\"(C1)\",LEFT(G95,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G93=\"10A4\",OR(LEFT(G95,4)=\"(A1)\",LEFT(G95,4)=\"(A2)\",LEFT(G95,4)=\"(A3)\",LEFT(G95,4)=\"(A4)\",LEFT(G95,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G93=\"10A22\",OR(LEFT(G95,3)=\"(2)\",LEFT(G95,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G93=\"10A22\",OR(LEFT(G95,3)=\"(4)\",LEFT(G95,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 00 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G93=\"10A22\",OR(LEFT(G95,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V27,'10A61 Naming'!F102:L131,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming Alarm'!K4:Q203,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming TA'!K4:Q63,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming PTFE'!K4:Q43,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V27,'10A45 Naming PVC'!K4:Q51,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[]
[null,null,null,null,null,"METER DETAILS"]
[null,null,null,null,null,"Meter Name",{"$f":"'VA Sizing'!$N$2","v":0}]
[null,null,null,null,null,"Details",{"$f":"IF(AND('VA Sizing'!N2=\"10A4\",'VA Sizing'!V22=\"Additional Floats\"),'VA Sizing'!V23,'VA Sizing'!V22)","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Tube Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Meter Size\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V28,'10A61 Naming'!F102:L131,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming Alarm'!K4:Q203,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming TA'!K4:Q63,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming PTFE'!K4:Q43,6,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming PVC'!K4:Q51,6,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]
[null,null,null,null,null,"Range",{"$f":"'VA Sizing'!Y28","v":""},{"$f":"'VA Sizing'!Z28","v":""}]
[null,null,null,null,null,{"$f":"IF(LEFT('VA Sizing'!V28,1)=\" \",\"Combination may require a viscosity calibration\",\nIF(RIGHT('VA Sizing'!V28,1)=\" \",\"Combination requires a greater operating pressure\",\"\"))","v":""}]
[null,null,null,null,null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$K$2=\"Optional\",'Modified Inputs'!$I$2=\"Optional\"),\"\",IF(AND(G102=\"10A61\",OR('Modified Inputs'!$K$2>150,'Modified Inputs'!$I$2>165)),\"Pressure and/or Temperature limits exceeded 150 Degrees F and 150 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G102=\"10A4\",OR(LEFT(G104,4)=\"(D1)\",LEFT(G104,4)=\"(D2)\",LEFT(G104,4)=\"(E1)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G102=\"10A4\",OR(LEFT(G104,4)=\"(B1)\",LEFT(G104,4)=\"(B2)\",LEFT(G104,4)=\"(C1)\",LEFT(G104,4)=\"(C2)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>215)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 200 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G102=\"10A4\",OR(LEFT(G104,4)=\"(A1)\",LEFT(G104,4)=\"(A2)\",LEFT(G104,4)=\"(A3)\",LEFT(G104,4)=\"(A4)\",LEFT(G104,4)=\"(A6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>265)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 250 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G102=\"10A22\",OR(LEFT(G104,3)=\"(2)\",LEFT(G104,3)=\"(3)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>190)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 175 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G102=\"10A22\",OR(LEFT(G104,3)=\"(4)\",LEFT(G104,3)=\"(5)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>115)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 100 psig                                                      Please refer to datasheet or contact ABB for more information\",\nIF(AND(G102=\"10A22\",OR(LEFT(G104,3)=\"(6)\"),OR('Modified Inputs'!$K$2>100,'Modified Inputs'!$I$2>90)),\"Pressure and/or Temperature limits exceeded 100 Degrees F and 75 psig                                                      Please refer to datasheet or contact ABB for more information\",\"\")))))))),\"\")","v":""}]
[null,null,null,null,null,{"$f":"IF('VA Sizing'!$N$2=\"10A61\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A4\",\"Float Code\",\nIF('VA Sizing'!$N$2=\"10A22\",\"Application\",\"\")))","v":""},{"$f":"IFERROR(IF('VA Sizing'!$N$2=\"10A61\",VLOOKUP('VA Sizing'!V28,'10A61 Naming'!F102:L131,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Alarm Floats\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming Alarm'!K4:Q203,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Tantalum Floats (TA)\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming TA'!K4:Q63,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"Teflon Floats (PTFE)\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming PTFE'!K4:Q43,7,FALSE),\nIF(AND('VA Sizing'!$N$2=\"10A4\",'VA Sizing'!V23=\"PVC Floats\"),VLOOKUP('VA Sizing'!V28,'10A45 Naming PVC'!K4:Q51,7,FALSE),\nIF('VA Sizing'!$N$2=\"10A22\",\"\",\"\")))))),\"\")","v":""}]

{"sheet":"Steam","index":45,"n_rows":70,"n_cols":18,"rows_kept":70,"cut":false,"hidden":true,"merged":[[14,1,14,2],[22,1,22,4]]}
[]
[null,"Input Temperature","Temperature Units","Input Pressure","Pressure Units"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temp","Pressure","Density","Viscosity"]
[null,"Modified Temp. C","Modified Pressure psia",null,null,null,null,null,null,null,null,null,null,null,"°C","psi","g/ml","cP"]
[null,{"$f":"IF(C3=\"⁰C\",B3,\nIF(C3=\"⁰F\",(B3-32)*(5/9),0))","v":0},{"$f":"IF(E3=\"psi(a)\",D3,\nIF(E3=\"psi(g)\",D3+14.7,\nIF(E3=\"bar(a)\",D3*14.5,\nIF(E3=\"bar(g)\",D3*14.5+14.7,\nIF(E3=\"atm(a)\",D3*14.7,\nIF(E3=\"atm(g)\",D3*14.7+14.7,0))))))","v":0},"⁰C","All Cells Empty (1)",null,null,null,null,null,null,null,null,null,100,14.709723534,5.9815767436296205E-4,1.2269000000000002E-2]
[null,null,null,"psi(a)",{"$f":"IF(AND(B3=\"\",C3=\"\",D3=\"\",E3=\"\"),1,\nIF(AND(NOT(D3=\"\"),E3=\"\"),1,\nIF(AND(NOT(E3=\"\"),D3=\"\"),1,\nIF(AND(NOT(B3=\"\"),C3=\"\"),1,\nIF(AND(NOT(C3=\"\"),B3=\"\"),1,0)))))","v":1},null,null,null,null,null,null,null,null,null,110,20.795505426000002,8.2692466716282145E-4,1.2611799999999999E-2]
[null,"Temp no pressure",null,null,null,null,null,null,null,null,null,null,null,null,120,28.814639859000003,1.1220825852782765E-3,1.2956000000000002E-2]
[null,"Input Temp","Calculated Pressure",null,"<14.7",null,null,null,null,null,null,null,null,null,130,39.200789556000004,1.497005988023952E-3,1.33013E-2]
[null,{"$f":"B5","v":0},{"$f":"H19*(B9)^4+I19*(B9)^3+J19*(B9)^2+K19*B9+L19","v":127.27195849156237},{"$f":"IF(NOT(B9=0),\"Filled\",\"Empty\")","v":"Empty"},{"$f":"IF(C17<14.7,1,0)","v":1},null,null,null,null,null,null,null,null,null,140,52.436930057999994,1.9667617268167964E-3,1.3646700000000001E-2]
[null,null,null,null,">3052",null,null,null,null,null,null,null,null,null,150,69.061151232,2.5480952987641738E-3,1.39919E-2]
[null,"Pressure no temp",null,null,{"$f":"IF(C17>3052,1,0)","v":0},null,null,null,null,null,null,null,null,null,160,89.662306139999998,3.2596649064476173E-3,1.4336800000000002E-2]
[null,"Calculated Temp","Input Pressure",null,null,null,null,null,null,null,null,null,null,null,170,114.89886594000001,4.1221814584278E-3,1.4681000000000001E-2]
[null,{"$f":"53.381*(C13^0.2424)","v":0},{"$f":"C5","v":0},{"$f":"IF(NOT(B13=0),\"Filled\",\"Empty\")","v":"Empty"},"<100",null,null,null,null,null,null,null,null,null,180,145.44380555999999,5.1588939331407343E-3,1.5025500000000002E-2]
[null,null,null,null,{"$f":"IF(B17<100,1,0)","v":1},null,null,null,null,null,null,null,null,null,190,182.05132104,6.3954975697109234E-3,1.5369799999999999E-2]
[null,"Final Pressure and Temp",null,null,null,null,null,null,null,null,null,null,null,null,200,225.51911973,7.8610172156277029E-3,1.5714800000000001E-2]
[null,"Temp C","Pressure psia",null,">370",null,null,null,null,null,null,null,null,null,210,276.68842029000001,9.5886470419023883E-3,1.6061400000000003E-2]
[null,{"$f":"IF(B9=0,B13,B9)","v":0},{"$f":"IF(B9=0,C13,C9)","v":0},null,{"$f":"IF(B17>370,1,0)","v":0},null,null,null,null,null,null,null,null,null,220,336.42944891999997,1.1615750958299455E-2,1.6410800000000003E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,230,405.68495066999998,1.3986013986013988E-2,1.67647E-2]
[null,"Operating Density g/ml","Operating Viscosity cP",null,"above error",null,null,{"$f":"LINEST(P5:P32,O5:O32^{1,2,3,4})","v":2.9579781942811233E-7},-9.6500714422309249E-5,2.4283267979178725E-2,-2.8645503880300134,127.27195849156237,null,null,240,485.42667813000003,1.6747613465081225E-2,1.7124999999999998E-2]
[null,{"$f":"IF(B17<260.00001,H49*(B17)^6+I49*(B17)^5+J49*(B17)^4+K49*(B17)^3+L49*(B17)^2+M49*B17+N49,H51*(B17)^6+I51*(B17)^5+J51*(B17)^4+K51*(B17)^3+L51*(B17)^2+M51*B17+N51)","v":3.2143294258594572E-3},{"$f":"IF(B17<260.0001,H70*(B20)^6+I70*(B20)^5+J70*(B20)^4+K70*(B20)^3+L70*(B20)^2+M70*B20+N70,0.0648*B20+0.0165)","v":1.4348852412725139E-2},null,{"$f":"IF(OR(E9=1,E11=1,E14=1,E17=1),1,0)","v":1},null,null,null,null,null,null,null,null,null,250,576.69890273999999,1.9968051118210862E-2,1.7495E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,260,680.56039971000007,2.3713540431586438E-2,1.7877000000000001E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,798.14246309999999,2.8074115665356541E-2,1.8277000000000002E-2]
[null,"Final Inputs",null,null,null,null,null,null,null,null,null,null,null,null,280,930.64890581999998,3.316749585406302E-2,1.8670000000000003E-2]
[null,"Temp","Units","Pressure","Units",null,null,null,null,null,null,null,null,null,290,1079.34155586,3.9123630672926443E-2,1.9154100000000004E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,1245.56926383,4.6168051708217916E-2,1.9651200000000004E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,310,1430.8114142700001,5.452562704471102E-2,2.0207000000000006E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,320,1636.6054068000001,6.464124111182934E-2,2.0846000000000003E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,1864.8947466000002,7.7041602465331288E-2,2.16054E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,340,2117.6954577000001,9.27643784786642E-2,2.2553000000000004E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,2397.3281433000002,0.11363636363636363,2.3821000000000002E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,2707.2737081999999,0.14388489208633096,2.5729000000000005E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,370,3052.1733588000002,0.20202020202020199,2.9700000000000004E-2]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,{"$f":"LINEST(Q5:Q21,O5:O21^{1,2,3,4,5,6})","v":2.8751233223996836E-16},-2.52406365640718E-13,1.0035540238038779E-10,-1.9504556642020205E-8,2.2152549244248422E-6,-1.3062956929503733E-4,3.2143294258594572E-3]
[]
[null,null,null,null,null,null,null,{"$f":"LINEST(Q21:Q32,O21:O32^{1,2,3,4,5,6})","v":1.1838634494303623E-12},-2.1706288468493398E-9,1.655182620264217E-6,-6.717925072005081E-4,0.15305380480574574,-18.557560539085618,935.48176204632114]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,{"$f":"LINEST(R5:R21,Q5:Q21^{1,2,3,4,5,6})","v":-937108391.31712174},73391534.461281061,-2262590.6326697329,35157.164949576254,-297.53466817093198,1.5449001368027202,1.1506940502944308E-2]

{"sheet":"MixedGas","index":46,"n_rows":15,"n_cols":12,"rows_kept":15,"cut":false,"hidden":true,"merged":[[1,5,1,6],[4,5,4,8],[6,5,6,8],[8,5,8,8],[12,0,12,1],[12,2,12,3]]}
["Gas 1","Gas 2","Gas 3","Gas 4"]
[null,null,null,null,null,"100% Test"]
[null,null,null,null,{"$f":"SUM(A3:D3)","v":0},{"$f":"IF(AND(NOT(A3=\"\"),NOT(E3=100)),1,0)","v":0},{"$f":"IF(OR(F3=1,F4=1),1,0)","v":0},"Vol%"]
[null,null,null,null,{"$f":"SUM(A4:D4)","v":0},{"$f":"IF(AND(NOT(A4=\"\"),NOT(E4=100)),1,0)","v":0},null,"Mass%"]
[{"$f":"SUM(VLOOKUP(A2,'10A61 5\" Calcs'!J3:L30,2,FALSE),VLOOKUP(B2,'10A61 5\" Calcs'!J3:L30,2,FALSE),VLOOKUP(C2,'10A61 5\" Calcs'!J3:L30,2,FALSE),VLOOKUP(D2,'10A61 5\" Calcs'!J3:L30,2,FALSE))","v":0},{"$f":"SUM(VLOOKUP(A2,'10A61 5\" Calcs'!J3:L30,3,FALSE),VLOOKUP(B2,'10A61 5\" Calcs'!J3:L30,3,FALSE),VLOOKUP(C2,'10A61 5\" Calcs'!J3:L30,3,FALSE),VLOOKUP(D2,'10A61 5\" Calcs'!J3:L30,3,FALSE))","v":0},null,null,null,"Gas but no Composition"]
["std sum above","normal sum above",null,null,null,{"$f":"IF(OR(AND(NOT(A2=\"\"),A3=\"\",A4=\"\")),1,0)","v":0},{"$f":"IF(OR(AND(NOT(B2=\"\"),B3=\"\",B4=\"\")),1,0)","v":0},{"$f":"IF(OR(AND(NOT(C2=\"\"),C3=\"\",C4=\"\")),1,0)","v":0},{"$f":"IF(OR(AND(NOT(D2=\"\"),D3=\"\",D4=\"\")),1,0)","v":0},{"$f":"IF(G3=1,0,\nIF(OR(F6=1,G6=1,H6=1,I6=1),1,0))","v":0}]
["std","std","std","std",null,"Volume and mass filled"]
[{"$f":"((A3*A5)/VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE))","v":0},{"$f":"(B3*A5)/VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},{"$f":"(C3*A5)/VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},{"$f":"(D3*A5)/VLOOKUP(D2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},null,{"$f":"IF(AND(NOT(A3=\"\"),NOT(A4=\"\")),1,0)","v":0},{"$f":"IF(AND(NOT(B3=\"\"),NOT(B4=\"\")),1,0)","v":0},0,0,{"$f":"IF(OR(F8=1,G8=1,H8=1,I8=1),1,0)","v":0},null,{"$f":"IF(OR(J6=1,J8=1,J10=1,F12=1),1,0)","v":1}]
[{"$f":"A8/SUM($A$8:$D$8)","v":{"$error":"#DIV/0!"}},{"$f":"B8/SUM($A$8:$D$8)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,"Composition but no gas",null,null,null,null,null,{"$f":"IF(AND(G3=0,J6=0,J8=0,J10=0,F12=0),0,1)","v":1}]
["normal","normal","normal","normal",null,{"$f":"IF(AND(OR(NOT(A3=\"\"),NOT(A4=\"\")),A2=\"\"),1,0)","v":0},{"$f":"IF(AND(OR(NOT(B3=\"\"),NOT(B4=\"\")),B2=\"\"),1,0)","v":0},0,0,{"$f":"IF(OR(F10=1,G10=1,H10=1,I10=1),1,0)","v":0}]
[{"$f":"(A3*B5)/VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},{"$f":"(B3*B5)/VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},{"$f":"(C3*B5)/VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},{"$f":"(D3*B5)/VLOOKUP(D2,'10A61 5\" Calcs'!$J$3:$O$30,6,FALSE)","v":0},null,"All Blank"]
[{"$f":"A11/SUM($A$11:$D$11)","v":{"$error":"#DIV/0!"}},{"$f":"B11/SUM($A$11:$D$11)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,{"$f":"IF(OR(AND(A2=\"\",A3=\"\",A4=\"\",B2=\"\",B3=\"\",B4=\"\",C2=\"\",C3=\"\",C4=\"\",D2=\"\",D3=\"\",D4=\"\"),E2=\"\"),1,0)","v":1}]
["STANDARD",null,"NORMAL/ACTUAL"]
["Density (Volume)","Density (Mass)","Density (Volume)","Density (Mass)","Viscosity","Coefficient"]
[{"$f":"IF(AND(NOT(A2=\"\"),NOT(B2=\"\"),NOT(C2=\"\"),NOT(D2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(MixedGas!A3/MixedGas!E3)+VLOOKUP(B2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(B3/MixedGas!E3)+VLOOKUP(C2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(C3/MixedGas!E3)+VLOOKUP(D2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(D3/MixedGas!E3),\nIF(AND(NOT(A2=\"\"),NOT(B2=\"\"),NOT(C2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(MixedGas!A3/MixedGas!E3)+VLOOKUP(B2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(B3/MixedGas!E3)+VLOOKUP(C2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(C3/MixedGas!E3),\nIF(AND(NOT(A2=\"\"),NOT(B2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(MixedGas!A3/MixedGas!E3)+VLOOKUP(B2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(B3/MixedGas!E3),\nIF(AND(NOT(A2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:K29,2,FALSE)*(MixedGas!A3/MixedGas!E3),\"\"))))","v":""},{"$f":"VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$L$30,2,FALSE)*MixedGas!A9+VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$L$30,2,FALSE)*MixedGas!B9+VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$L$30,2,FALSE)*MixedGas!C9+VLOOKUP(D2,'10A61 5\" Calcs'!$J$3:$L$30,2,FALSE)*MixedGas!D9","v":{"$error":"#DIV/0!"}},{"$f":"IF(AND(NOT(A2=\"\"),NOT(B2=\"\"),NOT(C2=\"\"),NOT(D2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(MixedGas!A3/MixedGas!E3)+VLOOKUP(B2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(B3/MixedGas!E3)+VLOOKUP(C2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(C3/MixedGas!E3)+VLOOKUP(D2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(D3/MixedGas!E3),\nIF(AND(NOT(A2=\"\"),NOT(B2=\"\"),NOT(C2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(MixedGas!A3/MixedGas!E3)+VLOOKUP(B2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(B3/MixedGas!E3)+VLOOKUP(C2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(C3/MixedGas!E3),\nIF(AND(NOT(A2=\"\"),NOT(B2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(MixedGas!A3/MixedGas!E3)+VLOOKUP(B2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(B3/MixedGas!E3),\nIF(AND(NOT(A2=\"\")),VLOOKUP(A2,'10A61 5\" Calcs'!J3:L29,3,FALSE)*(MixedGas!A3/MixedGas!E3),\"\"))))","v":""},{"$f":"VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$L$30,3,FALSE)*MixedGas!A12+VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$L$30,3,FALSE)*MixedGas!B12+VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$L$30,3,FALSE)*MixedGas!C12+VLOOKUP(D2,'10A61 5\" Calcs'!$J$3:$L$30,3,FALSE)*MixedGas!D12","v":{"$error":"#DIV/0!"}},{"$f":"EXP((A3/100)*LN(VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$M$30,4,FALSE))+(B3/100)*LN(VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$M$30,4,FALSE))+(C3/100)*LN(VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$M$30,4,FALSE))+(D3/100)*LN(VLOOKUP(D2,'10A61 5\" Calcs'!$J$3:$M$30,4,FALSE)))","v":1},{"$f":"IF(AND(NOT(A2=\"\"),NOT(B2=\"\"),NOT(C2=\"\"),NOT(D2=\"\")),AVERAGE(VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE),VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE),VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE),VLOOKUP(D2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE)),\nIF(AND(NOT(A2=\"\"),NOT(B2=\"\"),NOT(C2=\"\")),AVERAGE(VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE),VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE),VLOOKUP(C2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE)),\nIF(AND(NOT(A2=\"\"),NOT(B2=\"\")),AVERAGE(VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE),VLOOKUP(B2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE)),\nIF(AND(NOT(A2=\"\")),AVERAGE(VLOOKUP(A2,'10A61 5\" Calcs'!$J$3:$N$30,5,FALSE))))))","v":false}]

{"sheet":"10A4 Standard Floats Results","index":47,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"'Modified Inputs'!$O$2*'Modified Inputs'!$J$23*SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A4 Capacity Tables'!$C$26:$F$79,3,FALSE),\"                                                                                                  \",VLOOKUP(D5,'10A4 Capacity Tables'!$C$26:$F$79,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$C$26:$C$79<'10A4 Standard Floats Results'!$B$5,'10A4 Capacity Tables'!$C$26:$C$79))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A4 Capacity Tables'!$C$26:$F$79,3,FALSE),\"                                                                                                  \",VLOOKUP(D6,'10A4 Capacity Tables'!$C$26:$F$79,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$26:$C$79>'10A4 Standard Floats Results'!$B$5,'10A4 Capacity Tables'!$C$26:$C$79))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A4 Capacity Tables'!$C$26:$F$79,3,FALSE),\"                                                                                                  \",VLOOKUP(D7,'10A4 Capacity Tables'!$C$26:$F$79,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$26:$C$79>D6,'10A4 Capacity Tables'!$C$26:$C$79))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A4 Capacity Tables'!$C$26:$F$79,3,FALSE),\"                                                                                                  \",VLOOKUP(D8,'10A4 Capacity Tables'!$C$26:$F$79,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$26:$C$79>D7,'10A4 Capacity Tables'!$C$26:$C$79))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
["T0","P0","Standard Density","Density/ Reference Density","Qa Standard","Tube/Float","Max Flow SCFM","Min Flow Specified Units","Max Flow Specified Units","Min Flow CFM","Max Rounded","Min Rounded","Concatenated"]
[{"$f":"'Modified Inputs'!$K$2+459.67","v":459.67},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N37,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Normal\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!O46,\"\"))))))","v":""},{"$f":"C12/0.0012","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$5=\"Actual\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((B12*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(A12*'10A4 Standard Floats Results'!$B$12))+0.00000000001,\nIF('VA Sizing'!$C$5=\"Normal\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12))+0.00000000001,\n'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12))+0.00000000001))","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(G12,'10A4 Capacity Tables'!$D$26:$E$75,2,FALSE),\"                                                                                                  \",VLOOKUP(G12,'10A4 Capacity Tables'!$D$26:$F$75,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$D$26:$D$75<'10A4 Standard Floats Results'!$E$12,'10A4 Capacity Tables'!$D$26:$D$75))","v":{"$error":"#N/A"}},{"$f":"G12/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I12/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I12<0.99999,ROUND(I12,2),\nIF(I12<9.999,ROUND(I12,2),\nIF(I12<99.99,ROUND(I12,1),\nIF(I12<999.99,ROUND(I12,0),\nIF(I12<9999.99,ROUND(I12,-1),\nIF(I12<99999,ROUND(I12,-2),ROUND(I12,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J12,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L12,\" \",\"-\",\" \",K12)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G13,'10A4 Capacity Tables'!$D$26:$E$75,2,FALSE),\"                                                                                                  \",VLOOKUP(G13,'10A4 Capacity Tables'!$D$26:$F$75,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$26:$D$75>'10A4 Standard Floats Results'!$E$12,'10A4 Capacity Tables'!$D$26:$D$75))","v":{"$error":"#N/A"}},{"$f":"G13/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I13/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I13<0.99999,ROUND(I13,2),\nIF(I13<9.999,ROUND(I13,2),\nIF(I13<99.99,ROUND(I13,1),\nIF(I13<999.99,ROUND(I13,0),\nIF(I13<9999.99,ROUND(I13,-1),\nIF(I13<99999,ROUND(I13,-2),ROUND(I13,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J13,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L13,\" \",\"-\",\" \",K13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G14,'10A4 Capacity Tables'!$D$26:$E$75,2,FALSE),\"                                                                                                  \",VLOOKUP(G14,'10A4 Capacity Tables'!$D$26:$F$75,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$26:$D$75>'10A4 Standard Floats Results'!$G$13,'10A4 Capacity Tables'!$D$26:$D$75))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G15,'10A4 Capacity Tables'!$D$26:$E$75,2,FALSE),\"                                                                                                  \",VLOOKUP(G15,'10A4 Capacity Tables'!$D$26:$F$75,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$26:$D$75>'10A4 Standard Floats Results'!$G$14,'10A4 Capacity Tables'!$D$26:$D$75))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(530*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A4 Standard Floats Results'!$D$12*'10A4 Standard Floats Results'!$A$12)/(492*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT(('10A4 Standard Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Standard Floats Results'!$A$12)/('10A4 Standard Floats Results'!$A$12*'10A4 Standard Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K12,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Standard Floats Results'!D5,'10A4 Capacity Tables'!$C$26:$G$80,5,FALSE)),CONCATENATE(\" \",'10A4 Standard Floats Results'!C5),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!C5,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Standard Floats Results'!G12,'10A4 Capacity Tables'!$D$26:$H$75,5,FALSE)),CONCATENATE('10A4 Standard Floats Results'!F12,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!F12,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!M12,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K13,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Standard Floats Results'!D6,'10A4 Capacity Tables'!$C$26:$G$80,5,FALSE)),CONCATENATE(\" \",'10A4 Standard Floats Results'!C6),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!C6,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Standard Floats Results'!G13,'10A4 Capacity Tables'!$D$26:$H$75,5,FALSE)),CONCATENATE('10A4 Standard Floats Results'!F13,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!F13,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!M13,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K14,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Standard Floats Results'!D7,'10A4 Capacity Tables'!$C$26:$G$80,5,FALSE)),CONCATENATE(\" \",'10A4 Standard Floats Results'!C7),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!C7,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Standard Floats Results'!G14,'10A4 Capacity Tables'!$D$26:$H$75,5,FALSE)),CONCATENATE('10A4 Standard Floats Results'!F14,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!F14,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!M14,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K15,\"\"))","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Standard Floats Results'!D8,'10A4 Capacity Tables'!$C$26:$G$80,5,FALSE)),CONCATENATE(\" \",'10A4 Standard Floats Results'!C8),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!C8,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Standard Floats Results'!G15,'10A4 Capacity Tables'!$D$26:$H$75,5,FALSE)),CONCATENATE('10A4 Standard Floats Results'!F15,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!F15,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K12,\"\"))","v":""},{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!F5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!I12,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K13,\"\"))","v":""},{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!F6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!I13,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K14,\"\"))","v":""},{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!F7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!I14,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!H8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!K15,\"\"))","v":""},{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Standard Floats Results'!F8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Standard Floats Results'!I15,\"\"))","v":""}]

{"sheet":"10A22 Standard Results","index":48,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"('Modified Inputs'!$O$2*'Modified Inputs'!$J$23*'Modified Inputs'!M2*2.73819)/(SQRT((8.4977-'Modified Inputs'!M2)*'Modified Inputs'!M2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A22 Capacity Table'!$C$6:$E$19,2,FALSE),\"-\",VLOOKUP(D5,'10A22 Capacity Table'!$C$6:$E$19,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A22 Capacity Table'!$C$6:$C$19<'10A22 Standard Results'!$B$5,'10A22 Capacity Table'!$C$6:$C$19))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A22 Capacity Table'!$C$6:$E$19,2,FALSE),\"-\",VLOOKUP(D6,'10A22 Capacity Table'!$C$6:$E$19,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$6:$C$19>'10A22 Standard Results'!$B$5,'10A22 Capacity Table'!$C$6:$C$19))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A22 Capacity Table'!$C$6:$E$19,2,FALSE),\"-\",VLOOKUP(D7,'10A22 Capacity Table'!$C$6:$E$19,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$6:$C$19>D6,'10A22 Capacity Table'!$C$6:$C$19))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A22 Capacity Table'!$C$6:$E$19,2,FALSE),\"-\",VLOOKUP(D8,'10A22 Capacity Table'!$C$6:$E$19,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$6:$C$19>D7,'10A22 Capacity Table'!$C$6:$C$19))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
["T0","P0","Standard Density","Density/ Reference Density","Qa Standard","Tube/Float","Max Flow SCFM","Min Flow Specified Units","Max Flow Specified Units","Min Flow CFM","Max Rounded","Min Rounded","Concatenated"]
[{"$f":"'Modified Inputs'!$K$2+459.67","v":459.67},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N37,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Normal\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!O46,\"\"))))))","v":""},{"$f":"C12/0.0012","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$5=\"Actual\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((B12*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(A12*'10A22 Standard Results'!$B$12))+0.00000000001,\nIF('VA Sizing'!$C$5=\"Normal\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12))+0.00000000001,\n'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12))+0.00000000001))","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(G12,'10A22 Capacity Table'!$C$44:$E$57,2,FALSE),\"-\",VLOOKUP(G12,'10A22 Capacity Table'!$C$44:$E$57,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A22 Capacity Table'!$C$44:$C$57<'10A22 Standard Results'!$E$12,'10A22 Capacity Table'!$C$44:$C$57))","v":{"$error":"#N/A"}},{"$f":"G12/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I12/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I12<0.99999,ROUND(I12,2),\nIF(I12<9.999,ROUND(I12,2),\nIF(I12<99.99,ROUND(I12,1),\nIF(I12<999.99,ROUND(I12,0),\nIF(I12<9999.99,ROUND(I12,-1),\nIF(I12<99999,ROUND(I12,-2),ROUND(I12,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J12,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L12,\" \",\"-\",\" \",K12)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G13,'10A22 Capacity Table'!$C$44:$E$57,2,FALSE),\"-\",VLOOKUP(G13,'10A22 Capacity Table'!$C$44:$E$57,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$44:$C$57>'10A22 Standard Results'!$E$12,'10A22 Capacity Table'!$C$44:$C$57))","v":{"$error":"#N/A"}},{"$f":"G13/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I13/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I13<0.99999,ROUND(I13,2),\nIF(I13<9.999,ROUND(I13,2),\nIF(I13<99.99,ROUND(I13,1),\nIF(I13<999.99,ROUND(I13,0),\nIF(I13<9999.99,ROUND(I13,-1),\nIF(I13<99999,ROUND(I13,-2),ROUND(I13,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J13,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L13,\" \",\"-\",\" \",K13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G14,'10A22 Capacity Table'!$C$44:$E$57,2,FALSE),\"-\",VLOOKUP(G14,'10A22 Capacity Table'!$C$44:$E$57,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$44:$C$57>'10A22 Standard Results'!$G$13,'10A22 Capacity Table'!$C$44:$C$57))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G15,'10A22 Capacity Table'!$C$44:$E$57,2,FALSE),\"-\",VLOOKUP(G15,'10A22 Capacity Table'!$C$44:$E$57,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$44:$C$57>'10A22 Standard Results'!$G$14,'10A22 Capacity Table'!$C$44:$C$57))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!C5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!F12,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!C6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!F13,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!C7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!F14,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!C8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!F15,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!H5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!K12,\"\"))","v":""},{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!F5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!I12,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!H6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!K13,\"\"))","v":""},{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!F6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!I13,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!H7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!K14,\"\"))","v":""},{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!F7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!I14,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!H8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!K15,\"\"))","v":""},{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Standard Results'!F8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Standard Results'!I15,\"\"))","v":""}]

{"sheet":"10A61 Naming","index":49,"n_rows":131,"n_cols":17,"rows_kept":131,"cut":false,"hidden":true,"merged":[[1,0,1,2],[2,4,31,4],[32,4,100,4],[101,4,130,4]]}
[]
["Floats",null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["Designator","Code","Material",null,"3\"",{"$f":"'10A61 3\" Gas+liquid Results'!E4","v":{"$error":"#DIV/0!"}},"1/8-08-","P3","07","FP",{"$f":"CONCATENATE(\"(\",I3,\")\",\" \",J3,\"-\",G3,H3)","v":"(07) FP-1/8-08-P3"},{"$f":"CONCATENATE(\"(\",VLOOKUP(RIGHT(F3,2),$A$4:$C$9,2,FALSE),\")\",\" \",VLOOKUP(RIGHT(F3,2),$A$4:$C$9,3,FALSE))","v":{"$error":"#DIV/0!"}},null,null,"3\" Scale","5\" Scale","10\" Scale"]
["BG","A","Black Glass",null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E5","v":{"$error":"#DIV/0!"}},"1/8-08-","P3","07","FP",{"$f":"CONCATENATE(\"(\",I4,\")\",\" \",J4,\"-\",G4,H4)","v":"(07) FP-1/8-08-P3"},{"$f":"CONCATENATE(\"(\",VLOOKUP(RIGHT(F4,2),$A$4:$C$9,2,FALSE),\")\",\" \",VLOOKUP(RIGHT(F4,2),$A$4:$C$9,3,FALSE))","v":{"$error":"#DIV/0!"}}]
["CD","B","Constant Density",null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E6","v":{"$error":"#DIV/0!"}},"1/8-08-","P3","07","FP","(07) FP-1/8-08-P3",{"$error":"#DIV/0!"}]
["SA","C","Saphire",null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E7","v":{"$error":"#DIV/0!"}},"1/8-08-","P3","07","FP","(07) FP-1/8-08-P3",{"$error":"#DIV/0!"}]
["SS","D","Stainless Steel",null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E8","v":{"$error":"#DIV/0!"}},"1/8-08-","P3","07","FP","(07) FP-1/8-08-P3",{"$error":"#DIV/0!"}]
["CA","E","Carboloy",null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E9","v":{"$error":"#DIV/0!"}},"1/8-20-","P3","08","FP","(08) FP-1/8-20-P3",{"$error":"#DIV/0!"}]
["TA","F","Tantalum",null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E10","v":{"$error":"#DIV/0!"}},"1/8-20-","P3","08","FP","(08) FP-1/8-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E11","v":{"$error":"#DIV/0!"}},"1/8-20-","P3","08","FP","(08) FP-1/8-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E12","v":{"$error":"#DIV/0!"}},"1/8-20-","P3","08","FP","(08) FP-1/8-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E13","v":{"$error":"#DIV/0!"}},"1/8-20-","P3","08","FP","(08) FP-1/8-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E14","v":{"$error":"#DIV/0!"}},"1/4-15-","P3","09","FP","(09) FP-1/4-15-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E15","v":{"$error":"#DIV/0!"}},"1/4-15-","P3","09","FP","(09) FP-1/4-15-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E16","v":{"$error":"#DIV/0!"}},"1/4-15-","P3","09","FP","(09) FP-1/4-15-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E17","v":{"$error":"#DIV/0!"}},"1/4-15-","P3","09","FP","(09) FP-1/4-15-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E18","v":{"$error":"#DIV/0!"}},"1/4-15-","P3","09","FP","(09) FP-1/4-15-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E19","v":{"$error":"#DIV/0!"}},"1/4-20-","P3","10","FP","(10) FP-1/4-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E20","v":{"$error":"#DIV/0!"}},"1/4-20-","P3","10","FP","(10) FP-1/4-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E21","v":{"$error":"#DIV/0!"}},"1/4-20-","P3","10","FP","(10) FP-1/4-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E22","v":{"$error":"#DIV/0!"}},"1/4-20-","P3","10","FP","(10) FP-1/4-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E23","v":{"$error":"#DIV/0!"}},"1/4-20-","P3","10","FP","(10) FP-1/4-20-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E24","v":{"$error":"#DIV/0!"}},"1/4-41-","G3","11","FP","(11) FP-1/4-41-G3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E25","v":{"$error":"#DIV/0!"}},"1/4-41-","G3","11","FP","(11) FP-1/4-41-G3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E26","v":{"$error":"#DIV/0!"}},"1/4-41-","G3","11","FP","(11) FP-1/4-41-G3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E27","v":{"$error":"#DIV/0!"}},"1/4-41-","G3","11","FP","(11) FP-1/4-41-G3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E28","v":{"$error":"#DIV/0!"}},"1/4-41-","G3","11","FP","(11) FP-1/4-41-G3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E29","v":{"$error":"#DIV/0!"}},"1/4-41-","P3","12","FP","(12) FP-1/4-41-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E30","v":{"$error":"#DIV/0!"}},"1/4-41-","P3","12","FP","(12) FP-1/4-41-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E31","v":{"$error":"#DIV/0!"}},"1/4-41-","P3","12","FP","(12) FP-1/4-41-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E32","v":{"$error":"#DIV/0!"}},"1/4-41-","P3","12","FP","(12) FP-1/4-41-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 3\" Gas+liquid Results'!E33","v":{"$error":"#DIV/0!"}},"1/4-41-","P3","12","FP","(12) FP-1/4-41-P3",{"$error":"#DIV/0!"}]
[null,null,null,null,"5\"",{"$f":"'10A61 5\" + 6\" Results'!E3","v":{"$error":"#DIV/0!"}},"1/4-25-","G5","25","FP","(25) FP-1/4-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E4","v":{"$error":"#DIV/0!"}},"1/4-25-","G5","25","FP","(25) FP-1/4-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E5","v":{"$error":"#DIV/0!"}},"1/4-25-","G5","25","FP","(25) FP-1/4-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E6","v":{"$error":"#DIV/0!"}},"1/4-25-","G5","25","FP","(25) FP-1/4-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E7","v":{"$error":"#DIV/0!"}},"1/4-25-","G5","25","FP","(25) FP-1/4-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E8","v":{"$error":"#DIV/0!"}},"1/4-25-","G5","25","FP","(25) FP-1/4-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E9","v":{"$error":"#DIV/0!"}},"1/4-20-","G5","24","FP","(24) FP-1/4-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E10","v":{"$error":"#DIV/0!"}},"1/4-20-","G5","24","FP","(24) FP-1/4-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E11","v":{"$error":"#DIV/0!"}},"1/4-20-","G5","24","FP","(24) FP-1/4-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E12","v":{"$error":"#DIV/0!"}},"1/4-20-","G5","24","FP","(24) FP-1/4-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E13","v":{"$error":"#DIV/0!"}},"1/4-20-","G5","24","FP","(24) FP-1/4-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E14","v":{"$error":"#DIV/0!"}},"1/4-20-","G5","24","FP","(24) FP-1/4-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E15","v":{"$error":"#DIV/0!"}},"1/4-16-","G5","23","FP","(23) FP-1/4-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E16","v":{"$error":"#DIV/0!"}},"1/4-16-","G5","23","FP","(23) FP-1/4-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E17","v":{"$error":"#DIV/0!"}},"1/4-16-","G5","23","FP","(23) FP-1/4-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E18","v":{"$error":"#DIV/0!"}},"1/4-16-","G5","23","FP","(23) FP-1/4-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E19","v":{"$error":"#DIV/0!"}},"1/4-16-","G5","23","FP","(23) FP-1/4-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E20","v":{"$error":"#DIV/0!"}},"1/4-16-","G5","23","FP","(23) FP-1/4-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E21","v":{"$error":"#DIV/0!"}},"1/4-10-","G5","22","FP","(22) FP-1/4-10-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E22","v":{"$error":"#DIV/0!"}},"1/4-10-","G5","22","FP","(22) FP-1/4-10-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E23","v":{"$error":"#DIV/0!"}},"1/4-10-","G5","22","FP","(22) FP-1/4-10-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E24","v":{"$error":"#DIV/0!"}},"1/4-10-","G5","22","FP","(22) FP-1/4-10-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E25","v":{"$error":"#DIV/0!"}},"1/4-10-","G5","22","FP","(22) FP-1/4-10-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E26","v":{"$error":"#DIV/0!"}},"1/4-10-","G5","22","FP","(22) FP-1/4-10-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E27","v":{"$error":"#DIV/0!"}},"1/8-12-","G5","18","FP","(18) FP-1/8-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E28","v":{"$error":"#DIV/0!"}},"1/8-12-","G5","18","FP","(18) FP-1/8-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E29","v":{"$error":"#DIV/0!"}},"1/8-12-","G5","18","FP","(18) FP-1/8-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E30","v":{"$error":"#DIV/0!"}},"1/8-12-","G5","18","FP","(18) FP-1/8-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E31","v":{"$error":"#DIV/0!"}},"1/8-12-","G5","18","FP","(18) FP-1/8-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E32","v":{"$error":"#DIV/0!"}},"1/8-08-","G5","17","FP","(17) FP-1/8-08-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E33","v":{"$error":"#DIV/0!"}},"1/8-08-","G5","17","FP","(17) FP-1/8-08-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E34","v":{"$error":"#DIV/0!"}},"1/8-08-","G5","17","FP","(17) FP-1/8-08-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E35","v":{"$error":"#DIV/0!"}},"1/8-08-","G5","17","FP","(17) FP-1/8-08-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E36","v":{"$error":"#DIV/0!"}},"1/8-08-","G5","17","FP","(17) FP-1/8-08-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E37","v":{"$error":"#DIV/0!"}},"1/16-12-","G5","14","FP","(14) FP-1/16-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E38","v":{"$error":"#DIV/0!"}},"1/16-12-","G5","14","FP",{"$f":"CONCATENATE(\"(\",I68,\")\",\" \",J68,\"-\",G68,H68)","v":"(14) FP-1/16-12-G5"},{"$f":"CONCATENATE(\"(\",VLOOKUP(RIGHT(F68,2),$A$4:$C$9,2,FALSE),\")\",\" \",VLOOKUP(RIGHT(F68,2),$A$4:$C$9,3,FALSE))","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E39","v":{"$error":"#DIV/0!"}},"1/16-12-","G5","14","FP","(14) FP-1/16-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E40","v":{"$error":"#DIV/0!"}},"1/16-12-","G5","14","FP","(14) FP-1/16-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E41","v":{"$error":"#DIV/0!"}},"1/16-12-","G5","14","FP","(14) FP-1/16-12-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E42","v":{"$error":"#DIV/0!"}},"1/16-16-","G5","15","FP","(15) FP-1/16-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E43","v":{"$error":"#DIV/0!"}},"1/16-16-","G5","15","FP","(15) FP-1/16-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E44","v":{"$error":"#DIV/0!"}},"1/16-16-","G5","15","FP","(15) FP-1/16-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E45","v":{"$error":"#DIV/0!"}},"1/16-16-","G5","15","FP","(15) FP-1/16-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E46","v":{"$error":"#DIV/0!"}},"1/16-16-","G5","15","FP","(15) FP-1/16-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E47","v":{"$error":"#DIV/0!"}},"1/16-20-","G5","16","FP","(16) FP-1/16-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E48","v":{"$error":"#DIV/0!"}},"1/16-20-","G5","16","FP","(16) FP-1/16-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E49","v":{"$error":"#DIV/0!"}},"1/16-20-","G5","16","FP","(16) FP-1/16-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E50","v":{"$error":"#DIV/0!"}},"1/16-20-","G5","16","FP","(16) FP-1/16-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E51","v":{"$error":"#DIV/0!"}},"1/16-20-","G5","16","FP","(16) FP-1/16-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E52","v":{"$error":"#DIV/0!"}},"1/8-25-","G5","21","FP","(21) FP-1/8-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E53","v":{"$error":"#DIV/0!"}},"1/8-25-","G5","21","FP","(21) FP-1/8-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E54","v":{"$error":"#DIV/0!"}},"1/8-25-","G5","21","FP","(21) FP-1/8-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E55","v":{"$error":"#DIV/0!"}},"1/8-25-","G5","21","FP","(21) FP-1/8-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E56","v":{"$error":"#DIV/0!"}},"1/8-25-","G5","21","FP","(21) FP-1/8-25-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E57","v":{"$error":"#DIV/0!"}},"1/8-20-","G5","20","FP","(20) FP-1/8-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E58","v":{"$error":"#DIV/0!"}},"1/8-20-","G5","20","FP","(20) FP-1/8-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E59","v":{"$error":"#DIV/0!"}},"1/8-20-","G5","20","FP","(20) FP-1/8-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E60","v":{"$error":"#DIV/0!"}},"1/8-20-","G5","20","FP","(20) FP-1/8-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E61","v":{"$error":"#DIV/0!"}},"1/8-20-","G5","20","FP","(20) FP-1/8-20-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E62","v":{"$error":"#DIV/0!"}},"1/8-16-","G5","19","FP","(19) FP-1/8-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E63","v":{"$error":"#DIV/0!"}},"1/8-16-","G5","19","FP","(19) FP-1/8-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E64","v":{"$error":"#DIV/0!"}},"1/8-16-","G5","19","FP","(19) FP-1/8-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E65","v":{"$error":"#DIV/0!"}},"1/8-16-","G5","19","FP","(19) FP-1/8-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E66","v":{"$error":"#DIV/0!"}},"1/8-16-","G5","19","FP","(19) FP-1/8-16-G5",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E67","v":{"$error":"#DIV/0!"}},"1/4-40-","G6","26","FP","(26) FP-1/4-40-G6",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E68","v":{"$error":"#DIV/0!"}},"1/4-40-","G6","26","FP","(26) FP-1/4-40-G6",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E69","v":{"$error":"#DIV/0!"}},"1/4-40-","G6","26","FP","(26) FP-1/4-40-G6",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E70","v":{"$error":"#DIV/0!"}},"1/4-40-","G6","26","FP","(26) FP-1/4-40-G6",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 5\" + 6\" Results'!E71","v":{"$error":"#DIV/0!"}},"1/4-40-","G6","26","FP","(26) FP-1/4-40-G6",{"$error":"#DIV/0!"}]
[null,null,null,null,"10\"",{"$f":"'10A61 10\" Results'!F4","v":{"$error":"#DIV/0!"}},"1/8-077-","G10","27","FP","(27) FP-1/8-077-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F5","v":{"$error":"#DIV/0!"}},"1/8-077-","G10","27","FP","(27) FP-1/8-077-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F6","v":{"$error":"#DIV/0!"}},"1/8-077-","G10","27","FP","(27) FP-1/8-077-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F7","v":{"$error":"#DIV/0!"}},"1/8-077-","G10","27","FP","(27) FP-1/8-077-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F8","v":{"$error":"#DIV/0!"}},"1/8-077-","G10","27","FP","(27) FP-1/8-077-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F9","v":{"$error":"#DIV/0!"}},"1/8-13.3-","G10","28","FP","(28) FP-1/8-13.3-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F10","v":{"$error":"#DIV/0!"}},"1/8-13.3-","G10","28","FP","(28) FP-1/8-13.3-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F11","v":{"$error":"#DIV/0!"}},"1/8-13.3-","G10","28","FP","(28) FP-1/8-13.3-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F12","v":{"$error":"#DIV/0!"}},"1/8-13.3-","G10","28","FP","(28) FP-1/8-13.3-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F13","v":{"$error":"#DIV/0!"}},"1/8-13.3-","G10","28","FP","(28) FP-1/8-13.3-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F14","v":{"$error":"#DIV/0!"}},"1/8-32-","G10","29","FP","(29) FP-1/8-32-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F15","v":{"$error":"#DIV/0!"}},"1/8-32-","G10","29","FP","(29) FP-1/8-32-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F16","v":{"$error":"#DIV/0!"}},"1/8-32-","G10","29","FP","(29) FP-1/8-32-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F17","v":{"$error":"#DIV/0!"}},"1/8-32-","G10","29","FP","(29) FP-1/8-32-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F18","v":{"$error":"#DIV/0!"}},"1/8-32-","G10","29","FP","(29) FP-1/8-32-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F19","v":{"$error":"#DIV/0!"}},"1/4-10-","G10","30","FP","(30) FP-1/4-10-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F20","v":{"$error":"#DIV/0!"}},"1/4-10-","G10","30","FP","(30) FP-1/4-10-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F21","v":{"$error":"#DIV/0!"}},"1/4-10-","G10","30","FP","(30) FP-1/4-10-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F22","v":{"$error":"#DIV/0!"}},"1/4-10-","G10","30","FP","(30) FP-1/4-10-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F23","v":{"$error":"#DIV/0!"}},"1/4-10-","G10","30","FP","(30) FP-1/4-10-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F24","v":{"$error":"#DIV/0!"}},"1/4-19-","G10","31","FP","(31) FP-1/4-19-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F25","v":{"$error":"#DIV/0!"}},"1/4-19-","G10","31","FP","(31) FP-1/4-19-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F26","v":{"$error":"#DIV/0!"}},"1/4-19-","G10","31","FP","(31) FP-1/4-19-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F27","v":{"$error":"#DIV/0!"}},"1/4-19-","G10","31","FP","(31) FP-1/4-19-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F28","v":{"$error":"#DIV/0!"}},"1/4-19-","G10","31","FP","(31) FP-1/4-19-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F29","v":{"$error":"#DIV/0!"}},"1/4-40-","G10","32","FP","(32) FP-1/4-40-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F30","v":{"$error":"#DIV/0!"}},"1/4-40-","G10","32","FP","(32) FP-1/4-40-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F31","v":{"$error":"#DIV/0!"}},"1/4-40-","G10","32","FP","(32) FP-1/4-40-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F32","v":{"$error":"#DIV/0!"}},"1/4-40-","G10","32","FP","(32) FP-1/4-40-G10",{"$error":"#DIV/0!"}]
[null,null,null,null,null,{"$f":"'10A61 10\" Results'!F33","v":{"$error":"#DIV/0!"}},"1/4-40-","G10","32","FP","(32) FP-1/4-40-G10",{"$error":"#DIV/0!"}]

{"sheet":"10A45 Naming Standard","index":50,"n_rows":219,"n_cols":17,"rows_kept":219,"cut":false,"hidden":true,"merged":[[2,2,2,8]]}
[]
[]
["FP-1/2-17-G-10","A1","Std Floats",null,null,null,null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["FP-1/2-21-G-10","A2",null,"FP-1/2-17-G-10","1/2-GUSVT-40A",{"$f":"VLOOKUP(D4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E4,$A$17:$B$98,2,FALSE)","v":"09"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A"},"FP-1/2-17-G-10","1/2-GUSVT-40A","A1","09",{"$f":"CONCATENATE(\"(\",N4,\")\",\" \",L4)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O4,\")\",\" \",M4)","v":"(09) 1/2-GUSVT-40A"}]
["FP-1/2-27-G-10","A3",null,"FP-1/2-21-G-10","1/2-GUSVT-40A",{"$f":"VLOOKUP(D5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(E5,$A$17:$B$98,2,FALSE)","v":"09"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5)","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A"},"FP-1/2-21-G-10","1/2-GUSVT-40A","A2","09",{"$f":"CONCATENATE(\"(\",N5,\")\",\" \",L5)","v":"(A2) FP-1/2-21-G-10"},{"$f":"CONCATENATE(\"(\",O5,\")\",\" \",M5)","v":"(09) 1/2-GUSVT-40A"}]
["FP-1/2-35-G-10","A4",null,"FP-1/2-27-G-10","1/2-GUSVT-40A","A3","09",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A","FP-1/2-27-G-10","1/2-GUSVT-40A","A3","09","(A3) FP-1/2-27-G-10","(09) 1/2-GUSVT-40A"]
["FP-1/2-50-G-9","A6",null,"FP-1/2-17-G-10","1/2-GSVT-45A","A1","10",null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-17-G-10","1/2-GSVT-45A","A1","10","(A1) FP-1/2-17-G-10","(10) 1/2-GSVT-45A"]
["FP-3/4-21-G-10","B1",null,"FP-1/2-21-G-10","1/2-GSVT-45A","A2","10",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-21-G-10","1/2-GSVT-45A","A2","10","(A2) FP-1/2-21-G-10","(10) 1/2-GSVT-45A"]
["FP-3/4-27-G-10","B2",null,"FP-1/2-35-G-10","1/2-GUSVT-40A","A4","09",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A","FP-1/2-35-G-10","1/2-GUSVT-40A","A4","09","(A4) FP-1/2-35-G-10","(09) 1/2-GUSVT-40A"]
["FP-1-27-G-10","C1",null,"FP-1/2-17-G-10","1/2-GSVT-44A","A1","11",null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-17-G-10","1/2-GSVT-44A","A1","11","(A1) FP-1/2-17-G-10","(11) 1/2-GSVT-44A"]
["FP-1-35-G-10","C2",null,"FP-1/2-17-G-10","1/2-GSVT-48A","A1","12",null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-17-G-10","1/2-GSVT-48A","A1","12","(A1) FP-1/2-17-G-10","(12) 1/2-GSVT-48A"]
["FP-1-1/2-21-G-10","D1",null,"FP-1/2-27-G-10","1/2-GSVT-45A","A3","10",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-27-G-10","1/2-GSVT-45A","A3","10","(A3) FP-1/2-27-G-10","(10) 1/2-GSVT-45A"]
["FP-1-1/2-27-G-10","D2",null,"FP-1/2-21-G-10","1/2-GSVT-44A","A2","11",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-21-G-10","1/2-GSVT-44A","A2","11","(A2) FP-1/2-21-G-10","(11) 1/2-GSVT-44A"]
["FP-2-27-G-10","E1",null,"FP-1/2-21-G-10","1/2-GSVT-48A","A2","12",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-21-G-10","1/2-GSVT-48A","A2","12","(A2) FP-1/2-21-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,"FP-1/2-17-G-10","1/2-GNSVT-48A","A1","13",null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A","FP-1/2-17-G-10","1/2-GNSVT-48A","A1","13","(A1) FP-1/2-17-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,"FP-1/2-21-G-10","1/2-GNSVT-48A","A2","13",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A","FP-1/2-21-G-10","1/2-GNSVT-48A","A2","13","(A2) FP-1/2-21-G-10","(13) 1/2-GNSVT-48A"]
["1/2-GUSVT-410","01",null,"FP-1/2-27-G-10","1/2-GSVT-44A","A3","11",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-27-G-10","1/2-GSVT-44A","A3","11","(A3) FP-1/2-27-G-10","(11) 1/2-GSVT-44A"]
["3/4-GUSVT-510","02",null,"FP-1/2-35-G-10","1/2-GSVT-45A","A4","10",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-35-G-10","1/2-GSVT-45A","A4","10","(A4) FP-1/2-35-G-10","(10) 1/2-GSVT-45A"]
["1-GUSVT-611","03",null,"FP-1/2-27-G-10","1/2-GSVT-48A","A3","12",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-27-G-10","1/2-GSVT-48A","A3","12","(A3) FP-1/2-27-G-10","(12) 1/2-GSVT-48A"]
["1-GUSVT-610","04",null,"FP-1/2-27-G-10","1/2-GNSVT-48A","A3","13",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A","FP-1/2-27-G-10","1/2-GNSVT-48A","A3","13","(A3) FP-1/2-27-G-10","(13) 1/2-GNSVT-48A"]
["1-1/2-GUSVT-867","05",null,"FP-1/2-35-G-10","1/2-GSVT-44A","A4","11",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-35-G-10","1/2-GSVT-44A","A4","11","(A4) FP-1/2-35-G-10","(11) 1/2-GSVT-44A"]
["1-1/2-GUSVGT-814","06",null,"FP-1/2-35-G-10","1/2-GSVT-48A","A4","12",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-35-G-10","1/2-GSVT-48A","A4","12","(A4) FP-1/2-35-G-10","(12) 1/2-GSVT-48A"]
["2-GUSVT-913","07",null,"FP-1/2-50-G-9","1/2-GSVT-45A","A6","10",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A","FP-1/2-50-G-9","1/2-GSVT-45A","A6","10","(A6) FP-1/2-50-G-9","(10) 1/2-GSVT-45A"]
["2-GUSVGT-914","08",null,"FP-1/2-50-G-9","1/2-GSVT-44A","A6","11",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A","FP-1/2-50-G-9","1/2-GSVT-44A","A6","11","(A6) FP-1/2-50-G-9","(11) 1/2-GSVT-44A"]
["1/2-GUSVT-40A","09",null,"FP-1/2-50-G-9","1/2-GSVT-48A","A6","12",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A","FP-1/2-50-G-9","1/2-GSVT-48A","A6","12","(A6) FP-1/2-50-G-9","(12) 1/2-GSVT-48A"]
["1/2-GSVT-45A","10",null,"FP-1/2-50-G-9","1/2-GNSVT-48A","A6","13",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A","FP-1/2-50-G-9","1/2-GNSVT-48A","A6","13","(A6) FP-1/2-50-G-9","(13) 1/2-GNSVT-48A"]
["1/2-GSVT-44A","11",null,"FP-3/4-21-G-10","3/4-GSVGT-54A","B1","14",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A","FP-3/4-21-G-10","3/4-GSVGT-54A","B1","14","(B1) FP-3/4-21-G-10","(14) 3/4-GSVGT-54A"]
["1/2-GSVT-48A","12",null,"FP-3/4-21-G-10","3/4-GNSVGT-54A","B1","15",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A","FP-3/4-21-G-10","3/4-GNSVGT-54A","B1","15","(B1) FP-3/4-21-G-10","(15) 3/4-GNSVGT-54A"]
["1/2-GNSVT-48A","13",null,"FP-3/4-21-G-10","3/4-GSVGT-59A","B1","16",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A","FP-3/4-21-G-10","3/4-GSVGT-59A","B1","16","(B1) FP-3/4-21-G-10","(16) 3/4-GSVGT-59A"]
["3/4-GSVGT-54A","14",null,"FP-3/4-27-G-10","3/4-GSVGT-54A","B2","14",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A","FP-3/4-27-G-10","3/4-GSVGT-54A","B2","14","(B2) FP-3/4-27-G-10","(14) 3/4-GSVGT-54A"]
["3/4-GNSVGT-54A","15",null,"FP-3/4-21-G-10","3/4-GNSVGT-59A","B1","17",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A","FP-3/4-21-G-10","3/4-GNSVGT-59A","B1","17","(B1) FP-3/4-21-G-10","(17) 3/4-GNSVGT-59A"]
["3/4-GSVGT-59A","16",null,"FP-3/4-27-G-10","3/4-GNSVGT-54A","B2","15",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A","FP-3/4-27-G-10","3/4-GNSVGT-54A","B2","15","(B2) FP-3/4-27-G-10","(15) 3/4-GNSVGT-54A"]
["3/4-GNSVGT-59A","17",null,"FP-3/4-27-G-10","3/4-GSVGT-59A","B2","16",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A","FP-3/4-27-G-10","3/4-GSVGT-59A","B2","16","(B2) FP-3/4-27-G-10","(16) 3/4-GSVGT-59A"]
["1-GSVGT-64A","18",null,"FP-3/4-27-G-10","3/4-GNSVGT-59A","B2","17",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A","FP-3/4-27-G-10","3/4-GNSVGT-59A","B2","17","(B2) FP-3/4-27-G-10","(17) 3/4-GNSVGT-59A"]
["1-GSVGT-68A","19",null,"FP-1-27-G-10","1-GSVGT-64A","C1","18",null,null,null,"FP-1-27-G-10                                                                                                  1-GSVGT-64A","FP-1-27-G-10","1-GSVGT-64A","C1","18","(C1) FP-1-27-G-10","(18) 1-GSVGT-64A"]
["1-GNSVGT-64A","20",null,"FP-1-27-G-10","1-GSVGT-68A","C1","19",null,null,null,"FP-1-27-G-10                                                                                                  1-GSVGT-68A","FP-1-27-G-10","1-GSVGT-68A","C1","19","(C1) FP-1-27-G-10","(19) 1-GSVGT-68A"]
["1-GNSVGT-68A","21",null,"FP-1-27-G-10","1-GNSVGT-64A","C1","20",null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-64A","FP-1-27-G-10","1-GNSVGT-64A","C1","20","(C1) FP-1-27-G-10","(20) 1-GNSVGT-64A"]
["1-GSVGT-69A","22",null,"FP-1-35-G-10","1-GSVGT-64A","C2","18",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-64A","FP-1-35-G-10","1-GSVGT-64A","C2","18","(C2) FP-1-35-G-10","(18) 1-GSVGT-64A"]
["1-GNSVGT-69A","23",null,"FP-1-27-G-10","1-GNSVGT-68A","C1","21",null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-68A","FP-1-27-G-10","1-GNSVGT-68A","C1","21","(C1) FP-1-27-G-10","(21) 1-GNSVGT-68A"]
["1-1/2-GSVGT-87A","24",null,"FP-1-35-G-10","1-GSVGT-68A","C2","19",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-68A","FP-1-35-G-10","1-GSVGT-68A","C2","19","(C2) FP-1-35-G-10","(19) 1-GSVGT-68A"]
["1-1/2-GSVGT-86A","25",null,"FP-1-27-G-10","1-GNSVGT-69A","C1","23",null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-69A","FP-1-27-G-10","1-GNSVGT-69A","C1","23","(C1) FP-1-27-G-10","(23) 1-GNSVGT-69A"]
["1-1/2-GNSVGT-87A","26",null,"FP-1-35-G-10","1-GNSVGT-64A","C2","20",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-64A","FP-1-35-G-10","1-GNSVGT-64A","C2","20","(C2) FP-1-35-G-10","(20) 1-GNSVGT-64A"]
["1-1/2-GNSVGT-86A","27",null,"FP-1-35-G-10","1-GNSVGT-68A","C2","21",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-68A","FP-1-35-G-10","1-GNSVGT-68A","C2","21","(C2) FP-1-35-G-10","(21) 1-GNSVGT-68A"]
["2-GSVGT-97A","28",null,"FP-1-35-G-10","1-GSVGT-69A","C2","22",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-69A","FP-1-35-G-10","1-GSVGT-69A","C2","22","(C2) FP-1-35-G-10","(22) 1-GSVGT-69A"]
["2-GSVGT-98A","29",null,"FP-1-35-G-10","1-GNSVGT-69A","C2","23",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-69A","FP-1-35-G-10","1-GNSVGT-69A","C2","23","(C2) FP-1-35-G-10","(23) 1-GNSVGT-69A"]
["2-GNSVGT-97A","30",null,"FP-1-1/2-27-G-10","1-1/2-GSVGT-87A","D2","24",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A","FP-1-1/2-27-G-10","1-1/2-GSVGT-87A","D2","24","(D2) FP-1-1/2-27-G-10","(24) 1-1/2-GSVGT-87A"]
["2-GNSVGT-98A","31",null,"FP-1-1/2-27-G-10","1-1/2-GSVGT-86A","D2","25",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A","FP-1-1/2-27-G-10","1-1/2-GSVGT-86A","D2","25","(D2) FP-1-1/2-27-G-10","(25) 1-1/2-GSVGT-86A"]
["BL-954","32",null,"FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A","D2","26",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A","FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A","D2","26","(D2) FP-1-1/2-27-G-10","(26) 1-1/2-GNSVGT-87A"]
["BL-953","33",null,"FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A","D2","27",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A","FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A","D2","27","(D2) FP-1-1/2-27-G-10","(27) 1-1/2-GNSVGT-86A"]
["BL-950","34",null,"FP-2-27-G-10","2-GSVGT-97A","E1","28",null,null,null,"FP-2-27-G-10                                                                                                  2-GSVGT-97A","FP-2-27-G-10","2-GSVGT-97A","E1","28","(E1) FP-2-27-G-10","(28) 2-GSVGT-97A"]
["BL-951","35",null,"FP-2-27-G-10","2-GSVGT-98A","E1","29",null,null,null,"FP-2-27-G-10                                                                                                  2-GSVGT-98A","FP-2-27-G-10","2-GSVGT-98A","E1","29","(E1) FP-2-27-G-10","(29) 2-GSVGT-98A"]
["1/2-GSVTA-44","36",null,"FP-2-27-G-10","2-GNSVGT-97A","E1","30",null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVGT-97A","FP-2-27-G-10","2-GNSVGT-97A","E1","30","(E1) FP-2-27-G-10","(30) 2-GNSVGT-97A"]
["1/2-GSVTA-48","37",null,"FP-2-27-G-10","2-GNSVGT-98A","E1","31",null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVGT-98A","FP-2-27-G-10","2-GNSVGT-98A","E1","31","(E1) FP-2-27-G-10","(31) 2-GNSVGT-98A"]
["1/2-GNSVTA-48","38",null,"FP-2-27-G-10","BL-954","E1","32",null,null,null,"FP-2-27-G-10                                                                                                  BL-954","FP-2-27-G-10","BL-954","E1","32","(E1) FP-2-27-G-10","(32) BL-954"]
["1/2-GNSVTA-44","39",null,"FP-2-27-G-10","BL-953","E1","33",null,null,null,"FP-2-27-G-10                                                                                                  BL-953","FP-2-27-G-10","BL-953","E1","33","(E1) FP-2-27-G-10","(33) BL-953"]
["1/2-GNSVTA-43","40",null,"FP-2-27-G-10","BL-950","E1","34",null,null,null,"FP-2-27-G-10                                                                                                  BL-950","FP-2-27-G-10","BL-950","E1","34","(E1) FP-2-27-G-10","(34) BL-950"]
["3/4-GSVTA-54","41",null,"FP-2-27-G-10","BL-951","E1","35",null,null,null,"FP-2-27-G-10                                                                                                  BL-951","FP-2-27-G-10","BL-951","E1","35","(E1) FP-2-27-G-10","(35) BL-951"]
["3/4-GNSVTA-54","42",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4)","v":" FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A"},"FP-1/2-17-G-10","1/2-GUSVT-40A","A1","09","(A1) FP-1/2-17-G-10","(09) 1/2-GUSVT-40A"]
["3/4-GSVTA-53","43",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5)","v":" FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A"},"FP-1/2-21-G-10","1/2-GUSVT-40A","A2","09","(A2) FP-1/2-21-G-10","(09) 1/2-GUSVT-40A"]
["3/4-GSVTA-56","44",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A","FP-1/2-27-G-10","1/2-GUSVT-40A","A3","09","(A3) FP-1/2-27-G-10","(09) 1/2-GUSVT-40A"]
["3/4-GNSVTA-56","45",null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-17-G-10","1/2-GSVT-45A","A1","10","(A1) FP-1/2-17-G-10","(10) 1/2-GSVT-45A"]
["3/4-GNSVTA-53","46",null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-21-G-10","1/2-GSVT-45A","A2","10","(A2) FP-1/2-21-G-10","(10) 1/2-GSVT-45A"]
["1-GSVTA-64","47",null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A","FP-1/2-35-G-10","1/2-GUSVT-40A","A4","09","(A4) FP-1/2-35-G-10","(09) 1/2-GUSVT-40A"]
["1-GSVTA-65","48",null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-17-G-10","1/2-GSVT-44A","A1","11","(A1) FP-1/2-17-G-10","(11) 1/2-GSVT-44A"]
["1-GNSVTA-64","49",null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-17-G-10","1/2-GSVT-48A","A1","12","(A1) FP-1/2-17-G-10","(12) 1/2-GSVT-48A"]
["1-GSVTA-63","50",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-27-G-10","1/2-GSVT-45A","A3","10","(A3) FP-1/2-27-G-10","(10) 1/2-GSVT-45A"]
["1-GSVTA-66","51",null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-21-G-10","1/2-GSVT-44A","A2","11","(A2) FP-1/2-21-G-10","(11) 1/2-GSVT-44A"]
["1-GNSVTA-65","52",null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-21-G-10","1/2-GSVT-48A","A2","12","(A2) FP-1/2-21-G-10","(12) 1/2-GSVT-48A"]
["1-GNSVTA-66","53",null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A","FP-1/2-17-G-10","1/2-GNSVT-48A","A1","13",{"$f":"CONCATENATE(\"(\",N69,\")\",\" \",L69)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O69,\")\",\" \",M69)","v":"(13) 1/2-GNSVT-48A"}]
["1-GNSVTA-63","54",null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A","FP-1/2-21-G-10","1/2-GNSVT-48A","A2","13","(A2) FP-1/2-21-G-10","(13) 1/2-GNSVT-48A"]
["1-1/2-GSVTA-84","55",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-27-G-10","1/2-GSVT-44A","A3","11","(A3) FP-1/2-27-G-10","(11) 1/2-GSVT-44A"]
["1-1/2-GSVTA-85","56",null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A","FP-1/2-35-G-10","1/2-GSVT-45A","A4","10","(A4) FP-1/2-35-G-10","(10) 1/2-GSVT-45A"]
["1-1/2-GSVTA-83","57",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-27-G-10","1/2-GSVT-48A","A3","12","(A3) FP-1/2-27-G-10","(12) 1/2-GSVT-48A"]
["1-1/2-GNSVTA-84","58",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A","FP-1/2-27-G-10","1/2-GNSVT-48A","A3","13","(A3) FP-1/2-27-G-10","(13) 1/2-GNSVT-48A"]
["1-1/2-GNSVTA-85","59",null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A","FP-1/2-35-G-10","1/2-GSVT-44A","A4","11","(A4) FP-1/2-35-G-10","(11) 1/2-GSVT-44A"]
["1-1/2-GNSVTA-83","60",null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A","FP-1/2-35-G-10","1/2-GSVT-48A","A4","12","(A4) FP-1/2-35-G-10","(12) 1/2-GSVT-48A"]
["2-GSVTA-94","61",null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A","FP-1/2-50-G-9","1/2-GSVT-45A","A6","10","(A6) FP-1/2-50-G-9","(10) 1/2-GSVT-45A"]
["2-GSVTA-93","62",null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A","FP-1/2-50-G-9","1/2-GSVT-44A","A6","11","(A6) FP-1/2-50-G-9","(11) 1/2-GSVT-44A"]
["2-GNSVTA-94","63",null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A","FP-1/2-50-G-9","1/2-GSVT-48A","A6","12","(A6) FP-1/2-50-G-9","(12) 1/2-GSVT-48A"]
["2-GNSVTA-96","64",null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A","FP-1/2-50-G-9","1/2-GNSVT-48A","A6","13","(A6) FP-1/2-50-G-9","(13) 1/2-GNSVT-48A"]
["2-GNSVTA-93","65",null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A","FP-3/4-21-G-10","3/4-GSVGT-54A","B1","14","(B1) FP-3/4-21-G-10","(14) 3/4-GSVGT-54A"]
["BS-41","66",null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A","FP-3/4-21-G-10","3/4-GNSVGT-54A","B1","15","(B1) FP-3/4-21-G-10","(15) 3/4-GNSVGT-54A"]
["BS-50","67",null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A","FP-3/4-21-G-10","3/4-GSVGT-59A","B1","16","(B1) FP-3/4-21-G-10","(16) 3/4-GSVGT-59A"]
["BS-62","68",null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A","FP-3/4-27-G-10","3/4-GSVGT-54A","B2","14","(B2) FP-3/4-27-G-10","(14) 3/4-GSVGT-54A"]
["BS-60","69",null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A","FP-3/4-21-G-10","3/4-GNSVGT-59A","B1","17","(B1) FP-3/4-21-G-10","(17) 3/4-GNSVGT-59A"]
["BS-80","70",null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A","FP-3/4-27-G-10","3/4-GNSVGT-54A","B2","15","(B2) FP-3/4-27-G-10","(15) 3/4-GNSVGT-54A"]
["BS-90","71",null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A","FP-3/4-27-G-10","3/4-GSVGT-59A","B2","16","(B2) FP-3/4-27-G-10","(16) 3/4-GSVGT-59A"]
["BS-91","72",null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A","FP-3/4-27-G-10","3/4-GNSVGT-59A","B2","17","(B2) FP-3/4-27-G-10","(17) 3/4-GNSVGT-59A"]
["1/2-GL-471","73",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GSVGT-64A","FP-1-27-G-10","1-GSVGT-64A","C1","18","(C1) FP-1-27-G-10","(18) 1-GSVGT-64A"]
["1/2-GL-410","74",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GSVGT-68A","FP-1-27-G-10","1-GSVGT-68A","C1","19","(C1) FP-1-27-G-10","(19) 1-GSVGT-68A"]
["3/4-GL-571","75",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVGT-64A","FP-1-27-G-10","1-GNSVGT-64A","C1","20","(C1) FP-1-27-G-10","(20) 1-GNSVGT-64A"]
["3/4-GL-510","76",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVGT-64A","FP-1-35-G-10","1-GSVGT-64A","C2","18","(C2) FP-1-35-G-10","(18) 1-GSVGT-64A"]
["1-GL-671","77",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVGT-68A","FP-1-27-G-10","1-GNSVGT-68A","C1","21","(C1) FP-1-27-G-10","(21) 1-GNSVGT-68A"]
["1-GL-610","78",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVGT-68A","FP-1-35-G-10","1-GSVGT-68A","C2","19","(C2) FP-1-35-G-10","(19) 1-GSVGT-68A"]
["1-1/2-GL-871","79",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVGT-69A","FP-1-27-G-10","1-GNSVGT-69A","C1","23","(C1) FP-1-27-G-10","(23) 1-GNSVGT-69A"]
["1-1/2-GL-810","80",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVGT-64A","FP-1-35-G-10","1-GNSVGT-64A","C2","20","(C2) FP-1-35-G-10","(20) 1-GNSVGT-64A"]
["2-GL-971","81",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVGT-68A","FP-1-35-G-10","1-GNSVGT-68A","C2","21","(C2) FP-1-35-G-10","(21) 1-GNSVGT-68A"]
["2-GL-910","82",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVGT-69A","FP-1-35-G-10","1-GSVGT-69A","C2","22","(C2) FP-1-35-G-10","(22) 1-GSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVGT-69A","FP-1-35-G-10","1-GNSVGT-69A","C2","23","(C2) FP-1-35-G-10","(23) 1-GNSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A","FP-1-1/2-27-G-10","1-1/2-GSVGT-87A","D2","24","(D2) FP-1-1/2-27-G-10","(24) 1-1/2-GSVGT-87A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A","FP-1-1/2-27-G-10","1-1/2-GSVGT-86A","D2","25","(D2) FP-1-1/2-27-G-10","(25) 1-1/2-GSVGT-86A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A","FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A","D2","26","(D2) FP-1-1/2-27-G-10","(26) 1-1/2-GNSVGT-87A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A","FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A","D2","27","(D2) FP-1-1/2-27-G-10","(27) 1-1/2-GNSVGT-86A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVGT-97A","FP-2-27-G-10","2-GSVGT-97A","E1","28","(E1) FP-2-27-G-10","(28) 2-GSVGT-97A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVGT-98A","FP-2-27-G-10","2-GSVGT-98A","E1","29","(E1) FP-2-27-G-10","(29) 2-GSVGT-98A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVGT-97A","FP-2-27-G-10","2-GNSVGT-97A","E1","30","(E1) FP-2-27-G-10","(30) 2-GNSVGT-97A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVGT-98A","FP-2-27-G-10","2-GNSVGT-98A","E1","31","(E1) FP-2-27-G-10","(31) 2-GNSVGT-98A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-954","FP-2-27-G-10","BL-954","E1","32","(E1) FP-2-27-G-10","(32) BL-954"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-953","FP-2-27-G-10","BL-953","E1","33","(E1) FP-2-27-G-10","(33) BL-953"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-950","FP-2-27-G-10","BL-950","E1","34","(E1) FP-2-27-G-10","(34) BL-950"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-951","FP-2-27-G-10","BL-951","E1","35","(E1) FP-2-27-G-10","(35) BL-951"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4,\" \")","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A "},"FP-1/2-17-G-10","1/2-GUSVT-40A","A1","09","(A1) FP-1/2-17-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5,\" \")","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A "},"FP-1/2-21-G-10","1/2-GUSVT-40A","A2","09","(A2) FP-1/2-21-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A ","FP-1/2-27-G-10","1/2-GUSVT-40A","A3","09","(A3) FP-1/2-27-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-17-G-10","1/2-GSVT-45A","A1","10","(A1) FP-1/2-17-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-21-G-10","1/2-GSVT-45A","A2","10","(A2) FP-1/2-21-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A ","FP-1/2-35-G-10","1/2-GUSVT-40A","A4","09","(A4) FP-1/2-35-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-17-G-10","1/2-GSVT-44A","A1","11","(A1) FP-1/2-17-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-17-G-10","1/2-GSVT-48A","A1","12","(A1) FP-1/2-17-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-27-G-10","1/2-GSVT-45A","A3","10","(A3) FP-1/2-27-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-21-G-10","1/2-GSVT-44A","A2","11","(A2) FP-1/2-21-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-21-G-10","1/2-GSVT-48A","A2","12","(A2) FP-1/2-21-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A ","FP-1/2-17-G-10","1/2-GNSVT-48A","A1","13","(A1) FP-1/2-17-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A ","FP-1/2-21-G-10","1/2-GNSVT-48A","A2","13","(A2) FP-1/2-21-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-27-G-10","1/2-GSVT-44A","A3","11","(A3) FP-1/2-27-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-35-G-10","1/2-GSVT-45A","A4","10","(A4) FP-1/2-35-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-27-G-10","1/2-GSVT-48A","A3","12","(A3) FP-1/2-27-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A ","FP-1/2-27-G-10","1/2-GNSVT-48A","A3","13","(A3) FP-1/2-27-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-35-G-10","1/2-GSVT-44A","A4","11","(A4) FP-1/2-35-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-35-G-10","1/2-GSVT-48A","A4","12","(A4) FP-1/2-35-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A ","FP-1/2-50-G-9","1/2-GSVT-45A","A6","10","(A6) FP-1/2-50-G-9","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A ","FP-1/2-50-G-9","1/2-GSVT-44A","A6","11","(A6) FP-1/2-50-G-9","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A ","FP-1/2-50-G-9","1/2-GSVT-48A","A6","12",{"$f":"CONCATENATE(\"(\",N133,\")\",\" \",L133)","v":"(A6) FP-1/2-50-G-9"},{"$f":"CONCATENATE(\"(\",O133,\")\",\" \",M133)","v":"(12) 1/2-GSVT-48A"}]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A ","FP-1/2-50-G-9","1/2-GNSVT-48A","A6","13","(A6) FP-1/2-50-G-9","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A ","FP-3/4-21-G-10","3/4-GSVGT-54A","B1","14","(B1) FP-3/4-21-G-10","(14) 3/4-GSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A ","FP-3/4-21-G-10","3/4-GNSVGT-54A","B1","15","(B1) FP-3/4-21-G-10","(15) 3/4-GNSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A ","FP-3/4-21-G-10","3/4-GSVGT-59A","B1","16","(B1) FP-3/4-21-G-10","(16) 3/4-GSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A ","FP-3/4-27-G-10","3/4-GSVGT-54A","B2","14","(B2) FP-3/4-27-G-10","(14) 3/4-GSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A ","FP-3/4-21-G-10","3/4-GNSVGT-59A","B1","17","(B1) FP-3/4-21-G-10","(17) 3/4-GNSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A ","FP-3/4-27-G-10","3/4-GNSVGT-54A","B2","15","(B2) FP-3/4-27-G-10","(15) 3/4-GNSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A ","FP-3/4-27-G-10","3/4-GSVGT-59A","B2","16","(B2) FP-3/4-27-G-10","(16) 3/4-GSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A ","FP-3/4-27-G-10","3/4-GNSVGT-59A","B2","17","(B2) FP-3/4-27-G-10","(17) 3/4-GNSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GSVGT-64A ","FP-1-27-G-10","1-GSVGT-64A","C1","18","(C1) FP-1-27-G-10","(18) 1-GSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GSVGT-68A ","FP-1-27-G-10","1-GSVGT-68A","C1","19","(C1) FP-1-27-G-10","(19) 1-GSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-64A ","FP-1-27-G-10","1-GNSVGT-64A","C1","20","(C1) FP-1-27-G-10","(20) 1-GNSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-64A ","FP-1-35-G-10","1-GSVGT-64A","C2","18","(C2) FP-1-35-G-10","(18) 1-GSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-68A ","FP-1-27-G-10","1-GNSVGT-68A","C1","21","(C1) FP-1-27-G-10","(21) 1-GNSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-68A ","FP-1-35-G-10","1-GSVGT-68A","C2","19","(C2) FP-1-35-G-10","(19) 1-GSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVGT-69A ","FP-1-27-G-10","1-GNSVGT-69A","C1","23","(C1) FP-1-27-G-10","(23) 1-GNSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-64A ","FP-1-35-G-10","1-GNSVGT-64A","C2","20","(C2) FP-1-35-G-10","(20) 1-GNSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-68A ","FP-1-35-G-10","1-GNSVGT-68A","C2","21","(C2) FP-1-35-G-10","(21) 1-GNSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVGT-69A ","FP-1-35-G-10","1-GSVGT-69A","C2","22","(C2) FP-1-35-G-10","(22) 1-GSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVGT-69A ","FP-1-35-G-10","1-GNSVGT-69A","C2","23","(C2) FP-1-35-G-10","(23) 1-GNSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A ","FP-1-1/2-27-G-10","1-1/2-GSVGT-87A","D2","24","(D2) FP-1-1/2-27-G-10","(24) 1-1/2-GSVGT-87A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A ","FP-1-1/2-27-G-10","1-1/2-GSVGT-86A","D2","25","(D2) FP-1-1/2-27-G-10","(25) 1-1/2-GSVGT-86A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A ","FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A","D2","26","(D2) FP-1-1/2-27-G-10","(26) 1-1/2-GNSVGT-87A"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A ","FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A","D2","27","(D2) FP-1-1/2-27-G-10","(27) 1-1/2-GNSVGT-86A"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GSVGT-97A ","FP-2-27-G-10","2-GSVGT-97A","E1","28","(E1) FP-2-27-G-10","(28) 2-GSVGT-97A"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GSVGT-98A ","FP-2-27-G-10","2-GSVGT-98A","E1","29","(E1) FP-2-27-G-10","(29) 2-GSVGT-98A"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVGT-97A ","FP-2-27-G-10","2-GNSVGT-97A","E1","30","(E1) FP-2-27-G-10","(30) 2-GNSVGT-97A"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVGT-98A ","FP-2-27-G-10","2-GNSVGT-98A","E1","31","(E1) FP-2-27-G-10","(31) 2-GNSVGT-98A"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  BL-954 ","FP-2-27-G-10","BL-954","E1","32","(E1) FP-2-27-G-10","(32) BL-954"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  BL-953 ","FP-2-27-G-10","BL-953","E1","33","(E1) FP-2-27-G-10","(33) BL-953"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  BL-950 ","FP-2-27-G-10","BL-950","E1","34","(E1) FP-2-27-G-10","(34) BL-950"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  BL-951 ","FP-2-27-G-10","BL-951","E1","35","(E1) FP-2-27-G-10","(35) BL-951"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4,\" \")","v":" FP-1/2-17-G-10                                                                                                  1/2-GUSVT-40A "},"FP-1/2-17-G-10","1/2-GUSVT-40A","A1","09","(A1) FP-1/2-17-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5,\" \")","v":" FP-1/2-21-G-10                                                                                                  1/2-GUSVT-40A "},"FP-1/2-21-G-10","1/2-GUSVT-40A","A2","09","(A2) FP-1/2-21-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GUSVT-40A ","FP-1/2-27-G-10","1/2-GUSVT-40A","A3","09","(A3) FP-1/2-27-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-17-G-10","1/2-GSVT-45A","A1","10","(A1) FP-1/2-17-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-21-G-10","1/2-GSVT-45A","A2","10","(A2) FP-1/2-21-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GUSVT-40A ","FP-1/2-35-G-10","1/2-GUSVT-40A","A4","09","(A4) FP-1/2-35-G-10","(09) 1/2-GUSVT-40A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-17-G-10","1/2-GSVT-44A","A1","11","(A1) FP-1/2-17-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-17-G-10","1/2-GSVT-48A","A1","12","(A1) FP-1/2-17-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-27-G-10","1/2-GSVT-45A","A3","10","(A3) FP-1/2-27-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-21-G-10","1/2-GSVT-44A","A2","11","(A2) FP-1/2-21-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-21-G-10","1/2-GSVT-48A","A2","12","(A2) FP-1/2-21-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GNSVT-48A ","FP-1/2-17-G-10","1/2-GNSVT-48A","A1","13","(A1) FP-1/2-17-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GNSVT-48A ","FP-1/2-21-G-10","1/2-GNSVT-48A","A2","13","(A2) FP-1/2-21-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-27-G-10","1/2-GSVT-44A","A3","11","(A3) FP-1/2-27-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVT-45A ","FP-1/2-35-G-10","1/2-GSVT-45A","A4","10","(A4) FP-1/2-35-G-10","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-27-G-10","1/2-GSVT-48A","A3","12","(A3) FP-1/2-27-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GNSVT-48A ","FP-1/2-27-G-10","1/2-GNSVT-48A","A3","13","(A3) FP-1/2-27-G-10","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVT-44A ","FP-1/2-35-G-10","1/2-GSVT-44A","A4","11","(A4) FP-1/2-35-G-10","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVT-48A ","FP-1/2-35-G-10","1/2-GSVT-48A","A4","12","(A4) FP-1/2-35-G-10","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVT-45A ","FP-1/2-50-G-9","1/2-GSVT-45A","A6","10","(A6) FP-1/2-50-G-9","(10) 1/2-GSVT-45A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVT-44A ","FP-1/2-50-G-9","1/2-GSVT-44A","A6","11","(A6) FP-1/2-50-G-9","(11) 1/2-GSVT-44A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVT-48A ","FP-1/2-50-G-9","1/2-GSVT-48A","A6","12","(A6) FP-1/2-50-G-9","(12) 1/2-GSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GNSVT-48A ","FP-1/2-50-G-9","1/2-GNSVT-48A","A6","13","(A6) FP-1/2-50-G-9","(13) 1/2-GNSVT-48A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVGT-54A ","FP-3/4-21-G-10","3/4-GSVGT-54A","B1","14","(B1) FP-3/4-21-G-10","(14) 3/4-GSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-54A ","FP-3/4-21-G-10","3/4-GNSVGT-54A","B1","15","(B1) FP-3/4-21-G-10","(15) 3/4-GNSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVGT-59A ","FP-3/4-21-G-10","3/4-GSVGT-59A","B1","16","(B1) FP-3/4-21-G-10","(16) 3/4-GSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVGT-54A ","FP-3/4-27-G-10","3/4-GSVGT-54A","B2","14","(B2) FP-3/4-27-G-10","(14) 3/4-GSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GNSVGT-59A ","FP-3/4-21-G-10","3/4-GNSVGT-59A","B1","17","(B1) FP-3/4-21-G-10","(17) 3/4-GNSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-54A ","FP-3/4-27-G-10","3/4-GNSVGT-54A","B2","15","(B2) FP-3/4-27-G-10","(15) 3/4-GNSVGT-54A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVGT-59A ","FP-3/4-27-G-10","3/4-GSVGT-59A","B2","16","(B2) FP-3/4-27-G-10","(16) 3/4-GSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVGT-59A ","FP-3/4-27-G-10","3/4-GNSVGT-59A","B2","17","(B2) FP-3/4-27-G-10","(17) 3/4-GNSVGT-59A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GSVGT-64A ","FP-1-27-G-10","1-GSVGT-64A","C1","18",{"$f":"CONCATENATE(\"(\",N197,\")\",\" \",L197)","v":"(C1) FP-1-27-G-10"},{"$f":"CONCATENATE(\"(\",O197,\")\",\" \",M197)","v":"(18) 1-GSVGT-64A"}]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GSVGT-68A ","FP-1-27-G-10","1-GSVGT-68A","C1","19","(C1) FP-1-27-G-10","(19) 1-GSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVGT-64A ","FP-1-27-G-10","1-GNSVGT-64A","C1","20","(C1) FP-1-27-G-10","(20) 1-GNSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVGT-64A ","FP-1-35-G-10","1-GSVGT-64A","C2","18","(C2) FP-1-35-G-10","(18) 1-GSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVGT-68A ","FP-1-27-G-10","1-GNSVGT-68A","C1","21","(C1) FP-1-27-G-10","(21) 1-GNSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVGT-68A ","FP-1-35-G-10","1-GSVGT-68A","C2","19","(C2) FP-1-35-G-10","(19) 1-GSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVGT-69A ","FP-1-27-G-10","1-GNSVGT-69A","C1","23","(C1) FP-1-27-G-10","(23) 1-GNSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVGT-64A ","FP-1-35-G-10","1-GNSVGT-64A","C2","20","(C2) FP-1-35-G-10","(20) 1-GNSVGT-64A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVGT-68A ","FP-1-35-G-10","1-GNSVGT-68A","C2","21","(C2) FP-1-35-G-10","(21) 1-GNSVGT-68A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVGT-69A ","FP-1-35-G-10","1-GSVGT-69A","C2","22","(C2) FP-1-35-G-10","(22) 1-GSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVGT-69A ","FP-1-35-G-10","1-GNSVGT-69A","C2","23","(C2) FP-1-35-G-10","(23) 1-GNSVGT-69A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-87A ","FP-1-1/2-27-G-10","1-1/2-GSVGT-87A","D2","24","(D2) FP-1-1/2-27-G-10","(24) 1-1/2-GSVGT-87A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVGT-86A ","FP-1-1/2-27-G-10","1-1/2-GSVGT-86A","D2","25","(D2) FP-1-1/2-27-G-10","(25) 1-1/2-GSVGT-86A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-87A ","FP-1-1/2-27-G-10","1-1/2-GNSVGT-87A","D2","26","(D2) FP-1-1/2-27-G-10","(26) 1-1/2-GNSVGT-87A"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVGT-86A ","FP-1-1/2-27-G-10","1-1/2-GNSVGT-86A","D2","27","(D2) FP-1-1/2-27-G-10","(27) 1-1/2-GNSVGT-86A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVGT-97A ","FP-2-27-G-10","2-GSVGT-97A","E1","28","(E1) FP-2-27-G-10","(28) 2-GSVGT-97A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVGT-98A ","FP-2-27-G-10","2-GSVGT-98A","E1","29","(E1) FP-2-27-G-10","(29) 2-GSVGT-98A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVGT-97A ","FP-2-27-G-10","2-GNSVGT-97A","E1","30","(E1) FP-2-27-G-10","(30) 2-GNSVGT-97A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVGT-98A ","FP-2-27-G-10","2-GNSVGT-98A","E1","31","(E1) FP-2-27-G-10","(31) 2-GNSVGT-98A"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-954 ","FP-2-27-G-10","BL-954","E1","32","(E1) FP-2-27-G-10","(32) BL-954"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-953 ","FP-2-27-G-10","BL-953","E1","33","(E1) FP-2-27-G-10","(33) BL-953"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-950 ","FP-2-27-G-10","BL-950","E1","34","(E1) FP-2-27-G-10","(34) BL-950"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  BL-951 ","FP-2-27-G-10","BL-951","E1","35","(E1) FP-2-27-G-10","(35) BL-951"]

{"sheet":"10A22 Naming","index":51,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,null,"vlookup","Application","Meter Size","IX Code"]
[null,"1/4\"",2,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D6,\"-\",'10A22 Capacity Table'!E6)","v":"1/4\"-1B"},{"$f":"RIGHT(F3,2)","v":"1B"},{"$f":"IF(LEFT(F3,4)=$B$3,CONCATENATE(\"(\",$C$3,\")\",\" \",$B$3),\nIF(LEFT(F3,4)=$B$4,CONCATENATE(\"(\",$C$4,\")\",\" \",$B$4),\nIF(LEFT(F3,2)=$B$5,CONCATENATE(\"(\",$C$5,\")\",\" \",$B$5),\nIF(LEFT(F3,6)=$B$6,CONCATENATE(\"(\",$C$6,\")\",\" \",$B$6),\nIF(LEFT(F3,2)=$B$7,CONCATENATE(\"(\",$C$7,\")\",\" \",$B$7))))))","v":"(2) 1/4\""},{"$f":"RIGHT(LEFT(H3,2),1)","v":"2"}]
[null,"1/2\"",3,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D7,\"-\",'10A22 Capacity Table'!E7)","v":"1/4\"-1C"},{"$f":"RIGHT(F4,2)","v":"1C"},{"$f":"IF(LEFT(F4,4)=$B$3,CONCATENATE(\"(\",$C$3,\")\",\" \",$B$3),\nIF(LEFT(F4,4)=$B$4,CONCATENATE(\"(\",$C$4,\")\",\" \",$B$4),\nIF(LEFT(F4,2)=$B$5,CONCATENATE(\"(\",$C$5,\")\",\" \",$B$5),\nIF(LEFT(F4,6)=$B$6,CONCATENATE(\"(\",$C$6,\")\",\" \",$B$6),\nIF(LEFT(F4,2)=$B$7,CONCATENATE(\"(\",$C$7,\")\",\" \",$B$7))))))","v":"(2) 1/4\""},{"$f":"RIGHT(LEFT(H4,2),1)","v":"2"}]
[null,"1\"",4,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D8,\"-\",'10A22 Capacity Table'!E8)","v":"1/2\"-1D"},"1D","(3) 1/2\"","3"]
[null,"1-1/2\"",5,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D9,\"-\",'10A22 Capacity Table'!E9)","v":"1/2\"-1F"},"1F","(3) 1/2\"","3"]
[null,"2\"",6,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D10,\"-\",'10A22 Capacity Table'!E10)","v":"1/2\"-1G"},"1G","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D11,\"-\",'10A22 Capacity Table'!E11)","v":"1/2\"-1H"},"1H","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D12,\"-\",'10A22 Capacity Table'!E12)","v":"1\"-1J"},"1J","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D13,\"-\",'10A22 Capacity Table'!E13)","v":"1\"-1K"},"1K","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D14,\"-\",'10A22 Capacity Table'!E14)","v":"1\"-1L"},"1L","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D15,\"-\",'10A22 Capacity Table'!E15)","v":"1-1/2\"-1M"},"1M","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D16,\"-\",'10A22 Capacity Table'!E16)","v":"1-1/2\"-1N"},"1N","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D17,\"-\",'10A22 Capacity Table'!E17)","v":"1-1/2\"-1P"},"1P","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D18,\"-\",'10A22 Capacity Table'!E18)","v":"2\"-1Q"},"1Q","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D19,\"-\",'10A22 Capacity Table'!E19)","v":"2\"-1R"},"1R","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D27,\"-\",'10A22 Capacity Table'!E27)","v":"1/2\"-1E"},"1E","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D28,\"-\",'10A22 Capacity Table'!E28)","v":"1/2\"-1F"},"1F","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D29,\"-\",'10A22 Capacity Table'!E29)","v":"1/2\"-1H"},"1H","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D30,\"-\",'10A22 Capacity Table'!E30)","v":"1\"-1J"},"1J","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D31,\"-\",'10A22 Capacity Table'!E31)","v":"1\"-1K"},"1K","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D32,\"-\",'10A22 Capacity Table'!E32)","v":"1\"-1L"},"1L","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D33,\"-\",'10A22 Capacity Table'!E33)","v":"1-1/2\"-1M"},"1M","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D34,\"-\",'10A22 Capacity Table'!E34)","v":"1-1/2\"-1N"},"1N","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D35,\"-\",'10A22 Capacity Table'!E35)","v":"1-1/2\"-1P"},"1P","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D36,\"-\",'10A22 Capacity Table'!E36)","v":"2\"-1Q"},"1Q","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D37,\"-\",'10A22 Capacity Table'!E37)","v":"2\"-1R"},"1R","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D44,\"-\",'10A22 Capacity Table'!E44)","v":"1/4\"-2B"},"2B","(2) 1/4\"","2"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D45,\"-\",'10A22 Capacity Table'!E45)","v":"1/4\"-2C"},"2C","(2) 1/4\"","2"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D46,\"-\",'10A22 Capacity Table'!E46)","v":"1/2\"-2D"},"2D","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D47,\"-\",'10A22 Capacity Table'!E47)","v":"1/2\"-2E"},"2E","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D48,\"-\",'10A22 Capacity Table'!E48)","v":"1/2\"-2G"},"2G","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D49,\"-\",'10A22 Capacity Table'!E49)","v":"1/2\"-2K"},"2K","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D50,\"-\",'10A22 Capacity Table'!E50)","v":"1\"-2L"},"2L","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D51,\"-\",'10A22 Capacity Table'!E51)","v":"1\"-2N"},"2N","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D52,\"-\",'10A22 Capacity Table'!E52)","v":"1\"-2P"},"2P","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D53,\"-\",'10A22 Capacity Table'!E53)","v":"1-1/2\"-2Q"},"2Q","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D54,\"-\",'10A22 Capacity Table'!E54)","v":"1-1/2\"-2R"},"2R","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D55,\"-\",'10A22 Capacity Table'!E55)","v":"1-1/2\"-2S"},"2S","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D56,\"-\",'10A22 Capacity Table'!E56)","v":"2\"-2T"},"2T","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D57,\"-\",'10A22 Capacity Table'!E57)","v":"2\"-2U"},"2U","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D62,\"-\",'10A22 Capacity Table'!E62)","v":"1/2\"-2F"},"2F","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D63,\"-\",'10A22 Capacity Table'!E63)","v":"1/2\"-2H"},"2H","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D64,\"-\",'10A22 Capacity Table'!E64)","v":"1/2\"-2J"},"2J","(3) 1/2\"","3"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D65,\"-\",'10A22 Capacity Table'!E65)","v":"1\"-2L"},"2L","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D66,\"-\",'10A22 Capacity Table'!E66)","v":"1\"-2M"},"2M","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D67,\"-\",'10A22 Capacity Table'!E67)","v":"1\"-2P"},"2P","(4) 1\"","4"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D68,\"-\",'10A22 Capacity Table'!E68)","v":"1-1/2\"-2Q"},"2Q","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D69,\"-\",'10A22 Capacity Table'!E69)","v":"1-1/2\"-2R"},"2R","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D70,\"-\",'10A22 Capacity Table'!E70)","v":"1-1/2\"-2S"},"2S","(5) 1-1/2\"","5"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D71,\"-\",'10A22 Capacity Table'!E71)","v":"2\"-2T"},"2T","(6) 2\"","6"]
[null,null,null,null,null,{"$f":"CONCATENATE('10A22 Capacity Table'!D72,\"-\",'10A22 Capacity Table'!E72)","v":"2\"-2U"},"2U","(6) 2\"","6"]

{"sheet":"10A45 Naming Low PSI","index":52,"n_rows":98,"n_cols":17,"rows_kept":98,"cut":false,"hidden":true,"merged":[[2,2,2,8]]}
[]
[]
["FP-1/2-17-G-10","A1","Low PSI Floats",null,null,null,null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["FP-1/2-21-G-10","A2",null,"FP-1/2-17-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(D4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E4,$A$17:$B$98,2,FALSE)","v":"01"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410"},"FP-1/2-17-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M4,$A$17:$B$98,2,FALSE)","v":"01"},{"$f":"CONCATENATE(\"(\",N4,\")\",\" \",L4)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O4,\")\",\" \",M4)","v":"(01) 1/2-GUSVT-410"}]
["FP-1/2-27-G-10","A3",null,"FP-1/2-21-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(D5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(E5,$A$17:$B$98,2,FALSE)","v":"01"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5)","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410"},"FP-1/2-21-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M5,$A$17:$B$98,2,FALSE)","v":"01"},{"$f":"CONCATENATE(\"(\",N5,\")\",\" \",L5)","v":"(A2) FP-1/2-21-G-10"},"(01) 1/2-GUSVT-410"]
["FP-1/2-35-G-10","A4",null,"FP-1/2-27-G-10","1/2-GUSVT-410","A3","01",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410","FP-1/2-27-G-10","1/2-GUSVT-410","A3","01","(A3) FP-1/2-27-G-10","(01) 1/2-GUSVT-410"]
["FP-1/2-50-G-9","A6",null,"FP-1/2-35-G-10","1/2-GUSVT-410","A4","01",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410","FP-1/2-35-G-10","1/2-GUSVT-410","A4","01","(A4) FP-1/2-35-G-10","(01) 1/2-GUSVT-410"]
["FP-3/4-21-G-10","B1",null,"FP-1/2-50-G-9","1/2-GUSVT-410","A6","01",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410","FP-1/2-50-G-9","1/2-GUSVT-410","A6","01","(A6) FP-1/2-50-G-9","(01) 1/2-GUSVT-410"]
["FP-3/4-27-G-10","B2",null,"FP-3/4-21-G-10","3/4-GUSVT-510","B1","02",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510","FP-3/4-21-G-10","3/4-GUSVT-510","B1","02","(B1) FP-3/4-21-G-10","(02) 3/4-GUSVT-510"]
["FP-1-27-G-10","C1",null,"FP-3/4-27-G-10","3/4-GUSVT-510","B2","02",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510","FP-3/4-27-G-10","3/4-GUSVT-510","B2","02","(B2) FP-3/4-27-G-10","(02) 3/4-GUSVT-510"]
["FP-1-35-G-10","C2",null,"FP-1-27-G-10","1-GUSVT-611","C1","03",null,null,null,"FP-1-27-G-10                                                                                                  1-GUSVT-611","FP-1-27-G-10","1-GUSVT-611","C1","03","(C1) FP-1-27-G-10","(03) 1-GUSVT-611"]
["FP-1-1/2-21-G-10","D1",null,"FP-1-35-G-10","1-GUSVT-611","C2","03",null,null,null,"FP-1-35-G-10                                                                                                  1-GUSVT-611","FP-1-35-G-10","1-GUSVT-611","C2","03","(C2) FP-1-35-G-10","(03) 1-GUSVT-611"]
["FP-1-1/2-27-G-10","D2",null,"FP-1-27-G-10","1-GUSVT-610","C1","04",null,null,null,"FP-1-27-G-10                                                                                                  1-GUSVT-610","FP-1-27-G-10","1-GUSVT-610","C1","04","(C1) FP-1-27-G-10","(04) 1-GUSVT-610"]
["FP-2-27-G-10","E1",null,"FP-1-35-G-10","1-GUSVT-610","C2","04",null,null,null,"FP-1-35-G-10                                                                                                  1-GUSVT-610","FP-1-35-G-10","1-GUSVT-610","C2","04","(C2) FP-1-35-G-10","(04) 1-GUSVT-610"]
[null,null,null,"FP-1-1/2-21-G-10","1-1/2-GUSVT-867","D1","05",null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867","FP-1-1/2-21-G-10","1-1/2-GUSVT-867","D1","05","(D1) FP-1-1/2-21-G-10","(05) 1-1/2-GUSVT-867"]
[null,null,null,"FP-1-1/2-27-G-10","1-1/2-GUSVT-867","D2","05",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867","FP-1-1/2-27-G-10","1-1/2-GUSVT-867","D2","05","(D2) FP-1-1/2-27-G-10","(05) 1-1/2-GUSVT-867"]
["1/2-GUSVT-410","01",null,"FP-1-1/2-21-G-10","1-1/2-GUSVGT-814","D1","06",null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814","FP-1-1/2-21-G-10","1-1/2-GUSVGT-814","D1","06","(D1) FP-1-1/2-21-G-10","(06) 1-1/2-GUSVGT-814"]
["3/4-GUSVT-510","02",null,"FP-1-1/2-27-G-10","1-1/2-GUSVGT-814","D2","06",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814","FP-1-1/2-27-G-10","1-1/2-GUSVGT-814","D2","06","(D2) FP-1-1/2-27-G-10","(06) 1-1/2-GUSVGT-814"]
["1-GUSVT-611","03",null,"FP-2-27-G-10","2-GUSVT-913","E1","07",null,null,null,"FP-2-27-G-10                                                                                                  2-GUSVT-913","FP-2-27-G-10","2-GUSVT-913","E1","07","(E1) FP-2-27-G-10","(07) 2-GUSVT-913"]
["1-GUSVT-610","04",null,"FP-2-27-G-10","2-GUSVGT-914","E1","08",null,null,null,"FP-2-27-G-10                                                                                                  2-GUSVGT-914","FP-2-27-G-10","2-GUSVGT-914","E1","08","(E1) FP-2-27-G-10","(08) 2-GUSVGT-914"]
["1-1/2-GUSVT-867","05",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4)","v":" FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410"},"FP-1/2-17-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L21,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M21,$A$17:$B$98,2,FALSE)","v":"01"},"(A1) FP-1/2-17-G-10","(01) 1/2-GUSVT-410"]
["1-1/2-GUSVGT-814","06",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5)","v":" FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410"},"FP-1/2-21-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L22,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M22,$A$17:$B$98,2,FALSE)","v":"01"},"(A2) FP-1/2-21-G-10","(01) 1/2-GUSVT-410"]
["2-GUSVT-913","07",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410","FP-1/2-27-G-10","1/2-GUSVT-410","A3","01","(A3) FP-1/2-27-G-10","(01) 1/2-GUSVT-410"]
["2-GUSVGT-914","08",null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410","FP-1/2-35-G-10","1/2-GUSVT-410","A4","01","(A4) FP-1/2-35-G-10","(01) 1/2-GUSVT-410"]
["1/2-GUSVT-40A","09",null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410","FP-1/2-50-G-9","1/2-GUSVT-410","A6","01","(A6) FP-1/2-50-G-9","(01) 1/2-GUSVT-410"]
["1/2-GSVT-45A","10",null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510","FP-3/4-21-G-10","3/4-GUSVT-510","B1","02","(B1) FP-3/4-21-G-10","(02) 3/4-GUSVT-510"]
["1/2-GSVT-44A","11",null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510","FP-3/4-27-G-10","3/4-GUSVT-510","B2","02","(B2) FP-3/4-27-G-10","(02) 3/4-GUSVT-510"]
["1/2-GSVT-48A","12",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GUSVT-611","FP-1-27-G-10","1-GUSVT-611","C1","03","(C1) FP-1-27-G-10","(03) 1-GUSVT-611"]
["1/2-GNSVT-48A","13",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GUSVT-611","FP-1-35-G-10","1-GUSVT-611","C2","03","(C2) FP-1-35-G-10","(03) 1-GUSVT-611"]
["3/4-GSVGT-54A","14",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GUSVT-610","FP-1-27-G-10","1-GUSVT-610","C1","04","(C1) FP-1-27-G-10","(04) 1-GUSVT-610"]
["3/4-GNSVGT-54A","15",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GUSVT-610","FP-1-35-G-10","1-GUSVT-610","C2","04","(C2) FP-1-35-G-10","(04) 1-GUSVT-610"]
["3/4-GSVGT-59A","16",null,null,null,null,null,null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867","FP-1-1/2-21-G-10","1-1/2-GUSVT-867","D1","05","(D1) FP-1-1/2-21-G-10","(05) 1-1/2-GUSVT-867"]
["3/4-GNSVGT-59A","17",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D16,\"                                                                                                  \",E16)","v":" FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867"},"FP-1-1/2-27-G-10","1-1/2-GUSVT-867","D2","05","(D2) FP-1-1/2-27-G-10","(05) 1-1/2-GUSVT-867"]
["1-GSVGT-64A","18",null,null,null,null,null,null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814","FP-1-1/2-21-G-10","1-1/2-GUSVGT-814","D1","06","(D1) FP-1-1/2-21-G-10","(06) 1-1/2-GUSVGT-814"]
["1-GSVGT-68A","19",null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814","FP-1-1/2-27-G-10","1-1/2-GUSVGT-814","D2","06","(D2) FP-1-1/2-27-G-10","(06) 1-1/2-GUSVGT-814"]
["1-GNSVGT-64A","20",null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GUSVT-913","FP-2-27-G-10","2-GUSVT-913","E1","07","(E1) FP-2-27-G-10","(07) 2-GUSVT-913"]
["1-GNSVGT-68A","21",null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GUSVGT-914","FP-2-27-G-10","2-GUSVGT-914","E1","08","(E1) FP-2-27-G-10","(08) 2-GUSVGT-914"]
["1-GSVGT-69A","22",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4,\" \")","v":"FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410 "},"FP-1/2-17-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L38,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M38,$A$17:$B$98,2,FALSE)","v":"01"},"(A1) FP-1/2-17-G-10","(01) 1/2-GUSVT-410"]
["1-GNSVGT-69A","23",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5,\" \")","v":"FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410 "},"FP-1/2-21-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L39,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M39,$A$17:$B$98,2,FALSE)","v":"01"},"(A2) FP-1/2-21-G-10","(01) 1/2-GUSVT-410"]
["1-1/2-GSVGT-87A","24",null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410 ","FP-1/2-27-G-10","1/2-GUSVT-410","A3","01","(A3) FP-1/2-27-G-10","(01) 1/2-GUSVT-410"]
["1-1/2-GSVGT-86A","25",null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410 ","FP-1/2-35-G-10","1/2-GUSVT-410","A4","01","(A4) FP-1/2-35-G-10","(01) 1/2-GUSVT-410"]
["1-1/2-GNSVGT-87A","26",null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410 ","FP-1/2-50-G-9","1/2-GUSVT-410","A6","01","(A6) FP-1/2-50-G-9","(01) 1/2-GUSVT-410"]
["1-1/2-GNSVGT-86A","27",null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510 ","FP-3/4-21-G-10","3/4-GUSVT-510","B1","02","(B1) FP-3/4-21-G-10","(02) 3/4-GUSVT-510"]
["2-GSVGT-97A","28",null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510 ","FP-3/4-27-G-10","3/4-GUSVT-510","B2","02","(B2) FP-3/4-27-G-10","(02) 3/4-GUSVT-510"]
["2-GSVGT-98A","29",null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GUSVT-611 ","FP-1-27-G-10","1-GUSVT-611","C1","03","(C1) FP-1-27-G-10","(03) 1-GUSVT-611"]
["2-GNSVGT-97A","30",null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GUSVT-611 ","FP-1-35-G-10","1-GUSVT-611","C2","03","(C2) FP-1-35-G-10","(03) 1-GUSVT-611"]
["2-GNSVGT-98A","31",null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GUSVT-610 ","FP-1-27-G-10","1-GUSVT-610","C1","04","(C1) FP-1-27-G-10","(04) 1-GUSVT-610"]
["BL-954","32",null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GUSVT-610 ","FP-1-35-G-10","1-GUSVT-610","C2","04","(C2) FP-1-35-G-10","(04) 1-GUSVT-610"]
["BL-953","33",null,null,null,null,null,null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867 ","FP-1-1/2-21-G-10","1-1/2-GUSVT-867","D1","05","(D1) FP-1-1/2-21-G-10","(05) 1-1/2-GUSVT-867"]
["BL-950","34",null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867 ","FP-1-1/2-27-G-10","1-1/2-GUSVT-867","D2","05","(D2) FP-1-1/2-27-G-10","(05) 1-1/2-GUSVT-867"]
["BL-951","35",null,null,null,null,null,null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814 ","FP-1-1/2-21-G-10","1-1/2-GUSVGT-814","D1","06","(D1) FP-1-1/2-21-G-10","(06) 1-1/2-GUSVGT-814"]
["1/2-GSVTA-44","36",null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814 ","FP-1-1/2-27-G-10","1-1/2-GUSVGT-814","D2","06","(D2) FP-1-1/2-27-G-10","(06) 1-1/2-GUSVGT-814"]
["1/2-GSVTA-48","37",null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GUSVT-913 ","FP-2-27-G-10","2-GUSVT-913","E1","07","(E1) FP-2-27-G-10","(07) 2-GUSVT-913"]
["1/2-GNSVTA-48","38",null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GUSVGT-914 ","FP-2-27-G-10","2-GUSVGT-914","E1","08","(E1) FP-2-27-G-10","(08) 2-GUSVGT-914"]
["1/2-GNSVTA-44","39",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4,\" \")","v":" FP-1/2-17-G-10                                                                                                  1/2-GUSVT-410 "},"FP-1/2-17-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L55,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M55,$A$17:$B$98,2,FALSE)","v":"01"},"(A1) FP-1/2-17-G-10","(01) 1/2-GUSVT-410"]
["1/2-GNSVTA-43","40",null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5,\" \")","v":" FP-1/2-21-G-10                                                                                                  1/2-GUSVT-410 "},"FP-1/2-21-G-10","1/2-GUSVT-410",{"$f":"VLOOKUP(L56,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M56,$A$17:$B$98,2,FALSE)","v":"01"},"(A2) FP-1/2-21-G-10","(01) 1/2-GUSVT-410"]
["3/4-GSVTA-54","41",null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GUSVT-410 ","FP-1/2-27-G-10","1/2-GUSVT-410","A3","01","(A3) FP-1/2-27-G-10","(01) 1/2-GUSVT-410"]
["3/4-GNSVTA-54","42",null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GUSVT-410 ","FP-1/2-35-G-10","1/2-GUSVT-410","A4","01","(A4) FP-1/2-35-G-10","(01) 1/2-GUSVT-410"]
["3/4-GSVTA-53","43",null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GUSVT-410 ","FP-1/2-50-G-9","1/2-GUSVT-410","A6","01","(A6) FP-1/2-50-G-9","(01) 1/2-GUSVT-410"]
["3/4-GSVTA-56","44",null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GUSVT-510 ","FP-3/4-21-G-10","3/4-GUSVT-510","B1","02","(B1) FP-3/4-21-G-10","(02) 3/4-GUSVT-510"]
["3/4-GNSVTA-56","45",null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GUSVT-510 ","FP-3/4-27-G-10","3/4-GUSVT-510","B2","02","(B2) FP-3/4-27-G-10","(02) 3/4-GUSVT-510"]
["3/4-GNSVTA-53","46",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GUSVT-611 ","FP-1-27-G-10","1-GUSVT-611","C1","03","(C1) FP-1-27-G-10","(03) 1-GUSVT-611"]
["1-GSVTA-64","47",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GUSVT-611 ","FP-1-35-G-10","1-GUSVT-611","C2","03","(C2) FP-1-35-G-10","(03) 1-GUSVT-611"]
["1-GSVTA-65","48",null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GUSVT-610 ","FP-1-27-G-10","1-GUSVT-610","C1","04","(C1) FP-1-27-G-10","(04) 1-GUSVT-610"]
["1-GNSVTA-64","49",null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GUSVT-610 ","FP-1-35-G-10","1-GUSVT-610","C2","04","(C2) FP-1-35-G-10","(04) 1-GUSVT-610"]
["1-GSVTA-63","50",null,null,null,null,null,null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVT-867 ","FP-1-1/2-21-G-10","1-1/2-GUSVT-867","D1","05","(D1) FP-1-1/2-21-G-10","(05) 1-1/2-GUSVT-867"]
["1-GSVTA-66","51",null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVT-867 ","FP-1-1/2-27-G-10","1-1/2-GUSVT-867","D2","05","(D2) FP-1-1/2-27-G-10","(05) 1-1/2-GUSVT-867"]
["1-GNSVTA-65","52",null,null,null,null,null,null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GUSVGT-814 ","FP-1-1/2-21-G-10","1-1/2-GUSVGT-814","D1","06","(D1) FP-1-1/2-21-G-10","(06) 1-1/2-GUSVGT-814"]
["1-GNSVTA-66","53",null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GUSVGT-814 ","FP-1-1/2-27-G-10","1-1/2-GUSVGT-814","D2","06",{"$f":"CONCATENATE(\"(\",N69,\")\",\" \",L69)","v":"(D2) FP-1-1/2-27-G-10"},"(06) 1-1/2-GUSVGT-814"]
["1-GNSVTA-63","54",null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GUSVT-913 ","FP-2-27-G-10","2-GUSVT-913","E1","07","(E1) FP-2-27-G-10","(07) 2-GUSVT-913"]
["1-1/2-GSVTA-84","55",null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GUSVGT-914 ","FP-2-27-G-10","2-GUSVGT-914","E1","08","(E1) FP-2-27-G-10","(08) 2-GUSVGT-914"]
["1-1/2-GSVTA-85","56"]
["1-1/2-GSVTA-83","57"]
["1-1/2-GNSVTA-84","58"]
["1-1/2-GNSVTA-85","59"]
["1-1/2-GNSVTA-83","60"]
["2-GSVTA-94","61"]
["2-GSVTA-93","62"]
["2-GNSVTA-94","63"]
["2-GNSVTA-96","64"]
["2-GNSVTA-93","65"]
["BS-41","66"]
["BS-50","67"]
["BS-62","68"]
["BS-60","69"]
["BS-80","70"]
["BS-90","71"]
["BS-91","72"]
["1/2-GL-471","73"]
["1/2-GL-410","74"]
["3/4-GL-571","75"]
["3/4-GL-510","76"]
["1-GL-671","77"]
["1-GL-610","78"]
["1-1/2-GL-871","79"]
["1-1/2-GL-810","80"]
["2-GL-971","81"]
["2-GL-910","82"]

{"sheet":"10A45 Naming Alarm","index":53,"n_rows":203,"n_cols":17,"rows_kept":203,"cut":false,"hidden":true,"merged":[[2,2,2,8]]}
[]
[]
["FP-1/2-17-G-10","A1","Alarm Floats",null,null,null,null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["FP-1/2-21-G-10","A2",null,"FP-1/2-17-G-10","1/2-GSVTA-44",{"$f":"VLOOKUP(D4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E4,$A$17:$B$98,2,FALSE)","v":"36"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44"},"FP-1/2-17-G-10","1/2-GSVTA-44",{"$f":"VLOOKUP(L4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M4,$A$17:$B$98,2,FALSE)","v":"36"},{"$f":"CONCATENATE(\"(\",N4,\")\",\" \",L4)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O4,\")\",\" \",M4)","v":"(36) 1/2-GSVTA-44"}]
["FP-1/2-27-G-10","A3",null,"FP-1/2-17-G-10","1/2-GSVTA-48",{"$f":"VLOOKUP(D5,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E5,$A$17:$B$98,2,FALSE)","v":"37"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5)","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48"},"FP-1/2-17-G-10","1/2-GSVTA-48",{"$f":"VLOOKUP(L5,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M5,$A$17:$B$98,2,FALSE)","v":"37"},{"$f":"CONCATENATE(\"(\",N5,\")\",\" \",L5)","v":"(A1) FP-1/2-17-G-10"},"(37) 1/2-GSVTA-48"]
["FP-1/2-35-G-10","A4",null,"FP-1/2-21-G-10","1/2-GSVTA-44","A2","36",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44","FP-1/2-21-G-10","1/2-GSVTA-44","A2","36","(A2) FP-1/2-21-G-10","(36) 1/2-GSVTA-44"]
["FP-1/2-50-G-9","A6",null,"FP-1/2-21-G-10","1/2-GSVTA-48","A2","37",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48","FP-1/2-21-G-10","1/2-GSVTA-48","A2","37","(A2) FP-1/2-21-G-10","(37) 1/2-GSVTA-48"]
["FP-3/4-21-G-10","B1",null,"FP-1/2-17-G-10","1/2-GNSVTA-48","A1","38",null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-17-G-10","1/2-GNSVTA-48","A1","38","(A1) FP-1/2-17-G-10","(38) 1/2-GNSVTA-48"]
["FP-3/4-27-G-10","B2",null,"FP-1/2-21-G-10","1/2-GNSVTA-44","A2","39",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44","FP-1/2-21-G-10","1/2-GNSVTA-44","A2","39","(A2) FP-1/2-21-G-10","(39) 1/2-GNSVTA-44"]
["FP-1-27-G-10","C1",null,"FP-1/2-21-G-10","1/2-GNSVTA-48","A2","38",null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-21-G-10","1/2-GNSVTA-48","A2","38","(A2) FP-1/2-21-G-10","(38) 1/2-GNSVTA-48"]
["FP-1-35-G-10","C2",null,"FP-1/2-27-G-10","1/2-GSVTA-44","A3","36",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44","FP-1/2-27-G-10","1/2-GSVTA-44","A3","36","(A3) FP-1/2-27-G-10","(36) 1/2-GSVTA-44"]
["FP-1-1/2-21-G-10","D1",null,"FP-1/2-27-G-10","1/2-GSVTA-48","A3","37",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48","FP-1/2-27-G-10","1/2-GSVTA-48","A3","37","(A3) FP-1/2-27-G-10","(37) 1/2-GSVTA-48"]
["FP-1-1/2-27-G-10","D2",null,"FP-1/2-27-G-10","1/2-GNSVTA-48","A3","38",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-27-G-10","1/2-GNSVTA-48","A3","38","(A3) FP-1/2-27-G-10","(38) 1/2-GNSVTA-48"]
["FP-2-27-G-10","E1",null,"FP-1/2-35-G-10","1/2-GSVTA-44","A4","36",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44","FP-1/2-35-G-10","1/2-GSVTA-44","A4","36","(A4) FP-1/2-35-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,"FP-1/2-35-G-10","1/2-GSVTA-48","A4","37",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48","FP-1/2-35-G-10","1/2-GSVTA-48","A4","37","(A4) FP-1/2-35-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,"FP-1/2-27-G-10","1/2-GNSVTA-43","A3","40",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43","FP-1/2-27-G-10","1/2-GNSVTA-43","A3","40","(A3) FP-1/2-27-G-10","(40) 1/2-GNSVTA-43"]
["1/2-GUSVT-410","01",null,"FP-1/2-35-G-10","1/2-GNSVTA-48","A4","38",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-35-G-10","1/2-GNSVTA-48","A4","38","(A4) FP-1/2-35-G-10","(38) 1/2-GNSVTA-48"]
["3/4-GUSVT-510","02",null,"FP-1/2-35-G-10","1/2-GNSVTA-43","A4","40",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43","FP-1/2-35-G-10","1/2-GNSVTA-43","A4","40","(A4) FP-1/2-35-G-10","(40) 1/2-GNSVTA-43"]
["1-GUSVT-611","03",null,"FP-1/2-50-G-9","1/2-GSVTA-44","A6","36",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44","FP-1/2-50-G-9","1/2-GSVTA-44","A6","36","(A6) FP-1/2-50-G-9","(36) 1/2-GSVTA-44"]
["1-GUSVT-610","04",null,"FP-1/2-50-G-9","1/2-GSVTA-48","A6","37",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48","FP-1/2-50-G-9","1/2-GSVTA-48","A6","37","(A6) FP-1/2-50-G-9","(37) 1/2-GSVTA-48"]
["1-1/2-GUSVT-867","05",null,"FP-1/2-50-G-9","1/2-GNSVTA-48",{"$f":"VLOOKUP(D21,$A$3:$B$14,2,FALSE)","v":"A6"},{"$f":"VLOOKUP(E21,$A$17:$B$98,2,FALSE)","v":"38"},null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48","FP-1/2-50-G-9","1/2-GNSVTA-48",{"$f":"VLOOKUP(L21,$A$3:$B$14,2,FALSE)","v":"A6"},{"$f":"VLOOKUP(M21,$A$17:$B$98,2,FALSE)","v":"38"},"(A6) FP-1/2-50-G-9","(38) 1/2-GNSVTA-48"]
["1-1/2-GUSVGT-814","06",null,"FP-1/2-50-G-9","1/2-GNSVTA-43","A6","40",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43","FP-1/2-50-G-9","1/2-GNSVTA-43",{"$f":"VLOOKUP(L22,$A$3:$B$14,2,FALSE)","v":"A6"},{"$f":"VLOOKUP(M22,$A$17:$B$98,2,FALSE)","v":"40"},"(A6) FP-1/2-50-G-9","(40) 1/2-GNSVTA-43"]
["2-GUSVT-913","07",null,"FP-3/4-21-G-10","3/4-GSVTA-54","B1","41",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54","FP-3/4-21-G-10","3/4-GSVTA-54","B1","41","(B1) FP-3/4-21-G-10","(41) 3/4-GSVTA-54"]
["2-GUSVGT-914","08",null,"FP-3/4-21-G-10","3/4-GNSVTA-54","B1","42",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54","FP-3/4-21-G-10","3/4-GNSVTA-54","B1","42","(B1) FP-3/4-21-G-10","(42) 3/4-GNSVTA-54"]
["1/2-GUSVT-40A","09",null,"FP-3/4-27-G-10","3/4-GSVTA-54","B2","41",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54","FP-3/4-27-G-10","3/4-GSVTA-54","B2","41","(B2) FP-3/4-27-G-10","(41) 3/4-GSVTA-54"]
["1/2-GSVT-45A","10",null,"FP-3/4-21-G-10","3/4-GSVTA-53","B1","43",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53","FP-3/4-21-G-10","3/4-GSVTA-53","B1","43","(B1) FP-3/4-21-G-10","(43) 3/4-GSVTA-53"]
["1/2-GSVT-44A","11",null,"FP-3/4-27-G-10","3/4-GNSVTA-54","B2","42",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54","FP-3/4-27-G-10","3/4-GNSVTA-54","B2","42","(B2) FP-3/4-27-G-10","(42) 3/4-GNSVTA-54"]
["1/2-GSVT-48A","12",null,"FP-3/4-27-G-10","3/4-GSVTA-56","B2","44",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56","FP-3/4-27-G-10","3/4-GSVTA-56","B2","44","(B2) FP-3/4-27-G-10","(44) 3/4-GSVTA-56"]
["1/2-GNSVT-48A","13",null,"FP-3/4-27-G-10","3/4-GSVTA-53","B2","43",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53","FP-3/4-27-G-10","3/4-GSVTA-53","B2","43","(B2) FP-3/4-27-G-10","(43) 3/4-GSVTA-53"]
["3/4-GSVGT-54A","14",null,"FP-3/4-27-G-10","3/4-GNSVTA-56","B2","45",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56","FP-3/4-27-G-10","3/4-GNSVTA-56","B2","45","(B2) FP-3/4-27-G-10","(45) 3/4-GNSVTA-56"]
["3/4-GNSVGT-54A","15",null,"FP-3/4-27-G-10","3/4-GNSVTA-53","B2","46",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53","FP-3/4-27-G-10","3/4-GNSVTA-53","B2","46","(B2) FP-3/4-27-G-10","(46) 3/4-GNSVTA-53"]
["3/4-GSVGT-59A","16",null,"FP-1-27-G-10","1-GSVTA-64","C1","47",null,null,null,"FP-1-27-G-10                                                                                                  1-GSVTA-64","FP-1-27-G-10","1-GSVTA-64","C1","47","(C1) FP-1-27-G-10","(47) 1-GSVTA-64"]
["3/4-GNSVGT-59A","17",null,"FP-1-27-G-10","1-GSVTA-65","C1","48",null,null,null,"FP-1-27-G-10                                                                                                  1-GSVTA-65","FP-1-27-G-10","1-GSVTA-65","C1","48","(C1) FP-1-27-G-10","(48) 1-GSVTA-65"]
["1-GSVGT-64A","18",null,"FP-1-27-G-10","1-GNSVTA-64","C1","49",null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVTA-64","FP-1-27-G-10","1-GNSVTA-64","C1","49","(C1) FP-1-27-G-10","(49) 1-GNSVTA-64"]
["1-GSVGT-68A","19",null,"FP-1-35-G-10","1-GSVTA-64","C2","47",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-64","FP-1-35-G-10","1-GSVTA-64","C2","47","(C2) FP-1-35-G-10","(47) 1-GSVTA-64"]
["1-GNSVGT-64A","20",null,"FP-1-35-G-10","1-GSVTA-65","C2","48",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-65","FP-1-35-G-10","1-GSVTA-65","C2","48","(C2) FP-1-35-G-10","(48) 1-GSVTA-65"]
["1-GNSVGT-68A","21",null,"FP-1-35-G-10","1-GNSVTA-64","C2","49",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-64","FP-1-35-G-10","1-GNSVTA-64","C2","49","(C2) FP-1-35-G-10","(49) 1-GNSVTA-64"]
["1-GSVGT-69A","22",null,"FP-1-35-G-10","1-GSVTA-63","C2","50",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-63","FP-1-35-G-10","1-GSVTA-63",{"$f":"VLOOKUP(L38,$A$3:$B$14,2,FALSE)","v":"C2"},{"$f":"VLOOKUP(M38,$A$17:$B$98,2,FALSE)","v":"50"},"(C2) FP-1-35-G-10","(50) 1-GSVTA-63"]
["1-GNSVGT-69A","23",null,"FP-1-35-G-10","1-GNSVTA-65","C2","52",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-65","FP-1-35-G-10","1-GNSVTA-65",{"$f":"VLOOKUP(L39,$A$3:$B$14,2,FALSE)","v":"C2"},{"$f":"VLOOKUP(M39,$A$17:$B$98,2,FALSE)","v":"52"},"(C2) FP-1-35-G-10","(52) 1-GNSVTA-65"]
["1-1/2-GSVGT-87A","24",null,"FP-1-35-G-10","1-GSVTA-66","C2","51",null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-66","FP-1-35-G-10","1-GSVTA-66","C2","51","(C2) FP-1-35-G-10","(51) 1-GSVTA-66"]
["1-1/2-GSVGT-86A","25",null,"FP-1-35-G-10","1-GNSVTA-66","C2","53",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-66","FP-1-35-G-10","1-GNSVTA-66","C2","53","(C2) FP-1-35-G-10","(53) 1-GNSVTA-66"]
["1-1/2-GNSVGT-87A","26",null,"FP-1-35-G-10","1-GNSVTA-63","C2","54",null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-63","FP-1-35-G-10","1-GNSVTA-63","C2","54","(C2) FP-1-35-G-10","(54) 1-GNSVTA-63"]
["1-1/2-GNSVGT-86A","27",null,"FP-1-1/2-27-G-10","1-1/2-GSVTA-84","D2","55",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84","FP-1-1/2-27-G-10","1-1/2-GSVTA-84","D2","55","(D2) FP-1-1/2-27-G-10","(55) 1-1/2-GSVTA-84"]
["2-GSVGT-97A","28",null,"FP-1-1/2-27-G-10","1-1/2-GSVTA-85","D2","56",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85","FP-1-1/2-27-G-10","1-1/2-GSVTA-85","D2","56","(D2) FP-1-1/2-27-G-10","(56) 1-1/2-GSVTA-85"]
["2-GSVGT-98A","29",null,"FP-1-1/2-27-G-10","1-1/2-GSVTA-83","D2","57",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83","FP-1-1/2-27-G-10","1-1/2-GSVTA-83","D2","57","(D2) FP-1-1/2-27-G-10","(57) 1-1/2-GSVTA-83"]
["2-GNSVGT-97A","30",null,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-84","D2","58",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84","FP-1-1/2-27-G-10","1-1/2-GNSVTA-84","D2","58","(D2) FP-1-1/2-27-G-10","(58) 1-1/2-GNSVTA-84"]
["2-GNSVGT-98A","31",null,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-85","D2","59",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85","FP-1-1/2-27-G-10","1-1/2-GNSVTA-85","D2","59","(D2) FP-1-1/2-27-G-10","(59) 1-1/2-GNSVTA-85"]
["BL-954","32",null,"FP-1-1/2-27-G-10","1-1/2-GNSVTA-83","D2","60",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83","FP-1-1/2-27-G-10","1-1/2-GNSVTA-83","D2","60","(D2) FP-1-1/2-27-G-10","(60) 1-1/2-GNSVTA-83"]
["BL-953","33",null,"FP-2-27-G-10","2-GSVTA-94","E1","61",null,null,null,"FP-2-27-G-10                                                                                                  2-GSVTA-94","FP-2-27-G-10","2-GSVTA-94","E1","61","(E1) FP-2-27-G-10","(61) 2-GSVTA-94"]
["BL-950","34",null,"FP-2-27-G-10","2-GSVTA-93","E1","62",null,null,null,"FP-2-27-G-10                                                                                                  2-GSVTA-93","FP-2-27-G-10","2-GSVTA-93","E1","62","(E1) FP-2-27-G-10","(62) 2-GSVTA-93"]
["BL-951","35",null,"FP-2-27-G-10","2-GNSVTA-94","E1","63",null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-94","FP-2-27-G-10","2-GNSVTA-94","E1","63","(E1) FP-2-27-G-10","(63) 2-GNSVTA-94"]
["1/2-GSVTA-44","36",null,"FP-2-27-G-10","2-GNSVTA-96","E1","64",null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-96","FP-2-27-G-10","2-GNSVTA-96","E1","64","(E1) FP-2-27-G-10","(64) 2-GNSVTA-96"]
["1/2-GSVTA-48","37",null,"FP-2-27-G-10","2-GNSVTA-93","E1","65",null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-93","FP-2-27-G-10","2-GNSVTA-93","E1","65","(E1) FP-2-27-G-10","(65) 2-GNSVTA-93"]
["1/2-GNSVTA-48","38",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4)","v":" FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44"},"FP-1/2-17-G-10","1/2-GSVTA-44","A1","36","(A1) FP-1/2-17-G-10","(36) 1/2-GSVTA-44"]
["1/2-GNSVTA-44","39",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5)","v":" FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48"},"FP-1/2-17-G-10","1/2-GSVTA-48",{"$f":"VLOOKUP(L55,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M55,$A$17:$B$98,2,FALSE)","v":"37"},"(A1) FP-1/2-17-G-10","(37) 1/2-GSVTA-48"]
["1/2-GNSVTA-43","40",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44","FP-1/2-21-G-10","1/2-GSVTA-44",{"$f":"VLOOKUP(L56,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M56,$A$17:$B$98,2,FALSE)","v":"36"},"(A2) FP-1/2-21-G-10","(36) 1/2-GSVTA-44"]
["3/4-GSVTA-54","41",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48","FP-1/2-21-G-10","1/2-GSVTA-48","A2","37","(A2) FP-1/2-21-G-10","(37) 1/2-GSVTA-48"]
["3/4-GNSVTA-54","42",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-17-G-10","1/2-GNSVTA-48","A1","38","(A1) FP-1/2-17-G-10","(38) 1/2-GNSVTA-48"]
["3/4-GSVTA-53","43",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44","FP-1/2-21-G-10","1/2-GNSVTA-44","A2","39","(A2) FP-1/2-21-G-10","(39) 1/2-GNSVTA-44"]
["3/4-GSVTA-56","44",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-21-G-10","1/2-GNSVTA-48","A2","38","(A2) FP-1/2-21-G-10","(38) 1/2-GNSVTA-48"]
["3/4-GNSVTA-56","45",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44","FP-1/2-27-G-10","1/2-GSVTA-44","A3","36","(A3) FP-1/2-27-G-10","(36) 1/2-GSVTA-44"]
["3/4-GNSVTA-53","46",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48","FP-1/2-27-G-10","1/2-GSVTA-48","A3","37","(A3) FP-1/2-27-G-10","(37) 1/2-GSVTA-48"]
["1-GSVTA-64","47",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-27-G-10","1/2-GNSVTA-48","A3","38","(A3) FP-1/2-27-G-10","(38) 1/2-GNSVTA-48"]
["1-GSVTA-65","48",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44","FP-1/2-35-G-10","1/2-GSVTA-44","A4","36","(A4) FP-1/2-35-G-10","(36) 1/2-GSVTA-44"]
["1-GNSVTA-64","49",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48","FP-1/2-35-G-10","1/2-GSVTA-48","A4","37","(A4) FP-1/2-35-G-10","(37) 1/2-GSVTA-48"]
["1-GSVTA-63","50",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43","FP-1/2-27-G-10","1/2-GNSVTA-43","A3","40","(A3) FP-1/2-27-G-10","(40) 1/2-GNSVTA-43"]
["1-GSVTA-66","51",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48","FP-1/2-35-G-10","1/2-GNSVTA-48","A4","38","(A4) FP-1/2-35-G-10","(38) 1/2-GNSVTA-48"]
["1-GNSVTA-65","52",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43","FP-1/2-35-G-10","1/2-GNSVTA-43","A4","40","(A4) FP-1/2-35-G-10","(40) 1/2-GNSVTA-43"]
["1-GNSVTA-66","53",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44","FP-1/2-50-G-9","1/2-GSVTA-44","A6","36",{"$f":"CONCATENATE(\"(\",N69,\")\",\" \",L69)","v":"(A6) FP-1/2-50-G-9"},"(36) 1/2-GSVTA-44"]
["1-GNSVTA-63","54",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48","FP-1/2-50-G-9","1/2-GSVTA-48","A6","37","(A6) FP-1/2-50-G-9","(37) 1/2-GSVTA-48"]
["1-1/2-GSVTA-84","55",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48","FP-1/2-50-G-9","1/2-GNSVTA-48","A6","38","(A6) FP-1/2-50-G-9","(38) 1/2-GNSVTA-48"]
["1-1/2-GSVTA-85","56",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43","FP-1/2-50-G-9","1/2-GNSVTA-43","A6","40","(A6) FP-1/2-50-G-9","(40) 1/2-GNSVTA-43"]
["1-1/2-GSVTA-83","57",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54","FP-3/4-21-G-10","3/4-GSVTA-54","B1","41","(B1) FP-3/4-21-G-10","(41) 3/4-GSVTA-54"]
["1-1/2-GNSVTA-84","58",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54","FP-3/4-21-G-10","3/4-GNSVTA-54","B1","42","(B1) FP-3/4-21-G-10","(42) 3/4-GNSVTA-54"]
["1-1/2-GNSVTA-85","59",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54","FP-3/4-27-G-10","3/4-GSVTA-54","B2","41","(B2) FP-3/4-27-G-10","(41) 3/4-GSVTA-54"]
["1-1/2-GNSVTA-83","60",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53","FP-3/4-21-G-10","3/4-GSVTA-53","B1","43","(B1) FP-3/4-21-G-10","(43) 3/4-GSVTA-53"]
["2-GSVTA-94","61",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54","FP-3/4-27-G-10","3/4-GNSVTA-54","B2","42","(B2) FP-3/4-27-G-10","(42) 3/4-GNSVTA-54"]
["2-GSVTA-93","62",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56","FP-3/4-27-G-10","3/4-GSVTA-56","B2","44","(B2) FP-3/4-27-G-10","(44) 3/4-GSVTA-56"]
["2-GNSVTA-94","63",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53","FP-3/4-27-G-10","3/4-GSVTA-53","B2","43","(B2) FP-3/4-27-G-10","(43) 3/4-GSVTA-53"]
["2-GNSVTA-96","64",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56","FP-3/4-27-G-10","3/4-GNSVTA-56","B2","45","(B2) FP-3/4-27-G-10","(45) 3/4-GNSVTA-56"]
["2-GNSVTA-93","65",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53","FP-3/4-27-G-10","3/4-GNSVTA-53","B2","46","(B2) FP-3/4-27-G-10","(46) 3/4-GNSVTA-53"]
["BS-41","66",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GSVTA-64","FP-1-27-G-10","1-GSVTA-64","C1","47","(C1) FP-1-27-G-10","(47) 1-GSVTA-64"]
["BS-50","67",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GSVTA-65","FP-1-27-G-10","1-GSVTA-65","C1","48","(C1) FP-1-27-G-10","(48) 1-GSVTA-65"]
["BS-62","68",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GNSVTA-64","FP-1-27-G-10","1-GNSVTA-64","C1","49","(C1) FP-1-27-G-10","(49) 1-GNSVTA-64"]
["BS-60","69",null,null,null,{"$f":"VLOOKUP(D85,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(E85,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-64","FP-1-35-G-10","1-GSVTA-64","C2","47","(C2) FP-1-35-G-10","(47) 1-GSVTA-64"]
["BS-80","70",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-65","FP-1-35-G-10","1-GSVTA-65","C2","48","(C2) FP-1-35-G-10","(48) 1-GSVTA-65"]
["BS-90","71",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-64","FP-1-35-G-10","1-GNSVTA-64","C2","49","(C2) FP-1-35-G-10","(49) 1-GNSVTA-64"]
["BS-91","72",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-63","FP-1-35-G-10","1-GSVTA-63","C2","50","(C2) FP-1-35-G-10","(50) 1-GSVTA-63"]
["1/2-GL-471","73",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-65","FP-1-35-G-10","1-GNSVTA-65","C2","52","(C2) FP-1-35-G-10","(52) 1-GNSVTA-65"]
["1/2-GL-410","74",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-66","FP-1-35-G-10","1-GSVTA-66","C2","51","(C2) FP-1-35-G-10","(51) 1-GSVTA-66"]
["3/4-GL-571","75",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-66","FP-1-35-G-10","1-GNSVTA-66","C2","53","(C2) FP-1-35-G-10","(53) 1-GNSVTA-66"]
["3/4-GL-510","76",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-63","FP-1-35-G-10","1-GNSVTA-63","C2","54","(C2) FP-1-35-G-10","(54) 1-GNSVTA-63"]
["1-GL-671","77",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84","FP-1-1/2-27-G-10","1-1/2-GSVTA-84","D2","55","(D2) FP-1-1/2-27-G-10","(55) 1-1/2-GSVTA-84"]
["1-GL-610","78",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85","FP-1-1/2-27-G-10","1-1/2-GSVTA-85","D2","56","(D2) FP-1-1/2-27-G-10","(56) 1-1/2-GSVTA-85"]
["1-1/2-GL-871","79",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83","FP-1-1/2-27-G-10","1-1/2-GSVTA-83","D2","57","(D2) FP-1-1/2-27-G-10","(57) 1-1/2-GSVTA-83"]
["1-1/2-GL-810","80",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84","FP-1-1/2-27-G-10","1-1/2-GNSVTA-84","D2","58","(D2) FP-1-1/2-27-G-10","(58) 1-1/2-GNSVTA-84"]
["2-GL-971","81",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85","FP-1-1/2-27-G-10","1-1/2-GNSVTA-85","D2","59","(D2) FP-1-1/2-27-G-10","(59) 1-1/2-GNSVTA-85"]
["2-GL-910","82",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83","FP-1-1/2-27-G-10","1-1/2-GNSVTA-83","D2","60","(D2) FP-1-1/2-27-G-10","(60) 1-1/2-GNSVTA-83"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVTA-94","FP-2-27-G-10","2-GSVTA-94","E1","61","(E1) FP-2-27-G-10","(61) 2-GSVTA-94"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D50,\"                                                                                                  \",E50)","v":" FP-2-27-G-10                                                                                                  2-GSVTA-93"},"FP-2-27-G-10","2-GSVTA-93","E1","62","(E1) FP-2-27-G-10","(62) 2-GSVTA-93"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVTA-94","FP-2-27-G-10","2-GNSVTA-94","E1","63","(E1) FP-2-27-G-10","(63) 2-GNSVTA-94"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVTA-96","FP-2-27-G-10","2-GNSVTA-96","E1","64","(E1) FP-2-27-G-10","(64) 2-GNSVTA-96"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVTA-93","FP-2-27-G-10","2-GNSVTA-93","E1","65","(E1) FP-2-27-G-10","(65) 2-GNSVTA-93"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4,\" \")","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44 "},"FP-1/2-17-G-10","1/2-GSVTA-44","A1","36","(A1) FP-1/2-17-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5,\" \")","v":"FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48 "},"FP-1/2-17-G-10","1/2-GSVTA-48","A1","37","(A1) FP-1/2-17-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44 ","FP-1/2-21-G-10","1/2-GSVTA-44","A2","36","(A2) FP-1/2-21-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48 ","FP-1/2-21-G-10","1/2-GSVTA-48","A2","37","(A2) FP-1/2-21-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-17-G-10","1/2-GNSVTA-48","A1","38","(A1) FP-1/2-17-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44 ","FP-1/2-21-G-10","1/2-GNSVTA-44","A2","39","(A2) FP-1/2-21-G-10","(39) 1/2-GNSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-21-G-10","1/2-GNSVTA-48","A2","38","(A2) FP-1/2-21-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44 ","FP-1/2-27-G-10","1/2-GSVTA-44","A3","36","(A3) FP-1/2-27-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48 ","FP-1/2-27-G-10","1/2-GSVTA-48","A3","37","(A3) FP-1/2-27-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-27-G-10","1/2-GNSVTA-48","A3","38","(A3) FP-1/2-27-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44 ","FP-1/2-35-G-10","1/2-GSVTA-44","A4","36","(A4) FP-1/2-35-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48 ","FP-1/2-35-G-10","1/2-GSVTA-48","A4","37","(A4) FP-1/2-35-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43 ","FP-1/2-27-G-10","1/2-GNSVTA-43","A3","40","(A3) FP-1/2-27-G-10","(40) 1/2-GNSVTA-43"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-35-G-10","1/2-GNSVTA-48","A4","38","(A4) FP-1/2-35-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43 ","FP-1/2-35-G-10","1/2-GNSVTA-43","A4","40","(A4) FP-1/2-35-G-10","(40) 1/2-GNSVTA-43"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44 ","FP-1/2-50-G-9","1/2-GSVTA-44","A6","36","(A6) FP-1/2-50-G-9","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48 ","FP-1/2-50-G-9","1/2-GSVTA-48",{"$f":"VLOOKUP(L120,$A$3:$B$14,2,FALSE)","v":"A6"},{"$f":"VLOOKUP(M120,$A$17:$B$98,2,FALSE)","v":"37"},"(A6) FP-1/2-50-G-9","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48 ","FP-1/2-50-G-9","1/2-GNSVTA-48","A6","38","(A6) FP-1/2-50-G-9","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43 ","FP-1/2-50-G-9","1/2-GNSVTA-43","A6","40","(A6) FP-1/2-50-G-9","(40) 1/2-GNSVTA-43"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54 ","FP-3/4-21-G-10","3/4-GSVTA-54","B1","41","(B1) FP-3/4-21-G-10","(41) 3/4-GSVTA-54"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54 ","FP-3/4-21-G-10","3/4-GNSVTA-54","B1","42","(B1) FP-3/4-21-G-10","(42) 3/4-GNSVTA-54"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54 ","FP-3/4-27-G-10","3/4-GSVTA-54","B2","41","(B2) FP-3/4-27-G-10","(41) 3/4-GSVTA-54"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53 ","FP-3/4-21-G-10","3/4-GSVTA-53","B1","43","(B1) FP-3/4-21-G-10","(43) 3/4-GSVTA-53"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54 ","FP-3/4-27-G-10","3/4-GNSVTA-54","B2","42","(B2) FP-3/4-27-G-10","(42) 3/4-GNSVTA-54"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56 ","FP-3/4-27-G-10","3/4-GSVTA-56","B2","44","(B2) FP-3/4-27-G-10","(44) 3/4-GSVTA-56"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53 ","FP-3/4-27-G-10","3/4-GSVTA-53","B2","43","(B2) FP-3/4-27-G-10","(43) 3/4-GSVTA-53"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56 ","FP-3/4-27-G-10","3/4-GNSVTA-56","B2","45","(B2) FP-3/4-27-G-10","(45) 3/4-GNSVTA-56"]
[null,null,null,null,null,null,null,null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53 ","FP-3/4-27-G-10","3/4-GNSVTA-53","B2","46","(B2) FP-3/4-27-G-10","(46) 3/4-GNSVTA-53"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GSVTA-64 ","FP-1-27-G-10","1-GSVTA-64","C1","47","(C1) FP-1-27-G-10","(47) 1-GSVTA-64"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GSVTA-65 ","FP-1-27-G-10","1-GSVTA-65","C1","48",{"$f":"CONCATENATE(\"(\",N133,\")\",\" \",L133)","v":"(C1) FP-1-27-G-10"},"(48) 1-GSVTA-65"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-27-G-10                                                                                                  1-GNSVTA-64 ","FP-1-27-G-10","1-GNSVTA-64","C1","49","(C1) FP-1-27-G-10","(49) 1-GNSVTA-64"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-64 ","FP-1-35-G-10","1-GSVTA-64","C2","47","(C2) FP-1-35-G-10","(47) 1-GSVTA-64"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-65 ","FP-1-35-G-10","1-GSVTA-65","C2","48","(C2) FP-1-35-G-10","(48) 1-GSVTA-65"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-64 ","FP-1-35-G-10","1-GNSVTA-64","C2","49","(C2) FP-1-35-G-10","(49) 1-GNSVTA-64"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-63 ","FP-1-35-G-10","1-GSVTA-63","C2","50","(C2) FP-1-35-G-10","(50) 1-GSVTA-63"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-65 ","FP-1-35-G-10","1-GNSVTA-65","C2","52","(C2) FP-1-35-G-10","(52) 1-GNSVTA-65"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GSVTA-66 ","FP-1-35-G-10","1-GSVTA-66","C2","51","(C2) FP-1-35-G-10","(51) 1-GSVTA-66"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-66 ","FP-1-35-G-10","1-GNSVTA-66","C2","53","(C2) FP-1-35-G-10","(53) 1-GNSVTA-66"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-35-G-10                                                                                                  1-GNSVTA-63 ","FP-1-35-G-10","1-GNSVTA-63","C2","54","(C2) FP-1-35-G-10","(54) 1-GNSVTA-63"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84 ","FP-1-1/2-27-G-10","1-1/2-GSVTA-84","D2","55","(D2) FP-1-1/2-27-G-10","(55) 1-1/2-GSVTA-84"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85 ","FP-1-1/2-27-G-10","1-1/2-GSVTA-85","D2","56","(D2) FP-1-1/2-27-G-10","(56) 1-1/2-GSVTA-85"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83 ","FP-1-1/2-27-G-10","1-1/2-GSVTA-83","D2","57","(D2) FP-1-1/2-27-G-10","(57) 1-1/2-GSVTA-83"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84 ","FP-1-1/2-27-G-10","1-1/2-GNSVTA-84","D2","58","(D2) FP-1-1/2-27-G-10","(58) 1-1/2-GNSVTA-84"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85 ","FP-1-1/2-27-G-10","1-1/2-GNSVTA-85","D2","59","(D2) FP-1-1/2-27-G-10","(59) 1-1/2-GNSVTA-85"]
[null,null,null,null,null,null,null,null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83 ","FP-1-1/2-27-G-10","1-1/2-GNSVTA-83","D2","60","(D2) FP-1-1/2-27-G-10","(60) 1-1/2-GNSVTA-83"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GSVTA-94 ","FP-2-27-G-10","2-GSVTA-94","E1","61","(E1) FP-2-27-G-10","(61) 2-GSVTA-94"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GSVTA-93 ","FP-2-27-G-10","2-GSVTA-93","E1","62","(E1) FP-2-27-G-10","(62) 2-GSVTA-93"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-94 ","FP-2-27-G-10","2-GNSVTA-94","E1","63","(E1) FP-2-27-G-10","(63) 2-GNSVTA-94"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-96 ","FP-2-27-G-10","2-GNSVTA-96","E1","64","(E1) FP-2-27-G-10","(64) 2-GNSVTA-96"]
[null,null,null,null,null,null,null,null,null,null,"FP-2-27-G-10                                                                                                  2-GNSVTA-93 ","FP-2-27-G-10","2-GNSVTA-93","E1","65","(E1) FP-2-27-G-10","(65) 2-GNSVTA-93"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4,\" \")","v":" FP-1/2-17-G-10                                                                                                  1/2-GSVTA-44 "},"FP-1/2-17-G-10","1/2-GSVTA-44","A1","36","(A1) FP-1/2-17-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5,\" \")","v":" FP-1/2-17-G-10                                                                                                  1/2-GSVTA-48 "},"FP-1/2-17-G-10","1/2-GSVTA-48","A1","37",{"$f":"CONCATENATE(\"(\",N155,\")\",\" \",L155)","v":"(A1) FP-1/2-17-G-10"},"(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVTA-44 ","FP-1/2-21-G-10","1/2-GSVTA-44","A2","36","(A2) FP-1/2-21-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GSVTA-48 ","FP-1/2-21-G-10","1/2-GSVTA-48","A2","37","(A2) FP-1/2-21-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-17-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-17-G-10","1/2-GNSVTA-48","A1","38","(A1) FP-1/2-17-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-44 ","FP-1/2-21-G-10","1/2-GNSVTA-44","A2","39","(A2) FP-1/2-21-G-10","(39) 1/2-GNSVTA-44"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-21-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-21-G-10","1/2-GNSVTA-48","A2","38","(A2) FP-1/2-21-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVTA-44 ","FP-1/2-27-G-10","1/2-GSVTA-44","A3","36","(A3) FP-1/2-27-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GSVTA-48 ","FP-1/2-27-G-10","1/2-GSVTA-48","A3","37","(A3) FP-1/2-27-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-27-G-10","1/2-GNSVTA-48","A3","38","(A3) FP-1/2-27-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVTA-44 ","FP-1/2-35-G-10","1/2-GSVTA-44","A4","36","(A4) FP-1/2-35-G-10","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GSVTA-48 ","FP-1/2-35-G-10","1/2-GSVTA-48","A4","37","(A4) FP-1/2-35-G-10","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GNSVTA-43 ","FP-1/2-27-G-10","1/2-GNSVTA-43","A3","40","(A3) FP-1/2-27-G-10","(40) 1/2-GNSVTA-43"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-48 ","FP-1/2-35-G-10","1/2-GNSVTA-48","A4","38","(A4) FP-1/2-35-G-10","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GNSVTA-43 ","FP-1/2-35-G-10","1/2-GNSVTA-43","A4","40","(A4) FP-1/2-35-G-10","(40) 1/2-GNSVTA-43"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVTA-44 ","FP-1/2-50-G-9","1/2-GSVTA-44","A6","36","(A6) FP-1/2-50-G-9","(36) 1/2-GSVTA-44"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GSVTA-48 ","FP-1/2-50-G-9","1/2-GSVTA-48","A6","37","(A6) FP-1/2-50-G-9","(37) 1/2-GSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-48 ","FP-1/2-50-G-9","1/2-GNSVTA-48","A6","38","(A6) FP-1/2-50-G-9","(38) 1/2-GNSVTA-48"]
[null,null,null,null,null,null,null,null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GNSVTA-43 ","FP-1/2-50-G-9","1/2-GNSVTA-43","A6","40","(A6) FP-1/2-50-G-9","(40) 1/2-GNSVTA-43"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVTA-54 ","FP-3/4-21-G-10","3/4-GSVTA-54","B1","41","(B1) FP-3/4-21-G-10","(41) 3/4-GSVTA-54"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GNSVTA-54 ","FP-3/4-21-G-10","3/4-GNSVTA-54","B1","42","(B1) FP-3/4-21-G-10","(42) 3/4-GNSVTA-54"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVTA-54 ","FP-3/4-27-G-10","3/4-GSVTA-54","B2","41","(B2) FP-3/4-27-G-10","(41) 3/4-GSVTA-54"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GSVTA-53 ","FP-3/4-21-G-10","3/4-GSVTA-53","B1","43","(B1) FP-3/4-21-G-10","(43) 3/4-GSVTA-53"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-54 ","FP-3/4-27-G-10","3/4-GNSVTA-54","B2","42","(B2) FP-3/4-27-G-10","(42) 3/4-GNSVTA-54"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVTA-56 ","FP-3/4-27-G-10","3/4-GSVTA-56","B2","44","(B2) FP-3/4-27-G-10","(44) 3/4-GSVTA-56"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GSVTA-53 ","FP-3/4-27-G-10","3/4-GSVTA-53","B2","43","(B2) FP-3/4-27-G-10","(43) 3/4-GSVTA-53"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-56 ","FP-3/4-27-G-10","3/4-GNSVTA-56","B2","45","(B2) FP-3/4-27-G-10","(45) 3/4-GNSVTA-56"]
[null,null,null,null,null,null,null,null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GNSVTA-53 ","FP-3/4-27-G-10","3/4-GNSVTA-53","B2","46","(B2) FP-3/4-27-G-10","(46) 3/4-GNSVTA-53"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GSVTA-64 ","FP-1-27-G-10","1-GSVTA-64","C1","47","(C1) FP-1-27-G-10","(47) 1-GSVTA-64"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GSVTA-65 ","FP-1-27-G-10","1-GSVTA-65","C1","48","(C1) FP-1-27-G-10","(48) 1-GSVTA-65"]
[null,null,null,null,null,null,null,null,null,null," FP-1-27-G-10                                                                                                  1-GNSVTA-64 ","FP-1-27-G-10","1-GNSVTA-64",{"$f":"VLOOKUP(L184,$A$3:$B$14,2,FALSE)","v":"C1"},{"$f":"VLOOKUP(M184,$A$17:$B$98,2,FALSE)","v":"49"},"(C1) FP-1-27-G-10","(49) 1-GNSVTA-64"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-64 ","FP-1-35-G-10","1-GSVTA-64","C2","47","(C2) FP-1-35-G-10","(47) 1-GSVTA-64"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-65 ","FP-1-35-G-10","1-GSVTA-65","C2","48","(C2) FP-1-35-G-10","(48) 1-GSVTA-65"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-64 ","FP-1-35-G-10","1-GNSVTA-64","C2","49","(C2) FP-1-35-G-10","(49) 1-GNSVTA-64"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-63 ","FP-1-35-G-10","1-GSVTA-63","C2","50","(C2) FP-1-35-G-10","(50) 1-GSVTA-63"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-65 ","FP-1-35-G-10","1-GNSVTA-65","C2","52","(C2) FP-1-35-G-10","(52) 1-GNSVTA-65"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GSVTA-66 ","FP-1-35-G-10","1-GSVTA-66","C2","51","(C2) FP-1-35-G-10","(51) 1-GSVTA-66"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-66 ","FP-1-35-G-10","1-GNSVTA-66","C2","53","(C2) FP-1-35-G-10","(53) 1-GNSVTA-66"]
[null,null,null,null,null,null,null,null,null,null," FP-1-35-G-10                                                                                                  1-GNSVTA-63 ","FP-1-35-G-10","1-GNSVTA-63","C2","54","(C2) FP-1-35-G-10","(54) 1-GNSVTA-63"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-84 ","FP-1-1/2-27-G-10","1-1/2-GSVTA-84","D2","55","(D2) FP-1-1/2-27-G-10","(55) 1-1/2-GSVTA-84"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-85 ","FP-1-1/2-27-G-10","1-1/2-GSVTA-85","D2","56","(D2) FP-1-1/2-27-G-10","(56) 1-1/2-GSVTA-85"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GSVTA-83 ","FP-1-1/2-27-G-10","1-1/2-GSVTA-83","D2","57","(D2) FP-1-1/2-27-G-10","(57) 1-1/2-GSVTA-83"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-84 ","FP-1-1/2-27-G-10","1-1/2-GNSVTA-84","D2","58","(D2) FP-1-1/2-27-G-10","(58) 1-1/2-GNSVTA-84"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-85 ","FP-1-1/2-27-G-10","1-1/2-GNSVTA-85","D2","59","(D2) FP-1-1/2-27-G-10","(59) 1-1/2-GNSVTA-85"]
[null,null,null,null,null,null,null,null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GNSVTA-83 ","FP-1-1/2-27-G-10","1-1/2-GNSVTA-83","D2","60","(D2) FP-1-1/2-27-G-10","(60) 1-1/2-GNSVTA-83"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVTA-94 ","FP-2-27-G-10","2-GSVTA-94","E1","61","(E1) FP-2-27-G-10","(61) 2-GSVTA-94"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GSVTA-93 ","FP-2-27-G-10","2-GSVTA-93","E1","62","(E1) FP-2-27-G-10","(62) 2-GSVTA-93"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVTA-94 ","FP-2-27-G-10","2-GNSVTA-94","E1","63","(E1) FP-2-27-G-10","(63) 2-GNSVTA-94"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVTA-96 ","FP-2-27-G-10","2-GNSVTA-96","E1","64","(E1) FP-2-27-G-10","(64) 2-GNSVTA-96"]
[null,null,null,null,null,null,null,null,null,null," FP-2-27-G-10                                                                                                  2-GNSVTA-93 ","FP-2-27-G-10","2-GNSVTA-93","E1","65","(E1) FP-2-27-G-10","(65) 2-GNSVTA-93"]

{"sheet":"10A45 Naming TA","index":54,"n_rows":203,"n_cols":17,"rows_kept":203,"cut":false,"hidden":true,"merged":[[2,2,2,8]]}
[]
[]
["FP-1/2-17-G-10","A1","TA Floats",null,null,null,null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["FP-1/2-21-G-10","A2",null,"FP-1/2-17-G-10","BS-41",{"$f":"VLOOKUP(D4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E4,$A$17:$B$98,2,FALSE)","v":"66"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4)","v":"FP-1/2-17-G-10                                                                                                  BS-41"},"FP-1/2-17-G-10","BS-41",{"$f":"VLOOKUP(L4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M4,$A$17:$B$98,2,FALSE)","v":"66"},{"$f":"CONCATENATE(\"(\",N4,\")\",\" \",L4)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O4,\")\",\" \",M4)","v":"(66) BS-41"}]
["FP-1/2-27-G-10","A3",null,"FP-1/2-21-G-10","BS-41",{"$f":"VLOOKUP(D5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(E5,$A$17:$B$98,2,FALSE)","v":"66"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5)","v":"FP-1/2-21-G-10                                                                                                  BS-41"},"FP-1/2-21-G-10","BS-41",{"$f":"VLOOKUP(L5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M5,$A$17:$B$98,2,FALSE)","v":"66"},{"$f":"CONCATENATE(\"(\",N5,\")\",\" \",L5)","v":"(A2) FP-1/2-21-G-10"},"(66) BS-41"]
["FP-1/2-35-G-10","A4",null,"FP-1/2-27-G-10","BS-41","A3","66",null,null,null,"FP-1/2-27-G-10                                                                                                  BS-41","FP-1/2-27-G-10","BS-41","A3","66","(A3) FP-1/2-27-G-10","(66) BS-41"]
["FP-1/2-50-G-9","A6",null,"FP-1/2-35-G-10","BS-41","A4","66",null,null,null,"FP-1/2-35-G-10                                                                                                  BS-41","FP-1/2-35-G-10","BS-41","A4","66","(A4) FP-1/2-35-G-10","(66) BS-41"]
["FP-3/4-21-G-10","B1",null,"FP-1/2-50-G-9","BS-41","A6","66",null,null,null,"FP-1/2-50-G-9                                                                                                  BS-41","FP-1/2-50-G-9","BS-41","A6","66","(A6) FP-1/2-50-G-9","(66) BS-41"]
["FP-3/4-27-G-10","B2",null,"FP-3/4-21-G-10","BS-50","B1","67",null,null,null,"FP-3/4-21-G-10                                                                                                  BS-50","FP-3/4-21-G-10","BS-50","B1","67","(B1) FP-3/4-21-G-10","(67) BS-50"]
["FP-1-27-G-10","C1",null,"FP-3/4-27-G-10","BS-50","B2","67",null,null,null,"FP-3/4-27-G-10                                                                                                  BS-50","FP-3/4-27-G-10","BS-50","B2","67","(B2) FP-3/4-27-G-10","(67) BS-50"]
["FP-1-35-G-10","C2",null,"FP-1-27-G-10","BS-62","C1","68",null,null,null,"FP-1-27-G-10                                                                                                  BS-62","FP-1-27-G-10","BS-62","C1","68","(C1) FP-1-27-G-10","(68) BS-62"]
["FP-1-1/2-21-G-10","D1",null,"FP-1-27-G-10","BS-60","C1","69",null,null,null,"FP-1-27-G-10                                                                                                  BS-60","FP-1-27-G-10","BS-60","C1","69","(C1) FP-1-27-G-10","(69) BS-60"]
["FP-1-1/2-27-G-10","D2",null,"FP-1-35-G-10","BS-62","C2","68",null,null,null,"FP-1-35-G-10                                                                                                  BS-62","FP-1-35-G-10","BS-62","C2","68","(C2) FP-1-35-G-10","(68) BS-62"]
["FP-2-27-G-10","E1",null,"FP-1-35-G-10","BS-60","C2","69",null,null,null,"FP-1-35-G-10                                                                                                  BS-60","FP-1-35-G-10","BS-60","C2","69","(C2) FP-1-35-G-10","(69) BS-60"]
[null,null,null,"FP-1-1/2-21-G-10","BS-80","D1","70",null,null,null,"FP-1-1/2-21-G-10                                                                                                  BS-80","FP-1-1/2-21-G-10","BS-80","D1","70","(D1) FP-1-1/2-21-G-10","(70) BS-80"]
[null,null,null,"FP-1-1/2-27-G-10","BS-80","D2","70",null,null,null,"FP-1-1/2-27-G-10                                                                                                  BS-80","FP-1-1/2-27-G-10","BS-80","D2","70","(D2) FP-1-1/2-27-G-10","(70) BS-80"]
["1/2-GUSVT-410","01",null,"FP-2-27-G-10","BS-90","E1","71",null,null,null,"FP-2-27-G-10                                                                                                  BS-90","FP-2-27-G-10","BS-90","E1","71","(E1) FP-2-27-G-10","(71) BS-90"]
["3/4-GUSVT-510","02",null,"FP-2-27-G-10","BS-91","E1","72",null,null,null,"FP-2-27-G-10                                                                                                  BS-91","FP-2-27-G-10","BS-91","E1","72","(E1) FP-2-27-G-10","(72) BS-91"]
["1-GUSVT-611","03",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4)","v":" FP-1/2-17-G-10                                                                                                  BS-41"},"FP-1/2-17-G-10","BS-41","A1","66","(A1) FP-1/2-17-G-10","(66) BS-41"]
["1-GUSVT-610","04",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5)","v":" FP-1/2-21-G-10                                                                                                  BS-41"},"FP-1/2-21-G-10","BS-41","A2","66","(A2) FP-1/2-21-G-10","(66) BS-41"]
["1-1/2-GUSVT-867","05",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  BS-41","FP-1/2-27-G-10","BS-41",{"$f":"VLOOKUP(L21,$A$3:$B$14,2,FALSE)","v":"A3"},{"$f":"VLOOKUP(M21,$A$17:$B$98,2,FALSE)","v":"66"},"(A3) FP-1/2-27-G-10","(66) BS-41"]
["1-1/2-GUSVGT-814","06",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  BS-41","FP-1/2-35-G-10","BS-41",{"$f":"VLOOKUP(L22,$A$3:$B$14,2,FALSE)","v":"A4"},{"$f":"VLOOKUP(M22,$A$17:$B$98,2,FALSE)","v":"66"},"(A4) FP-1/2-35-G-10","(66) BS-41"]
["2-GUSVT-913","07",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  BS-41","FP-1/2-50-G-9","BS-41","A6","66","(A6) FP-1/2-50-G-9","(66) BS-41"]
["2-GUSVGT-914","08",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  BS-50","FP-3/4-21-G-10","BS-50","B1","67","(B1) FP-3/4-21-G-10","(67) BS-50"]
["1/2-GUSVT-40A","09",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  BS-50","FP-3/4-27-G-10","BS-50","B2","67","(B2) FP-3/4-27-G-10","(67) BS-50"]
["1/2-GSVT-45A","10",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  BS-62","FP-1-27-G-10","BS-62","C1","68","(C1) FP-1-27-G-10","(68) BS-62"]
["1/2-GSVT-44A","11",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  BS-60","FP-1-27-G-10","BS-60","C1","69","(C1) FP-1-27-G-10","(69) BS-60"]
["1/2-GSVT-48A","12",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  BS-62","FP-1-35-G-10","BS-62","C2","68","(C2) FP-1-35-G-10","(68) BS-62"]
["1/2-GNSVT-48A","13",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  BS-60","FP-1-35-G-10","BS-60","C2","69","(C2) FP-1-35-G-10","(69) BS-60"]
["3/4-GSVGT-54A","14",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-21-G-10                                                                                                  BS-80","FP-1-1/2-21-G-10","BS-80","D1","70","(D1) FP-1-1/2-21-G-10","(70) BS-80"]
["3/4-GNSVGT-54A","15",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  BS-80","FP-1-1/2-27-G-10","BS-80","D2","70","(D2) FP-1-1/2-27-G-10","(70) BS-80"]
["3/4-GSVGT-59A","16",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  BS-90","FP-2-27-G-10","BS-90","E1","71","(E1) FP-2-27-G-10","(71) BS-90"]
["3/4-GNSVGT-59A","17",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  BS-91","FP-2-27-G-10","BS-91","E1","72","(E1) FP-2-27-G-10","(72) BS-91"]
["1-GSVGT-64A","18",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4,\" \")","v":"FP-1/2-17-G-10                                                                                                  BS-41 "},"FP-1/2-17-G-10","BS-41","A1","66","(A1) FP-1/2-17-G-10","(66) BS-41"]
["1-GSVGT-68A","19",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5,\" \")","v":"FP-1/2-21-G-10                                                                                                  BS-41 "},"FP-1/2-21-G-10","BS-41","A2","66","(A2) FP-1/2-21-G-10","(66) BS-41"]
["1-GNSVGT-64A","20",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-27-G-10                                                                                                  BS-41 ","FP-1/2-27-G-10","BS-41","A3","66","(A3) FP-1/2-27-G-10","(66) BS-41"]
["1-GNSVGT-68A","21",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-35-G-10                                                                                                  BS-41 ","FP-1/2-35-G-10","BS-41","A4","66","(A4) FP-1/2-35-G-10","(66) BS-41"]
["1-GSVGT-69A","22",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-50-G-9                                                                                                  BS-41 ","FP-1/2-50-G-9","BS-41",{"$f":"VLOOKUP(L38,$A$3:$B$14,2,FALSE)","v":"A6"},{"$f":"VLOOKUP(M38,$A$17:$B$98,2,FALSE)","v":"66"},"(A6) FP-1/2-50-G-9","(66) BS-41"]
["1-GNSVGT-69A","23",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-3/4-21-G-10                                                                                                  BS-50 ","FP-3/4-21-G-10","BS-50",{"$f":"VLOOKUP(L39,$A$3:$B$14,2,FALSE)","v":"B1"},{"$f":"VLOOKUP(M39,$A$17:$B$98,2,FALSE)","v":"67"},"(B1) FP-3/4-21-G-10","(67) BS-50"]
["1-1/2-GSVGT-87A","24",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-3/4-27-G-10                                                                                                  BS-50 ","FP-3/4-27-G-10","BS-50","B2","67","(B2) FP-3/4-27-G-10","(67) BS-50"]
["1-1/2-GSVGT-86A","25",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-27-G-10                                                                                                  BS-62 ","FP-1-27-G-10","BS-62","C1","68","(C1) FP-1-27-G-10","(68) BS-62"]
["1-1/2-GNSVGT-87A","26",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-27-G-10                                                                                                  BS-60 ","FP-1-27-G-10","BS-60","C1","69","(C1) FP-1-27-G-10","(69) BS-60"]
["1-1/2-GNSVGT-86A","27",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-35-G-10                                                                                                  BS-62 ","FP-1-35-G-10","BS-62","C2","68","(C2) FP-1-35-G-10","(68) BS-62"]
["2-GSVGT-97A","28",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-35-G-10                                                                                                  BS-60 ","FP-1-35-G-10","BS-60","C2","69","(C2) FP-1-35-G-10","(69) BS-60"]
["2-GSVGT-98A","29",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-1/2-21-G-10                                                                                                  BS-80 ","FP-1-1/2-21-G-10","BS-80","D1","70","(D1) FP-1-1/2-21-G-10","(70) BS-80"]
["2-GNSVGT-97A","30",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-1/2-27-G-10                                                                                                  BS-80 ","FP-1-1/2-27-G-10","BS-80","D2","70","(D2) FP-1-1/2-27-G-10","(70) BS-80"]
["2-GNSVGT-98A","31",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-2-27-G-10                                                                                                  BS-90 ","FP-2-27-G-10","BS-90","E1","71","(E1) FP-2-27-G-10","(71) BS-90"]
["BL-954","32",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-2-27-G-10                                                                                                  BS-91 ","FP-2-27-G-10","BS-91","E1","72","(E1) FP-2-27-G-10","(72) BS-91"]
["BL-953","33",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4,\" \")","v":" FP-1/2-17-G-10                                                                                                  BS-41 "},"FP-1/2-17-G-10","BS-41","A1","66","(A1) FP-1/2-17-G-10","(66) BS-41"]
["BL-950","34",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5,\" \")","v":" FP-1/2-21-G-10                                                                                                  BS-41 "},"FP-1/2-21-G-10","BS-41","A2","66","(A2) FP-1/2-21-G-10","(66) BS-41"]
["BL-951","35",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  BS-41 ","FP-1/2-27-G-10","BS-41","A3","66","(A3) FP-1/2-27-G-10","(66) BS-41"]
["1/2-GSVTA-44","36",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  BS-41 ","FP-1/2-35-G-10","BS-41","A4","66","(A4) FP-1/2-35-G-10","(66) BS-41"]
["1/2-GSVTA-48","37",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  BS-41 ","FP-1/2-50-G-9","BS-41","A6","66","(A6) FP-1/2-50-G-9","(66) BS-41"]
["1/2-GNSVTA-48","38",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  BS-50 ","FP-3/4-21-G-10","BS-50","B1","67","(B1) FP-3/4-21-G-10","(67) BS-50"]
["1/2-GNSVTA-44","39",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  BS-50 ","FP-3/4-27-G-10","BS-50",{"$f":"VLOOKUP(L55,$A$3:$B$14,2,FALSE)","v":"B2"},{"$f":"VLOOKUP(M55,$A$17:$B$98,2,FALSE)","v":"67"},"(B2) FP-3/4-27-G-10","(67) BS-50"]
["1/2-GNSVTA-43","40",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  BS-62 ","FP-1-27-G-10","BS-62",{"$f":"VLOOKUP(L56,$A$3:$B$14,2,FALSE)","v":"C1"},{"$f":"VLOOKUP(M56,$A$17:$B$98,2,FALSE)","v":"68"},"(C1) FP-1-27-G-10","(68) BS-62"]
["3/4-GSVTA-54","41",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  BS-60 ","FP-1-27-G-10","BS-60","C1","69","(C1) FP-1-27-G-10","(69) BS-60"]
["3/4-GNSVTA-54","42",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  BS-62 ","FP-1-35-G-10","BS-62","C2","68","(C2) FP-1-35-G-10","(68) BS-62"]
["3/4-GSVTA-53","43",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  BS-60 ","FP-1-35-G-10","BS-60","C2","69","(C2) FP-1-35-G-10","(69) BS-60"]
["3/4-GSVTA-56","44",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-21-G-10                                                                                                  BS-80 ","FP-1-1/2-21-G-10","BS-80","D1","70","(D1) FP-1-1/2-21-G-10","(70) BS-80"]
["3/4-GNSVTA-56","45",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  BS-80 ","FP-1-1/2-27-G-10","BS-80","D2","70","(D2) FP-1-1/2-27-G-10","(70) BS-80"]
["3/4-GNSVTA-53","46",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  BS-90 ","FP-2-27-G-10","BS-90","E1","71","(E1) FP-2-27-G-10","(71) BS-90"]
["1-GSVTA-64","47",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  BS-91 ","FP-2-27-G-10","BS-91","E1","72","(E1) FP-2-27-G-10","(72) BS-91"]
["1-GSVTA-65","48",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-64","49",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-63","50",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-66","51",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-65","52",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-66","53",null,null,null,{"$f":"VLOOKUP(D69,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(E69,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N69,\")\",\" \",L69)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
["1-GNSVTA-63","54",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-84","55",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-85","56",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-83","57",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-84","58",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-85","59",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-83","60",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVTA-94","61",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVTA-93","62",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-94","63",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-96","64",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-93","65",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-41","66",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-50","67",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-62","68",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-60","69",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-80","70",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-90","71",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-91","72",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GL-471","73",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GL-410","74",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GL-571","75",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GL-510","76",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GL-671","77",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GL-610","78",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GL-871","79",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GL-810","80",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GL-971","81",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GL-910","82",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L120,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M120,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N133,\")\",\" \",L133)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N155,\")\",\" \",L155)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L184,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M184,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]

{"sheet":"10A45 Naming PTFE","index":55,"n_rows":203,"n_cols":17,"rows_kept":203,"cut":false,"hidden":true,"merged":[[2,2,2,8]]}
[]
[]
["FP-1/2-17-G-10","A1","PTFE Floats",null,null,null,null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["FP-1/2-21-G-10","A2",null,"FP-1/2-17-G-10","1/2-GL-471",{"$f":"VLOOKUP(D4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E4,$A$17:$B$98,2,FALSE)","v":"73"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GL-471"},"FP-1/2-17-G-10","1/2-GL-471",{"$f":"VLOOKUP(L4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M4,$A$17:$B$98,2,FALSE)","v":"73"},{"$f":"CONCATENATE(\"(\",N4,\")\",\" \",L4)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O4,\")\",\" \",M4)","v":"(73) 1/2-GL-471"}]
["FP-1/2-27-G-10","A3",null,"FP-1/2-21-G-10","1/2-GL-471",{"$f":"VLOOKUP(D5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(E5,$A$17:$B$98,2,FALSE)","v":"73"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5)","v":"FP-1/2-21-G-10                                                                                                  1/2-GL-471"},"FP-1/2-21-G-10","1/2-GL-471",{"$f":"VLOOKUP(L5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M5,$A$17:$B$98,2,FALSE)","v":"73"},{"$f":"CONCATENATE(\"(\",N5,\")\",\" \",L5)","v":"(A2) FP-1/2-21-G-10"},"(73) 1/2-GL-471"]
["FP-1/2-35-G-10","A4",null,"FP-1/2-27-G-10","1/2-GL-471","A3","73",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GL-471","FP-1/2-27-G-10","1/2-GL-471","A3","73","(A3) FP-1/2-27-G-10","(73) 1/2-GL-471"]
["FP-1/2-50-G-9","A6",null,"FP-1/2-35-G-10","1/2-GL-471","A4","73",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GL-471","FP-1/2-35-G-10","1/2-GL-471","A4","73","(A4) FP-1/2-35-G-10","(73) 1/2-GL-471"]
["FP-3/4-21-G-10","B1",null,"FP-1/2-50-G-9","1/2-GL-471","A6","73",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GL-471","FP-1/2-50-G-9","1/2-GL-471","A6","73","(A6) FP-1/2-50-G-9","(73) 1/2-GL-471"]
["FP-3/4-27-G-10","B2",null,"FP-3/4-21-G-10","3/4-GL-571","B1","75",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GL-571","FP-3/4-21-G-10","3/4-GL-571","B1","75","(B1) FP-3/4-21-G-10","(75) 3/4-GL-571"]
["FP-1-27-G-10","C1",null,"FP-1-27-G-10","1-GL-671","C1","77",null,null,null,"FP-1-27-G-10                                                                                                  1-GL-671","FP-1-27-G-10","1-GL-671","C1","77","(C1) FP-1-27-G-10","(77) 1-GL-671"]
["FP-1-35-G-10","C2",null,"FP-1-1/2-21-G-10","1-1/2-GL-871","D1","79",null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-871","FP-1-1/2-21-G-10","1-1/2-GL-871","D1","79","(D1) FP-1-1/2-21-G-10","(79) 1-1/2-GL-871"]
["FP-1-1/2-21-G-10","D1",null,"FP-1-1/2-27-G-10","1-1/2-GL-871","D2","79",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-871","FP-1-1/2-27-G-10","1-1/2-GL-871","D2","79","(D2) FP-1-1/2-27-G-10","(79) 1-1/2-GL-871"]
["FP-1-1/2-27-G-10","D2",null,"FP-2-27-G-10","2-GL-971","E1","81",null,null,null,"FP-2-27-G-10                                                                                                  2-GL-971","FP-2-27-G-10","2-GL-971","E1","81","(E1) FP-2-27-G-10","(81) 2-GL-971"]
["FP-2-27-G-10","E1",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4)","v":" FP-1/2-17-G-10                                                                                                  1/2-GL-471"},"FP-1/2-17-G-10","1/2-GL-471","A1","73","(A1) FP-1/2-17-G-10","(73) 1/2-GL-471"]
[null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5)","v":" FP-1/2-21-G-10                                                                                                  1/2-GL-471"},"FP-1/2-21-G-10","1/2-GL-471","A2","73","(A2) FP-1/2-21-G-10","(73) 1/2-GL-471"]
[null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GL-471","FP-1/2-27-G-10","1/2-GL-471","A3","73","(A3) FP-1/2-27-G-10","(73) 1/2-GL-471"]
["1/2-GUSVT-410","01",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GL-471","FP-1/2-35-G-10","1/2-GL-471","A4","73","(A4) FP-1/2-35-G-10","(73) 1/2-GL-471"]
["3/4-GUSVT-510","02",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GL-471","FP-1/2-50-G-9","1/2-GL-471","A6","73","(A6) FP-1/2-50-G-9","(73) 1/2-GL-471"]
["1-GUSVT-611","03",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GL-571","FP-3/4-21-G-10","3/4-GL-571","B1","75","(B1) FP-3/4-21-G-10","(75) 3/4-GL-571"]
["1-GUSVT-610","04",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GL-671","FP-1-27-G-10","1-GL-671","C1","77","(C1) FP-1-27-G-10","(77) 1-GL-671"]
["1-1/2-GUSVT-867","05",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-871","FP-1-1/2-21-G-10","1-1/2-GL-871",{"$f":"VLOOKUP(L21,$A$3:$B$14,2,FALSE)","v":"D1"},{"$f":"VLOOKUP(M21,$A$17:$B$98,2,FALSE)","v":"79"},"(D1) FP-1-1/2-21-G-10","(79) 1-1/2-GL-871"]
["1-1/2-GUSVGT-814","06",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-871","FP-1-1/2-27-G-10","1-1/2-GL-871",{"$f":"VLOOKUP(L22,$A$3:$B$14,2,FALSE)","v":"D2"},{"$f":"VLOOKUP(M22,$A$17:$B$98,2,FALSE)","v":"79"},"(D2) FP-1-1/2-27-G-10","(79) 1-1/2-GL-871"]
["2-GUSVT-913","07",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  2-GL-971","FP-2-27-G-10","2-GL-971","E1","81","(E1) FP-2-27-G-10","(81) 2-GL-971"]
["2-GUSVGT-914","08",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4,\" \")","v":"FP-1/2-17-G-10                                                                                                  1/2-GL-471 "},"FP-1/2-17-G-10","1/2-GL-471","A1","73","(A1) FP-1/2-17-G-10","(73) 1/2-GL-471"]
["1/2-GUSVT-40A","09",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5,\" \")","v":"FP-1/2-21-G-10                                                                                                  1/2-GL-471 "},"FP-1/2-21-G-10","1/2-GL-471","A2","73","(A2) FP-1/2-21-G-10","(73) 1/2-GL-471"]
["1/2-GSVT-45A","10",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GL-471 ","FP-1/2-27-G-10","1/2-GL-471","A3","73","(A3) FP-1/2-27-G-10","(73) 1/2-GL-471"]
["1/2-GSVT-44A","11",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GL-471 ","FP-1/2-35-G-10","1/2-GL-471","A4","73","(A4) FP-1/2-35-G-10","(73) 1/2-GL-471"]
["1/2-GSVT-48A","12",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GL-471 ","FP-1/2-50-G-9","1/2-GL-471","A6","73","(A6) FP-1/2-50-G-9","(73) 1/2-GL-471"]
["1/2-GNSVT-48A","13",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GL-571 ","FP-3/4-21-G-10","3/4-GL-571","B1","75","(B1) FP-3/4-21-G-10","(75) 3/4-GL-571"]
["3/4-GSVGT-54A","14",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-27-G-10                                                                                                  1-GL-671 ","FP-1-27-G-10","1-GL-671","C1","77","(C1) FP-1-27-G-10","(77) 1-GL-671"]
["3/4-GNSVGT-54A","15",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-871 ","FP-1-1/2-21-G-10","1-1/2-GL-871","D1","79","(D1) FP-1-1/2-21-G-10","(79) 1-1/2-GL-871"]
["3/4-GSVGT-59A","16",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-871 ","FP-1-1/2-27-G-10","1-1/2-GL-871","D2","79","(D2) FP-1-1/2-27-G-10","(79) 1-1/2-GL-871"]
["3/4-GNSVGT-59A","17",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-2-27-G-10                                                                                                  2-GL-971 ","FP-2-27-G-10","2-GL-971","E1","81","(E1) FP-2-27-G-10","(81) 2-GL-971"]
["1-GSVGT-64A","18",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4,\" \")","v":" FP-1/2-17-G-10                                                                                                  1/2-GL-471 "},"FP-1/2-17-G-10","1/2-GL-471","A1","73","(A1) FP-1/2-17-G-10","(73) 1/2-GL-471"]
["1-GSVGT-68A","19",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5,\" \")","v":" FP-1/2-21-G-10                                                                                                  1/2-GL-471 "},"FP-1/2-21-G-10","1/2-GL-471","A2","73","(A2) FP-1/2-21-G-10","(73) 1/2-GL-471"]
["1-GNSVGT-64A","20",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GL-471 ","FP-1/2-27-G-10","1/2-GL-471","A3","73","(A3) FP-1/2-27-G-10","(73) 1/2-GL-471"]
["1-GNSVGT-68A","21",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GL-471 ","FP-1/2-35-G-10","1/2-GL-471","A4","73","(A4) FP-1/2-35-G-10","(73) 1/2-GL-471"]
["1-GSVGT-69A","22",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GL-471 ","FP-1/2-50-G-9","1/2-GL-471",{"$f":"VLOOKUP(L38,$A$3:$B$14,2,FALSE)","v":"A6"},{"$f":"VLOOKUP(M38,$A$17:$B$98,2,FALSE)","v":"73"},"(A6) FP-1/2-50-G-9","(73) 1/2-GL-471"]
["1-GNSVGT-69A","23",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GL-571 ","FP-3/4-21-G-10","3/4-GL-571",{"$f":"VLOOKUP(L39,$A$3:$B$14,2,FALSE)","v":"B1"},{"$f":"VLOOKUP(M39,$A$17:$B$98,2,FALSE)","v":"75"},"(B1) FP-3/4-21-G-10","(75) 3/4-GL-571"]
["1-1/2-GSVGT-87A","24",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GL-671 ","FP-1-27-G-10","1-GL-671","C1","77","(C1) FP-1-27-G-10","(77) 1-GL-671"]
["1-1/2-GSVGT-86A","25",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-871 ","FP-1-1/2-21-G-10","1-1/2-GL-871","D1","79","(D1) FP-1-1/2-21-G-10","(79) 1-1/2-GL-871"]
["1-1/2-GNSVGT-87A","26",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-871 ","FP-1-1/2-27-G-10","1-1/2-GL-871","D2","79","(D2) FP-1-1/2-27-G-10","(79) 1-1/2-GL-871"]
["1-1/2-GNSVGT-86A","27",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  2-GL-971 ","FP-2-27-G-10","2-GL-971","E1","81","(E1) FP-2-27-G-10","(81) 2-GL-971"]
["2-GSVGT-97A","28",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVGT-98A","29",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVGT-97A","30",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVGT-98A","31",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BL-954","32",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BL-953","33",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BL-950","34",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BL-951","35",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GSVTA-44","36",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GSVTA-48","37",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GNSVTA-48","38",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GNSVTA-44","39",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$f":"VLOOKUP(L55,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M55,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GNSVTA-43","40",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$f":"VLOOKUP(L56,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M56,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GSVTA-54","41",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GNSVTA-54","42",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GSVTA-53","43",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GSVTA-56","44",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GNSVTA-56","45",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GNSVTA-53","46",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-64","47",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-65","48",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-64","49",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-63","50",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-66","51",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-65","52",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-66","53",null,null,null,{"$f":"VLOOKUP(D69,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(E69,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N69,\")\",\" \",L69)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
["1-GNSVTA-63","54",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-84","55",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-85","56",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-83","57",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-84","58",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-85","59",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-83","60",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVTA-94","61",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVTA-93","62",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-94","63",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-96","64",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-93","65",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-41","66",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-50","67",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-62","68",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-60","69",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-80","70",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-90","71",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-91","72",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GL-471","73",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GL-410","74",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GL-571","75",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GL-510","76",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GL-671","77",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GL-610","78",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GL-871","79",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GL-810","80",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GL-971","81",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GL-910","82",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L120,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M120,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N133,\")\",\" \",L133)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N155,\")\",\" \",L155)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L184,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M184,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]

{"sheet":"10A45 Naming PVC","index":56,"n_rows":203,"n_cols":17,"rows_kept":203,"cut":false,"hidden":true,"merged":[[2,2,2,8]]}
[]
[]
["FP-1/2-17-G-10","A1","PVC Floats",null,null,null,null,null,null,null,"VLOOKUP",null,null,null,null,"Tube","Float"]
["FP-1/2-21-G-10","A2",null,"FP-1/2-17-G-10","1/2-GL-410",{"$f":"VLOOKUP(D4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(E4,$A$17:$B$98,2,FALSE)","v":"74"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4)","v":"FP-1/2-17-G-10                                                                                                  1/2-GL-410"},"FP-1/2-17-G-10","1/2-GL-410",{"$f":"VLOOKUP(L4,$A$3:$B$14,2,FALSE)","v":"A1"},{"$f":"VLOOKUP(M4,$A$17:$B$98,2,FALSE)","v":"74"},{"$f":"CONCATENATE(\"(\",N4,\")\",\" \",L4)","v":"(A1) FP-1/2-17-G-10"},{"$f":"CONCATENATE(\"(\",O4,\")\",\" \",M4)","v":"(74) 1/2-GL-410"}]
["FP-1/2-27-G-10","A3",null,"FP-1/2-21-G-10","1/2-GL-410",{"$f":"VLOOKUP(D5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(E5,$A$17:$B$98,2,FALSE)","v":"74"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5)","v":"FP-1/2-21-G-10                                                                                                  1/2-GL-410"},"FP-1/2-21-G-10","1/2-GL-410",{"$f":"VLOOKUP(L5,$A$3:$B$14,2,FALSE)","v":"A2"},{"$f":"VLOOKUP(M5,$A$17:$B$98,2,FALSE)","v":"74"},{"$f":"CONCATENATE(\"(\",N5,\")\",\" \",L5)","v":"(A2) FP-1/2-21-G-10"},"(74) 1/2-GL-410"]
["FP-1/2-35-G-10","A4",null,"FP-1/2-27-G-10","1/2-GL-410","A3","74",null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GL-410","FP-1/2-27-G-10","1/2-GL-410","A3","74","(A3) FP-1/2-27-G-10","(74) 1/2-GL-410"]
["FP-1/2-50-G-9","A6",null,"FP-1/2-35-G-10","1/2-GL-410","A4","74",null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GL-410","FP-1/2-35-G-10","1/2-GL-410","A4","74","(A4) FP-1/2-35-G-10","(74) 1/2-GL-410"]
["FP-3/4-21-G-10","B1",null,"FP-1/2-50-G-9","1/2-GL-410","A6","74",null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GL-410","FP-1/2-50-G-9","1/2-GL-410","A6","74","(A6) FP-1/2-50-G-9","(74) 1/2-GL-410"]
["FP-3/4-27-G-10","B2",null,"FP-3/4-21-G-10","3/4-GL-510","B1","76",null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GL-510","FP-3/4-21-G-10","3/4-GL-510","B1","76","(B1) FP-3/4-21-G-10","(76) 3/4-GL-510"]
["FP-1-27-G-10","C1",null,"FP-3/4-27-G-10","3/4-GL-510","B2","76",null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GL-510","FP-3/4-27-G-10","3/4-GL-510","B2","76","(B2) FP-3/4-27-G-10","(76) 3/4-GL-510"]
["FP-1-35-G-10","C2",null,"FP-1-27-G-10","1-GL-610","C1","78",null,null,null,"FP-1-27-G-10                                                                                                  1-GL-610","FP-1-27-G-10","1-GL-610","C1","78","(C1) FP-1-27-G-10","(78) 1-GL-610"]
["FP-1-1/2-21-G-10","D1",null,"FP-1-35-G-10","1-GL-610","C2","78",null,null,null,"FP-1-35-G-10                                                                                                  1-GL-610","FP-1-35-G-10","1-GL-610","C2","78","(C2) FP-1-35-G-10","(78) 1-GL-610"]
["FP-1-1/2-27-G-10","D2",null,"FP-1-1/2-21-G-10","1-1/2-GL-810","D1","80",null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-810","FP-1-1/2-21-G-10","1-1/2-GL-810","D1","80","(D1) FP-1-1/2-21-G-10","(80) 1-1/2-GL-810"]
["FP-2-27-G-10","E1",null,"FP-1-1/2-27-G-10","1-1/2-GL-810","D2","80",null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-810","FP-1-1/2-27-G-10","1-1/2-GL-810","D2","80","(D2) FP-1-1/2-27-G-10","(80) 1-1/2-GL-810"]
[null,null,null,"FP-2-27-G-10","2-GL-910","E1","82",null,null,null,"FP-2-27-G-10                                                                                                  2-GL-910","FP-2-27-G-10","2-GL-910","E1","82","(E1) FP-2-27-G-10","(82) 2-GL-910"]
[null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4)","v":" FP-1/2-17-G-10                                                                                                  1/2-GL-410"},"FP-1/2-17-G-10","1/2-GL-410","A1","74","(A1) FP-1/2-17-G-10","(74) 1/2-GL-410"]
["1/2-GUSVT-410","01",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5)","v":" FP-1/2-21-G-10                                                                                                  1/2-GL-410"},"FP-1/2-21-G-10","1/2-GL-410","A2","74","(A2) FP-1/2-21-G-10","(74) 1/2-GL-410"]
["3/4-GUSVT-510","02",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GL-410","FP-1/2-27-G-10","1/2-GL-410","A3","74","(A3) FP-1/2-27-G-10","(74) 1/2-GL-410"]
["1-GUSVT-611","03",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GL-410","FP-1/2-35-G-10","1/2-GL-410","A4","74","(A4) FP-1/2-35-G-10","(74) 1/2-GL-410"]
["1-GUSVT-610","04",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GL-410","FP-1/2-50-G-9","1/2-GL-410","A6","74","(A6) FP-1/2-50-G-9","(74) 1/2-GL-410"]
["1-1/2-GUSVT-867","05",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GL-510","FP-3/4-21-G-10","3/4-GL-510",{"$f":"VLOOKUP(L21,$A$3:$B$14,2,FALSE)","v":"B1"},{"$f":"VLOOKUP(M21,$A$17:$B$98,2,FALSE)","v":"76"},"(B1) FP-3/4-21-G-10","(76) 3/4-GL-510"]
["1-1/2-GUSVGT-814","06",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GL-510","FP-3/4-27-G-10","3/4-GL-510",{"$f":"VLOOKUP(L22,$A$3:$B$14,2,FALSE)","v":"B2"},{"$f":"VLOOKUP(M22,$A$17:$B$98,2,FALSE)","v":"76"},"(B2) FP-3/4-27-G-10","(76) 3/4-GL-510"]
["2-GUSVT-913","07",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GL-610","FP-1-27-G-10","1-GL-610","C1","78","(C1) FP-1-27-G-10","(78) 1-GL-610"]
["2-GUSVGT-914","08",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GL-610","FP-1-35-G-10","1-GL-610","C2","78","(C2) FP-1-35-G-10","(78) 1-GL-610"]
["1/2-GUSVT-40A","09",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-810","FP-1-1/2-21-G-10","1-1/2-GL-810","D1","80","(D1) FP-1-1/2-21-G-10","(80) 1-1/2-GL-810"]
["1/2-GSVT-45A","10",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-810","FP-1-1/2-27-G-10","1-1/2-GL-810","D2","80","(D2) FP-1-1/2-27-G-10","(80) 1-1/2-GL-810"]
["1/2-GSVT-44A","11",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-2-27-G-10                                                                                                  2-GL-910","FP-2-27-G-10","2-GL-910","E1","82","(E1) FP-2-27-G-10","(82) 2-GL-910"]
["1/2-GSVT-48A","12",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(D4,\"                                                                                                  \",E4,\" \")","v":"FP-1/2-17-G-10                                                                                                  1/2-GL-410 "},"FP-1/2-17-G-10","1/2-GL-410","A1","74","(A1) FP-1/2-17-G-10","(74) 1/2-GL-410"]
["1/2-GNSVT-48A","13",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(D5,\"                                                                                                  \",E5,\" \")","v":"FP-1/2-21-G-10                                                                                                  1/2-GL-410 "},"FP-1/2-21-G-10","1/2-GL-410","A2","74","(A2) FP-1/2-21-G-10","(74) 1/2-GL-410"]
["3/4-GSVGT-54A","14",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-27-G-10                                                                                                  1/2-GL-410 ","FP-1/2-27-G-10","1/2-GL-410","A3","74","(A3) FP-1/2-27-G-10","(74) 1/2-GL-410"]
["3/4-GNSVGT-54A","15",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-35-G-10                                                                                                  1/2-GL-410 ","FP-1/2-35-G-10","1/2-GL-410","A4","74","(A4) FP-1/2-35-G-10","(74) 1/2-GL-410"]
["3/4-GSVGT-59A","16",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1/2-50-G-9                                                                                                  1/2-GL-410 ","FP-1/2-50-G-9","1/2-GL-410","A6","74","(A6) FP-1/2-50-G-9","(74) 1/2-GL-410"]
["3/4-GNSVGT-59A","17",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-3/4-21-G-10                                                                                                  3/4-GL-510 ","FP-3/4-21-G-10","3/4-GL-510","B1","76","(B1) FP-3/4-21-G-10","(76) 3/4-GL-510"]
["1-GSVGT-64A","18",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-3/4-27-G-10                                                                                                  3/4-GL-510 ","FP-3/4-27-G-10","3/4-GL-510","B2","76","(B2) FP-3/4-27-G-10","(76) 3/4-GL-510"]
["1-GSVGT-68A","19",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-27-G-10                                                                                                  1-GL-610 ","FP-1-27-G-10","1-GL-610","C1","78","(C1) FP-1-27-G-10","(78) 1-GL-610"]
["1-GNSVGT-64A","20",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-35-G-10                                                                                                  1-GL-610 ","FP-1-35-G-10","1-GL-610","C2","78","(C2) FP-1-35-G-10","(78) 1-GL-610"]
["1-GNSVGT-68A","21",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-810 ","FP-1-1/2-21-G-10","1-1/2-GL-810","D1","80","(D1) FP-1-1/2-21-G-10","(80) 1-1/2-GL-810"]
["1-GSVGT-69A","22",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-810 ","FP-1-1/2-27-G-10","1-1/2-GL-810",{"$f":"VLOOKUP(L38,$A$3:$B$14,2,FALSE)","v":"D2"},{"$f":"VLOOKUP(M38,$A$17:$B$98,2,FALSE)","v":"80"},"(D2) FP-1-1/2-27-G-10","(80) 1-1/2-GL-810"]
["1-GNSVGT-69A","23",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"FP-2-27-G-10                                                                                                  2-GL-910 ","FP-2-27-G-10","2-GL-910",{"$f":"VLOOKUP(L39,$A$3:$B$14,2,FALSE)","v":"E1"},{"$f":"VLOOKUP(M39,$A$17:$B$98,2,FALSE)","v":"82"},"(E1) FP-2-27-G-10","(82) 2-GL-910"]
["1-1/2-GSVGT-87A","24",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D4,\"                                                                                                  \",E4,\" \")","v":" FP-1/2-17-G-10                                                                                                  1/2-GL-410 "},"FP-1/2-17-G-10","1/2-GL-410","A1","74","(A1) FP-1/2-17-G-10","(74) 1/2-GL-410"]
["1-1/2-GSVGT-86A","25",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D5,\"                                                                                                  \",E5,\" \")","v":" FP-1/2-21-G-10                                                                                                  1/2-GL-410 "},"FP-1/2-21-G-10","1/2-GL-410","A2","74","(A2) FP-1/2-21-G-10","(74) 1/2-GL-410"]
["1-1/2-GNSVGT-87A","26",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-27-G-10                                                                                                  1/2-GL-410 ","FP-1/2-27-G-10","1/2-GL-410","A3","74","(A3) FP-1/2-27-G-10","(74) 1/2-GL-410"]
["1-1/2-GNSVGT-86A","27",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-35-G-10                                                                                                  1/2-GL-410 ","FP-1/2-35-G-10","1/2-GL-410","A4","74","(A4) FP-1/2-35-G-10","(74) 1/2-GL-410"]
["2-GSVGT-97A","28",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1/2-50-G-9                                                                                                  1/2-GL-410 ","FP-1/2-50-G-9","1/2-GL-410","A6","74","(A6) FP-1/2-50-G-9","(74) 1/2-GL-410"]
["2-GSVGT-98A","29",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-21-G-10                                                                                                  3/4-GL-510 ","FP-3/4-21-G-10","3/4-GL-510","B1","76","(B1) FP-3/4-21-G-10","(76) 3/4-GL-510"]
["2-GNSVGT-97A","30",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-3/4-27-G-10                                                                                                  3/4-GL-510 ","FP-3/4-27-G-10","3/4-GL-510","B2","76","(B2) FP-3/4-27-G-10","(76) 3/4-GL-510"]
["2-GNSVGT-98A","31",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-27-G-10                                                                                                  1-GL-610 ","FP-1-27-G-10","1-GL-610","C1","78","(C1) FP-1-27-G-10","(78) 1-GL-610"]
["BL-954","32",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-35-G-10                                                                                                  1-GL-610 ","FP-1-35-G-10","1-GL-610","C2","78","(C2) FP-1-35-G-10","(78) 1-GL-610"]
["BL-953","33",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-21-G-10                                                                                                  1-1/2-GL-810 ","FP-1-1/2-21-G-10","1-1/2-GL-810","D1","80","(D1) FP-1-1/2-21-G-10","(80) 1-1/2-GL-810"]
["BL-950","34",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null," FP-1-1/2-27-G-10                                                                                                  1-1/2-GL-810 ","FP-1-1/2-27-G-10","1-1/2-GL-810","D2","80","(D2) FP-1-1/2-27-G-10","(80) 1-1/2-GL-810"]
["BL-951","35",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,{"$f":"CONCATENATE(\" \",D15,\"                                                                                                  \",E15,\" \")","v":" FP-2-27-G-10                                                                                                  2-GL-910 "},"FP-2-27-G-10","2-GL-910","E1","82","(E1) FP-2-27-G-10","(82) 2-GL-910"]
["1/2-GSVTA-44","36",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GSVTA-48","37",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GNSVTA-48","38",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GNSVTA-44","39",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$f":"VLOOKUP(L55,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M55,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GNSVTA-43","40",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$f":"VLOOKUP(L56,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M56,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GSVTA-54","41",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GNSVTA-54","42",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GSVTA-53","43",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GSVTA-56","44",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GNSVTA-56","45",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GNSVTA-53","46",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-64","47",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-65","48",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-64","49",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-63","50",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GSVTA-66","51",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-65","52",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GNSVTA-66","53",null,null,null,{"$f":"VLOOKUP(D69,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(E69,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N69,\")\",\" \",L69)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
["1-GNSVTA-63","54",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-84","55",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-85","56",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GSVTA-83","57",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-84","58",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-85","59",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GNSVTA-83","60",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVTA-94","61",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GSVTA-93","62",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-94","63",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-96","64",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GNSVTA-93","65",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-41","66",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-50","67",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-62","68",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-60","69",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-80","70",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-90","71",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["BS-91","72",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GL-471","73",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1/2-GL-410","74",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GL-571","75",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["3/4-GL-510","76",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GL-671","77",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-GL-610","78",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GL-871","79",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["1-1/2-GL-810","80",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GL-971","81",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["2-GL-910","82",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L120,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M120,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N133,\")\",\" \",L133)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$f":"CONCATENATE(\"(\",N155,\")\",\" \",L155)","v":{"$error":"#N/A"}},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(L184,$A$3:$B$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(M184,$A$17:$B$98,2,FALSE)","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]

{"sheet":"10A4 Low PSI Drop Floats Result","index":57,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"'Modified Inputs'!$O$2*'Modified Inputs'!$J$23*SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A4 Capacity Tables'!$C$5:$F$21,3,FALSE),\"                                                                                                  \",VLOOKUP(D5,'10A4 Capacity Tables'!$C$5:$F$21,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$C$5:$C$21<'10A4 Low PSI Drop Floats Result'!$B$5,'10A4 Capacity Tables'!$C$5:$C$21))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A4 Capacity Tables'!$C$5:$F$21,3,FALSE),\"                                                                                                  \",VLOOKUP(D6,'10A4 Capacity Tables'!$C$5:$F$21,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$5:$C$21>'10A4 Low PSI Drop Floats Result'!$B$5,'10A4 Capacity Tables'!$C$5:$C$21))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A4 Capacity Tables'!$C$5:$F$21,3,FALSE),\"                                                                                                  \",VLOOKUP(D7,'10A4 Capacity Tables'!$C$5:$F$21,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$5:$C$21>D6,'10A4 Capacity Tables'!$C$5:$C$21))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A4 Capacity Tables'!$C$5:$F$21,3,FALSE),\"                                                                                                  \",VLOOKUP(D8,'10A4 Capacity Tables'!$C$5:$F$21,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$5:$C$21>D7,'10A4 Capacity Tables'!$C$5:$C$21))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
["T0","P0","Standard Density","Density/ Reference Density","Qa Standard","Tube/Float","Max Flow SCFM","Min Flow Specified Units","Max Flow Specified Units","Min Flow CFM","Max Rounded","Min Rounded","Concatenated"]
[{"$f":"'Modified Inputs'!$K$2+459.67","v":459.67},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N37,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Normal\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!O46,\"\"))))))","v":""},{"$f":"C12/0.0012","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$5=\"Actual\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((B12*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(A12*'10A4 Low PSI Drop Floats Result'!$B$12))+0.00000000001,\nIF('VA Sizing'!$C$5=\"Normal\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(492*'10A4 Low PSI Drop Floats Result'!$B$12))+0.00000000001,\n'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(530*'10A4 Low PSI Drop Floats Result'!$B$12))+0.00000000001))","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(G12,'10A4 Capacity Tables'!$D$5:$F$21,2,FALSE),\"                                                                                                  \",VLOOKUP(G12,'10A4 Capacity Tables'!$D$5:$F$21,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$D$5:$D$21<'10A4 Low PSI Drop Floats Result'!$E$12,'10A4 Capacity Tables'!$D$5:$D$21))","v":{"$error":"#N/A"}},{"$f":"G12/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(530*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(492*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT(('10A4 Low PSI Drop Floats Result'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Low PSI Drop Floats Result'!$A$12)/('10A4 Low PSI Drop Floats Result'!$A$12*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I12/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I12<0.99999,ROUND(I12,2),\nIF(I12<9.999,ROUND(I12,2),\nIF(I12<99.99,ROUND(I12,1),\nIF(I12<999.99,ROUND(I12,0),\nIF(I12<9999.99,ROUND(I12,-1),\nIF(I12<99999,ROUND(I12,-2),ROUND(I12,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J12,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L12,\" \",\"-\",\" \",K12)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G13,'10A4 Capacity Tables'!$D$5:$F$21,2,FALSE),\"                                                                                                  \",VLOOKUP(G13,'10A4 Capacity Tables'!$D$5:$F$21,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$5:$D$21>'10A4 Low PSI Drop Floats Result'!$E$12,'10A4 Capacity Tables'!$D$5:$D$21))","v":{"$error":"#N/A"}},{"$f":"G13/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(530*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(492*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT(('10A4 Low PSI Drop Floats Result'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Low PSI Drop Floats Result'!$A$12)/('10A4 Low PSI Drop Floats Result'!$A$12*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I13/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I13<0.99999,ROUND(I13,2),\nIF(I13<9.999,ROUND(I13,2),\nIF(I13<99.99,ROUND(I13,1),\nIF(I13<999.99,ROUND(I13,0),\nIF(I13<9999.99,ROUND(I13,-1),\nIF(I13<99999,ROUND(I13,-2),ROUND(I13,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J13,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L13,\" \",\"-\",\" \",K13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G14,'10A4 Capacity Tables'!$D$5:$F$21,2,FALSE),\"                                                                                                  \",VLOOKUP(G14,'10A4 Capacity Tables'!$D$5:$F$21,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$5:$D$21>'10A4 Low PSI Drop Floats Result'!$G$13,'10A4 Capacity Tables'!$D$5:$D$21))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(530*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(492*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT(('10A4 Low PSI Drop Floats Result'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Low PSI Drop Floats Result'!$A$12)/('10A4 Low PSI Drop Floats Result'!$A$12*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G15,'10A4 Capacity Tables'!$D$5:$F$21,2,FALSE),\"                                                                                                  \",VLOOKUP(G15,'10A4 Capacity Tables'!$D$5:$F$21,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$5:$D$21>'10A4 Low PSI Drop Floats Result'!$G$14,'10A4 Capacity Tables'!$D$5:$D$21))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(530*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A4 Low PSI Drop Floats Result'!$D$12*'10A4 Low PSI Drop Floats Result'!$A$12)/(492*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT(('10A4 Low PSI Drop Floats Result'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Low PSI Drop Floats Result'!$A$12)/('10A4 Low PSI Drop Floats Result'!$A$12*'10A4 Low PSI Drop Floats Result'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Low PSI Drop Floats Result'!D5,'10A4 Capacity Tables'!$C$5:$G$22,5,FALSE)),CONCATENATE(\" \",'10A4 Low PSI Drop Floats Result'!C5),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!C5,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Low PSI Drop Floats Result'!G12,'10A4 Capacity Tables'!$D$5:$H$21,5,FALSE)),CONCATENATE('10A4 Low PSI Drop Floats Result'!F12,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!F12,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Low PSI Drop Floats Result'!D6,'10A4 Capacity Tables'!$C$5:$G$22,5,FALSE)),CONCATENATE(\" \",'10A4 Low PSI Drop Floats Result'!C6),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!C6,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Low PSI Drop Floats Result'!G13,'10A4 Capacity Tables'!$D$5:$H$21,5,FALSE)),CONCATENATE('10A4 Low PSI Drop Floats Result'!F13,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!F13,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Low PSI Drop Floats Result'!D7,'10A4 Capacity Tables'!$C$5:$G$22,5,FALSE)),CONCATENATE(\" \",'10A4 Low PSI Drop Floats Result'!C7),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!C7,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Low PSI Drop Floats Result'!G14,'10A4 Capacity Tables'!$D$5:$H$21,5,FALSE)),CONCATENATE('10A4 Low PSI Drop Floats Result'!F14,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!F14,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Low PSI Drop Floats Result'!D8,'10A4 Capacity Tables'!$C$5:$G$22,5,FALSE)),CONCATENATE(\" \",'10A4 Low PSI Drop Floats Result'!C8),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!C8,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Low PSI Drop Floats Result'!G15,'10A4 Capacity Tables'!$D$5:$H$21,5,FALSE)),CONCATENATE('10A4 Low PSI Drop Floats Result'!F15,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!F15,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!H5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!K12,\"\"))","v":""},{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!F5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!I12,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!H6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!K13,\"\"))","v":""},{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!F6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!I13,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!H7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!K14,\"\"))","v":""},{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!F7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!I14,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!H8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!K15,\"\"))","v":""},{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Low PSI Drop Floats Result'!F8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Low PSI Drop Floats Result'!I15,\"\"))","v":""}]

{"sheet":"Photos","index":58,"n_rows":36,"n_cols":12,"rows_kept":36,"cut":false,"hidden":true,"merged":[[3,3,3,4],[16,10,16,11],[30,10,30,11]]}
[]
["Object"]
[{"$f":"'VA Sizing'!N2","v":0}]
[null,null,null,"VLOOKUP"]
[null,null,null,"10A61",5]
[null,null,null,"10A4",6]
[null,null,null,"10A22",7]
[null,null,null,"10A32",8]
[null,null,null,"FAM54",9]
[null,null,null,0,10]
[null,null,null,{"$f":"\"\"","v":""},11]
[]
[]
[]
[null,null,null,null,null,null,null,"Mixed Gas"]
[null,null,null,null,null,null,null,{"$f":"IF(AND(RIGHT('VA Sizing'!B4,1)=\" \",'VA Sizing'!C3=\"Gas\"),\"Pressed\",'VA Sizing'!C3)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"VLOOKUP"]
[null,null,null,null,null,null,null,null,null,null,"Liquid",18]
[null,null,null,null,null,null,null,null,null,null,0,19]
[null,null,null,null,null,null,null,null,null,null,"Gas",20]
[]
[null,null,null,null,null,null,null,"Mixed Gas",null,null,"Pressed",22]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Steam"]
[null,null,null,null,null,null,null,{"$f":"IF(AND(RIGHT('VA Sizing'!B3,1)=\" \",'VA Sizing'!C3=\"Gas\"),\"Pressed\",'VA Sizing'!C3)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"VLOOKUP"]
[null,null,null,null,null,null,null,null,null,null,"Liquid",32]
[null,null,null,null,null,null,null,null,null,null,0,33]
[null,null,null,null,null,null,null,"Steam",null,null,"Gas",34]
[]
[null,null,null,null,null,null,null,"Steam",null,null,"Pressed",36]

{"sheet":"10A4 Alarm Floats Results","index":59,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"'Modified Inputs'!$O$2*'Modified Inputs'!$J$23*SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A4 Capacity Tables'!$C$88:$F$137,3,FALSE),\"                                                                                                  \",VLOOKUP(D5,'10A4 Capacity Tables'!$C$88:$F$137,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$C$88:$C$137<'10A4 Alarm Floats Results'!$B$5,'10A4 Capacity Tables'!$C$88:$C$137))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A4 Capacity Tables'!$C$88:$F$137,3,FALSE),\"                                                                                                  \",VLOOKUP(D6,'10A4 Capacity Tables'!$C$88:$F$137,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$88:$C$137>'10A4 Alarm Floats Results'!$B$5,'10A4 Capacity Tables'!$C$88:$C$137))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A4 Capacity Tables'!$C$88:$F$137,3,FALSE),\"                                                                                                  \",VLOOKUP(D7,'10A4 Capacity Tables'!$C$88:$F$137,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$88:$C$137>D6,'10A4 Capacity Tables'!$C$88:$C$137))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A4 Capacity Tables'!$C$88:$F$137,3,FALSE),\"                                                                                                  \",VLOOKUP(D8,'10A4 Capacity Tables'!$C$88:$F$137,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$88:$C$137>D7,'10A4 Capacity Tables'!$C$88:$C$137))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((7.02*'Modified Inputs'!$M$2)/(8.02-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
["T0","P0","Standard Density","Density/ Reference Density","Qa Standard","Tube/Float","Max Flow SCFM","Min Flow Specified Units","Max Flow Specified Units","Min Flow CFM","Max Rounded","Min Rounded","Concatenated"]
[{"$f":"'Modified Inputs'!$K$2+459.67","v":459.67},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N37,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Normal\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!O46,\"\"))))))","v":""},{"$f":"C12/0.0012","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$5=\"Actual\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((B12*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(A12*'10A4 Alarm Floats Results'!$B$12))+0.00000000001,\nIF('VA Sizing'!$C$5=\"Normal\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(492*'10A4 Alarm Floats Results'!$B$12))+0.00000000001,\n'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(530*'10A4 Alarm Floats Results'!$B$12))+0.00000000001))","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(G12,'10A4 Capacity Tables'!$D$88:$F$137,2,FALSE),\"                                                                                                  \",VLOOKUP(G12,'10A4 Capacity Tables'!$D$88:$F$137,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$D$88:$D$137<'10A4 Alarm Floats Results'!$E$12,'10A4 Capacity Tables'!$D$88:$D$137))","v":{"$error":"#N/A"}},{"$f":"G12/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(530*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(492*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT(('10A4 Alarm Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Alarm Floats Results'!$A$12)/('10A4 Alarm Floats Results'!$A$12*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I12/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I12<0.99999,ROUND(I12,2),\nIF(I12<9.999,ROUND(I12,2),\nIF(I12<99.99,ROUND(I12,1),\nIF(I12<999.99,ROUND(I12,0),\nIF(I12<9999.99,ROUND(I12,-1),\nIF(I12<99999,ROUND(I12,-2),ROUND(I12,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J12,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L12,\" \",\"-\",\" \",K12)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G13,'10A4 Capacity Tables'!$D$88:$F$137,2,FALSE),\"                                                                                                  \",VLOOKUP(G13,'10A4 Capacity Tables'!$D$88:$F$137,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$88:$D$137>'10A4 Alarm Floats Results'!$E$12,'10A4 Capacity Tables'!$D$88:$D$137))","v":{"$error":"#N/A"}},{"$f":"G13/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(530*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(492*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT(('10A4 Alarm Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Alarm Floats Results'!$A$12)/('10A4 Alarm Floats Results'!$A$12*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I13/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I13<0.99999,ROUND(I13,2),\nIF(I13<9.999,ROUND(I13,2),\nIF(I13<99.99,ROUND(I13,1),\nIF(I13<999.99,ROUND(I13,0),\nIF(I13<9999.99,ROUND(I13,-1),\nIF(I13<99999,ROUND(I13,-2),ROUND(I13,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J13,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L13,\" \",\"-\",\" \",K13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G14,'10A4 Capacity Tables'!$D$88:$F$137,2,FALSE),\"                                                                                                  \",VLOOKUP(G14,'10A4 Capacity Tables'!$D$88:$F$137,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$88:$D$137>'10A4 Alarm Floats Results'!$G$13,'10A4 Capacity Tables'!$D$88:$D$137))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(530*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(492*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT(('10A4 Alarm Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Alarm Floats Results'!$A$12)/('10A4 Alarm Floats Results'!$A$12*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G15,'10A4 Capacity Tables'!$D$88:$F$137,2,FALSE),\"                                                                                                  \",VLOOKUP(G15,'10A4 Capacity Tables'!$D$88:$F$137,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$D$88:$D$137>'10A4 Alarm Floats Results'!$G$14,'10A4 Capacity Tables'!$D$88:$D$137))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(530*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A4 Alarm Floats Results'!$D$12*'10A4 Alarm Floats Results'!$A$12)/(492*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT(('10A4 Alarm Floats Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A4 Alarm Floats Results'!$A$12)/('10A4 Alarm Floats Results'!$A$12*'10A4 Alarm Floats Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Alarm Floats Results'!D5,'10A4 Capacity Tables'!$C$88:$G$138,5,FALSE)),CONCATENATE(\" \",'10A4 Alarm Floats Results'!C5),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!C5,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Alarm Floats Results'!G12,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 Alarm Floats Results'!F12,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!F12,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Alarm Floats Results'!D6,'10A4 Capacity Tables'!$C$88:$G$138,5,FALSE)),CONCATENATE(\" \",'10A4 Alarm Floats Results'!C6),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!C6,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Alarm Floats Results'!G13,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 Alarm Floats Results'!F13,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!F13,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Alarm Floats Results'!D7,'10A4 Capacity Tables'!$C$88:$G$138,5,FALSE)),CONCATENATE(\" \",'10A4 Alarm Floats Results'!C7),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!C7,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Alarm Floats Results'!G14,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 Alarm Floats Results'!F14,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!F14,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 Alarm Floats Results'!D8,'10A4 Capacity Tables'!$C$88:$G$138,5,FALSE)),CONCATENATE(\" \",'10A4 Alarm Floats Results'!C8),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!C8,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 Alarm Floats Results'!G15,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 Alarm Floats Results'!F15,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!F15,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 Alarm Floats Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 Alarm Floats Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""}]
[null,null,null,{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""}]

{"sheet":"10A4 TA Floats Results","index":60,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"'Modified Inputs'!$O$2*'Modified Inputs'!$J$23*SQRT((15.6*'Modified Inputs'!$M$2)/(16.6-'Modified Inputs'!$M$2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A4 Capacity Tables'!$C$143:$F$157,3,FALSE),\"                                                                                                  \",VLOOKUP(D5,'10A4 Capacity Tables'!$C$143:$F$157,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$C$143:$C$157<'10A4 TA Floats Results'!$B$5,'10A4 Capacity Tables'!$C$143:$C$157))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((15.6*'Modified Inputs'!$M$2)/(16.6-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A4 Capacity Tables'!$C$143:$F$157,3,FALSE),\"                                                                                                  \",VLOOKUP(D6,'10A4 Capacity Tables'!$C$143:$F$157,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$143:$C$157>'10A4 TA Floats Results'!$B$5,'10A4 Capacity Tables'!$C$143:$C$157))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((15.6*'Modified Inputs'!$M$2)/(16.6-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A4 Capacity Tables'!$C$143:$F$157,3,FALSE),\"                                                                                                  \",VLOOKUP(D7,'10A4 Capacity Tables'!$C$143:$F$157,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$143:$C$157>D6,'10A4 Capacity Tables'!$C$143:$C$157))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((15.6*'Modified Inputs'!$M$2)/(16.6-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A4 Capacity Tables'!$C$143:$F$157,3,FALSE),\"                                                                                                  \",VLOOKUP(D8,'10A4 Capacity Tables'!$C$143:$F$157,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$143:$C$157>D7,'10A4 Capacity Tables'!$C$143:$C$157))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((15.6*'Modified Inputs'!$M$2)/(16.6-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 TA Floats Results'!D5,'10A4 Capacity Tables'!$C$143:$G$157,5,FALSE)),CONCATENATE(\" \",'10A4 TA Floats Results'!C5),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!C5,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 TA Floats Results'!G12,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 TA Floats Results'!F12,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!F12,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 TA Floats Results'!D6,'10A4 Capacity Tables'!$C$143:$G$157,5,FALSE)),CONCATENATE(\" \",'10A4 TA Floats Results'!C6),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!C6,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 TA Floats Results'!G13,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 TA Floats Results'!F13,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!F13,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 TA Floats Results'!D7,'10A4 Capacity Tables'!$C$143:$G$157,5,FALSE)),CONCATENATE(\" \",'10A4 TA Floats Results'!C7),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!C7,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 TA Floats Results'!G14,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 TA Floats Results'!F14,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!F14,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 TA Floats Results'!D8,'10A4 Capacity Tables'!$C$143:$G$157,5,FALSE)),CONCATENATE(\" \",'10A4 TA Floats Results'!C8),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!C8,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 TA Floats Results'!G15,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 TA Floats Results'!F15,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!F15,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 TA Floats Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 TA Floats Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""}]
[null,null,null,{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""}]

{"sheet":"10A4 PTFE Floats Results","index":61,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"'Modified Inputs'!$O$2*'Modified Inputs'!$J$23*SQRT((1.31*'Modified Inputs'!$M$2)/(2.31-'Modified Inputs'!$M$2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A4 Capacity Tables'!$C$162:$F$171,3,FALSE),\"                                                                                                  \",VLOOKUP(D5,'10A4 Capacity Tables'!$C$162:$F$171,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$C$162:$C$171<'10A4 PTFE Floats Results'!$B$5,'10A4 Capacity Tables'!$C$162:$C$171))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((1.31*'Modified Inputs'!$M$2)/(2.31-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A4 Capacity Tables'!$C$162:$F$171,3,FALSE),\"                                                                                                  \",VLOOKUP(D6,'10A4 Capacity Tables'!$C$162:$F$171,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$162:$C$171>'10A4 PTFE Floats Results'!$B$5,'10A4 Capacity Tables'!$C$162:$C$171))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((1.31*'Modified Inputs'!$M$2)/(2.31-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A4 Capacity Tables'!$C$162:$F$171,3,FALSE),\"                                                                                                  \",VLOOKUP(D7,'10A4 Capacity Tables'!$C$162:$F$171,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$162:$C$171>D6,'10A4 Capacity Tables'!$C$162:$C$171))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((1.31*'Modified Inputs'!$M$2)/(2.31-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A4 Capacity Tables'!$C$162:$F$171,3,FALSE),\"                                                                                                  \",VLOOKUP(D8,'10A4 Capacity Tables'!$C$162:$F$171,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$162:$C$171>D7,'10A4 Capacity Tables'!$C$162:$C$171))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((1.31*'Modified Inputs'!$M$2)/(2.31-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PTFE Floats Results'!D5,'10A4 Capacity Tables'!$C$162:$G$171,5,FALSE)),CONCATENATE(\" \",'10A4 PTFE Floats Results'!C5),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!C5,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PTFE Floats Results'!G12,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PTFE Floats Results'!F12,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!F12,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PTFE Floats Results'!D6,'10A4 Capacity Tables'!$C$162:$G$171,5,FALSE)),CONCATENATE(\" \",'10A4 PTFE Floats Results'!C6),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!C6,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PTFE Floats Results'!G13,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PTFE Floats Results'!F13,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!F13,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PTFE Floats Results'!D7,'10A4 Capacity Tables'!$C$162:$G$171,5,FALSE)),CONCATENATE(\" \",'10A4 PTFE Floats Results'!C7),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!C7,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PTFE Floats Results'!G14,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PTFE Floats Results'!F14,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!F14,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PTFE Floats Results'!D8,'10A4 Capacity Tables'!$C$162:$G$171,5,FALSE)),CONCATENATE(\" \",'10A4 PTFE Floats Results'!C8),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!C8,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PTFE Floats Results'!G15,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PTFE Floats Results'!F15,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!F15,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PTFE Floats Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PTFE Floats Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""}]
[null,null,null,{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""}]

{"sheet":"10A4 PVC Floats Results","index":62,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"'Modified Inputs'!$O$2*'Modified Inputs'!$J$23*SQRT((4.5*'Modified Inputs'!$M$2)/(5.5-'Modified Inputs'!$M$2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A4 Capacity Tables'!$C$176:$F$187,3,FALSE),\"                                                                                                  \",VLOOKUP(D5,'10A4 Capacity Tables'!$C$176:$F$187,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A4 Capacity Tables'!$C$176:$C$187<'10A4 PVC Floats Results'!$B$5,'10A4 Capacity Tables'!$C$176:$C$187))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((4.5*'Modified Inputs'!$M$2)/(5.5-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(K5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A4 Capacity Tables'!$C$176:$F$187,3,FALSE),\"                                                                                                  \",VLOOKUP(D6,'10A4 Capacity Tables'!$C$176:$F$187,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$176:$C$187>'10A4 PVC Floats Results'!$B$5,'10A4 Capacity Tables'!$C$176:$C$187))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((4.5*'Modified Inputs'!$M$2)/(5.5-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(K6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A4 Capacity Tables'!$C$176:$F$187,3,FALSE),\"                                                                                                  \",VLOOKUP(D7,'10A4 Capacity Tables'!$C$176:$F$187,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$176:$C$187>D6,'10A4 Capacity Tables'!$C$176:$C$187))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((4.5*'Modified Inputs'!$M$2)/(5.5-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A4 Capacity Tables'!$C$176:$F$187,3,FALSE),\"                                                                                                  \",VLOOKUP(D8,'10A4 Capacity Tables'!$C$176:$F$187,4,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A4 Capacity Tables'!$C$176:$C$187>D7,'10A4 Capacity Tables'!$C$176:$C$187))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/SQRT((4.5*'Modified Inputs'!$M$2)/(5.5-'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PVC Floats Results'!D5,'10A4 Capacity Tables'!$C$176:$G$187,5,FALSE)),CONCATENATE(\" \",'10A4 PVC Floats Results'!C5),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!C5,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PVC Floats Results'!G12,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PVC Floats Results'!F12,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!F12,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PVC Floats Results'!D6,'10A4 Capacity Tables'!$C$176:$G$187,5,FALSE)),CONCATENATE(\" \",'10A4 PVC Floats Results'!C6),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!C6,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PVC Floats Results'!G13,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PVC Floats Results'!F13,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!F13,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PVC Floats Results'!D7,'10A4 Capacity Tables'!$C$176:$G$187,5,FALSE)),CONCATENATE(\" \",'10A4 PVC Floats Results'!C7),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!C7,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PVC Floats Results'!G14,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PVC Floats Results'!F14,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!F14,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>VLOOKUP('10A4 PVC Floats Results'!D8,'10A4 Capacity Tables'!$C$176:$G$187,5,FALSE)),CONCATENATE(\" \",'10A4 PVC Floats Results'!C8),\nIF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!C8,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$I$2<VLOOKUP('10A4 PVC Floats Results'!G15,'10A4 Capacity Tables'!$D$88:$H$137,5,FALSE)),CONCATENATE('10A4 PVC Floats Results'!F15,\" \"),\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!F15,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A4 PVC Floats Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A4 PVC Floats Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""}]
[null,null,null,{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""}]

{"sheet":"10A22 Alarm Results","index":63,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,1,2,9],[9,0,9,12],[23,3,23,4]]}
[]
[]
[null,"Liquid"]
[null,"Qw","Tube/Float","Max Flow US GPM","Min Flow US GPM","Max Flow Specified Units","Min Flow Specified Units","Max Rounded","Min Rounded","Concatenated"]
[null,{"$f":"('Modified Inputs'!$O$2*'Modified Inputs'!$J$23*'Modified Inputs'!M2*2.73819)/(SQRT((8.4977-'Modified Inputs'!M2)*'Modified Inputs'!M2))-0.0000000000001","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(D5,'10A22 Capacity Table'!$C$27:$E$37,2,FALSE),\"-\",VLOOKUP(D5,'10A22 Capacity Table'!$C$27:$E$37,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A22 Capacity Table'!$C$27:$C$37<'10A22 Alarm Results'!$B$5,'10A22 Capacity Table'!$C$27:$C$37))","v":{"$error":"#N/A"}},{"$f":"D5/10","v":{"$error":"#N/A"}},{"$f":"(D5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F5/10","v":{"$error":"#N/A"}},{"$f":"IF(F5<0.99999,ROUND(F5,2),\nIF(F5<9.999,ROUND(F5,2),\nIF(F5<99.99,ROUND(F5,1),\nIF(F5<999.99,ROUND(F5,0),\nIF(F5<9999.99,ROUND(F5,-1),\nIF(F5<99999,ROUND(F5,-2),ROUND(F5,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G5,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I5,\" \",\"-\",\" \",H5)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D6,'10A22 Capacity Table'!$C$27:$E$37,2,FALSE),\"-\",VLOOKUP(D6,'10A22 Capacity Table'!$C$27:$E$37,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$27:$C$37>'10A22 Alarm Results'!$B$5,'10A22 Capacity Table'!$C$27:$C$37))","v":{"$error":"#N/A"}},{"$f":"D6/10","v":{"$error":"#N/A"}},{"$f":"(D6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$f":"F6/10","v":{"$error":"#N/A"}},{"$f":"IF(F6<0.99999,ROUND(F6,2),\nIF(F6<9.999,ROUND(F6,2),\nIF(F6<99.99,ROUND(F6,1),\nIF(F6<999.99,ROUND(F6,0),\nIF(F6<9999.99,ROUND(F6,-1),\nIF(F6<99999,ROUND(F6,-2),ROUND(F6,2)))))))","v":{"$error":"#N/A"}},{"$f":"ROUND(G6,1)","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(I6,\" \",\"-\",\" \",H6)","v":{"$error":"#N/A"}}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D7,'10A22 Capacity Table'!$C$27:$E$37,2,FALSE),\"-\",VLOOKUP(D7,'10A22 Capacity Table'!$C$27:$E$37,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$27:$C$37>D6,'10A22 Capacity Table'!$C$27:$C$37))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,{"$f":"CONCATENATE(VLOOKUP(D8,'10A22 Capacity Table'!$C$27:$E$37,2,FALSE),\"-\",VLOOKUP(D8,'10A22 Capacity Table'!$C$27:$E$37,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$27:$C$37>D7,'10A22 Capacity Table'!$C$27:$C$37))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"(D8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
[]
["Gas"]
["T0","P0","Standard Density","Density/ Reference Density","Qa Standard","Tube/Float","Max Flow SCFM","Min Flow Specified Units","Max Flow Specified Units","Min Flow CFM","Max Rounded","Min Rounded","Concatenated"]
[{"$f":"'Modified Inputs'!$K$2+459.67","v":459.67},{"$f":"'Modified Inputs'!$I$2","v":0},{"$f":"IF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",'VA Sizing'!$C$5=\"Standard\"),'10A61 5\" Calcs'!O46/'10A61 5\" Calcs'!M46,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Operating Conditions\",OR('VA Sizing'!$C$5=\"Normal\",'VA Sizing'!$C$5=\"Actual\")),'10A61 5\" Calcs'!O46/N37,\nIF(AND('VA Sizing'!$C$4=\" Other\",'VA Sizing'!$C$6=\"at Reference Conditions\"),'Modified Inputs'!$M$4,\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$K$29,2,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Normal\"),VLOOKUP('VA Sizing'!$C$4,'10A61 5\" Calcs'!$J$3:$L$29,3,FALSE),\nIF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Actual\"),'10A61 5\" Calcs'!O46,\"\"))))))","v":""},{"$f":"C12/0.0012","v":{"$error":"#VALUE!"}},{"$f":"IF('VA Sizing'!$C$5=\"Actual\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((B12*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(A12*'10A22 Alarm Results'!$B$12))+0.00000000001,\nIF('VA Sizing'!$C$5=\"Normal\",'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(492*'10A22 Alarm Results'!$B$12))+0.00000000001,\n'Modified Inputs'!$O$2*'Modified Inputs'!$J$18*SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(530*'10A22 Alarm Results'!$B$12))+0.00000000001))","v":{"$error":"#N/A"}},{"$f":"CONCATENATE(VLOOKUP(G12,'10A22 Capacity Table'!$C$62:$E$72,2,FALSE),\"-\",VLOOKUP(G12,'10A22 Capacity Table'!$C$62:$E$72,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MAX(IF('10A22 Capacity Table'!$C$62:$C$72<'10A22 Alarm Results'!$E$12,'10A22 Capacity Table'!$C$62:$C$72))","v":{"$error":"#N/A"}},{"$f":"G12/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(530*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(492*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G12/SQRT(('10A22 Alarm Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Alarm Results'!$A$12)/('10A22 Alarm Results'!$A$12*'10A22 Alarm Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I12/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I12<0.99999,ROUND(I12,2),\nIF(I12<9.999,ROUND(I12,2),\nIF(I12<99.99,ROUND(I12,1),\nIF(I12<999.99,ROUND(I12,0),\nIF(I12<9999.99,ROUND(I12,-1),\nIF(I12<99999,ROUND(I12,-2),ROUND(I12,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J12,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L12,\" \",\"-\",\" \",K12)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G13,'10A22 Capacity Table'!$C$62:$E$72,2,FALSE),\"-\",VLOOKUP(G13,'10A22 Capacity Table'!$C$62:$E$72,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$62:$C$72>'10A22 Alarm Results'!$E$12,'10A22 Capacity Table'!$C$62:$C$72))","v":{"$error":"#N/A"}},{"$f":"G13/10","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(530*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(492*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G13/SQRT(('10A22 Alarm Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Alarm Results'!$A$12)/('10A22 Alarm Results'!$A$12*'10A22 Alarm Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"I13/10","v":{"$error":"#VALUE!"}},{"$f":"IF(I13<0.99999,ROUND(I13,2),\nIF(I13<9.999,ROUND(I13,2),\nIF(I13<99.99,ROUND(I13,1),\nIF(I13<999.99,ROUND(I13,0),\nIF(I13<9999.99,ROUND(I13,-1),\nIF(I13<99999,ROUND(I13,-2),ROUND(I13,2)))))))","v":{"$error":"#VALUE!"}},{"$f":"ROUND(J13,1)","v":{"$error":"#VALUE!"}},{"$f":"CONCATENATE(L13,\" \",\"-\",\" \",K13)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G14,'10A22 Capacity Table'!$C$62:$E$72,2,FALSE),\"-\",VLOOKUP(G14,'10A22 Capacity Table'!$C$62:$E$72,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$62:$C$72>'10A22 Alarm Results'!$G$13,'10A22 Capacity Table'!$C$62:$C$72))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(530*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(492*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G14/SQRT(('10A22 Alarm Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Alarm Results'!$A$12)/('10A22 Alarm Results'!$A$12*'10A22 Alarm Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,{"$f":"CONCATENATE(VLOOKUP(G15,'10A22 Capacity Table'!$C$62:$E$72,2,FALSE),\"-\",VLOOKUP(G15,'10A22 Capacity Table'!$C$62:$E$72,3,FALSE))","v":{"$error":"#N/A"}},{"$f":"MIN(IF('10A22 Capacity Table'!$C$62:$C$72>'10A22 Alarm Results'!$G$14,'10A22 Capacity Table'!$C$62:$C$72))","v":{"$error":"#N/A"}},{"$error":"#N/A"},{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(530*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT((14.7*'10A22 Alarm Results'!$D$12*'10A22 Alarm Results'!$A$12)/(492*'10A22 Alarm Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!D12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(G15/SQRT(('10A22 Alarm Results'!$B$12*('10A61 5\" Calcs'!O46/0.0012)*'10A22 Alarm Results'!$A$12)/('10A22 Alarm Results'!$A$12*'10A22 Alarm Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!C5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!F12,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!J5,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!M12,\"\"))","v":""}]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!C6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!F13,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!J6,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!M13,\"\"))","v":""}]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!C7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!F14,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!J7,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!M14,\"\"))","v":""}]
[null,null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!C8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!F15,\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'10A22 Alarm Results'!J8,\nIF('VA Sizing'!$C$3=\"Gas\",'10A22 Alarm Results'!M15,\"\"))","v":""}]
[]
[null,null,null,"Output"]
[null,null,null,"Tube/Float","Range"]
[null,null,null,{"$f":"IFERROR(D19,\"\")","v":""},{"$f":"IF(D26=\"\",\"\",E19)","v":""}]
[null,null,null,{"$f":"IFERROR(D20,\"\")","v":""},{"$f":"IF(D27=\"\",\"\",E20)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(D27=\"\",\"\",D21),\"\")","v":""},{"$f":"IF(D28=\"\",\"\",E21)","v":""}]
[null,null,null,{"$f":"IFERROR(IF(OR(D27=\"\",D28=\"\"),\"\",D22),\"\")","v":""},{"$f":"IF(D29=\"\",\"\",E22)","v":""}]

{"sheet":"Modified Inputs","index":64,"n_rows":62,"n_cols":15,"rows_kept":62,"cut":false,"hidden":true,"merged":[]}
[null,"FLUID TYPE","FLUID NAME","REFERENCE CONDITION","Type of Density",null,"Input Viscosity (cP)","Input Pressure","Modified Pressure (psia)","Input Temperature","Modified Temperature (Deg F)","Input Density at operating","Modified Density at operating (g/mL)","Input Flowrate","Modified Flowrate (mL/min)"]
[null,"Liquid",{"$f":"IF('VA Sizing'!C3=\"Liquid\",\"\",\nIF('VA Sizing'!C3=\"Gas\",\"Air\",\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Actual\",\"\")","v":""},"at Reference Conditions",null,{"$f":"IF('VA Sizing'!$D$8=\"cP\",'VA Sizing'!$C$8,'VA Sizing'!C8*'Modified Inputs'!$M$2)","v":0},{"$f":"'VA Sizing'!$C$9","v":0},{"$f":"IF('VA Sizing'!D9=\"kpa(a)\",'Modified Inputs'!H2*0.145038,\nIF('VA Sizing'!D9=\"kpa(g)\",'Modified Inputs'!H2*0.145038+14.7,\nIF('VA Sizing'!D9=\"inH2O(a)\",'Modified Inputs'!H2*0.0360912,\nIF('VA Sizing'!D9=\"inH2O(g)\",'Modified Inputs'!H2*0.0360912+14.7,\nIF('VA Sizing'!D9=\"kg/cm2(a)\",'Modified Inputs'!H2*14.2233,\nIF('VA Sizing'!D9=\"kg/cm2(g)\",'Modified Inputs'!H2*14.2233+14.7,$I$3))))))","v":0},{"$f":"'VA Sizing'!C10","v":0},{"$f":"IF('VA Sizing'!D10='Modified Inputs'!G10,'Modified Inputs'!J2*9/5+32,'Modified Inputs'!J2)","v":0},{"$f":"'VA Sizing'!C11","v":0},{"$f":"IF('VA Sizing'!$D$11='Modified Inputs'!$H$8,'Modified Inputs'!L2,\nIF('VA Sizing'!$D$11='Modified Inputs'!$H$9,'Modified Inputs'!L2*0.001,\nIF('VA Sizing'!$D$11='Modified Inputs'!$H$10,'Modified Inputs'!L2,\nIF('VA Sizing'!$D$11='Modified Inputs'!$H$11,'Modified Inputs'!L2,\nIF('VA Sizing'!$D$11='Modified Inputs'!$H$12,'Modified Inputs'!L2,\nIF('VA Sizing'!$D$11='Modified Inputs'!$H$13,'Modified Inputs'!L2*0.0160184,\nIF('VA Sizing'!$D$11='Modified Inputs'!$H$14,'Modified Inputs'!L2*0.119826,'Modified Inputs'!L2)))))))","v":0},{"$f":"'VA Sizing'!C12","v":0},{"$f":"N2/VLOOKUP('VA Sizing'!D12,'Modified Inputs'!I8:J32,2,FALSE)","v":{"$error":"#N/A"}}]
[null,"Gas",{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",\"Potable Water\",\nIF('VA Sizing'!$C$3=\"Gas\",\"Argon (Ar)\",\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Normal\",\"\")","v":""},"at Operating Conditions",null,null,null,{"$f":"IF('VA Sizing'!D9=\"psi(g)\",'Modified Inputs'!H2+14.7,\nIF('VA Sizing'!D9=\"bar(a)\",'Modified Inputs'!H2*14.5,\nIF('VA Sizing'!D9=\"bar(g)\",'Modified Inputs'!H2*14.5+14.7,\nIF('VA Sizing'!D9=\"atm(a)\",'Modified Inputs'!H2*14.7,\nIF('VA Sizing'!D9=\"atm(g)\",'Modified Inputs'!H2*14.7+14.7,'Modified Inputs'!H2)))))","v":0},{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",'VA Sizing'!$C$9=\"Optional\",'VA Sizing'!$N$2=\"10A32\"),0,\nIF('VA Sizing'!$C$4=\"Steam\",(Steam!$C$17-14.7)*0.0689476,\nIF('VA Sizing'!$D$9=\"bar(g)\",'VA Sizing'!$C$9,(I2-14.7)*0.0689476)))","v":-1.01352972},{"$f":"(K2+460)*(5/9)","v":255.55555555555557},"Input Density at reference","Modified Density at reference (g/mL)",500]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",\"Other Water\",\nIF('VA Sizing'!$C$3=\"Gas\",\"Butane (C4H10)\",\"\"))","v":""},{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Standard\",\"\")","v":""},null,null,"Viscosity Units",null,null,"bar(g)^",null,{"$f":"'VA Sizing'!C7","v":0},{"$f":"IF('VA Sizing'!$D$7='Modified Inputs'!$H$9,'Modified Inputs'!L4*0.001,\nIF('VA Sizing'!$D$7='Modified Inputs'!$H$10,'Modified Inputs'!L4,\nIF('VA Sizing'!$D$7='Modified Inputs'!$H$11,'Modified Inputs'!L4,\nIF('VA Sizing'!$D$7='Modified Inputs'!$H$12,'Modified Inputs'!L4,\nIF('VA Sizing'!$D$7='Modified Inputs'!$H$13,'Modified Inputs'!L4*0.0160184,\nIF('VA Sizing'!$D$7='Modified Inputs'!$H$14,'Modified Inputs'!L4*0.119826,'Modified Inputs'!L4))))))","v":0}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",\"Other Liquid\",\nIF('VA Sizing'!$C$3=\"Gas\",\"Acetylene (C2H2)\",\"\"))","v":""},null,null,null,"cP"]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Ammonia (NH3)\",\"\")","v":""},null,null,null,"cSt",null,"Flowrate Units","Flowrate Conversion"]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Carbon Monoxide (CO)\",\"\")","v":""},null,null,null,null,"Density Units",null,null,null,{"$f":"IF(AND(OR('VA Sizing'!N2=\"10A61\",'VA Sizing'!N2=\"10A22\",'VA Sizing'!N2=\"10A4\"),OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\")),1,0)","v":0}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Carbon Dioxide (CO2)\",\"\")","v":""},null,null,"Pressure Units","Temperature Units",{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",\"S.G.\",\"\")","v":""},{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),\"sccm\",\"cc/min\")","v":"cc/min"},1,null,{"$f":"IF('VA Sizing'!$N$2=\"10A32\",\"Please consult the factory or the 10A32 Specification Sheet for the meter's temperature and pressure limitations\",\nIF(L7=1,\"ABB recommends that glass tube meters not be used with hazardous gases.  It is safer to use a metal 10A32 or FAM54 Meter for this application. Please contact the factory for exceptions.\",\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Chlorine (Cl2)\",\"\")","v":""},null,null,"psi(a)","°F","kg/m3","mL/min",1]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Ethane (C2H6)\",\"\")","v":""},null,null,"psi(g)","°C","kg/L","mL/h",60]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Ethylene (C2H4)\",\"\")","v":""},null,null,"bar(a)",null,"g/mL","mL/s",{"$f":"1/60","v":1.6666666666666666E-2}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Helium (He)\",\"\")","v":""},null,null,"bar(g)",null,"g/cm3","l/h",0.06]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Hydrochloric Acid (HCl)\",\"\")","v":""},null,null,"atm(a)",null,"lb/ft3","l/min",1E-3]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Hydrogen (H2)\",\"\")","v":""},null,null,"atm(g)",null,"lb/USgal","l/s",1.6666666699999999E-5]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Hydrogen Sulfide (H2S)\",\"\")","v":""},null,null,"kpa(a)",null,null,"m3/h",6.0000000000000002E-5,null,"g/mL",1]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Krypton (Kr)\",\"\")","v":""},null,null,"kpa(g)","⁰F",null,"m3/min",9.9999999999999995E-7,null,"g/cm3",1]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Methane (CH4)\",\"\")","v":""},null,null,"inH2O(a)","⁰C",null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),\"scfh\",\"ft3/h\")","v":"ft3/h"},2.1189999999999998E-3,null,"kg/m3",1E-3]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Methyl Chloride (CH3Cl)\",\"\")","v":""},null,null,"inH2O(g)",null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),\"scfm\",\"ft3/min\")","v":"ft3/min"},3.5309999999999999E-5,null,"kg/L",1]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Natural Gas\",\"\")","v":""},null,null,"kg/cm2(a)",null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'VA Sizing'!$C$5=\"Standard\"),\"scfs\",\"ft3/s\")","v":"ft3/s"},5.8859999999999996E-7,null,"lb/ft3",1.6018399999999999E-2]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Neon (Ne)\",\"\")","v":""},null,null,"kg/cm2(g)",null,null,"I GPH",1.32E-2,null,"lb/USgal",0.119826]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Nitric Oxide (NO)\",\"\")","v":""},null,null,null,null,null,"I GPM",2.2000000000000001E-4]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Nitrogen (N2)\",\"\")","v":""},null,null,null,null,null,"US GPH",1.585E-2]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Nitrous Oxide (N2O)\",\"\")","v":""},null,null,null,null,null,"US GPM",2.6420000000000003E-4]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Oxygen (O2)\",\"\")","v":""},null,null,null,null,null,"in3/h",3.6629999999999998]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Propane (C3H8)\",\"\")","v":""},null,null,null,null,null,"in3/min",6.1019999999999998E-2]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Propylene (C3H6)\",\"\")","v":""},null,null,null,null,null,"in3/s",1.018E-3]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\"Sulfur Dioxide (SO2)\",\"\")","v":""},null,null,null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Standard\",'VA Sizing'!$C$5=\"Normal\")),\"\",\"g/min\")","v":"g/min"},{"$f":"IF('VA Sizing'!C3=\"Gas\",'10A61 5\" Calcs'!O46,\nIF('VA Sizing'!C3=\"Liquid\",'Modified Inputs'!M2,\"\"))","v":""}]
[null,null,{"$f":"IF('VA Sizing'!$C$3=\"Gas\",\" Other\",\"\")","v":""},null,null,null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Standard\",'VA Sizing'!$C$5=\"Normal\")),\"\",\"g/h\")","v":"g/h"},{"$f":"IF('VA Sizing'!C3=\"Gas\",'10A61 5\" Calcs'!O46*60,\nIF('VA Sizing'!C3=\"Liquid\",'Modified Inputs'!M2*60,\"\"))","v":""}]
[null,null,null,null,null,null,null,null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Standard\",'VA Sizing'!$C$5=\"Normal\")),\"\",\"kg/min\")","v":"kg/min"},{"$f":"IF('VA Sizing'!C3=\"Gas\",'10A61 5\" Calcs'!O46/1000,\nIF('VA Sizing'!C3=\"Liquid\",'Modified Inputs'!M2/1000,\"\"))","v":""}]
[null,null,null,"Volume %",null,null,"List of Meters",null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Standard\",'VA Sizing'!$C$5=\"Normal\")),\"\",\"kg/h\")","v":"kg/h"},{"$f":"IF('VA Sizing'!C3=\"Gas\",'10A61 5\" Calcs'!O46*(60/1000),\nIF('VA Sizing'!C3=\"Liquid\",'Modified Inputs'!M2*(60/1000),\"\"))","v":""}]
[null,null,null,"Mass %",null,"10A61",{"$f":"IF('VA Sizing'!$C$4=\"Steam\",\"10A32\",\nIF('VA Sizing'!$C$12=\"\",\"\",\"10A61\"))","v":""},null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Standard\",'VA Sizing'!$C$5=\"Normal\")),\"\",\"lb/min\")","v":"lb/min"},{"$f":"IF('VA Sizing'!C3=\"Gas\",'10A61 5\" Calcs'!O46/453.592,\nIF('VA Sizing'!C3=\"Liquid\",'Modified Inputs'!M2/453.592,\"\"))","v":""}]
[null,null,null,null,null,"10A32",{"$f":"IF('VA Sizing'!$C$4=\"Steam\",\"FAM54\",\nIF('VA Sizing'!$C$12=\"\",\"\",\"10A4\"))","v":""},null,{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",OR('VA Sizing'!$C$5=\"Standard\",'VA Sizing'!$C$5=\"Normal\")),\"\",\"lb/h\")","v":"lb/h"},{"$f":"IF('VA Sizing'!C3=\"Gas\",'10A61 5\" Calcs'!O46*(60/453.592),\nIF('VA Sizing'!C3=\"Liquid\",'Modified Inputs'!M2*(60/453.592),\"\"))","v":""}]
[null,null,null,null,null,"10A4",{"$f":"IF('VA Sizing'!$C$4=\"Steam\",\"\",\nIF('VA Sizing'!$C$12=\"\",\"\",\"10A22\"))","v":""}]
[null,null,null,null,null,"10A22",{"$f":"IF('VA Sizing'!$C$4=\"Steam\",\"\",\nIF('VA Sizing'!$C$12=\"\",\"\",\"10A32\"))","v":""},null,"cc/min","Actual","S.G."]
[null,null,null,null,null,null,{"$f":"IF('VA Sizing'!$C$4=\"Steam\",\"\",\nIF('VA Sizing'!$C$12=\"\",\"\",\"FAM54\"))","v":""},null,"sccm","Normal","kg/m3"]
[null,null,null,null,null,null,null,null,"mL/min","Standard","kg/L"]
[null,null,null,null,null,null,null,null,"mL/h",null,"g/mL"]
[null,null,null,null,null,null,null,null,"mL/s",null,"g/cm3"]
[null,null,null,{"$f":"IF('VA Sizing'!V22=\"Additional Floats\",\"Alarm Floats\",\"\")","v":""},null,null,null,null,"l/h",null,"lb/ft3"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!V22=\"Additional Floats\",'VA Sizing'!C3=\"Liquid\"),\"Teflon Floats (PTFE)\",\"\")","v":""},"Tantalum Floats (TA)",null,null,null,"l/min",null,"lb/USgal"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!V22=\"Additional Floats\",'VA Sizing'!C3=\"Liquid\"),\"PVC Floats\",\"\")","v":""},null,null,null,null,"l/s"]
[null,null,null,{"$f":"IF(AND('VA Sizing'!V22=\"Additional Floats\",'VA Sizing'!C3=\"Liquid\"),\"PVC Floats\",\"\")","v":""},null,null,null,null,"m3/h"]
[null,null,null,null,null,null,null,null,"m3/min"]
[null,null,null,null,null,null,null,null,"scfh"]
[null,null,null,null,null,null,null,null,"ft3/h"]
[null,null,null,null,null,null,null,null,"scfm"]
[null,null,null,null,null,null,null,null,"ft3/min"]
[null,null,null,null,null,null,null,null,"scfs"]
[null,null,null,null,null,null,null,null,"ft3/s"]
[null,null,null,null,null,null,null,null,"I GPH"]
[null,null,null,null,null,null,null,null,"I GPM"]
[null,null,null,null,null,null,null,null,"US GPH"]
[null,null,null,null,null,null,null,null,"US GPM"]
[null,null,null,null,null,null,null,null,"in3/h"]
[null,null,null,null,null,null,null,null,"in3/min"]
[null,null,null,null,null,null,null,null,"in3/s"]
[null,null,null,null,null,null,null,null,"g/min"]
[null,null,null,null,null,null,null,null,"g/h"]
[null,null,null,null,null,null,null,null,"kg/min"]
[null,null,null,null,null,null,null,null,"kg/h"]
[null,null,null,null,null,null,null,null,"lb/min"]
[null,null,null,null,null,null,null,null,"lb/h"]

{"sheet":"10A22 Capacity Table","index":65,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":true,"merged":[[3,2,3,5],[24,2,24,5],[41,2,41,5],[59,2,59,5]]}
[]
[]
[]
[null,null,"Liquid Standard"]
[null,"Water GPM","Compensated Water GPM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded"]
[null,0.36,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B6,\nIF(20.99<'Modified Inputs'!G2,\"viscosity\",'10A22 Curves'!F7*('Modified Inputs'!G2)^5+'10A22 Curves'!G7*('Modified Inputs'!G2)^4+'10A22 Curves'!H7*('Modified Inputs'!G2)^3+'10A22 Curves'!I7*('Modified Inputs'!G2)^2+'10A22 Curves'!J7*'Modified Inputs'!G2+'10A22 Curves'!K7))","v":0.36},"1/4\"","1B",21,{"$f":"IFERROR((C6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(G6<0.99999,ROUND(G6,2),\nIF(G6<9.999,ROUND(G6,2),\nIF(G6<99.99,ROUND(G6,1),\nIF(G6<999.99,ROUND(G6,0),\nIF(G6<9999.99,ROUND(G6,-1),\nIF(G6<99999,ROUND(G6,-2),ROUND(G6,2))))))),\"viscosity\")","v":"viscosity"}]
[null,0.6,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B7,\nIF('Modified Inputs'!G2>49.99,\"viscosity\",IF('Modified Inputs'!G2<20.01,'10A22 Curves'!F28*LN('Modified Inputs'!G2)+'10A22 Curves'!G28,'10A22 Curves'!M29*LN('Modified Inputs'!G2)+'10A22 Curves'!N29)))","v":0.6},"1/4\"","1C",50,{"$f":"IFERROR((C7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(G7<0.99999,ROUND(G7,2),\nIF(G7<9.999,ROUND(G7,2),\nIF(G7<99.99,ROUND(G7,1),\nIF(G7<999.99,ROUND(G7,0),\nIF(G7<9999.99,ROUND(G7,-1),\nIF(G7<99999,ROUND(G7,-2),ROUND(G7,2))))))),\"viscosity\")","v":"viscosity"}]
[null,1,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B8,\nIF('Modified Inputs'!G2>99.99,\"viscosity\",IF('Modified Inputs'!G2<35.01,'10A22 Curves'!G46,'10A22 Curves'!N47)))","v":1},"1/2\"","1D",100,{"$f":"IFERROR((C8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,2,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B9,\nIF('Modified Inputs'!G2>274.99,\"viscosity\",IF('Modified Inputs'!G2<49.99,'10A22 Curves'!H77,'10A22 Curves'!O77)))","v":2},"1/2\"","1F",275,{"$f":"IFERROR((C9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,3,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B10,\nIF('Modified Inputs'!G2>499.99,\"viscosity\",IF('Modified Inputs'!G2<10.0001,'10A22 Curves'!$H$92,'10A22 Curves'!$P$92)))","v":3},"1/2\"","1G",500,{"$f":"IFERROR((C10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,4,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B11,\nIF('Modified Inputs'!G2>899.99,\"viscosity\",IF('Modified Inputs'!G2<80.01,'10A22 Curves'!F106,'10A22 Curves'!Q106)))","v":4},"1/2\"","1H",900,{"$f":"IFERROR((C11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,6,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B12,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<100.01,'10A22 Curves'!$E$121,'10A22 Curves'!$Q$119)))","v":6},"1\"","1J",1000,{"$f":"IFERROR((C12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,8,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B13,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<70.01,'10A22 Curves'!E139,'10A22 Curves'!S137)))","v":8},"1\"","1K",1000,{"$f":"IFERROR((C13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,11,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B14,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<150.01,'10A22 Curves'!I155,'10A22 Curves'!O155)))","v":11},"1\"","1L",1000,{"$f":"IFERROR((C14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,15,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B15,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<100.01,'10A22 Curves'!$I$169,'10A22 Curves'!$P$168)))","v":15},"1-1/2\"","1M",1000,{"$f":"IFERROR((C15/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,20,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B16,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<300.01,'10A22 Curves'!$J$183,'10A22 Curves'!$P$183)))","v":20},"1-1/2\"","1N",1000,{"$f":"IFERROR((C16/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,24,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B17,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<120.01,'10A22 Curves'!$G$199,'10A22 Curves'!$N$198)))","v":24},"1-1/2\"","1P",1000,{"$f":"IFERROR((C17/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,35,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B18,\nIF('Modified Inputs'!G2>1.99,\"viscosity\",'10A22 Curves'!J207))","v":35},"2\"","1Q",2,{"$f":"IFERROR((C18/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,50,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B19,\nIF('Modified Inputs'!G2>1.99,\"viscosity\",'10A22 Curves'!M219))","v":50},"2\"","1R",2,{"$f":"IFERROR((C19/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,0,0,null,null,0,{"$f":"IFERROR((C20/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[]
[]
[]
[]
[null,null,"Liquid Alarm"]
[null,"Water GPM","Compensated Water GPM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded"]
[null,1.3,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B27,\nIF('Modified Inputs'!G2>149.99,\"viscosity\",IF('Modified Inputs'!G2<40.01,'10A22 Curves'!$G$61,'10A22 Curves'!$O$62)))","v":1.3},"1/2\"","1E",150,{"$f":"IFERROR((C27/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(G27<0.99999,ROUND(G27,2),\nIF(G27<9.999,ROUND(G27,2),\nIF(G27<99.99,ROUND(G27,1),\nIF(G27<999.99,ROUND(G27,0),\nIF(G27<9999.99,ROUND(G27,-1),\nIF(G27<99999,ROUND(G27,-2),ROUND(G27,2))))))),\"viscosity\")","v":"viscosity"}]
[null,2,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B28,\nIF('Modified Inputs'!G2>274.99,\"viscosity\",IF('Modified Inputs'!G2<49.99,'10A22 Curves'!H77,'10A22 Curves'!O77)))","v":2},"1/2\"","1F",275,{"$f":"IFERROR((C28/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(G28<0.99999,ROUND(G28,2),\nIF(G28<9.999,ROUND(G28,2),\nIF(G28<99.99,ROUND(G28,1),\nIF(G28<999.99,ROUND(G28,0),\nIF(G28<9999.99,ROUND(G28,-1),\nIF(G28<99999,ROUND(G28,-2),ROUND(G28,2))))))),\"viscosity\")","v":"viscosity"}]
[null,4,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B29,\nIF('Modified Inputs'!G2>899.99,\"viscosity\",IF('Modified Inputs'!G2<80.01,'10A22 Curves'!F106,'10A22 Curves'!Q106)))","v":4},"1/2\"","1H",900,{"$f":"IFERROR((C29/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,6,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B30,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<100.01,'10A22 Curves'!$E$121,'10A22 Curves'!$Q$119)))","v":6},"1\"","1J",1000,{"$f":"IFERROR((C30/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,8,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B31,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<70.01,'10A22 Curves'!E139,'10A22 Curves'!S137)))","v":8},"1\"","1K",1000,{"$f":"IFERROR((C31/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,11,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B32,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<150.01,'10A22 Curves'!I155,'10A22 Curves'!O155)))","v":11},"1\"","1L",1000,{"$f":"IFERROR((C32/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,15,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B33,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<100.01,'10A22 Curves'!$I$169,'10A22 Curves'!$P$168)))","v":15},"1-1/2\"","1M",1000,{"$f":"IFERROR((C33/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,20,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B34,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<300.01,'10A22 Curves'!$J$183,'10A22 Curves'!$P$183)))","v":20},"1-1/2\"","1N",1000,{"$f":"IFERROR((C34/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,24,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B35,\nIF('Modified Inputs'!G2>999.99,\"viscosity\",IF('Modified Inputs'!G2<120.01,'10A22 Curves'!$G$199,'10A22 Curves'!$N$198)))","v":24},"1-1/2\"","1P",1000,{"$f":"IFERROR((C35/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,35,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B36,\nIF('Modified Inputs'!G2>1.99,\"viscosity\",'10A22 Curves'!J207))","v":35},"2\"","1Q",2,{"$f":"IFERROR((C36/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,50,{"$f":"IF(OR('Modified Inputs'!G2=1,'Modified Inputs'!G2<1),'10A22 Capacity Table'!B37,\nIF('Modified Inputs'!G2>1.99,\"viscosity\",'10A22 Curves'!M219))","v":50},"2\"","1R",2,{"$f":"IFERROR((C37/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity"]
[null,0,0,null,null,0]
[]
[]
[]
[null,null,"Gas Standard"]
[null,null,"Air SCFM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded"]
[null,0.6,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B44)","v":0.6},"1/4\"","2B",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C44/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C44/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C44/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(G44<0.99999,ROUND(G44,2),\nIF(G44<9.999,ROUND(G44,2),\nIF(G44<99.99,ROUND(G44,1),\nIF(G44<999.99,ROUND(G44,0),\nIF(G44<9999.99,ROUND(G44,-1),\nIF(G44<99999,ROUND(G44,-2),ROUND(G44,2)))))))","v":{"$error":"#VALUE!"}}]
[null,1.3,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B45)","v":1.3},"1/4\"","2C",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C45/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C45/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C45/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(G45<0.99999,ROUND(G45,2),\nIF(G45<9.999,ROUND(G45,2),\nIF(G45<99.99,ROUND(G45,1),\nIF(G45<999.99,ROUND(G45,0),\nIF(G45<9999.99,ROUND(G45,-1),\nIF(G45<99999,ROUND(G45,-2),ROUND(G45,2)))))))","v":{"$error":"#VALUE!"}}]
[null,2,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B46)","v":2},"1/2\"","2D",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C46/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C46/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C46/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,4.5,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B47)","v":4.5},"1/2\"","2E",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C47/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C47/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C47/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,7,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B48)","v":7},"1/2\"","2G",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C48/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C48/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C48/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,9,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B49)","v":9},"1/2\"","2K",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C49/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C49/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C49/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,14,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B50)","v":14},"1\"","2L",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C50/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C50/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C50/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,20,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B51)","v":20},"1\"","2N",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C51/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C51/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C51/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,26,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B52)","v":26},"1\"","2P",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C52/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C52/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C52/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,36,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B53)","v":36},"1-1/2\"","2Q",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C53/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C53/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C53/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,50,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B54)","v":50},"1-1/2\"","2R",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C54/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C54/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C54/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,60,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B55)","v":60},"1-1/2\"","2S",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C55/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C55/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C55/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,80,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B56)","v":80},"2\"","2T",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C56/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C56/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C56/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,110,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B57)","v":110},"2\"","2U",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C57/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C57/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C57/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[]
[]
[null,null,"Gas Alarms"]
[null,null,"Air SCFM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded"]
[null,5.5,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B62)","v":5.5},"1/2\"","2F",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C62/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C62/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C62/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(G62<0.99999,ROUND(G62,2),\nIF(G62<9.999,ROUND(G62,2),\nIF(G62<99.99,ROUND(G62,1),\nIF(G62<999.99,ROUND(G62,0),\nIF(G62<9999.99,ROUND(G62,-1),\nIF(G62<99999,ROUND(G62,-2),ROUND(G62,2)))))))","v":{"$error":"#VALUE!"}}]
[null,8.5,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B63)","v":8.5},"1/2\"","2H",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C63/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C63/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C63/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(G63<0.99999,ROUND(G63,2),\nIF(G63<9.999,ROUND(G63,2),\nIF(G63<99.99,ROUND(G63,1),\nIF(G63<999.99,ROUND(G63,0),\nIF(G63<9999.99,ROUND(G63,-1),\nIF(G63<99999,ROUND(G63,-2),ROUND(G63,2)))))))","v":{"$error":"#VALUE!"}}]
[null,9,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B64)","v":9},"1/2\"","2J",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C64/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C64/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C64/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,14,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B65)","v":14},"1\"","2L",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C65/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C65/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C65/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,19,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B66)","v":19},"1\"","2M",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C66/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C66/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C66/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,26,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B67)","v":26},"1\"","2P",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C67/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C67/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C67/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,36,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B68)","v":36},"1-1/2\"","2Q",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C68/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C68/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C68/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,50,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B69)","v":50},"1-1/2\"","2R",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C69/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C69/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C69/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,60,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B70)","v":60},"1-1/2\"","2S",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C70/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C70/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C70/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,80,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B71)","v":80},"2\"","2T",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C71/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C71/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C71/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]
[null,110,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",B72)","v":110},"2\"","2U",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C72/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C72/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(C72/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"}]

{"sheet":"BasicMeter10A22 Standard Liquid","index":66,"n_rows":58,"n_cols":40,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,5,1,8],[2,26,2,27]]}
[]
[null,"Current Tab","Current Step",null,null,"Liquid Standard",null,null,null,null,null,null,null,null,null,"10A22 All",null,null,null,"10A22\" Range Limit",null,null,"10A22 Range Limit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,"Water GPM","Compensated Water GPM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded",null,null,null,null,"Tube/Float","Max Rounded","Tube/Float",null,"Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded",null,null,"Final Standard"]
[null,null,null,null,0.36,{"$f":"'10A22 Capacity Table'!C6","v":0.36},"1/4\"","1B",21,{"$f":"IFERROR((F4/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(J4<0.00000099999,ROUND(J4,7),\nIF(J4<0.0000099999,ROUND(J4,6),\nIF(J4<0.000099999,ROUND(J4,5),\nIF(J4<0.00099999,ROUND(J4,4),\nIF(J4<0.0099999,ROUND(J4,3),\nIF(J4<0.099999,ROUND(J4,2),\nIF(J4<0.99999,ROUND(J4,2),\nIF(J4<9.999,ROUND(J4,2),\nIF(J4<99.99,ROUND(J4,1),\nIF(J4<999.99,ROUND(J4,0),\nIF(J4<9999.99,ROUND(J4,-1),\nIF(J4<99999,ROUND(J4,-2),ROUND(J4,2))))))))))))),\"viscosity\")","v":"viscosity"},null,null,null,null,{"$f":"CONCATENATE(G4,\"-\",H4)","v":"1/4\"-1B"},{"$f":"K4","v":"viscosity"},{"$f":"P4","v":"1/4\"-1B"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q4*0.45),'BasicMeter10A22 Standard Liquid'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q4*0.45),'BasicMeter10A22 Standard Liquid'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(X4,$Q$4:$R$17,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$17>0,U4:U17))","v":0},null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,null,0.6,{"$f":"'10A22 Capacity Table'!C7","v":0.6},"1/4\"","1C",50,{"$f":"IFERROR((F5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(J5<0.00000099999,ROUND(J5,7),\nIF(J5<0.0000099999,ROUND(J5,6),\nIF(J5<0.000099999,ROUND(J5,5),\nIF(J5<0.00099999,ROUND(J5,4),\nIF(J5<0.0099999,ROUND(J5,3),\nIF(J5<0.099999,ROUND(J5,2),\nIF(J5<0.99999,ROUND(J5,2),\nIF(J5<9.999,ROUND(J5,2),\nIF(J5<99.99,ROUND(J5,1),\nIF(J5<999.99,ROUND(J5,0),\nIF(J5<9999.99,ROUND(J5,-1),\nIF(J5<99999,ROUND(J5,-2),ROUND(J5,2))))))))))))),\"viscosity\")","v":"viscosity"},null,null,null,null,{"$f":"CONCATENATE(G5,\"-\",H5)","v":"1/4\"-1C"},{"$f":"K5","v":"viscosity"},{"$f":"P5","v":"1/4\"-1C"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q5*0.45),'BasicMeter10A22 Standard Liquid'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q5*0.45),'BasicMeter10A22 Standard Liquid'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(X5,$Q$4:$R$17,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$17<X4,$U$4:$U$17))","v":0},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$W$33,1/0),\nIFERROR(IF($Z$32=\"\",$W$32,1/0),\nIFERROR(IF($Z$31=\"\",$W$31,1/0),\nIFERROR(IF($Z$30=\"\",$W$30,1/0),\nIFERROR(IF($Z$29=\"\",$W$29,1/0),\nIFERROR(IF($Z$28=\"\",$W$28,1/0),\nIFERROR(IF($Z$27=\"\",$W$27,1/0),\nIFERROR(IF($Z$26=\"\",$W$26,1/0),\nIFERROR(IF($Z$25=\"\",$W$25,1/0),\nIFERROR(IF($Z$24=\"\",$W$24,1/0),\nIFERROR(IF($Z$23=\"\",$W$23,1/0),\nIFERROR(IF($Z$22=\"\",$W$22,1/0),\nIFERROR(IF($Z$21=\"\",$W$21,1/0),\nIFERROR(IF($Z$20=\"\",$W$20,1/0),\nIFERROR(IF($Z$19=\"\",$W$19,1/0),\nIFERROR(IF($Z$18=\"\",$W$18,1/0),\nIFERROR(IF($Z$17=\"\",$W$17,1/0),\nIFERROR(IF($Z$16=\"\",$W$16,1/0),\nIFERROR(IF($Z$15=\"\",$W$15,1/0),\nIFERROR(IF($Z$14=\"\",$W$14,1/0),\nIFERROR(IF($Z$13=\"\",$W$13,1/0),\nIFERROR(IF($Z$12=\"\",$W$12,1/0),\nIFERROR(IF($Z$11=\"\",$W$11,1/0),\nIFERROR(IF($Z$10=\"\",$W$10,1/0),\nIFERROR(IF($Z$9=\"\",$W$9,1/0),\nIFERROR(IF($Z$8=\"\",$W$8,1/0),\nIFERROR(IF($Z$7=\"\",$W$7,1/0),\nIFERROR(IF($Z$6=\"\",$W$6,1/0),\nIFERROR(IF($Z$5=\"\",$W$5,1/0),\nIFERROR(IF($Z$4=\"\",$W$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AA5,$W$4:$X$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IF(AA5=\"none\",\"sizing\",\"\")","v":"sizing"},null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,null,1,{"$f":"'10A22 Capacity Table'!C8","v":1},"1/2\"","1D",100,{"$f":"IFERROR((F6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1/2\"-1D","viscosity","1/2\"-1D",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q6*0.45),'BasicMeter10A22 Standard Liquid'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q6*0.45),'BasicMeter10A22 Standard Liquid'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X5,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,null,2,{"$f":"'10A22 Capacity Table'!C9","v":2},"1/2\"","1F",275,{"$f":"IFERROR((F7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1/2\"-1F","viscosity","1/2\"-1F",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q7*0.45),'BasicMeter10A22 Standard Liquid'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q7*0.45),'BasicMeter10A22 Standard Liquid'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X6,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,null,3,{"$f":"'10A22 Capacity Table'!C10","v":3},"1/2\"","1G",500,{"$f":"IFERROR((F8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1/2\"-1G","viscosity","1/2\"-1G",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q8*0.45),'BasicMeter10A22 Standard Liquid'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q8*0.45),'BasicMeter10A22 Standard Liquid'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X7,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,null,4,{"$f":"'10A22 Capacity Table'!C11","v":4},"1/2\"","1H",900,{"$f":"IFERROR((F9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1/2\"-1H","viscosity","1/2\"-1H",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q9*0.45),'BasicMeter10A22 Standard Liquid'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q9*0.45),'BasicMeter10A22 Standard Liquid'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X8,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,null,6,{"$f":"'10A22 Capacity Table'!C12","v":6},"1\"","1J",1000,{"$f":"IFERROR((F10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1\"-1J","viscosity","1\"-1J",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q10*0.45),'BasicMeter10A22 Standard Liquid'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q10*0.45),'BasicMeter10A22 Standard Liquid'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X9,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,null,8,{"$f":"'10A22 Capacity Table'!C13","v":8},"1\"","1K",1000,{"$f":"IFERROR((F11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1\"-1K","viscosity","1\"-1K",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q11*0.45),'BasicMeter10A22 Standard Liquid'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q11*0.45),'BasicMeter10A22 Standard Liquid'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X10,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,null,11,{"$f":"'10A22 Capacity Table'!C14","v":11},"1\"","1L",1000,{"$f":"IFERROR((F12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1\"-1L","viscosity","1\"-1L",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q12*0.45),'BasicMeter10A22 Standard Liquid'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q12*0.45),'BasicMeter10A22 Standard Liquid'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X11,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,null,15,{"$f":"'10A22 Capacity Table'!C15","v":15},"1-1/2\"","1M",1000,{"$f":"IFERROR((F13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1-1/2\"-1M","viscosity","1-1/2\"-1M",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q13*0.45),'BasicMeter10A22 Standard Liquid'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q13*0.45),'BasicMeter10A22 Standard Liquid'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X12,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,null,20,{"$f":"'10A22 Capacity Table'!C16","v":20},"1-1/2\"","1N",1000,{"$f":"IFERROR((F14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1-1/2\"-1N","viscosity","1-1/2\"-1N",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q14*0.45),'BasicMeter10A22 Standard Liquid'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q14*0.45),'BasicMeter10A22 Standard Liquid'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X13,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,null,24,{"$f":"'10A22 Capacity Table'!C17","v":24},"1-1/2\"","1P",1000,{"$f":"IFERROR((F15/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1-1/2\"-1P","viscosity","1-1/2\"-1P",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q15*0.45),'BasicMeter10A22 Standard Liquid'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q15*0.45),'BasicMeter10A22 Standard Liquid'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X14,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,null,35,{"$f":"'10A22 Capacity Table'!C18","v":35},"2\"","1Q",2,{"$f":"IFERROR((F16/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"2\"-1Q","viscosity","2\"-1Q",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q16*0.45),'BasicMeter10A22 Standard Liquid'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q16*0.45),'BasicMeter10A22 Standard Liquid'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X15,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,null,50,{"$f":"'10A22 Capacity Table'!C19","v":50},"2\"","1R",2,{"$f":"IFERROR((F17/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"2\"-1R","viscosity","2\"-1R",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q17*0.45),'BasicMeter10A22 Standard Liquid'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q17*0.45),'BasicMeter10A22 Standard Liquid'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X16,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,null,0,{"$f":"'10A22 Capacity Table'!C20","v":0},null,null,0,{"$f":"IFERROR((F18/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"-","viscosity","-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q18*0.45),'BasicMeter10A22 Standard Liquid'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q18*0.45),'BasicMeter10A22 Standard Liquid'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X17,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q19*0.45),'BasicMeter10A22 Standard Liquid'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q19*0.45),'BasicMeter10A22 Standard Liquid'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X18,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q20*0.45),'BasicMeter10A22 Standard Liquid'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q20*0.45),'BasicMeter10A22 Standard Liquid'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X19,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q21*0.45),'BasicMeter10A22 Standard Liquid'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q21*0.45),'BasicMeter10A22 Standard Liquid'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X20,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q22*0.45),'BasicMeter10A22 Standard Liquid'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q22*0.45),'BasicMeter10A22 Standard Liquid'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X21,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q23*0.45),'BasicMeter10A22 Standard Liquid'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q23*0.45),'BasicMeter10A22 Standard Liquid'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X22,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q24*0.45),'BasicMeter10A22 Standard Liquid'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q24*0.45),'BasicMeter10A22 Standard Liquid'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X23,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q25*0.45),'BasicMeter10A22 Standard Liquid'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q25*0.45),'BasicMeter10A22 Standard Liquid'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X24,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q26*0.45),'BasicMeter10A22 Standard Liquid'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q26*0.45),'BasicMeter10A22 Standard Liquid'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X25,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q27*0.45),'BasicMeter10A22 Standard Liquid'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q27*0.45),'BasicMeter10A22 Standard Liquid'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X26,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q28*0.45),'BasicMeter10A22 Standard Liquid'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q28*0.45),'BasicMeter10A22 Standard Liquid'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X27,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q29*0.45),'BasicMeter10A22 Standard Liquid'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q29*0.45),'BasicMeter10A22 Standard Liquid'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X28,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q30*0.45),'BasicMeter10A22 Standard Liquid'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q30*0.45),'BasicMeter10A22 Standard Liquid'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X29,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q31*0.45),'BasicMeter10A22 Standard Liquid'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q31*0.45),'BasicMeter10A22 Standard Liquid'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X30,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q32*0.45),'BasicMeter10A22 Standard Liquid'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q32*0.45),'BasicMeter10A22 Standard Liquid'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X31,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q33*0.45),'BasicMeter10A22 Standard Liquid'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q33*0.45),'BasicMeter10A22 Standard Liquid'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X32,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q34*0.45),'BasicMeter10A22 Standard Liquid'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q34*0.45),'BasicMeter10A22 Standard Liquid'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X33,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q35*0.45),'BasicMeter10A22 Standard Liquid'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q35*0.45),'BasicMeter10A22 Standard Liquid'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X34,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q36*0.45),'BasicMeter10A22 Standard Liquid'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q36*0.45),'BasicMeter10A22 Standard Liquid'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X35,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q37*0.45),'BasicMeter10A22 Standard Liquid'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q37*0.45),'BasicMeter10A22 Standard Liquid'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X36,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q38*0.45),'BasicMeter10A22 Standard Liquid'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q38*0.45),'BasicMeter10A22 Standard Liquid'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X37,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q39*0.45),'BasicMeter10A22 Standard Liquid'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q39*0.45),'BasicMeter10A22 Standard Liquid'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X38,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q40*0.45),'BasicMeter10A22 Standard Liquid'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q40*0.45),'BasicMeter10A22 Standard Liquid'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X39,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q41*0.45),'BasicMeter10A22 Standard Liquid'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q41*0.45),'BasicMeter10A22 Standard Liquid'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X40,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q42*0.45),'BasicMeter10A22 Standard Liquid'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q42*0.45),'BasicMeter10A22 Standard Liquid'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X41,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q43*0.45),'BasicMeter10A22 Standard Liquid'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q43*0.45),'BasicMeter10A22 Standard Liquid'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X42,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q44*0.45),'BasicMeter10A22 Standard Liquid'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q44*0.45),'BasicMeter10A22 Standard Liquid'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X43,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q45*0.45),'BasicMeter10A22 Standard Liquid'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q45*0.45),'BasicMeter10A22 Standard Liquid'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X44,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q46*0.45),'BasicMeter10A22 Standard Liquid'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q46*0.45),'BasicMeter10A22 Standard Liquid'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X45,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q47*0.45),'BasicMeter10A22 Standard Liquid'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q47*0.45),'BasicMeter10A22 Standard Liquid'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X46,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q48*0.45),'BasicMeter10A22 Standard Liquid'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q48*0.45),'BasicMeter10A22 Standard Liquid'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X47,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q49*0.45),'BasicMeter10A22 Standard Liquid'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q49*0.45),'BasicMeter10A22 Standard Liquid'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X48,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q50*0.45),'BasicMeter10A22 Standard Liquid'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q50*0.45),'BasicMeter10A22 Standard Liquid'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X49,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q51*0.45),'BasicMeter10A22 Standard Liquid'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q51*0.45),'BasicMeter10A22 Standard Liquid'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X50,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q52*0.45),'BasicMeter10A22 Standard Liquid'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q52*0.45),'BasicMeter10A22 Standard Liquid'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X51,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q53*0.45),'BasicMeter10A22 Standard Liquid'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q53*0.45),'BasicMeter10A22 Standard Liquid'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X52,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q54*0.45),'BasicMeter10A22 Standard Liquid'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q54*0.45),'BasicMeter10A22 Standard Liquid'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X53,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q55*0.45),'BasicMeter10A22 Standard Liquid'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q55*0.45),'BasicMeter10A22 Standard Liquid'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X54,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q56*0.45),'BasicMeter10A22 Standard Liquid'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q56*0.45),'BasicMeter10A22 Standard Liquid'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X55,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q57*0.45),'BasicMeter10A22 Standard Liquid'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q57*0.45),'BasicMeter10A22 Standard Liquid'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X56,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q58*0.45),'BasicMeter10A22 Standard Liquid'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Liquid'!Q58*0.45),'BasicMeter10A22 Standard Liquid'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Liquid'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X57,$U$4:$U$17))","v":0}]

{"sheet":"BasicMeter Consolidation","index":67,"n_rows":120,"n_cols":22,"rows_kept":120,"cut":false,"hidden":true,"merged":[[14,3,14,4],[14,5,14,6]]}
[]
["Requested Flowrate too High/Low",null,null,"Tube/Float","Range","Sizing Error?","Hazardous Gas Check","Pressure/Temp Check","Available?",null,"Error Explanation 1","Error Explanation 2","Error Explanation 3"]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A61 3 inch'!$I$4:$I$33),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A61 3 inch'!$I$4:$I$33),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A61 3\" Standard",{"$f":"'BasicMeter10A61 3 inch'!U4","v":"none"},{"$f":"'BasicMeter10A61 3 inch'!V4","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A61 3 inch'!W4","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>264,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},{"$f":"IF(AND(F3=\"\",G3=\"\",H3=\"\"),\"yes\",\"no\")","v":"no"},null,{"$f":"IF(F3=\"sizing\",\"The requested flowrate is too \"&A3& \" to be measured accurately with this meter\",\nIF(F3=\"viscosity\",\"The liquid's viscosity is too large to provide an accurate sizing. Please contact ABB for more information\",\nIF(F3=\"pressure\",\"The operating pressure is too low to provide an accurate sizing. Please contact ABB for more information\",\"\")))","v":{"$error":"#VALUE!"}},{"$f":"IF(G3=\"stop\",\"For safety measures, ABB does not recommend glass meters to be used for hazardous gas applications\",\"\")","v":""},{"$f":"IF(H3=\"stop\",\"The operating pressure or temperature are beyond the maximum limitations of this meter\",\"\")","v":""}]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A61 3 inch'!$I$4:$I$33),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A61 3 inch'!$I$4:$I$33),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A61 3\" Alarm",{"$f":"'BasicMeter10A61 3 inch'!Y4","v":"none"},{"$f":"'BasicMeter10A61 3 inch'!Z4","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A61 3 inch'!AA4","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>264,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},{"$f":"IF(AND(F4=\"\",G4=\"\",H4=\"\"),\"yes\",\"no\")","v":"no"},null,{"$f":"IF(F4=\"sizing\",\"The requested flowrate is too \"&A4& \" to be measured accurately with this meter\",\nIF(F4=\"viscosity\",\"The liquid's viscosity is too large to provide an accurate sizing. Please contact ABB for more information\",\nIF(F4=\"pressure\",\"The operating pressure is too low to provide an accurate sizing. Please contact ABB for more information\",\"\")))","v":{"$error":"#VALUE!"}},{"$f":"IF(G4=\"stop\",\"For safety measures, ABB does not recommend glass meters to be used for hazardous gas applications\",\"\")","v":""},{"$f":"IF(H4=\"stop\",\"The operating pressure or temperature are beyond the maximum limitations of this meter\",\"\")","v":""}]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A61 5 inch'!$I$4:$I$72),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A61 5 inch'!I4:I72),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A61 5\" Standard",{"$f":"'BasicMeter10A61 5 inch'!V5","v":"none"},{"$f":"'BasicMeter10A61 5 inch'!W5","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A61 5 inch'!X5","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>264,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A61 5 inch'!$I$4:$I$72),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A61 5 inch'!I5:I73),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A61 5\" Alarm",{"$f":"'BasicMeter10A61 5 inch'!Z5","v":"none"},{"$f":"'BasicMeter10A61 5 inch'!AA5","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A61 5 inch'!AB5","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>264,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A4 Standard'!$Q$4:$Q$57),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A4 Standard'!$Q$4:$Q$57),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A4 Standard",{"$f":"'BasicMeter10A4 Standard'!AC5","v":"none"},{"$f":"'BasicMeter10A4 Standard'!AD5","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A4 Standard'!AF5","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>114,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A4 Low Pressure Dro'!$Q$4:$Q$20),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A4 Low Pressure Dro'!$Q$4:$Q$20),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A4 Low Pressure",{"$f":"'BasicMeter10A4 Low Pressure Dro'!AC5","v":"none"},{"$f":"'BasicMeter10A4 Low Pressure Dro'!AD5","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A4 Low Pressure Dro'!AF5","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>114,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF(BasicFluid!$F$12>MAX('BasicMeter10A4 Alarm'!$Q$4:$Q$52),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A4 Alarm'!$Q$4:$Q$52),\"low\",\"Good\"))","v":{"$error":"#VALUE!"}},null,"10A4 Alarm",{"$f":"'BasicMeter10A4 Alarm'!AC5","v":"none"},{"$f":"'BasicMeter10A4 Alarm'!AD5","v":{"$error":"#N/A"}},{"$f":"'BasicMeter10A4 Alarm'!AF5","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>114,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",\nIF(BasicFluid!$F$12>MAX('BasicMeter10A22 Standard Liquid'!$Q$4:$Q$17),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A22 Standard Liquid'!$Q$4:$Q$17),\"low\",\"Good\")),\n\nIF(BasicFluid!$F$12>MAX('BasicMeter10A22 Standard Gas'!$Q$4:$Q$17),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A22 Standard Gas'!$Q$4:$Q$17),\"low\",\"Good\")))","v":{"$error":"#VALUE!"}},null,"10A22 Standard",{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'BasicMeter10A22 Standard Liquid'!AA5,'BasicMeter10A22 Standard Gas'!AA4)","v":"none"},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'BasicMeter10A22 Standard Liquid'!AB5,'BasicMeter10A22 Standard Gas'!AB4)","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'BasicMeter10A22 Standard Liquid'!AD5,'BasicMeter10A22 Standard Gas'!AD4)","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>90,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",\nIF(BasicFluid!$F$12>MAX('BasicMeter10A22 Alarm Liquid'!$Q$4:$Q$14),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A22 Alarm Liquid'!$Q$4:$Q$14),\"low\",\"Good\")),\n\nIF(BasicFluid!$F$12>MAX('BasicMeter10A22 Alarm Gas'!$Q$4:$Q$14),\"high\",\nIF(BasicFluid!$F$12<MIN('BasicMeter10A22 Alarm Gas'!$Q$4:$Q$14),\"low\",\"Good\")))","v":{"$error":"#VALUE!"}},null,"10A22 Alarm",{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'BasicMeter10A22 Alarm Liquid'!AA4,'BasicMeter10A22 Alarm Gas'!AA4)","v":"none"},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'BasicMeter10A22 Alarm Liquid'!AB4,'BasicMeter10A22 Alarm Gas'!AB4)","v":{"$error":"#N/A"}},{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",'BasicMeter10A22 Alarm Liquid'!AD4,'BasicMeter10A22 Alarm Gas'!AD4)","v":"sizing"},{"$f":"IF(OR('VA Sizing'!C4=\"Butane (C4H10)\",'VA Sizing'!C4=\"Carbon Monoxide (CO)\",'VA Sizing'!C4=\"Chlorine (Cl)\",'VA Sizing'!C4=\"Ethane (C2H6)\",'VA Sizing'!C4=\"Ethylene (C2H4)\",'VA Sizing'!C4=\"Hydrochloric Acid (HCl)\",'VA Sizing'!C4=\"Acetylene (C2H2)\",'VA Sizing'!C4=\"Hydrogen (H2)\",'VA Sizing'!C4=\"Hydrogen Sulfide (H2S)\",'VA Sizing'!C4=\"Methane (CH4)\",'VA Sizing'!C4=\"Methyl Chloride (CH3Cl)\",'VA Sizing'!C4=\"Natural Gas\",'VA Sizing'!C4=\"Propane (C3H8)\",'VA Sizing'!C4=\"Propylene (C3H6)\",'VA Sizing'!C4=\"Sulfur Dioxide (SO2)\"),\"stop\",\"\")","v":""},{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>250,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>90,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,{"$error":"#VALUE!"},"",""]
[{"$f":"IF(BasicFluid!$F$12>MAX(Basic10A32!$BW$6:$BW$32),\"high\",\nIF(BasicFluid!$F$12<MIN(Basic10A32!$BW$6:$BW$32),\"low\",\"Good\"))","v":"Good"},null,"10A32",{"$f":"Basic10A32!CL7","v":"none"},{"$f":"Basic10A32!CM7","v":{"$error":"#N/A"}},{"$f":"Basic10A32!CO7","v":"sizing"},null,{"$f":"IFERROR(IF(OR(AND('Modified Inputs'!$K$2>248,NOT('Modified Inputs'!$K$2=\"Optional\")),AND('Modified Inputs'!$I$2>1450,NOT('Modified Inputs'!$I$2=\"Optional\"))),\"stop\",\"\"),\"\")","v":""},"no",null,"The requested flowrate is too Good to be measured accurately with this meter","",""]
[]
[]
[null,null,null,"Standard",null,"Alarm"]
[null,"Meter","Type","Tube/Float","Range","Tube/Float","Range"]
[null,"10A61",{"$f":"IF(I3=\"yes\",\"3 inch 10A61\",\nIF(I5=\"yes\",\"5 inch 10A61\",\"\"))","v":""},{"$f":"IF(I3=\"yes\",D3,\nIF(I5=\"yes\",D5,\"\"))","v":""},{"$f":"IF(I3=\"yes\",E3,\nIF(I5=\"yes\",E5,\"\"))","v":""},{"$f":"IF(I4=\"yes\",D4,\nIF(I6=\"yes\",D6,\"\"))","v":""},{"$f":"IF(I4=\"yes\",E4,\nIF(I6=\"yes\",E6,\"\"))","v":""}]
[null,"10A4",{"$f":"IF(I7=\"yes\",\"standard 10A4\",\nIF(I8=\"yes\",\"low pressure 10A4\",\"\"))","v":""},{"$f":"IF($I$7=\"yes\",D7,\nIF($I$8=\"yes\",D8,\"\"))","v":""},{"$f":"IF($I$7=\"yes\",E7,\nIF($I$8=\"yes\",E8,\"\"))","v":""},{"$f":"IF($I$9=\"yes\",D9,\"\")","v":""},{"$f":"IF($I$9=\"yes\",E9,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('BasicMeter Consolidation'!$D$56=\"standard 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Standard'!$D$4:$H$57,5,FALSE),'10A45 Naming Standard'!$M$4:$O$219,3,FALSE))","v":{"$error":"#N/A"}}]
[null,"10A22",{"$f":"IF(I10=\"yes\",\"standard 10A22\",\"\")","v":""},{"$f":"IF($I$10=\"yes\",D10,\"\")","v":""},{"$f":"IF($I$10=\"yes\",E10,\"\")","v":""},{"$f":"IF($I$11=\"yes\",D11,\"\")","v":""},{"$f":"IF($I$11=\"yes\",E11,\"\")","v":""}]
[null,"10A32",{"$f":"IF(I12=\"yes\",\"standard 10A32\",\"\")","v":""},{"$f":"IF($I$12=\"yes\",D12,\"\")","v":""},{"$f":"IF($I$12=\"yes\",E12,\"\")","v":""},"-","-"]
[]
[]
[]
[]
[null,"Meter","Type","Tube/Float","Range","Error Reason 1","Error Reason 2","Error Reason 3","Meter"]
[null,"10A61 Std",{"$f":"IF(I3=\"yes\",\"3 inch 10A61\",\nIF(I5=\"yes\",\"5 inch 10A61\",\"\"))","v":""},{"$f":"IF(I3=\"yes\",D3,\nIF(I5=\"yes\",D5,\"\"))","v":""},{"$f":"IF(I3=\"yes\",E3,\nIF(I5=\"yes\",E5,\"\"))","v":""},{"$f":"IF(C26=\"\",K5,\"\")","v":{"$error":"#VALUE!"}},"","","10A61"]
[null,"10A61 Alarm",{"$f":"IF(I4=\"yes\",\"3 inch 10A61 alarm\",\nIF(I6=\"yes\",\"5 inch 10A61 alarm\",\"\"))","v":""},{"$f":"F17","v":""},{"$f":"G17","v":""},{"$f":"IF(C27=\"\",K6,\"\")","v":{"$error":"#VALUE!"}},"","","10A61 Alarm"]
[null,"10A4 Std",{"$f":"IF(I7=\"yes\",\"standard 10A4\",\nIF(I8=\"yes\",\"low pressure 10A4\",\"\"))","v":""},{"$f":"IF($I$7=\"yes\",D7,\nIF($I$8=\"yes\",D8,\"\"))","v":""},{"$f":"IF($I$7=\"yes\",E7,\nIF($I$8=\"yes\",E8,\"\"))","v":""},{"$f":"IF(C28=\"\",K8,\"\")","v":{"$error":"#VALUE!"}},"","","10A4"]
[null,"10A4 Alarm",{"$f":"IF($I$9=\"yes\",\"standard 10A4 alarm\",\"\")","v":""},{"$f":"IF($I$9=\"yes\",D9,\"\")","v":""},{"$f":"IF($I$9=\"yes\",E9,\"\")","v":""},{"$error":"#VALUE!"},"","","10A4 Alarm"]
[null,"10A22 Std",{"$f":"IF(I10=\"yes\",\"standard 10A22\",\"\")","v":""},{"$f":"IF($I$10=\"yes\",D10,\"\")","v":""},{"$f":"IF($I$10=\"yes\",E10,\"\")","v":""},{"$error":"#VALUE!"},"","","10A22"]
[null,"10A22 Alarm",{"$f":"IF(I11=\"yes\",\"standard 10A22 alarm\",\"\")","v":""},{"$f":"IF($I$11=\"yes\",D11,\"\")","v":""},{"$f":"IF($I$11=\"yes\",E11,\"\")","v":""},{"$error":"#VALUE!"},"","","10A22 Alarm"]
[null,"10A32",{"$f":"IF(I12=\"yes\",\"standard 10A32\",\"\")","v":""},{"$f":"IF($I$12=\"yes\",D12,\"\")","v":""},{"$f":"IF($I$12=\"yes\",E12,\"\")","v":""},"The requested flowrate is too Good to be measured accurately with this meter","","","10A32"]
[null,null,null,null,null,null,"\""]
[]
[null,"Available Standard Meters","Type","Tube/Float","Range","Tube Size","Connection Size"]
[null,{"$f":"IF(C36=\"\",\"\",VLOOKUP(C36,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(NOT(C26=\"\"),C26,\nIF(NOT(C28=\"\"),C28,\nIF(NOT(C30=\"\"),C30,\nIF(NOT(C32=\"\"),C32,\"\"))))","v":""},{"$f":"VLOOKUP(C36,$C$26:$E$32,2,FALSE)","v":""},{"$f":"VLOOKUP(C36,$C$26:$E$32,3,FALSE)","v":""},{"$f":"IF(C36=\"standard 10A4\",VLOOKUP(D36,'BasicMeter10A4 Standard'!$P$4:$T$57,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C36=\"low pressure 10A4\",VLOOKUP('BasicMeter Consolidation'!D36,'BasicMeter10A4 Low Pressure Dro'!$P$4:$T$20,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C36=\"standard 10A4 alarm\",VLOOKUP('BasicMeter Consolidation'!D36,'BasicMeter10A4 Alarm'!$P$4:$T$52,5,FALSE)&$G$33,\nIF(C36=\"standard 10A32\",VLOOKUP(D36,Basic10A32!$AO$6:$AX$32,10,FALSE),\nIF(B36=\"10A22\",VLOOKUP(RIGHT(D36,2),$J$37:$K$69,2,FALSE),\nIF(B36=\"10A61\",\"1/4\"&$G$33,\n\"\"))))))","v":""},{"$f":"IF(B36=\"10A61\",F36,\nIF(B36=\"10A4\",VLOOKUP(F36,$N$37:$O$41,2,FALSE),\nIF(B36=\"10A22\",F36,\nIF(B36=\"10A32\",VLOOKUP(F36,$N$44:$O$47,2,FALSE),\"\"))))","v":""},null,null,"Code","Meter Size","Code",null,"10A4 Tube Size","10A4 Connection Size",null,null,"10A61 Tube Size","IX Digit"]
[null,{"$f":"IF(C37=\"\",\"\",VLOOKUP(C37,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(AND(NOT(C26=\"\"),NOT(C36=C26)),C26,\nIF(AND(NOT(C28=\"\"),NOT(C36=C28)),C28,\nIF(AND(NOT(C30=\"\"),NOT(C36=C30)),C30,\nIF(AND(NOT(C32=\"\"),NOT(C36=C32)),C32,\"\"))))","v":""},{"$f":"VLOOKUP(C37,$C$26:$E$32,2,FALSE)","v":""},{"$f":"VLOOKUP(C37,$C$26:$E$32,3,FALSE)","v":""},{"$f":"IF(C37=\"standard 10A4\",VLOOKUP(D37,'BasicMeter10A4 Standard'!$P$4:$T$57,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C37=\"low pressure 10A4\",VLOOKUP('BasicMeter Consolidation'!D37,'BasicMeter10A4 Low Pressure Dro'!$P$4:$T$20,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C37=\"standard 10A4 alarm\",VLOOKUP('BasicMeter Consolidation'!D37,'BasicMeter10A4 Alarm'!$P$4:$T$52,5,FALSE)&$G$33,\nIF(C37=\"standard 10A32\",VLOOKUP(D37,Basic10A32!$AO$6:$AX$32,10,FALSE),\nIF(B37=\"10A22\",VLOOKUP(RIGHT(D37,2),$J$37:$K$69,2,FALSE),\nIF(B37=\"10A61\",\"1/4\"&$G$33,\n\"\"))))))","v":""},{"$f":"IF(B37=\"10A61\",F37,\nIF(B37=\"10A4\",VLOOKUP(F37,$N$37:$O$41,2,FALSE),\nIF(B37=\"10A22\",F37,\nIF(B37=\"10A32\",VLOOKUP(F37,$N$44:$O$47,2,FALSE),\"\"))))","v":""},null,null,"2F","1/2\"","2F",null,"1/2\"","1/2\"",null,null,"1/8",1]
[null,{"$f":"IF(C38=\"\",\"\",VLOOKUP(C38,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(AND(NOT(C26=\"\"),NOT(C36=C26),NOT(C37=C26)),C26,\nIF(AND(NOT(C28=\"\"),NOT(C36=C28),NOT(C37=C28)),C28,\nIF(AND(NOT(C30=\"\"),NOT(C36=C30),NOT(C37=C30)),C30,\nIF(AND(NOT(C32=\"\"),NOT(C36=C32),NOT(C37=C32)),C32,\"\"))))","v":""},{"$f":"VLOOKUP(C38,$C$26:$E$32,2,FALSE)","v":""},{"$f":"VLOOKUP(C38,$C$26:$E$32,3,FALSE)","v":""},{"$f":"IF(C38=\"standard 10A4\",VLOOKUP(D38,'BasicMeter10A4 Standard'!$P$4:$T$57,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C38=\"low pressure 10A4\",VLOOKUP('BasicMeter Consolidation'!D38,'BasicMeter10A4 Low Pressure Dro'!$P$4:$T$20,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C38=\"standard 10A4 alarm\",VLOOKUP('BasicMeter Consolidation'!D38,'BasicMeter10A4 Alarm'!$P$4:$T$52,5,FALSE)&$G$33,\nIF(C38=\"standard 10A32\",VLOOKUP(D38,Basic10A32!$AO$6:$AX$32,10,FALSE),\nIF(B38=\"10A22\",VLOOKUP(RIGHT(D38,2),$J$37:$K$69,2,FALSE),\nIF(B38=\"10A61\",\"1/4\"&$G$33,\n\"\"))))))","v":""},"",null,null,"2H","1/2\"","2H",null,"3/4\"","3/4\", 1\"",null,null,"1/4",2]
[null,{"$f":"IF(C39=\"\",\"\",VLOOKUP(C39,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(AND(NOT(C26=\"\"),NOT(C36=C26),NOT(C37=C26),NOT(C38=C26)),C26,\nIF(AND(NOT(C28=\"\"),NOT(C36=C28),NOT(C37=C28),NOT(C38=C28)),C28,\nIF(AND(NOT(C30=\"\"),NOT(C36=C30),NOT(C37=C30),NOT(C38=C30)),C30,\nIF(AND(NOT(C32=\"\"),NOT(C36=C32),NOT(C37=C32),NOT(C38=C32)),C32,\"\"))))","v":""},{"$f":"VLOOKUP(C39,$C$26:$E$32,2,FALSE)","v":""},{"$f":"VLOOKUP(C39,$C$26:$E$32,3,FALSE)","v":""},{"$f":"IF(C39=\"standard 10A4\",VLOOKUP(D39,'BasicMeter10A4 Standard'!$P$4:$T$57,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C39=\"low pressure 10A4\",VLOOKUP('BasicMeter Consolidation'!D39,'BasicMeter10A4 Low Pressure Dro'!$P$4:$T$20,5,FALSE)&$G$33,\nIF('BasicMeter Consolidation'!C39=\"standard 10A4 alarm\",VLOOKUP('BasicMeter Consolidation'!D39,'BasicMeter10A4 Alarm'!$P$4:$T$52,5,FALSE)&$G$33,\nIF(C39=\"standard 10A32\",VLOOKUP(D39,Basic10A32!$AO$6:$AX$32,10,FALSE),\nIF(B39=\"10A22\",VLOOKUP(RIGHT(D39,2),$J$37:$K$69,2,FALSE),\nIF(B39=\"10A61\",\"1/4\"&$G$33,\n\"\"))))))","v":""},"",null,null,"2J","1/2\"","2J",null,"1\"","3/4\", 1\"",null,null,"1/16",3]
[null,null,null,null,null,null,null,null,null,"2M","1\"","2M",null,"1-1/2\"","1-1/2\""]
[null,null,null,null,null,null,null,null,null,"2B","1/4\"","2B",null,"2\"","1-1/2\""]
[null,"Available Alarm Meters","Type","Tube/Float","Range",null,null,null,null,"2C","1/4\"","2C",null,null,null,null,null,"10A61 Float","IX Digit"]
[{"$f":"VLOOKUP(B43,$N$58:$O$62,2,FALSE)","v":""},{"$f":"IF(C43=\"\",\"\",VLOOKUP(C43,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(NOT(C27=\"\"),C27,\nIF(NOT(C29=\"\"),C29,\nIF(NOT(C31=\"\"),C31,\"\")))","v":""},{"$f":"VLOOKUP(C43,$C$26:$E$32,2,FALSE)","v":""},{"$f":"VLOOKUP(C43,$C$26:$E$32,3,FALSE)","v":""},null,null,null,null,"2D","1/2\"","2D",null,"10A32 Tube Size","10A32 Connection Size",null,null,"BG","A"]
[{"$f":"VLOOKUP(B44,$N$58:$O$62,2,FALSE)","v":""},{"$f":"IF(C44=\"\",\"\",VLOOKUP(C44,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(AND(NOT(C27=\"\"),NOT(C43=C27)),C27,\nIF(AND(NOT(C29=\"\"),NOT(C43=C29)),C29,\nIF(AND(NOT(C31=\"\"),NOT(C43=C31)),C31,\"\")))","v":""},{"$f":"VLOOKUP(C44,$C$26:$E$32,2,FALSE)","v":""},{"$f":"VLOOKUP(C44,$C$26:$E$32,3,FALSE)","v":""},null,null,null,null,"2E","1/2\"","2E",null,"1/4\"","1/4\"",null,null,"CD","B"]
["",{"$f":"IF(C45=\"\",\"\",VLOOKUP(C45,$C$26:$I$32,7,FALSE))","v":""},{"$f":"IF(AND(NOT(C27=\"\"),NOT(C43=C27),NOT(C44=C27)),C27,\nIF(AND(NOT(C29=\"\"),NOT(C43=C29),NOT(C44=C29)),C29,\nIF(AND(NOT(C31=\"\"),NOT(C43=C31),NOT(C44=C31)),C31,\"\")))","v":""},{"$f":"VLOOKUP(C45,$C$26:$E$32,2,FALSE)","v":""},"",null,null,null,null,"2G","1/2\"","2G",null,"3/8\"","3/8\", 1/2\"",null,null,"SA","C"]
[null,null,null,null,null,null,null,null,null,"2K","1/2\"","2K",null,"1/2\"","1/2\"",null,null,"SS","D"]
[null,null,null,null,null,null,null,null,null,"2L","1\"","2L",null,"1\"","1\"",null,null,"CA","E"]
[null,"Unavailable Meters","Error Reason 1","Error Reason 2","Error Reason 3","Error Label 1","Error Label 2","Error Label 3",null,"2N","1\"","2N",null,null,null,null,null,"TA","F"]
[{"$f":"VLOOKUP(B49,$N$50:$O$54,2,FALSE)","v":"10A61"},{"$f":"IF((C26=\"\"),\"10A61 Std\",\nIF((C28=\"\"),\"10A4 Std\",\nIF((C30=\"\"),\"10A22 Std\",\nIF((C32=\"\"),\"10A32\",\"\"))))","v":"10A61 Std"},{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,$B$26:$H$32,5,FALSE))","v":{"$error":"#VALUE!"}},{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,$B$26:$H$32,6,FALSE))","v":""},{"$f":"IF(B49=\"\",\"\",VLOOKUP(B49,$B$26:$H$32,7,FALSE))","v":""},{"$f":"IF(LEFT(C49,5)=\"The r\",\"Flowrate\",\nIF(C49=\"The liquid's viscosity is too large to provide an accurate sizing. Please contact ABB for more information\",\"Viscosity\",\nIF(C49=\"The operating pressure is too low to provide an accurate sizing. Please contact ABB for more information\",\"Pressure\",\"\")))","v":{"$error":"#VALUE!"}},{"$f":"IF(D49=\"\",\"\",\"Haz. Gas\")","v":""},{"$f":"IF(E49=\"\",\"\",\"Temp/Pressure\")","v":""},null,"2P","1\"","2P"]
[{"$f":"VLOOKUP(B50,$N$50:$O$54,2,FALSE)","v":"10A4"},{"$f":"IF(AND((C26=\"\"),NOT(B49=B26)),\"10A61 Std\",\nIF(AND((C28=\"\"),NOT(B49=B28)),\"10A4 Std\",\nIF(AND((C30=\"\"),NOT(B49=B30)),\"10A22 Std\",\nIF(AND((C32=\"\"),NOT(B49=B32)),\"10A32\",\"\"))))","v":"10A4 Std"},{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,$B$26:$H$32,5,FALSE))","v":{"$error":"#VALUE!"}},{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,$B$26:$H$32,6,FALSE))","v":""},{"$f":"IF(B50=\"\",\"\",VLOOKUP(B50,$B$26:$H$32,7,FALSE))","v":""},{"$f":"IF(LEFT(C50,5)=\"The r\",\"Flowrate\",\nIF(C50=\"The liquid's viscosity is too large to provide an accurate sizing. Please contact ABB for more information\",\"Viscosity\",\nIF(C50=\"The operating pressure is too low to provide an accurate sizing. Please contact ABB for more information\",\"Pressure\",\"\")))","v":{"$error":"#VALUE!"}},{"$f":"IF(D50=\"\",\"\",\"Haz. Gas\")","v":""},{"$f":"IF(E50=\"\",\"\",\"Temp/Pressure\")","v":""},null,"2Q","1-1/2\"","2Q",null,"10A61 Std","10A61"]
["10A22",{"$f":"IF(AND((C26=\"\"),NOT(B49=B26),NOT(B50=B26)),\"10A61 Std\",\nIF(AND((C28=\"\"),NOT(B49=B28),NOT(B50=B28)),\"10A4 Std\",\nIF(AND((C30=\"\"),NOT(B49=B30),NOT(B50=B30)),\"10A22 Std\",\nIF(AND((C32=\"\"),NOT(B49=B32),NOT(B50=B32)),\"10A32\",\"\"))))","v":"10A22 Std"},{"$error":"#VALUE!"},"","",{"$error":"#VALUE!"},"","",null,"2R","1-1/2\"","2R",null,"10A4 Std","10A4",null,null,"10A61 3\" Tube","IX Digit",null,"10A61 5\" Tube","IX Digit"]
["10A32",{"$f":"IF(AND((C26=\"\"),NOT(B49=B26),NOT(B50=B26),NOT(B51=B26)),\"10A61 Std\",\nIF(AND((C28=\"\"),NOT(B49=B28),NOT(B50=B28),NOT(B51=B28)),\"10A4 Std\",\nIF(AND((C30=\"\"),NOT(B49=B30),NOT(B50=B30),NOT(B51=B30)),\"10A22 Std\",\nIF(AND((C32=\"\"),NOT(B49=B32),NOT(B50=B32),NOT(B51=B32)),\"10A32\",\"\"))))","v":"10A32"},"The requested flowrate is too Good to be measured accurately with this meter","","","Flowrate","","",null,"2S","1-1/2\"","2S",null,"10A22 Std","10A22",null,null,"1/8-08-BG","07",null,"1/4-25-CD","25"]
[null,null,null,null,null,null,null,null,null,"2T","2\"","2T",null,"10A32","10A32",null,null,"1/8-08-SA","07",null,"1/4-25-SA","25"]
[null,null,null,null,null,null,null,null,null,"2U","2\"","2U",null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"1/8-08-SS","07",null,"1/4-25-SS","25"]
[null,"Selected Meter (auto)","Alarm (auto)","Type","Tube/Float","Range","VA Sizing Column","10A32 Scale",null,"1E","1/2\"","1E",null,null,null,null,null,"1/8-08-CA","07",null,"1/4-25-CA","25"]
[null,"10A61","no",{"$f":"IF($B$56=\"\",\"\",\nIF($B$56=\"10A32\",VLOOKUP($B$56,$B$36:$E$39,2,FALSE),\nIF($C$56=\"no\",VLOOKUP($B$56,$B$36:$E$39,2,FALSE),\nIF($C$56=\"yes\",VLOOKUP($B$56,$A$43:$E$45,3,FALSE),\n\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF($B$56=\"\",\"\",\nIF($B$56=\"10A32\",VLOOKUP($B$56,$B$36:$E$39,3,FALSE),\nIF($C$56=\"no\",VLOOKUP($B$56,$B$36:$E$39,3,FALSE),\nIF($C$56=\"yes\",VLOOKUP($B$56,$A$43:$E$45,4,FALSE),\n\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF($B$56=\"\",\"\",\nIF($B$56=\"10A32\",VLOOKUP($B$56,$B$36:$E$39,4,FALSE),\nIF($C$56=\"no\",VLOOKUP($B$56,$B$36:$E$39,4,FALSE),\nIF($C$56=\"yes\",VLOOKUP($B$56,$A$43:$E$45,5,FALSE),\n\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF(B56=\"\",\"\",VLOOKUP(D56,N65:O74,2,FALSE))","v":{"$error":"#N/A"}},{"$f":"VLOOKUP(E56,Basic10A32!$AO$6:$AW$32,9,FALSE)","v":{"$error":"#N/A"}},null,"1B","1/4\"","1B",null,null,null,null,null,"1/8-08-TA","07",null,"1/4-25-TA","25"]
[null,null,null,null,null,null,null,null,null,"1C","1/4\"","1C",null,null,null,null,null,"1/8-20-BG","08",null,"1/4-25-BG","25"]
[null,null,null,null,null,null,null,null,null,"1D","1/2\"","1D",null,"10A61 Alarm","10A61",null,null,"1/8-20-SA","08",null,"1/4-20-CD","24"]
[null,null,null,null,null,null,null,null,null,"1F","1/2\"","1F",null,"10A4 Alarm","10A4",null,null,"1/8-20-SS","08",null,"1/4-20-SA","24"]
[null,null,null,null,null,null,null,null,null,"1G","1/2\"","1G",null,"10A22 Alarm","10A22",null,null,"1/8-20-CA","08",null,"1/4-20-SS","24"]
[null,null,null,null,null,null,null,null,null,"1H","1/2\"","1H",null,"10A32","10A32",null,null,"1/8-20-TA","08",null,"1/4-20-CA","24"]
[null,null,null,null,null,null,null,null,null,"1J","1\"","1J",null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"1/4-15-BG","09",null,"1/4-20-TA","24"]
[null,null,null,null,null,null,null,null,null,"1K","1\"","1K",null,null,null,null,null,"1/4-15-SA","09",null,"1/4-20-BG","24"]
[null,null,null,null,null,null,null,null,null,"1L","1\"","1L",null,"Type","Column",null,null,"1/4-15-SS","09",null,"1/4-16-CD","23"]
[null,null,null,null,null,null,null,null,null,"1M","1-1/2\"","1M",null,"3 inch 10A61",1,null,null,"1/4-15-CA","09",null,"1/4-16-SA","23"]
[null,null,null,null,null,null,null,null,null,"1N","1-1/2\"","1N",null,"3 inch 10A61 alarm",1,null,null,"1/4-15-TA","09",null,"1/4-16-SS","23"]
[null,null,null,null,null,null,null,null,null,"1P","1-1/2\"","1P",null,"5 inch 10A61",2,null,null,"1/4-20-BG","10",null,"1/4-16-CA","23"]
[null,null,null,null,null,null,null,null,null,"1Q","2\"","1Q",null,"5 inch 10A61 alarm",2,null,null,"1/4-20-SA","10",null,"1/4-16-TA","23"]
[null,null,null,null,null,null,null,null,null,"1R","2\"","1R",null,"standard 10A4",1,null,null,"1/4-20-SS","10",null,"1/4-16-BG","23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"standard 10A4 Alarm",3,null,null,"1/4-20-CA","10",null,"1/4-10-CD","22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"low pressure 10A4",2,null,null,"1/4-20-TA","10",null,"1/4-10-SA","22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"standard 10A22",1,null,null,"1/4-41-G-BG","11",null,"1/4-10-SS","22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"standard 10A22 Alarm",2,null,null,"1/4-41-G-SA","11",null,"1/4-10-CA","22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"standard 10A32",1,null,null,"1/4-41-G-SS","11",null,"1/4-10-TA","22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-G-CA","11",null,"1/4-10-BG","22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-G-TA","11",null,"1/8-12-SA","18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-P-BG","12",null,"1/8-12-SS","18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-P-SA","12",null,"1/8-12-CA","18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-P-SS","12",null,"1/8-12-TA","18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-P-CA","12",null,"1/8-12-BG","18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-41-P-TA","12",null,"1/8-08-SA","17"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-08-SS","17"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-08-CA","17"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-08-TA","17"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-08-BG","17"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-12-SA","14"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-12-SS","14"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-12-CA","14"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-12-TA","14"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-12-BG","14"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-16-SA","15"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-16-SS","15"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-16-CA","15"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-16-TA","15"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-16-BG","15"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-20-SA","16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-20-SS","16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-20-CA","16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-20-TA","16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/16-20-BG","16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-25-SA","21"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-25-SS","21"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-25-CA","21"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-25-TA","21"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-25-BG","21"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-20-SA","20"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-20-SS","20"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-20-CA","20"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-20-TA","20"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-20-BG","20"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-16-SA","19"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-16-SS","19"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-16-CA","19"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-16-TA","19"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/8-16-BG","19"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-40-G-6-BG","26"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-40-G-6-SA","26"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-40-G-6-SS","26"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-40-G-6-CA","26"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1/4-40-G-6-TA","26"]

{"sheet":"BasicPartNumber","index":68,"n_rows":54,"n_cols":20,"rows_kept":54,"cut":false,"hidden":true,"merged":[]}
["."]
[null,"10A61"]
[]
[null,"Static","Static","Variable","Static","Static","Variable","Static","Static","static","static","static","static","static","static","static","variable","variable","variable"]
[null,"Base","Connection","Scale","Valve","Design","Tube Size","Material","Mounting","Regulator","Alarm","Connection","Tag","Language","Alarm","External Scale","Scale","Float","Tube"]
[null,"10A61",3,{"$f":"IF(LEFT('BasicMeter Consolidation'!D56,1)=\"3\",1,\nIF(LEFT('BasicMeter Consolidation'!D56,1)=\"5\",2,\"\"))","v":{"$error":"#N/A"}},"__","B",{"$f":"IF(LEFT('BasicMeter Consolidation'!$E$56,3)=\"1/8\",1,\nIF(LEFT('BasicMeter Consolidation'!$E$56,3)=\"1/4\",2,\nIF(LEFT('BasicMeter Consolidation'!$E$56,4)=\"1/16\",3,\"\")))","v":{"$error":"#N/A"}},"__","__","__","__","A","A","E","__","__","E",{"$f":"VLOOKUP(RIGHT('BasicMeter Consolidation'!$E$56,2),'BasicMeter Consolidation'!$R$43:$S$48,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF($D$6=1,VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter Consolidation'!$R$52:$S$81,2,FALSE),\nIF($D$6=2,VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter Consolidation'!$U$52:$V$120,2,FALSE),\"\"))","v":{"$error":"#N/A"}}]
[]
[]
[null,"10A61 Part Number"]
[null,{"$f":"B6&$A$1&C6&$A$1&D6&$A$1&E6&$A$1&F6&$A$1&G6&$A$1&H6&$A$1&I6&$A$1&J6&$A$1&K6&$A$1&L6&$A$1&M6&$A$1&N6&$A$1&O6&$A$1&P6&$A$1&Q6&$A$1&R6&$A$1&S6","v":{"$error":"#N/A"}}]
[]
[]
[]
[null,"10A4"]
[]
[null,"Static","Static","Static","Static","Static","Static","Static","Static","Static","Static","Static","Static","Static","Static","Variable","Variable","Static"]
[null,"Base","Seals","Connection Type","Scale Type","Mounting","Design","Size","Fitting Mat.","Seal Mat.","Connection Type","Alarm","Reserved","Orientation 1","Orientation 2","Float","Tube","Float Material"]
[null,"10A4","__","__","__","__","B","__","C","__","__","__","__","__","__",{"$f":"IF('BasicMeter Consolidation'!$D$56=\"standard 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Standard'!$D$4:$H$57,5,FALSE),'10A45 Naming Standard'!$M$4:$O$219,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"low pressure 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Low Pressure Dro'!$D$4:$H$20,5,FALSE),'10A45 Naming Low PSI'!$M$4:$O$71,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"standard 10A4 Alarm\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Alarm'!$D$4:$H$52,5,FALSE),'10A45 Naming Alarm'!$M$4:$O$203,3,FALSE),\"\")))","v":{"$error":"#N/A"}},{"$f":"IF('BasicMeter Consolidation'!$D$56=\"standard 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Standard'!$D$4:$G$57,4,FALSE),'10A45 Naming Standard'!$L$4:$N$219,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"low pressure 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Low Pressure Dro'!$D$4:$H$20,4,FALSE),'10A45 Naming Low PSI'!$L$4:$N$71,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"standard 10A4 Alarm\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Alarm'!$D$4:$G$52,4,FALSE),'10A45 Naming Alarm'!$L$4:$N$203,3,FALSE),\"\")))","v":{"$error":"#N/A"}},1]
[]
[]
[null,"10A4 Part Number"]
[null,{"$f":"B18&$A$1&C18&$A$1&D18&$A$1&E18&$A$1&F18&$A$1&G18&$A$1&H18&$A$1&I18&$A$1&J18&$A$1&K18&$A$1&L18&$A$1&M18&$A$1&N18&$A$1&O18&$A$1&P18&$A$1&Q18&$A$1&R18","v":{"$error":"#N/A"}}]
[]
[]
[]
[null,"10A22"]
[]
[null,"Static","variable","variable","variable","variable","variable","variable","variable","variable","variable","static","variable"]
[null,"Base","alarm?","size","tube/float","alarm type","relay","type relay","relay voltage","inlet orientation","outlet orientation","scale","float material"]
[null,"10A22",{"$f":"IF('BasicMeter Consolidation'!$C$56=\"yes\",\"XXA\",\"XXX\")","v":"XXX"},{"$f":"VLOOKUP('BasicMeter Consolidation'!$E$56,'10A22 Naming'!$F$3:$I$52,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('BasicMeter Consolidation'!$E$56,'10A22 Naming'!$F$3:$I$52,2,FALSE)","v":{"$error":"#N/A"}},"__","__","__","__","__","__","E",{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",1,2)","v":2}]
[]
[]
[null,"10A22 Part Number"]
[null,{"$f":"B30&$A$1&C30&$A$1&D30&$A$1&E30&$A$1&F30&$A$1&G30&$A$1&H30&$A$1&I30&$A$1&J30&$A$1&K30&$A$1&L30&$A$1&M30","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[null,"10A32"]
[]
[null,"Static","Variable","Variable","Static","Variable","Variable","Variable","Variable","Variable","Variable","Variable","Variable","Static","Static","Variable","Variable","Variable","Variable","Variable"]
[null,"Base","Secondary","Construction","Design","Valve","Material","Cert","Float Design","Housing","Output","Regulator","Regulator Mounting","Size","Tag","Relay","Tube/Float","Scale Type","Scale Design","Accuracy"]
[null,"10A32","__","__","D","__","__","__",{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<VLOOKUP('BasicMeter Consolidation'!$E$56,'10A32 Capacity'!$AY$6:$BB$32,4,FALSE)),1,0)","v":{"$error":"#N/A"}},"__","__","__","__","__",1,"__",{"$f":"LEFT('BasicMeter Consolidation'!$E$56,2)","v":{"$error":"#N/A"}},{"$f":"'BasicMeter Consolidation'!H56","v":{"$error":"#N/A"}},"__","__"]
[]
[]
[null,"10A32 Part Number"]
[null,{"$f":"B43&$A$1&C43&$A$1&D43&$A$1&E43&$A$1&F43&$A$1&G43&$A$1&H43&$A$1&I43&$A$1&J43&$A$1&K43&$A$1&L43&$A$1&M43&$A$1&N43&$A$1&O43&$A$1&P43&$A$1&Q43&$A$1&R43&$A$1&S43&$A$1&T43","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[]
[null,"FINAL PART NUMBER"]
[null,{"$f":"IF('BasicMeter Consolidation'!$B$56=\"10A61\",BasicPartNumber!$B$10,\nIF('BasicMeter Consolidation'!$B$56=\"10A4\",BasicPartNumber!$B$22,\nIF('BasicMeter Consolidation'!$B$56=\"10A22\",BasicPartNumber!$B$34,\nIF('BasicMeter Consolidation'!$B$56=\"10A32\",BasicPartNumber!$B$47,\"\"))))","v":{"$error":"#N/A"}}]

{"sheet":"BulkPartNumber","index":69,"n_rows":54,"n_cols":20,"rows_kept":54,"cut":false,"hidden":true,"merged":[]}
["."]
[null,"10A61"]
[]
[null,"Static","Static","Variable","Variable","Static","Variable","Static","Static","static","static","static","static","static","static","static","variable","variable","variable"]
[null,"Base","Connection","Scale","Valve","Design","Tube Size","Material","Mounting","Regulator","Alarm","Connection","Tag","Language","Alarm","External Scale","Scale","Float","Tube"]
[null,"10A61",3,{"$f":"IF(LEFT('BasicMeter Consolidation'!D56,1)=\"3\",1,\nIF(LEFT('BasicMeter Consolidation'!D56,1)=\"5\",2,\"\"))","v":{"$error":"#N/A"}},{"$f":"IF(D6=1,\"N\",\nIF(AND(D6=2,G6=3),\"D\",\"N\"))","v":{"$error":"#N/A"}},"B",{"$f":"IF(LEFT('BasicMeter Consolidation'!$E$56,3)=\"1/8\",1,\nIF(LEFT('BasicMeter Consolidation'!$E$56,3)=\"1/4\",2,\nIF(LEFT('BasicMeter Consolidation'!$E$56,4)=\"1/16\",3,\"\")))","v":{"$error":"#N/A"}},"B",1,"X",{"$f":"\"00\"","v":"00"},"A","A","E","X","B","E",{"$f":"VLOOKUP(RIGHT('BasicMeter Consolidation'!$E$56,2),'BasicMeter Consolidation'!$R$43:$S$48,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF($D$6=1,VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter Consolidation'!$R$52:$S$81,2,FALSE),\nIF($D$6=2,VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter Consolidation'!$U$52:$V$120,2,FALSE),\"\"))","v":{"$error":"#N/A"}}]
["List Adder",null,198,{"$f":"IF(D6=1,0,\nIF(D6=2,88,\"\"))","v":{"$error":"#N/A"}},{"$f":"IF(E6=\"D\",70,\nIF(E6=\"N\",29,\"\"))","v":{"$error":"#N/A"}},0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"10A61 Part Number","List Price"]
[null,{"$f":"B6&$A$1&C6&$A$1&D6&$A$1&E6&$A$1&F6&$A$1&G6&$A$1&H6&$A$1&I6&$A$1&J6&$A$1&K6&$A$1&L6&$A$1&M6&$A$1&N6&$A$1&O6&$A$1&P6&$A$1&Q6&$A$1&R6&$A$1&S6","v":{"$error":"#N/A"}},{"$f":"SUM(C7:S7)","v":{"$error":"#N/A"}}]
[]
[]
[]
[null,"10A4"]
[]
[null,"Static","Static","Static","Static","Static","Static","Variable","Static","Static","Static","Static","Static","Static","Static","Variable","Variable","Static"]
[null,"Base","Seals","Connection Type","Scale Type","Mounting","Design","Size","Fitting Mat.","Seal Mat.","Connection Type","Alarm","Reserved","Orientation 1","Orientation 2","Float","Tube","Float Material"]
[null,"10A4",55,5,"S","X","B",{"$f":"IF(RIGHT(LEFT('BasicMeter Consolidation'!E56,6),3)=\"1/2\",\"H\",\nIF(RIGHT(LEFT('BasicMeter Consolidation'!E56,6),3)=\"3/4\",\"J\",\nIF(RIGHT(LEFT('BasicMeter Consolidation'!E56,8),5)=\"1-1/2\",\"N\",\nIF(RIGHT(LEFT('BasicMeter Consolidation'!E56,4),1)=\"1\",\"K\",\nIF(RIGHT(LEFT('BasicMeter Consolidation'!E56,4),1)=\"2\",\"P\",\"\")))))","v":{"$error":"#N/A"}},"C","F","B","X","X",2,2,{"$f":"IF('BasicMeter Consolidation'!$D$56=\"standard 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Standard'!$D$4:$H$57,5,FALSE),'10A45 Naming Standard'!$M$4:$O$219,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"low pressure 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Low Pressure Dro'!$D$4:$H$20,5,FALSE),'10A45 Naming Low PSI'!$M$4:$O$71,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"standard 10A4 Alarm\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Alarm'!$D$4:$H$52,5,FALSE),'10A45 Naming Alarm'!$M$4:$O$203,3,FALSE),\"\")))","v":{"$error":"#N/A"}},{"$f":"IF('BasicMeter Consolidation'!$D$56=\"standard 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Standard'!$D$4:$G$57,4,FALSE),'10A45 Naming Standard'!$L$4:$N$219,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"low pressure 10A4\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Low Pressure Dro'!$D$4:$H$20,4,FALSE),'10A45 Naming Low PSI'!$L$4:$N$71,3,FALSE),\nIF('BasicMeter Consolidation'!$D$56=\"standard 10A4 Alarm\",VLOOKUP(VLOOKUP('BasicMeter Consolidation'!$E$56,'BasicMeter10A4 Alarm'!$D$4:$G$52,4,FALSE),'10A45 Naming Alarm'!$L$4:$N$203,3,FALSE),\"\")))","v":{"$error":"#N/A"}},1]
["List Adder",null,0,0,73,0,0,{"$f":"IF(H18=\"H\",888,\nIF(H18=\"J\",1267,\nIF(H18=\"K\",1267,\nIF(H18=\"N\",2273,\nIF(H18=\"P\",2273,\"\")))))","v":{"$error":"#N/A"}},0,0,0,0,0,0,0,0,0,0]
[]
[null,"10A4 Part Number","List Price"]
[null,{"$f":"B18&$A$1&C18&$A$1&D18&$A$1&E18&$A$1&F18&$A$1&G18&$A$1&H18&$A$1&I18&$A$1&J18&$A$1&K18&$A$1&L18&$A$1&M18&$A$1&N18&$A$1&O18&$A$1&P18&$A$1&Q18&$A$1&R18","v":{"$error":"#N/A"}},{"$f":"SUM(C19:R19)","v":{"$error":"#N/A"}}]
[]
[]
[]
[null,"10A22"]
[]
[null,"Static","variable","variable","variable","variable","variable","variable","variable","variable","variable","static","variable"]
[null,"Base","alarm?","size","tube/float","alarm type","relay","type relay","relay voltage","inlet orientation","outlet orientation","scale","float material"]
[null,"10A22",{"$f":"IF('BasicMeter Consolidation'!$C$56=\"yes\",\"XXA\",\"XXX\")","v":"XXX"},{"$f":"VLOOKUP('BasicMeter Consolidation'!$E$56,'10A22 Naming'!$F$3:$I$52,4,FALSE)","v":{"$error":"#N/A"}},{"$f":"VLOOKUP('BasicMeter Consolidation'!$E$56,'10A22 Naming'!$F$3:$I$52,2,FALSE)","v":{"$error":"#N/A"}},"X","X","X","X","L","L","E",{"$f":"IF('VA Sizing'!$C$3=\"Liquid\",1,2)","v":2}]
["List Adder",463,0,{"$f":"IF(D30=\"2\",0,\nIF(D30=\"3\",0,\nIF(D30=\"4\",172,\nIF(D30=\"5\",628,\nIF(D30=\"6\",1510,\"\")))))","v":{"$error":"#N/A"}},0,0,0,0,0,0,0,73,0]
[]
[null,"10A22 Part Number","List Price"]
[null,{"$f":"B30&$A$1&C30&$A$1&D30&$A$1&E30&$A$1&F30&$A$1&G30&$A$1&H30&$A$1&I30&$A$1&J30&$A$1&K30&$A$1&L30&$A$1&M30","v":{"$error":"#N/A"}},{"$f":"SUM(B31:M31)","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[null,"10A32"]
[]
[null,"Static","Variable","Variable","Static","Variable","Variable","Variable","Variable","Variable","Variable","Variable","Variable","Static","Static","Variable","Variable","Variable","Variable","Variable"]
[null,"Base","Secondary","Construction","Design","Valve","Material","Cert","Float Design","Housing","Output","Regulator","Regulator Mounting","Size","Tag","Relay","Tube/Float","Scale Type","Scale Design","Accuracy"]
[null,"10A32",2,{"$f":"IF(_xlfn.NUMBERVALUE(Q43)<19,0,5)","v":{"$error":"#N/A"}},"D",{"$f":"IF(D43=0,\"N\",\"A\")","v":{"$error":"#N/A"}},{"$f":"IF(D43=0,1,4)","v":{"$error":"#N/A"}},"A",{"$f":"IF(AND('VA Sizing'!$C$3=\"Gas\",'Modified Inputs'!$J$3<VLOOKUP('BasicMeter Consolidation'!$E$56,'10A32 Capacity'!$AY$6:$BB$32,4,FALSE)),1,0)","v":{"$error":"#N/A"}},"A",0,"A",1,{"$f":"IF(_xlfn.NUMBERVALUE(Q43)<19,\"A\",\nIF(_xlfn.NUMBERVALUE(Q43)<29,\"K\",\nIF(_xlfn.NUMBERVALUE(Q43)<39,\"N\",\nIF(_xlfn.NUMBERVALUE(Q43)<49,\"P\",\"\"))))","v":{"$error":"#N/A"}},1,0,{"$f":"LEFT('BasicMeter Consolidation'!$E$56,2)","v":{"$error":"#N/A"}},{"$f":"'BasicMeter Consolidation'!H56","v":{"$error":"#N/A"}},"D","B"]
["List Adder",null,0,{"$f":"IF(D43=0,983,\nIF(D43=5,820,\"\"))","v":{"$error":"#N/A"}},0,0,0,0,{"$f":"IF(I43=1,121,0)","v":{"$error":"#N/A"}},0,0,0,0,{"$f":"IF(N43=\"A\",0,\nIF(N43=\"K\",80,\nIF(N43=\"N\",158,\nIF(N43=\"P\",333,\"\"))))","v":{"$error":"#N/A"}},0,0,0,0,0,0]
[]
[null,"10A32 Part Number","List Price"]
[null,{"$f":"B43&$A$1&C43&$A$1&D43&$A$1&E43&$A$1&F43&$A$1&G43&$A$1&H43&$A$1&I43&$A$1&J43&$A$1&K43&$A$1&L43&$A$1&M43&$A$1&N43&$A$1&O43&$A$1&P43&$A$1&Q43&$A$1&R43&$A$1&S43&$A$1&T43","v":{"$error":"#N/A"}},{"$f":"SUM(C44:T44)","v":{"$error":"#N/A"}}]
[]
[]
[]
[]
[]
[null,"FINAL PART NUMBER","List Price"]
[null,{"$f":"IF('BasicMeter Consolidation'!$B$56=\"10A61\",BulkPartNumber!$B$10,\nIF('BasicMeter Consolidation'!$B$56=\"10A4\",BulkPartNumber!$B$22,\nIF('BasicMeter Consolidation'!$B$56=\"10A22\",BulkPartNumber!$B$34,\nIF('BasicMeter Consolidation'!$B$56=\"10A32\",BulkPartNumber!$B$47,\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF('BasicMeter Consolidation'!$B$56=\"10A61\",BulkPartNumber!$C$10,\nIF('BasicMeter Consolidation'!$B$56=\"10A4\",BulkPartNumber!$C$22,\nIF('BasicMeter Consolidation'!$B$56=\"10A22\",BulkPartNumber!$C$34,\nIF('BasicMeter Consolidation'!$B$56=\"10A32\",BulkPartNumber!$C$47,\"\"))))","v":{"$error":"#N/A"}}]

{"sheet":"BasicMeter10A22 Alarm Liquid","index":70,"n_rows":58,"n_cols":40,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,5,1,8],[1,26,1,27]]}
[]
[null,"Current Tab","Current Step",null,null,"Liquid Alarm",null,null,null,null,null,null,null,null,null,"10A22 All",null,null,null,"10A22\" Range Limit",null,null,"10A22\" Range Limit",null,null,null,"Final Standard",null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,"Water GPM","Compensated Water GPM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded",null,null,null,null,"Tube/Float","Max Rounded","Tube/Float",null,"Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded",null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,null,1.3,{"$f":"'10A22 Capacity Table'!C27","v":1.3},"1/2\"","1E",150,{"$f":"IFERROR((F4/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(J4<0.00000099999,ROUND(J4,7),\nIF(J4<0.0000099999,ROUND(J4,6),\nIF(J4<0.000099999,ROUND(J4,5),\nIF(J4<0.00099999,ROUND(J4,4),\nIF(J4<0.0099999,ROUND(J4,3),\nIF(J4<0.099999,ROUND(J4,2),\nIF(J4<0.99999,ROUND(J4,2),\nIF(J4<9.999,ROUND(J4,2),\nIF(J4<99.99,ROUND(J4,1),\nIF(J4<999.99,ROUND(J4,0),\nIF(J4<9999.99,ROUND(J4,-1),\nIF(J4<99999,ROUND(J4,-2),ROUND(J4,2))))))))))))),\"viscosity\")","v":"viscosity"},null,null,null,null,{"$f":"CONCATENATE(G4,\"-\",H4)","v":"1/2\"-1E"},{"$f":"K4","v":"viscosity"},{"$f":"P4","v":"1/2\"-1E"},null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q4*0.45),'BasicMeter10A22 Alarm Liquid'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q4*0.45),'BasicMeter10A22 Alarm Liquid'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(X4,$Q$4:$R$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$14>0,U4:U14))","v":0},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$W$33,1/0),\nIFERROR(IF($Z$32=\"\",$W$32,1/0),\nIFERROR(IF($Z$31=\"\",$W$31,1/0),\nIFERROR(IF($Z$30=\"\",$W$30,1/0),\nIFERROR(IF($Z$29=\"\",$W$29,1/0),\nIFERROR(IF($Z$28=\"\",$W$28,1/0),\nIFERROR(IF($Z$27=\"\",$W$27,1/0),\nIFERROR(IF($Z$26=\"\",$W$26,1/0),\nIFERROR(IF($Z$25=\"\",$W$25,1/0),\nIFERROR(IF($Z$24=\"\",$W$24,1/0),\nIFERROR(IF($Z$23=\"\",$W$23,1/0),\nIFERROR(IF($Z$22=\"\",$W$22,1/0),\nIFERROR(IF($Z$21=\"\",$W$21,1/0),\nIFERROR(IF($Z$20=\"\",$W$20,1/0),\nIFERROR(IF($Z$19=\"\",$W$19,1/0),\nIFERROR(IF($Z$18=\"\",$W$18,1/0),\nIFERROR(IF($Z$17=\"\",$W$17,1/0),\nIFERROR(IF($Z$16=\"\",$W$16,1/0),\nIFERROR(IF($Z$15=\"\",$W$15,1/0),\nIFERROR(IF($Z$14=\"\",$W$14,1/0),\nIFERROR(IF($Z$13=\"\",$W$13,1/0),\nIFERROR(IF($Z$12=\"\",$W$12,1/0),\nIFERROR(IF($Z$11=\"\",$W$11,1/0),\nIFERROR(IF($Z$10=\"\",$W$10,1/0),\nIFERROR(IF($Z$9=\"\",$W$9,1/0),\nIFERROR(IF($Z$8=\"\",$W$8,1/0),\nIFERROR(IF($Z$7=\"\",$W$7,1/0),\nIFERROR(IF($Z$6=\"\",$W$6,1/0),\nIFERROR(IF($Z$5=\"\",$W$5,1/0),\nIFERROR(IF($Z$4=\"\",$W$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AA4,$W$4:$X$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IF(AA4=\"none\",\"sizing\",\"\")","v":"sizing"}]
[null,null,null,null,2,{"$f":"'10A22 Capacity Table'!C28","v":2},"1/2\"","1F",275,{"$f":"IFERROR((F5/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},{"$f":"IFERROR(\nIF(J5<0.00000099999,ROUND(J5,7),\nIF(J5<0.0000099999,ROUND(J5,6),\nIF(J5<0.000099999,ROUND(J5,5),\nIF(J5<0.00099999,ROUND(J5,4),\nIF(J5<0.0099999,ROUND(J5,3),\nIF(J5<0.099999,ROUND(J5,2),\nIF(J5<0.99999,ROUND(J5,2),\nIF(J5<9.999,ROUND(J5,2),\nIF(J5<99.99,ROUND(J5,1),\nIF(J5<999.99,ROUND(J5,0),\nIF(J5<9999.99,ROUND(J5,-1),\nIF(J5<99999,ROUND(J5,-2),ROUND(J5,2))))))))))))),\"viscosity\")","v":"viscosity"},null,null,null,null,{"$f":"CONCATENATE(G5,\"-\",H5)","v":"1/2\"-1F"},{"$f":"K5","v":"viscosity"},{"$f":"P5","v":"1/2\"-1F"},null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q5*0.45),'BasicMeter10A22 Alarm Liquid'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q5*0.45),'BasicMeter10A22 Alarm Liquid'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(X5,$Q$4:$R$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$14<X4,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,null,4,{"$f":"'10A22 Capacity Table'!C29","v":4},"1/2\"","1H",900,{"$f":"IFERROR((F6/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1/2\"-1H","viscosity","1/2\"-1H",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q6*0.45),'BasicMeter10A22 Alarm Liquid'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q6*0.45),'BasicMeter10A22 Alarm Liquid'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X5,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,null,6,{"$f":"'10A22 Capacity Table'!C30","v":6},"1\"","1J",1000,{"$f":"IFERROR((F7/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1\"-1J","viscosity","1\"-1J",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q7*0.45),'BasicMeter10A22 Alarm Liquid'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q7*0.45),'BasicMeter10A22 Alarm Liquid'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X6,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,null,8,{"$f":"'10A22 Capacity Table'!C31","v":8},"1\"","1K",1000,{"$f":"IFERROR((F8/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1\"-1K","viscosity","1\"-1K",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q8*0.45),'BasicMeter10A22 Alarm Liquid'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q8*0.45),'BasicMeter10A22 Alarm Liquid'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X7,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,null,11,{"$f":"'10A22 Capacity Table'!C32","v":11},"1\"","1L",1000,{"$f":"IFERROR((F9/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1\"-1L","viscosity","1\"-1L",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q9*0.45),'BasicMeter10A22 Alarm Liquid'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q9*0.45),'BasicMeter10A22 Alarm Liquid'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X8,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,null,15,{"$f":"'10A22 Capacity Table'!C33","v":15},"1-1/2\"","1M",1000,{"$f":"IFERROR((F10/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1-1/2\"-1M","viscosity","1-1/2\"-1M",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q10*0.45),'BasicMeter10A22 Alarm Liquid'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q10*0.45),'BasicMeter10A22 Alarm Liquid'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X9,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,null,20,{"$f":"'10A22 Capacity Table'!C34","v":20},"1-1/2\"","1N",1000,{"$f":"IFERROR((F11/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1-1/2\"-1N","viscosity","1-1/2\"-1N",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q11*0.45),'BasicMeter10A22 Alarm Liquid'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q11*0.45),'BasicMeter10A22 Alarm Liquid'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X10,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,null,24,{"$f":"'10A22 Capacity Table'!C35","v":24},"1-1/2\"","1P",1000,{"$f":"IFERROR((F12/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"1-1/2\"-1P","viscosity","1-1/2\"-1P",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q12*0.45),'BasicMeter10A22 Alarm Liquid'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q12*0.45),'BasicMeter10A22 Alarm Liquid'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X11,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,null,35,{"$f":"'10A22 Capacity Table'!C36","v":35},"2\"","1Q",2,{"$f":"IFERROR((F13/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"2\"-1Q","viscosity","2\"-1Q",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q13*0.45),'BasicMeter10A22 Alarm Liquid'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q13*0.45),'BasicMeter10A22 Alarm Liquid'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X12,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,null,50,{"$f":"'10A22 Capacity Table'!C37","v":50},"2\"","1R",2,{"$f":"IFERROR((F14/'Modified Inputs'!$J$23*VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE))/(('Modified Inputs'!$M$2*2.73819)/SQRT((8.4977-'Modified Inputs'!$M$2)*'Modified Inputs'!$M$2)),\"viscosity\")","v":"viscosity"},"viscosity",null,null,null,null,"2\"-1R","viscosity","2\"-1R",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q14*0.45),'BasicMeter10A22 Alarm Liquid'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q14*0.45),'BasicMeter10A22 Alarm Liquid'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X13,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,null,0,{"$f":"'10A22 Capacity Table'!C38","v":0},null,null,0,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q15*0.45),'BasicMeter10A22 Alarm Liquid'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q15*0.45),'BasicMeter10A22 Alarm Liquid'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X14,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q16*0.45),'BasicMeter10A22 Alarm Liquid'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q16*0.45),'BasicMeter10A22 Alarm Liquid'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X15,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q17*0.45),'BasicMeter10A22 Alarm Liquid'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q17*0.45),'BasicMeter10A22 Alarm Liquid'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X16,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q18*0.45),'BasicMeter10A22 Alarm Liquid'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q18*0.45),'BasicMeter10A22 Alarm Liquid'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X17,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q19*0.45),'BasicMeter10A22 Alarm Liquid'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q19*0.45),'BasicMeter10A22 Alarm Liquid'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X18,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q20*0.45),'BasicMeter10A22 Alarm Liquid'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q20*0.45),'BasicMeter10A22 Alarm Liquid'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X19,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q21*0.45),'BasicMeter10A22 Alarm Liquid'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q21*0.45),'BasicMeter10A22 Alarm Liquid'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X20,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q22*0.45),'BasicMeter10A22 Alarm Liquid'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q22*0.45),'BasicMeter10A22 Alarm Liquid'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X21,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q23*0.45),'BasicMeter10A22 Alarm Liquid'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q23*0.45),'BasicMeter10A22 Alarm Liquid'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X22,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q24*0.45),'BasicMeter10A22 Alarm Liquid'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q24*0.45),'BasicMeter10A22 Alarm Liquid'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X23,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q25*0.45),'BasicMeter10A22 Alarm Liquid'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q25*0.45),'BasicMeter10A22 Alarm Liquid'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X24,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q26*0.45),'BasicMeter10A22 Alarm Liquid'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q26*0.45),'BasicMeter10A22 Alarm Liquid'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X25,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q27*0.45),'BasicMeter10A22 Alarm Liquid'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q27*0.45),'BasicMeter10A22 Alarm Liquid'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X26,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q28*0.45),'BasicMeter10A22 Alarm Liquid'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q28*0.45),'BasicMeter10A22 Alarm Liquid'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X27,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q29*0.45),'BasicMeter10A22 Alarm Liquid'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q29*0.45),'BasicMeter10A22 Alarm Liquid'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X28,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q30*0.45),'BasicMeter10A22 Alarm Liquid'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q30*0.45),'BasicMeter10A22 Alarm Liquid'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X29,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q31*0.45),'BasicMeter10A22 Alarm Liquid'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q31*0.45),'BasicMeter10A22 Alarm Liquid'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X30,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q32*0.45),'BasicMeter10A22 Alarm Liquid'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q32*0.45),'BasicMeter10A22 Alarm Liquid'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X31,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q33*0.45),'BasicMeter10A22 Alarm Liquid'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q33*0.45),'BasicMeter10A22 Alarm Liquid'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X32,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q34*0.45),'BasicMeter10A22 Alarm Liquid'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q34*0.45),'BasicMeter10A22 Alarm Liquid'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X33,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q35*0.45),'BasicMeter10A22 Alarm Liquid'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q35*0.45),'BasicMeter10A22 Alarm Liquid'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X34,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q36*0.45),'BasicMeter10A22 Alarm Liquid'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q36*0.45),'BasicMeter10A22 Alarm Liquid'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X35,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q37*0.45),'BasicMeter10A22 Alarm Liquid'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q37*0.45),'BasicMeter10A22 Alarm Liquid'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X36,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q38*0.45),'BasicMeter10A22 Alarm Liquid'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q38*0.45),'BasicMeter10A22 Alarm Liquid'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X37,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q39*0.45),'BasicMeter10A22 Alarm Liquid'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q39*0.45),'BasicMeter10A22 Alarm Liquid'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X38,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q40*0.45),'BasicMeter10A22 Alarm Liquid'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q40*0.45),'BasicMeter10A22 Alarm Liquid'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X39,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q41*0.45),'BasicMeter10A22 Alarm Liquid'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q41*0.45),'BasicMeter10A22 Alarm Liquid'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X40,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q42*0.45),'BasicMeter10A22 Alarm Liquid'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q42*0.45),'BasicMeter10A22 Alarm Liquid'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X41,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q43*0.45),'BasicMeter10A22 Alarm Liquid'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q43*0.45),'BasicMeter10A22 Alarm Liquid'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X42,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q44*0.45),'BasicMeter10A22 Alarm Liquid'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q44*0.45),'BasicMeter10A22 Alarm Liquid'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X43,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q45*0.45),'BasicMeter10A22 Alarm Liquid'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q45*0.45),'BasicMeter10A22 Alarm Liquid'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X44,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q46*0.45),'BasicMeter10A22 Alarm Liquid'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q46*0.45),'BasicMeter10A22 Alarm Liquid'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X45,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q47*0.45),'BasicMeter10A22 Alarm Liquid'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q47*0.45),'BasicMeter10A22 Alarm Liquid'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X46,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q48*0.45),'BasicMeter10A22 Alarm Liquid'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q48*0.45),'BasicMeter10A22 Alarm Liquid'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X47,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q49*0.45),'BasicMeter10A22 Alarm Liquid'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q49*0.45),'BasicMeter10A22 Alarm Liquid'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X48,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q50*0.45),'BasicMeter10A22 Alarm Liquid'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q50*0.45),'BasicMeter10A22 Alarm Liquid'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X49,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q51*0.45),'BasicMeter10A22 Alarm Liquid'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q51*0.45),'BasicMeter10A22 Alarm Liquid'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X50,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q52*0.45),'BasicMeter10A22 Alarm Liquid'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q52*0.45),'BasicMeter10A22 Alarm Liquid'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X51,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q53*0.45),'BasicMeter10A22 Alarm Liquid'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q53*0.45),'BasicMeter10A22 Alarm Liquid'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X52,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q54*0.45),'BasicMeter10A22 Alarm Liquid'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q54*0.45),'BasicMeter10A22 Alarm Liquid'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X53,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q55*0.45),'BasicMeter10A22 Alarm Liquid'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q55*0.45),'BasicMeter10A22 Alarm Liquid'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X54,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q56*0.45),'BasicMeter10A22 Alarm Liquid'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q56*0.45),'BasicMeter10A22 Alarm Liquid'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X55,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q57*0.45),'BasicMeter10A22 Alarm Liquid'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q57*0.45),'BasicMeter10A22 Alarm Liquid'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X56,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IFERROR(IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q58*0.45),'BasicMeter10A22 Alarm Liquid'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0),0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Liquid'!Q58*0.45),'BasicMeter10A22 Alarm Liquid'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Liquid'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X57,$U$4:$U$14))","v":0}]

{"sheet":"BasicMeter10A22 Standard Gas","index":71,"n_rows":58,"n_cols":40,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,5,1,8],[1,26,1,27]]}
[]
[null,"Current Tab","Current Step",null,null,"Gas Standard",null,null,null,null,null,null,null,null,null,"10A22 All",null,null,null,"10A22\" Range Limit",null,null,"10A22 Range Limit",null,null,null,"Final Standard",null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,null,"Air SCFM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded",null,null,null,null,"Tube/Float","Max Rounded","Tube/Float",null,"Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded",null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,null,0.6,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E4)","v":0.6},"1/4\"","2B",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(J4<0.00000099999,ROUND(J4,7),\nIF(J4<0.0000099999,ROUND(J4,6),\nIF(J4<0.000099999,ROUND(J4,5),\nIF(J4<0.00099999,ROUND(J4,4),\nIF(J4<0.0099999,ROUND(J4,3),\nIF(J4<0.099999,ROUND(J4,2),\nIF(J4<0.99999,ROUND(J4,2),\nIF(J4<9.999,ROUND(J4,2),\nIF(J4<99.99,ROUND(J4,1),\nIF(J4<999.99,ROUND(J4,0),\nIF(J4<9999.99,ROUND(J4,-1),\nIF(J4<99999,ROUND(J4,-2),ROUND(J4,2)))))))))))))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"CONCATENATE(G4,\"-\",H4)","v":"1/4\"-2B"},{"$f":"K4","v":{"$error":"#VALUE!"}},{"$f":"P4","v":"1/4\"-2B"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q4*0.45),'BasicMeter10A22 Standard Gas'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q4*0.45),'BasicMeter10A22 Standard Gas'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(X4,$Q$4:$R$17,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$17>0,U4:U17))","v":0},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$W$33,1/0),\nIFERROR(IF($Z$32=\"\",$W$32,1/0),\nIFERROR(IF($Z$31=\"\",$W$31,1/0),\nIFERROR(IF($Z$30=\"\",$W$30,1/0),\nIFERROR(IF($Z$29=\"\",$W$29,1/0),\nIFERROR(IF($Z$28=\"\",$W$28,1/0),\nIFERROR(IF($Z$27=\"\",$W$27,1/0),\nIFERROR(IF($Z$26=\"\",$W$26,1/0),\nIFERROR(IF($Z$25=\"\",$W$25,1/0),\nIFERROR(IF($Z$24=\"\",$W$24,1/0),\nIFERROR(IF($Z$23=\"\",$W$23,1/0),\nIFERROR(IF($Z$22=\"\",$W$22,1/0),\nIFERROR(IF($Z$21=\"\",$W$21,1/0),\nIFERROR(IF($Z$20=\"\",$W$20,1/0),\nIFERROR(IF($Z$19=\"\",$W$19,1/0),\nIFERROR(IF($Z$18=\"\",$W$18,1/0),\nIFERROR(IF($Z$17=\"\",$W$17,1/0),\nIFERROR(IF($Z$16=\"\",$W$16,1/0),\nIFERROR(IF($Z$15=\"\",$W$15,1/0),\nIFERROR(IF($Z$14=\"\",$W$14,1/0),\nIFERROR(IF($Z$13=\"\",$W$13,1/0),\nIFERROR(IF($Z$12=\"\",$W$12,1/0),\nIFERROR(IF($Z$11=\"\",$W$11,1/0),\nIFERROR(IF($Z$10=\"\",$W$10,1/0),\nIFERROR(IF($Z$9=\"\",$W$9,1/0),\nIFERROR(IF($Z$8=\"\",$W$8,1/0),\nIFERROR(IF($Z$7=\"\",$W$7,1/0),\nIFERROR(IF($Z$6=\"\",$W$6,1/0),\nIFERROR(IF($Z$5=\"\",$W$5,1/0),\nIFERROR(IF($Z$4=\"\",$W$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AA4,$W$4:$X$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IF(AA4=\"none\",\"sizing\",\"\")","v":"sizing"}]
[null,null,null,null,1.3,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E5)","v":1.3},"1/4\"","2C",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(J5<0.00000099999,ROUND(J5,7),\nIF(J5<0.0000099999,ROUND(J5,6),\nIF(J5<0.000099999,ROUND(J5,5),\nIF(J5<0.00099999,ROUND(J5,4),\nIF(J5<0.0099999,ROUND(J5,3),\nIF(J5<0.099999,ROUND(J5,2),\nIF(J5<0.99999,ROUND(J5,2),\nIF(J5<9.999,ROUND(J5,2),\nIF(J5<99.99,ROUND(J5,1),\nIF(J5<999.99,ROUND(J5,0),\nIF(J5<9999.99,ROUND(J5,-1),\nIF(J5<99999,ROUND(J5,-2),ROUND(J5,2)))))))))))))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"CONCATENATE(G5,\"-\",H5)","v":"1/4\"-2C"},{"$f":"K5","v":{"$error":"#VALUE!"}},{"$f":"P5","v":"1/4\"-2C"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q5*0.45),'BasicMeter10A22 Standard Gas'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q5*0.45),'BasicMeter10A22 Standard Gas'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(X5,$Q$4:$R$17,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$17<X4,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,null,2,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E6)","v":2},"1/2\"","2D",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1/2\"-2D",{"$error":"#VALUE!"},"1/2\"-2D",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q6*0.45),'BasicMeter10A22 Standard Gas'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q6*0.45),'BasicMeter10A22 Standard Gas'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X5,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,null,4.5,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E7)","v":4.5},"1/2\"","2E",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1/2\"-2E",{"$error":"#VALUE!"},"1/2\"-2E",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q7*0.45),'BasicMeter10A22 Standard Gas'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q7*0.45),'BasicMeter10A22 Standard Gas'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X6,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,null,7,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E8)","v":7},"1/2\"","2G",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1/2\"-2G",{"$error":"#VALUE!"},"1/2\"-2G",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q8*0.45),'BasicMeter10A22 Standard Gas'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q8*0.45),'BasicMeter10A22 Standard Gas'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X7,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,null,9,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E9)","v":9},"1/2\"","2K",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1/2\"-2K",{"$error":"#VALUE!"},"1/2\"-2K",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q9*0.45),'BasicMeter10A22 Standard Gas'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q9*0.45),'BasicMeter10A22 Standard Gas'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X8,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,null,14,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E10)","v":14},"1\"","2L",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1\"-2L",{"$error":"#VALUE!"},"1\"-2L",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q10*0.45),'BasicMeter10A22 Standard Gas'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q10*0.45),'BasicMeter10A22 Standard Gas'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X9,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,null,20,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E11)","v":20},"1\"","2N",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1\"-2N",{"$error":"#VALUE!"},"1\"-2N",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q11*0.45),'BasicMeter10A22 Standard Gas'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q11*0.45),'BasicMeter10A22 Standard Gas'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X10,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,null,26,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E12)","v":26},"1\"","2P",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1\"-2P",{"$error":"#VALUE!"},"1\"-2P",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q12*0.45),'BasicMeter10A22 Standard Gas'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q12*0.45),'BasicMeter10A22 Standard Gas'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X11,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,null,36,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E13)","v":36},"1-1/2\"","2Q",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1-1/2\"-2Q",{"$error":"#VALUE!"},"1-1/2\"-2Q",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q13*0.45),'BasicMeter10A22 Standard Gas'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q13*0.45),'BasicMeter10A22 Standard Gas'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X12,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,null,50,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E14)","v":50},"1-1/2\"","2R",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1-1/2\"-2R",{"$error":"#VALUE!"},"1-1/2\"-2R",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q14*0.45),'BasicMeter10A22 Standard Gas'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q14*0.45),'BasicMeter10A22 Standard Gas'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X13,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,null,60,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E15)","v":60},"1-1/2\"","2S",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F15/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1-1/2\"-2S",{"$error":"#VALUE!"},"1-1/2\"-2S",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q15*0.45),'BasicMeter10A22 Standard Gas'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q15*0.45),'BasicMeter10A22 Standard Gas'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X14,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,null,80,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E16)","v":80},"2\"","2T",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F16/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"2\"-2T",{"$error":"#VALUE!"},"2\"-2T",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q16*0.45),'BasicMeter10A22 Standard Gas'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q16*0.45),'BasicMeter10A22 Standard Gas'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X15,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,null,110,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E17)","v":110},"2\"","2U",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F17/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"2\"-2U",{"$error":"#VALUE!"},"2\"-2U",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q17*0.45),'BasicMeter10A22 Standard Gas'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q17*0.45),'BasicMeter10A22 Standard Gas'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X16,$U$4:$U$17))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q18*0.45),'BasicMeter10A22 Standard Gas'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q18*0.45),'BasicMeter10A22 Standard Gas'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X17,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q19*0.45),'BasicMeter10A22 Standard Gas'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q19*0.45),'BasicMeter10A22 Standard Gas'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X18,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q20*0.45),'BasicMeter10A22 Standard Gas'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q20*0.45),'BasicMeter10A22 Standard Gas'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X19,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q21*0.45),'BasicMeter10A22 Standard Gas'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q21*0.45),'BasicMeter10A22 Standard Gas'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X20,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q22*0.45),'BasicMeter10A22 Standard Gas'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q22*0.45),'BasicMeter10A22 Standard Gas'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X21,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q23*0.45),'BasicMeter10A22 Standard Gas'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q23*0.45),'BasicMeter10A22 Standard Gas'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X22,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q24*0.45),'BasicMeter10A22 Standard Gas'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q24*0.45),'BasicMeter10A22 Standard Gas'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X23,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q25*0.45),'BasicMeter10A22 Standard Gas'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q25*0.45),'BasicMeter10A22 Standard Gas'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X24,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q26*0.45),'BasicMeter10A22 Standard Gas'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q26*0.45),'BasicMeter10A22 Standard Gas'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X25,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q27*0.45),'BasicMeter10A22 Standard Gas'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q27*0.45),'BasicMeter10A22 Standard Gas'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X26,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q28*0.45),'BasicMeter10A22 Standard Gas'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q28*0.45),'BasicMeter10A22 Standard Gas'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X27,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q29*0.45),'BasicMeter10A22 Standard Gas'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q29*0.45),'BasicMeter10A22 Standard Gas'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X28,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q30*0.45),'BasicMeter10A22 Standard Gas'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q30*0.45),'BasicMeter10A22 Standard Gas'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X29,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q31*0.45),'BasicMeter10A22 Standard Gas'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q31*0.45),'BasicMeter10A22 Standard Gas'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X30,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q32*0.45),'BasicMeter10A22 Standard Gas'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q32*0.45),'BasicMeter10A22 Standard Gas'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X31,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q33*0.45),'BasicMeter10A22 Standard Gas'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q33*0.45),'BasicMeter10A22 Standard Gas'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X32,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q34*0.45),'BasicMeter10A22 Standard Gas'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q34*0.45),'BasicMeter10A22 Standard Gas'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X33,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q35*0.45),'BasicMeter10A22 Standard Gas'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q35*0.45),'BasicMeter10A22 Standard Gas'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X34,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q36*0.45),'BasicMeter10A22 Standard Gas'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q36*0.45),'BasicMeter10A22 Standard Gas'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X35,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q37*0.45),'BasicMeter10A22 Standard Gas'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q37*0.45),'BasicMeter10A22 Standard Gas'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X36,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q38*0.45),'BasicMeter10A22 Standard Gas'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q38*0.45),'BasicMeter10A22 Standard Gas'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X37,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q39*0.45),'BasicMeter10A22 Standard Gas'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q39*0.45),'BasicMeter10A22 Standard Gas'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X38,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q40*0.45),'BasicMeter10A22 Standard Gas'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q40*0.45),'BasicMeter10A22 Standard Gas'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X39,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q41*0.45),'BasicMeter10A22 Standard Gas'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q41*0.45),'BasicMeter10A22 Standard Gas'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X40,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q42*0.45),'BasicMeter10A22 Standard Gas'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q42*0.45),'BasicMeter10A22 Standard Gas'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X41,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q43*0.45),'BasicMeter10A22 Standard Gas'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q43*0.45),'BasicMeter10A22 Standard Gas'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X42,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q44*0.45),'BasicMeter10A22 Standard Gas'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q44*0.45),'BasicMeter10A22 Standard Gas'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X43,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q45*0.45),'BasicMeter10A22 Standard Gas'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q45*0.45),'BasicMeter10A22 Standard Gas'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X44,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q46*0.45),'BasicMeter10A22 Standard Gas'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q46*0.45),'BasicMeter10A22 Standard Gas'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X45,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q47*0.45),'BasicMeter10A22 Standard Gas'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q47*0.45),'BasicMeter10A22 Standard Gas'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X46,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q48*0.45),'BasicMeter10A22 Standard Gas'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q48*0.45),'BasicMeter10A22 Standard Gas'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X47,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q49*0.45),'BasicMeter10A22 Standard Gas'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q49*0.45),'BasicMeter10A22 Standard Gas'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X48,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q50*0.45),'BasicMeter10A22 Standard Gas'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q50*0.45),'BasicMeter10A22 Standard Gas'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X49,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q51*0.45),'BasicMeter10A22 Standard Gas'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q51*0.45),'BasicMeter10A22 Standard Gas'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X50,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q52*0.45),'BasicMeter10A22 Standard Gas'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q52*0.45),'BasicMeter10A22 Standard Gas'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X51,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q53*0.45),'BasicMeter10A22 Standard Gas'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q53*0.45),'BasicMeter10A22 Standard Gas'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X52,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q54*0.45),'BasicMeter10A22 Standard Gas'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q54*0.45),'BasicMeter10A22 Standard Gas'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X53,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q55*0.45),'BasicMeter10A22 Standard Gas'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q55*0.45),'BasicMeter10A22 Standard Gas'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X54,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q56*0.45),'BasicMeter10A22 Standard Gas'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q56*0.45),'BasicMeter10A22 Standard Gas'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X55,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q57*0.45),'BasicMeter10A22 Standard Gas'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q57*0.45),'BasicMeter10A22 Standard Gas'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X56,$U$4:$U$17))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q58*0.45),'BasicMeter10A22 Standard Gas'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Standard Gas'!Q58*0.45),'BasicMeter10A22 Standard Gas'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Standard Gas'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$17<X57,$U$4:$U$17))","v":0}]

{"sheet":"BasicMeter10A22 Alarm Gas","index":72,"n_rows":58,"n_cols":40,"rows_kept":58,"cut":false,"hidden":true,"merged":[[1,5,1,8],[1,26,1,27]]}
[]
[null,"Current Tab","Current Step",null,null,"Gas Alarms",null,null,null,null,null,null,null,null,null,"10A22 All",null,null,null,"10A22\" Range Limit",null,null,"10A22 Range Limit",null,null,null,"Final Standard",null,null,null,null,null,null,null,null,null,null,"Capability Matrix"]
[null,"Fluid",{"$f":"BasicStructure!$C$3","v":1},null,null,"Air SCFM","Meter Size","Code","VIC","Max Flow Specified Units","Max Flow Rounded",null,null,null,null,"Tube/Float","Max Rounded","Tube/Float",null,"Tube/Float","Max Rounded",null,"Tube/Float","Max Rounded",null,null,"Tube/Float","Max",null,"Error Reason"]
[null,null,null,null,5.5,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E4)","v":5.5},"1/2\"","2F",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F4/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(J4<0.99999,ROUND(J4,2),\nIF(J4<9.999,ROUND(J4,2),\nIF(J4<99.99,ROUND(J4,1),\nIF(J4<999.99,ROUND(J4,0),\nIF(J4<9999.99,ROUND(J4,-1),\nIF(J4<99999,ROUND(J4,-2),ROUND(J4,2)))))))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"CONCATENATE(G4,\"-\",H4)","v":"1/2\"-2F"},{"$f":"K4","v":{"$error":"#VALUE!"}},{"$f":"P4","v":"1/2\"-2F"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q4*0.45),'BasicMeter10A22 Alarm Gas'!Q4+0.000001>'Modified Inputs'!$N$2),P4,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q4*0.45),'BasicMeter10A22 Alarm Gas'!Q4+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q4,0),0)","v":0},null,{"$f":"VLOOKUP(X4,$Q$4:$R$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$14>0,U4:U14))","v":0},null,null,{"$f":"IFERROR(IF($Z$33=\"\",$W$33,1/0),\nIFERROR(IF($Z$32=\"\",$W$32,1/0),\nIFERROR(IF($Z$31=\"\",$W$31,1/0),\nIFERROR(IF($Z$30=\"\",$W$30,1/0),\nIFERROR(IF($Z$29=\"\",$W$29,1/0),\nIFERROR(IF($Z$28=\"\",$W$28,1/0),\nIFERROR(IF($Z$27=\"\",$W$27,1/0),\nIFERROR(IF($Z$26=\"\",$W$26,1/0),\nIFERROR(IF($Z$25=\"\",$W$25,1/0),\nIFERROR(IF($Z$24=\"\",$W$24,1/0),\nIFERROR(IF($Z$23=\"\",$W$23,1/0),\nIFERROR(IF($Z$22=\"\",$W$22,1/0),\nIFERROR(IF($Z$21=\"\",$W$21,1/0),\nIFERROR(IF($Z$20=\"\",$W$20,1/0),\nIFERROR(IF($Z$19=\"\",$W$19,1/0),\nIFERROR(IF($Z$18=\"\",$W$18,1/0),\nIFERROR(IF($Z$17=\"\",$W$17,1/0),\nIFERROR(IF($Z$16=\"\",$W$16,1/0),\nIFERROR(IF($Z$15=\"\",$W$15,1/0),\nIFERROR(IF($Z$14=\"\",$W$14,1/0),\nIFERROR(IF($Z$13=\"\",$W$13,1/0),\nIFERROR(IF($Z$12=\"\",$W$12,1/0),\nIFERROR(IF($Z$11=\"\",$W$11,1/0),\nIFERROR(IF($Z$10=\"\",$W$10,1/0),\nIFERROR(IF($Z$9=\"\",$W$9,1/0),\nIFERROR(IF($Z$8=\"\",$W$8,1/0),\nIFERROR(IF($Z$7=\"\",$W$7,1/0),\nIFERROR(IF($Z$6=\"\",$W$6,1/0),\nIFERROR(IF($Z$5=\"\",$W$5,1/0),\nIFERROR(IF($Z$4=\"\",$W$4,1/0),\"none\"))))))))))))))))))))))))))))))","v":"none"},{"$f":"VLOOKUP(AA4,$W$4:$X$33,2,FALSE)","v":{"$error":"#N/A"}},null,{"$f":"IF(AA4=\"none\",\"sizing\",\"\")","v":"sizing"}]
[null,null,null,null,8.5,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E5)","v":8.5},"1/2\"","2H",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F5/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$f":"IF(J5<0.99999,ROUND(J5,2),\nIF(J5<9.999,ROUND(J5,2),\nIF(J5<99.99,ROUND(J5,1),\nIF(J5<999.99,ROUND(J5,0),\nIF(J5<9999.99,ROUND(J5,-1),\nIF(J5<99999,ROUND(J5,-2),ROUND(J5,2)))))))","v":{"$error":"#VALUE!"}},null,null,null,null,{"$f":"CONCATENATE(G5,\"-\",H5)","v":"1/2\"-2H"},{"$f":"K5","v":{"$error":"#VALUE!"}},{"$f":"P5","v":"1/2\"-2H"},null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q5*0.45),'BasicMeter10A22 Alarm Gas'!Q5+0.000001>'Modified Inputs'!$N$2),P5,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q5*0.45),'BasicMeter10A22 Alarm Gas'!Q5+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q5,0),0)","v":0},null,{"$f":"VLOOKUP(X5,$Q$4:$R$14,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"MAX(IF($U$4:$U$14<X4,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,"10A61","10A4","10A22","10A32"]
[null,null,null,null,9,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E6)","v":9},"1/2\"","2J",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F6/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1/2\"-2J",{"$error":"#VALUE!"},"1/2\"-2J",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q6*0.45),'BasicMeter10A22 Alarm Gas'!Q6+0.000001>'Modified Inputs'!$N$2),P6,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q6*0.45),'BasicMeter10A22 Alarm Gas'!Q6+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q6,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X5,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Type","NPT"]
[null,null,null,null,14,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E7)","v":14},"1\"","2L",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F7/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1\"-2L",{"$error":"#VALUE!"},"1\"-2L",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q7*0.45),'BasicMeter10A22 Alarm Gas'!Q7+0.000001>'Modified Inputs'!$N$2),P7,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q7*0.45),'BasicMeter10A22 Alarm Gas'!Q7+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q7,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X6,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Flange"]
[null,null,null,null,19,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E8)","v":19},"1\"","2M",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F8/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1\"-2M",{"$error":"#VALUE!"},"1\"-2M",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q8*0.45),'BasicMeter10A22 Alarm Gas'!Q8+0.000001>'Modified Inputs'!$N$2),P8,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q8*0.45),'BasicMeter10A22 Alarm Gas'!Q8+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q8,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X7,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Connection Size","1/4\""]
[null,null,null,null,26,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E9)","v":26},"1\"","2P",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F9/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1\"-2P",{"$error":"#VALUE!"},"1\"-2P",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q9*0.45),'BasicMeter10A22 Alarm Gas'!Q9+0.000001>'Modified Inputs'!$N$2),P9,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q9*0.45),'BasicMeter10A22 Alarm Gas'!Q9+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q9,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X8,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1/2\""]
[null,null,null,null,36,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E10)","v":36},"1-1/2\"","2Q",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F10/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1-1/2\"-2Q",{"$error":"#VALUE!"},"1-1/2\"-2Q",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q10*0.45),'BasicMeter10A22 Alarm Gas'!Q10+0.000001>'Modified Inputs'!$N$2),P10,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q10*0.45),'BasicMeter10A22 Alarm Gas'!Q10+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q10,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X9,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"1\""]
[null,null,null,null,50,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E11)","v":50},"1-1/2\"","2R",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F11/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1-1/2\"-2R",{"$error":"#VALUE!"},"1-1/2\"-2R",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q11*0.45),'BasicMeter10A22 Alarm Gas'!Q11+0.000001>'Modified Inputs'!$N$2),P11,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q11*0.45),'BasicMeter10A22 Alarm Gas'!Q11+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q11,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X10,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"2\""]
[null,null,null,null,60,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E12)","v":60},"1-1/2\"","2S",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F12/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"1-1/2\"-2S",{"$error":"#VALUE!"},"1-1/2\"-2S",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q12*0.45),'BasicMeter10A22 Alarm Gas'!Q12+0.000001>'Modified Inputs'!$N$2),P12,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q12*0.45),'BasicMeter10A22 Alarm Gas'!Q12+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q12,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X11,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Tube Material","Glass"]
[null,null,null,null,80,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E13)","v":80},"2\"","2T",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F13/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"2\"-2T",{"$error":"#VALUE!"},"2\"-2T",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q13*0.45),'BasicMeter10A22 Alarm Gas'!Q13+0.000001>'Modified Inputs'!$N$2),P13,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q13*0.45),'BasicMeter10A22 Alarm Gas'!Q13+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q13,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X12,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Metal (316SST)"]
[null,null,null,null,110,{"$f":"IF(AND('VA Sizing'!$C$3=\"Liquid\",cP>1.49),\"viscosity\",E14)","v":110},"2\"","2U",null,{"$f":"IF('VA Sizing'!$C$5=\"Standard\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(530*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Normal\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT((14.7*'10A22 Standard Results'!$D$12*'10A22 Standard Results'!$A$12)/(492*'10A22 Standard Results'!$B$12)))/0.00003531,\nIF('VA Sizing'!$C$5=\"Actual\",VLOOKUP('VA Sizing'!$D$12,'Modified Inputs'!$I$8:$J$32,2,FALSE)*(F14/SQRT(('10A22 Standard Results'!$B$12*('10A61 5\" Calcs'!$O$46/0.0012)*'10A22 Standard Results'!$A$12)/('10A22 Standard Results'!$A$12*'10A22 Standard Results'!$B$12)))/0.00003531,\"\")))","v":""},{"$error":"#VALUE!"},null,null,null,null,"2\"-2U",{"$error":"#VALUE!"},"2\"-2U",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q14*0.45),'BasicMeter10A22 Alarm Gas'!Q14+0.000001>'Modified Inputs'!$N$2),P14,0)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q14*0.45),'BasicMeter10A22 Alarm Gas'!Q14+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q14,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X13,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Integral Needle Valve","Yes"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q15*0.45),'BasicMeter10A22 Alarm Gas'!Q15+0.000001>'Modified Inputs'!$N$2),P15,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q15*0.45),'BasicMeter10A22 Alarm Gas'!Q15+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q15,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X14,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"No"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q16*0.45),'BasicMeter10A22 Alarm Gas'!Q16+0.000001>'Modified Inputs'!$N$2),P16,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q16*0.45),'BasicMeter10A22 Alarm Gas'!Q16+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q16,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X15,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,"Function","Indicate"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q17*0.45),'BasicMeter10A22 Alarm Gas'!Q17+0.000001>'Modified Inputs'!$N$2),P17,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q17*0.45),'BasicMeter10A22 Alarm Gas'!Q17+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q17,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X16,$U$4:$U$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,"Transmit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q18*0.45),'BasicMeter10A22 Alarm Gas'!Q18+0.000001>'Modified Inputs'!$N$2),P18,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q18*0.45),'BasicMeter10A22 Alarm Gas'!Q18+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q18,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X17,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q19*0.45),'BasicMeter10A22 Alarm Gas'!Q19+0.000001>'Modified Inputs'!$N$2),P19,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q19*0.45),'BasicMeter10A22 Alarm Gas'!Q19+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q19,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X18,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q20*0.45),'BasicMeter10A22 Alarm Gas'!Q20+0.000001>'Modified Inputs'!$N$2),P20,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q20*0.45),'BasicMeter10A22 Alarm Gas'!Q20+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q20,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X19,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q21*0.45),'BasicMeter10A22 Alarm Gas'!Q21+0.000001>'Modified Inputs'!$N$2),P21,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q21*0.45),'BasicMeter10A22 Alarm Gas'!Q21+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q21,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X20,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q22*0.45),'BasicMeter10A22 Alarm Gas'!Q22+0.000001>'Modified Inputs'!$N$2),P22,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q22*0.45),'BasicMeter10A22 Alarm Gas'!Q22+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q22,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X21,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q23*0.45),'BasicMeter10A22 Alarm Gas'!Q23+0.000001>'Modified Inputs'!$N$2),P23,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q23*0.45),'BasicMeter10A22 Alarm Gas'!Q23+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q23,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X22,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q24*0.45),'BasicMeter10A22 Alarm Gas'!Q24+0.000001>'Modified Inputs'!$N$2),P24,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q24*0.45),'BasicMeter10A22 Alarm Gas'!Q24+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q24,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X23,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q25*0.45),'BasicMeter10A22 Alarm Gas'!Q25+0.000001>'Modified Inputs'!$N$2),P25,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q25*0.45),'BasicMeter10A22 Alarm Gas'!Q25+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q25,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X24,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q26*0.45),'BasicMeter10A22 Alarm Gas'!Q26+0.000001>'Modified Inputs'!$N$2),P26,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q26*0.45),'BasicMeter10A22 Alarm Gas'!Q26+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q26,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X25,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q27*0.45),'BasicMeter10A22 Alarm Gas'!Q27+0.000001>'Modified Inputs'!$N$2),P27,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q27*0.45),'BasicMeter10A22 Alarm Gas'!Q27+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q27,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X26,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q28*0.45),'BasicMeter10A22 Alarm Gas'!Q28+0.000001>'Modified Inputs'!$N$2),P28,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q28*0.45),'BasicMeter10A22 Alarm Gas'!Q28+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q28,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X27,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q29*0.45),'BasicMeter10A22 Alarm Gas'!Q29+0.000001>'Modified Inputs'!$N$2),P29,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q29*0.45),'BasicMeter10A22 Alarm Gas'!Q29+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q29,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X28,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q30*0.45),'BasicMeter10A22 Alarm Gas'!Q30+0.000001>'Modified Inputs'!$N$2),P30,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q30*0.45),'BasicMeter10A22 Alarm Gas'!Q30+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q30,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X29,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q31*0.45),'BasicMeter10A22 Alarm Gas'!Q31+0.000001>'Modified Inputs'!$N$2),P31,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q31*0.45),'BasicMeter10A22 Alarm Gas'!Q31+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q31,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X30,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q32*0.45),'BasicMeter10A22 Alarm Gas'!Q32+0.000001>'Modified Inputs'!$N$2),P32,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q32*0.45),'BasicMeter10A22 Alarm Gas'!Q32+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q32,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X31,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q33*0.45),'BasicMeter10A22 Alarm Gas'!Q33+0.000001>'Modified Inputs'!$N$2),P33,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q33*0.45),'BasicMeter10A22 Alarm Gas'!Q33+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q33,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X32,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q34*0.45),'BasicMeter10A22 Alarm Gas'!Q34+0.000001>'Modified Inputs'!$N$2),P34,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q34*0.45),'BasicMeter10A22 Alarm Gas'!Q34+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q34,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X33,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q35*0.45),'BasicMeter10A22 Alarm Gas'!Q35+0.000001>'Modified Inputs'!$N$2),P35,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q35*0.45),'BasicMeter10A22 Alarm Gas'!Q35+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q35,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X34,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q36*0.45),'BasicMeter10A22 Alarm Gas'!Q36+0.000001>'Modified Inputs'!$N$2),P36,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q36*0.45),'BasicMeter10A22 Alarm Gas'!Q36+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q36,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X35,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q37*0.45),'BasicMeter10A22 Alarm Gas'!Q37+0.000001>'Modified Inputs'!$N$2),P37,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q37*0.45),'BasicMeter10A22 Alarm Gas'!Q37+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q37,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X36,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q38*0.45),'BasicMeter10A22 Alarm Gas'!Q38+0.000001>'Modified Inputs'!$N$2),P38,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q38*0.45),'BasicMeter10A22 Alarm Gas'!Q38+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q38,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X37,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q39*0.45),'BasicMeter10A22 Alarm Gas'!Q39+0.000001>'Modified Inputs'!$N$2),P39,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q39*0.45),'BasicMeter10A22 Alarm Gas'!Q39+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q39,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X38,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q40*0.45),'BasicMeter10A22 Alarm Gas'!Q40+0.000001>'Modified Inputs'!$N$2),P40,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q40*0.45),'BasicMeter10A22 Alarm Gas'!Q40+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q40,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X39,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q41*0.45),'BasicMeter10A22 Alarm Gas'!Q41+0.000001>'Modified Inputs'!$N$2),P41,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q41*0.45),'BasicMeter10A22 Alarm Gas'!Q41+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q41,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X40,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q42*0.45),'BasicMeter10A22 Alarm Gas'!Q42+0.000001>'Modified Inputs'!$N$2),P42,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q42*0.45),'BasicMeter10A22 Alarm Gas'!Q42+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q42,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X41,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q43*0.45),'BasicMeter10A22 Alarm Gas'!Q43+0.000001>'Modified Inputs'!$N$2),P43,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q43*0.45),'BasicMeter10A22 Alarm Gas'!Q43+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q43,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X42,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q44*0.45),'BasicMeter10A22 Alarm Gas'!Q44+0.000001>'Modified Inputs'!$N$2),P44,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q44*0.45),'BasicMeter10A22 Alarm Gas'!Q44+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q44,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X43,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q45*0.45),'BasicMeter10A22 Alarm Gas'!Q45+0.000001>'Modified Inputs'!$N$2),P45,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q45*0.45),'BasicMeter10A22 Alarm Gas'!Q45+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q45,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X44,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q46*0.45),'BasicMeter10A22 Alarm Gas'!Q46+0.000001>'Modified Inputs'!$N$2),P46,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q46*0.45),'BasicMeter10A22 Alarm Gas'!Q46+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q46,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X45,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q47*0.45),'BasicMeter10A22 Alarm Gas'!Q47+0.000001>'Modified Inputs'!$N$2),P47,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q47*0.45),'BasicMeter10A22 Alarm Gas'!Q47+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q47,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X46,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q48*0.45),'BasicMeter10A22 Alarm Gas'!Q48+0.000001>'Modified Inputs'!$N$2),P48,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q48*0.45),'BasicMeter10A22 Alarm Gas'!Q48+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q48,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X47,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q49*0.45),'BasicMeter10A22 Alarm Gas'!Q49+0.000001>'Modified Inputs'!$N$2),P49,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q49*0.45),'BasicMeter10A22 Alarm Gas'!Q49+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q49,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X48,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q50*0.45),'BasicMeter10A22 Alarm Gas'!Q50+0.000001>'Modified Inputs'!$N$2),P50,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q50*0.45),'BasicMeter10A22 Alarm Gas'!Q50+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q50,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X49,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q51*0.45),'BasicMeter10A22 Alarm Gas'!Q51+0.000001>'Modified Inputs'!$N$2),P51,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q51*0.45),'BasicMeter10A22 Alarm Gas'!Q51+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q51,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X50,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q52*0.45),'BasicMeter10A22 Alarm Gas'!Q52+0.000001>'Modified Inputs'!$N$2),P52,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q52*0.45),'BasicMeter10A22 Alarm Gas'!Q52+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q52,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X51,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q53*0.45),'BasicMeter10A22 Alarm Gas'!Q53+0.000001>'Modified Inputs'!$N$2),P53,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q53*0.45),'BasicMeter10A22 Alarm Gas'!Q53+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q53,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X52,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q54*0.45),'BasicMeter10A22 Alarm Gas'!Q54+0.000001>'Modified Inputs'!$N$2),P54,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q54*0.45),'BasicMeter10A22 Alarm Gas'!Q54+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q54,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X53,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q55*0.45),'BasicMeter10A22 Alarm Gas'!Q55+0.000001>'Modified Inputs'!$N$2),P55,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q55*0.45),'BasicMeter10A22 Alarm Gas'!Q55+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q55,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X54,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q56*0.45),'BasicMeter10A22 Alarm Gas'!Q56+0.000001>'Modified Inputs'!$N$2),P56,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q56*0.45),'BasicMeter10A22 Alarm Gas'!Q56+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q56,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X55,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q57*0.45),'BasicMeter10A22 Alarm Gas'!Q57+0.000001>'Modified Inputs'!$N$2),P57,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q57*0.45),'BasicMeter10A22 Alarm Gas'!Q57+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q57,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X56,$U$4:$U$14))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",0,"-",null,{"$f":"IF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q58*0.45),'BasicMeter10A22 Alarm Gas'!Q58+0.000001>'Modified Inputs'!$N$2),P58,0)","v":0},{"$f":"IFERROR(\nIF(AND('Modified Inputs'!$N$2>('BasicMeter10A22 Alarm Gas'!Q58*0.45),'BasicMeter10A22 Alarm Gas'!Q58+0.0000001>'Modified Inputs'!$N$2),'BasicMeter10A22 Alarm Gas'!Q58,0),0)","v":0},null,{"$error":"#N/A"},{"$f":"MAX(IF($U$4:$U$14<X57,$U$4:$U$14))","v":0}]

{"sheet":"Assistant","index":73,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Fluid Type","$C$3","Select if the fluid is either a liquid or gas"]
[null,null,null,null,"Fluid Name","$C$4","Select the name of the fluid"]
[null,null,null,null,"Reference Condition","$C$5","Actual - Operating conditions. Select for mass flow units\n\nNormal - 0 ⁰C and 1013 mbar(a) conditions (ex. Nm3/hr)\n\nStandard - 70 ⁰F and 14.7 psi(a) conditions (ex. SCFH)"]
[null,null,null,null,"Type of Density","$C$6","Select whether the sizing will use the density of the gas at reference or operating conditions"]
[null,null,null,null,"Density at Reference Conditions","$C$7","Enter the density of the gas at reference conditions"]
[null,null,null,null,"Viscosity at Operating Conditions","$C$8","Enter the viscosity of the fluid at operating conditions. Note the viscosity of a fluid can significantly change with temperature."]
[null,null,null,null,"Operating Pressure","$C$9","Enter the operating pressure of this application. VA Meters can only be sized to one process condition at a time."]
[null,null,null,null,"Operating Temperature","$C$10","Enter the operating temperature of this application. VA Meters can only be sized to one process condition at a time."]
[null,null,null,null,"Density at Operating Conditions","$C$11","Enter the density of the gas at operating conditions"]
[null,null,null,null,"Maximum Flowrate","$C$12","Enter the flowrate the meter should be sized to. It is recommended the meter is sized to the maximum flowrate of the application."]

{"sheet":"Descriptions","index":74,"n_rows":10,"n_cols":6,"rows_kept":10,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[null,"Meter","Description","Features","Notes"]
[null,"10A61","PurgeMaster 10A6100 flowmeters are low flow capacity  variable area flowmeters for both liquid and gas with an excellent selection of material and scale lengths in a single product family design. They feature a corrosion resistant, high strength stainless steel body, quick, easy snap-in tube construction and a safety tested operator protection shield.","• Single or Dual Alarm Sensors\n• Optional Needle Valve\n• Optional Differential Pressure Regulator\n• Operator Protection Shield\n• Snap-in Removable Tube\n• 1/4\"  Threaded Connections\n","Alarms for the 10A61 can only be configured with SS or CA Floats. The 3\" Meter has an accuracy of 10% while the 5\", 6\", and 10\" Meters provide an accuracy of 2%.","• Snap-in Removable Tube\n• 1/4\"  Threaded Connections"]
[null,"10A4","The VA Master is of the highest quality and versatility in the market and has been proven over a long history. Fully retrofitable with several float and tube designs for practically any clean liquid or gas process. Its wide view angle visibility, highly stable stainless steel frame and alarming capabilities make the V/A Master the one for all solutions.","• Easily removeable tube for maintenance or reranging\n• Wide-Angle View\n• Optional Alarm System\n• Up to 3 Scales for Varying  Operating Conditions\n• Optional PVC end fittings\n• 1/2 to 1-1/2\" threaded or flanged connections","Floats for alarms and other specialty floats are selectable via the dropdown list below. Floats other than SST are intended for liquid measurement only.","• Up to 3 Scales for Varying  Operating Conditions\n• Optional PVC end fittings\n• 1/2 to 1-1/2\" threaded or flanged connections"]
[null,"10A22","The RatoSight is a rugged, low cost glass tube meter providing stable and reliable operation. Its materials selection and outstanding installation flexibility make it the solution for visual indication of moderate viscosity liquids. It can be suited with fully adjustable, vibration-proof magnetic switches and relays.","• All brass fittings\n• Aluminum and brass floats\n• Optional PVC end fittings\n• 1/2 to 2\" threaded connections\n• Multiport orientations for horizontal, vertical or a variation of both\n• Optional Alarm","Brass floats are best suited for liquid flows, aluminum are best for gas flowrates. ","• Multiport orientations for horizontal, vertical or a variation of both\n• Optional Alarm"]
[null,"10A32","This 10A32 is compact, rugged Armored Purgemeter is especially designed for low flow measurements at high pressure ratings and/or high temperatures and in applications where glass tubes are not satisfactory.  Available with or without an integral control valve, alarms, 4-20mA Analog transmitter and pressure regulator.","• Interchangeable Primaries and Secondaries\n• Threaded vertical NPT or G Connections for all sizes and horizontal with valve connections for 1/4\" size\n\n","Damping through a twisted guide rod is required for low static gauge pressure applications. Consult with ABB on operating pressures that are close to atmospheric. Error is displayed if it is a potential issue.","• Various choices for secondaries; materials and functions\n• Optional Constant Flow DP Regulator\n• Rated for 6% Full Scale without calibration"]
[null,"FAM54","The FAM54 Armored VA Master is an all metal 316 SST meter designed for clean fluids and steam for sizes up to 4”. It is particularly suited for aggressive or opaque fluids where glass tubes cannot be used for high pressures/temperatures. Alarms, digital communication and all PTFE wetted parts are available","• Rugged secondary, approved for several hazardous area applications. Upgradeable and interchangeable\n• Non-protruding floats and float guides \n","Varying maximum flowrates can be achieved using the same tube and float combination.","• State of the art magnetic coupling system\n• Re-rangeable and suitable for re-purposing for a variaty of process applications\n• Option for PTFE lined wetted components"]

{"sheet":"Viscosity Limits","index":75,"n_rows":15,"n_cols":12,"rows_kept":15,"cut":false,"hidden":true,"merged":[[1,1,1,3],[1,5,1,7],[1,9,1,11]]}
[]
[null,"10A61 3\"",null,null,null,"10A61 5\"",null,null,null,"10A61 10\" + 6\""]
[null,"Tube","Variable","Value",null,"Tube","Variable","Value",null,"Tube","Variable","Value"]
[null,"1/8-08","X",10,null,"1/4-25","N",30,null,"1/8-077","X",10]
[null,"1/8-20","X",60,null,"1/4-20","N",30,null,"1/8-13.3","X",60]
[null,"1/4-15","X",60,null,"1/4-16","N",30,null,"1/8-32","X",60]
[null,"1/4-20","X",60,null,"1/4-10","N",30,null,"1/4-10","X",60]
[null,"1/4-41-G","X",60,null,"1/8-12","N",30,null,"1/4-19","X",60]
[null,"1/4-41-P","X",60,null,"1/8-08","N",30,null,"1/4-40","X",60]
[null,null,null,null,null,"1/16-12","N",30]
[null,null,null,null,null,"1/16-16","N",30]
[null,null,null,null,null,"1/16-20","N",30]
[null,null,null,null,null,"1/8-25","N",30]
[null,null,null,null,null,"1/8-20","N",30]
[null,null,null,null,null,"1/8-16","N",30]